{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["RDL browser","Settings","about","Results1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"RDL browser","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[[0,0,0,4]]}
["RDL2 browser to spreadsheet tool version 75",null,null,null,null,null,"Endpoint: http://data.15926.org/rdl/"]
["Contact: onno.paap@gmail.com",null,null,null,null,"Action","ELECTRICAL DEVICE","http://data.15926.org/rdl/RDS1407117061"]
[]
["Search:","ELECTRICAL DEVICE"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Note: first set coloring on in Settings"]
[null,"Coloring (containing this string will give this color)"]
[null,"ClassOfFunctionalObject"]
[null,"ClassOfInanimatePhysicalObject "]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Namespace replacer (definition containing this string replaces the namespace)"]
[null,"API","API:"]
[null,"ASME","ASME:"]
[null,"ASTM","ASTM:"]
[null,"DIN","DIN:"]
[null,"EN","EN:"]
[null,"ISO","ISO:"]
[null,"NORSOK","NOR:"]
[null,"NPD","NOR:"]
[null,"NS","NOR:"]
[null,"ROSEMOUNT","ROS:"]
[null,"SAE","SAE:"]
[null,"SIEMENS","SIE:"]
[null,"SKOTSELV","SKOT:"]
[null,"TWR","TWR:"]

{"sheet":"Settings","index":1,"n_rows":87,"n_cols":8,"rows_kept":87,"cut":false,"hidden":true,"merged":[]}
["Setting name","Select name","OnKey","Value","Status","RDLType"]
["Endpoint","RDL2 (15926.org)",null,"http://data.15926.org/rdl/","Current",null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA RDL",null,"http://data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA Staging",null,"http://staging.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA SVRDL",null,"http://svrdl.community.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P4",null,"http://posccaesar.org/p4/sparql",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P12",null,"http://sti.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","Localhost",null,"http://localhost:8890/sparql/",null,null,null,"Note: end address always with a slash (/)"]
[]
["gBaseNamespace",null,"http://data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://staging.data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://svrdl.community.data.posccaesar.org/rdl/","http://svrdl.community.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://posccaesar.org/p4/sparql","http://posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://sti.data.posccaesar.org/rdl/","http://sti.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://localhost:8890/sparql/","http://data.15926.org/rdl/",null,"RDL2"]
["gKeepSettings",null,null,"T"]
["gShowDeprecated",null,null,"F"]
["gColoring",null,null,"T"]
["gNamespaceReplacing",null,null,"F"]
["gHyperlinkReplacing",null,null,"F"]
[]
["Endpoint","aisi",null,"http://data.15926.org/aisi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ansi",null,"http://data.15926.org/ansi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","api",null,"http://data.15926.org/api/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","all",null,"http://data.15926.org/all/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","asme",null,"http://data.15926.org/asme/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","astm",null,"http://data.15926.org/astm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","atex",null,"http://data.15926.org/atex/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","bs",null,"http://data.15926.org/bs/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","din",null,"http://data.15926.org/din/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dm",null,"http://data.15926.org/dm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dnv",null,"http://data.15926.org/dnv/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","edm",null,"http://data.15926.org/edm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","en",null,"http://data.15926.org/en/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","eu",null,"http://data.15926.org/eu/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iec",null,"http://data.15926.org/iec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ieee",null,"http://data.15926.org/ieee/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iso",null,"http://data.15926.org/iso/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","lci",null,"http://data.15926.org/lci/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","mss",null,"http://data.15926.org/mss/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nace",null,"http://data.15926.org/nace/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nec",null,"http://data.15926.org/nec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nema",null,"http://data.15926.org/nema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nfpa",null,"http://data.15926.org/nfpa/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nor",null,"http://data.15926.org/nor/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","rdl",null,"http://data.15926.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sae",null,"http://data.15926.org/sae/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sie",null,"http://data.15926.org/sie/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","tema",null,"http://data.15926.org/tema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","twr",null,"http://data.15926.org/twr/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","uns",null,"http://data.15926.org/uns/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","wits",null,"http://data.15926.org/wits/",null,null,null,"Note: end address always with a slash (/)"]
[]
[]
["gBaseNamespace",null,"http://data.15926.org/aisi/","http://data.15926.org/aisi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ansi/","http://data.15926.org/ansi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/api/","http://data.15926.org/api/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/asme/","http://data.15926.org/asme/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/all/","http://data.15926.org/all/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/astm/","http://data.15926.org/astm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/atex/","http://data.15926.org/atex/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/bs/","http://data.15926.org/bs/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/din/","http://data.15926.org/din/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dm/","http://data.15926.org/dm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dnv/","http://data.15926.org/dnv/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/edm/","http://data.15926.org/edm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/en/","http://data.15926.org/en/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/eu/","http://data.15926.org/eu/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iec/","http://data.15926.org/iec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ieee/","http://data.15926.org/ieee/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iso/","http://data.15926.org/iso/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/lci/","http://data.15926.org/lci/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/mss/","http://data.15926.org/mss/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nace/","http://data.15926.org/nace/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nec/","http://data.15926.org/nec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nema/","http://data.15926.org/nema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nfpa/","http://data.15926.org/nfpa/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nor/","http://data.15926.org/nor/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sae/","http://data.15926.org/sae/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sie/","http://data.15926.org/sie/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/tema/","http://data.15926.org/tema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/twr/","http://data.15926.org/twr/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/uns/","http://data.15926.org/uns/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/wits/","http://data.15926.org/wits/",null,"RDL2"]
["                                          "]

{"sheet":"about","index":2,"n_rows":176,"n_cols":3,"rows_kept":176,"cut":false,"hidden":false,"merged":[]}
["Version 75 changes","2018-10-05","Onno Paap"]
["missing superclasses - and orphans- filter no deprecated classes"]
[]
["Version 74 changes","2018-09-30","Onno Paap"]
["Repaired bug missing label"]
[]
["Version 73 changes","2018-05-16","Onno Paap"]
["Repaired bug Deprecated Superclass"]
[]
[]
[]
["Version 71 changes","2016-07-17","Onno Paap"]
["Aded report button for comparison of RDL2 with a subfolder called views filled with spreadsheets."]
[]
[]
["Version 69 changes","2016-06-16","Onno Paap"]
["Added button: \"errors in definitions\" that lists all classes that have more or less \"<\" brackets than the number of super class relationships + 1. Where the part after the word \"that \"  is ignored in the count of \"<\" brackets."]
[]
["Version 68 changes","2016-06-13","Onno Paap"]
["Updated endpoint of RDL2 sparql "]
[]
["Version 67 changes","2016-05-22","Onno Paap"]
["Added button list subclasses from superclass "]
[]
["Version 65 changes","2016-04-25","Onno Paap"]
["Added checkbox at action dialog \"supress double child occurances\" so that this built-in feature can be switched off"]
[]
["Version 64 changes","2016-04-20","Onno Paap"]
["Made search case-insensitive and added endpoint \"all\""]
[]
["Version 63 changes","2016-09-28","Onno Paap"]
["Made entity list working on P4 endpoint (they changed the database version which was not accepting som sparql setting)"]
["Version 62 changes","2016-09-28","Onno Paap"]
["Applied show deprecated to searched result list"]
[]
["Version 61 changes","2016-08-29","Onno Paap"]
["Added query from pcardl for ClassOfIndirectProperty"]
[]
["Version 60 changes","2016-08-19","Onno Paap"]
["Repaired failing entity reports"]
[]
["Version 59 changes","2016-08-19","Onno Paap"]
["Missing superclasses now queries whole federation of RDL2"]
[]
["Version 58 changes","2016-08-16","Onno Paap"]
["Repaired missing output for entities and doubles in RDL2 endpoints other than rdl"]
[]
["Version 57 changes","2016-08-13","Onno Paap"]
["Doubles report now skips classes that are deprecated"]
[]
["Version 56 changes","2016-07-22","Onno Paap"]
["Made rowheight suitable for longer definitions to example DESIGN BASIS"]
[]
["Version 55 changes","2016-07-19","Onno Paap"]
["Made rowheight suitable for longer definitions"]
[]
["Version 54 changes","2016-07-03","Onno Paap"]
["Entity Type field changed to 6 merged cells."]
[]
["Version 53 changes","2016-06-23","Onno Paap"]
["added lci namespace"]
[]
["Version 52 changes","2016-06-23","Onno Paap"]
["Added deprecated count to list entities"]
[]
["Version 51 changes","2016-06-19","Onno Paap"]
["Updated namespaces of staging RDL"]
[]
["Version 50 changes","2016-06-19","Onno Paap"]
["taxonomy view repaired missing entity type"]
[]
["Version 49 changes","2016-06-14","Onno Paap"]
["Room for 12 superclasses"]
[]
["Version 48 changes","2016-06-14","Onno Paap"]
["Repaired NOR:/RDS  bug"]
[]
["Version 47 changes","2016-06-14","Onno Paap"]
["Repaired endpoint bug"]
[]
["Version 46 changes","2016-06-13","Onno Paap"]
["Updated endpoints"]
[]
["Version 45 changes","2016-06-06","Onno Paap"]
["Completed Missing Superclasses report"]
[]
["Version 44 changes","2016-05-20","Onno Paap"]
["Added Clear Cache button (use on any database changes)"]
[]
["Version 43 changes","2016-05-19","Onno Paap"]
["Changed non-existing super classes to show as \"no label\""]
[]
["Version 42 changes","2016-05-02","Onno Paap"]
["bug fix"]
[]
["Version 41 changes","2016-05-02","Onno Paap"]
["Added setting to show/not show deprecated items. If shown, they are stricken through"]
[]
["Version 40 changes","2016-03-31","Onno Paap"]
["Added  in doubles: two classes having the same label."]
[]
["Version 39 changes","2016-03-21","Onno Paap"]
["Made the query more robust, after the server hass been returning a 404 occasionally"]
[]
["Version 38 changes","2016-03-03","Onno Paap"]
["Repaired bug entity type query on PCA endpoint"]
[]
["Version 37 changes","2016-01-29","Onno Paap"]
["Showing deprecated class in taxonomy with label in strikethrough."]
[]
["Version 36 changes","2016-01-13","Onno Paap"]
["Added the 17 endpoints of http://data.15926.org/rdl"]
[]
["Version 35 changes","2016-01-13","Onno Paap"]
["In taxonomy view, disregard all rdf:type that is not data model.  So only show rdf:type that is dm:"]
[]
["Version 34 changes","2016-01-13","Onno Paap"]
["Solved taxonomy levels regression bug"]
[]
["Version 33 changes","2016-01-11","Onno Paap"]
["Enhanced the doubled query. First 4 columns are about the triple, the rest is info."]
[]
["Repaired bug in entity type query."]
[]
["Version 30 changes","2016-01-03","Onno Paap"]
["Repaired entity type query for old PCA RDL. \nRepaired bug in entity type query where a class that has a superclass of the wanted type as well as  of another type became  the start point of a new taxonomy as well as part in the main taxonomy. (read that again)"]
[]
["Version 29 changes","2016-01-02","Onno Paap"]
["Filtered entity filtered taxonomy to only show the filtered entity not subClassOf of another entity"]
[]
["Version 27 changes","2016-01-01","Onno Paap"]
["few bugs repaired.  Changed entity search into presenting taxonomies. "]
[]
["Version 26 changes","2015-12-26","Onno Paap"]
["few bugs repaired. "]
[]
["Version 25 changes","2015-12-26","Onno Paap"]
["Added Part 12 and localhost endpoints"]
["Added button for selecting double labels and definitions. "]
["Version 24 changes","2015-12-14","Onno Paap"]
["Added button to list all distinct entity data types and their counts, and click to show."]
["Added a button to show all orphans that have a rdfs:label"]
["Version 23 changes"]
["Added endpoint posccaesar.org/p4/sparql"]
["Version 22 changes"]
["Added endpoint staging.data.posccaesar.org/rdl"]
[]
["Version 21 changes"]
["Repaired bug where namespace replace was based upon definition instead of class label"]
[]
["Version 20 changes"]
["Repaired bug where definition did not show up if hyperlink replace was on."]
[]
["Version 19 changes (skip version 16-18)"]
["Settings expanded with persist settings, namespace replacer and hyperlink replacer"]
["Added namespace replacer which will replace the RDL: namespace of the ID with the namespace given in the list on the front page."]
["Added hyperlink replacer which will find terms between single quotes and look them up in the RDL, then add a hyperlink in the text if found. Anchor tag <a></a> used not &hyperlink() so looks ugly."]
[]
["Version 15 changes"]
["Changed browser page Action buttons to hyperlinks because buttons are not equally spaced between Excel versions (Office 2007 versus Office 365)"]
["First row is empty. Move all up."]
["Make stop button for during query taxonomy query execution"]
[]
[]
["Version 14 changes"]
["Aligned buttons on browser page"]
["Made color notification work. Note: switch it on first in settings. Default is off"]
["Top align subclasses in taxonomy"]
["Subclasses made to hyperlink in taxonomy"]
["Subclasses made to increase column width in taxonomy"]
["Made browser search go when hitting enter in search field"]
[]
[]
[]
["todo"]
["Make setting for outputting to other result pages"]

{"sheet":"Results1","index":3,"n_rows":476,"n_cols":36,"rows_kept":476,"cut":false,"hidden":false,"merged":[[71,31,71,34],[72,31,72,34],[65,30,65,33],[66,31,66,34],[67,31,67,34],[68,31,68,34],[69,31,69,34],[70,31,70,34],[72,23,72,24],[66,25,66,30],[67,25,67,30],[68,25,68,30],[69,25,69,30],[70,25,70,30],[71,25,71,30],[72,25,72,30],[475,21,475,22],[475,15,475,20],[475,23,475,28],[475,29,475,32],[65,16,65,21],[66,17,66,22],[67,17,67,22],[68,17,68,22],[69,17,69,22],[70,17,70,22],[473,22,473,23],[473,16,473,21],[473,24,473,29],[473,30,473,33],[474,22,474,23],[474,16,474,21],[474,24,474,29],[474,30,474,33],[471,21,471,22],[471,15,471,20],[471,23,471,28],[471,29,471,32],[472,22,472,23],[472,16,472,21],[472,24,472,29],[472,30,472,33],[71,17,71,22],[72,17,72,22],[69,23,69,24],[70,23,70,24],[67,23,67,24],[68,23,68,24],[65,22,65,23],[65,24,65,29],[469,22,469,23],[469,16,469,21],[469,24,469,29],[469,30,469,33],[470,22,470,23],[470,16,470,21],[470,24,470,29],[470,30,470,33],[467,23,467,24],[467,17,467,22],[467,25,467,30],[467,31,467,34],[468,22,468,23],[468,16,468,21],[468,24,468,29],[468,30,468,33],[465,21,465,22],[465,15,465,20],[465,23,465,28],[465,29,465,32],[466,22,466,23],[466,16,466,21],[466,24,466,29],[466,30,466,33],[463,23,463,24],[463,17,463,22],[463,25,463,30],[463,31,463,34],[464,22,464,23],[464,16,464,21],[464,24,464,29],[464,30,464,33],[461,24,461,25],[461,18,461,23],[461,26,461,31],[461,32,461,35],[462,24,462,25],[462,18,462,23],[462,26,462,31],[462,32,462,35],[459,24,459,25],[459,18,459,23],[459,26,459,31],[459,32,459,35],[460,24,460,25],[460,18,460,23],[460,26,460,31],[460,32,460,35],[457,24,457,25],[457,18,457,23],[457,26,457,31],[457,32,457,35],[458,24,458,25],[458,18,458,23],[458,26,458,31],[458,32,458,35],[455,24,455,25],[455,18,455,23],[455,26,455,31],[455,32,455,35],[456,24,456,25],[456,18,456,23],[456,26,456,31],[456,32,456,35],[453,23,453,24],[453,17,453,22],[453,25,453,30],[453,31,453,34],[454,24,454,25],[454,18,454,23],[454,26,454,31],[454,32,454,35],[451,22,451,23],[451,16,451,21],[451,24,451,29],[451,30,451,33],[452,22,452,23],[452,16,452,21],[452,24,452,29],[452,30,452,33],[449,27,449,28],[449,21,449,26],[449,29,449,34],[449,35,449,38],[450,26,450,27],[450,20,450,25],[450,28,450,33],[450,34,450,37],[447,25,447,26],[447,19,447,24],[447,27,447,32],[447,33,447,36],[448,26,448,27],[448,20,448,25],[448,28,448,33],[448,34,448,37],[445,24,445,25],[445,18,445,23],[445,26,445,31],[445,32,445,35],[446,24,446,25],[446,18,446,23],[446,26,446,31],[446,32,446,35],[443,24,443,25],[443,18,443,23],[443,26,443,31],[443,32,443,35],[444,24,444,25],[444,18,444,23],[444,26,444,31],[444,32,444,35],[441,24,441,25],[441,18,441,23],[441,26,441,31],[441,32,441,35],[442,23,442,24],[442,17,442,22],[442,25,442,30],[442,31,442,34],[439,24,439,25],[439,18,439,23],[439,26,439,31],[439,32,439,35],[440,24,440,25],[440,18,440,23],[440,26,440,31],[440,32,440,35],[437,24,437,25],[437,18,437,23],[437,26,437,31],[437,32,437,35],[438,24,438,25],[438,18,438,23],[438,26,438,31],[438,32,438,35],[435,23,435,24],[435,17,435,22],[435,25,435,30],[435,31,435,34],[436,24,436,25],[436,18,436,23],[436,26,436,31],[436,32,436,35],[433,24,433,25],[433,18,433,23],[433,26,433,31],[433,32,433,35],[434,24,434,25],[434,18,434,23],[434,26,434,31],[434,32,434,35],[431,24,431,25],[431,18,431,23],[431,26,431,31],[431,32,431,35],[432,24,432,25],[432,18,432,23],[432,26,432,31],[432,32,432,35],[429,24,429,25],[429,18,429,23],[429,26,429,31],[429,32,429,35],[430,25,430,26],[430,19,430,24],[430,27,430,32],[430,33,430,36],[427,24,427,25],[427,18,427,23],[427,26,427,31],[427,32,427,35],[428,24,428,25],[428,18,428,23],[428,26,428,31],[428,32,428,35],[425,24,425,25],[425,18,425,23],[425,26,425,31],[425,32,425,35],[426,24,426,25],[426,18,426,23],[426,26,426,31],[426,32,426,35],[423,23,423,24],[423,17,423,22],[423,25,423,30],[423,31,423,34],[424,23,424,24],[424,17,424,22],[424,25,424,30],[424,31,424,34],[421,23,421,24],[421,17,421,22],[421,25,421,30],[421,31,421,34],[422,23,422,24],[422,17,422,22],[422,25,422,30],[422,31,422,34],[419,23,419,24],[419,17,419,22],[419,25,419,30],[419,31,419,34],[420,22,420,23],[420,16,420,21],[420,24,420,29],[420,30,420,33],[417,25,417,26],[417,19,417,24],[417,27,417,32],[417,33,417,36],[418,24,418,25],[418,18,418,23],[418,26,418,31],[418,32,418,35],[415,23,415,24],[415,17,415,22],[415,25,415,30],[415,31,415,34],[416,24,416,25],[416,18,416,23],[416,26,416,31],[416,32,416,35],[413,23,413,24],[413,17,413,22],[413,25,413,30],[413,31,413,34],[414,23,414,24],[414,17,414,22],[414,25,414,30],[414,31,414,34],[411,23,411,24],[411,17,411,22],[411,25,411,30],[411,31,411,34],[412,23,412,24],[412,17,412,22],[412,25,412,30],[412,31,412,34],[409,22,409,23],[409,16,409,21],[409,24,409,29],[409,30,409,33],[410,22,410,23],[410,16,410,21],[410,24,410,29],[410,30,410,33],[407,23,407,24],[407,17,407,22],[407,25,407,30],[407,31,407,34],[408,22,408,23],[408,16,408,21],[408,24,408,29],[408,30,408,33],[405,23,405,24],[405,17,405,22],[405,25,405,30],[405,31,405,34],[406,23,406,24],[406,17,406,22],[406,25,406,30],[406,31,406,34],[403,23,403,24],[403,17,403,22],[403,25,403,30],[403,31,403,34],[404,23,404,24],[404,17,404,22],[404,25,404,30],[404,31,404,34],[401,23,401,24],[401,17,401,22],[401,25,401,30],[401,31,401,34],[402,23,402,24],[402,17,402,22],[402,25,402,30],[402,31,402,34],[399,23,399,24],[399,17,399,22],[399,25,399,30],[399,31,399,34],[400,23,400,24],[400,17,400,22],[400,25,400,30],[400,31,400,34],[397,23,397,24],[397,17,397,22],[397,25,397,30],[397,31,397,34],[398,22,398,23],[398,16,398,21],[398,24,398,29],[398,30,398,33],[395,24,395,25],[395,18,395,23],[395,26,395,31],[395,32,395,35],[396,23,396,24],[396,17,396,22],[396,25,396,30],[396,31,396,34],[393,22,393,23],[393,16,393,21],[393,24,393,29],[393,30,393,33],[394,23,394,24],[394,17,394,22],[394,25,394,30],[394,31,394,34],[391,23,391,24],[391,17,391,22],[391,25,391,30],[391,31,391,34],[392,23,392,24],[392,17,392,22],[392,25,392,30],[392,31,392,34],[389,23,389,24],[389,17,389,22],[389,25,389,30],[389,31,389,34],[390,22,390,23],[390,16,390,21],[390,24,390,29],[390,30,390,33],[387,23,387,24],[387,17,387,22],[387,25,387,30],[387,31,387,34],[388,23,388,24],[388,17,388,22],[388,25,388,30],[388,31,388,34],[385,23,385,24],[385,17,385,22],[385,25,385,30],[385,31,385,34],[386,23,386,24],[386,17,386,22],[386,25,386,30],[386,31,386,34],[383,22,383,23],[383,16,383,21],[383,24,383,29],[383,30,383,33],[384,23,384,24],[384,17,384,22],[384,25,384,30],[384,31,384,34],[381,26,381,27],[381,20,381,25],[381,28,381,33],[381,34,381,37],[382,25,382,26],[382,19,382,24],[382,27,382,32],[382,33,382,36],[379,26,379,27],[379,20,379,25],[379,28,379,33],[379,34,379,37],[380,26,380,27],[380,20,380,25],[380,28,380,33],[380,34,380,37],[377,26,377,27],[377,20,377,25],[377,28,377,33],[377,34,377,37],[378,25,378,26],[378,19,378,24],[378,27,378,32],[378,33,378,36],[375,26,375,27],[375,20,375,25],[375,28,375,33],[375,34,375,37],[376,26,376,27],[376,20,376,25],[376,28,376,33],[376,34,376,37],[373,25,373,26],[373,19,373,24],[373,27,373,32],[373,33,373,36],[374,25,374,26],[374,19,374,24],[374,27,374,32],[374,33,374,36],[371,25,371,26],[371,19,371,24],[371,27,371,32],[371,33,371,36],[372,25,372,26],[372,19,372,24],[372,27,372,32],[372,33,372,36],[369,25,369,26],[369,19,369,24],[369,27,369,32],[369,33,369,36],[370,25,370,26],[370,19,370,24],[370,27,370,32],[370,33,370,36],[367,24,367,25],[367,18,367,23],[367,26,367,31],[367,32,367,35],[368,24,368,25],[368,18,368,23],[368,26,368,31],[368,32,368,35],[365,26,365,27],[365,20,365,25],[365,28,365,33],[365,34,365,37],[366,26,366,27],[366,20,366,25],[366,28,366,33],[366,34,366,37],[363,25,363,26],[363,19,363,24],[363,27,363,32],[363,33,363,36],[364,26,364,27],[364,20,364,25],[364,28,364,33],[364,34,364,37],[361,25,361,26],[361,19,361,24],[361,27,361,32],[361,33,361,36],[362,24,362,25],[362,18,362,23],[362,26,362,31],[362,32,362,35],[359,24,359,25],[359,18,359,23],[359,26,359,31],[359,32,359,35],[360,24,360,25],[360,18,360,23],[360,26,360,31],[360,32,360,35],[357,24,357,25],[357,18,357,23],[357,26,357,31],[357,32,357,35],[358,25,358,26],[358,19,358,24],[358,27,358,32],[358,33,358,36],[355,25,355,26],[355,19,355,24],[355,27,355,32],[355,33,355,36],[356,25,356,26],[356,19,356,24],[356,27,356,32],[356,33,356,36],[353,24,353,25],[353,18,353,23],[353,26,353,31],[353,32,353,35],[354,25,354,26],[354,19,354,24],[354,27,354,32],[354,33,354,36],[351,26,351,27],[351,20,351,25],[351,28,351,33],[351,34,351,37],[352,24,352,25],[352,18,352,23],[352,26,352,31],[352,32,352,35],[349,25,349,26],[349,19,349,24],[349,27,349,32],[349,33,349,36],[350,26,350,27],[350,20,350,25],[350,28,350,33],[350,34,350,37],[347,25,347,26],[347,19,347,24],[347,27,347,32],[347,33,347,36],[348,25,348,26],[348,19,348,24],[348,27,348,32],[348,33,348,36],[345,24,345,25],[345,18,345,23],[345,26,345,31],[345,32,345,35],[346,25,346,26],[346,19,346,24],[346,27,346,32],[346,33,346,36],[343,25,343,26],[343,19,343,24],[343,27,343,32],[343,33,343,36],[344,25,344,26],[344,19,344,24],[344,27,344,32],[344,33,344,36],[341,25,341,26],[341,19,341,24],[341,27,341,32],[341,33,341,36],[342,25,342,26],[342,19,342,24],[342,27,342,32],[342,33,342,36],[339,25,339,26],[339,19,339,24],[339,27,339,32],[339,33,339,36],[340,25,340,26],[340,19,340,24],[340,27,340,32],[340,33,340,36],[337,24,337,25],[337,18,337,23],[337,26,337,31],[337,32,337,35],[338,25,338,26],[338,19,338,24],[338,27,338,32],[338,33,338,36],[335,27,335,28],[335,21,335,26],[335,29,335,34],[335,35,335,38],[336,27,336,28],[336,21,336,26],[336,29,336,34],[336,35,336,38],[333,26,333,27],[333,20,333,25],[333,28,333,33],[333,34,333,37],[334,27,334,28],[334,21,334,26],[334,29,334,34],[334,35,334,38],[331,26,331,27],[331,20,331,25],[331,28,331,33],[331,34,331,37],[332,26,332,27],[332,20,332,25],[332,28,332,33],[332,34,332,37],[329,25,329,26],[329,19,329,24],[329,27,329,32],[329,33,329,36],[330,25,330,26],[330,19,330,24],[330,27,330,32],[330,33,330,36],[327,26,327,27],[327,20,327,25],[327,28,327,33],[327,34,327,37],[328,25,328,26],[328,19,328,24],[328,27,328,32],[328,33,328,36],[325,25,325,26],[325,19,325,24],[325,27,325,32],[325,33,325,36],[326,25,326,26],[326,19,326,24],[326,27,326,32],[326,33,326,36],[323,24,323,25],[323,18,323,23],[323,26,323,31],[323,32,323,35],[324,25,324,26],[324,19,324,24],[324,27,324,32],[324,33,324,36],[321,24,321,25],[321,18,321,23],[321,26,321,31],[321,32,321,35],[322,24,322,25],[322,18,322,23],[322,26,322,31],[322,32,322,35],[319,24,319,25],[319,18,319,23],[319,26,319,31],[319,32,319,35],[320,24,320,25],[320,18,320,23],[320,26,320,31],[320,32,320,35],[317,23,317,24],[317,17,317,22],[317,25,317,30],[317,31,317,34],[318,24,318,25],[318,18,318,23],[318,26,318,31],[318,32,318,35],[315,23,315,24],[315,17,315,22],[315,25,315,30],[315,31,315,34],[316,23,316,24],[316,17,316,22],[316,25,316,30],[316,31,316,34],[313,23,313,24],[313,17,313,22],[313,25,313,30],[313,31,313,34],[314,23,314,24],[314,17,314,22],[314,25,314,30],[314,31,314,34],[311,23,311,24],[311,17,311,22],[311,25,311,30],[311,31,311,34],[312,24,312,25],[312,18,312,23],[312,26,312,31],[312,32,312,35],[309,23,309,24],[309,17,309,22],[309,25,309,30],[309,31,309,34],[310,23,310,24],[310,17,310,22],[310,25,310,30],[310,31,310,34],[307,25,307,26],[307,19,307,24],[307,27,307,32],[307,33,307,36],[308,23,308,24],[308,17,308,22],[308,25,308,30],[308,31,308,34],[305,25,305,26],[305,19,305,24],[305,27,305,32],[305,33,305,36],[306,25,306,26],[306,19,306,24],[306,27,306,32],[306,33,306,36],[303,25,303,26],[303,19,303,24],[303,27,303,32],[303,33,303,36],[304,25,304,26],[304,19,304,24],[304,27,304,32],[304,33,304,36],[301,25,301,26],[301,19,301,24],[301,27,301,32],[301,33,301,36],[302,25,302,26],[302,19,302,24],[302,27,302,32],[302,33,302,36],[299,25,299,26],[299,19,299,24],[299,27,299,32],[299,33,299,36],[300,25,300,26],[300,19,300,24],[300,27,300,32],[300,33,300,36],[297,26,297,27],[297,20,297,25],[297,28,297,33],[297,34,297,37],[298,26,298,27],[298,20,298,25],[298,28,298,33],[298,34,298,37],[295,25,295,26],[295,19,295,24],[295,27,295,32],[295,33,295,36],[296,26,296,27],[296,20,296,25],[296,28,296,33],[296,34,296,37],[293,25,293,26],[293,19,293,24],[293,27,293,32],[293,33,293,36],[294,25,294,26],[294,19,294,24],[294,27,294,32],[294,33,294,36],[291,25,291,26],[291,19,291,24],[291,27,291,32],[291,33,291,36],[292,25,292,26],[292,19,292,24],[292,27,292,32],[292,33,292,36],[289,24,289,25],[289,18,289,23],[289,26,289,31],[289,32,289,35],[290,25,290,26],[290,19,290,24],[290,27,290,32],[290,33,290,36],[287,24,287,25],[287,18,287,23],[287,26,287,31],[287,32,287,35],[288,24,288,25],[288,18,288,23],[288,26,288,31],[288,32,288,35],[285,24,285,25],[285,18,285,23],[285,26,285,31],[285,32,285,35],[286,24,286,25],[286,18,286,23],[286,26,286,31],[286,32,286,35],[283,24,283,25],[283,18,283,23],[283,26,283,31],[283,32,283,35],[284,24,284,25],[284,18,284,23],[284,26,284,31],[284,32,284,35],[281,25,281,26],[281,19,281,24],[281,27,281,32],[281,33,281,36],[282,25,282,26],[282,19,282,24],[282,27,282,32],[282,33,282,36],[279,25,279,26],[279,19,279,24],[279,27,279,32],[279,33,279,36],[280,25,280,26],[280,19,280,24],[280,27,280,32],[280,33,280,36],[277,24,277,25],[277,18,277,23],[277,26,277,31],[277,32,277,35],[278,25,278,26],[278,19,278,24],[278,27,278,32],[278,33,278,36],[275,24,275,25],[275,18,275,23],[275,26,275,31],[275,32,275,35],[276,23,276,24],[276,17,276,22],[276,25,276,30],[276,31,276,34],[273,24,273,25],[273,18,273,23],[273,26,273,31],[273,32,273,35],[274,24,274,25],[274,18,274,23],[274,26,274,31],[274,32,274,35],[271,25,271,26],[271,19,271,24],[271,27,271,32],[271,33,271,36],[272,25,272,26],[272,19,272,24],[272,27,272,32],[272,33,272,36],[269,25,269,26],[269,19,269,24],[269,27,269,32],[269,33,269,36],[270,25,270,26],[270,19,270,24],[270,27,270,32],[270,33,270,36],[267,25,267,26],[267,19,267,24],[267,27,267,32],[267,33,267,36],[268,25,268,26],[268,19,268,24],[268,27,268,32],[268,33,268,36],[265,25,265,26],[265,19,265,24],[265,27,265,32],[265,33,265,36],[266,25,266,26],[266,19,266,24],[266,27,266,32],[266,33,266,36],[263,25,263,26],[263,19,263,24],[263,27,263,32],[263,33,263,36],[264,25,264,26],[264,19,264,24],[264,27,264,32],[264,33,264,36],[261,25,261,26],[261,19,261,24],[261,27,261,32],[261,33,261,36],[262,25,262,26],[262,19,262,24],[262,27,262,32],[262,33,262,36],[259,25,259,26],[259,19,259,24],[259,27,259,32],[259,33,259,36],[260,25,260,26],[260,19,260,24],[260,27,260,32],[260,33,260,36],[257,24,257,25],[257,18,257,23],[257,26,257,31],[257,32,257,35],[258,24,258,25],[258,18,258,23],[258,26,258,31],[258,32,258,35],[255,24,255,25],[255,18,255,23],[255,26,255,31],[255,32,255,35],[256,24,256,25],[256,18,256,23],[256,26,256,31],[256,32,256,35],[253,24,253,25],[253,18,253,23],[253,26,253,31],[253,32,253,35],[254,24,254,25],[254,18,254,23],[254,26,254,31],[254,32,254,35],[251,24,251,25],[251,18,251,23],[251,26,251,31],[251,32,251,35],[252,24,252,25],[252,18,252,23],[252,26,252,31],[252,32,252,35],[249,24,249,25],[249,18,249,23],[249,26,249,31],[249,32,249,35],[250,24,250,25],[250,18,250,23],[250,26,250,31],[250,32,250,35],[247,24,247,25],[247,18,247,23],[247,26,247,31],[247,32,247,35],[248,24,248,25],[248,18,248,23],[248,26,248,31],[248,32,248,35],[245,25,245,26],[245,19,245,24],[245,27,245,32],[245,33,245,36],[246,25,246,26],[246,19,246,24],[246,27,246,32],[246,33,246,36],[243,25,243,26],[243,19,243,24],[243,27,243,32],[243,33,243,36],[244,25,244,26],[244,19,244,24],[244,27,244,32],[244,33,244,36],[241,24,241,25],[241,18,241,23],[241,26,241,31],[241,32,241,35],[242,25,242,26],[242,19,242,24],[242,27,242,32],[242,33,242,36],[239,25,239,26],[239,19,239,24],[239,27,239,32],[239,33,239,36],[240,26,240,27],[240,20,240,25],[240,28,240,33],[240,34,240,37],[237,25,237,26],[237,19,237,24],[237,27,237,32],[237,33,237,36],[238,26,238,27],[238,20,238,25],[238,28,238,33],[238,34,238,37],[235,25,235,26],[235,19,235,24],[235,27,235,32],[235,33,235,36],[236,25,236,26],[236,19,236,24],[236,27,236,32],[236,33,236,36],[233,25,233,26],[233,19,233,24],[233,27,233,32],[233,33,233,36],[234,24,234,25],[234,18,234,23]],"merged_total":1904,"flags":["merged_cut"]}
[null,null,"FunctionalObject",null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL DEVICE",null,null,null,null,null,"rdl:RDS1407117061",null,"An <ELECTRICAL DEVICE> is a <FunctionalObject> that has the capability of <PARTAKING> in an electrical system",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRICAL DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"ALTERNATING CURRENT DEVICE",null,null,null,null,null,"rdl:RDS1407134441",null,"An <ALTERNATING CURRENT DEVICE> is an <ELECTRICAL DEVICE> that has the capability of <OPERATING> in an alternating current circuit",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRICAL DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"ANODE",null,null,null,null,null,"rdl:RDS781033661",null,"An <ANODE> is an <ELECTRICAL DEVICE> that has a capability of <EMITTING> positive charge carriers to, and/or <RECEIVING> negative charge carriers from, the medium of lower conductivity",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANODE","ARTEFACT",null,null,null,null,null,null,null,null,null,null,null,null,"IMPRESSED CURRENT ANODE",null,null,null,null,null,"rdl:RDS781040881",null,"An <IMPRESSED CURRENT ANODE> is an <ARTEFACT> and an <ANODE> that is capable <PROTECTING> carbon and low-alloy steel equipment or structures against corrosion with impressed current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANODE","ARTEFACT",null,null,null,null,null,null,null,null,null,null,null,null,"SACRIFICIAL ANODE",null,null,null,null,null,"rdl:RDS781048261",null,"A <SACRIFICIAL ANODE> is an <ARTEFACT> and an <ANODE> made of highly active metals that are used to prevent a less active material surface from corroding; they are created from a metal alloy with a more negative electrochemical potential than the other metal it will be used to protect",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL DEVICE",null,null,null,null,null,null,null,null,null,null,null,"ANTI STATIC ARTEFACT",null,null,null,null,null,"rdl:RDS6912022",null,"An <ANTI STATIC ARTEFACT> is an <ARTEFACT> and an <ELECTRICAL DEVICE> intended to provide electric continuity to prevent ignition of flammable fluids",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"CATHODE",null,null,null,null,null,"rdl:RDS5854420",null,"A <CATHODE> is an <ELECTRICAL DEVICE> that is capable of <EMITTING> negative charge carriers and/or receiving positive charge carriers from the medium of lower conductivity",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRICAL DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"DIRECT CURRENT DEVICE",null,null,null,null,null,"rdl:RDS1407135641",null,"A <DIRECT CURRENT DEVICE> is an <ELECTRICAL DEVICE> that has the capability of <OPERATING> in an direct current circuit",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","ELECTRICAL DEVICE",null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL APPARATUS",null,null,null,null,null,"rdl:RDS497678601",null,"An <ELECTRICAL APPARATUS> is an <ARTEFACT> and an <ELECTRICAL DEVICE>, applied as a whole or in part for the utilization of electrical energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS463994",null,"A <CIRCUIT BREAKER> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE> that at regular intervals interrupts an electric current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876239",null,"An <AIR CIRCUIT BREAKER> is a <CIRCUIT BREAKER> in which the contacts open and close in air at atmospheric pressure.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AIR CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTH LEAKAGE CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876509",null,"An <EARTH LEAKAGE CIRCUIT BREAKER> is an <AIR CIRCUIT BREAKER> intended to break the supply in the event of an earth fault being detected.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EARTH LEAKAGE CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESIDUAL CURRENT CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876644",null,"A <RESIDUAL CURRENT CIRCUIT BREAKER> is an <EARTH LEAKAGE CIRCUIT BREAKER> in which the earth fault is detected by an imbalance in the current in the phase and neutral conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AIR CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MINIATURE CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876554",null,"A <MINIATURE CIRCUIT BREAKER> is an <AIR CIRCUIT BREAKER> intended for low power low voltage installations.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AIR CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOULDED-CASE CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876599",null,"An <MOULDED-CASE CIRCUIT BREAKER> is an <AIR CIRCUIT BREAKER> having a supporting housing of moulded insulating material forming an integral part of the <CIRCUIT BREAKER>.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CIRCUIT BREAKER WITH LOCK-OUT PREVENTING CLOSING",null,null,null,null,null,"rdl:RDS913814",null,"A <CIRCUIT BREAKER WITH LOCK-OUT PREVENTING CLOSING> is a <CIRCUIT BREAKER> in which none of the moving contacts can make current if the closing command is initiated while the conditions which should cause the opening operation remain established.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT-LIMITING CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS913724",null,"A <CURRENT-LIMITING CIRCUIT BREAKER> is a <CIRCUIT BREAKER> with a break-time short enough to prevent the short circuit current reaching its otherwise attainable peak value.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DEAD TANK CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS913679",null,"A <DEAD TANK CIRCUIT BREAKER> is a <CIRCUIT BREAKER> with interrupters in an earthed metal tank.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS-BLAST CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS913544",null,"A <GAS-BLAST CIRCUIT BREAKER> is a <CIRCUIT BREAKER> in which the arc develops in a blast of gas.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS-BLAST CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR-BLAST CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876284",null,"An <AIR-BLAST CIRCUIT BREAKER> is a <GAS-BLAST CIRCUIT BREAKER> in which the gas used is air.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRALLY FUSED CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS913769",null,"An <INTEGRALLY FUSED CIRCUIT BREAKER> is a <CIRCUIT BREAKER> that is a combination, in a single device, of A <CIRCUIT BREAKER> and fuses, one fuse being placed in series with each pole of the circuit breaker intended to be connected to a phase conductor.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIVE TANK CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS913634",null,"A <LIVE TANK CIRCUIT BREAKER> is a <CIRCUIT BREAKER> with interrupters in a tank insulated from earth.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OIL CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876329",null,"An <OIL CIRCUIT BREAKER> is a <CIRCUIT BREAKER> in which the contacts open and close in oil.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SF6 CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876419",null,"An <SF6 CIRCUIT BREAKER> is a <CIRCUIT BREAKER> in which the contacts open and close in sulphur hexafluoride.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VACUUM CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876464",null,"A <VACUUM CIRCUIT BREAKER> is a <CIRCUIT BREAKER> in which the contacts open and close within a highly evacuated envelope.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"CONTACTOR",null,null,null,null,null,"rdl:RDS464039",null,"A <CONTACTOR> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE> having only one position of rest, operated otherwise than by hand, capable of making, carrying and breaking currents under normal circuit conditions including operating overload conditions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTACTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR CONTACTOR",null,null,null,null,null,"rdl:RDS876734",null,"An <AIR CONTACTOR> is a <CONTACTOR> that has its contacts in air.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","CONTACTOR","RELAY",null,null,null,null,null,null,null,null,null,null,null,null,"CONTACTOR RELAY",null,null,null,null,null,"rdl:RDS935189",null,"A <CONTACTOR RELAY> is an <ARTEFACT> and a <RELAY> and a <CONTACTOR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTACTOR RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTANTANEOUS CONTACTOR RELAY",null,null,null,null,null,"rdl:RDS935234",null,"An <INSTANTANEOUS CONTACTOR RELAY> is a <CONTACTOR RELAY> operating without any intentional time delay.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTACTOR RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TIME-DELAY CONTACTOR RELAY",null,null,null,null,null,"rdl:RDS935279",null,"A <TIME-DELAY CONTACTOR RELAY> is a <CONTACTOR RELAY> with specified time-delay characteristics.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTACTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LATCHED CONTACTOR",null,null,null,null,null,"rdl:RDS935144",null,"A <LATCHED CONTACTOR> is a <CONTACTOR>, the moving elements of which are prevented by means of a latching arrangement from returning to the position of rest when the operating means are de-energized.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTACTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VACUUM CONTACTOR",null,null,null,null,null,"rdl:RDS876779",null,"A <VACUUM CONTACTOR> is a <CONTACTOR> that make/break electrical contacts inside a sealed vacuum interrupter called a vacuum bottle.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"DISCONNECTOR",null,null,null,null,null,"rdl:RDS934559",null,"A <DISCONNECTOR> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE> that provides, in the open position, an isolating distance in accordance with specified requirements",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CENTRE-BREAK DISCONNECTOR",null,null,null,null,null,"rdl:RDS934694",null,"A <CENTRE-BREAK DISCONNECTOR> is a <DISCONNECTOR> in which both contacts of each pole are movable and engage at a point substantially midway between their supports.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DISCONNECTOR FUSE",null,null,null,null,null,"rdl:RDS934919",null,"A <DISCONNECTOR FUSE> is a <DISCONNECTOR> in which one or more poles have a fuse in series in a composite unit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIVIDED SUPPORT DISCONNECTOR",null,null,null,null,null,"rdl:RDS934604",null,"A <DIVIDED SUPPORT DISCONNECTOR> is a <DISCONNECTOR> in which the fixed and moving contacts of each pole are not supported by a common base or frame.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE-BREAK DISCONNECTOR",null,null,null,null,null,"rdl:RDS934739",null,"A <DOUBLE-BREAK DISCONNECTOR> is a <DISCONNECTOR> that opens a circuit at two points.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTHING SWITCH",null,null,null,null,null,"rdl:RDS876869",null,"An <EARTHING SWITCH> is a <DISCONNECTOR> for earthing parts of a circuit, capable of withstanding for a specified time currents under abnormal conditions such as those of short circuit, but not required to carry current under normal conditions of the circuit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EARTHING SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIVIDED SUPPORT EARTHING SWITCH",null,null,null,null,null,"rdl:RDS934649",null,"A <DIVIDED SUPPORT EARTHING SWITCH> is an <EARTHING SWITCH> in which the fixed and moving contacts of each pole are not supported by a common base or frame.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FUSE-DISCONNECTOR",null,null,null,null,null,"rdl:RDS935054",null,"A <FUSE-DISCONNECTOR> is a <DISCONNECTOR> in which a fuse-link or a fuse-carrier with fuse-link forms the moving contact.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAGNETIC DOOR CLOSER RELEASE",null,null,null,null,null,"rdl:RDS1299240441",null,"A <MAGNETIC DOOR CLOSER RELEASE> is a <DISCONNECTOR> that switches off the current to a magnetic door shutter so that the door closes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","ELECTRICAL APPARATUS","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC ACTUATOR",null,null,null,null,null,"rdl:RDS430379",null,"An <ELECTRIC ACTUATOR> is an <INSTRUMENTATION ITEM> and an <ELECTRICAL APPARATUS> and a <CONTROLLED ACTUATOR> that produces a specified movement when actuated by electrical energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC ACTUATOR WITH HANDWHEEL",null,null,null,null,null,"rdl:RDS11507710",null,"An <ELECTRIC ACTUATOR WITH HANDWHEEL> is an <ELECTRIC ACTUATOR> with a handwheel for operating the valve manually",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ACTUATOR","HYDRAULIC ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC HYDRAULIC ACTUATOR",null,null,null,null,null,"rdl:RDS7195780",null,"An <ELECTRIC HYDRAULIC ACTUATOR> is an <ELECTRIC ACTUATOR> and a <HYDRAULIC ACTUATOR> having a fluid pump driven by an electric motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC HYDRAULIC ACTUATOR","VALVE ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRO-HYDRAULIC VALVE ACTUATOR",null,null,null,null,null,"rdl:RDS16742011",null,"An <ELECTRO-HYDRAULIC VALVE ACTUATOR> is a <VALVE ACTUATOR> and a <ELECTRIC HYDRAULIC ACTUATOR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ACTUATOR","VALVE ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC VALVE ACTUATOR",null,null,null,null,null,"rdl:RDS7028560",null,"An <ELECTRIC VALVE ACTUATOR> is an <ELECTRIC ACTUATOR> and a <VALVE ACTUATOR> that is a valve actuator that is intended to be driven by an electric motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLENOID ACTUATOR",null,null,null,null,null,"rdl:RDS7191376",null,"A <SOLENOID ACTUATOR> is an <ELECTRIC ACTUATOR> that is utilizing a continuous duty linear solenoid to convert electrical energy into mechanical power via a plunger with an axial stroke in either a push or pull action",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLENOID ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DUAL SOLENOID ACTUATOR",null,null,null,null,null,"rdl:RDS7191440",null,"A <DUAL SOLENOID ACTUATOR> is a <SOLENOID ACTUATOR> with two solenoids that are energized one at a time, each causing a move in an opposite direction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLENOID ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PILOT AIR OPERATED SOLENOID ACTUATOR",null,null,null,null,null,"rdl:RDS7191609",null,"A <PILOT AIR OPERATED SOLENOID ACTUATOR> is a <SOLENOID ACTUATOR> in which operation is boosted by an external supply of pilot air",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLENOID ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE SOLENOID ACTUATOR",null,null,null,null,null,"rdl:RDS7191502",null,"A <SINGLE SOLENOID ACTUATOR> is a <SOLENOID ACTUATOR> with one solenoid where the two opposite positions are for energized vs de-energized",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC POWER SUPPLY","ELECTRICAL APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,"rdl:RDS860129",null,"A <ELECTRIC ELECTRIC POWER SUPPLY UNIT> is an <ELECTRICAL APPARATUS> and an <ELECTRIC POWER SUPPLY> for the supply of electric power according to specified levels and tolerances",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AC POWER SUPPLY","ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,"AC ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,"rdl:RDS874619",null,"An <AC ELECTRIC POWER SUPPLY UNIT> is a <ELECTRIC POWER SUPPLY UNIT> and an <AC POWER SUPPLY> with Alternate Current output",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AC ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONDITIONED AC POWER SUPPLY UNIT",null,null,null,null,null,"rdl:RDS6233595",null,"A <CONDITIONED AC POWER SUPPLY UNIT> is an <AC POWER SUPPLY UNIT> in which the output meets strict tolerances. Typically waveform, frequency and voltage restrictions.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AC ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UPS UNIT",null,null,null,null,null,"rdl:RDS874754",null,"A <UPS UNIT> is an <AC POWER SUPPLY UNIT> that maintains a uninterrupted supply of electric power to the equipment it protects.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"UPS UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OFF-LINE UPS",null,null,null,null,null,"rdl:RDS874799",null,"An <OFF-LINE UPS> is a <UPS UNIT> supplying the load via a bypass circuit having a fast-acting static switch to switch to the battery/inverter in the event of mains failure.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"UPS UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ON-LINE UPS",null,null,null,null,null,"rdl:RDS874844",null,"An <ON-LINE UPS> is a <UPS UNIT> supplying the load through a charger/inverter during normal operation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DC POWER SUPPLY","ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,"DC ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,"rdl:RDS874664",null,"A <DC ELECTRIC POWER SUPPLY UNIT> is a <ELECTRIC POWER SUPPLY UNIT> and a <DC POWER SUPPLY> with Direct Current output",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DC ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BATTERY BACK-UP POWER SUPPLY UNIT",null,null,null,null,null,"rdl:RDS874889",null,"A <BATTERY BACK-UP POWER SUPPLY UNIT> is a <DC POWER SUPPLY UNIT> that provides an uninterrupted supply to a load in the event of a main supply failure.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DC ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BATTERY CHARGER",null,null,null,null,null,"rdl:RDS874934",null,"A <BATTERY CHARGER> is a <DIRECT CURRENT POWER SUPPLY UNIT> for charging batteries.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DC ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STABILISED DC POWER SUPPLY UNIT",null,null,null,null,null,"rdl:RDS874979",null,"A <STABILISED DC POWER SUPPLY UNIT> is a <DC POWER SUPPLY UNIT> intended to supply stabilised d.c. electric power according to specified levels and tolerances.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INTERNAL ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,"rdl:RDS6810190",null,"An <INTERNAL ELECTRIC POWER SUPPLY UNIT> is a <ELECTRIC POWER SUPPLY UNIT> that is an arrangement for delivering power to internal functions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT BOARD","INTERNAL ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER SUPPLY CARD",null,null,null,null,null,"rdl:RDS5784219",null,"A <POWER SUPPLY CARD> is an <ELECTRONIC CIRCUIT BOARD> and an <INTERNAL ELECTRIC POWER SUPPLY UNIT> that is a power supply arranged on an electronic circuit board",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","TIMER",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC TIMER",null,null,null,null,null,"rdl:RDS6590405",null,"An <ELECTRIC TIMER> is a <TIMER> and an <ELECTRICAL APPARATUS> that is electrically powered/",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DRAWWORKS","ELECTRICAL APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL DRAWWORKS",null,null,null,null,null,"rdl:RDS1287864381",null,"An <ELECTRICAL DRAWWORKS> is a <DRAWWORKS> and an <ELECTRICAL APPARATUS> that is operated by electrical power",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","INSTRUMENTATION ITEM","TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL TRANSMITTER",null,null,null,null,null,"rdl:RDS1455527751",null,"An <ELECTRICAL TRANSMITTER> is an <INSTRUMENTATION ITEM> and a <TRANSMITTER> and an <ELECTRICAL APPARATUS>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC MODULE",null,null,null,null,null,"rdl:RDS7055701",null,"An <ELECTRONIC MODULE> is an <ELECTRICAL APPARATUS> that is an assembly of electronic components housed in a special container",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC MODULE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALARM ELECTRONIC MODULE",null,null,null,null,null,"rdl:RDS7055882",null,"An <ALARM ELECTRONIC MODULE> is an <ELECTRONIC MODULE> capable of alarm handling",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC MODULE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INPUT MODULE",null,null,null,null,null,"rdl:RDS5773720",null,"An <INPUT MODULE> is an <ELECTRONIC MODULE> for input functions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC MODULE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INTERFACE MODULE",null,null,null,null,null,"rdl:RDS5773782",null,"An <INTERFACE MODULE> is an <ELECTRONIC MODULE> for interface functions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC MODULE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OUTPUT MODULE",null,null,null,null,null,"rdl:RDS5773844",null,"An <OUTPUT MODULE> is an <ELECTRONIC MODULE> for output functions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC MODULE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA ELECTRONIC MODULE",null,null,null,null,null,"rdl:RDS16700516",null,"A <SUBSEA ELECTRONIC MODULE> is an <ELECTRONIC MODULE> that is housed in a special container housing the operating system of the subsea control module",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC MODULE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TOPSIDE ELECTRONIC MODULE",null,null,null,null,null,"rdl:RDS16700420",null,"A <TOPSIDE ELECTRONIC MODULE> is an <ELECTRONIC MODULE> that is a part of subsea power, communication and control unit on a production platform",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC MODULE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRANSMITTER ELECTRONIC MODULE",null,null,null,null,null,"rdl:RDS428984",null,"A <TRANSMITTER ELECTRONIC MODULE> is an <ELECTRONIC MODULE> that is an assembly of the electronic parts of an transmitter",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","HAZARDOUS AREA APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,"EXPLOSION-PROTECTED ELECTRICAL APPARATUS",null,null,null,null,null,"rdl:RDS1090799",null,"An <EXPLOSION-PROTECTED ELECTRICAL APPARATUS> is an <ELECTRICAL APPARATUS> and a <HAZARDOUS AREA APPARATUS> constructed in such a way as not to produce an ignition of the surrounding explosive atmosphere, under specified conditions.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR","EXPLOSION-PROTECTED ELECTRICAL APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC EX MOTOR",null,null,null,null,null,"rdl:RDS5772282",null,"An <ELECTRIC EX MOTOR> is an <ELECTRIC MOTOR> and an <EXPLOSION-PROTECTED ELECTRICAL APPARATUS> that is designed to be operating in hazardous areas",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALTERNATING CURRENT MOTOR","ELECTRIC EX MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALTERNATING CURRENT EX MOTOR",null,null,null,null,null,"rdl:RDS1454491841",null,"An <ALTERNATING CURRENT EX MOTOR> is an <ELECTRIC EX MOTOR> that operates on Alternating Current.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EXPLOSION-PROTECTED ELECTRICAL APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURIZED ENCLOSURE ELECTRICAL APPARATUS",null,null,null,null,null,"rdl:RDS4976786142",null,"A <PRESSURIZED ENCLOSURE ELECTRICAL APPARATUS> is an <EXPLOSION-PROTECTED ELECTRICAL APPARATUS> into which entry of the external gas atmosphere is prevented by pressurization.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"FIXED TRIP MECHANICAL SWITCHING DEVICE",null,null,null,null,null,"rdl:RDS935729",null,"A <FIXED TRIP MECHANICAL SWITCHING DEVICE> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE> that cannot be released except when it is in the closed position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,null,"FREQUENCY RATED APPARATUS",null,null,null,null,null,"rdl:RDS8970440",null,"A <FREQUENCY RATED APPARATUS> is an <ELECTRICAL APPARATUS> rated for use on a power supply of fixed frequency",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"FUSE-COMBINATION UNIT",null,null,null,null,null,"rdl:RDS934514",null,"A <FUSE-COMBINATION UNIT> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE> and one or more fuses in a composite unit, assembled by the manufacturer or in accordance with his instructions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"GAS EVOLVING SWITCH",null,null,null,null,null,"rdl:RDS934829",null,"A <GAS EVOLVING SWITCH> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE> in which the gas is evolved and moved by the thermal action of the arc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","HAND-HELD DRILLING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,"HAND-HELD ELECTRIC DRILL",null,null,null,null,null,"rdl:RDS891629",null,"A <HAND-HELD ELECTRIC DRILL> is a <HAND-HELD DRILLING MACHINE> and an <ELECTRICAL APPARATUS> that has electric power supply",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,null,"INGRESS PROTECTED ELECTRICAL APPARATUS",null,null,null,null,null,"rdl:RDS1008224",null,"An <INGRESS PROTECTED ELECTRICAL APPARATUS> is an <ELECTRICAL APPARATUS> equipped with an ingress protection enclosure for protection against the intrusion of solid objects or dust, accidental contact, and water",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,null,"INTRINSICALLY SAFE ELECTRICAL APPARATUS",null,null,null,null,null,"rdl:RDS4976786127",null,"An <INTRINSICALLY SAFE ELECTRICAL APPARATUS> is an <ELECTRICAL APPARATUS> in which all the circuits are intrinsically safe",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE","ELECTRICAL APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,"MOTOR OPERATED VALVE",null,null,null,null,null,"rdl:RDS11142220",null,"A <MOTOR OPERATED VALVE> is an <ACTUATED VALVE> and an <ELECTRICAL APPARATUS> that is opened and closed with a motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"TRIP-FREE MECHANICAL SWITCHING DEVICE",null,null,null,null,null,"rdl:RDS935774",null,"A <TRIP-FREE MECHANICAL SWITCHING DEVICE> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE>, the moving contacts of which return to and remain in the open position when the opening operation is initiated after the initiation of the closing operation, even if the closing command is maintained",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ELEMENT",null,null,null,null,null,"rdl:RDS1293971491",null,"An <ELECTRICAL ELEMENT> is an <ELECTICAL DEVICE> that affects the voltage in the network or current through the network in a particular way",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"BRUSH(electric)",null,null,null,null,null,"rdl:RDS2221030",null,"A <BRUSH(electric)> is an <ARTEFACT> and an <ELECTRICAL ELEMENT> that is a device that conducts current between stationary wires and moving parts, most commonly in a rotating shaft. Typical applications include electric motors, alternators and electric generators",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"BUS DUCT",null,null,null,null,null,"rdl:RDS869039",null,"A <BUS DUCT> is an <ARTEFACT> and an <ELECTRICAL ELEMENT> function and that is an assembly of busbar, bus duct enclosure, busbar insulation mounts etc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"CAPACITOR",null,null,null,null,null,"rdl:RDS869129",null,"A <CAPACITOR> is an <ARTEFACT> and an <ELECTRICAL ELEMENT> function and that stores electricity during part of an operation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAPACITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAPACITOR BANK",null,null,null,null,null,"rdl:RDS1084454",null,"A <CAPACITOR BANK> is an <ARTEFACT> and a <CAPACITOR> that is a number of capacitor units connected so as to act together",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAPACITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAPACITOR ELEMENT",null,null,null,null,null,"rdl:RDS1084319",null,"A <CAPACITOR ELEMENT> is an <ARTEFACT> and a <CAPACITOR> that is consisting essentially of two electrodes separated by a dielectric",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAPACITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAPACITOR INSTALLATION",null,null,null,null,null,"rdl:RDS1084499",null,"A <CAPACITOR INSTALLATION> is an <ARTEFACT> and a <CAPACITOR> that is one or more capacitor banks and their accessories",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAPACITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAPACITOR STACK",null,null,null,null,null,"rdl:RDS1084409",null,"A <CAPACITOR STACK> is an <ARTEFACT> and a <CAPACITOR> that is an assembly of capacitor units connected in series/",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAPACITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAPACITOR UNIT",null,null,null,null,null,"rdl:RDS1084364",null,"A <CAPACITOR UNIT> is an <ARTEFACT> and a <CAPACITOR> that is an assembly of one or more capacitor elements in the same container with terminals brought out",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAPACITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTROLYTIC CAPACITOR",null,null,null,null,null,"rdl:RDS6568835",null,"An <ELECTROLYTIC CAPACITOR> is an <ARTEFACT> and a <CAPACITOR> in which the dielectric consists of an anodically formed oxide film on one or both electrodes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTROLYTIC CAPACITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AC ELECTROLYTIC CAPACITOR",null,null,null,null,null,"rdl:RDS6568910",null,"An <AC ELECTROLYTIC CAPACITOR> is an <ELECTROLYTIC CAPACITOR> specially designed for ac operation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAPACITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER CAPACITOR",null,null,null,null,null,"rdl:RDS1089854",null,"A <POWER CAPACITOR> is an <ARTEFACT> and a <CAPACITOR> intended for use in a power network",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER CAPACITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENERGY STORAGE CAPACITOR",null,null,null,null,null,"rdl:RDS1090169",null,"An <ENERGY STORAGE CAPACITOR> is a <POWER CAPACITOR> intended to store energy and release it within a very short time.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAPACITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SELF-HEALING CAPACITOR",null,null,null,null,null,"rdl:RDS6622803",null,"A <SELF-HEALING CAPACITOR> is an <ARTEFACT> and a <CAPACITOR> of which the electrical properties after local breakdown of the dielectric, are rapidly and essentially restored",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"COMMUTATOR",null,null,null,null,null,"rdl:RDS1005029",null,"A <COMMUTATOR> is an <ARTEFACT> and an <ELECTRICAL ELEMENT> function, usually consisting of a ring of copper segments separated by insulating strips, connected with the armature of a dynamo, which by revolving in contact with the brushes, directs and makes continuous the current produced in the armature coils of the machine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"COMMUTATOR SEGMENT",null,null,null,null,null,"rdl:RDS1005074",null,"A <COMMUTATOR SEGMENT> is an <ARTEFACT> and an <ELECTRICAL ELEMENT> function, that is a conducting member of a commutator, which is connected to the common end of two consecutive sections of a winding",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"CONNECTOR CONTACT",null,null,null,null,null,"rdl:RDS5763462",null,"A <CONNECTOR CONTACT> is an <ARTEFACT> and an <ELECTRICAL ELEMENT> function that mates with a corresponding element to provide an electric path",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONNECTOR CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BIFURCATED CONTACT",null,null,null,null,null,"rdl:RDS962009",null,"A <BIFURCATED CONTACT> is a <CONNECTOR CONTACT> containing forked/branched contact members with one contact point on each branch, designed to improve the reliability of contacting by establishing two conductive paths in parallel",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONNECTOR CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BLADE CONTACT",null,null,null,null,null,"rdl:RDS962054",null,"A <BLADE CONTACT> is a <CONNECTOR CONTACT> that is solid with a rectangular cross-section, usually with a chamfered mating edge",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONNECTOR CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPUTER HARDWARE PORT",null,null,null,null,null,"rdl:RDS892843521",null,"A <COMPUTER HARDWARE PORT> is a <CONNECTOR CONTACT> that provides a physical interface between a computer and other computers or devices",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONNECTOR CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONCENTRIC CONTACT",null,null,null,null,null,"rdl:RDS962144",null,"A <CONCENTRIC CONTACT> is a <CONNECTOR CONTACT> that is a set of coaxial contacts providing independent circuits through a single mechanical assembly",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONNECTOR CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CRIMP CONTACT",null,null,null,null,null,"rdl:RDS962189",null,"A <CRIMP CONTACT> is a <CONNECTOR CONTACT> having a conductor barrel designed to be crimped",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONNECTOR CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIP-SOLDER CONTACT",null,null,null,null,null,"rdl:RDS962234",null,"A <DIP-SOLDER CONTACT> is a <CONNECTOR CONTACT> with a termination intended to be bath-soldered",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONNECTOR CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FEMALE CONTACT",null,null,null,null,null,"rdl:RDS962279",null,"A <FEMALE CONTACT> is a <CONNECTOR CONTACT> intended to make electric engagement on its inner surface for mating with the outer surface of another contact member",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONNECTOR CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FILTER CONTACT",null,null,null,null,null,"rdl:RDS962324",null,"A <FILTER CONTACT> is a <CONNECTOR CONTACT> with filter to discriminate against certain frequencies",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONNECTOR CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MALE CONTACT",null,null,null,null,null,"rdl:RDS5424020",null,"A <MALE CONTACT> is a <CONNECTOR CONTACT> intended to make electrical engagement on its outer surface, and which will enter a female contact",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONNECTOR CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESILIENT CONTACT",null,null,null,null,null,"rdl:RDS962369",null,"A <RESILIENT CONTACT> is a <CONNECTOR CONTACT> having elastic properties to provide a force to its mating part",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RESILIENT CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TUNING FORK CONTACT",null,null,null,null,null,"rdl:RDS962504",null,"A <TUNING FORK CONTACT> is a <RESILIENT CONTACT> having a shape similar to that of a tuning fork, the two arms of which apply contact force in opposite directions.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONNECTOR CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SNAP-ON CONTACT",null,null,null,null,null,"rdl:RDS962414",null,"A <SNAP-ON CONTACT> is a <CONNECTOR CONTACT> in which retention is achieved by means of a deformation of the contact area which provides positive axial location",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONNECTOR CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLDER CONTACT",null,null,null,null,null,"rdl:RDS962459",null,"A <SOLDER CONTACT> is a <CONNECTOR CONTACT> designed for the attachment of the conductor by solder",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONNECTOR CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WRAP CONTACT",null,null,null,null,null,"rdl:RDS962549",null,"A <WRAP CONTACT> is a <CONNECTOR CONTACT> designed to accept a wrapped connection",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL ELEMENT","INSTRUMENT LOOP ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT SIGNAL LOOP ELEMENT",null,null,null,null,null,"rdl:RDS2221029",null,"A <CURRENT SIGNAL LOOP ELEMENT> is an <INSTRUMENT LOOP ELEMENT> and an <ELECTRICAL ELEMENT> that has the capability of <PARTAKING> in an <ANALOG CURRENT LOOP>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"CURRENT SIGNAL LOOP ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"10-50 mA SIGNAL LOOP ELEMENT",null,null,null,null,null,"rdl:RDS1422806811",null,"A <10-50 mA SIGNAL LOOP ELEMENT> is an <INSTRUMENTATION ITEM> and a <CURRENT SIGNAL LOOP ELEMENT> that can be installed in a <10-50 mA SIGNAL LOOP>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT SIGNAL LOOP ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"4-20 mA SIGNAL LOOP ELEMENT",null,null,null,null,null,"rdl:RDS1422805611",null,"A <4-20 mA SIGNAL LOOP ELEMENT> is an <INSTRUMENTATION ITEM> and a <CURRENT SIGNAL LOOP ELEMENT> that can be installed in a <4-20 mA SIGNAL LOOP>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONDUCTOR","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL CONDUCTOR",null,null,null,null,null,"rdl:RDS7782845814",null,"An <ELECTRICAL CONDUCTOR> is a <CONDUCTOR> that is capable of <CONDUCTIONG> electrical currents",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","ELECTRICAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"BUSBAR",null,null,null,null,null,"rdl:RDS871559",null,"A <BUSBAR> is an <ARTEFACT> and an <ELECTRICAL CONDUCTOR> that is of low-impedance, to which several electric circuits can be connected at separate points",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BUSBAR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DISCONNECTABLE BUSBAR",null,null,null,null,null,"rdl:RDS1005749",null,"A <DISCONNECTABLE BUSBAR> is a <BUSBAR> including disconnector(s) in series intended to connect or disconnect two sections of that busbar, off load.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BUSBAR","EARTHING CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTH BUSBAR",null,null,null,null,null,"rdl:RDS7052389",null,"An <EARTH BUSBAR> is a <BUSBAR> and an <EARTHING CONDUCTOR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BUSBAR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE BUSBAR",null,null,null,null,null,"rdl:RDS1005479",null,"A <FLEXIBLE BUSBAR> is a <BUSBAR> for substations made up of flexible conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BUSBAR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIGID BUSBAR",null,null,null,null,null,"rdl:RDS1005434",null,"A <RIGID BUSBAR> is a <BUSBAR> for substations made up of metallic tubes or bars, and supported by insulator posts.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BUSBAR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SWITCHABLE BUSBAR",null,null,null,null,null,"rdl:RDS1005704",null,"A <SWITCHABLE BUSBAR> is a <BUSBAR> including a switch (or a circuit-breaker) in series, intended to connect or disconnect two sections of that busbar.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BUSBAR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRANSFER BUSBAR",null,null,null,null,null,"rdl:RDS1005839",null,"A <TRANSFER BUSBAR> is a <BUSBAR> to which any circuit can be connected independently of its bay equipment (circuit-breaker, instrument transformer), the control of this circuit being ensured by another specific bay, available for any circuit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE CONDUCTOR",null,null,null,null,null,"rdl:RDS444464",null,"A <CABLE CONDUCTOR> is an <ARTEFACT> and an <ELECTRICAL CONDUCTOR> that is a part of an <ELECTRIC CABLE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONCENTRIC CONDUCTOR",null,null,null,null,null,"rdl:RDS933389",null,"A <CONCENTRIC CONDUCTOR> is a <CABLE CONDUCTOR> so constructed as to surround one or more insulated conductors",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HOLLOW CONDUCTOR",null,null,null,null,null,"rdl:RDS933344",null,"A <HOLLOW CONDUCTOR> is a <CABLE CONDUCTOR> so constructed as to provide a central channel",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"METAL-CLAD CONDUCTOR",null,null,null,null,null,"rdl:RDS932849",null,"A <METAL-CLAD CONDUCTOR> is a <CABLE CONDUCTOR> in which each wire consists of an inner part of one metal and a metallurgically bonded outer shell of another metal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"METAL-COATED CONDUCTOR",null,null,null,null,null,"rdl:RDS932759",null,"A <METAL-COATED CONDUCTOR> is a <CABLE CONDUCTOR> in which each individual wire is covered with a thin layer of a different metal or metal alloy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"METAL-COATED CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TINNED CONDUCTOR",null,null,null,null,null,"rdl:RDS932804",null,"A <TINNED CONDUCTOR> is a <METAL-COATED CONDUCTOR> in which the metal coating is of tin.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PLAIN CONDUCTOR",null,null,null,null,null,"rdl:RDS932714",null,"A <PLAIN CONDUCTOR> is a <CABLE CONDUCTOR> in which the wire or wires are not coated with an additional metal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHAPED CONDUCTOR",null,null,null,null,null,"rdl:RDS933164",null,"A <SHAPED CONDUCTOR> is a <CABLE CONDUCTOR> the cross-section of which is other than circular",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SHAPED CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SECTOR-SHAPED CONDUCTOR",null,null,null,null,null,"rdl:RDS933209",null,"An <SECTOR-SHAPED CONDUCTOR> is a <SHAPED CONDUCTOR> the cross-section of which approximates to a sector of a circle.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHIELDING CONDUCTOR",null,null,null,null,null,"rdl:RDS950624",null,"A <SHIELDING CONDUCTOR> is a <CABLE CONDUCTOR> that is a separate conductor or single-core cable laid parallel to a cable or cable circuit and itself forming part of a closed circuit in which induced currents may flow whose magnetic field will opposed the field caused by the current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID CONDUCTOR",null,null,null,null,null,"rdl:RDS932894",null,"A <SOLID CONDUCTOR> is a <CABLE CONDUCTOR> consisting of a single wire",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STANDARD SIZE CABLE CONDUCTOR",null,null,null,null,null,"rdl:RDS7337231",null,"A <STANDARD SIZE CABLE CONDUCTOR> is a <CABLE CONDUCTOR> which conforms to a standard cross section specification",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STRANDED CONDUCTOR",null,null,null,null,null,"rdl:RDS932939",null,"A <STRANDED CONDUCTOR> is a <CABLE CONDUCTOR> consisting of a number of wires, all or some of which are wound in a helix",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRANDED CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUNCHED CONDUCTOR",null,null,null,null,null,"rdl:RDS933029",null,"A <BUNCHED CONDUCTOR> is a <STRANDED CONDUCTOR> in which the wires are assembled together in helical formation in a random manner, all in the same direction and with the same length of lay.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRANDED CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPACTED CONDUCTOR",null,null,null,null,null,"rdl:RDS933254",null,"A <COMPACTED CONDUCTOR> is a <STRANDED CONDUCTOR> in which the interstices between the component wires have been reduced by mechanical compression or by drawing or by suitable choice of the shape and disposition of wires.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRANDED CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONCENTRICALLY STRANDED CIRCULAR CONDUCTOR",null,null,null,null,null,"rdl:RDS932984",null,"A <CONCENTRICALLY STRANDED CIRCULAR CONDUCTOR> is a <STRANDED CONDUCTOR> in which the individual wires are assembled together in helical formation, in one or more separate concentric layers and generally with an alternating direction of lay.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRANDED CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE CONDUCTOR",null,null,null,null,null,"rdl:RDS933119",null,"A <FLEXIBLE CONDUCTOR> is a <STRANDED CONDUCTOR> having wires of diameters small enough and so assembled that the conductor is suitable for use in a flexible cable.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRANDED CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MILLIKEN CONDUCTOR",null,null,null,null,null,"rdl:RDS933299",null,"A <MILLIKEN CONDUCTOR> is a <STRANDED CONDUCTOR> comprising an assembly of shaped stranded conductors, lightly insulated from each other.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRANDED CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTIPLE-STRANDED CONDUCTOR",null,null,null,null,null,"rdl:RDS933074",null,"A <MULTIPLE-STRANDED CONDUCTOR> is a <STRANDED CONDUCTOR> consisting of a number of groups of wires assembled together in one or more helical layers, the wires in each group being either bunched or stranded.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TINSEL CONDUCTOR",null,null,null,null,null,"rdl:RDS933434",null,"A <TINSEL CONDUCTOR> is a <CABLE CONDUCTOR> comprising one or more elements stranded together, each element consisting of one or more thin metal tapes helically wound and supported by a textile thread",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE CORE",null,null,null,null,null,"rdl:RDS485459",null,"A <CABLE CORE> is an <ARTEFACT> and an <ELECTRICAL CONDUCTOR> and that is an assembly consisting of a conductor with its own insulation (and screens if any)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"CONDUCTOR STRAND",null,null,null,null,null,"rdl:RDS6588875",null,"A <CONDUCTOR STRAND> is an <ARTEFACT> and an <ELECTRICAL CONDUCTOR> that is a single wire of conducting metal intended to be formed into a stranded conductor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTHING CONDUCTOR",null,null,null,null,null,"rdl:RDS778457471",null,"An <EARTHING CONDUCTOR> is an <ARTEFACT> and an <ELECTRICAL CONDUCTOR> that provides a conductive path, or part of the conductive path, between a given point in a system or in an installation or in equipment and an earth electrode",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EARTHING CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTH BAR",null,null,null,null,null,"rdl:RDS6233460",null,"An <EARTH BAR> is an <EARTHING CONDUCTOR>, forming a common junction for a number of earth conductors",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EARTHING CONDUCTOR","ELECTRODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTH ELECTRODE",null,null,null,null,null,"rdl:RDS7503182",null,"An <EARTH ELECTRODE> is an <ELECTRODE> and an <EARTHING CONDUCTOR> and that is a conductive part that can be embedded in a specific conductive medium, e.g. concrete or coke, in electric contact with the earth",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EARTHING CONDUCTOR","ELECTRODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTH PLATE",null,null,null,null,null,"rdl:RDS871694",null,"An <EARTH PLATE> is an <ELECTRODE> and an <EARTHING CONDUCTOR> and that is an earth electrode consisting of a metal plate buried in the ground",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EARTHING CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTHING BOSS",null,null,null,null,null,"rdl:RDS813959",null,"An <EARTHING BOSS> is an <EARTHING CONDUCTOR>, and are designed to provide an earth connection point on a steel structure - the earth boss is welded onto steel vessels, tanks and other structures",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EARTHING CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTHING STRAP",null,null,null,null,null,"rdl:RDS882269",null,"An <EARTHING STRAP> is an <EARTHING CONDUCTOR>, and is used to equalise the potential between different structures",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EARTHING CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTHING STUD",null,null,null,null,null,"rdl:RDS814004",null,"An <EARTHING STUD> is an <EARTHING CONDUCTOR>, that connects equipment to the <EARTH BAR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL CABLE",null,null,null,null,null,"rdl:RDS642779",null,"An <ELECTRICAL CABLE> is an <ARTEFACT> and an <ELECTRICAL CONDUCTOR> that consists of one or more <CABLE CONNECTOR>s, that is held together with an overall sheath, and is used to distribute electricity",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-CORE CABLE",null,null,null,null,null,"rdl:RDS476144",null,"A <1-CORE CABLE> is an <ELECTRICAL CABLE> consisting of one core only",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANTI TWIST CABLE",null,null,null,null,null,"rdl:RDS6458874",null,"An <ANTI TWIST CABLE> is an <ELECTRICAL CABLE> designed to minimize torque under mechanical tension",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BLASTING CABLE",null,null,null,null,null,"rdl:RDS6458919",null,"A <BLASTING CABLE> is an <ELECTRICAL CABLE> for triggering explosions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COAXIAL CABLE",null,null,null,null,null,"rdl:RDS475874",null,"A <COAXIAL CABLE> is an <ELECTRICAL CABLE> consisting of an inner conductor surrounded by an outer tubular conductor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMMON SCREENED ELECTRIC CABLE",null,null,null,null,null,"rdl:RDS6653960",null,"A <COMMON SCREENED ELECTRIC CABLE> is an <ELECTRICAL CABLE> where all the insulated conductors are surrounded by a common protective shield connected to earth to prevent signal disturbance created by electromagnetic fields",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONCENTRIC NEUTRAL CABLE",null,null,null,null,null,"rdl:RDS949319",null,"A <CONCENTRIC NEUTRAL CABLE> is an <ELECTRICAL CABLE> having a concentric conductor which is intended to be used for the neutral",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONCENTRIC NEUTRAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE-PHASE CONCENTRIC NEUTRAL CABLE",null,null,null,null,null,"rdl:RDS949364",null,"A <SINGLE-PHASE CONCENTRIC NEUTRAL CABLE> is a <CONCENTRIC NEUTRAL CABLE> that is a single-core cable consisting of a concentric conductor intended used for the neutral.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONCENTRIC NEUTRAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE-PHASE CONCENTRIC NEUTRAL CABLE",null,null,null,null,null,"rdl:RDS949409",null,"A <THREE-PHASE CONCENTRIC NEUTRAL CABLE> is a <CONCENTRIC NEUTRAL CABLE> that is a three-core cable consisting of a concentric conductor intended used for the neutral.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE","ELECTRICAL SIGNAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC SIGNAL CABLE",null,null,null,null,null,"rdl:RDS5757130",null,"An <ELECTRIC SIGNAL CABLE> is an <ELECTRICAL CABLE> and a <ELECTRICAL SIGNAL CONDUCTOR> for transmission of electric signals",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC SIGNAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONTROL CABLE",null,null,null,null,null,"rdl:RDS5757085",null,"A <CONTROL CABLE> is a <SIGNAL CABLE> that is intended to be involved in some control function.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC SIGNAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE DETECTOR CABLE",null,null,null,null,null,"rdl:RDS13599027",null,"A <TEMPERATURE DETECTOR CABLE> is a <SIGNAL CABLE> for the transfer of signals from a thermal detector/detectors to a receiver or connection point.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EMERGENCY SHUT DOWN CABLE",null,null,null,null,null,"rdl:RDS1070467070",null,"An <EMERGENCY SHUT DOWN CABLE> is an <ELECTRICAL CABLE> intended for use in shut down processes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE","FIRE RESISTANT ARTEFACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIRE RESISTANT CABLE",null,null,null,null,null,"rdl:RDS464489",null,"A <FIRE RESISTANT CABLE> is a <FIRE RESISTANT ARTEFACT> and a <ELECTRICAL CABLE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLAME RETARDANT CABLE",null,null,null,null,null,"rdl:RDS464444",null,"A <FLAME RETARDANT CABLE> is an <ELECTRICAL CABLE> that resists the spread of fire",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE CABLE",null,null,null,null,null,"rdl:RDS949634",null,"A <FLEXIBLE CABLE> is an <ELECTRICAL CABLE> that is required to be capable of being flexed while in service and of which the structure and materials are such as to fulfil this requirement",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CORD",null,null,null,null,null,"rdl:RDS949679",null,"A <CORD> is a <FLEXIBLE CABLE> with a limited number of conductors of small cross-sectional area.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC HEATER","ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HEATING CABLE",null,null,null,null,null,"rdl:RDS14069935",null,"A <HEATING CABLE> is an <ELECTRICAL CABLE> and an <ELECTRIC HEATER>, with or without a shield or a metallic sheath, intended to give off heat for heating purposes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HEATING CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRACE HEATING CABLE",null,null,null,null,null,"rdl:RDS14069755",null,"A <TRACE HEATING CABLE> is a <HEATING CABLE> intended to trace heat pipework and other equipment.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRACE HEATING CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SELF-REGULATING TRACE HEATING CABLE",null,null,null,null,null,"rdl:RDS14069530",null,"A <SELF-REGULATING TRACE HEATING CABLE> is a <TRACE HEATING CABLE> in which the thermal output generated at its operating voltage decreases as the temperature of its environment increases.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HEATING CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UNDERFLOOR HEATING CABLE",null,null,null,null,null,"rdl:RDS14069440",null,"A <UNDERFLOOR HEATING CABLE> is a <HEATING CABLE> intended to be laid under a floor in a building.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IGNITION CABLE",null,null,null,null,null,"rdl:RDS6458964",null,"An <IGNITION CABLE> is an <ELECTRICAL CABLE> designed for electric ignition systems",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDIVIDUALLY SCREENED CABLE",null,null,null,null,null,"rdl:RDS949544",null,"An <INDIVIDUALLY SCREENED CABLE> is an <ELECTRICAL CABLE> in which each core is covered with an individual screen",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LEAD",null,null,null,null,null,"rdl:RDS953549",null,"An <INSTRUMENT LEAD> is an <ELECTRICAL CABLE> comprising one or more conductors, specially designed for interconnecting measuring instruments and accessories",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSULATED CABLE",null,null,null,null,null,"rdl:RDS949094",null,"An <INSULATED CABLE> is an <ELECTRICAL CABLE> with an assembly consisting of: one or more cores, their individual covering(s) (if any), assembly protection (if any), protective covering(s) (if any). Additional uninsulated conductor(s) may be included in the cable",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSULATED CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AERIAL INSULATED CABLE",null,null,null,null,null,"rdl:RDS950039",null,"An <AERIAL INSULATED CABLE> is an <INSULATED CABLE> designed to be suspended overhead and outdoors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AERIAL INSULATED CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUNDLE ASSEMBLED AERIAL CABLE",null,null,null,null,null,"rdl:RDS950084",null,"A <BUNDLE ASSEMBLED AERIAL CABLE> is an <AERIAL INSULATED CABLE> consisting of a group of insulated conductors with or without an uninsulated conductor, twisted together.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEAD SHEATHED CABLE",null,null,null,null,null,"rdl:RDS6459009",null,"A <LEAD SHEATHED CABLE> is an <ELECTRICAL CABLE> that has a lead sheath",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MUD RESISTANT CABLE",null,null,null,null,null,"rdl:RDS464579",null,"A <MUD RESISTANT CABLE> is an <ELECTRICAL CABLE> that is resistant to mud",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTICORE CABLE",null,null,null,null,null,"rdl:RDS464309",null,"A <MULTICORE CABLE> is an <ELECTRICAL CABLE> consisting of more than one core",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10-CORE CABLE",null,null,null,null,null,"rdl:RDS867104",null,"A <10-CORE CABLE> is a <MULTICORE CABLE> consisting of 10 cable conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12-CORE CABLE",null,null,null,null,null,"rdl:RDS550979",null,"A <12-CORE CABLE> is a <MULTICORE CABLE> consisting of 12 cable conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14-CORE CABLE",null,null,null,null,null,"rdl:RDS867149",null,"A <14-CORE CABLE> is a <MULTICORE CABLE> consisting of 14 cable conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16-CORE CABLE",null,null,null,null,null,"rdl:RDS867194",null,"A <16-CORE CABLE> is a <MULTICORE CABLE> consisting of 16 cable conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"19-CORE CABLE",null,null,null,null,null,"rdl:RDS551024",null,"A <19-CORE CABLE> is a <MULTICORE CABLE> consisting of 19 cable conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2-CORE CABLE",null,null,null,null,null,"rdl:RDS550529",null,"A <2-CORE CABLE> is a <MULTICORE CABLE> consisting of 2 cable conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24-CORE CABLE",null,null,null,null,null,"rdl:RDS867239",null,"A <24-CORE CABLE> is a <MULTICORE CABLE> consisting of 24 cable conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"27-CORE CABLE",null,null,null,null,null,"rdl:RDS551069",null,"A <27-CORE CABLE> is a <MULTICORE CABLE> consisting of 27 cable conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3-CORE CABLE",null,null,null,null,null,"rdl:RDS550799",null,"A <3-CORE CABLE> is a <MULTICORE CABLE> consisting of 3 cable conductors",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"3-CORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEPARATELY LEAD-SHEATHED CABLE",null,null,null,null,null,"rdl:RDS949589",null,"A <SEPARATELY LEAD-SHEATHED CABLE> is a <3-C0RE CABLE> in which each core is individually sheathed with lead or lead alloy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"37-CORE CABLE",null,null,null,null,null,"rdl:RDS551114",null,"A <37-CORE CABLE> is a <MULTICORE CABLE> consisting of 3 cable conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4-CORE CABLE",null,null,null,null,null,"rdl:RDS550844",null,"A <4-CORE CABLE> is a <MULTICORE CABLE> consisting of 4 cable conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5-CORE CABLE",null,null,null,null,null,"rdl:RDS550889",null,"A <5-CORE CABLE> is a <MULTICORE CABLE> consisting of 5 cable conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6-CORE CABLE",null,null,null,null,null,"rdl:RDS869354",null,"A <6-CORE CABLE> is a <MULTICORE CABLE> consisting of 6 cable conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"7-CORE CABLE",null,null,null,null,null,"rdl:RDS550934",null,"A <7-CORE CABLE> is a <MULTICORE CABLE> consisting of 7 cable conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BELTED CABLE",null,null,null,null,null,"rdl:RDS949499",null,"A <BELTED CABLE> is a <MULTICORE CABLE> in which part of the insulation is applied to each conductor individually, and the remainder is applied over the assembled cores",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COLLECTIVELY SHIELDED CABLE",null,null,null,null,null,"rdl:RDS949274",null,"A <COLLECTIVELY SHIELDED CABLE> is a <MULTICORE CABLE> having a shield arranged around the cores concentrically with the axis of the cable.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTICORE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLAT MULTICORE CABLE",null,null,null,null,null,"rdl:RDS949229",null,"A <FLAT MULTICORE CABLE> is a <MULTICORE CABLE> having cores or groups of cores arranged in parallel flat formation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NEUTRAL ELECTRIC CABLE",null,null,null,null,null,"rdl:RDS4238875",null,"A <NEUTRAL ELECTRIC CABLE> is an <ELECTRICAL CABLE> intended to be a part of a neutral system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OIL RESISTANT CABLE",null,null,null,null,null,"rdl:RDS464534",null,"An <OIL RESISTANT CABLE> is an <ELECTRICAL CABLE> that is resistant to oil",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OVERHEAD CABLE",null,null,null,null,null,"rdl:RDS6459054",null,"An <OVERHEAD CABLE> is an <ELECTRICAL CABLE> intended to be installed overhead",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PAIR CABLE",null,null,null,null,null,"rdl:RDS464354",null,"A <PAIR CABLE> is an <ELECTRICAL CABLE> in which the cores are arranged in pairs twisted together",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-PAIR CABLE",null,null,null,null,null,"rdl:RDS549404",null,"A <1-PAIR CABLE> is a <PAIR CABLE> consisting of one pair only",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10-PAIR CABLE",null,null,null,null,null,"rdl:RDS867644",null,"A <10-PAIR CABLE> is a <PAIR CABLE> consisting of 10 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12-PAIR CABLE",null,null,null,null,null,"rdl:RDS549674",null,"A <12-PAIR CABLE> is a <PAIR CABLE> consisting of 12 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14-PAIR CABLE",null,null,null,null,null,"rdl:RDS867419",null,"A <14-PAIR CABLE> is a <PAIR CABLE> consisting of 14 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16-PAIR CABLE",null,null,null,null,null,"rdl:RDS549719",null,"A <16-PAIR CABLE> is a <PAIR CABLE> consisting of 16 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"19-PAIR CABLE",null,null,null,null,null,"rdl:RDS867464",null,"A <19-PAIR CABLE> is a <PAIR CABLE> consisting of 19 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2-PAIR CABLE",null,null,null,null,null,"rdl:RDS549449",null,"A <2-PAIR CABLE> is a <PAIR CABLE> consisting of 2 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20-PAIR CABLE",null,null,null,null,null,"rdl:RDS867689",null,"A <20-PAIR CABLE> is a <PAIR CABLE> consisting of 20 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24-PAIR CABLE",null,null,null,null,null,"rdl:RDS549764",null,"A <24-PAIR CABLE> is a <PAIR CABLE> consisting of 24 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"27-PAIR CABLE",null,null,null,null,null,"rdl:RDS867509",null,"A <27-PAIR CABLE> is a <PAIR CABLE> consisting of 27 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3-PAIR CABLE",null,null,null,null,null,"rdl:RDS867284",null,"A <3-PAIR CABLE> is a <PAIR CABLE> consisting of 3 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30-PAIR CABLE",null,null,null,null,null,"rdl:RDS867554",null,"A <30-PAIR CABLE> is a <PAIR CABLE> consisting of 30 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32-PAIR CABLE",null,null,null,null,null,"rdl:RDS549809",null,"A <32-PAIR CABLE> is a <PAIR CABLE> consisting of 32 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"37-PAIR CABLE",null,null,null,null,null,"rdl:RDS867599",null,"A <37-PAIR CABLE> is a <PAIR CABLE> consisting of 37 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4-PAIR CABLE",null,null,null,null,null,"rdl:RDS549494",null,"A <4-PAIR CABLE> is a <PAIR CABLE> consisting of 4 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5-PAIR CABLE",null,null,null,null,null,"rdl:RDS867329",null,"A <5-PAIR CABLE> is a <PAIR CABLE> consisting of 5 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"50-PAIR CABLE",null,null,null,null,null,"rdl:RDS867734",null,"A <50-PAIR CABLE> is a <PAIR CABLE> consisting of 50 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"7-PAIR CABLE",null,null,null,null,null,"rdl:RDS867374",null,"A <7-PAIR CABLE> is a <PAIR CABLE> consisting of 7 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PAIR CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8-PAIR CABLE",null,null,null,null,null,"rdl:RDS549539",null,"An <8-PAIR CABLE> is a <PAIR CABLE> consisting of 8 pairs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER CABLE",null,null,null,null,null,"rdl:RDS5757040",null,"A <POWER CABLE> is an <ELECTRICAL CABLE> intended for transmission of electric power",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HEATER POWER CABLE",null,null,null,null,null,"rdl:RDS14147578",null,"A <HEATER POWER CABLE> is a <POWER CABLE> that is intended to transfer electrical power to an electric heater.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOTOR POWER CABLE",null,null,null,null,null,"rdl:RDS13598982",null,"A <MOTOR POWER CABLE> is a <POWER CABLE> that is intended to transfer electrical power to an electrical motor.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPACE HEATER CABLE",null,null,null,null,null,"rdl:RDS13598937",null,"A <SPACE HEATER CABLE> is a <POWER CABLE> that is intended to transfer electrical power to a space heater.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRANSFORMER PRIMARY WINDING CABLE",null,null,null,null,null,"rdl:RDS4231445",null,"A <TRANSFORMER PRIMARY WINDING CABLE> is a <POWER CABLE> intended to be connected to the primary side of a transformer.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRANSFORMER SECONDARY WINDING CABLE",null,null,null,null,null,"rdl:RDS4238830",null,"A <TRANSFORMER SECONDARY WINDING CABLE> is a <POWER CABLE> intended to be connected to the secondary side of a transformer.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE CABLE",null,null,null,null,null,"rdl:RDS949724",null,"A <PRESSURE CABLE> is an <ELECTRIC CABLE> in which the insulation is maintained under pressure by means of a fluid.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PRESSURE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXTERNAL GAS PRESSURE CABLE",null,null,null,null,null,"rdl:RDS949994",null,"An <EXTERNAL GAS PRESSURE CABLE> is a <PRESSURE CABLE> usually pipe-type in which the pressurizing fluid is a gas separated from the insulation by a diaphragm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PRESSURE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INTERNAL GAS PRESSURE CABLE",null,null,null,null,null,"rdl:RDS949949",null,"An <INTERNAL GAS PRESSURE CABLE> is a <PRESSURE CABLE> in which the pressurizing fluid is a gas in contact with the insulation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PRESSURE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PIPE-TYPE CABLE",null,null,null,null,null,"rdl:RDS949814",null,"A <PIPE-TYPE CABLE> is a <PRESSURE CABLE> in which the cores are drawn into a pipe, usually of steel and already installed, and which in service contains a fluid under pressure.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPE-TYPE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OIL-FILLED PIPE-TYPE CABLE",null,null,null,null,null,"rdl:RDS949904",null,"An <OIL-FILLED PIPE-TYPE CABLE> is a <PIPE-TYPE CABLE> in which the pressurizing fluid is the insulating oil.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PRESSURE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SELF-CONTAINED PRESSURE CABLE",null,null,null,null,null,"rdl:RDS949769",null,"A <SELF-CONTAINED PRESSURE CABLE> is a <PRESSURE CABLE> in which the pressurizing fluid is contained within the metallic sheath applied during manufacture.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SELF-CONTAINED PRESSURE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OIL-FILLED CABLE",null,null,null,null,null,"rdl:RDS949859",null,"An <OIL-FILLED CABLE> is a <SELF-CONTAINED PRESSURE CABLE> in which the pressurizing fluid is the insulating oil and which is designed to facilitate the free movement of the oil within the cable.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"QUAD CABLE",null,null,null,null,null,"rdl:RDS868049",null,"A <QUAD CABLE> is an <ELECTRICAL CABLE> that consists of a group of four insulated conductors twisted together, the conductors usually forming two circuits",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"QUAD CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-QUAD CABLE",null,null,null,null,null,"rdl:RDS868094",null,"A <1-QUAD CABLE> is a <QUAD CABLE> consisting of one quad only.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"QUAD CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2-QUAD CABLE",null,null,null,null,null,"rdl:RDS869399",null,"A <2-QUAD CABLE> is a <QUAD CABLE> consisting of 2 quads.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"QUAD CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3-QUAD CABLE",null,null,null,null,null,"rdl:RDS869444",null,"A <3-QUAD CABLE> is a <QUAD CABLE> consisting of 3 quads.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"QUAD CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5-QUAD CABLE",null,null,null,null,null,"rdl:RDS869489",null,"A <5-QUAD CABLE> is a <QUAD CABLE> consisting of 5 quads.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"QUAD CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"7-QUAD CABLE",null,null,null,null,null,"rdl:RDS869534",null,"A <7-QUAD CABLE> is a <QUAD CABLE> consisting of 7 quads.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIATION RESISTANT CABLE",null,null,null,null,null,"rdl:RDS6459099",null,"A <RADIATION RESISTANT CABLE> is an <ELECTRICAL CABLE> in which the insulation is resistant to degradation by ionising radiation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHIELDED CABLE",null,null,null,null,null,"rdl:RDS6459144",null,"A <SHIELDED CABLE> is a <SIGNAL CONVEYING ITEM> and a <ELECTRICAL CABLE> that contains a cable shield",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE-CONDUCTOR CABLE",null,null,null,null,null,"rdl:RDS949139",null,"A <SINGLE-CONDUCTOR CABLE> is an <ELECTRICAL CABLE> having only one core",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPECIAL CABLE",null,null,null,null,null,"rdl:RDS1070472110",null,"A <SPECIAL CABLE> is an <ELECTRICAL CABLE> intended for special purposes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPLIT CONCENTRIC CABLE",null,null,null,null,null,"rdl:RDS949454",null,"An <SPLIT CONCENTRIC CABLE> is an <ELECTRICAL CABLE> having two conductors in a single concentric layer separated from each other by insulating material",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBMERSIBLE POWER CABLE",null,null,null,null,null,"rdl:RDS816974",null,"A <SUBMERSIBLE POWER CABLE> is an <ELECTRICAL CABLE> that is a special power cable suitable to supply power to the submersed electric motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA CABLE",null,null,null,null,null,"rdl:RDS6459189",null,"A <SUBSEA CABLE> is an <ELECTRICAL CABLE> intended for underwater installation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TELECOMMUNICATIONS CABLE",null,null,null,null,null,"rdl:RDS1070463891",null,"A <TELECOMMUNICATIONS CABLE> is an <ELECTRICAL CABLE> intended for telecomunications",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMOCOUPLE COMPENSATION CABLE",null,null,null,null,null,"rdl:RDS6459234",null,"A <THERMOCOUPLE COMPENSATION CABLE> is a <SIGNAL CONVEYING ITEM> and a <ELECTRICAL CABLE> having conductors differing in nature or quality from that of the thermocouple, but having thermoelectric characteristics such that the resulting error is within specified limits for a given temperature range",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMOCOUPLE EXTENSION CABLE",null,null,null,null,null,"rdl:RDS6459279",null,"A <THERMOCOUPLE EXTENSION CABLE> is a <SIGNAL CONVEYING ITEM> and a <ELECTRICAL CABLE> consisting of conductors of the same nature as the thermocouple elements, extending it to the reference junction and having the same thermo-electric properties as those of the thermocouple within the whole temperature range of utilisation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRIAXIAL CABLE",null,null,null,null,null,"rdl:RDS869759",null,"A <TRIAXIAL CABLE> is an <ELECTRICAL CABLE> consisting of three concentric conductors",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRIPLE CABLE",null,null,null,null,null,"rdl:RDS464399",null,"A <TRIPLE CABLE> is an <ELECTRICAL CABLE> in which the conductors are arranged in threes twisted together",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS549854",null,"A <1-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of one triple only.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS867824",null,"A <10-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of 10 triples",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS550124",null,"A <12-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of 12 triples",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"14-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS867869",null,"A <14-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of 14 triples",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS550169",null,"A <16-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of 16 triples",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"19-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS867914",null,"A <19-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of 19 triples",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS549899",null,"A <2-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of 2 triples.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS867959",null,"A <20-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of 20 triples",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS550214",null,"A <24-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of 24 triples",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS868004",null,"A <3-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of 3 triples.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS550259",null,"A <32-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of 32 triples",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS549944",null,"A <4-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of 4 triples.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"7-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS867779",null,"A <7-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of 7 triples.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRIPLE CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8-TRIPLE CABLE",null,null,null,null,null,"rdl:RDS550079",null,"An <8-TRIPLE CABLE> is a <TRIPLE CABLE> consisting of 8 triples.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TWISTED LOOM",null,null,null,null,null,"rdl:RDS6459324",null,"A <TWISTED LOOM> is an <ELECTRICAL CABLE> consisting of insulated or single-core cables twisted together without a common covering",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE RATED CABLE",null,null,null,null,null,"rdl:RDS7290100",null,"A <VOLTAGE RATED CABLE> is an <ELECTRICAL CABLE> conforming to a specification for highest allowable voltage under rated conditions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"XLPE CABLE",null,null,null,null,null,"rdl:RDS6459369",null,"An <XLPE CABLE> is an <ELECTRICAL CABLE> having cross linked polyethylene as insulation and sheath layers",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL COMPONENT","ELECTRICAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL CONTACT",null,null,null,null,null,"rdl:RDS957419",null,"An <ELECTRICAL CONTACT is an <ARTEFACT> and an <ELECTRICAL COMPONENT> and an <ELECTRICAL CONDUCTOR> that is the conductive element in a component which mates with a corresponding element to provide an electrical path",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTACT ASSEMBLY","ELECTRICAL CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHANGE-OVER CONTACT",null,null,null,null,null,"rdl:RDS957689",null,"A <CHANGE-OVER CONTACT> is an <ELECTRICAL CONTACT> and a <CONTACT ASSEMBLY> that is a combination of two contact circuits including three contact members, one of them being common to the two contact circuits. When one of these contact circuits is open, the other is closed and vice versa.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHANGE-OVER CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHANGE-OVER BREAK-BEFORE-MAKE CONTACT",null,null,null,null,null,"rdl:RDS957779",null,"A <CHANGE-OVER BREAK-BEFORE-MAKE CONTACT> is a <CHANGE-OVER CONTACT> having one contact circuit that breaks before the other makes.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHANGE-OVER CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHANGE-OVER MAKE-BEFORE-BREAK CONTACT",null,null,null,null,null,"rdl:RDS957734",null,"A <CHANGE-OVER MAKE-BEFORE-BREAK CONTACT> is a <CHANGE-OVER CONTACT> having one contact circuit that makes before the other breaks.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHANGE-OVER CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHANGE-OVER WITH NEUTRAL POSITION",null,null,null,null,null,"rdl:RDS957824",null,"A <CHANGE-OVER WITH NEUTRAL POSITION> is a <CHANGE-OVER CONTACT> having a stable position in which its two contact circuits are open (or closed).",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHANGE-OVER CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PASSING CONTACT",null,null,null,null,null,"rdl:RDS957914",null,"A <PASSING CONTACT> is a <CHANGE-OVER CONTACT> designed for opening or closing in a passing fashion the corresponding contact circuit when the relay changes over.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHANGE-OVER CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REED CONTACT",null,null,null,null,null,"rdl:RDS957869",null,"A <REED CONTACT> is a <CHANGE-OVER CONTACT>, the contact members of which are blades either fully or partly of magnetic material and which are moved directly by a magnetic force.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONTACT ASSEMBLY",null,null,null,null,null,"rdl:RDS957554",null,"A <CONTACT ASSEMBLY> is an <ELECTRICAL CONTACT> that is an assembly of contact members, with their insulation, which close or open their contact circuit by their relative movement.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FUSE-BASE CONTACT",null,null,null,null,null,"rdl:RDS955754",null,"A <FUSE-BASE CONTACT> is an <ELECTRICAL CONTACT> that is the contact piece of a fuse-base, designed to engage with a corresponding part of the fuse.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FUSE-CARRIER CONTACT",null,null,null,null,null,"rdl:RDS955844",null,"A <FUSE-CARRIER CONTACT> is an <ELECTRICAL CONTACT> that is the contact piece of a fuse-carrier, designed to engage with a corresponding part of the fuse.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FUSE-LINK CONTACT",null,null,null,null,null,"rdl:RDS955799",null,"A <FUSE-LINK CONTACT> is an <ELECTRICAL CONTACT> that is the contact piece of a fuse-link, designed to engage with a corresponding part of the fuse.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NORMALLY CLOSED CONTACT",null,null,null,null,null,"rdl:RDS7460987",null,"A <NORMALLY CLOSED CONTACT> is an <ELECTRICAL CONTACT> which under normal conditions performs an closed circuit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NORMALLY OPEN CONTACT",null,null,null,null,null,"rdl:RDS7460942",null,"A <NORMALLY OPEN CONTACT> is an <ELECTRICAL CONTACT> which under normal conditions performs an open circuit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SWITCH CONTACT",null,null,null,null,null,"rdl:RDS954359",null,"A <SWITCH CONTACT> is an <ELECTRICAL CONTACT> that is one of the conductive parts forming a contact.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ARCING CONTACT",null,null,null,null,null,"rdl:RDS954494",null,"An <ARCING CONTACT> is a <SWITCH CONTACT> on which the arc is intended to be established.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AUXILIARY CONTACT",null,null,null,null,null,"rdl:RDS954584",null,"An <AUXILIARY CONTACT> is a <SWITCH CONTACT> included in an auxiliary circuit and mechanically operated by the switching device.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUTT CONTACT",null,null,null,null,null,"rdl:RDS954764",null,"A <BUTT CONTACT> is a <SWITCH CONTACT> in which relative movement of the contact pieces is substantially in a direction perpendicular to the contact surface.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHANGE OVER CONTACT",null,null,null,null,null,"rdl:RDS7461066",null,"A <CHANGE OVER CONTACT> is a <SWITCH CONTACT> that changes between two contact positions.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONTROL CONTACT",null,null,null,null,null,"rdl:RDS954539",null,"A <CONTROL CONTACT> is a <SWITCH CONTACT> included in a control circuit of a mechanical switching device and mechanically operated by this device.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAIN CONTACT",null,null,null,null,null,"rdl:RDS954449",null,"An <MAIN CONTACT> is a <SWITCH CONTACT> included in the main circuit of a mechanical switching device, intended to carry, in the closed position, the current of the main circuit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MAIN CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONTACTOR MAIN CONTACT",null,null,null,null,null,"rdl:RDS6589085",null,"A <CONTACTOR MAIN CONTACT> is an <MAIN CONTACT> designed to switch the main circuit in a contactor.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MAIN CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DISCONNECTOR MAIN CONTACT",null,null,null,null,null,"rdl:RDS6589850",null,"A <DISCONNECTOR MAIN CONTACT> is an <MAIN CONTACT> designed to switch the main circuit in a disconnector.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MAIN CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SWITCH MAIN CONTACT",null,null,null,null,null,"rdl:RDS6624108",null,"A <SWITCH MAIN CONTACT> is an <MAIN CONTACT> designed to switch the main circuit in an electric switch.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAKE CONTACT",null,null,null,null,null,"rdl:RDS954629",null,"An <MAKE CONTACT> is a <SWITCH CONTACT> that is closed when the main contacts of the mechanical switching device are closed and open when they are open.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-SHORTING CONTACT",null,null,null,null,null,"rdl:RDS965024",null,"A <NON-SHORTING CONTACT> is a <SWITCH CONTACT> designed such that one contact is completely open before the next contact is made.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"QUICK ACTION CONTACT",null,null,null,null,null,"rdl:RDS964889",null,"A <QUICK ACTION CONTACT> is a <SWITCH CONTACT>, the relative displacement of which is always rapid regardless of the speed of the actuating part.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RELAY BREAK CONTACT",null,null,null,null,null,"rdl:RDS954719",null,"A <RELAY BREAK CONTACT> is a <SWITCH CONTACT> that is open when the main contacts of a mechanical switching device are closed and closed when they are open.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROLLING CONTACT",null,null,null,null,null,"rdl:RDS954854",null,"A <ROLLING CONTACT> is a <SWITCH CONTACT> in which one contact piece rolls on the other.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTOR CONTACT",null,null,null,null,null,"rdl:RDS964979",null,"A <ROTOR CONTACT> is a <SWITCH CONTACT> that is the conductive segment of a rotary switch carried by the rotor and shaped to engage with the contacts on the stator as required.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHORTING CONTACT",null,null,null,null,null,"rdl:RDS965069",null,"A <SHORTING CONTACT> is a <SWITCH CONTACT> designed such that one contact is maintained until after the next contact is made.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLIDING CONTACT",null,null,null,null,null,"rdl:RDS954809",null,"A <SLIDING CONTACT> is a <SWITCH CONTACT> in which relative movement of the contact pieces is substantially in a direction parallel to the contact surface.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH CONTACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLOW ACTION CONTACT",null,null,null,null,null,"rdl:RDS964934",null,"A <SLOW ACTION CONTACT> is a <SWITCH CONTACT> the relative displacement of which is directly related to the speed of the actuating part.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL CONDUCTOR","POWER DISTRIBUTOR",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL DISTRIBUTION UNIT",null,null,null,null,null,"rdl:RDS316439",null,"An <ELECTRICAL DISTRIBUTION UNIT> is an <ARTEFACT> and a <POWER DISTRIBUTOR> and an <ELECTRICAL CONDUCTOR> and several power distribution points",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL SIGNAL CONDUCTOR",null,null,null,null,null,"rdl:RDS7782845837",null,"An <ELECTRICAL SIGNAL CONDUCTOR> is an <ELECTRICAL CONDUCTOR> that has a capability of <CONDUCTING> an <ELECTRICAL SIGNAL>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRICAL CONDUCTOR","WIRE",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL WIRE",null,null,null,null,null,"rdl:RDS3397114511",null,"A <ELECTRICAL WIRE> is a <WIRE> and an <ELECTRICAL CONDUCTOR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRODE",null,null,null,null,null,"rdl:RDS483749",null,"An <ELECTRODE> is an <ARTEFACT> and an <ELECTRICAL CONDUCTOR> by means of which electricity enters or leaves an electrolyte, gas, or other medium, or a vacuum",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BATTERY ELECTRODE",null,null,null,null,null,"rdl:RDS6568670",null,"A <BATTERY ELECTRODE> is an <ELECTRODE> that is electrically connected to one terminal of a cell, in electric contact with the electrolyte of that cell and on which the electrode reaction occurs.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"SHUNT",null,null,null,null,null,"rdl:RDS966464",null,"A <SHUNT> is an <ARTEFACT> and an <ELECTRICAL CONDUCTOR> connected in parallel with part of a current-carrying electric circuit to divert current from that part",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL CONDUCTOR","RING",null,null,null,null,null,null,null,null,null,null,null,null,"SLIP RING",null,null,null,null,null,"rdl:RDS5796125",null,"A <SLIP RING> is an <ARTEFACT> and an <ELECTRICAL CONDUCTOR> and a <RING> of conducting material which is attached to and rotates with a shaft, so that the electric current may be transferred to a stationary circuit through a fixed brush pressing against it",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"TEST PROBE",null,null,null,null,null,"rdl:RDS873584",null,"A <TEST PROBE> is an <ARTEFACT> and an <ELECTRICAL CONDUCTOR> used to connect electronic test equipment to the device under test",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"TURN",null,null,null,null,null,"rdl:RDS965609",null,"A <TURN> is an <ARTEFACT> and an <ELECTRICAL CONDUCTOR> formed into a curve with the end points close together but not coincident",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL CONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"WINDING",null,null,null,null,null,"rdl:RDS872684",null,"A <WINDING> is an <ARTEFACT> and an <ELECTRICAL CONDUCTOR> consisting of an assembly of interconnected turns and/or coils intended for common operation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BAR WINDING",null,null,null,null,null,"rdl:RDS7250045",null,"A <BAR WINDING> is a <WINDING> consisting of conducting bars intended for use in large rotors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BIFILAR WINDING",null,null,null,null,null,"rdl:RDS965699",null,"A <BIFILAR WINDING> is a <WINDING> consisting of a set of two coils the turns of which consist of two contiguous conductors isolated from one another.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAGE WINDING",null,null,null,null,null,"rdl:RDS7250090",null,"A <CAGE WINDING> is a <WINDING> consisting of a number of conducting bars having their extremities connected by conducting rings or plates at each end.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONCENTRATED WINDING",null,null,null,null,null,"rdl:RDS7250225",null,"A <CONCENTRATED WINDING> is a <WINDING> of a field system with salient poles or a winding, the coil sides of which occupy only one slot per pole.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECT COOLED WINDING",null,null,null,null,null,"rdl:RDS7249820",null,"A <DIRECT COOLED WINDING> is a <WINDING> mainly cooled by coolant flowing in direct contact with the cooled part through hollow conductors, tubes, ducts or channels which, regardless of their orientation, form an integral part of the winding inside the main insulation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DISTRIBUTED WINDING",null,null,null,null,null,"rdl:RDS7249865",null,"A <DISTRIBUTED WINDING> is a <WINDING> the coil sides of which occupy several slots per pole.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISTRIBUTED WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONCENTRIC WINDING",null,null,null,null,null,"rdl:RDS7250270",null,"A <CONCENTRIC WINDING> is a <DISTRIBUTED WINDING> in which the individual coils of each phase group per pole are concentric and have different coil spans",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISTRIBUTED WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIAMOND WINDING",null,null,null,null,null,"rdl:RDS7249775",null,"A <DIAMOND WINDING> is a <DISTRIBUTED WINDING> in which all coils have the same shape and coil span",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISTRIBUTED WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FRACTIONAL SLOT WINDING",null,null,null,null,null,"rdl:RDS7249415",null,"A <FRACTIONAL SLOT WINDING> is a <DISTRIBUTED WINDING> in which the number of slots per pole and per phase is a fraction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRACTIONAL SLOT WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYMMETRICAL FRACTIONAL SLOT WINDING",null,null,null,null,null,"rdl:RDS7248920",null,"A <SYMMETRICAL FRACTIONAL SLOT WINDING> is a <FRACTIONAL SLOT WINDING> in which a symmetrical polyphase voltage system is induced by the principal air-gap field",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISTRIBUTED WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRAL SLOT WINDING",null,null,null,null,null,"rdl:RDS7249550",null,"A <INTEGRAL SLOT WINDING> is a <DISTRIBUTED WINDING> in which the number of slots per pole and per phase is an integer and is the same for all poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISTRIBUTED WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE LAYER WINDING",null,null,null,null,null,"rdl:RDS7248740",null,"A <SINGLE LAYER WINDING> is a <DISTRIBUTED WINDING> in which there is only one coil side in the depth of each slot",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISTRIBUTED WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TWO LAYER WINDING",null,null,null,null,null,"rdl:RDS7248965",null,"A <TWO LAYER WINDING> is a <DISTRIBUTED WINDING> in which there are two coil sides in the depth of each slot",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TWO LAYER WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FROG-LEG WINDING",null,null,null,null,null,"rdl:RDS7249460",null,"A <FROG-LEG WINDING> is a <TWO LAYER WINDING> consisting of one lap winding and one wave winding, placed in the same slots and connected to the same commutator",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TWO LAYER WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPLIT THROW WINDING",null,null,null,null,null,"rdl:RDS7248785",null,"A <SPLIT THROW WINDING> is a <TWO LAYER WINDING> in which the conductors which constitute a coil side in one slot are not all together in another slot",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TWO LAYER WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WAVE WINDING",null,null,null,null,null,"rdl:RDS7249010",null,"A <WAVE WINDING> is a <TWO LAYER WINDING> in which the sequence of connections is such that consecutive coil sections lie under adjacent main pole pairs in one direction around the machine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WAVE WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DUPLEX WAVE WINDING",null,null,null,null,null,"rdl:RDS7249955",null,"A <DUPLEX WAVE WINDING> is a <WAVE WINDING> in which the number of parallel circuits is four whatever the number of poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WAVE WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTIPLEX WAVE WINDING",null,null,null,null,null,"rdl:RDS7249055",null,"A <MULTIPLEX WAVE WINDING> is a <WAVE WINDING> in which the number of parallel circuits is a multiple of two, other than four, whatever the number of poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WAVE WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SIMPLEX WAVE WINDING",null,null,null,null,null,"rdl:RDS7248695",null,"A <SIMPLEX WAVE WINDING> is a <WAVE WINDING> in which the number of parallel circuits is two, whatever the number of poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","COIL","WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTROMAGNETIC COIL",null,null,null,null,null,"rdl:RDS872774",null,"An <ELECTROMAGNETIC COIL> is an <ARTEFACT> and a <COIL> and a <WINDING> that is a set of series-connected turns, usually coaxial",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTROMAGNETIC COIL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BLOW-OUT COIL",null,null,null,null,null,"rdl:RDS955034",null,"A <BLOW-OUT COIL> is an <ELECTROMAGNETIC COIL> designed to produce a magnetic field arranged to deflect an arc, e.g. into an arc-chute",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTROMAGNETIC COIL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONTACTOR COIL",null,null,null,null,null,"rdl:RDS6588980",null,"A <CONTACTOR COIL> is an <ELECTROMAGNETIC COIL> that operates a contactor when energised",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTROMAGNETIC COIL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PICKUP COIL",null,null,null,null,null,"rdl:RDS7497410",null,"A <PICKUP COIL> is an <ELECTROMAGNETIC COIL> designed to produce a voltage pulse",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTROMAGNETIC COIL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RELAY COIL",null,null,null,null,null,"rdl:RDS6622098",null,"A <RELAY COIL> is an <ELECTROMAGNETIC COIL> that operates a relay when energised",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTROMAGNETIC COIL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHUNT COIL",null,null,null,null,null,"rdl:RDS5763215",null,"A <SHUNT COIL> is an <ELECTROMAGNETIC COIL> in which current passing will create a magnetic field, designed for shunt",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTROMAGNETIC COIL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLENOID",null,null,null,null,null,"rdl:RDS965654",null,"A <SOLENOID> is an <ELECTROMAGNETIC COIL> , which is a cylindrical coil, the length of which is much greater than its transverse dimensions and which is used to produce a magnetic field",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTROMAGNETIC COIL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UNDERVOLTAGE COIL",null,null,null,null,null,"rdl:RDS5763260",null,"An <UNDERVOLTAGE COIL> is an <ELECTROMAGNETIC COIL> in which current passing will create a magnetic field, designed for undervoltage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXCITATION WINDING",null,null,null,null,null,"rdl:RDS7250000",null,"An <EXCITATION WINDING> is a <WINDING> for the production of a magnetic field which is stationary with respect to that winding",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EXCITATION WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMMUTATING WINDING",null,null,null,null,null,"rdl:RDS7250135",null,"A <COMMUTATING WINDING> is an <EXITATION WINDING>, in a machine having a commutator, that carries the load current or a current proportional thereto and is so disposed as to accelerate the reversal of current in the coils undergoing commutation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EXCITATION WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPENSATING WINDING",null,null,null,null,null,"rdl:RDS7250180",null,"A <COMPENSATING WINDING> is an <EXITATION WINDING> that carries the load current or a current proportional thereto and is so disposed as to reduce distortion of the magnetic field by the load current passing through other windings",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EXCITATION WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONTROL WINDING",null,null,null,null,null,"rdl:RDS7249730",null,"A <CONTROL WINDING> is an <EXITATION WINDING> that carries an adjustable current controlling the performance of a machine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EXCITATION WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIELD WINDING",null,null,null,null,null,"rdl:RDS7249370",null,"A <FIELD WINDING> is an <EXITATION WINDING> contributing to the creation of the principal magnetic field of a machine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FIELD WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SERIES WINDING",null,null,null,null,null,"rdl:RDS7249235",null,"A <SERIES WINDING> is a <FIELD WINDING> connected in series with the armature winding and carrying the whole or part of the armature current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FIELD WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHUNT WINDING",null,null,null,null,null,"rdl:RDS7249280",null,"A <SHUNT WINDING> is a <FIELD WINDING> connected across the whole or part of the armature circuit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDIRECT COOLED WINDING",null,null,null,null,null,"rdl:RDS7249505",null,"An <INDIRECT COOLED WINDING> is a <WINDING> that is not directly cooled.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LAP WINDING",null,null,null,null,null,"rdl:RDS7249595",null,"An <LAP WINDING> is a <WINDING> in which the two ends of each coil are connected to adjacent commutator segments, so that each coil overlaps the next.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LAP WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DUPLEX LAP WINDING",null,null,null,null,null,"rdl:RDS7249910",null,"A <DUPLEX LAP WINDING> is a <LAP WINDING> in which the number of parallel circuits is equal to twice the number of poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LAP WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTIPLEX LAP WINDING",null,null,null,null,null,"rdl:RDS7249685",null,"A <MULTIPLEX LAP WINDING> is a <LAP WINDING> in which the number of parallel circuits is equal to a multiple greater than two of the number of poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LAP WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SIMPLEX LAP WINDING",null,null,null,null,null,"rdl:RDS7249325",null,"A <SIMPLEX LAP WINDING> is a <LAP WINDING> in which the number of parallel circuits is equal to the number of poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POLE CHANGING WINDING",null,null,null,null,null,"rdl:RDS7249145",null,"A <POLE CHANGING WINDING> is a <WINDING> in which two or more groups of connected coils are connected to terminals in such a manner that the number of poles of the winding can be changed by altering the interconnection of those terminals.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POLE CHANGING WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POLE AMPLITUDE MODULATING WINDING",null,null,null,null,null,"rdl:RDS7249100",null,"A <POLE AMPLITUDE MODULATING WINDING> is a <POLE CHANGING WINDING> in which non-integral rations of pole numbers are achieved by suppressing or enhancing harmonics of the magnetic field",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTOR WINDING",null,null,null,null,null,"rdl:RDS872819",null,"A <ROTOR WINDING> is a <WINDING> on the rotor of a machine.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STARTING WINDING",null,null,null,null,null,"rdl:RDS7248830",null,"A <STARTING WINDING> is a <WINDING> that helps starting a motor having insufficient standstill torque or starting a generator acting as a motor.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STARTING WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AUXILIARY STARTING WINDING",null,null,null,null,null,"rdl:RDS7250315",null,"An <AUXILIARY STARTING WINDING> is a <STARTING WINDING> of a split phase motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STATOR WINDING",null,null,null,null,null,"rdl:RDS872864",null,"A <STATOR WINDING> is a <WINDING> on the stator of a machine.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STATOR WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STATOR WINDING WITH THERMAL PROTECTION",null,null,null,null,null,"rdl:RDS6480801",null,"A <STATOR WINDING WITH THERMAL PROTECTION> is a <STATOR WINDING> which is equipped with a thermal protection to avoid overheating",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STATOR WINDING WITH THERMAL PROTECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOTOR STATOR WINDING WITH 2 RTD THERMISTORS",null,null,null,null,null,"rdl:RDS6480953",null,"A <MOTOR STATOR WINDING WITH 2 RTD THERMISTORS> is a <STATOR WINDING WITH THERMAL PROTECTION> with two built in RTD (100 Ohm Platinum) 3-wire thermistors to protect motor from overheating",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STATOR WINDING WITH THERMAL PROTECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOTOR STATOR WINDING WITH 3 PTC THERMISTORS",null,null,null,null,null,"rdl:RDS6480908",null,"A <MOTOR STATOR WINDING WITH 3 PTC THERMISTORS> is a <STATOR WINDING WITH THERMAL PROTECTION> with three built in PTC thermistors to protect motor from overheating",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STATOR WINDING WITH THERMAL PROTECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOTOR STATOR WINDING WITH 6 PTC THERMISTORS",null,null,null,null,null,"rdl:RDS6480863",null,"A <MOTOR STATOR WINDING WITH 6 PTC THERMISTORS> is a <STATOR WINDING WITH THERMAL PROTECTION> with six built in PTC thermistors to protect motor from overheating",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMAL RATED WINDING",null,null,null,null,null,"rdl:RDS4253387",null,"A <THERMAL RATED WINDING> is a <WINDING> in which the temperature rise is within specified limits.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRANSFORMER WINDING",null,null,null,null,null,"rdl:RDS872909",null,"A <TRANSFORMER WINDING> is a <WINDING> that is an assembly of turns forming an electric circuit associated with one of the voltages assigned to the transformer.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMMON WINDING",null,null,null,null,null,"rdl:RDS6588635",null,"A <COMMON WINDING> is a <TRANSFORMER WINDING> that is the common part of the windings of an auto-transformer",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DELTA CONNECTED WINDING",null,null,null,null,null,"rdl:RDS6589490",null,"A <DELTA CONNECTED WINDING> is a <TRANSFORMER WINDING> so arranged that the phase windings of a three-phase transformer or reactor, or the windings for the same rated voltage of single-phase transformer or reactors associated in a three-phase bank, are connected in series to form a closed circuit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESIDUAL VOLTAGE WINDING",null,null,null,null,null,"rdl:RDS6622203",null,"A <RESIDUAL VOLTAGE WINDING> is a <TRANSFORMER WINDING> between the terminals of which is produced the residual voltage or one of the three component voltages which when added together constitute the residual voltage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SANDWICH WINDING",null,null,null,null,null,"rdl:RDS6622548",null,"A <SANDWICH WINDING> is a <TRANSFORMER WINDING> that is an arrangement where the windings or parts of windings are arranged axially",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STAR CONNECTED WINDING",null,null,null,null,null,"rdl:RDS6623703",null,"A <STAR CONNECTED WINDING> is a <TRANSFORMER WINDING> so arranged that one end of each of the phase windings of a polyphase transformer or reactor, or of each of the windings for the same rated voltage of single-phase transformers or reactors associated in a polyphase bank, is connected",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRANSFORMER PRIMARY WINDING",null,null,null,null,null,"rdl:RDS16200233",null,"A <TRANSFORMER PRIMARY WINDING> is a <TRANSFORMER WINDING> sitting on the ingoing side of a transformer",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER PRIMARY WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT TRANSFORMER PRIMARY WINDING",null,null,null,null,null,"rdl:RDS6589625",null,"A <CURRENT TRANSFORMER PRIMARY WINDING> is a <TRANSFORMER PRIMARY WINDING> through which flows the current to be transformed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER PRIMARY WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER TRANSFORMER PRIMARY WINDING",null,null,null,null,null,"rdl:RDS6698671",null,"A <POWER TRANSFORMER PRIMARY WINDING> is a <TRANSFORMER PRIMARY WINDING> intended to be the winding of a power transformer",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER PRIMARY WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE TRANSFORMER PRIMARY WINDING",null,null,null,null,null,"rdl:RDS6625008",null,"A <VOLTAGE TRANSFORMER PRIMARY WINDING> is a <TRANSFORMER PRIMARY WINDING> to which the voltage to be transformed is applied",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRANSFORMER SECONDARY WINDING",null,null,null,null,null,"rdl:RDS16200120",null,"A <TRANSFORMER SECONDARY WINDING> is a <TRANSFORMER WINDING> that supplies the current or voltage circuits of measuring instruments, meters, protective or control devices",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER SECONDARY WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT TRANSFORMER SECONDARY WINDING",null,null,null,null,null,"rdl:RDS6589415",null,"A <CURRENT TRANSFORMER SECONDARY WINDING> is a <TRANSFORMER SECONDARY WINDING> that supplies the current circuits of measuring instruments, meters, protective or control devices",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER SECONDARY WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER TRANSFORMER SECONDARY WINDING",null,null,null,null,null,"rdl:RDS6698767",null,"A <POWER TRANSFORMER SECONDARY WINDING> is a <TRANSFORMER SECONDARY WINDING> intended to be the secondary winding of a power transformer",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER SECONDARY WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE TRANSFORMER SECONDARY WINDING",null,null,null,null,null,"rdl:RDS6621993",null,"A <VOLTAGE TRANSFORMER SECONDARY WINDING> is a <TRANSFORMER SECONDARY WINDING> that supplies voltage to the circuits of measuring instruments, meters, protective or control devices",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER WINDING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ZIGZAG CONNECTED WINDING",null,null,null,null,null,"rdl:RDS6625248",null,"A <ZIGZAG CONNECTED WINDING> is a <TRANSFORMER WINDING> in which one end of each phase winding of a polyphase transformer or reactor is connected to a common point, i.e. the neutral point, and each phase winding consists of two parts in which phase-displaced voltages are induced",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL ELEMENT","FILTER",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL FILTER",null,null,null,null,null,"rdl:RDS859994",null,"An <ELECTRICAL FILTER> is a <FILTER> and an <ELECTRICAL ELEMENT> function and that is a passive circuit that attenuates all signals except those within one or more frequency bands",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","ELECTRICAL FILTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"AC FILTER",null,null,null,null,null,"rdl:RDS953324",null,"An <AC FILTER> is an <ARTEFACT> and an <ELECTRICAL FILTER> on the AC side of a converter, designed to reduce the circulation of harmonic currents in the associated system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL FILTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"BAND-PASS FILTER",null,null,null,null,null,"rdl:RDS987074",null,"A <BAND-PASS FILTER> is an <ARTEFACT> and an <ELECTRICAL FILTER> with a very low attenuation for currents within given limits of frequency",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL FILTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"BAND-STOP FILTER",null,null,null,null,null,"rdl:RDS987119",null,"A <BAND-STOP FILTER> is an <ARTEFACT> and an <ELECTRICAL FILTER> having a single stop-band with specified cut-off frequencies different from zero or infinite",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL FILTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"DC FILTER",null,null,null,null,null,"rdl:RDS6234045",null,"A <DC FILTER> is an <ARTEFACT> and an <ELECTRICAL FILTER> on the DC side of a converter, designed to reduce the ripple in the associated system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL FILTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"HIGH-PASS FILTER",null,null,null,null,null,"rdl:RDS987029",null,"A <HIGH-PASS FILTER> is an <ARTEFACT> and an <ELECTRICAL FILTER> having a single pass-band extending from a specified cut-off frequency upwards",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL FILTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"LOW-PASS FILTER",null,null,null,null,null,"rdl:RDS986984",null,"A <LOW-PASS FILTER> is an <ARTEFACT> and an <ELECTRICAL FILTER> having a single pass-band extending from zero frequency to a specified cut-off frequency",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT","HEATER ELEMENT",null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL HEATING ELEMENT",null,null,null,null,null,"rdl:RDS444329",null,"An <ELECTRICAL HEATING ELEMENT> is an <ARTEFACT> and an <ELECTRICAL ELEMENT> and a <HEATER ELEMENT> in which heat is produced by the passage of an electric current through a resistance",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","COIL","ELECTRICAL HEATING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL HEATER COIL",null,null,null,null,null,"rdl:RDS414224",null,"An <ELECTRICAL HEATER COIL> is an <ARTEFACT> and a <COIL> and an <ELECTRICAL HEATING ELEMENT> for heating a fluid by electric power",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL HEATING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GLOW PLUG",null,null,null,null,null,"rdl:RDS406110191",null,"A <GLOW PLUG> is an <ELECTRICAL HEATING ELEMENT> that is a heating device used to aid starting diesel engines.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC TUBE",null,null,null,null,null,"rdl:RDS987164",null,"An <ELECTRONIC TUBE> is an <ARTEFACT> and an <ELECTRICAL ELEMENT> , that is a sealed container containing two or more electrodes between which an electric current can be made to flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC TUBE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIODE",null,null,null,null,null,"rdl:RDS875834",null,"A <DIODE> is an <ELECTRONIC TUBE> containing only an anode and a cathode",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIGHT-EMITTING DIODE",null,null,null,null,null,"rdl:RDS5763400",null,"A <LIGHT-EMITTING DIODE> is a <DIODE>, semiconductor type, that radiates light in the visible region. Used in alphanumeric displays and as an indicator or warning lamp.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC TUBE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS-FILLED TUBE",null,null,null,null,null,"rdl:RDS987254",null,"A <GAS-FILLED TUBE> is an <ELECTRONIC TUBE> in which the electric characteristics are substantially established by the ionization of deliberately introduced vapour or gas",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC TUBE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VACUUM TUBE",null,null,null,null,null,"rdl:RDS987209",null,"A <VACUUM TUBE> is an <ELECTRONIC TUBE> evacuated to such a degree that its electric characteristics are essentially unaffected by the ionization of any residual vapour or gas",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT","PROTECTOR",null,null,null,null,null,null,null,null,null,null,null,"FUSE",null,null,null,null,null,"rdl:RDS875024",null,"A <FUSE> is an <ARTEFACT> and a <PROTECTOR> and an <ELECTRICAL ELEMENT> that opens the circuit in which it is inserted by breaking the current when this exceeds a given value for a sufficient time",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FUSE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DROP-OUT FUSE",null,null,null,null,null,"rdl:RDS955889",null,"A <DROP-OUT FUSE> is a <FUSE> in which the fuse-carrier automatically drops into a position providing an isolating distance after the fuse has operated.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FUSE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXPULSION FUSE",null,null,null,null,null,"rdl:RDS956069",null,"An <EXPULSION FUSE> is a <FUSE> in which operation is accomplished by expulsion of gases produced by the arc.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FUSE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GLASS FUSE",null,null,null,null,null,"rdl:RDS5761931",null,"A <GLASS FUSE> is a <FUSE> that has a housing made of glass.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FUSE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HRC FUSE",null,null,null,null,null,"rdl:RDS875249",null,"An <HRC FUSE> is a <FUSE> that during its operation limits the circuit current to a value much lower than the peak value of the prospective current.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FUSE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDICATING FUSE",null,null,null,null,null,"rdl:RDS956294",null,"An <INDICATING FUSE> is a <FUSE> provided with an indicator.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FUSE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER ELECTRONIC FUSE",null,null,null,null,null,"rdl:RDS875339",null,"A <POWER ELECTRONIC FUSE> is a <FUSE> that has a current/time rupture characteristic suitable to protect power semiconductor devices.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FUSE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STRIKER FUSE",null,null,null,null,null,"rdl:RDS956249",null,"A <STRIKER FUSE> is a <FUSE> provided with a striker.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","FUSE","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"SWITCH-FUSE",null,null,null,null,null,"rdl:RDS934874",null,"A <SWITCH-FUSE> is an <ARTEFACT> and a <SWITCHING DEVICE> and a <FUSE> in which one or more poles have a fuse in series in a composite unit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FUSE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THYRISTOR FUSE",null,null,null,null,null,"rdl:RDS5764322",null,"A <THYRISTOR FUSE> is a <FUSE> of special characteristics connected in series with one or more thyristors to protect the thyristor or other circuit components, or both.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"JUMPER BOARD",null,null,null,null,null,"rdl:RDS1006109",null,"A <JUMPER BOARD> is an <ARTEFACT> and an <ELECTRICAL ELEMENT> function, consisting of terminals and connecting devices so arranged that they can be cross-connected in any desired manner",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL ELEMENT","LIMITER",null,null,null,null,null,null,null,null,null,null,null,null,"POWER LIMITER",null,null,null,null,null,"rdl:RDS316529",null,"A <POWER LIMITER> is an <ELECTRICAL ELEMENT> and a <LIMITER> whose output is restricted to a certain range of values irrespective of the size of the input",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT","LIMITER",null,null,null,null,null,null,null,null,null,null,null,"RESISTOR",null,null,null,null,null,"rdl:RDS860174",null,"A <RESISTOR> is an <ARTEFACT> and an <ELECTRICAL ELEMENT>and a <LIMITER> that impedes the flow of an electric current, used to develop a voltage drop across itself or to limit current flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIVERTER","RESISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"DIVERTER SPOOL",null,null,null,null,null,"rdl:RDS5786948",null,"A <DIVERTER SPOOL> is a <RESISTOR> and a <DIVERTER>, connected in parallel with the series winding or the compole winding of a d.c. machine in order to divert some of the current from it, thereby varying the m.m.f. produced by the winding",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RESISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTHING RESISTOR",null,null,null,null,null,"rdl:RDS1070896071",null,"An <EARTHING RESISTOR> is a <RESISTOR> through which the neutral point of a supply system is earthed, in order to limit the current that flows on the occurrence of an earth fault",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RESISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIXED RESISTOR",null,null,null,null,null,"rdl:RDS875564",null,"A <FIXED RESISTOR> is a <RESISTOR> and a fixed resistance at a given temperature independent of voltage or current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RESISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NEUTRAL RESISTOR",null,null,null,null,null,"rdl:RDS1186874",null,"A <NEUTRAL RESISTOR> is a <RESISTOR> that is used between earth and the neutral point in a transformer or generator",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RESISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VARIABLE RESISTOR",null,null,null,null,null,"rdl:RDS875609",null,"A <VARIABLE RESISTOR> is a <RESISTOR> of which the resistance can be varied",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VARIABLE RESISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-LINEAR VARIABLE RESISTOR",null,null,null,null,null,"rdl:RDS875699",null,"A <NON-LINEAR VARIABLE RESISTOR> is a <VARIABLE RESISTOR> in which the resistance varies in a non-linear manner.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"NON-LINEAR VARIABLE RESISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE DEPENDENT RESISTOR",null,null,null,null,null,"rdl:RDS875744",null,"A <VOLTAGE DEPENDENT RESISTOR> is a <NON-LINEAR VARIABLE RESISTOR> in which the resistance depends on the voltage across it.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VARIABLE RESISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POTENTIOMETER",null,null,null,null,null,"rdl:RDS875654",null,"A <POTENTIOMETER> is a <VARIABLE RESISTOR> with one or more intermediate tappings allowing fractions of the voltage across the resistor to be obtained.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RESISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VARISTOR",null,null,null,null,null,"rdl:RDS966104",null,"A <VARISTOR> is a <RESISTOR> that is a semiconductor diode whose resistance varies non-linearly with the applied voltage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"SEMICONDUCTOR",null,null,null,null,null,"rdl:RDS860309",null,"A <SEMICONDUCTOR> is an <ARTEFACT> and an <ELECTRICAL ELEMENT>, whose essential characteristics are due to the flow of charge carriers within a semi-conductor material",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMBINATOR",null,null,null,null,null,"rdl:RDS13611515",null,"A <COMBINATOR> is a <SEMICONDUCTOR> that adds two ore more incoming signals to one signal out",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPARATOR",null,null,null,null,null,"rdl:RDS13611200",null,"A <COMPARATOR> is a <SEMICONDUCTOR> that compares two ore more signals and returns one signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PHOTOELECTRIC TRANSDUCER","SEMICONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"PHOTODIODE",null,null,null,null,null,"rdl:RDS6646330",null,"A <PHOTODIODE> is a <PHOTOELECTRIC TRANSDUCER> and a <SEMICONDUCTOR> that is a diode that exhibits sensitivity to light, either by varying its electrical resistance like a photoresistor, or generating a electric potential in the manner of a photoelectric cell",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEMICONDUCTOR DIODE",null,null,null,null,null,"rdl:RDS6646255",null,"A <SEMICONDUCTOR DIODE> is a <SEMICONDUCTOR> whose rectifying action depends on the properties of a junction between a semiconductor and either a metal or another type of semiconductor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR DIODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FREQUENCY-MULTIPLICATION DIODE",null,null,null,null,null,"rdl:RDS6646405",null,"A <FREQUENCY-MULTIPLICATION DIODE> is a <SEMICONDUCTOR DIODE> designed for multiplying the frequency of a signal.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR DIODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIXER DIODE",null,null,null,null,null,"rdl:RDS6646480",null,"A <MIXER DIODE> is a <SEMICONDUCTOR DIODE> designed for frequency conversion of signals by means of a local oscillator.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR DIODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEMICONDUCTOR RECTIFIER DIODE",null,null,null,null,null,"rdl:RDS6646855",null,"A <SEMICONDUCTOR RECTIFIER DIODE> is a <SEMICONDUCTOR DIODE> designed for rectification and including its associated mounting and cooling attachments if integral with it.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR DIODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SWITCHING DIODE",null,null,null,null,null,"rdl:RDS6646585",null,"A <SWITCHING DIODE> is a <SEMICONDUCTOR DIODE> designed for a fast transition from a high-impedance state to a low impedance state and vice versa, depending on the polarity of the applied voltage.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR DIODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TUNNEL DIODE",null,null,null,null,null,"rdl:RDS6646660",null,"A <TUNNEL DIODE> is a <SEMICONDUCTOR DIODE> that is a two-terminal semiconductor device, consisting of a heavily doped p-n junction, which has negative resistance at low voltage due to quantum-mechanical tunnelling and is principally used as a high-speed switching device.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUNNEL DIODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UNITUNNEL DIODE",null,null,null,null,null,"rdl:RDS6646975",null,"A <UNITUNNEL DIODE> is a <TUNNEL DIODE> whose peak and valley point currents are approximately equal.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR DIODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VARIABLE-CAPACITANCE DIODE",null,null,null,null,null,"rdl:RDS6646735",null,"A <VARIABLE-CAPACITANCE DIODE> is a <SEMICONDUCTOR DIODE>, the terminal capacitance of which varies in a defined manner as a function of applied voltage when biased in the reverse direction, and that is intended for specific applications of this capacitance-voltage relationship.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR DIODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE-REFERENCE DIODE",null,null,null,null,null,"rdl:RDS6646810",null,"A <VOLTAGE-REFERENCE DIODE> is a <SEMICONDUCTOR DIODE> that develops across its terminals a reference voltage of specified accuracy, when biased to operate within a specified current range.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR DIODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE-REGULATOR DIODE",null,null,null,null,null,"rdl:RDS6646900",null,"A <VOLTAGE-REGULATOR DIODE> is a <SEMICONDUCTOR DIODE> that develops across its terminals an essentially constant voltage throughout specified current range.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR DIODE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ZENER DIODE",null,null,null,null,null,"rdl:RDS5760900",null,"A <ZENER DIODE> is a <SEMICONDUCTOR DIODE> with a characteristic showing a sharp increase in reverse current at a certain critical voltage.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THYRISTOR",null,null,null,null,null,"rdl:RDS876014",null,"A <THYRISTOR> is a <SEMICONDUCTOR> that is a three-terminal semiconductor rectifier made up of four layers, p-n-p-n, so that when the fourth is positive with respect to the first, a voltage pulse applied to the third layer initiates a flow of current through the device which continues as long as it is greater than some minimum value",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THYRISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BIDIRECTIONAL DIODE THYRISTOR",null,null,null,null,null,"rdl:RDS6568325",null,"A <BIDIRECTIONAL DIODE THYRISTOR> is a <THYRISTOR> having two terminals and substantially the same switching behaviour in the first and third quadrants of the current-voltage characteristic.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THYRISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BIDIRECTIONAL TRIODE THYRISTOR",null,null,null,null,null,"rdl:RDS6568130",null,"A <BIDIRECTIONAL TRIODE THYRISTOR> is a <THYRISTOR> having three terminals and substantially the same switching behaviour in the first and third quadrants of the current-voltage characteristic.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THYRISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REVERSE BLOCKING DIODE THYRISTOR",null,null,null,null,null,"rdl:RDS6622278",null,"A <REVERSE BLOCKING DIODE THYRISTOR> is a <THYRISTOR> having two terminals and which for negative anode voltage does not switch, but exhibits reverse blocking state.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THYRISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REVERSE BLOCKING TRIODE THYRISTOR",null,null,null,null,null,"rdl:RDS6622323",null,"A <REVERSE BLOCKING TRIODE THYRISTOR> is a <THYRISTOR> having three terminals and which for negative anode voltage does not switch, but exhibits a reverse blocking state.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THYRISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REVERSE CONDUCTING DIODE THYRISTOR",null,null,null,null,null,"rdl:RDS6622398",null,"A <REVERSE CONDUCTING DIODE THYRISTOR> is a <THYRISTOR> having two terminals and which for negative anode voltage does not switch and conducts large currents at voltages comparable in magnitude to the forward on-state voltage.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THYRISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REVERSE CONDUCTING TRIODE THYRISTOR",null,null,null,null,null,"rdl:RDS6622473",null,"A <REVERSE CONDUCTING TRIODE THYRISTOR> is a <THYRISTOR> having three terminals and which for negative anode voltage does not switch and conducts large currents at voltages comparable in magnitude to the forward on-state voltage.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRANSISTOR",null,null,null,null,null,"rdl:RDS875789",null,"A <TRANSISTOR> is a <SEMICONDUCTOR>, usually having three terminals and two junctions, in which the load current can be made to be proportional to a small input current, so that it is functionally equivalent to a valve but is much smaller and more robust, operates at lower voltages, and consumes less power and produces less heat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BIDIRECTIONAL TRANSISTOR",null,null,null,null,null,"rdl:RDS6568205",null,"A <BIDIRECTIONAL TRANSISTOR> is a <TRANSISTOR> that has substantially the same electrical characteristics when the electrodes normally designated as emitter (or source) and collector (or drain) are interchanged.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BIPOLAR JUNCTION TRANSISTOR",null,null,null,null,null,"rdl:RDS6570815",null,"A <BIPOLAR JUNCTION TRANSISTOR> is a <TRANSISTOR> having at least two junctions and whose functioning depends on both majority carriers and minority carriers.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PHOTOTRANSISTOR",null,null,null,null,null,"rdl:RDS6647050",null,"A <PHOTOTRANSISTOR> is a <TRANSISTOR> that responds to incident light by generating and amplifying an electric current.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UNIPOLAR TRANSISTOR",null,null,null,null,null,"rdl:RDS6647125",null,"A <UNIPOLAR TRANSISTOR> is a <TRANSISTOR> whose functioning depends predominantly on charge carriers of one polarity.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"UNIPOLAR TRANSISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIELD-EFFECT TRANSISTOR",null,null,null,null,null,"rdl:RDS5779444",null,"A <FIELD-EFFECT TRANSISTOR> is a <UNIPOLAR TRANSISTOR> in which the majority carriers flow along a channel whose effective resistance is controlled by a transverse electric field produced by a reverse bias applied to a gate region surrounding the channel, the gate and the channel being of opposite conductivity types.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FIELD-EFFECT TRANSISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSULATED-GATE FIELD-EFFECT TRANSISTOR",null,null,null,null,null,"rdl:RDS6647200",null,"An <INSULATED-GATE FIELD-EFFECT TRANSISTOR> is a <FIELD-EFFECT TRANSISTOR> having one or more gate electrodes which are electrically insulated from the channel.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSULATED-GATE FIELD-EFFECT TRANSISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"METAL-OXIDE-SEMICONDUCTOR FIELD-EFFECT TRANSISTOR",null,null,null,null,null,"rdl:RDS6647335",null,"A <METAL-OXIDE-SEMICONDUCTOR FIELD-EFFECT TRANSISTOR> is an <INSULATED-GATE FIELD-EFFECT TRANSISTOR> in which the insulating layer between each gate electrode and the channel is oxide material.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FIELD-EFFECT TRANSISTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JUNCTION-GATE FIELD-EFFECT TRANSISTOR",null,null,null,null,null,"rdl:RDS6647410",null,"A <JUNCTION-GATE FIELD-EFFECT TRANSISTOR> is a <FIELD-EFFECT TRANSISTOR> having one or more gate regions which form PN junctions with the channel.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"SHUTTER",null,null,null,null,null,"rdl:RDS954089",null,"A <SHUTTER> is an <ARTEFACT> and an <ELECTRICAL ELEMENT> function and that is a part of an assembly that can be moved from a position where it permits contacts of a removable part to engage fixed contacts, to a position where it becomes a part of the enclosure or partition shielding the fixed contacts",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"SOLENOID VALVE",null,null,null,null,null,"rdl:RDS431279",null,"A <SOLENOID VALVE> is a <VALVE> and an <ACTUATED VALVE> and an <ELECTRIC ELEMENT> with a linear action, fitted with a solenoid for quick operation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,"rdl:RDS5791925",null,"A <DIRECTIONAL SOLENOID VALVE> is a <SOLENOID VALVE> that operates in only one direction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CORE-DISC SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1460612641",null,"A <CORE-DISC SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a core-disc valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECTIONAL SPOOL SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465954351",null,"A <DIRECTIONAL SPOOL SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a directional spool valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLAPPER DISC SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465901811",null,"A <FLAPPER DISC SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a swing check valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOATING DIAPHRAGM SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465915931",null,"A <FLOATING DIAPHRAGM SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a floating diaphragm valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HUNG DIAPHRAGM SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465943841",null,"A <HUNG DIAPHRAGM SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a hung diaphragm valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVER DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465939741",null,"A <LEVER DIRECTIONAL SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a lever operated valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PISTON SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465946921",null,"A <PISTON SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a piston valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POPPET DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1460663261",null,"A <POPPET DIRECTIONAL SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a poppet valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLIDE DISC DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465952771",null,"A <SLIDE DISC DIRECTIONAL SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a sliding disc valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"SPRING RETURN SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1472598331",null,"An <SPRING RETURN SOLENOID VALVE> is an <ARTEFACT> and a <SOLENOID VALVE> equipped with a spring reurn mechanism that closes the valve when de-enegized",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"TRANSDUCTOR",null,null,null,null,null,"rdl:RDS888794",null,"A <TRANSDUCTOR> is an <ARTEFACT> and an <ELECTRICAL ELEMENT> function, having a dc winding to control the saturation of a core and an ac winding whose impedance is thereby changed, so that a small change in direct current produces a large change in alternating current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL DEVICE","REACTOR",null,null,null,null,null,null,null,null,null,null,"ELECTRICAL REACTOR",null,null,null,null,null,"rdl:RDS859859",null,"An <ELECTRICAL REACTOR> is an <ARTEFACT> and an <ELECTRICAL DEVICE> and a <REACT0R> that is electrically powered",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL REACTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"DRY-TYPE REACTOR",null,null,null,null,null,"rdl:RDS6590270",null,"A <DRY-TYPE REACTOR> is an <ELECTRICAL REACTOR> of which the magnetic circuit and winding are not immersed in an insulating liquid",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DRY-TYPE REACTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENCAPSULATED-WINDING DRY-TYPE REACTOR",null,null,null,null,null,"rdl:RDS6590570",null,"An <ENCAPSULATED-WINDING DRY-TYPE REACTOR> is a <DRY-TYPE REACTOR> having its winding encapsulated with solid insulation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL REACTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"SATURABLE REACTOR",null,null,null,null,null,"rdl:RDS888749",null,"A <SATURABLE REACTOR> is an <ELECTRICAL REACTOR> whose magnetic circuit in normal operation becomes saturated when the current exceeds a certain value",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL REACTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"SEALED REACTOR",null,null,null,null,null,"rdl:RDS6622728",null,"A <SEALED REACTOR> is an <ELECTRICAL REACTOR> that is non-breathing, that is, so sealed that there can be no significant interchange between its contents and the external atmosphere",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL REACTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE-PHASE NEUTRAL REACTOR",null,null,null,null,null,"rdl:RDS6624318",null,"A <THREE-PHASE NEUTRAL REACTOR> is an <ELECTRICAL REACTOR>, that is intended for connection in a network without a neutral to provide an artificial neutral",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"OSCILLATOR",null,null,null,null,null,"rdl:RDS13610885",null,"An <OSCILLATOR> is an <ELECTRICAL DEVICE> that is a source of alternating current of any frequency, which is sustained in a circuit by a valve or transisstor using positive feedback principle or by a negative resistance device. There are two types: 1) stabletype, in which frequency is determined by a line or a tuned (LC) circuit, waveform being substantially sinusoidal, and 2) relaxation-type, in which frequency is determined by resistors and capacitors, waveform havning considerable content of harmonics. Also applied to mechanical systems, velocities being equivalent to currents",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","OSCILLATOR",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC OSCILLATOR",null,null,null,null,null,"rdl:RDS986939",null,"An <ELECTRIC OSCILLATOR> is an <ARTEFACT> and a <OSCILLATOR> that is an apparatus for generating oscillatory currents by non-mechanical means",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","OSCILLATOR",null,null,null,null,null,null,null,null,null,null,null,null,"MECHANICAL OSCILLATOR",null,null,null,null,null,"rdl:RDS2220031",null,"A <MECHANICAL OSCILLATOR> is an <ARTEFACT> and a <OSCILLATOR> that is an apparatus for generating oscillatory currents by mechanical means",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","OSCILLATOR","VIBRATION DETECTOR",null,null,null,null,null,null,null,null,null,null,null,"VIBRATION OSCILLATOR-DETECTOR",null,null,null,null,null,"rdl:RDS14206609",null,"A <VIBRATION OSCILLATOR-DETECTOR> is an <INSTRUMENTATION ITEM> and a <VIBRATION DETECTOR> and an <OSCILLATOR> that detects motion that can be translated into a signal which can be displayed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL DEVICE",null,null,null,null,null,null,null,null,null,null,null,"THERMAL RATED ELECTRICAL ARTEFACT",null,null,null,null,null,"rdl:RDS948374",null,"A <THERMAL RATED ELECTRICAL ARTEFACT> is an <ARTEFACT> and an <ELECTRICAL DEVICE> that has a defined endurance of the electrical insulation of the product based on the maximum temperature appropriate to the product under rated load and other conditions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]