{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["RDL browser","Settings","about","Results1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"RDL browser","index":0,"n_rows":73,"n_cols":8,"rows_kept":73,"cut":false,"hidden":false,"merged":[[0,0,0,4]]}
["RDL2 browser to spreadsheet tool version 75",null,null,null,null,null,"Endpoint: http://data.15926.org/rdl/"]
["Contact: onno.paap@gmail.com",null,null,null,null,"Action","ANALOGUE TO DIGITAL SIGNAL CONVERTER","http://data.15926.org/rdl/RDS851354"]
[null,null,null,null,null,"Action","CATALYTIC CONVERTER","http://data.15926.org/rdl/RDS4316590660"]
["Search:","CONVERTER",null,null,null,"Action","CHEMICAL CONVERTER","http://data.15926.org/rdl/RDS4316590754"]
[null,null,null,null,null,"Action","CHEMICAL TO MECHANICAL ENERGY CONVERTER","http://data.15926.org/rdl/RDS278234"]
[null,null,null,null,null,"Action","COMMUTATOR TYPE FREQUENCY CONVERTER","http://data.15926.org/rdl/RDS7222063"]
[null,null,null,null,null,"Action","CONVERTER","http://data.15926.org/rdl/RDS13048460"]
[null,null,null,null,null,"Action","CONVERTER DATA SHEET","http://data.15926.org/rdl/RDS17985509"]
[null,null,null,null,null,"Action","CONVERTER DATA SHEET DEFINITION","http://data.15926.org/rdl/RDS6820510"]
[null,null,null,null,null,"Action","CONVERTER SUBSTATION","http://data.15926.org/rdl/RDS958229"]
[null,null,null,null,null,"Action","CURRENT TO CURRENT SIGNAL CONVERTER","http://data.15926.org/rdl/RDS5762894"]
[null,null,null,null,null,"Action","CURRENT TO PRESSURE SIGNAL CONVERTER","http://data.15926.org/rdl/RDS460484"]
[null,"Note: first set coloring on in Settings",null,null,null,"Action","CURRENT TO VOLTAGE SIGNAL CONVERTER","http://data.15926.org/rdl/RDS851219"]
[null,"Coloring (containing this string will give this color)",null,null,null,"Action","CYCLOCONVERTER","http://data.15926.org/rdl/RDS952604"]
[null,"ClassOfFunctionalObject",null,null,null,"Action","DIGITAL TO ANALOGUE SIGNAL CONVERTER","http://data.15926.org/rdl/RDS851399"]
[null,"ClassOfInanimatePhysicalObject ",null,null,null,"Action","DIRECT AC CONVERTER","http://data.15926.org/rdl/RDS6234000"]
[null,null,null,null,null,"Action","DIRECT DC CONVERTER","http://data.15926.org/rdl/RDS952694"]
[null,null,null,null,null,"Action","DOUBLE CONVERTER","http://data.15926.org/rdl/RDS953009"]
[null,null,null,null,null,"Action","ELECTRIC CONVERTER","http://data.15926.org/rdl/RDS885059"]
[null,null,null,null,null,"Action","ELECTRIC POWER CONVERTER","http://data.15926.org/rdl/RDS281924"]
[null,null,null,null,null,"Action","ELECTRIC TO ELECTRIC ENERGY CONVERTER","http://data.15926.org/rdl/RDS222503"]
[null,null,null,null,null,"Action","ELECTRIC TO MECHANICAL ENERGY CONVERTER","http://data.15926.org/rdl/RDS2220072"]
[null,null,null,null,null,"Action","ELECTRICAL TO OPTICAL CONVERTER","http://data.15926.org/rdl/RDS1066706051"]
[null,null,null,null,null,"Action","ELECTRICAL TO OPTICAL SIGNAL CONVERTER","http://data.15926.org/rdl/RDS1066703201"]
[null,"Namespace replacer (definition containing this string replaces the namespace)",null,null,null,"Action","ELECTRONIC AC CONVERTER","http://data.15926.org/rdl/RDS6233775"]
[null,"API","API:",null,null,"Action","ELECTRONIC AC VOLTAGE CONVERTER","http://data.15926.org/rdl/RDS952559"]
[null,"ASME","ASME:",null,null,"Action","ELECTRONIC CONVERTER","http://data.15926.org/rdl/RDS952199"]
[null,"ASTM","ASTM:",null,null,"Action","ELECTRONIC DC CONVERTER","http://data.15926.org/rdl/RDS952649"]
[null,"DIN","DIN:",null,null,"Action","ELECTRONIC DC POWER CONVERTER","http://data.15926.org/rdl/RDS953189"]
[null,"EN","EN:",null,null,"Action","ELECTRONIC FREQUENCY CONVERTER","http://data.15926.org/rdl/RDS17859175"]
[null,"ISO","ISO:",null,null,"Action","ELECTRONIC PHASE CONVERTER","http://data.15926.org/rdl/RDS952514"]
[null,"NORSOK","NOR:",null,null,"Action","ENERGY CONVERTER","http://data.15926.org/rdl/RDS339575363"]
[null,"NPD","NOR:",null,null,"Action","ENERGY CONVERTER EQUIPMENT CLASS","http://data.15926.org/rdl/RDS204164"]
[null,"NS","NOR:",null,null,"Action","FLUID TOFROM FLUID POWER CONVERTER","http://data.15926.org/rdl/RDS280124"]
[null,"ROSEMOUNT","ROS:",null,null,"Action","FLUID TOFROM MECHANICAL POWER CONVERTER","http://data.15926.org/rdl/RDS278189"]
[null,"SAE","SAE:",null,null,"Action","FOUR-QUADRANT CONVERTER","http://data.15926.org/rdl/RDS952874"]
[null,"SIEMENS","SIE:",null,null,"Action","FREQUENCY CONVERTER SUBSTATION","http://data.15926.org/rdl/RDS958274"]
[null,"SKOTSELV","SKOT:",null,null,"Action","FREQUENCY TO CURRENT SIGNAL CONVERTER","http://data.15926.org/rdl/RDS1011104"]
[null,"TWR","TWR:",null,null,"Action","FREQUENCY TO VOLTAGE SIGNAL CONVERTER","http://data.15926.org/rdl/RDS1011149"]
[null,null,null,null,null,"Action","HYDRAULIC TO MECHANICAL ENERGY CONVERTER","http://data.15926.org/rdl/RDS279944"]
[null,null,null,null,null,"Action","HYDRAULIC TO ROTATION ENERGY CONVERTER","http://data.15926.org/rdl/RDS2220074"]
[null,null,null,null,null,"Action","HYDRAULIC TORQUE CONVERTER","http://data.15926.org/rdl/RDS891179"]
[null,null,null,null,null,"Action","INDIRECT AC CONVERTER","http://data.15926.org/rdl/RDS952424"]
[null,null,null,null,null,"Action","INDIRECT DC CONVERTER","http://data.15926.org/rdl/RDS952739"]
[null,null,null,null,null,"Action","INDUCTION FREQUENCY CONVERTER","http://data.15926.org/rdl/RDS7222125"]
[null,null,null,null,null,"Action","INDUCTOR FREQUENCY CONVERTER","http://data.15926.org/rdl/RDS7222187"]
[null,null,null,null,null,"Action","KINETIC TO MECHANICAL ENERGY CONVERTER","http://data.15926.org/rdl/RDS2220075"]
[null,null,null,null,null,"Action","LINEAR CONVERTER","http://data.15926.org/rdl/RDS278324"]
[null,null,null,null,null,"Action","MECHANICAL TO ELECTRIC ENERGY CONVERTER","http://data.15926.org/rdl/RDS2220076"]
[null,null,null,null,null,"Action","MECHANICAL TO MECHANICAL ENERGY CONVERTER","http://data.15926.org/rdl/RDS2225766"]
[null,null,null,null,null,"Action","ONE-QUADRANT CONVERTER","http://data.15926.org/rdl/RDS952784"]
[null,null,null,null,null,"Action","OPTICAL TO ELECTRICAL SIGNAL CONVERTER","http://data.15926.org/rdl/RDS1066704961"]
[null,null,null,null,null,"Action","PHASE CONVERTER","http://data.15926.org/rdl/RDS986759"]
[null,null,null,null,null,"Action","PNEUMATIC TO MECHANICAL ENERGY CONVERTER","http://data.15926.org/rdl/RDS279989"]
[null,null,null,null,null,"Action","PNEUMATIC TO ROTATION ENERGY CONVERTER","http://data.15926.org/rdl/RDS2220078"]
[null,null,null,null,null,"Action","POTENTIAL TO MECHANICAL ENERGY CONVERTER","http://data.15926.org/rdl/RDS316169"]
[null,null,null,null,null,"Action","PRESSURE TO CURRENT SIGNAL CONVERTER","http://data.15926.org/rdl/RDS460439"]
[null,null,null,null,null,"Action","PRESSURE TO VOLTAGE SIGNAL CONVERTER","http://data.15926.org/rdl/RDS851264"]
[null,null,null,null,null,"Action","RESISTANCE TO CURRENT SIGNAL CONVERTER","http://data.15926.org/rdl/RDS5763018"]
[null,null,null,null,null,"Action","REVERSIBLE CONVERTER","http://data.15926.org/rdl/RDS952919"]
[null,null,null,null,null,"Action","ROTARY CONVERTER","http://data.15926.org/rdl/RDS1004174"]
[null,null,null,null,null,"Action","ROTATING FREQUENCY CONVERTER","http://data.15926.org/rdl/RDS7220623"]
[null,null,null,null,null,"Action","ROTATING PHASE CONVERTER","http://data.15926.org/rdl/RDS7220685"]
[null,null,null,null,null,"Action","ROTATIONAL CONVERTER","http://data.15926.org/rdl/RDS278279"]
[null,null,null,null,null,"Action","SEMICONDUCTOR CONVERTER","http://data.15926.org/rdl/RDS953234"]
[null,null,null,null,null,"Action","SIGNAL CONVERTER","http://data.15926.org/rdl/RDS460394"]
[null,null,null,null,null,"Action","SINGLE CONVERTER","http://data.15926.org/rdl/RDS952964"]
[null,null,null,null,null,"Action","TORQUE CONVERTER","http://data.15926.org/rdl/RDS427153411"]
[null,null,null,null,null,"Action","TWO-QUADRANT CONVERTER","http://data.15926.org/rdl/RDS952829"]
[null,null,null,null,null,"Action","VARIABLE SPEED DRIVE CONVERTER","http://data.15926.org/rdl/RDS6624633"]
[null,null,null,null,null,"Action","VOLTAGE TO CURRENT SIGNAL CONVERTER","http://data.15926.org/rdl/RDS851174"]
[null,null,null,null,null,"Action","VOLTAGE TO PRESSURE SIGNAL CONVERTER","http://data.15926.org/rdl/RDS851309"]
[null,null,null,null,null,"Action","VOLTAGE TO VOLTAGE SIGNAL CONVERTER","http://data.15926.org/rdl/RDS5762939"]

{"sheet":"Settings","index":1,"n_rows":87,"n_cols":8,"rows_kept":87,"cut":false,"hidden":true,"merged":[]}
["Setting name","Select name","OnKey","Value","Status","RDLType"]
["Endpoint","RDL2 (15926.org)",null,"http://data.15926.org/rdl/","Current",null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA RDL",null,"http://data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA Staging",null,"http://staging.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA SVRDL",null,"http://svrdl.community.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P4",null,"http://posccaesar.org/p4/sparql",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P12",null,"http://sti.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","Localhost",null,"http://localhost:8890/sparql/",null,null,null,"Note: end address always with a slash (/)"]
[]
["gBaseNamespace",null,"http://data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://staging.data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://svrdl.community.data.posccaesar.org/rdl/","http://svrdl.community.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://posccaesar.org/p4/sparql","http://posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://sti.data.posccaesar.org/rdl/","http://sti.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://localhost:8890/sparql/","http://data.15926.org/rdl/",null,"RDL2"]
["gKeepSettings",null,null,"T"]
["gShowDeprecated",null,null,"T"]
["gColoring",null,null,"T"]
["gNamespaceReplacing",null,null,"F"]
["gHyperlinkReplacing",null,null,"F"]
[]
["Endpoint","aisi",null,"http://data.15926.org/aisi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ansi",null,"http://data.15926.org/ansi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","api",null,"http://data.15926.org/api/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","all",null,"http://data.15926.org/all/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","asme",null,"http://data.15926.org/asme/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","astm",null,"http://data.15926.org/astm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","atex",null,"http://data.15926.org/atex/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","bs",null,"http://data.15926.org/bs/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","din",null,"http://data.15926.org/din/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dm",null,"http://data.15926.org/dm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dnv",null,"http://data.15926.org/dnv/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","edm",null,"http://data.15926.org/edm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","en",null,"http://data.15926.org/en/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","eu",null,"http://data.15926.org/eu/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iec",null,"http://data.15926.org/iec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ieee",null,"http://data.15926.org/ieee/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iso",null,"http://data.15926.org/iso/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","lci",null,"http://data.15926.org/lci/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","mss",null,"http://data.15926.org/mss/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nace",null,"http://data.15926.org/nace/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nec",null,"http://data.15926.org/nec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nema",null,"http://data.15926.org/nema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nfpa",null,"http://data.15926.org/nfpa/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nor",null,"http://data.15926.org/nor/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","rdl",null,"http://data.15926.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sae",null,"http://data.15926.org/sae/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sie",null,"http://data.15926.org/sie/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","tema",null,"http://data.15926.org/tema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","twr",null,"http://data.15926.org/twr/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","uns",null,"http://data.15926.org/uns/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","wits",null,"http://data.15926.org/wits/",null,null,null,"Note: end address always with a slash (/)"]
[]
[]
["gBaseNamespace",null,"http://data.15926.org/aisi/","http://data.15926.org/aisi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ansi/","http://data.15926.org/ansi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/api/","http://data.15926.org/api/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/asme/","http://data.15926.org/asme/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/all/","http://data.15926.org/all/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/astm/","http://data.15926.org/astm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/atex/","http://data.15926.org/atex/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/bs/","http://data.15926.org/bs/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/din/","http://data.15926.org/din/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dm/","http://data.15926.org/dm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dnv/","http://data.15926.org/dnv/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/edm/","http://data.15926.org/edm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/en/","http://data.15926.org/en/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/eu/","http://data.15926.org/eu/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iec/","http://data.15926.org/iec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ieee/","http://data.15926.org/ieee/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iso/","http://data.15926.org/iso/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/lci/","http://data.15926.org/lci/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/mss/","http://data.15926.org/mss/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nace/","http://data.15926.org/nace/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nec/","http://data.15926.org/nec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nema/","http://data.15926.org/nema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nfpa/","http://data.15926.org/nfpa/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nor/","http://data.15926.org/nor/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sae/","http://data.15926.org/sae/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sie/","http://data.15926.org/sie/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/tema/","http://data.15926.org/tema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/twr/","http://data.15926.org/twr/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/uns/","http://data.15926.org/uns/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/wits/","http://data.15926.org/wits/",null,"RDL2"]
["                                          "]

{"sheet":"about","index":2,"n_rows":176,"n_cols":3,"rows_kept":176,"cut":false,"hidden":false,"merged":[]}
["Version 75 changes","2018-10-05","Onno Paap"]
["missing superclasses - and orphans- filter no deprecated classes"]
[]
["Version 74 changes","2018-09-30","Onno Paap"]
["Repaired bug missing label"]
[]
["Version 73 changes","2018-05-16","Onno Paap"]
["Repaired bug Deprecated Superclass"]
[]
[]
[]
["Version 71 changes","2016-07-17","Onno Paap"]
["Aded report button for comparison of RDL2 with a subfolder called views filled with spreadsheets."]
[]
[]
["Version 69 changes","2016-06-16","Onno Paap"]
["Added button: \"errors in definitions\" that lists all classes that have more or less \"<\" brackets than the number of super class relationships + 1. Where the part after the word \"that \"  is ignored in the count of \"<\" brackets."]
[]
["Version 68 changes","2016-06-13","Onno Paap"]
["Updated endpoint of RDL2 sparql "]
[]
["Version 67 changes","2016-05-22","Onno Paap"]
["Added button list subclasses from superclass "]
[]
["Version 65 changes","2016-04-25","Onno Paap"]
["Added checkbox at action dialog \"supress double child occurances\" so that this built-in feature can be switched off"]
[]
["Version 64 changes","2016-04-20","Onno Paap"]
["Made search case-insensitive and added endpoint \"all\""]
[]
["Version 63 changes","2016-09-28","Onno Paap"]
["Made entity list working on P4 endpoint (they changed the database version which was not accepting som sparql setting)"]
["Version 62 changes","2016-09-28","Onno Paap"]
["Applied show deprecated to searched result list"]
[]
["Version 61 changes","2016-08-29","Onno Paap"]
["Added query from pcardl for ClassOfIndirectProperty"]
[]
["Version 60 changes","2016-08-19","Onno Paap"]
["Repaired failing entity reports"]
[]
["Version 59 changes","2016-08-19","Onno Paap"]
["Missing superclasses now queries whole federation of RDL2"]
[]
["Version 58 changes","2016-08-16","Onno Paap"]
["Repaired missing output for entities and doubles in RDL2 endpoints other than rdl"]
[]
["Version 57 changes","2016-08-13","Onno Paap"]
["Doubles report now skips classes that are deprecated"]
[]
["Version 56 changes","2016-07-22","Onno Paap"]
["Made rowheight suitable for longer definitions to example DESIGN BASIS"]
[]
["Version 55 changes","2016-07-19","Onno Paap"]
["Made rowheight suitable for longer definitions"]
[]
["Version 54 changes","2016-07-03","Onno Paap"]
["Entity Type field changed to 6 merged cells."]
[]
["Version 53 changes","2016-06-23","Onno Paap"]
["added lci namespace"]
[]
["Version 52 changes","2016-06-23","Onno Paap"]
["Added deprecated count to list entities"]
[]
["Version 51 changes","2016-06-19","Onno Paap"]
["Updated namespaces of staging RDL"]
[]
["Version 50 changes","2016-06-19","Onno Paap"]
["taxonomy view repaired missing entity type"]
[]
["Version 49 changes","2016-06-14","Onno Paap"]
["Room for 12 superclasses"]
[]
["Version 48 changes","2016-06-14","Onno Paap"]
["Repaired NOR:/RDS  bug"]
[]
["Version 47 changes","2016-06-14","Onno Paap"]
["Repaired endpoint bug"]
[]
["Version 46 changes","2016-06-13","Onno Paap"]
["Updated endpoints"]
[]
["Version 45 changes","2016-06-06","Onno Paap"]
["Completed Missing Superclasses report"]
[]
["Version 44 changes","2016-05-20","Onno Paap"]
["Added Clear Cache button (use on any database changes)"]
[]
["Version 43 changes","2016-05-19","Onno Paap"]
["Changed non-existing super classes to show as \"no label\""]
[]
["Version 42 changes","2016-05-02","Onno Paap"]
["bug fix"]
[]
["Version 41 changes","2016-05-02","Onno Paap"]
["Added setting to show/not show deprecated items. If shown, they are stricken through"]
[]
["Version 40 changes","2016-03-31","Onno Paap"]
["Added  in doubles: two classes having the same label."]
[]
["Version 39 changes","2016-03-21","Onno Paap"]
["Made the query more robust, after the server hass been returning a 404 occasionally"]
[]
["Version 38 changes","2016-03-03","Onno Paap"]
["Repaired bug entity type query on PCA endpoint"]
[]
["Version 37 changes","2016-01-29","Onno Paap"]
["Showing deprecated class in taxonomy with label in strikethrough."]
[]
["Version 36 changes","2016-01-13","Onno Paap"]
["Added the 17 endpoints of http://data.15926.org/rdl"]
[]
["Version 35 changes","2016-01-13","Onno Paap"]
["In taxonomy view, disregard all rdf:type that is not data model.  So only show rdf:type that is dm:"]
[]
["Version 34 changes","2016-01-13","Onno Paap"]
["Solved taxonomy levels regression bug"]
[]
["Version 33 changes","2016-01-11","Onno Paap"]
["Enhanced the doubled query. First 4 columns are about the triple, the rest is info."]
[]
["Repaired bug in entity type query."]
[]
["Version 30 changes","2016-01-03","Onno Paap"]
["Repaired entity type query for old PCA RDL. \nRepaired bug in entity type query where a class that has a superclass of the wanted type as well as  of another type became  the start point of a new taxonomy as well as part in the main taxonomy. (read that again)"]
[]
["Version 29 changes","2016-01-02","Onno Paap"]
["Filtered entity filtered taxonomy to only show the filtered entity not subClassOf of another entity"]
[]
["Version 27 changes","2016-01-01","Onno Paap"]
["few bugs repaired.  Changed entity search into presenting taxonomies. "]
[]
["Version 26 changes","2015-12-26","Onno Paap"]
["few bugs repaired. "]
[]
["Version 25 changes","2015-12-26","Onno Paap"]
["Added Part 12 and localhost endpoints"]
["Added button for selecting double labels and definitions. "]
["Version 24 changes","2015-12-14","Onno Paap"]
["Added button to list all distinct entity data types and their counts, and click to show."]
["Added a button to show all orphans that have a rdfs:label"]
["Version 23 changes"]
["Added endpoint posccaesar.org/p4/sparql"]
["Version 22 changes"]
["Added endpoint staging.data.posccaesar.org/rdl"]
[]
["Version 21 changes"]
["Repaired bug where namespace replace was based upon definition instead of class label"]
[]
["Version 20 changes"]
["Repaired bug where definition did not show up if hyperlink replace was on."]
[]
["Version 19 changes (skip version 16-18)"]
["Settings expanded with persist settings, namespace replacer and hyperlink replacer"]
["Added namespace replacer which will replace the RDL: namespace of the ID with the namespace given in the list on the front page."]
["Added hyperlink replacer which will find terms between single quotes and look them up in the RDL, then add a hyperlink in the text if found. Anchor tag <a></a> used not &hyperlink() so looks ugly."]
[]
["Version 15 changes"]
["Changed browser page Action buttons to hyperlinks because buttons are not equally spaced between Excel versions (Office 2007 versus Office 365)"]
["First row is empty. Move all up."]
["Make stop button for during query taxonomy query execution"]
[]
[]
["Version 14 changes"]
["Aligned buttons on browser page"]
["Made color notification work. Note: switch it on first in settings. Default is off"]
["Top align subclasses in taxonomy"]
["Subclasses made to hyperlink in taxonomy"]
["Subclasses made to increase column width in taxonomy"]
["Made browser search go when hitting enter in search field"]
[]
[]
[]
["todo"]
["Make setting for outputting to other result pages"]

{"sheet":"Results1","index":3,"n_rows":453,"n_cols":39,"rows_kept":453,"cut":false,"hidden":false,"merged":[[274,28,274,33],[275,28,275,33],[276,26,276,31],[277,26,277,31],[278,27,278,32],[279,28,279,33],[268,28,268,33],[269,27,269,32],[270,27,270,32],[271,28,271,33],[272,28,272,33],[273,28,273,33],[262,28,262,33],[263,28,263,33],[264,28,264,33],[265,28,265,33],[266,28,266,33],[267,28,267,33],[256,28,256,33],[257,28,257,33],[258,28,258,33],[259,28,259,33],[260,28,260,33],[261,28,261,33],[261,26,261,27],[260,26,260,27],[259,26,259,27],[258,26,258,27],[257,26,257,27],[256,26,256,27],[268,26,268,27],[267,26,267,27],[265,26,265,27],[264,26,264,27],[263,26,263,27],[262,26,262,27],[274,26,274,27],[273,26,273,27],[272,26,272,27],[271,26,271,27],[270,25,270,26],[269,25,269,26],[281,18,281,23],[282,18,282,23],[282,24,282,25],[281,24,281,25],[280,25,280,26],[279,26,279,27],[280,27,280,32],[281,26,281,31],[282,26,282,31],[275,20,275,25],[276,18,276,23],[277,18,277,23],[278,19,278,24],[279,20,279,25],[280,19,280,24],[278,25,278,26],[277,24,277,25],[276,24,276,25],[275,26,275,27],[270,19,270,24],[272,20,272,25],[271,20,271,25],[273,20,273,25],[274,20,274,25],[264,20,264,25],[265,20,265,25],[266,20,266,25],[267,20,267,25],[268,20,268,25],[269,19,269,24],[258,20,258,25],[259,20,259,25],[260,20,260,25],[261,20,261,25],[262,20,262,25],[263,20,263,25],[281,32,281,35],[282,32,282,35],[252,19,252,24],[252,25,252,26],[252,27,252,32],[253,20,253,25],[254,20,254,25],[255,20,255,25],[256,20,256,25],[257,20,257,25],[251,27,251,32],[251,33,251,36],[252,33,252,36],[253,34,253,37],[254,34,254,37],[255,34,255,37],[255,26,255,27],[254,26,254,27],[253,26,253,27],[253,28,253,33],[249,17,249,22],[249,23,249,24],[249,25,249,30],[249,31,249,34],[250,18,250,23],[250,24,250,25],[451,22,451,23],[451,16,451,21],[451,24,451,29],[451,30,451,33],[452,22,452,23],[452,16,452,21],[452,24,452,29],[452,30,452,33],[449,22,449,23],[449,16,449,21],[449,24,449,29],[449,30,449,33],[450,22,450,23],[450,16,450,21],[450,24,450,29],[450,30,450,33],[447,22,447,23],[447,16,447,21],[447,24,447,29],[447,30,447,33],[448,22,448,23],[448,16,448,21],[448,24,448,29],[448,30,448,33],[445,22,445,23],[445,16,445,21],[445,24,445,29],[445,30,445,33],[446,22,446,23],[446,16,446,21],[446,24,446,29],[446,30,446,33],[443,22,443,23],[443,16,443,21],[443,24,443,29],[443,30,443,33],[444,22,444,23],[444,16,444,21],[444,24,444,29],[444,30,444,33],[441,22,441,23],[441,16,441,21],[441,24,441,29],[441,30,441,33],[442,22,442,23],[442,16,442,21],[442,24,442,29],[442,30,442,33],[439,22,439,23],[439,16,439,21],[439,24,439,29],[439,30,439,33],[440,22,440,23],[440,16,440,21],[440,24,440,29],[440,30,440,33],[437,21,437,22],[437,15,437,20],[437,23,437,28],[437,29,437,32],[438,22,438,23],[438,16,438,21],[438,24,438,29],[438,30,438,33],[279,34,279,37],[280,33,280,36],[277,32,277,35],[278,33,278,36],[275,34,275,37],[276,32,276,35],[273,34,273,37],[274,34,274,37],[271,34,271,37],[272,34,272,37],[269,33,269,36],[270,33,270,36],[267,34,267,37],[268,34,268,37],[265,34,265,37],[266,34,266,37],[263,34,263,37],[264,34,264,37],[261,34,261,37],[262,34,262,37],[259,34,259,37],[260,34,260,37],[257,34,257,37],[258,34,258,37],[256,34,256,37],[255,28,255,33],[254,28,254,33],[251,19,251,24],[251,25,251,26],[250,26,250,31],[250,32,250,35],[435,23,435,24],[435,17,435,22],[435,25,435,30],[435,31,435,34],[436,23,436,24],[436,17,436,22],[436,25,436,30],[436,31,436,34],[433,26,433,27],[433,20,433,25],[433,28,433,33],[433,34,433,37],[434,24,434,25],[434,18,434,23],[434,26,434,31],[434,32,434,35],[431,24,431,25],[431,18,431,23],[431,26,431,31],[431,32,431,35],[432,25,432,26],[432,19,432,24],[432,27,432,32],[432,33,432,36],[429,23,429,24],[429,17,429,22],[429,25,429,30],[429,31,429,34],[430,23,430,24],[430,17,430,22],[430,25,430,30],[430,31,430,34],[428,23,428,24],[428,17,428,22],[428,25,428,30],[428,31,428,34],[426,25,426,26],[426,19,426,24],[426,27,426,32],[426,33,426,36],[427,24,427,25],[427,18,427,23],[427,26,427,31],[427,32,427,35],[424,25,424,26],[424,19,424,24],[424,27,424,32],[424,33,424,36],[425,25,425,26],[425,19,425,24],[425,27,425,32],[425,33,425,36],[422,25,422,26],[422,19,422,24],[422,27,422,32],[422,33,422,36],[423,25,423,26],[423,19,423,24],[423,27,423,32],[423,33,423,36],[420,25,420,26],[420,19,420,24],[420,27,420,32],[420,33,420,36],[421,25,421,26],[421,19,421,24],[421,27,421,32],[421,33,421,36],[418,25,418,26],[418,19,418,24],[418,27,418,32],[418,33,418,36],[419,25,419,26],[419,19,419,24],[419,27,419,32],[419,33,419,36],[416,25,416,26],[416,19,416,24],[416,27,416,32],[416,33,416,36],[417,25,417,26],[417,19,417,24],[417,27,417,32],[417,33,417,36],[414,25,414,26],[414,19,414,24],[414,27,414,32],[414,33,414,36],[415,25,415,26],[415,19,415,24],[415,27,415,32],[415,33,415,36],[412,25,412,26],[412,19,412,24],[412,27,412,32],[412,33,412,36],[413,25,413,26],[413,19,413,24],[413,27,413,32],[413,33,413,36],[410,25,410,26],[410,19,410,24],[410,27,410,32],[410,33,410,36],[411,25,411,26],[411,19,411,24],[411,27,411,32],[411,33,411,36],[408,25,408,26],[408,19,408,24],[408,27,408,32],[408,33,408,36],[409,25,409,26],[409,19,409,24],[409,27,409,32],[409,33,409,36],[406,23,406,24],[406,17,406,22],[406,25,406,30],[406,31,406,34],[407,24,407,25],[407,18,407,23],[407,26,407,31],[407,32,407,35],[404,24,404,25],[404,18,404,23],[404,26,404,31],[404,32,404,35],[405,23,405,24],[405,17,405,22],[405,25,405,30],[405,31,405,34],[402,24,402,25],[402,18,402,23],[402,26,402,31],[402,32,402,35],[403,25,403,26],[403,19,403,24],[403,27,403,32],[403,33,403,36],[401,23,401,24],[401,17,401,22],[401,25,401,30],[401,31,401,34],[400,23,400,24],[400,17,400,22],[400,25,400,30],[400,31,400,34],[398,24,398,25],[398,18,398,23],[398,26,398,31],[398,32,398,35],[399,22,399,23],[399,16,399,21],[399,24,399,29],[399,30,399,33],[396,22,396,23],[396,16,396,21],[396,24,396,29],[396,30,396,33],[397,23,397,24],[397,17,397,22],[397,25,397,30],[397,31,397,34],[394,23,394,24],[394,17,394,22],[394,25,394,30],[395,22,395,23],[395,16,395,21],[395,24,395,29],[395,30,395,33],[392,25,392,26],[392,19,392,24],[392,27,392,32],[392,33,392,36],[393,22,393,23],[393,16,393,21],[393,24,393,29],[393,30,393,33],[390,25,390,26],[390,19,390,24],[390,27,390,32],[390,33,390,36],[391,25,391,26],[391,19,391,24],[391,27,391,32],[391,33,391,36],[388,26,388,27],[388,20,388,25],[388,28,388,33],[388,34,388,37],[389,25,389,26],[389,19,389,24],[389,27,389,32],[389,33,389,36],[386,25,386,26],[386,19,386,24],[386,27,386,32],[386,33,386,36],[387,25,387,26],[387,19,387,24],[387,27,387,32],[387,33,387,36],[384,25,384,26],[384,19,384,24],[384,27,384,32],[384,33,384,36],[385,25,385,26],[385,19,385,24],[385,27,385,32],[385,33,385,36],[382,25,382,26],[382,19,382,24],[382,27,382,32],[382,33,382,36],[383,26,383,27],[383,20,383,25],[383,28,383,33],[383,34,383,37],[380,25,380,26],[380,19,380,24],[380,27,380,32],[380,33,380,36],[381,24,381,25],[381,18,381,23],[381,26,381,31],[381,32,381,35],[379,24,379,25],[379,18,379,23],[379,26,379,31],[379,32,379,35],[377,26,377,27],[377,20,377,25],[377,28,377,33],[377,34,377,37],[378,26,378,27],[378,20,378,25],[378,28,378,33],[378,34,378,37],[375,26,375,27],[375,20,375,25],[375,28,375,33],[375,34,375,37],[376,26,376,27],[376,20,376,25],[376,28,376,33],[376,34,376,37],[373,25,373,26],[373,19,373,24],[373,27,373,32],[373,33,373,36],[374,26,374,27],[374,20,374,25],[374,28,374,33],[374,34,374,37],[371,26,371,27],[371,20,371,25],[371,28,371,33],[371,34,371,37],[372,25,372,26],[372,19,372,24],[372,27,372,32],[372,33,372,36],[369,26,369,27],[369,20,369,25],[369,28,369,33],[369,34,369,37],[370,26,370,27],[370,20,370,25],[370,28,370,33],[370,34,370,37],[367,27,367,28],[367,21,367,26],[367,29,367,34],[367,35,367,38],[368,27,368,28],[368,21,368,26],[368,29,368,34],[368,35,368,38],[365,25,365,26],[365,19,365,24],[365,27,365,32],[365,33,365,36],[366,26,366,27],[366,20,366,25],[366,28,366,33],[366,34,366,37],[363,24,363,25],[363,18,363,23],[363,26,363,31],[363,32,363,35],[364,24,364,25],[364,18,364,23],[364,26,364,31],[364,32,364,35],[361,24,361,25],[361,18,361,23],[361,26,361,31],[361,32,361,35],[362,24,362,25],[362,18,362,23],[362,26,362,31],[362,32,362,35],[359,24,359,25],[359,18,359,23],[359,26,359,31],[359,32,359,35],[360,24,360,25],[360,18,360,23],[360,26,360,31],[360,32,360,35],[358,24,358,25],[358,18,358,23],[358,26,358,31],[358,32,358,35],[356,22,356,23],[356,16,356,21],[356,24,356,29],[356,30,356,33],[357,23,357,24],[357,17,357,22],[357,25,357,30],[357,31,357,34],[354,22,354,23],[354,16,354,21],[354,24,354,29],[354,30,354,33],[355,23,355,24],[355,17,355,22],[355,25,355,30],[355,31,355,34],[352,23,352,24],[352,17,352,22],[352,25,352,30],[352,31,352,34],[353,22,353,23],[353,16,353,21],[353,24,353,29],[353,30,353,33],[350,25,350,26],[350,19,350,24],[350,27,350,32],[350,33,350,36],[351,24,351,25],[351,18,351,23],[351,26,351,31],[351,32,351,35],[348,25,348,26],[348,19,348,24],[348,27,348,32],[348,33,348,36],[349,25,349,26],[349,19,349,24],[349,27,349,32],[349,33,349,36],[346,25,346,26],[346,19,346,24],[346,27,346,32],[346,33,346,36],[347,24,347,25],[347,18,347,23],[347,26,347,31],[347,32,347,35],[344,23,344,24],[344,17,344,22],[344,25,344,30],[344,31,344,34],[345,24,345,25],[345,18,345,23],[345,26,345,31],[345,32,345,35],[342,24,342,25],[342,18,342,23],[342,26,342,31],[342,32,342,35],[343,22,343,23],[343,16,343,21],[343,24,343,29],[343,30,343,33],[340,26,340,27],[340,20,340,25],[340,28,340,33],[340,34,340,37],[341,24,341,25],[341,18,341,23],[341,26,341,31],[341,32,341,35],[338,25,338,26],[338,19,338,24],[338,27,338,32],[338,33,338,36],[339,26,339,27],[339,20,339,25],[339,28,339,33],[339,34,339,37],[336,25,336,26],[336,19,336,24],[336,27,336,32],[336,33,336,36],[337,26,337,27],[337,20,337,25],[337,28,337,33],[337,34,337,37],[334,25,334,26],[334,19,334,24],[334,27,334,32],[334,33,334,36],[335,25,335,26],[335,19,335,24],[335,27,335,32],[335,33,335,36],[332,26,332,27],[332,20,332,25],[332,28,332,33],[332,34,332,37],[333,25,333,26],[333,19,333,24],[333,27,333,32],[333,33,333,36],[330,26,330,27],[330,20,330,25],[330,28,330,33],[330,34,330,37],[331,25,331,26],[331,19,331,24],[331,27,331,32],[331,33,331,36],[328,25,328,26],[328,19,328,24],[328,27,328,32],[328,33,328,36],[329,26,329,27],[329,20,329,25],[329,28,329,33],[329,34,329,37],[326,25,326,26],[326,19,326,24],[326,27,326,32],[326,33,326,36],[327,25,327,26],[327,19,327,24],[327,27,327,32],[327,33,327,36],[324,25,324,26],[324,19,324,24],[324,27,324,32],[324,33,324,36],[325,25,325,26],[325,19,325,24],[325,27,325,32],[325,33,325,36],[322,25,322,26],[322,19,322,24],[322,27,322,32],[322,33,322,36],[323,25,323,26],[323,19,323,24],[323,27,323,32],[323,33,323,36],[320,25,320,26],[320,19,320,24],[320,27,320,32],[320,33,320,36],[321,25,321,26],[321,19,321,24],[321,27,321,32],[321,33,321,36],[318,25,318,26],[318,19,318,24],[318,27,318,32],[318,33,318,36],[319,25,319,26],[319,19,319,24],[319,27,319,32],[319,33,319,36],[316,25,316,26],[316,19,316,24],[316,27,316,32],[316,33,316,36],[317,25,317,26],[317,19,317,24],[317,27,317,32],[317,33,317,36],[314,25,314,26],[314,19,314,24],[314,27,314,32],[314,33,314,36],[315,25,315,26],[315,19,315,24],[315,27,315,32],[315,33,315,36],[312,26,312,27],[312,20,312,25],[312,28,312,33],[312,34,312,37],[313,25,313,26],[313,19,313,24],[313,27,313,32],[313,33,313,36],[310,25,310,26],[310,19,310,24],[310,27,310,32],[310,33,310,36],[311,26,311,27],[311,20,311,25],[311,28,311,33],[311,34,311,37],[308,25,308,26],[308,19,308,24],[308,27,308,32],[308,33,308,36],[309,25,309,26],[309,19,309,24],[309,27,309,32],[309,33,309,36],[306,25,306,26],[306,19,306,24],[306,27,306,32],[306,33,306,36],[307,25,307,26],[307,19,307,24],[307,27,307,32],[307,33,307,36],[304,25,304,26],[304,19,304,24],[304,27,304,32],[304,33,304,36],[305,25,305,26],[305,19,305,24],[305,27,305,32],[305,33,305,36],[302,25,302,26],[302,19,302,24],[302,27,302,32],[302,33,302,36],[303,25,303,26],[303,19,303,24],[303,27,303,32],[303,33,303,36],[300,25,300,26],[300,19,300,24],[300,27,300,32],[300,33,300,36],[301,25,301,26],[301,19,301,24],[301,27,301,32],[301,33,301,36],[298,25,298,26],[298,19,298,24],[298,27,298,32],[298,33,298,36],[299,25,299,26],[299,19,299,24],[299,27,299,32],[299,33,299,36],[296,25,296,26],[296,19,296,24],[296,27,296,32],[296,33,296,36],[297,25,297,26],[297,19,297,24],[297,27,297,32],[297,33,297,36],[294,24,294,25],[294,18,294,23],[294,26,294,31],[294,32,294,35],[295,25,295,26],[295,19,295,24],[295,27,295,32],[295,33,295,36],[292,25,292,26],[292,19,292,24],[292,27,292,32],[292,33,292,36],[293,26,293,27],[293,20,293,25],[293,28,293,33],[293,34,293,37],[290,25,290,26],[290,19,290,24],[290,27,290,32],[290,33,290,36],[291,25,291,26],[291,19,291,24],[291,27,291,32],[291,33,291,36],[288,24,288,25],[288,18,288,23],[288,26,288,31],[288,32,288,35],[289,24,289,25],[289,18,289,23],[289,26,289,31],[289,32,289,35],[286,25,286,26],[286,19,286,24],[286,27,286,32],[286,33,286,36],[287,26,287,27],[287,20,287,25],[287,28,287,33],[287,34,287,37],[284,23,284,24],[284,17,284,22],[284,25,284,30],[284,31,284,34],[285,24,285,25],[285,18,285,23],[285,26,285,31],[285,32,285,35],[283,22,283,23],[283,16,283,21],[283,24,283,29],[283,30,283,33],[248,23,248,24],[248,17,248,22],[248,25,248,30],[248,31,248,34],[246,24,246,25],[246,18,246,23],[246,26,246,31],[246,32,246,35],[247,23,247,24],[247,17,247,22],[247,25,247,30],[247,31,247,34],[244,23,244,24],[244,17,244,22],[244,25,244,30],[244,31,244,34],[245,23,245,24],[245,17,245,22],[245,25,245,30],[245,31,245,34],[242,24,242,25],[242,18,242,23],[242,26,242,31],[242,32,242,35],[243,23,243,24],[243,17,243,22],[243,25,243,30],[243,31,243,34],[240,24,240,25],[240,18,240,23],[240,26,240,31],[240,32,240,35],[241,24,241,25],[241,18,241,23],[241,26,241,31],[241,32,241,35],[238,24,238,25],[238,18,238,23],[238,26,238,31],[238,32,238,35],[239,24,239,25],[239,18,239,23],[239,26,239,31],[239,32,239,35],[236,25,236,26],[236,19,236,24],[236,27,236,32],[236,33,236,36],[237,24,237,25],[237,18,237,23],[237,26,237,31],[237,32,237,35],[234,25,234,26],[234,19,234,24],[234,27,234,32],[234,33,234,36],[235,25,235,26],[235,19,235,24],[235,27,235,32],[235,33,235,36],[232,24,232,25],[232,18,232,23],[232,26,232,31],[232,32,232,35],[233,25,233,26],[233,19,233,24],[233,27,233,32],[233,33,233,36],[230,25,230,26],[230,19,230,24],[230,27,230,32],[230,33,230,36],[231,24,231,25],[231,18,231,23],[231,26,231,31],[231,32,231,35],[228,26,228,27],[228,20,228,25],[228,28,228,33],[228,34,228,37],[229,25,229,26],[229,19,229,24],[229,27,229,32],[229,33,229,36],[226,25,226,26],[226,19,226,24],[226,27,226,32],[226,33,226,36],[227,26,227,27],[227,20,227,25],[227,28,227,33],[227,34,227,37],[224,25,224,26],[224,19,224,24],[224,27,224,32],[224,33,224,36],[225,25,225,26],[225,19,225,24],[225,27,225,32],[225,33,225,36],[222,23,222,24],[222,17,222,22],[222,25,222,30],[222,31,222,34],[223,24,223,25],[223,18,223,23],[223,26,223,31],[223,32,223,35],[220,25,220,26],[220,19,220,24],[220,27,220,32],[220,33,220,36],[221,25,221,26],[221,19,221,24],[221,27,221,32],[221,33,221,36],[218,26,218,27],[218,20,218,25],[218,28,218,33],[218,34,218,37],[219,25,219,26],[219,19,219,24],[219,27,219,32],[219,33,219,36],[216,25,216,26],[216,19,216,24],[216,27,216,32],[216,33,216,36],[217,26,217,27],[217,20,217,25],[217,28,217,33],[217,34,217,37],[214,25,214,26],[214,19,214,24],[214,27,214,32],[214,33,214,36],[215,25,215,26],[215,19,215,24],[215,27,215,32],[215,33,215,36],[212,25,212,26],[212,19,212,24],[212,27,212,32],[212,33,212,36],[213,25,213,26],[213,19,213,24],[213,27,213,32],[213,33,213,36],[210,26,210,27],[210,20,210,25],[210,28,210,33],[210,34,210,37],[211,25,211,26],[211,19,211,24],[211,27,211,32],[211,33,211,36],[208,25,208,26],[208,19,208,24],[208,27,208,32],[208,33,208,36],[209,26,209,27],[209,20,209,25],[209,28,209,33],[209,34,209,37],[206,25,206,26],[206,19,206,24],[206,27,206,32],[206,33,206,36],[207,25,207,26],[207,19,207,24],[207,27,207,32],[207,33,207,36],[204,25,204,26],[204,19,204,24],[204,27,204,32],[204,33,204,36],[205,25,205,26],[205,19,205,24],[205,27,205,32],[205,33,205,36],[202,26,202,27],[202,20,202,25],[202,28,202,33],[202,34,202,37],[203,26,203,27],[203,20,203,25]],"merged_total":1810,"flags":["merged_cut"]}
[null,null,"FunctionalObject",null,null,null,null,null,null,null,null,null,null,null,"CONVERTER",null,null,null,null,null,"rdl:RDS13048460",null,"A <CONVERTER> is a <FunctionalObject> that is capable of <CONVERTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"CHEMICAL CONVERTER",null,null,null,null,null,"rdl:RDS4316590754",null,"A <CHEMICAL CONVERTER> is a <CONVERTER> capable of <CONVERTING> one <SUBSTANCE> into another by means of a chemical reaction",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","CHEMICAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"CATALYTIC CONVERTER",null,null,null,null,null,"rdl:RDS4316590660",null,"A <CATALYTIC CONVERTER> is an <ARTEFACT> and a <CHEMICAL CONVERTER> that uses a <CATALYST> to increase the chemical conversion rate",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"ENCODER",null,null,null,null,null,"rdl:RDS5855360",null,"An <ENCODER> is a <CONVERTER> that converts information from one system of communication into another",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"ENERGY CONVERTER",null,null,null,null,null,"rdl:RDS339575363",null,"An <ENERGY CONVERTER> is a <CONVERTER> that is capable of <ENERGY CONVERTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"CHEMICAL TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,"rdl:RDS278234",null,"A <CHEMICAL TO MECHANICAL ENERGY CONVERTER> is an <ENERGY CONVERTER> that is capable of <CHEMICAL TO MECHANICAL ENERGY CONVERTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","CHEMICAL TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"LINEAR CONVERTER",null,null,null,null,null,"rdl:RDS278324",null,"A <LINEAR CONVERTER> is an <ARTEFACT> and a <CHEMICAL TO MECHANICAL ENERGY CONVERTER> that is a facility to convert internal chemical energy from a fluid into mechanical energy by controlled combustion in a linear engine (i.e. the Otto process)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"DRIVER(function)",null,null,null,null,null,"rdl:RDS299024",null,"A <DRIVER(function)> is an <ENERGY CONVERTER> that is capable of kinetically <DRIVING> a <PhysicalObject>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DRIVER(function)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOTOR",null,null,null,null,null,"rdl:RDS7191198",null,"A <MOTOR> is an <ARTEFACT> and a <DRIVER(function)>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","MOTOR","PNEUMATIC TO ROTATION ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR MOTOR",null,null,null,null,null,"rdl:RDS393998231",null,"An <AIR MOTOR> is an <ARTEFACT> and a <MOTOR> and a <PNEUMATIC TO ROTATION ENERGY CONVERTER>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AIR MOTOR","STARTING MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR STARTING MOTOR",null,null,null,null,null,"rdl:RDS13234280",null,"An <AIR STARTING MOTOR> is a <STARTING MOTOR> and an <AIR MOTOR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AIR MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC MOTOR",null,null,null,null,null,"rdl:RDS812294",null,"A <PNEUMATIC MOTOR> is an <AIR MOTOR> that is driven by compressed gas (typically air)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PNEUMATIC MOTOR","STARTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR STARTER MOTOR",null,null,null,null,null,"rdl:RDS433034",null,"An <AIR STARTER MOTOR> is a <PNEUMATIC MOTOR> and a <STARTER> using compressed air as the power source",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PNEUMATIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BIDIRECTIONAL PNEUMATIC MOTOR",null,null,null,null,null,"rdl:RDS7191280",null,"A <BIDIRECTIONAL PNEUMATIC MOTOR> is a <PNEUMATIC MOTOR> capable of delivering rotary motion in two in two directions.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PNEUMATIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC MOTOR RECIPROCATING",null,null,null,null,null,"rdl:RDS439694",null,"A <PNEUMATIC MOTOR RECIPROCATING> is a <PNEUMATIC MOTOR> utilizing reciprocating motion which usually is converted into rotary motion.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PNEUMATIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC MOTOR ROTARY",null,null,null,null,null,"rdl:RDS461069",null,"A <PNEUMATIC MOTOR ROTARY> is a <PNEUMATIC MOTOR> utilizing a rotor or turbine wheel to convert pressure energy into rotational energy.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AIR MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RECIPROCATING AIR MOTOR",null,null,null,null,null,"rdl:RDS414791591",null,"A <RECIPROCATING AIR MOTOR> is an <AIR MOTOR> intended to use reciprocating motion which usually is converted into rotary motion",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AIR MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTARY AIR MOTOR",null,null,null,null,null,"rdl:RDS414875961",null,"A <ROTARY AIR MOTOR> is an <AIR MOTOR> intended to use a rotor or turbine wheel to convert pressure energy into rotational energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE","MOTOR","ELECTRIC TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC MOTOR",null,null,null,null,null,"rdl:RDS415124",null,"An <ELECTRIC MOTOR> is an ELECTRIC ROTATING MACHINE> and a <MOTOR> and an <ELECTRIC TO MECHANICAL ENERGY CONVERTER>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ADJUSTABLE SPEED MOTOR",null,null,null,null,null,"rdl:RDS1003634",null,"An <ADJUSTABLE SPEED MOTOR> is an <ELECTRIC MOTOR> for which the speed for a given load can be adjusted to any value within a specified range",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ADJUSTABLE SPEED MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ADJUSTABLE CONSTANT SPEED MOTOR",null,null,null,null,null,"rdl:RDS1003679",null,"An <ADJUSTABLE CONSTANT SPEED MOTOR> is an <ADJUSTABLE SPEED MOTOR> that behaves at all speed settings as a constant-speed motor.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ADJUSTABLE SPEED MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ADJUSTABLE VARYING SPEED MOTOR",null,null,null,null,null,"rdl:RDS1003724",null,"An <ADJUSTABLE VARYING SPEED MOTOR> is an <ADJUSTABLE SPEED MOTOR> that behaves at all speed settings as a varying-speed motor.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALTERNATING CURRENT MOTOR",null,null,null,null,null,"rdl:RDS472994",null,"An <ALTERNATING CURRENT MOTOR> is an <ELECTRIC MOTOR> driven by alternating electric current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALTERNATING CURRENT MOTOR","ELECTRIC EX MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALTERNATING CURRENT EX MOTOR",null,null,null,null,null,"rdl:RDS1454491841",null,"An <ALTERNATING CURRENT EX MOTOR> is an <ELECTRIC EX MOTOR> that operates on Alternating Current.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALTERNATING CURRENT MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALTERNATING CURRENT COMMUTATOR MOTOR",null,null,null,null,null,"rdl:RDS872639",null,"An <ALTERNATING CURRENT COMMUTATOR MOTOR> is an <ALTERNATING CURRENT MOTOR> having an armature winding connected to its commutator and included in an alternating current circuit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALTERNATING CURRENT COMMUTATOR MOTOR","POLYPHASE MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SCHRAGE MOTOR",null,null,null,null,null,"rdl:RDS1002869",null,"A <SCHRAGE MOTOR> is a <POLYPHASE MACHINE> that is an alternating current commutator motor in which the rotor carries two windings, one of the windings receiving current from the supply by means of slip-rings while the other is connected to a commutator",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONICAL ROTOR MOTOR",null,null,null,null,null,"rdl:RDS7215040",null,"A <CONICAL ROTOR MOTOR> is an <ELECTRIC MOTOR> with a rotor in the shape of a frustum of a cone",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONSTANT SPEED MOTOR",null,null,null,null,null,"rdl:RDS1003409",null,"A <CONSTANT SPEED MOTOR> is an <ELECTRIC MOTOR> with inherently constant or substantially constant speed over its normal range of load",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DEFINITE PURPOSE MOTOR",null,null,null,null,null,"rdl:RDS1003184",null,"A <DEFINITE PURPOSE MOTOR> is an <ELECTRIC MOTOR> designed, listed and offered in standard ratings with operating characteristics and mechanical construction suitable for use on a particular type of application",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECT CURRENT MOTOR",null,null,null,null,null,"rdl:RDS472949",null,"A <DIRECT CURRENT MOTOR> is an <ELECTRIC MOTOR> for operation by direct current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR","EXPLOSION-PROTECTED ELECTRICAL APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC EX MOTOR",null,null,null,null,null,"rdl:RDS5772282",null,"An <ELECTRIC EX MOTOR> is an <ELECTRIC MOTOR> and an <EXPLOSION-PROTECTED ELECTRICAL APPARATUS> that is designed to be operating in hazardous areas",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC INDUSTRIAL MOTOR",null,null,null,null,null,"rdl:RDS5772327",null,"An <ELECTRIC INDUSTRIAL MOTOR> is an <ELECTRIC MOTOR> designed for industrial purposes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC MARINE MOTOR",null,null,null,null,null,"rdl:RDS5772372",null,"An <ELECTRIC MARINE MOTOR> is an <ELECTRIC MOTOR> designed for marine purposes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC MOTOR WITH CANOPY",null,null,null,null,null,"rdl:RDS6508449",null,"An <ELECTRIC MOTOR WITH CANOPY> is an <ELECTRIC MOTOR> equipped with a motor canopy to prevent rain from entering the cooling air inlet",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR","STARTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC STARTER MOTOR",null,null,null,null,null,"rdl:RDS1003814",null,"An <ELECTRIC STARTER MOTOR> is an <ELECTRIC MOTOR> and a <STARTER> used to facilitate the starting and accelerating of a main machine to which it is mechanically connected",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR","STARTING MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC STARTING MOTOR",null,null,null,null,null,"rdl:RDS13282000",null,"An <ELECTRIC STARTING MOTOR> is an <ELECTRIC MOTOR> and a <STARTING MOTOR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC SUBMERSIBLE MOTOR",null,null,null,null,null,"rdl:RDS7215181",null,"An <ELECTRIC SUBMERSIBLE MOTOR> is an <ELECTRIC MOTOR> designed to operate submerged, but isolated from the liquid to be pumped, and which is cooled by a clean liquid or gas",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FRACTIONAL HORSEPOWER MOTOR",null,null,null,null,null,"rdl:RDS1003319",null,"A <FRACTIONAL HORSEPOWER MOTOR> is an <ELECTRIC MOTOR> having a continuous rating not exceeding 1 h.p. per 1 000> rev/min",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GENERAL PURPOSE MOTOR",null,null,null,null,null,"rdl:RDS1003139",null,"A <GENERAL PURPOSE MOTOR> is an <ELECTRIC MOTOR> designed, listed and offered in standard ratings with operating characteristics and mechanical construction suitable for use under usual service conditions without restrictions to a particular application or type of application",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR","INDUCTION MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDUCTION MOTOR",null,null,null,null,null,"rdl:RDS486449",null,"An <INDUCTION MOTOR> is an <ELECTRIC MOTOR> and an <INDUCTION MACHINE> in which the torque or force is due to the interaction between a moving magnetic field produced by stationary primary windings and currents induced by this field in moving secondary conductors",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDUCTION MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAGE INDUCTION MOTOR",null,null,null,null,null,"rdl:RDS1002329",null,"A <CAGE INDUCTION MOTOR> is an <INDUCTION MOTOR> in which a primary winding on one member, usually the stator, is connected to the power source, and a secondary cage-winding on the other member, usually the rotor, carries induced current.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDUCTION MOTOR","SINGLE-PHASE MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REPULSION MOTOR",null,null,null,null,null,"rdl:RDS1002914",null,"A <REPULSION MOTOR> is an <INDUCTION MOTOR> and a <SINGLE-PHASE MACHINE> in which the current is supplied to the stator only, the armature being short-circuited through the brushes and its current induced from the stator winding.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"REPULSION MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPENSATED REPULSION MOTOR",null,null,null,null,null,"rdl:RDS1003004",null,"A <COMPENSATED REPULSION MOTOR> is a <REPULSION MOTOR> in which the primary winding on the stator is connected in series with the rotor winding via a second set of brushes on the commutator in order to improve the power factor and commutation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"REPULSION MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DERI MOTOR",null,null,null,null,null,"rdl:RDS1002959",null,"A <DERI MOTOR> is a <REPULSION MOTOR> having two sets of brushes of which one set is fixed and the other movable.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"REPULSION MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REPULSION INDUCTION MOTOR",null,null,null,null,null,"rdl:RDS1003094",null,"A <REPULSION INDUCTION MOTOR> is a <REPULSION MOTOR> with an additional rotor cage winding.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"REPULSION MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REPULSION START INDUCTION MOTOR",null,null,null,null,null,"rdl:RDS1003049",null,"A <REPULSION START INDUCTION MOTOR> is a <REPULSION MOTOR> in which the commutator bars are short-circuited or otherwise connected at an appropriate speed to give the equivalent of a cage winding.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDUCTION MOTOR","SINGLE-PHASE MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHADED POLE MOTOR",null,null,null,null,null,"rdl:RDS1002509",null,"A <SHADED POLE MOTOR> is an <INDUCTION MOTOR> and a <SINGLE-PHASE MACHINE> having one or more auxiliary short-circuited windings displaced in magnetic position from the main winding, all these windings being on the primary core, usually the stator.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDUCTION MOTOR","SINGLE-PHASE MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPLIT PHASE MOTOR",null,null,null,null,null,"rdl:RDS1002554",null,"An <SPLIT PHASE MOTOR> is an <INDUCTION MOTOR> and a <SINGLE-PHASE MACHINE> with an auxiliary circuit which is connected in parallel with the main winding, including an auxiliary winding displaced in magnetic position from the main winding, a phase displacement between the currents in these two primary windings being arranged.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPLIT PHASE MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAPACITOR MOTOR",null,null,null,null,null,"rdl:RDS1002689",null,"A <CAPACITOR MOTOR> is an <SPLIT PHASE MOTOR> in which the phase displacement results from a capacitor in the auxiliary circuit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAPACITOR MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAPACITOR START AND RUN MOTOR",null,null,null,null,null,"rdl:RDS1002779",null,"A <CAPACITOR START AND RUN MOTOR> is a <CAPACITOR MOTOR> in which the auxiliary circuit is energized during both starting and running.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAPACITOR START AND RUN MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TWO-VALUE CAPACITOR MOTOR",null,null,null,null,null,"rdl:RDS1002824",null,"A <TWO-VALUE CAPACITOR MOTOR> is a <CAPACITOR START AND RUN MOTOR> intended to use different values of capacitance for starting and running.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAPACITOR MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAPACITOR START MOTOR",null,null,null,null,null,"rdl:RDS1002734",null,"A <CAPACITOR START MOTOR> is a <CAPACITOR MOTOR> in which the auxiliary circuit is energized only during the starting period.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPLIT PHASE MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REACTOR START SPLIT PHASE MOTOR",null,null,null,null,null,"rdl:RDS1002644",null,"A <REACTOR START SPLIT PHASE MOTOR> is an <SPLIT PHASE MOTOR> in which the phase displacement results from additional inductive reactance in the main circuit, this additional reactance being short-circuited or otherwise made ineffective when the auxiliary circuit is opened.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPLIT PHASE MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESISTANCE START SPLIT PHASE MOTOR",null,null,null,null,null,"rdl:RDS1002599",null,"A <RESISTANCE START SPLIT PHASE MOTOR> is an <SPLIT PHASE MOTOR> in which the auxiliary primary winding is connected in series with a resistor or provides itself the necessary resistance.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDUCTION MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WOUND-ROTOR INDUCTION MOTOR",null,null,null,null,null,"rdl:RDS1002374",null,"A <WOUND-ROTOR INDUCTION MOTOR> is an <INDUCTION MOTOR> with secondary polyphase coil winding(s).",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WOUND-ROTOR INDUCTION MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BRUSHLESS WOUND-ROTOR INDUCTION MOTOR",null,null,null,null,null,"rdl:RDS1002419",null,"A <BRUSHLESS WOUND-ROTOR INDUCTION MOTOR> is a <WOUND-ROTOR INDUCTION MOTOR> in which the ends of the secondary winding are directly connected with an incorporated starting device.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WOUND-ROTOR INDUCTION MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDUCTION FREQUENCY CONVERTER",null,null,null,null,null,"rdl:RDS7222125",null,"An <INDUCTION FREQUENCY CONVERTER> is a <WOUND-ROTOR INDUCTION MOTOR> in which the frequency conversion is obtained by induction between a primary winding and a secondary winding rotating with respect to each other, the secondary winding delivering power at a frequency proportional to the relative speed of the primary magnetic field and the member carrying the secondary winding.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WOUND-ROTOR INDUCTION MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLIP-RING INDUCTION MOTOR",null,null,null,null,null,"rdl:RDS7222001",null,"A <SLIP-RING INDUCTION MOTOR> is a <WOUND-ROTOR INDUCTION MOTOR> with the secondary winding(s) connected to slip-rings.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTI-SPEED MOTOR",null,null,null,null,null,"rdl:RDS1003499",null,"A <MULTI-SPEED MOTOR> is an <ELECTRIC MOTOR> that can be operated at any of two or more definite speeds at a given load",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTI-SPEED MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTI CONSTANT SPEED MOTOR",null,null,null,null,null,"rdl:RDS1003544",null,"A <MULTI CONSTANT SPEED MOTOR> is a <MULTI-SPEED MOTOR> whose two or more definite speeds are inherently constant or substantially constant over its normal ranges of load.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTI-SPEED MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTI VARYING SPEED MOTOR",null,null,null,null,null,"rdl:RDS1003589",null,"A <MULTI VARYING SPEED MOTOR> is a <MULTI-SPEED MOTOR> whose two or more definite speeds will inherently vary appreciably over its normal ranges of load.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POLE CHANGE WINDING MOTOR",null,null,null,null,null,"rdl:RDS816164",null,"A <POLE CHANGE WINDING MOTOR> is an <ELECTRIC MOTOR> having 2 sets of stator windings, allowing the motor speed to be varied by use of one or the other of these sets of windings",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POLYPHASE COMMUTATOR MOTOR",null,null,null,null,null,"rdl:RDS7222249",null,"A <POLYPHASE COMMUTATOR MOTOR> is an <ELECTRIC MOTOR> with a polyphase armature winding fed through a commutator",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SMALL-POWER MOTOR",null,null,null,null,null,"rdl:RDS1003364",null,"A <SMALL-POWER MOTOR> is an <ELECTRIC MOTOR> having a maximum continuous rating not exceeding 1.1 kW per 1500> rev/min",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPECIAL PURPOSE MOTOR",null,null,null,null,null,"rdl:RDS1003229",null,"A <SPECIAL PURPOSE MOTOR> is an <ELECTRIC MOTOR> with special operating characteristics or special mechanical construction, or both, designed for a particular application and not falling into the definitions of general purpose or definite purpose motors",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STEPPER MOTOR",null,null,null,null,null,"rdl:RDS7220366",null,"A <STEPPER MOTOR> is an <ELECTRIC MOTOR> designed to make a rapid succession of small, equal movements in response to a pulsed input, each pulse causing one movement",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR","SYNCHRONOUS MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYNCHRONOUS MOTOR",null,null,null,null,null,"rdl:RDS817019",null,"A <SYNCHRONOUS MOTOR> is an <ELECTRIC MOTOR> and a <SYNCHRONOUS MACHINE> in which the speed of the motor is in a fixed ratio with the frequency of the current supplied",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SALIENT POLE MACHINE","SYNCHRONOUS MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAGE SYNCHRONOUS MOTOR",null,null,null,null,null,"rdl:RDS1002014",null,"A <CAGE SYNCHRONOUS MOTOR> is a <SALIENT POLE MACHINE> that is a synchronous motor that has a cage winding embedded in the pole shoes for starting",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SYNCHRONOUS MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYSTERESIS MOTOR",null,null,null,null,null,"rdl:RDS1002464",null,"A <HYSTERESIS MOTOR> is a <SYNCHRONOUS MOTOR> with a smooth cylindrically shaped member, of magnetic material without a field winding, which starts by virtue of hysteresis losses induced in that member and operates at synchronous speed due to the retentivity of that member",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDUCTOR MACHINE","SYNCHRONOUS MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDUCTOR TYPE SYNCHRONOUS MOTOR",null,null,null,null,null,"rdl:RDS1002149",null,"An <INDUCTOR TYPE SYNCHRONOUS MOTOR> is an <INDUCTOR MACHINE> running as a motor, the torque being produced by forces between the stationary poles and salient rotor teeth.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SYNCHRONOUS MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RELUCTANCE MOTOR",null,null,null,null,null,"rdl:RDS1002239",null,"A <RELUCTANCE MOTOR> is a <SYNCHRONOUS MOTOR> with an unexcited rotor carrying a number of regular projections which may or may not have a cage winding for starting",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELUCTANCE MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSYNCHRONOUS RELUCTANCE MOTOR",null,null,null,null,null,"rdl:RDS1002284",null,"A <SUBSYNCHRONOUS RELUCTANCE MOTOR> is a <RELUCTANCE MOTOR> in which the number of projections acting as salient poles is greater than the number of the poles formed by the primary winding, thus causing the motor to operate at a constant average speed that is a submultiple of its apparent synchronous speed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SYNCHRONOUS MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYNCHRONOUS INDUCTION MOTOR",null,null,null,null,null,"rdl:RDS1002059",null,"A <SYNCHRONOUS INDUCTION MOTOR> is a <SYNCHRONOUS MOTOR> having a secondary coil winding similar to that of a wound rotor induction motor, that is used for both starting and excitation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UNIVERSAL MOTOR",null,null,null,null,null,"rdl:RDS1001969",null,"A <UNIVERSAL MOTOR> is an <ELECTRIC MOTOR> that can be operated by either direct current or single phase alternating current of normal supply frequencies",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","MOTOR","MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,"ENGINE",null,null,null,null,null,"rdl:RDS13068410",null,"An <ENGINE> is an <ARTEFACT> and a <MOTOR> and a <MACHINE> that converts energy into mechanical force and motion",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIRCRAFT ENGINE",null,null,null,null,null,"rdl:RDS13290300",null,"An <AIRCRAFT ENGINE> is an <ENGINE> that is a driver which is the power unit of an aircraft",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMBUSTION ENGINE",null,null,null,null,null,"rdl:RDS1083734",null,"A <COMBUSTION ENGINE> is an <ENGINE> intended to deliver power by means of burning fuels",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COMBUSTION ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXTERNAL COMBUSTION ENGINE",null,null,null,null,null,"rdl:RDS1083869",null,"An <EXTERNAL COMBUSTION ENGINE> is a <COMBUSTION ENGINE> that is intended to receive its heat from fuel burning outside the cylinder.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EXTERNAL COMBUSTION ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STIRLING ENGINE",null,null,null,null,null,"rdl:RDS1083914",null,"An <STIRLING ENGINE> is an <EXTERNAL COMBUSTION ENGINE> that is a reciprocating engine consisting essentially of a cylinder with a working piston and a displacer. When the gas in the cylinder is heated it expands, driving the working piston. The displacer then transfers the gas to a cold region for cooling; it is then recompressed by the working piston and transferred by the displacer to the hot region to start the cycle again.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COMBUSTION ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INTERNAL COMBUSTION ENGINE",null,null,null,null,null,"rdl:RDS433889",null,"An <INTERNAL COMBUSTION ENGINE> is a <COMBUSTION ENGINE> where the combustion takes place inside the engine cylinder.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTERNAL COMBUSTION ENGINE","RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIESEL ENGINE",null,null,null,null,null,"rdl:RDS421154",null,"A <DIESEL ENGINE> is an <INTERNAL COMBUSTION ENGINE> and a <RECIPROCATING PISTON ENGINE> in which ignition of the fuel injected into the cylinder is performed by the heat of compression of the air charge.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIESEL ENGINE","PROPULSION ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIESEL PROPULSION ENGINE",null,null,null,null,null,"rdl:RDS13311055",null,"A <DIESEL PROPULSION ENGINE> is a <PROPULSION ENGINE> and a <DIESEL ENGINE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIESEL ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS OIL DIESEL ENGINE",null,null,null,null,null,"rdl:RDS13312540",null,"A <GAS OIL DIESEL ENGINE> is a <DIESEL ENGINE> designed to run on gas oil.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIESEL ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HEAVY OIL DIESEL ENGINE",null,null,null,null,null,"rdl:RDS13312450",null,"A <HEAVY OIL DIESEL ENGINE> is a <DIESEL ENGINE> designed to run on heavy oil.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIESEL ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HIGH-SPEED DIESEL ENGINE",null,null,null,null,null,"rdl:RDS13291404",null,"A <HIGH-SPEED DIESEL ENGINE> is a <DIESEL ENGINE> with a relatively high rotational speed, i.e above 600 rpm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIESEL ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LOW-SPEED DIESEL ENGINE",null,null,null,null,null,"rdl:RDS13291280",null,"A <LOW-SPEED DIESEL ENGINE> is a <DIESEL ENGINE> with a relatively low rotational speed, i.e less than 360 rpm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIESEL ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MARINE DIESEL ENGINE",null,null,null,null,null,"rdl:RDS409523321",null,"A <MARINE DIESEL ENGINE> is a <DIESEL ENGINE> designed for marine environment.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIESEL ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MDO DIESEL ENGINE",null,null,null,null,null,"rdl:RDS13312495",null,"An <MDO DIESEL ENGINE> is a <DIESEL ENGINE> designed to run on medium heavy diesel oil.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIESEL ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEDIUM-SPEED DIESEL ENGINE",null,null,null,null,null,"rdl:RDS13291342",null,"A <MEDIUM-SPEED DIESEL ENGINE> is a <DIESEL ENGINE> with a medium rotational speed, i.e between 360 and 600 rpm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTERNAL COMBUSTION ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DUAL FUEL COMBUSTION ENGINE",null,null,null,null,null,"rdl:RDS13295199",null,"A <DUAL FUEL COMBUSTION ENGINE> is an <INTERNAL COMBUSTION ENGINE> that has a dual fuel system, i.e. it can e.g. run on either diesel or gas.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTERNAL COMBUSTION ENGINE","RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS ENGINE",null,null,null,null,null,"rdl:RDS433934",null,"A <GAS ENGINE> is an <INTERNAL COMBUSTION ENGINE> and a <RECIPROCATING PISTON ENGINE> in which gaseous fuel is mixed with air to form a combustible mixture in a cylinder which is fired by spark ignition.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTERNAL COMBUSTION ENGINE","SYSTEM","TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS TURBINE SYSTEM",null,null,null,null,null,"rdl:RDS1010924",null,"A <GAS TURBINE SYSTEM> is a <TURBINE> and an <INTERNAL COMBUSTION ENGINE> and a <SYSTEM> that has an upstream rotating compressor coupled to a downstream turbine, and a combustion chamber or area, called a combustor, in between",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTERNAL COMBUSTION ENGINE","RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PETROL ENGINE",null,null,null,null,null,"rdl:RDS435149",null,"A <PETROL ENGINE> is an <INTERNAL COMBUSTION ENGINE> and a <RECIPROCATING PISTON ENGINE> that is an induction compression ignition exhaust engine which ignites a petrol air mixture with an electric spark.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTERNAL COMBUSTION ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PISTON ENGINE",null,null,null,null,null,"rdl:RDS13118382",null,"A <PISTON ENGINE> is an <INTERNAL COMBUSTION ENGINE> in which the combustion takes place inside a chamber where the rising pressure acts on a piston through which pressure energy is transformed into rotating energy.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR COOLED MOTOR",null,null,null,null,null,"rdl:RDS13118901",null,"An <AIR COOLED MOTOR> is a <PISTON ENGINE> which is cooled by air.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NATURAL ASPIRATED ENGINE",null,null,null,null,null,"rdl:RDS13284271",null,"A <NATURAL ASPIRATED ENGINE> is a <PISTON ENGINE> which has natural aspiration, i.e. not equipped with turbocharger.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,"rdl:RDS13118444",null,"A <RECIPROCATING PISTON ENGINE> is a <PISTON ENGINE> which employs a piston working in a cylinder. The piston being caused to oscillate by the periodic pressure of the working fuid, transfering the linear motion to rotating motion through its connection to a crankshaft.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13285380",null,"A <1-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 1 cylinder",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13285876",null,"A <10-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 10 cylinders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13285938",null,"A <12-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 12 cylinders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"16-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13286000",null,"A <16-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 16 cylinders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13286062",null,"A <18-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 18 cylinders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13285442",null,"A <2-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 2 cylinders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2-STROKE ENGINE",null,null,null,null,null,"rdl:RDS13118743",null,"A <2-STROKE ENGINE> is a <RECIPROCATING PISTON ENGINE> that uses a 2-stroke working cycle. The charge being introduced by a blower or by other means, compressed, ignited, expanded and exhausted through ports in the cylinder wall (uncovered by the piston), before and during the entry of a new fresh charge",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"2-STROKE ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2-STROKE TRUNK ENGINE",null,null,null,null,null,"rdl:RDS13312135",null,"A <2-STROKE TRUNK ENGINE> is a <2-STROKE ENGINE> that is a diesel engine were the piston is direct coupled to the crank through the connecting rod. The combustion air is compressed by the descending piston in a separate crankcase compartment for each cylinder and enters the cylinder through the intake ports as they are uncovered by the piston.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"2-STROKE ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CROSSHEAD ENGINE",null,null,null,null,null,"rdl:RDS13312180",null,"A <CROSSHEAD ENGINE> is a <2-STROKE ENGINE> that is a diesel engine with crosshead and piston rod design. These type of motors have a stuffing box around the piston rod preventing combusting products from contaminating the crankcase oil system. The air in the space between the piston and the diaphragm carrying the stuffing box is displaced by the descending piston into the cylinder through the intake ports as they are uncovered by the piston.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"2-STROKE ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-REVERSIBLE DIESEL ENGINE",null,null,null,null,null,"rdl:RDS13312630",null,"A <NON-REVERSIBLE DIESEL ENGINE> is a <2-STROKE ENGINE> that is a diesel engine designed to run in one direction only.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"2-STROKE ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REVERSIBLE DIESEL ENGINE",null,null,null,null,null,"rdl:RDS13312585",null,"A <REVERSIBLE DIESEL ENGINE> is a <2-STROKE ENGINE> that is a diesel engine designed to run in both directions.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13286124",null,"A <20-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 20 cylinders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13285504",null,"A <3-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 3 cylinders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13285566",null,"A <4-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 4 cylinders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"4-CYLINDER ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4-CYLINDER ENGINE WITH FIRING ORDER 1-3-4-2",null,null,null,null,null,"rdl:RDS13422124",null,"A <4-CYLINDER ENGINE WITH FIRING ORDER 1-3-4-2> is a <4-CYLINDER ENGINE> that is designed to have a firing order 1-3-4-2",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4-STROKE ENGINE",null,null,null,null,null,"rdl:RDS13118630",null,"A <4-STROKE ENGINE> is a <RECIPROCATING PISTON ENGINE> that uses a 4-stroke working cycle; suction, compression, explosion, expansion and exhaust, occupying 2 revolutions of the crankshaft",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"4-STROKE ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4-STROKE TRUNK ENGINE",null,null,null,null,null,"rdl:RDS13312405",null,"A <4-STROKE TRUNK ENGINE> is a <4-STROKE ENGINE> that is a diesel engine were the piston is direct coupled to the crank through the connecting rod. The combustion air enters the cylinder through vales on top of the cylinder.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13285628",null,"A <5-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 5 cylinders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13285690",null,"A <6-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 6 cylinders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"6-CYLINDER ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6-CYLINDER ENGINE WITH FIRING ORDER 1-2-4-6-5-3",null,null,null,null,null,"rdl:RDS13697001",null,"A <6-CYLINDER ENGINE WITH FIRING ORDER 1-3-4-2> is a <6-CYLINDER ENGINE> that is designed to have a firing order 1-2-4-6-5-3",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"6-CYLINDER ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6-CYLINDER ENGINE WITH FIRING ORDER 1-3-5-6-4-2",null,null,null,null,null,"rdl:RDS13697080",null,"A <6-CYLINDER ENGINE WITH FIRING ORDER 1-3-4-2> is a <6-CYLINDER ENGINE> that is designed to have a firing order 1-3-5-6-4-2",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"6-CYLINDER ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6-CYLINDER ENGINE WITH FIRING ORDER 1-5-3-6-4-2",null,null,null,null,null,"rdl:RDS13422045",null,"A <6-CYLINDER ENGINE WITH FIRING ORDER 1-3-4-2> is a <6-CYLINDER ENGINE> that is designed to have a firing order 1-5-3-6-4-2",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"7-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13285752",null,"A <7-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 7 cylinders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13286280",null,"A <8-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 8 cylinders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"9-CYLINDER ENGINE",null,null,null,null,null,"rdl:RDS13285814",null,"A <9-CYLINDER ENGINE> is a <RECIPROCATING PISTON ENGINE> that has 9 cylinders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BOXER ENGINE",null,null,null,null,null,"rdl:RDS13289357",null,"A <BOXER ENGINE> is a <RECIPROCATING PISTON ENGINE> with an engine block where the cylinders are placed in the horizontal plane, i.e. in a flat cylinder configuration.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DELTA ENGINE",null,null,null,null,null,"rdl:RDS13289605",null,"A <DELTA ENGINE> is a <RECIPROCATING PISTON ENGINE> with an engine block where the cylinders forms a delta configuration.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IN-LINE ENGINE",null,null,null,null,null,"rdl:RDS13289667",null,"An <IN-LINE ENGINE> is a <RECIPROCATING PISTON ENGINE> with an engine block where the cylinders are standing in a line.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEMI-DIESEL ENGINE",null,null,null,null,null,"rdl:RDS13118805",null,"A <SEMI-DIESEL ENGINE> is a <RECIPROCATING PISTON ENGINE> in which the fuel is injected into the cylinder by means of a fuel pump after compression of the air charge. As the compression heat is less than in a diesel engine, the the fuel is ignited by a hot bulb.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STAR ENGINE",null,null,null,null,null,"rdl:RDS13289419",null,"A <STAR ENGINE> is a <RECIPROCATING PISTON ENGINE> with an engine block where the cylinders are placed in a star configuration.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"V-ENGINE",null,null,null,null,null,"rdl:RDS13289481",null,"A <V-ENGINE> is a <RECIPROCATING PISTON ENGINE> with an engine block where the cylinders forms a V configuration.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RECIPROCATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W-ENGINE",null,null,null,null,null,"rdl:RDS13289543",null,"A <W-ENGINE> is a <RECIPROCATING PISTON ENGINE> with an engine block where the cylinders forms a W configuration.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTATING PISTON ENGINE",null,null,null,null,null,"rdl:RDS13118506",null,"A <ROTATING PISTON ENGINE> is a <PISTON ENGINE> which employs a rotating piston working inside a chamber. The piston being caused to rotate by the periodic pressure of the working fluid.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROTATING PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WANKEL ENGINE",null,null,null,null,null,"rdl:RDS13118568",null,"A <WANKEL ENGINE> is a <ROTATING PISTON ENGINE> having an approximately triangular central rotor geared epitrochoidally to the central driving shaft and turning in a close-fitting oval-shaped chamber so that the power stroke is applied to each of the three faces of the rotor in turn as they pass a single sparking plug.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TURBO CHARGED ENGINE",null,null,null,null,null,"rdl:RDS13119025",null,"A <TURBO CHARGED ENGINE> is a <PISTON ENGINE> eqipped with a compressor to supply air or combustible mixture to the cyliner(s).",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PISTON ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WATER COOLED MOTOR",null,null,null,null,null,"rdl:RDS13118963",null,"A <WATER COOLED MOTOR> is a <PISTON ENGINE> which is using water as the primary coolant.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROPULSION ENGINE",null,null,null,null,null,"rdl:RDS13308700",null,"A <PROPULSION ENGINE> is an <ENGINE> utilized as propulsion engine for a craft, vessel or boat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PROPULSION ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIESEL-ELECTRIC PROPULSION ENGINE",null,null,null,null,null,"rdl:RDS13290362",null,"A <DIESEL-ELECTRIC PROPULSION ENGINE> is a <PROPULSION ENGINE> that is a marine engine utilized as a generator driver for the propulsion of a ship.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PROPULSION ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHIP PROPULSION ENGINE",null,null,null,null,null,"rdl:RDS13284972",null,"A <SHIP PROPULSION ENGINE> is a <PROPULSION ENGINE> for a ship.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHIP EMERGENCY GENERATOR ENGINE",null,null,null,null,null,"rdl:RDS13309101",null,"A <SHIP EMERGENCY GENERATOR ENGINE> is an <ENGINE> that is a driver for an emergency power generator on board a ship",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHIP FIRE WATER PUMP ENGINE",null,null,null,null,null,"rdl:RDS13308971",null,"A <SHIP FIRE WATER PUMP ENGINE> is an <ENGINE> that is a ship auxiliary engine utilized as the driving motor of a fire water pump on board a ship",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHIP MAIN GENERATOR DRIVER",null,null,null,null,null,"rdl:RDS13309180",null,"A <SHIP MAIN GENERATOR DRIVER> is an <ENGINE> that is a driver for a main power generator on board a ship",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENGINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THRUSTER ENGINE",null,null,null,null,null,"rdl:RDS13290424",null,"A <THRUSTER ENGINE> is an <ENGINE> that is an auxiliary engine utilized as the driving motor of a thruster",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","MOTOR","HYDRAULIC TO ROTATION ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC MOTOR",null,null,null,null,null,"rdl:RDS1090214",null,"A <HYDRAULIC MOTOR> is an <ARTEFACT> and a <MOTOR> and a <HYDRAULIC TO ROTATION ENERGY CONVERTER> that is intended to generate power by means of high pressure oil",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC RECIPROCATING MOTOR",null,null,null,null,null,"rdl:RDS439649",null,"A <HYDRAULIC RECIPROCATING MOTOR> is a <HYDRAULIC MOTOR> that uses a reciprocating motion which usually is converted into rotary motion",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC ROTARY MOTOR",null,null,null,null,null,"rdl:RDS461114",null,"A <HYDRAULIC ROTARY MOTOR> is a <HYDRAULIC MOTOR> that uses a vane-rotor or a gear-rotor to convert pressure energy into rotational energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC MOTOR","STARTING MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC STARTING MOTOR",null,null,null,null,null,"rdl:RDS13281871",null,"A <HYDRAULIC STARTING MOTOR> is a <HYDRAULIC MOTOR> and a <STARTING MOTOR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LUFFING MOTOR",null,null,null,null,null,"rdl:RDS1325089891",null,"A <LUFFING MOTOR> is an <ARTEFACT> and a <MOTOR> that is intended to alter the inclination of something",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REVERSING MOTOR",null,null,null,null,null,"rdl:RDS310004",null,"A <REVERSING MOTOR> is an <ARTEFACT> and a <MOTOR> which has the ability to supply rotating energy in two oposite directions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SERVOMOTOR",null,null,null,null,null,"rdl:RDS418655761",null,"A <SERVOMOTOR> is an <ARTEFACT> and a <MOTOR> that serves as a drive for control or steering mechanisms",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLEWING MOTOR",null,null,null,null,null,"rdl:RDS1325082721",null,"An <SLEWING MOTOR> is an <ARTEFACT> and a <MOTOR> that is intended for turning something, or causing it to turn, without change of place",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","MOTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STARTING MOTOR",null,null,null,null,null,"rdl:RDS7247930",null,"A <STARTING MOTOR> is an <ARTEFACT> and a <MOTOR> that is an auxiliary motor, used to facilitate the starting and accelerating of a main machine to which it is mechanically connected",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FunctionalObject","DRIVER(function)",null,null,null,null,null,null,null,null,null,null,null,null,null,"TURBINE",null,null,null,null,null,"rdl:RDS313289",null,"A <TURBINE> is a <FunctionalObject> and a <DRIVER> that is a rotary mechanical device that extracts energy from a fluid flow and converts it into useful work",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMBINED CYCLE GAS TURBINE",null,null,null,null,null,"rdl:RDS16765929",null,"A <COMBINED CYCLE GAS TURBINE> is an <ARTEFACT> and a <TURBINE> that is an assembly of both a gas- and steam turbine system by which the exhaust heat from the gas turbine is used to drive the steam turbine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","EXPANDER","TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,"EXPANDER TURBINE DRIVE",null,null,null,null,null,"rdl:RDS292859",null,"An <EXPANDER TURBINE DRIVE> is an <ARTEFACT> and a <TURBINE> and an <EXPANDER> that is a power source driven by energy generated when the pressure in a medium is taken down through a <TURBINE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS TURBINE",null,null,null,null,null,"rdl:RDS820799",null,"A <GAS TURBINE> is an <ARTEFACT> and a <TURBINE> that compresses air which is then mixed with fuel for combustion and expansion through a turbine section to generate relatively high power output for either mechanical drive or power generation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AERO-DERIVATIVE GAS TURBINE",null,null,null,null,null,"rdl:RDS432944",null,"An <AERO-DERIVATIVE GAS TURBINE> is a <GAS TURBINE> that is an industrial turbine derived from an aircraft turbine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AXIAL FLOW GAS TURBINE",null,null,null,null,null,"rdl:RDS1044899",null,"An <AXIAL FLOW GAS TURBINE> is a <GAS TURBINE> in witch the gas flow is along the rotation axis of the rotor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDUSTRIAL GAS TURBINE",null,null,null,null,null,"rdl:RDS434429",null,"An <INDUSTRIAL GAS TURBINE> is a <GAS TURBINE> that is intended for application in the field of mechanical drive or generator drive and is positioned in a ground-based fixed location",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MECHANICAL DRIVE GAS TURBINE",null,null,null,null,null,"rdl:RDS409539791",null,"A <MECHANICAL DRIVE GAS TURBINE> is a <GAS TURBINE> that is used to provide mechanical energy as opposed to driving a generator of electrical power",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER GENERATION GAS TURBINE",null,null,null,null,null,"rdl:RDS413211711",null,"A <POWER GENERATION GAS TURBINE> is a <GAS TURBINE> that is used for power generation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL FLOW GAS TURBINE",null,null,null,null,null,"rdl:RDS1044854",null,"A <RADIAL FLOW GAS TURBINE> is a <GAS TURBINE> where the gas flow is made to discharge radially to the periphery of the runner",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC TURBINE",null,null,null,null,null,"rdl:RDS407017331",null,"A <HYDRAULIC TURBINE> is an <ARTEFACT> and a <TURBINE> that is driven by liquid",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WATER TURBINE",null,null,null,null,null,"rdl:RDS1083689",null,"A <WATER TURBINE> is a <HYDRAULIC TURBINE> that contains a wheel or runner which carries curved vanes or buckets and is supplied with water directed by a number of stationary guide vanes or hit by a high pressure water jet, intended to recover energy and to serve as a driver",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IMPULSE TURBINE",null,null,null,null,null,"rdl:RDS1089719",null,"An <IMPULSE TURBINE> is an <ARTEFACT> and a <TURBINE> that contains a high pressure impulse wheel, followed by intermediate and low pressure reaction blading, mounted on a drum-shaped rotor, in which a fluid drives the wheel chiefly by its kinetic energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"IMPULSE TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC IMPULSE TURBINE",null,null,null,null,null,"rdl:RDS1018664",null,"A <HYDRAULIC IMPULSE TURBINE> is a <IMPULSE TURBINE> in which a liquid acts chiefly by its kinetic energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC IMPULSE TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PELTON TURBINE",null,null,null,null,null,"rdl:RDS1018754",null,"A <PELTON TURBINE> is a <HYDRAULIC IMPULSE TURBINE> operated from a high head source with small flow rate",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"IMPULSE TURBINE","STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IMPULSE STEAM TURBINE",null,null,null,null,null,"rdl:RDS815084",null,"An <IMPULSE STEAM TURBINE> is a <STEAM TURBINE> and an <IMPULSE TURBINE> that contains nozzles intended to act as high-speed jets and impulse blading. The pressure drops takes only place by expanding steam across the nozzle vanes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"IMPULSE STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CURTISS TURBINE",null,null,null,null,null,"rdl:RDS813509",null,"A <CURTISS TURBINE> is an <IMPULSE STEAM TURBINE> that is provided with one pressure stage, followed by more velocity stages",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"IMPULSE STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LAVAL TURBINE",null,null,null,null,null,"rdl:RDS815399",null,"A <LAVAL TURBINE> is an <IMPULSE STEAM TURBINE> that is provided with one pressure stage and one velocity stage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"IMPULSE STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ZOELLY-RATEAU TURBINE",null,null,null,null,null,"rdl:RDS817424",null,"A <ZOELLY-RATEAU TURBINE> is an <IMPULSE STEAM TURBINE> that is provided with more than one pressure stage, each followed by a velocity stage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TURBINE","KINETIC TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"REACTION TURBINE",null,null,null,null,null,"rdl:RDS406999491",null,"A <REACTION TURBINE> is an <ARTEFACT> and a <TURBINE> and a <KINETIC TO MECHANICAL ENERGY CONVERTER> in which a fluid acts both by its kinetic energy and by its pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"REACTION TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC REACTION TURBINE",null,null,null,null,null,"rdl:RDS1018709",null,"A <HYDRAULIC REACTION TURBINE> is a <REACTION TURBINE> that converts the potential energy of a flowing liquid to rotational energy for further use",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC REACTION TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AXIAL HYDRAULIC REACTION TURBINE",null,null,null,null,null,"rdl:RDS16772364",null,"An <AXIAL HYDRAULIC REACTION TURBINE> is a <HYDRAULIC REACTION TURBINE> where the flow path of the liquid is mainly parallel to the axis of rotation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AXIAL HYDRAULIC REACTION TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KAPLAN TURBINE",null,null,null,null,null,"rdl:RDS1018844",null,"A <KAPLAN TURBINE> is an <AXIAL HYDRAULIC REACTION TURBINE> that is provided with adjustable runner blades and operates at relatively high flow rates",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"KAPLAN TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROPELLER TURBINE",null,null,null,null,null,"rdl:RDS1018889",null,"A <PROPELLER TURBINE> is a <KAPLAN TURBINE> with non-adjustable runner blades suitable for non-varying head sources",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC REACTION TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FRANCIS TURBINE",null,null,null,null,null,"rdl:RDS1018799",null,"A <FRANCIS TURBINE> is a <HYDRAULIC REACTION TURBINE> with fixed runner blades usually operated from a medium or low head source with a medium flow rate",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"REACTION TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JET ENGINE",null,null,null,null,null,"rdl:RDS13118320",null,"A <JET ENGINE> is a <REACTION TURBINE> that generates thrust by jet propulsion. This includes airbreathing jet engines (turbojets, turbofans, ramjets, and pulse jets) and non-airbreathing jet engines (such as rocket engines)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"REACTION TURBINE","STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REACTION STEAM TURBINE",null,null,null,null,null,"rdl:RDS816389",null,"A <REACTION STEAM TURBINE> is a <STEAM TURBINE> and a <REACTION TURBINE> that is provided with stationary blades, which direct steam into passages between moving blades. The pressure drops across both fixed and moving blades",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"REACTION STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PARSONS TURBINE",null,null,null,null,null,"rdl:RDS815894",null,"A <PARSONS TURBINE> is a <REACTION STEAM TURBINE> that is of the multi-stage design",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STEAM TURBINE",null,null,null,null,null,"rdl:RDS416744",null,"A <STEAM TURBINE> is an <ARTEFACT> and a <TURBINE> that is a heat engine in which energy of steam is transformed into kinetic energy by means of expansion through nozzles and the kinetic energy of the resulting jet is in turn converted into force doing work on rings of blading mounted on a rotating shaft",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BACK PRESSURE STEAM TURBINE",null,null,null,null,null,"rdl:RDS433304",null,"A <BACK PRESSURE STEAM TURBINE> is a <STEAM TURBINE> where the exhaust is above atmospheric pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BACK PRESSURE STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXTRACTION BACK PRESSURE STEAM TURBINE",null,null,null,null,null,"rdl:RDS814274",null,"An <EXTRACTION BACK PRESSURE STEAM TURBINE> is a <BACK PRESSURE STEAM TURBINE> where steam is extracted from one or more stages",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EXTRACTION BACK PRESSURE STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AUTOMATIC EXTRACTION BACK PRESSURE STEAM TURBINE",null,null,null,null,null,"rdl:RDS16765164",null,"An <AUTOMATIC EXTRACTION BACK PRESSURE STEAM TURBINE> is an <EXTRACTION BACK PRESSURE STEAM TURBINE> where extraction takes place with a system for controlling the pressures of the extracted steam",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EXTRACTION BACK PRESSURE STEAM TURBINE","EXTRACTION CONDENSING STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-AUTOMATIC EXTRACTION CONDENSING STEAM TURBINE",null,null,null,null,null,"rdl:RDS409801401",null,"A <NON-AUTOMATIC EXTRACTION CONDENSING STEAM TURBINE> is an <EXTRACTION BACK PRESSURE STEAM TURBINE> where extraction takes place without means for controlling the pressures of the extracted steam",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BACK PRESSURE STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIXED PRESSURE BACK PRESSURE STEAM TURBINE",null,null,null,null,null,"rdl:RDS409578041",null,"A <MIXED PRESSURE BACK PRESSURE STEAM TURBINE> is a <BACK PRESSURE STEAM TURBINE> where steam enters the turbine at two or more pressures through separate inlet openings with means to control the inlet flows",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BACK PRESSURE STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STRAIGHT-FLOW BACK PRESSURE STEAM TURBINE",null,null,null,null,null,"rdl:RDS425446371",null,"A <STRAIGHT-FLOW BACK PRESSURE STEAM TURBINE> is a <BACK PRESSURE STEAM TURBINE> where all the steam enters the turbine at one pressure level and all the steam leaves the turbine at a pressure equal to or above atmospheric pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONDENSING STEAM TURBINE",null,null,null,null,null,"rdl:RDS813014",null,"A <> is a <STEAM TURBINE> where the exhaust steam pressure is below atmospheric pressure and the exhaust steam is condensed by means of a surface condenser",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONDENSING STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXTRACTION CONDENSING STEAM TURBINE",null,null,null,null,null,"rdl:RDS814319",null,"A <> is a <CONDENSING STEAM TURBINE> where steam is extracted from one or more stages",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EXTRACTION CONDENSING STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AUTOMATIC EXTRACTION CONDENSING STEAM TURBINE",null,null,null,null,null,"rdl:RDS16765209",null,"An extraction condensing steam turbine where extraction takes place with a system for controlling the pressures of the extracted steam",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONDENSING STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIXED PRESSURE CONDENSING STEAM TURBINE",null,null,null,null,null,"rdl:RDS409581461",null,"A <MIXED PRESSURE CONDENSING STEAM TURBINE> is a <CONDENSING STEAM TURBINE> where steam enters the turbine at two or more pressures through separate inlet openings with means to control the inlet flows",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONDENSING STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STRAIGHT-FLOW CONDENSING STEAM TURBINE",null,null,null,null,null,"rdl:RDS425447911",null,"A <STRAIGHT-FLOW CONDENSING STEAM TURBINE> is a <CONDENSING STEAM TURBINE> where all the steam enters the turbine at one pressure level and all the steam leaves the turbine at a pressure below atmospheric pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRALLY GEARED STEAM TURBINE",null,null,null,null,null,"rdl:RDS407884761",null,"An <INTEGRALLY GEARED STEAM TURBINE> is a <STEAM TURBINE> that",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LJUNGSTROM TURBINE",null,null,null,null,null,"rdl:RDS815579",null,"A <LJUNGSTROM TURBINE> is a <STEAM TURBINE> that is of the radial double-rotation design in which the blading is mounted on two wheels running in opposite direction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE COMPOUND TURBINE",null,null,null,null,null,"rdl:RDS413215851",null,"A <PRESSURE COMPOUND TURBINE> is a <STEAM TURBINE> where the pressure drop may be split with a number of stages and the velocity is absorbed over a number of bladed wheels",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STEAM TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VELOCITY COMPOUND TURBINE",null,null,null,null,null,"rdl:RDS427266821",null,"A <VELOCITY COMPOUND TURBINE> is a <STEAM TURBINE> where the pressure drop is in the nozzle only and the velocity is absorbed in a number of both fixed nozzles and bladed wheels",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TURBOCHARGER TURBINE",null,null,null,null,null,"rdl:RDS13662660",null,"A <TURBOCHARGER TURBINE> is a <TURBINE> that is utilized as driver of a turbocharger compressor, and in which rotary motion is produced by the exhaust gases from a combustion engine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TURBINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WIND TURBINE",null,null,null,null,null,"rdl:RDS2220058",null,"A <WIND TURBINE> is an <ARTEFACT> and a <TURBINE> that converts the kinetic energy of the wind into electrical power",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC TO ELECTRIC ENERGY CONVERTER",null,null,null,null,null,"rdl:RDS222503",null,"An <ELECTRIC TO ELECTRIC ENERGY CONVERTER> is an <ENERGY CONVERTER> that is capable of <ELECTRIC TO ELECTRIC ENERGY CONVERTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","ELECTRIC TO ELECTRIC ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC POWER CONVERTER",null,null,null,null,null,"rdl:RDS281924",null,"An <ELECTRIC POWER CONVERTER> is an <ARTEFACT> and an <ELECTRIC TO ELECTRIC ENERGY CONVERTER> that is an electrical circuit that changes the electric energy from one form into the desired form optimized for the specific load. A converter may do one or more functions and give an output that differs from the input. It is used to increase or decrease the magnitude of the input voltage, invert polarity, or produce several output voltages of either the same polarity with the input, different polarity, or mixed polarities such as in the computer power supply unit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC POWER CONVERTER","TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER TRANSFORMER",null,null,null,null,null,"rdl:RDS877814",null,"A <POWER TRANSFORMER> is a <TRANSFORMER> and an <ELECTRIC POWER CONVERTER> that, by electromagnetic induction, transforms a system of alternating voltage and current into another system of voltage and current usually of different values and at the same frequency for the purpose of transmitting electrical power",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AUTO-TRANSFORMER",null,null,null,null,null,"rdl:RDS644039",null,"An <AUTO-TRANSFORMER> is a <POWER TRANSFORMER> in which a part of the primary coil is used as a secondary, or a part of the secondary is used as a primary coil.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AUTO-TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTHING AUTOTRANSFORMER",null,null,null,null,null,"rdl:RDS878129",null,"An <EARTHING AUTOTRANSFORMER> is an <AUTO-TRANSFORMER> that is connected to a polyphase system in such a way that a neutral point is artificially obtained.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BOOSTER TRANSFORMER",null,null,null,null,null,"rdl:RDS888704",null,"A <BOOSTER TRANSFORMER> is a <POWER TRANSFORMER> of which one winding is intended to be connected in series with a circuit in order to alter its voltage and the other winding is an energizing winding.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DRY-TYPE TRANSFORMER",null,null,null,null,null,"rdl:RDS877994",null,"A <DRY-TYPE TRANSFORMER> is a <POWER TRANSFORMER> of which the magnetic circuit and windings are not immersed in an insulating liquid.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DRY-TYPE TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENCAPSULATED-WINDING DRY-TYPE TRANSFORMER",null,null,null,null,null,"rdl:RDS6232920",null,"An <ENCAPSULATED-WINDING DRY-TYPE TRANSFORMER> is a <DRY-TYPE TRANSFORMER> having one or more windings encapsulated with solid insulation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DRY-TYPE TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-ENCAPSULATED-WINDING DRY-TYPE TRANSFORMER",null,null,null,null,null,"rdl:RDS6232965",null,"A <NON-ENCAPSULATED-WINDING DRY-TYPE TRANSFORMER> is a <DRY-TYPE TRANSFORMER> having none of the windings encapsulated with solid insulation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FORCED COOLED TRANSFORMER",null,null,null,null,null,"rdl:RDS878174",null,"A <FORCED COOLED TRANSFORMER> is a <POWER TRANSFORMER> where either the primary or secondary cooling circuit is force cooled.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ISOLATION TRANSFORMER",null,null,null,null,null,"rdl:RDS878264",null,"An <ISOLATION TRANSFORMER> is a <POWER TRANSFORMER> designed to provide electrical isolation without stepping voltage and current either up or down.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MATCHING TRANSFORMER",null,null,null,null,null,"rdl:RDS987389",null,"A <MATCHING TRANSFORMER> is a <POWER TRANSFORMER> designed for insertion between two circuits having different impedances to optimize the power of the signal transferred.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NATURAL COOLED TRANSFORMER",null,null,null,null,null,"rdl:RDS878354",null,"A <NATURAL COOLED TRANSFORMER> is a <POWER TRANSFORMER> where both primary and secondary cooling circuits have natural circulation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OIL-IMMERSED TYPE TRANSFORMER",null,null,null,null,null,"rdl:RDS878309",null,"An <OIL-IMMERSED TYPE TRANSFORMER> is a <POWER TRANSFORMER> of which the magnetic circuit and windings are immersed in oil.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"OIL-IMMERSED TYPE TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIQUID IMMERSED TRANSFORMER WITH CONSERVATOR",null,null,null,null,null,"rdl:RDS878534",null,"A <LIQUID IMMERSED TRANSFORMER WITH CONSERVATOR> is an <OIL-IMMERSED TYPE TRANSFORMER> that has a liquid conservator.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"OIL-IMMERSED TYPE TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEALED TRANSFORMER",null,null,null,null,null,"rdl:RDS878624",null,"A <SEALED TRANSFORMER> is an <OIL-IMMERSED TYPE TRANSFORMER> that is non-breathing, that is, so sealed that there can be no significant interchange between its contents and the external atmosphere.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PORTABLE TRANSFORMER",null,null,null,null,null,"rdl:RDS878444",null,"A <PORTABLE TRANSFORMER> is a <POWER TRANSFORMER> that is portable and used for low voltage power tools.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED POWER TRANSFORMER",null,null,null,null,null,"rdl:RDS1186109",null,"A <RATED POWER TRANSFORMER> is a <POWER TRANSFORMER> conforming to a specification for performance given a set of conditions under which the transformer is designed to operate.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REGULATING TRANSFORMER",null,null,null,null,null,"rdl:RDS888659",null,"A <REGULATING TRANSFORMER> is a <POWER TRANSFORMER> with a special winding divided into several sections enabling the voltage to be varied at will.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEPARATE WINDING TRANSFORMER",null,null,null,null,null,"rdl:RDS6457996",null,"A <SEPARATE WINDING TRANSFORMER> is a <POWER TRANSFORMER>r having windings with no common parts.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE PHASE TRANSFORMER",null,null,null,null,null,"rdl:RDS878399",null,"A <SINGLE PHASE TRANSFORMER> is a <POWER TRANSFORMER> with two wire connection for single or two phase use.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE PHASE TRANSFORMER",null,null,null,null,null,"rdl:RDS878759",null,"A <THREE PHASE TRANSFORMER> is a <POWER TRANSFORMER> with three wire connection for three phase use.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THREE PHASE TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE-PHASE EARTHING TRANSFORMER",null,null,null,null,null,"rdl:RDS6458235",null,"A <THREE-PHASE EARTHING TRANSFORMER> is a <THREE PHASE TRANSFORMER> intended for connection in a network without a neutral, to provide an artificial neutral.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THREE PHASE TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VECTOR GROUP DYN 11 CONNECTED TRANSFORMER",null,null,null,null,null,"rdl:RDS1176254",null,"A <VECTOR GROUP DYN 11 CONNECTED TRANSFORMER> is a <THREE PHASE TRANSFORMER> with the primary winding delta-connected and the secondary winding star-connected with neutral brought out. The secondary winding lags the primary winding by 330 degree.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE WINDING TRANSFORMER",null,null,null,null,null,"rdl:RDS878804",null,"A <THREE WINDING TRANSFORMER> is a <POWER TRANSFORMER> that has an additional winding between primary and secondary.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TWO WINDING TRANSFORMER",null,null,null,null,null,"rdl:RDS878849",null,"A <TWO WINDING TRANSFORMER> is a <POWER TRANSFORMER> with primary and secondary windings.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POWER TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WELDING TRANSFORMER",null,null,null,null,null,"rdl:RDS878894",null,"A <WELDING TRANSFORMER> is a <POWER TRANSFORMER> that is intended to provide power for electric arc welding.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRIC TO ELECTRIC ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC CONVERTER",null,null,null,null,null,"rdl:RDS952199",null,"An <ELECTRONIC CONVERTER> is an <ARTEFACT> and an <ELECTRIC TO ELECTRIC ENERGY CONVERTER> for electronic power conversion, comprising one or more electronic valve devices, transformers and filters if necessary and auxiliaries if any",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC AC CONVERTER",null,null,null,null,null,"rdl:RDS6233775",null,"An <ELECTRONIC AC CONVERTER> is an <ELECTRONIC CONVERTER> for AC conversion",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC AC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECT AC CONVERTER",null,null,null,null,null,"rdl:RDS6234000",null,"A <DIRECT AC CONVERTER> is an <ELECTRONIC AC CONVERTER> without a d.c. link",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC AC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC AC VOLTAGE CONVERTER",null,null,null,null,null,"rdl:RDS952559",null,"An <ELECTRONIC AC VOLTAGE CONVERTER> is an <ELECTRONIC AC CONVERTER> for changing the voltage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC AC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC FREQUENCY CONVERTER",null,null,null,null,null,"rdl:RDS17859175",null,"An <ELECTRONIC FREQUENCY CONVERTER> is an <ELECTRONIC AC CONVERTER> for changing the frequency",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC FREQUENCY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CYCLOCONVERTER",null,null,null,null,null,"rdl:RDS952604",null,"A <CYCLOCONVERTER> is an <ELECTRONIC FREQUENCY CONVERTER> that by creating an alternating voltage from successive voltage samples of suitable frequency and duration provides a higher or lower output frequency",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC FREQUENCY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THYRISTOR UNIT",null,null,null,null,null,"rdl:RDS427143161",null,"A <THYRISTOR UNIT> is an <ELECTRONIC FREQUENCY CONVERTER> for a electric motor of a variable transmission to run at variable speed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC AC CONVERTER","PHASE CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC PHASE CONVERTER",null,null,null,null,null,"rdl:RDS952514",null,"A <ELECTRONIC PHASE CONVERTER> is an <ELECTRONIC AC CONVERTER> and a <PHASE CONVERTER> for changing the number of phases",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC AC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDIRECT AC CONVERTER",null,null,null,null,null,"rdl:RDS952424",null,"An <INDIRECT AC CONVERTER> is an <ELECTRONIC AC CONVERTER> with a dc link",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC AC POWER CONTROLLER",null,null,null,null,null,"rdl:RDS953144",null,"An <ELECTRONIC AC POWER CONTROLLER> is an <ELECTRONIC CONVERTER> that is able to operate as a controllable direct electronic ac voltage converter as well as an electronic ac switch",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC DC CONVERTER",null,null,null,null,null,"rdl:RDS952649",null,"An <ELECTRONIC DC CONVERTER> is an <ELECTRONIC CONVERTER> for dc conversion",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC DC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECT DC CONVERTER",null,null,null,null,null,"rdl:RDS952694",null,"A <DIRECT DC CONVERTER> is an <ELECTRONIC DC CONVERTER> without an ac link",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC DC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE CONVERTER",null,null,null,null,null,"rdl:RDS953009",null,"A <DOUBLE CONVERTER> is an <ELECTRONIC DC CONVERTER> that is a current stiff reversible ac/dc converter with direct current in both directions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC DC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDIRECT DC CONVERTER",null,null,null,null,null,"rdl:RDS952739",null,"An <INDIRECT DC CONVERTER> is an <ELECTRONIC DC CONVERTER> with an ac link",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC DC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE CONVERTER",null,null,null,null,null,"rdl:RDS952964",null,"A <SINGLE CONVERTER> is an <ELECTRONIC DC CONVERTER> that is a current stiff reversible ac/dc converter with direct current in one direction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC DC POWER CONTROLLER",null,null,null,null,null,"rdl:RDS339711440",null,"An <ELECTRONIC DC POWER CONTROLLER> is an <ELECTRONIC CONVERTER> that is able to operate as a controllable direct electronic d.c. voltage converter as well as an electronic d.c. switch",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC DC POWER CONVERTER",null,null,null,null,null,"rdl:RDS953189",null,"An <ELECTRONIC DC POWER CONVERTER> is an <ELECTRONIC CONVERTER> which is able to operate as a controllable direct electronic d.c. voltage convertor as well as an electronic d.c. switch",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC POWER INVERTER",null,null,null,null,null,"rdl:RDS952289",null,"An <ELECTRONIC POWER INVERTER> is an <ELECTRONIC CONVERTER> that changes direct electric current to single-phase or polyphase alternating currents",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CONVERTER","RECTIFIER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC POWER RECTIFIER",null,null,null,null,null,"rdl:RDS952244",null,"An <ELECTRONIC POWER RECTIFIER> is an <ELECTRONIC CONVERTER> and a <RECTIFIER>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REVERSIBLE CONVERTER",null,null,null,null,null,"rdl:RDS952919",null,"A <REVERSIBLE CONVERTER> is an <ELECTRONIC CONVERTER> in which the direction of the power flow is reversible",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEMICONDUCTOR CONVERTER",null,null,null,null,null,"rdl:RDS953234",null,"A <SEMICONDUCTOR CONVERTER> is an <ELECTRONIC CONVERTER> with semiconductor valve devices",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRIC TO ELECTRIC ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"FOUR-QUADRANT CONVERTER",null,null,null,null,null,"rdl:RDS952874",null,"A <FOUR-QUADRANT CONVERTER> is an <ARTEFACT> and an <ELECTRIC TO ELECTRIC ENERGY CONVERTER> with two directions of d.c. power flow, associated with two directions of direct voltage and two directions of direct current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRIC TO ELECTRIC ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"ONE-QUADRANT CONVERTER",null,null,null,null,null,"rdl:RDS952784",null,"A <ONE-QUADRANT CONVERTER> is an <ARTEFACT> and an <ELECTRIC TO ELECTRIC ENERGY CONVERTER> with one possible direction of dc power flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRIC TO ELECTRIC ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"PHASE CONVERTER",null,null,null,null,null,"rdl:RDS986759",null,"A <PHASE CONVERTER> is an <ARTEFACT> and an <ELECTRIC TO ELECTRIC ENERGY CONVERTER> that changes the number of phases associated with electric energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE","PHASE CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTATING PHASE CONVERTER",null,null,null,null,null,"rdl:RDS7220685",null,"A <ROTATING PHASE CONVERTER> is an <ELECTRIC ROTATING MACHINE> and a <PHASE CONVERTER> that transfers electrical energy with change in the number of phases",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRIC TO ELECTRIC ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"PHASE SHIFTER",null,null,null,null,null,"rdl:RDS986804",null,"A <PHASE SHIFTER> is an <ARTEFACT> and an <ELECTRIC TO ELECTRIC ENERGY CONVERTER> that introduces a change in the phase of an oscillation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRIC TO ELECTRIC ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"RECTIFIER",null,null,null,null,null,"rdl:RDS478034",null,"A <RECTIFIER> is an <ARTEFACT> and an <ELECTRIC TO ELECTRIC ENERGY CONVERTER> for converting an alternating current into a direct current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC TO ELECTRIC ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRANSFORMER",null,null,null,null,null,"rdl:RDS643994",null,"A <TRANSFORMER> is an <ENERGY CONVERTER> that is capable of <TRANSFORMING> power from one circuit to another without changing frequency and works on the principle of mutual induction",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT TRANSFORMER",null,null,null,null,null,"rdl:RDS877769",null,"An <INSTRUMENT TRANSFORMER> is an <ARTEFACT> and a <TRANSFORMER> that is used to isolate or transform voltage or current levels. The most common usage of instrument transformers is to operate instruments or metering from high voltage or high current circuits, safely isolating secondary control circuitry from the high voltages or currents",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMBINED TRANSFORMER",null,null,null,null,null,"rdl:RDS6454817",null,"A <COMBINED TRANSFORMER> is an <INSTRUMENT TRANSFORMER> consisting of a current and a voltage transformer in the same case.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS877859",null,"A <CURRENT TRANSFORMER> is an <INSTRUMENT TRANSFORMER> in which the secondary current, in normal conditions of use, is substantially proportional to the primary current and differs in phase from it by an angle which is approximately zero for an appropriate direction of the connections.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AUTO-COMPOUND CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6455280",null,"An <AUTO-COMPOUND CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> having an auxiliary winding in series with the secondary of the transformer, especially intended to reduce the phase displacement between the primary and secondary currents.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BAR PRIMARY BUSHING TYPE CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6455325",null,"A <BAR PRIMARY BUSHING TYPE CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> so constructed that it can be used as a bushing.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BAR PRIMARY TYPE CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6455415",null,"A <BAR PRIMARY TYPE CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> in which the primary conductor is made up of a bar or a set of bars in parallel.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUS TYPE CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6455460",null,"A <BUS TYPE CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> without primary conductor, but with primary insulation, which can be fitted directly over a conductor or busbar.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUSHING TYPE CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6455505",null,"A <BUSHING TYPE CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> without primary conductor and primary insulation of its own which can be fitted directly over an insulated bushing or conductor.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TYPE CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6455550",null,"A <CABLE TYPE CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> without primary conductor and primary insulation of its own, which can be mounted over an insulated cable.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPOUND-WOUND CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6455612",null,"A <COMPOUND-WOUND CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> having an auxiliary winding with an independent supply especially intended to reduce the phase displacement between the primary and secondary currents.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT MATCHING TRANSFORMER",null,null,null,null,null,"rdl:RDS6455657",null,"A <CURRENT MATCHING TRANSFORMER> is a <CURRENT TRANSFORMER> for matching the rated secondary current of the main current transformer to the rated current of the burden, or for reducing the instrument security factor.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXTENDED RATING TYPE CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6455702",null,"An <EXTENDED RATING TYPE CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> having a rated continuous thermal current higher than rated primary current and for which accuracy requirements are prescribed at that current.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FULLY INSULATED CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6455747",null,"A <FULLY INSULATED CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> having as an integral part of its construction, insulation suitable for its rated insulation level.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTI-CORE TYPE CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6455792",null,"A <MULTI-CORE TYPE CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> comprising a number of magnetically separated cores with individual secondary windings and a common primary winding.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE-CORE TYPE CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6455837",null,"A <SINGLE-CORE TYPE CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> in which only one magnetic core with one secondary winding and one primary winding are provided.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPLIT CORE TYPE CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6455927",null,"An <SPLIT CORE TYPE CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> without primary conductor, and primary insulation of its own, the magnetic circuit of which can be hinged open (or otherwise separated into two parts) and then closed around the insulated conductor carrying the current to be measured.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUMMATION CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS877904",null,"A <SUMMATION CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> for the measurement of the sum of the instantaneous values of currents having the same frequency within a power system.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUPPORT TYPE CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6455972",null,"A <SUPPORT TYPE CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> so arranged that it acts as a support for the conductor in the primary circuit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WOUND PRIMARY TYPE CURRENT TRANSFORMER",null,null,null,null,null,"rdl:RDS6456017",null,"A <WOUND PRIMARY TYPE CURRENT TRANSFORMER> is a <CURRENT TRANSFORMER> in which the primary winding consists of a single or multi-turn coil.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT AUTOTRANSFORMER",null,null,null,null,null,"rdl:RDS6454977",null,"An <INSTRUMENT AUTOTRANSFORMER> is an <INSTRUMENT TRANSFORMER> in which the primary and the secondary windings have a common part.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE TRANSFORMER",null,null,null,null,null,"rdl:RDS877949",null,"A <VOLTAGE TRANSFORMER> is an <INSTRUMENT TRANSFORMER> in which the secondary voltage, in normal conditions of use, is substantially proportional to the primary voltage and differs in phase from it by an angle which is approximately zero for an appropriate direction of the connections.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLTAGE TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAPACITOR VOLTAGE TRANSFORMER",null,null,null,null,null,"rdl:RDS6462557",null,"A <CAPACITOR VOLTAGE TRANSFORMER> is a <VOLTAGE TRANSFORMER> comprising a capacitor divider unit and an electromagnetic.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLTAGE TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CASCADE VOLTAGE TRANSFORMER",null,null,null,null,null,"rdl:RDS6462602",null,"A <CASCADE VOLTAGE TRANSFORMER> is a <VOLTAGE TRANSFORMER>in which the primary winding is equally distributed over two or more insulated magnetic cores suitably electro-magnetically coupled.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLTAGE TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTHED VOLTAGE TRANSFORMER",null,null,null,null,null,"rdl:RDS6462647",null,"An <EARTHED VOLTAGE TRANSFORMER> is a <VOLTAGE TRANSFORMER> that is single phase and intended to have one end of its primary winding directly earthed, or a three phase voltage transformer which is intended to have the star point of its primary winding directly earthed.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLTAGE TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UNEARTHED VOLTAGE TRANSFORMER",null,null,null,null,null,"rdl:RDS6462692",null,"A <UNEARTHED VOLTAGE TRANSFORMER> is a <VOLTAGE TRANSFORMER> that has all parts of its primary winding, including terminals, insulated from earth at a level corresponding to its rated insulation level.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLTAGE TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE MATCHING TRANSFORMER",null,null,null,null,null,"rdl:RDS6462737",null,"A <VOLTAGE MATCHING TRANSFORMER> is a <VOLTAGE TRANSFORMER> for matching the rated secondary voltage of the main voltage transformer to the rated voltage of the burden.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PULSE TRANSFORMER",null,null,null,null,null,"rdl:RDS5771511",null,"A <PULSE TRANSFORMER> is an <ARTEFACT> and a <TRANSFORMER> that is optimised for transmitting rectangular electrical pulses, i.e. pulses with fast rise and fall times and a constant rate",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TAPPED TRANSFORMER",null,null,null,null,null,"rdl:RDS644084",null,"A <TAPPED TRANSFORMER> is an <ARTEFACT> and a <TRANSFORMER> comprising a tapped primary or secondary winding to obtain a variable secondary voltage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TAPPED TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRANSFORMER TAPPED AT PRIMARY SIDE",null,null,null,null,null,"rdl:RDS1176299",null,"A <TRANSFORMER TAPPED AT PRIMARY SIDE> is a <TAPPED TRANSFORMER> in which the primary winding is tapped.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER TAPPED AT PRIMARY SIDE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TAPPED TRANSFORMER AT PRIMARY SIDE +/- 2X2,5%",null,null,null,null,null,"rdl:RDS1176344",null,"A <TAPPED TRANSFORMER AT PRIMARY SIDE +/- 2X2,5%> is a <TRANSFORMER TAPPED AT PRIMARY SIDE> having altogether 2 tappings symmetrical placed, one 2,5 % above and one 2,5 % below rated voltage.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TAPPED TRANSFORMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRANSFORMER TAPPED AT SECONDARY SIDE",null,null,null,null,null,"rdl:RDS6697480",null,"A <TRANSFORMER TAPPED AT SECONDARY SIDE> is a <TAPPED TRANSFORMER> in which the secondary winding is tapped.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRIC TO ELECTRIC ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TWO-QUADRANT CONVERTER",null,null,null,null,null,"rdl:RDS952829",null,"A <TWO-QUADRANT CONVERTER> is an <ARTEFACT> and an <ELECTRIC TO ELECTRIC ENERGY CONVERTER> with two possible directions of d.c. power flow associated with one direction of direct current and two directions of direct voltage or vice versa",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRIC TO ELECTRIC ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VARIABLE SPEED DRIVE CONVERTER",null,null,null,null,null,"rdl:RDS6624633",null,"A <VARIABLE SPEED DRIVE CONVERTER> is an <ARTEFACT> and an <ELECTRIC TO ELECTRIC ENERGY CONVERTER> that is intended to provide power to electric motor(s) such that the speed or torque of the motor(s) may be varied in proportion with a <STANDARD SIGNAL>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,"rdl:RDS2220072",null,"A <ELECTRIC TO MECHANICAL ENERGY CONVERTER> is an <ENERGY CONVERTER> that is capable of <ELECTRIC TO MECHANICAL ENERGY CONVERTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","MACHINE","ELECTRIC TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC MACHINE",null,null,null,null,null,"rdl:RDS986714",null,"An <ELECTRIC MACHINE> is an <ARTEFACT> and a <MACHINE> and an <ELECTRIC TO MECHANICAL ENERGY CONVERTER>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ASYNCHRONOUS MACHINE",null,null,null,null,null,"rdl:RDS1000979",null,"An <ASYNCHRONOUS MACHINE> is an <ELECTRIC ROTATING MACHINE> in which the speed on load and the frequency of the system to which it is connected are not in a constant ratio",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ASYNCHRONOUS MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDUCTION MACHINE",null,null,null,null,null,"rdl:RDS1001069",null,"An <INDUCTION MACHINE> is an <ASYNCHRONOUS MACHINE> of which only one set poles is energized.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDUCTION MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALTERNATING CURRENT COMMUTATOR MACHINE",null,null,null,null,null,"rdl:RDS1001114",null,"An <ALTERNATING CURRENT COMMUTATOR MACHINE> is an <INDUCTION MACHINE> having an armature winding connected to a commutator.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CANNED MACHINE",null,null,null,null,null,"rdl:RDS7248200",null,"A <CANNED MACHINE> is an <ELECTRIC MACHINE> of which specified parts are completely enclosed and protected against a fluid by a sealing sheath so the stator is moving/rotor is static",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CLOSED MACHINE",null,null,null,null,null,"rdl:RDS7248245",null,"A <CLOSED MACHINE> is an <ELECTRIC MACHINE> where no medium from the surrounding medium, for the purpose of cooling, passes through the machine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CLOSED MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR-TO-AIR COOLED MACHINE",null,null,null,null,null,"rdl:RDS7248110",null,"An <AIR-TO-AIR COOLED MACHINE> is a <CLOSED MACHINE> having integral or machine-mounted heat exchanger, using air as the primary and secondary coolant",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CLOSED MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR-TO-WATER COOLED MACHINE",null,null,null,null,null,"rdl:RDS7248155",null,"An <AIR-TO-WATER COOLED MACHINE> is a <CLOSED MACHINE> with a heat exchanger using air as primary coolant and water as secondary coolant",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CLOSED MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FRAME SURFACE COOLED MACHINE",null,null,null,null,null,"rdl:RDS7247660",null,"A <FRAME SURFACE COOLED MACHINE> is a <CLOSED MACHINE> in which the frame surface is cooled by the surrounding medium",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRAME SURFACE COOLED MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TOTALLY ENCLOSED FAN COOLED MACHINE",null,null,null,null,null,"rdl:RDS7247120",null,"A <TOTALLY ENCLOSED FAN COOLED MACHINE> is a <FRAME SURFACE COOLED MACHINE> over which the surrounding air is driven by a fan for cooling purposes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,"rdl:RDS1000844",null,"An <ELECTRIC ROTATING MACHINE> is an <ELECTRIC MACHINE> depending on electromagnetic induction for its operation and having components capable of relative rotary movement and intended for converting energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONICAL ROTOR MACHINE",null,null,null,null,null,"rdl:RDS1001384",null,"A <CONICAL ROTOR MACHINE> is an <ELECTRIC ROTATING MACHINE> with a rotor in the shape of a frustum of a cone",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CYLINDRICAL ROTOR MACHINE",null,null,null,null,null,"rdl:RDS1001339",null,"A <CYLINDRICAL ROTOR MACHINE> is an <ELECTRIC ROTATING MACHINE> having a cylindrically shaped rotor the periphery of which may be provided with slots which accommodate the coil sides of a winding",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECT CURRENT MACHINE",null,null,null,null,null,"rdl:RDS7215102",null,"A <DIRECT CURRENT MACHINE> is an <ELECTRIC ROTATING MACHINE> incorporating an armature winding connected via a commutator to a direct current system and having magnetic poles which are excited from a source of direct or undulating current or which are permanent magnets",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECT WATER-COOLED MACHINE",null,null,null,null,null,"rdl:RDS7247615",null,"A <DIRECT WATER-COOLED MACHINE> is an <ELECTRIC ROTATING MACHINE> that is water cooled",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC ROTATING MACHINE FOR VERTICAL MOUNTING",null,null,null,null,null,"rdl:RDS1128239",null,"An <ELECTRIC ROTATING MACHINE FOR VERTICAL MOUNTING> is an <ELECTRIC ROTATING MACHINE> that is designed for vertical orientation on site with regard to alignment and position of fixing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC ROTATING MACHINE FOR HORIZONTAL AND VERTICAL MOUNTING",null,null,null,null,null,"rdl:RDS1128194",null,"An <ELECTRIC ROTATING MACHINE FOR HORIZONTAL AND VERTICAL MOUNTING> is an <ELECTRIC ROTATING MACHINE> that is designed for horizontal and vertical orientation on site with regard to alignment and position of fixing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL DYNAMOMETER",null,null,null,null,null,"rdl:RDS7220747",null,"An <ELECTRICAL DYNAMOMETER> is an <ELECTRIC ROTATING MACHINE> equipped with means for indicating torque and additionally with means for indicating speed when used for determining power",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE DESIGNED FOR SHAFT DRIVEN TRANSMISSION",null,null,null,null,null,"rdl:RDS14128484",null,"An <ELECTRICAL ROTATING MACHINE DESIGNED FOR SHAFT DRIVEN TRANSMISSION> is an <ELECTRIC ROTATING MACHINE> that is designed to take the forces connected to the direct transmission of rotational power through a shaft",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE DESIGNED FOR BELT DRIVEN TRANSMISSION",null,null,null,null,null,"rdl:RDS14128377",null,"An <ELECTRICAL ROTATING MACHINE DESIGNED FOR BELT DRIVEN TRANSMISSION> is an <ELECTRIC ROTATING MACHINE> that is designed to to take the forces connected to transmission of rotational power through a belt drive",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 10 POLES",null,null,null,null,null,"rdl:RDS1012679",null,"An <ELECTRICAL ROTATING MACHINE 10 POLES> is an <ELECTRIC ROTATING MACHINE> that has 10 poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 12 POLES",null,null,null,null,null,"rdl:RDS1012724",null,"An <ELECTRICAL ROTATING MACHINE 12 POLES> is an <ELECTRIC ROTATING MACHINE> that has 12 poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 2 POLES",null,null,null,null,null,"rdl:RDS1012499",null,"An <ELECTRICAL ROTATING MACHINE 2 POLES> is an <ELECTRIC ROTATING MACHINE> that has 2 poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 4 POLES",null,null,null,null,null,"rdl:RDS1012544",null,"An <ELECTRICAL ROTATING MACHINE 4 POLES> is an <ELECTRIC ROTATING MACHINE> that has 4 poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 6 POLES",null,null,null,null,null,"rdl:RDS1012589",null,"An <ELECTRICAL ROTATING MACHINE 6 POLES> is an <ELECTRIC ROTATING MACHINE> that has 6 poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 8 POLES",null,null,null,null,null,"rdl:RDS1012634",null,"An <ELECTRICAL ROTATING MACHINE 8 POLES> is an <ELECTRIC ROTATING MACHINE> that has 8 poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE THREE PHASE",null,null,null,null,null,"rdl:RDS1016909",null,"An <ELECTRICAL ROTATING MACHINE THREE PHASE> is an <ELECTRIC ROTATING MACHINE> connected to a three phase system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL ROTATING MACHINE THREE PHASE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE DELTA CONNECTED",null,null,null,null,null,"rdl:RDS1018169",null,"An <ELECTRICAL ROTATING MACHINE DELTA CONNECTED> is an <ELECTRICAL ROTATING MACHINE THREE PHASE> where the windings are delta connected.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL ROTATING MACHINE THREE PHASE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE STAR CONNECTED",null,null,null,null,null,"rdl:RDS1018124",null,"An <ELECTRICAL ROTATING MACHINE STAR CONNECTED> is an <ELECTRICAL ROTATING MACHINE THREE PHASE> where the windings are star connected.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 1000 RPM",null,null,null,null,null,"rdl:RDS8631287",null,"An <ELECTRICAL ROTATING MACHINE 1000 RPM> is an <ELECTRIC ROTATING MACHINE> that is rotating at 1000 rpm",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 1200 RPM",null,null,null,null,null,"rdl:RDS8631332",null,"An <ELECTRICAL ROTATING MACHINE 1200 RPM> is an <ELECTRIC ROTATING MACHINE> that is rotating at a nominal speed of 1200 rpm",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 1500 RPM",null,null,null,null,null,"rdl:RDS8631242",null,"An <ELECTRICAL ROTATING MACHINE 1500 RPM> is an <ELECTRIC ROTATING MACHINE> that is rotating at 1500 rpm",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 1800 RPM",null,null,null,null,null,"rdl:RDS8631377",null,"An <ELECTRICAL ROTATING MACHINE 1800 RPM> is an <ELECTRIC ROTATING MACHINE> is rotating at a nominal speed of 1800 rpm",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 3000 RPM",null,null,null,null,null,"rdl:RDS8631422",null,"An <ELECTRICAL ROTATING MACHINE 3000 RPM> is an <ELECTRIC ROTATING MACHINE> that is rotating at a nominal speed of 3000 rpm",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 3600 RPM",null,null,null,null,null,"rdl:RDS8631467",null,"An <ELECTRICAL ROTATING MACHINE 3600 RPM> is an <ELECTRIC ROTATING MACHINE> that is rotating at a nominal speed of 3600 rpm",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 500 RPM",null,null,null,null,null,"rdl:RDS8631512",null,"An <ELECTRICAL ROTATING MACHINE 500 RPM> is an <ELECTRIC ROTATING MACHINE> that is rotating at a nominal sped of <500 rpm",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 600 RPM",null,null,null,null,null,"rdl:RDS8631602",null,"An <ELECTRICAL ROTATING MACHINE 600 RPM> is an <ELECTRIC ROTATING MACHINE> that is rotating at a nominal speed of 600 rpm",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 720 RPM",null,null,null,null,null,"rdl:RDS8631647",null,"An <ELECTRICAL ROTATING MACHINE 720 RPM> is an <ELECTRIC ROTATING MACHINE> that is rotating at a nominal speed of 720 rpm",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 750 RPM",null,null,null,null,null,"rdl:RDS8631692",null,"An <ELECTRICAL ROTATING MACHINE 750 RPM> is an <ELECTRIC ROTATING MACHINE> that is rotating at a nominal speed of 750 rpm",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ROTATING MACHINE 900 RPM",null,null,null,null,null,"rdl:RDS8631737",null,"An <ELECTRICAL ROTATING MACHINE 900 RPM> is an <ELECTRIC ROTATING MACHINE> that is rotating at a nominal speed of 900 rpm",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OPEN MACHINE",null,null,null,null,null,"rdl:RDS7247705",null,"An <OPEN MACHINE> is an <ELECTRIC ROTATING MACHINE> with an open cooling circuit in which the coolant is drawn directly from the surrounding medium passing through the machine and then returning directly to the surrounding medium",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PERMANENT MAGNET MACHINE",null,null,null,null,null,"rdl:RDS7220146",null,"A <PERMANENT MAGNET MACHINE> is an <ELECTRIC ROTATING MACHINE> in which the field system consists of one or more permanent magnets",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POLYPHASE MACHINE",null,null,null,null,null,"rdl:RDS1001249",null,"A <POLYPHASE MACHINE> is an <ELECTRIC ROTATING MACHINE> for the generation or utilization of polyphase alternating voltage and current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURIZED MACHINE",null,null,null,null,null,"rdl:RDS7247750",null,"A <PRESSURIZED MACHINE> is an <ELECTRIC ROTATING MACHINE> in which the internal coolant is kept at a higher pressure than the surrounding medium",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTATING FREQUENCY CONVERTER",null,null,null,null,null,"rdl:RDS7220623",null,"A <ROTATING FREQUENCY CONVERTER> is an <ELECTRIC ROTATING MACHINE> that converts electrical energy from one frequency to another",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROTATING FREQUENCY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMMUTATOR TYPE FREQUENCY CONVERTER",null,null,null,null,null,"rdl:RDS7222063",null,"A <COMMUTATOR TYPE FREQUENCY CONVERTER> is a <ROTATING FREQUENCY CONVERTER> the rotor of which has one or two windings connected to a set of slip-rings and to a commutator such that by feeding one set of brushes with a voltage of a given frequency, a voltage of another frequency may be obtained from the other set",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROTATING FREQUENCY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDUCTOR FREQUENCY CONVERTER",null,null,null,null,null,"rdl:RDS7222187",null,"An <INDUCTOR FREQUENCY CONVERTER> is a <ROTATING FREQUENCY CONVERTER> having a stationary input alternating current winding which supplies the excitation, and a stationary output winding of a different number of poles in which the generated voltage at the output frequency is induced through change in field reluctance by a number of regular projections of the rotor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SALIENT POLE MACHINE",null,null,null,null,null,"rdl:RDS1001294",null,"A <SALIENT POLE MACHINE> is an <ELECTRIC ROTATING MACHINE> in which the field poles project from the frame yoke or hub towards the air-gap",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SALIENT POLE MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID POLE SHOE MACHINE",null,null,null,null,null,"rdl:RDS7221939",null,"A <SOLID POLE SHOE MACHINE> is a <SALIENT POLE MACHINE> having non-laminated pole shoes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEALED MACHINE",null,null,null,null,null,"rdl:RDS7247795",null,"A <SEALED MACHINE> is an <ELECTRIC ROTATING MACHINE> provided with special seals to minimise the leakage of the internal coolant out of the enclosure, or of the surrounding medium into the machine, during normal operation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SELF-COOLED MACHINE",null,null,null,null,null,"rdl:RDS7247840",null,"A <SELF-COOLED MACHINE> is an <ELECTRIC ROTATING MACHINE> where the cooling is obtained by means of its own rotation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEPARATELY-COOLED MACHINE",null,null,null,null,null,"rdl:RDS7247885",null,"A <SEPARATELY-COOLED MACHINE> is an <ELECTRIC ROTATING MACHINE> where the cooling is obtained by other means than its own rotation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE-PHASE MACHINE",null,null,null,null,null,"rdl:RDS1001204",null,"A <SINGLE-PHASE MACHINE> is an <ELECTRIC ROTATING MACHINE> for the generation or utilization of single-phase alternating voltage and current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SINGLE-PHASE MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE PHASE COMMUTATOR MOTOR",null,null,null,null,null,"rdl:RDS7221860",null,"A <SINGLE PHASE COMMUTATOR MOTOR> is a <SINGLE-PHASE MACHINE> that is an electric motor with a single phase armature winding fed through a commutator",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ROTATING MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYNCHRONOUS MACHINE",null,null,null,null,null,"rdl:RDS1000934",null,"A <SYNCHRONOUS MACHINE> is an <ELECTRIC ROTATING MACHINE> in which the frequency of the generated voltages and the speed of the machine are in a constant ratio",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SYNCHRONOUS MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDUCTOR MACHINE",null,null,null,null,null,"rdl:RDS1001159",null,"An <INDUCTOR MACHINE> is a <A SYNCHRONOUS MACHINE> in which one member, usually stationary, carries main and exciting windings effectively disposed relative to each other, and in which the other member, usually rotating, is without windings but carries a number of regular projections. Permanent magnets may be used instead of the exciting winding.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRIC GENERATOR","SYNCHRONOUS MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYNCHRONOUS GENERATOR",null,null,null,null,null,"rdl:RDS1001564",null,"A <SYNCHRONOUS GENERATOR> is an <ARTEFACT> and an <ELECTRIC GENERATOR> and a <SYNCHRONOUS MACHINE> used as a generator",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL BOOSTER",null,null,null,null,null,"rdl:RDS1003904",null,"An <ELECTRICAL BOOSTER> is an <ELECTRIC MACHINE> connected in a circuit so that its voltage either adds to or subtracts from the voltage furnished by another source",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC MACHINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PHASE ADVANCER",null,null,null,null,null,"rdl:RDS1004084",null,"A <PHASE ADVANCER> is an <ELECTRIC MACHINE> that supplies reactive power to the secondary of a wound rotor induction motor to improve the power factor of the latter",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,"rdl:RDS279944",null,"A <HYDRAULIC TO MECHANICAL ENERGY CONVERTER> is an <ENERGY CONVERTER> that is capable of <HYDRAULIC TO MECHANICAL ENERGY CONVERTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","CONTROLLED ACTUATOR","HYDRAULIC TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC ACTUATOR",null,null,null,null,null,"rdl:RDS430154",null,"A <HYDRAULIC ACTUATOR> is an <INSTRUMENTATION ITEM> and a <CONTROLLED ACTUATOR> and a <HYDRAULIC TO MECHANICAL ENERGY CONVERTER>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ACTUATOR","HYDRAULIC ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC HYDRAULIC ACTUATOR",null,null,null,null,null,"rdl:RDS7195780",null,"An <ELECTRIC HYDRAULIC ACTUATOR> is an <ELECTRIC ACTUATOR> and a <HYDRAULIC ACTUATOR> having a fluid pump driven by an electric motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC HYDRAULIC ACTUATOR","VALVE ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRO-HYDRAULIC VALVE ACTUATOR",null,null,null,null,null,"rdl:RDS16742011",null,"An <ELECTRO-HYDRAULIC VALVE ACTUATOR> is a <VALVE ACTUATOR> and a <ELECTRIC HYDRAULIC ACTUATOR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC PISTON ACTUATOR",null,null,null,null,null,"rdl:RDS884879",null,"A <HYDRAULIC PISTON ACTUATOR> is a <HYDRAULIC ACTUATOR> that is intended to operate by a displacement of a piston using hydraulic energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOUBLE ACTING ACTUATOR","HYDRAULIC PISTON ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE ACTING HYDRAULIC PISTON ACTUATOR",null,null,null,null,null,"rdl:RDS6625578",null,"A <DOUBLE ACTING HYDRAULIC PISTON ACTUATOR> is a <HYDRAULIC PISTON ACTUATOR> and a <DOUBLE ACTING ACTUATOR> that is a hydraulic piston actuator that is actuated by hydraulic fluid and is driven in both directions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC PISTON ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC PISTON ACTUATOR SPRING RETURN",null,null,null,null,null,"rdl:RDS11507614",null,"A <HYDRAULIC PISTON ACTUATOR SPRING RETURN> is a <HYDRAULIC PISTON ACTUATOR> with a spring acting on one side of the piston",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC PISTON ACTUATOR","SINGLE ACTING ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE ACTING HYDRAULIC PISTON ACTUATOR",null,null,null,null,null,"rdl:RDS6625353",null,"A <SINGLE ACTING HYDRAULIC PISTON ACTUATOR> is a <HYDRAULIC PISTON ACTUATOR> that is actuated by hydraulic fluid and is driven in one direction only",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC ACTUATOR","VALVE ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC VALVE ACTUATOR",null,null,null,null,null,"rdl:RDS7503442",null,"A <HYDRAULIC VALVE ACTUATOR> is a <HYDRAULIC ACTUATOR> and a <VALVE ACTUATOR> that is designed to operate a valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC TO ROTATION ENERGY CONVERTER",null,null,null,null,null,"rdl:RDS2220074",null,"A <HYDRAULIC TO ROTATION ENERGY CONVERTER> is an <HYDRAULIC TO MECHANICAL ENERGY CONVERTER> that is capable of <HYDRAULIC TO ROTATION ENERGY CONVERTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"KINETIC TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,"rdl:RDS2220075",null,"A <KINETIC TO MECHANICAL ENERGY CONVERTER> is an <ENERGY CONVERTER> that is capable of <KINETIC TO MECHANICAL ENERGY CONVERTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"MECHANICAL TO ELECTRIC ENERGY CONVERTER",null,null,null,null,null,"rdl:RDS2220076",null,"A <MECHANICAL TO ELECTRIC ENERGY CONVERTER> is an <ENERGY CONVERTER> that is capable of <MECHANICAL TO ELECTRIC ENERGY CONVERTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","GENERATOR","MECHANICAL TO ELECTRIC ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC POWER GENERATOR",null,null,null,null,null,"rdl:RDS2221104",null,"An <ELECTRIC POWER GENERATOR> is an <ARTEFACT> and a <GENERATOR> and a <MECHANICAL TO ELECTRIC ENERGY CONVERTER>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"MECHANICAL TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,"rdl:RDS2225766",null,"A <MECHANICAL TO MECHANICAL ENERGY CONVERTER> is an <ENERGY CONVERTER> that is capable of <MECHANICAL TO MECHANICAL ENERGY CONVERTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","MECHANICAL TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"IMPELLER",null,null,null,null,null,"rdl:RDS414539",null,"An <IMPELLER> is an <ARTEFACT> and a <MECHANICAL TO MECHANICAL ENERGY CONVERTER> that is an assembly of rotating vanes within an enclosure which is used to impart energy to or derive energy from a fluid through dynamic force",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AUXILIARY IMPELLER",null,null,null,null,null,"rdl:RDS16765389",null,"An <AUXILIARY IMPELLER> is an <ARTEFACT> and a <IMPELLER> that is used to control the internal pressure and flow in the pump",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPRESSOR IMPELLER",null,null,null,null,null,"rdl:RDS397690521",null,"A <COMPRESSOR IMPELLER> is an <ARTEFACT> and a <IMPELLER> that is intended to be part of a compressor and used to impart energy to a gas through dynamic force in order to generate a required pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE IMPELLER",null,null,null,null,null,"rdl:RDS402677001",null,"A <DOUBLE IMPELLER> is an <ARTEFACT> and an <IMPELLER> that is a double-suction impeller that is a more balanced design than a single-suction impeller because the two sides of the impeller balance the axial thrust loads being placed on the impeller, shaft, and bearings",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXPANDER IMPELLER",null,null,null,null,null,"rdl:RDS814184",null,"An <EXPANDER IMPELLER> is an <ARTEFACT> and a <IMPELLER> that is intended to derive energy through dynamic force in order to generate power. Typically applied in expanders",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FAN IMPELLER",null,null,null,null,null,"rdl:RDS5772220",null,"A <FAN IMPELLER> is an <ARTEFACT> and a <IMPELLER> forming part of the rotating assembly of a fan imparting kinetic energy to the air or gas being transported",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IMPELLER BETWEEN BEARINGS",null,null,null,null,null,"rdl:RDS2227301",null,"An <IMPELLER BETWEEN BEARINGS> is an <IMPELLER> that is mounted on a shaft with the bearings at both ends",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIXER IMPELLER",null,null,null,null,null,"rdl:RDS815714",null,"A <MIXER IMPELLER> is an <ARTEFACT> and an <IMPELLER> that is intended for use to impart energy to a fluid through centrifugal and axial force in order to perform flow, head and shear required for a mixing process",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AXIAL FLOW MIXER IMPELLER",null,null,null,null,null,"rdl:RDS904814",null,"An <AXIAL FLOW MIXER IMPELLER> is a <MIXER IMPELLER> intended to produce flow parallel to the impeller shaft with relatively less shear and higher flow rates in mixing fluids.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AXIAL FLOW MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HELICAL MIXER IMPELLER",null,null,null,null,null,"rdl:RDS814859",null,"A <HELICAL MIXER IMPELLER> is an <AXIAL FLOW MIXER IMPELLER> that contains a specially curved spiral-shaped blade intended to mix high viscous liquids.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HELICAL MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE HELICAL MIXER IMPELLER",null,null,null,null,null,"rdl:RDS813824",null,"A <DOUBLE HELICAL MIXER IMPELLER> is a <HELICAL MIXER IMPELLER> that is provided with both a single spiral-shaped blade and an inner flight of similar blade shape.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HELICAL MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE HELICAL MIXER IMPELLER",null,null,null,null,null,"rdl:RDS816614",null,"A <SINGLE HELICAL MIXER IMPELLER> is a <HELICAL MIXER IMPELLER> that has a single spiral-shaped blade.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AXIAL FLOW MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MARINE TYPE IMPELLER",null,null,null,null,null,"rdl:RDS409526231",null,"A <MARINE TYPE IMPELLER> is an <AXIAL FLOW MIXER IMPELLER> that is provided with constant pitch, skewed-back blades as three(3) blade propeller in order to perform down-pumping actions to tank bottom in mixing liquids.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AXIAL FLOW MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PITCHED-BLADE MIXER IMPELLER",null,null,null,null,null,"rdl:RDS816119",null,"A <PITCHED-BLADE MIXER IMPELLER> is an <AXIAL FLOW MIXER IMPELLER> that contains axial flow blades. Typically with four blades positioned at constant angles of 45 degree.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AXIAL FLOW MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VARIABLE PITCH BLADE MIXER IMPELLER",null,null,null,null,null,"rdl:RDS817379",null,"A <VARIABLE PITCH BLADE MIXER IMPELLER> is an <AXIAL FLOW MIXER IMPELLER> that has a variable pitch, from hub to blade tip, but constant blade angle in order to produce a variable pitch-velocity discharge and variable shear rates across the impeller diameter.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE SPIRAL",null,null,null,null,null,"rdl:RDS813869",null,"A <DOUBLE SPIRAL> is a <MIXER IMPELLER> that contains a helical inner and a helical outer flight intended to mix highly viscous materials.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL FLOW MIXER IMPELLER",null,null,null,null,null,"rdl:RDS904769",null,"A <RADIAL FLOW MIXER IMPELLER> is a <MIXER IMPELLER> intended to produce flow along the impeller radius in distinct patterns with relatively more shear and smaller flow rates in mixing fluids.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RADIAL FLOW MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANCHOR TYPE IMPELLER",null,null,null,null,null,"rdl:RDS433079",null,"An <ANCHOR TYPE IMPELLER> is a <RADIAL FLOW MIXER IMPELLER> that is a contoured, two-bladed impeller for mixing of high viscosity liquids.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RADIAL FLOW MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BAR TURBINE IMPELLER",null,null,null,null,null,"rdl:RDS812474",null,"A <BAR TURBINE IMPELLER> is a <RADIAL FLOW MIXER IMPELLER> that is multi bladed and bolted or welded to top and bottom of support disk in order to produce high shear rate in mixing fluids.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RADIAL FLOW MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLAT BLADE IMPELLER",null,null,null,null,null,"rdl:RDS403614201",null,"A <FLAT BLADE IMPELLER> is a <RADIAL FLOW MIXER IMPELLER>that uses vertical blades connected to a support disc to produce fairly high shear or turbulence in mixing liquids.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RADIAL FLOW MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PADDLE TYPE IMPELLER",null,null,null,null,null,"rdl:RDS412278081",null,"A <PADDLE TYPE IMPELLER> is a <RADIAL FLOW MIXER IMPELLER> that is provided with two (2) large-radial paddles and typically applied in solid suspension and blending applications.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RADIAL FLOW MIXER IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPIRAL BACKSWEPT TURBINE IMPELLER",null,null,null,null,null,"rdl:RDS424635251",null,"A <SPIRAL BACKSWEPT TURBINE IMPELLER> is a <RADIAL FLOW MIXER IMPELLER> that is of the open type and provided with radially curved blades.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROPELLER",null,null,null,null,null,"rdl:RDS13067150",null,"A <PROPELLER> is an <ARTEFACT> and a <IMPELLER> that is an axial flow impeller which is typically unenclosed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PROPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MARINE SCREW PROPELLER",null,null,null,null,null,"rdl:RDS16195065",null,"A <MARINE SCREW PROPELLER> is a <PROPELLER> that is carrying 2, 3 or 4 blades of helical form, which produces the thrust to drive a ship by giving momentum to the column of water which it displaces in an astern direction.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PUMP IMPELLER",null,null,null,null,null,"rdl:RDS816299",null,"A <PUMP IMPELLER> is an <ARTEFACT> and a <IMPELLER> that forms part of a rotating assembly of a pump imparting kinetic energy to the liquid being pumped",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUMP IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AXIAL FLOW PUMP IMPELLER",null,null,null,null,null,"rdl:RDS461339",null,"An <AXIAL FLOW PUMP IMPELLER> is a <PUMP IMPELLER> where the flow direction is along the shaft axis and the flow is discharged nearly axially by which most of the head is developed by the propelling or lifting action of the vanes on the liquid.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AXIAL FLOW PUMP IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDUCER TYPE PUMP IMPELLER",null,null,null,null,null,"rdl:RDS903419",null,"An <INDUCER TYPE PUMP IMPELLER> is an <AXIAL FLOW PUMP IMPELLER> with one or a few screw type blades which are placed in front of a conventional impeller, on the same shaft, to reduce the <NPSH> requirement of the pump.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUMP IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CLOSED PUMP IMPELLER",null,null,null,null,null,"rdl:RDS1001519",null,"A <CLOSED PUMP IMPELLER> is a <PUMP IMPELLER> that is provided with vanes covered by shrouds or sidewalls both in the back and front.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUMP IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE SUCTION PUMP IMPELLER",null,null,null,null,null,"rdl:RDS432449",null,"A <DOUBLE SUCTION PUMP IMPELLER> is a <PUMP IMPELLER> where the liquid is intended to enter the two suction inlet eyes from both sides.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUMP IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDIVIDUALLY SECURED PUMP IMPELLER",null,null,null,null,null,"rdl:RDS7479017",null,"An <INDIVIDUALLY SECURED PUMP IMPELLER> is a <PUMP IMPELLER> of a multistage pump which is locked against axial movement, related to the shaft, in oposite direction to normal hydraulic thrust.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUMP IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIXED FLOW PUMP IMPELLER",null,null,null,null,null,"rdl:RDS432764",null,"A <MIXED FLOW PUMP IMPELLER> is a <PUMP IMPELLER> where the shape of the impeller includes for specific speed values in between of those for radial and axial flow type impellers, resulting in a combined axial and radial flow.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MIXED FLOW PUMP IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FRANCIS-VANE PUMP IMPELLER",null,null,null,null,null,"rdl:RDS1001429",null,"A <FRANCIS-VANE PUMP IMPELLER> is a <MIXED FLOW PUMP IMPELLER> with double curvature vanes extending over the full vane surface and resulting in a low specific speed.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUMP IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OPEN PUMP IMPELLER",null,null,null,null,null,"rdl:RDS432539",null,"An <OPEN PUMP IMPELLER> is a <PUMP IMPELLER> that consists of nothing but vanes, without impeller front and back cover, attached to a central hub for mounting on the shaft.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUMP IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL FLOW PUMP IMPELLER",null,null,null,null,null,"rdl:RDS461384",null,"A <RADIAL FLOW PUMP IMPELLER> is a <PUMP IMPELLER> where the flow direction is radial to the shaft axis and the values of specific speed are relatively low. It can have either a single or double suction and be of the open, closed or semi-open design.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUMP IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEMI-OPEN PUMP IMPELLER",null,null,null,null,null,"rdl:RDS1001474",null,"A <SEMI-OPEN PUMP IMPELLER> is a <PUMP IMPELLER> with vanes partly supported by a shroud on the back of the impeller.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUMP IMPELLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE SUCTION PUMP IMPELLER",null,null,null,null,null,"rdl:RDS432494",null,"A <SINGLE SUCTION PUMP IMPELLER> is a <PUMP IMPELLER> where the liquid enters the suction eye on one side only.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,"rdl:RDS279989",null,"A <PNEUMATIC TO MECHANICAL ENERGY CONVERTER> is an <ENERGY CONVERTER> that is capable of <PNEUMATIC TO MECHANICAL ENERGY CONVERTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","PISTON CYLINDER","PNEUMATIC TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC CYLINDER",null,null,null,null,null,"rdl:RDS5767025",null,"A <PNEUMATIC CYLINDER> is an <ARTEFACT> and a <PISTON CYLINDER> and a <PNEUMATIC TO MECHANICAL ENERGY CONVERTER> where the piston is actuated by compressed air"]
[null,null,"ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC TO ROTATION ENERGY CONVERTER",null,null,null,null,null,"rdl:RDS2220078",null,"A <PNEUMATIC TO ROTATION ENERGY CONVERTER> is an <ENERGY CONVERTER> that is capable of <PNEUMATIC TO ROTATION ENERGY CONVERTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"POTENTIAL TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,"rdl:RDS316169",null,"A <POTENTIAL TO MECHANICAL ENERGY CONVERTER> is an <ENERGY CONVERTER> that is capable of <POTENTIAL TO MECHANICAL ENERGY CONVERTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","BALANCER","POTENTIAL TO MECHANICAL ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"COUNTERWEIGHT",null,null,null,null,null,"rdl:RDS13310200",null,"A <COUNTERWEIGHT> is an <ARTEFACT> and a <BALANCER> and a <POTENTIAL TO MECHANICAL ENERGY CONVERTER> intended to compensate for unbalanced masses and subsequent dynamic forces",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COUNTERWEIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CRANKSHAFT COUNTERWEIGHT",null,null,null,null,null,"rdl:RDS13656820",null,"A <CRANKSHAFT COUNTERWEIGHT> is a <COUNTERWEIGHT> that is a weight connected opposite a crank",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ENERGY CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"TRANSDUCER",null,null,null,null,null,"rdl:RDS812024",null,"A <TRANSDUCER> is an <ENERGY CONVERTER> that is capable of converting a <PROCESS VARIABLE> in one form or magnitude of energy to another form or magnitude of energy",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,"DIAPHRAGM SEAL",null,null,null,null,null,"rdl:RDS298079",null,"A <DIAPHRAGM SEAL> is an <INSTRUMENTATION ITEM> and a <TRANSDUCER> that provides a <BARRIER> between two substance using an impenetrable membrane or <DIAPHRAGM>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTROACOUSTIC TRANSDUCER",null,null,null,null,null,"rdl:RDS17600859",null,"An <ELECTROACOUSTIC TRANSDUCER> is an <ARTEFACT> and a <TRANSDUCER> that is capable of producing an acoustic signal based on an electric signal or vice versa",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTROACOUSTIC TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LOUDSPEAKER",null,null,null,null,null,"rdl:RDS884699",null,"A <LOUDSPEAKER> is an <ELECTROACOUSTIC TRANSDUCER> that converts an electric signal into sound",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LOUDSPEAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PUBLIC ADDRESS LOUDSPEAKER",null,null,null,null,null,"rdl:RDS309464",null,"A <PUBLIC ADDRESS LOUDSPEAKER> is a <LOUDSPEAKER> that spreads messages to all people in the area where it is installed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTROACOUSTIC TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MICROWAVE TRANSDUCER",null,null,null,null,null,"rdl:RDS7921725",null,"A <MICROWAVE TRANSDUCER> is an <ELECTROACOUSTIC TRANSDUCER> that utilizes microwaves to accept information in the form of a physical or chemical variable (its input variable) and converts it into an output variable of the same or another nature",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTROCHEMICAL TRANSDUCER",null,null,null,null,null,"rdl:RDS17600972",null,"An <ELECTROCHEMICAL TRANSDUCER> is an <ARTEFACT> and a <TRANSDUCER> that is capable of producing an electric signal based on an electrochemical reaction or vice versa",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTROMAGNETIC TRANSDUCER",null,null,null,null,null,"rdl:RDS17601217",null,"An <ELECTROMAGNETIC TRANSDUCER> is an <ARTEFACT> and a <TRANSDUCER> that is capable of producing an electric signal based on an electromagnetic signal or vice versa",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTROMAGNETIC TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANTENNA",null,null,null,null,null,"rdl:RDS5788403",null,"An <ANTENNA> is an <ELECTROMAGNETIC TRANSDUCER> that is a physical object made of conducting material which is capable of radiating or receiving electromagnetic waves",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANTENNA EX RATED",null,null,null,null,null,"rdl:RDS1066711971",null,"An <ANTENNA EX RATED> is an <ANTENNA> that is EX rated",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CYLINDRICAL ANTENNA",null,null,null,null,null,"rdl:RDS5787749",null,"A <CYLINDRICAL ANTENNA> is an <ANTENNA> having a cylindrical shape",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIELECTRIC ROD ANTENNA",null,null,null,null,null,"rdl:RDS1455509861",null,"A <DIELECTRIC ROD ANTENNA> is an <ANTENNA> that is an end-fire antenna which employs a shaped dielectric as a significant part of a radiating element",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIPOLE ANTENNA",null,null,null,null,null,"rdl:RDS5787704",null,"A <DIPOLE ANTENNA> is an <ANTENNA> most commonly made up by two equal halves, but may be of folded type",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FERRITE ROD ANTENNA",null,null,null,null,null,"rdl:RDS1455509411",null,"A <FERRITE ROD ANTENNA> is an <ANTENNA> with several turns of wire around a magnetic ferrite rod and acting as a loop antenna",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GRID ANTENNA",null,null,null,null,null,"rdl:RDS5787659",null,"A <GRID ANTENNA> is an <ANTENNA> having the shape of a grid of parallel bars",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GYRO STABILISED ANTENNA",null,null,null,null,null,"rdl:RDS5836423",null,"A <GYRO STABILISED ANTENNA> is an <ANTENNA> that is a reflector antenna for floating structures, normally used for satellite based applications",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HF ANTENNA",null,null,null,null,null,"rdl:RDS5788223",null,"An <HF ANTENNA> is an <ANTENNA> that is designed for radiating or receiving electromagnetic waves in the high frequency range (HF = 3 - 30 MHz)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LOG PERIODIC ANTENNA",null,null,null,null,null,"rdl:RDS5836135",null,"A <LOG PERIODIC ANTENNA> is an <ANTENNA> that is a wideband antenna used in the HF, VHF and UHF bands, made up of a number of dipoles mounted along a straight line",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MF ANTENNA",null,null,null,null,null,"rdl:RDS5788268",null,"An <MF ANTENNA> is an <ANTENNA> that is capable of radiating or receiving electromagnetic waves in the medium frequency area (MF = 0,3 - 3 MHz)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OFFSET REFLECTOR ANTENNA",null,null,null,null,null,"rdl:RDS5836344",null,"An <OFFSET REFLECTOR ANTENNA> is an <ANTENNA> where the application and construction is similar to the parabolic reflector antenna, but the reflector is shaped so that the focal point has an offset location when compared to the parabolic type",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PANEL ANTENNA",null,null,null,null,null,"rdl:RDS5836248",null,"A <PANEL ANTENNA> is an <ANTENNA> where the array of dipoles normally are made for the UHF or VHF band",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PARABOLIC REFLECTOR ANTENNA",null,null,null,null,null,"rdl:RDS5787794",null,"A <PARABOLIC REFLECTOR ANTENNA> is an <ANTENNA> that is made up by a reflector with the shape of a rotational paraboloid, and a feedhorn located in the focal point of the reflector",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROD ANTENNA",null,null,null,null,null,"rdl:RDS1459069290",null,"A <ROD ANTENNA> is an <ANTENNA> where the antenna structure made from copper wire ending in isolators",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UHF ANTENNA",null,null,null,null,null,"rdl:RDS5788313",null,"A <UHF ANTENNA> is an <ANTENNA> that is capable of radiating or receiving electromagnetic waves in the ultra high frequency area (UHF = 300 - 3000 MHz)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VHF ANTENNA",null,null,null,null,null,"rdl:RDS5788358",null,"A <VHF ANTENNA> is an <ANTENNA> that is capable of radiating or receiving electromagnetic waves in the very high frequency area (VHF = 30 - 300 MHz)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WHIP ANTENNA",null,null,null,null,null,"rdl:RDS5835796",null,"A <WHIP ANTENNA> is an <ANTENNA> that is a single-element antenna that can be used with an electrically unbalanced feed line with respect to ground",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WIRE ANTENNA",null,null,null,null,null,"rdl:RDS5835926",null,"A <WIRE ANTENNA> is an <ANTENNA> where the antenna structure made from copper wire ending in isolators",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANTENNA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"YAGI ANTENNA",null,null,null,null,null,"rdl:RDS5836022",null,"A <YAGI ANTENNA> is an <ANTENNA> that is normally made up by one dipole, as a reflector element and several directors, all mounted on a boom",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTROMAGNETIC TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ULTRASONIC TRANSDUCER",null,null,null,null,null,"rdl:RDS7921663",null,"An <ULTRASONIC TRANSDUCER> is an <ELECTROMAGNETIC TRANSDUCER> that is capable of producing ultrasonic pulses based on electric signals or vice versa",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTROMECHANICAL TRANSDUCER",null,null,null,null,null,"rdl:RDS17601085",null,"An <ELECTROMECHANICAL TRANSDUCER> is an <ARTEFACT> and a <TRANSDUCER> that is designed to receive an electric input signal and to furnish a mechanical output signal, or vice versa",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-WETTED TRANSDUCER",null,null,null,null,null,"rdl:RDS7502222",null,"A <NON-WETTED TRANSDUCER> is an <ARTEFACT> and a <TRANSDUCER> that is designed not to be in contact with the process medium",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,"PHOTOELECTRIC TRANSDUCER",null,null,null,null,null,"rdl:RDS5770366",null,"A <PHOTOELECTRIC TRANSDUCER> is an <ARTEFACT> and a <TRANSDUCER> whose electric characteristics vary when light is incident upon it",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PHOTOELECTRIC TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PHOTOCELL",null,null,null,null,null,"rdl:RDS1322468351",null,"A <PHOTOCELL> is a <PHOTOELECTRIC TRANSDUCER> that generates an electric current or voltage dependent on its degree of illumination",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PHOTOCELL","PHOTOVOLTAIC DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PHOTOVOLTAIC CELL",null,null,null,null,null,"rdl:RDS1294898741",null,"A <PHOTOVOLTAIC CELL> is a <PHOTOCELL> and a <PHOTOVOLTAIC DEVICE> that is the smallest voltage generating part from which other photovoltaic devices are assembled",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PHOTOVOLTAIC CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLAR CELL",null,null,null,null,null,"rdl:RDS1294949591",null,"A <SOLAR CELL> is a <PHOTOVOLTAIC CELL> that converts solar radiation into electrical energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PHOTOELECTRIC TRANSDUCER","SEMICONDUCTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PHOTODIODE",null,null,null,null,null,"rdl:RDS6646330",null,"A <PHOTODIODE> is a <PHOTOELECTRIC TRANSDUCER> and a <SEMICONDUCTOR> that is a diode that exhibits sensitivity to light, either by varying its electrical resistance like a photoresistor, or generating a electric potential in the manner of a photoelectric cell",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMOELECTRIC TRANSDUCER",null,null,null,null,null,"rdl:RDS17602596",null,"A <THERMOELECTRIC TRANSDUCER> is an <ARTEFACT> and a <TRANSDUCER> that by sensing variations in heat differentials is capable of producing a quantitative electric signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,"WETTED TRANSDUCER",null,null,null,null,null,"rdl:RDS7502160",null,"A <WETTED TRANSDUCER> is an <ARTEFACT> and a <TRANSDUCER> that is designed to be in contact with the process medium",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS460394",null,"A <SIGNAL CONVERTER> is a <CONVERTER> that has the capability of <CONVERTING> a <SIGNAL>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"ANALOGUE TO DIGITAL SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS851354",null,"An <ANALOGUE TO DIGITALL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert an analogue input signal into a digital output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT TO CURRENT SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS5762894",null,"A <CURRENT TO CURRENTL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a current input signal to a current output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT TO PRESSURE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS460484",null,"A <CURRENT TO PRESSUREL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a current input signal to a proportional linear pneumatic output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT TO VOLTAGE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS851219",null,"A <CURRENT TO VOLTAGEL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a current input signal to a proportional voltage output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"DIGITAL TO ANALOGUE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS851399",null,"A <DIGITAL TO ANALOGUEL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a digital input signal into an analogue output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL TO OPTICAL SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS1066703201",null,"An <ELECTRICAL TO OPTICALL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that converts an electrical input signal to an optical output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"FREQUENCY TO CURRENT SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS1011104",null,"A <FREQUENCY TO CURRENTL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a frequency or rotational speed input signal into a current output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"FREQUENCY TO VOLTAGE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS1011149",null,"A <FREQUENCY TO VOLTAGEL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a frequency or rotational speed input signal into a voltage output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"OPTICAL TO ELECTRICAL SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS1066704961",null,"An <OPTICAL TO ELECTRICALL SIGNAL CONVERTER > is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that converts an optical input signal to an electrical output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE TO CURRENT SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS460439",null,"A <PRESSURE TO CURRENTL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a pressure input signal to a current output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE TO VOLTAGE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS851264",null,"A <PRESSURE TO VOLTAGEL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a pressure input signal into a voltage output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"RESISTANCE TO CURRENT SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS5763018",null,"A <RESISTANCE TO CURRENTL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a measured resistance as input into a current output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE TO CURRENT SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS851174",null,"A <VOLTAGE TO CURRENTL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended for converting an input voltage signal into a current output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE TO PRESSURE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS851309",null,"A <VOLTAGE TO PRESSUREL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended for converting a voltage input signal into proportional linear pneumatic output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE TO VOLTAGE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS5762939",null,"A <VOLTAGE TO VOLTAGEL SIGNALCONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended for converting a voltage input signal to a voltage output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]