{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["RDL browser","Settings","about","Results1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"RDL browser","index":0,"n_rows":113,"n_cols":10,"rows_kept":113,"cut":false,"hidden":false,"merged":[[0,0,0,4]]}
["RDL2 browser to spreadsheet tool version 71",null,null,null,null,null,"Endpoint: http://data.15926.org/rdl/"]
["Contact: onno.paap@gmail.com",null,null,null,null,null,null,"Active count","Deprecated","Total count"]
[null,null,null,null,null,"Show","dm:ArrangedIndividual",0,3,3]
["Search:",null,null,null,null,"Show","dm:AssemblyOfIndividual",0,1,1]
[null,null,null,null,null,"Show","dm:BoundaryOfPropertySpace",0,1,1]
[null,null,null,null,null,"Show","dm:Cardinality",7,2,9]
[null,null,null,null,null,"Show","dm:Class",0,52,52]
[null,null,null,null,null,"Show","dm:ClassOfAbstractObject",351,12,363]
[null,null,null,null,null,"Show","dm:ClassOfActivity",2057,196,2253]
[null,null,null,null,null,"Show","dm:ClassOfArrangedIndividual",0,12,12]
[null,null,null,null,null,"Show","dm:ClassOfArrangementOfIndividual",0,2,2]
[null,null,null,null,null,"Show","dm:ClassOfAssertion",22,0,22]
[null,"Note: first set coloring on in Settings",null,null,null,"Show","dm:ClassOfAtom",201,8,209]
[null,"Coloring (containing this string will give this color)",null,null,null,"Show","dm:ClassOfBiologicalMatter",16,4,20]
[null,"ClassOfFunctionalObject",null,null,null,"Show","dm:ClassOfClass",59,113,172]
[null,"ClassOfInanimatePhysicalObject ",null,null,null,"Show","dm:ClassOfClassOfComposition",0,2,2]
[null,null,null,null,null,"Show","dm:ClassOfClassOfDefinition",3,6,9]
[null,null,null,null,null,"Show","dm:ClassOfClassOfDescription",6,49,55]
[null,null,null,null,null,"Show","dm:ClassOfClassOfIdentification",39,2,41]
[null,null,null,null,null,"Show","dm:ClassOfClassOfIndividual",582,729,1311]
[null,null,null,null,null,"Show","dm:ClassOfClassOfIndiviual",1,0,1]
[null,null,null,null,null,"Show","dm:ClassOfClassOfInformationRepresentation",35,6,41]
[null,null,null,null,null,"Show","dm:ClassOfClassOfRelationship",0,6,6]
[null,null,null,null,null,"Show","dm:ClassOfClassOfRelationshipWithSignature",0,7,7]
[null,"Namespace replacer (definition containing this string replaces the namespace)",null,null,null,"Show","dm:ClassOfClassOfRepresentation",0,2,2]
[null,"API","API:",null,null,"Show","dm:ClassOfClassification",0,2,2]
[null,"ASME","ASME:",null,null,"Show","dm:ClassOfCompositeMaterial",12,2,14]
[null,"ASTM","ASTM:",null,null,"Show","dm:ClassOfCompositionOfIndividual",0,7,7]
[null,"DIN","DIN:",null,null,"Show","dm:ClassOfCompound",454,190,644]
[null,"EN","EN:",null,null,"Show","dm:ClassOfConnectionOfIndividual",0,1,1]
[null,"ISO","ISO:",null,null,"Show","dm:ClassOfContainmentOfIndividual",0,3,3]
[null,"NORSOK","NOR:",null,null,"Show","dm:ClassOfDefinition",0,2,2]
[null,"NPD","NOR:",null,null,"Show","dm:ClassOfDimensionForShape",0,2,2]
[null,"NS","NOR:",null,null,"Show","dm:ClassOfDirectConnection",21,1,22]
[null,"ROSEMOUNT","ROS:",null,null,"Show","dm:ClassOfEvent",109,13,122]
[null,"SAE","SAE:",null,null,"Show","dm:ClassOfExpressInformationRepresentation",0,4,4]
[null,"SIEMENS","SIE:",null,null,"Show","dm:ClassOfFeature",338,399,737]
[null,"SKOTSELV","SKOT:",null,null,"Show","dm:ClassOfFeatureWholePart",0,2,2]
[null,"TWR","TWR:",null,null,"Show","dm:ClassOfFunctionalMapping",2,158,160]
[null,null,null,null,null,"Show","dm:ClassOfFunctionalObject",1157,70,1227]
[null,null,null,null,null,"Show","dm:ClassOfIdentification",0,5,5]
[null,null,null,null,null,"Show","dm:ClassOfInanimatePhysicalObject",7951,11603,19554]
[null,null,null,null,null,"Show","dm:ClassOfIndirectConnection",4,1,5]
[null,null,null,null,null,"Show","dm:ClassOfIndirectProperty",800,1191,1991]
[null,null,null,null,null,"Show","dm:ClassOfIndividual",50,16,66]
[null,null,null,null,null,"Show","dm:ClassOfInformationObject",332,91,423]
[null,null,null,null,null,"Show","dm:ClassOfInformationPresentation",13,2,15]
[null,null,null,null,null,"Show","dm:ClassOfInformationRepresentation",0,513,513]
[null,null,null,null,null,"Show","dm:ClassOfInvolvementByReference",2,0,2]
[null,null,null,null,null,"Show","dm:ClassOfIsomorphicFunctionalMapping",0,1,1]
[null,null,null,null,null,"Show","dm:ClassOfLifecycleStage",7,1,8]
[null,null,null,null,null,"Show","dm:ClassOfMolecule",1543,6,1549]
[null,null,null,null,null,"Show","dm:ClassOfMultidimensionalObject",0,449,449]
[null,null,null,null,null,"Show","dm:ClassOfNumber",2,4,6]
[null,null,null,null,null,"Show","dm:ClassOfOrganism",1,2,3]
[null,null,null,null,null,"Show","dm:ClassOfOrganization",35,9,44]
[null,null,null,null,null,"Show","dm:ClassOfParticipation",0,1,1]
[null,null,null,null,null,"Show","dm:ClassOfParticulateMaterial",8,2,10]
[null,null,null,null,null,"Show","dm:ClassOfParticulateObject",1,0,1]
[null,null,null,null,null,"Show","dm:ClassOfPeriodInTime",16,4,20]
[null,null,null,null,null,"Show","dm:ClassOfPerson",207,3,210]
[null,null,null,null,null,"Show","dm:ClassOfPhysicalObject",2,0,2]
[null,null,null,null,null,"Show","dm:ClassOfPointInTime",3,9,12]
[null,null,null,null,null,"Show","dm:ClassOfProperty",0,1,1]
[null,null,null,null,null,"Show","dm:ClassOfPropertySpace",0,2,2]
[null,null,null,null,null,"Show","dm:ClassOfRecognition",0,1,1]
[null,null,null,null,null,"Show","dm:ClassOfRelationship",0,23,23]
[null,null,null,null,null,"Show","dm:ClassOfRelationshipWithSignature",4,24,28]
[null,null,null,null,null,"Show","dm:ClassOfRelativeLocation",19,15,34]
[null,null,null,null,null,"Show","dm:ClassOfRepresented",1,0,1]
[null,null,null,null,null,"Show","dm:ClassOfScale",69,3,72]
[null,null,null,null,null,"Show","dm:ClassOfShape",25,2,27]
[null,null,null,null,null,"Show","dm:ClassOfShapeDimension",285,731,1016]
[null,null,null,null,null,"Show","dm:ClassOfSpatialLocation",2,0,2]
[null,null,null,null,null,"Show","dm:ClassOfSpecialization",0,4,4]
[null,null,null,null,null,"Show","dm:ClassOfStatus",14,3,17]
[null,null,null,null,null,"Show","dm:ClassOfSubAtomicParticle",12,2,14]
[null,null,null,null,null,"Show","dm:CoordinateSystem",3,0,3]
[null,null,null,null,null,"Show","dm:CrystallineStructure",6,0,6]
[null,null,null,null,null,"Show","dm:DescriptionSpace",0,1,1]
[null,null,null,null,null,"Show","dm:DimensionOfShape",0,2,2]
[null,null,null,null,null,"Show","dm:DocumentDefinition",682,1929,2611]
[null,null,null,null,null,"Show","dm:EnumeratedSetOfClass",0,11,11]
[null,null,null,null,null,"Show","dm:ExpressReal",1,1,2]
[null,null,null,null,null,"Show","dm:FunctionalPhysicalObject",0,6,6]
[null,null,null,null,null,"Show","dm:IntegerNumber",0,2,2]
[null,null,null,null,null,"Show","dm:Language",32,1,33]
[null,null,null,null,null,"Show","dm:MultidimensionalProperty",2,0,2]
[null,null,null,null,null,"Show","dm:MultidimensionalPropertySpace",1,0,1]
[null,null,null,null,null,"Show","dm:NumberRange",10,2,12]
[null,null,null,null,null,"Show","dm:NumberSpace",0,2,2]
[null,null,null,null,null,"Show","dm:OtherRelationship",0,171,171]
[null,null,null,null,null,"Show","dm:ParticipatingRoleAndDomain",0,35,35]
[null,null,null,null,null,"Show","dm:Phase",6,1,7]
[null,null,null,null,null,"Show","dm:PhysicalObject",0,4,4]
[null,null,null,null,null,"Show","dm:PhysicalQuantityKind",0,1,1]
[null,null,null,null,null,"Show","dm:PossibleIndividual",0,2,2]
[null,null,null,null,null,"Show","dm:Property",8,609,617]
[null,null,null,null,null,"Show","dm:PropertyForShapeDimension",0,1,1]
[null,null,null,null,null,"Show","dm:PropertyQuantification",0,8,8]
[null,null,null,null,null,"Show","dm:PropertyRange",21,534,555]
[null,null,null,null,null,"Show","dm:PropertySpace",1,10,11]
[null,null,null,null,null,"Show","dm:PropertySpaceForClassOfShapeDimension",0,2,2]
[null,null,null,null,null,"Show","dm:RealNumber",0,472,472]
[null,null,null,null,null,"Show","dm:RepresentationForm",31,252,283]
[null,null,null,null,null,"Show","dm:Role",92,435,527]
[null,null,null,null,null,"Show","dm:RoleAndDomain",0,2,2]
[null,null,null,null,null,"Show","dm:Scale",1366,3,1369]
[null,null,null,null,null,"Show","dm:Shape",0,2,2]
[null,null,null,null,null,"Show","dm:ShapeDimension",0,1,1]
[null,null,null,null,null,"Show","dm:SinglePropertyDimension",1012,2876,3888]
[null,null,null,null,null,"Show","dm:Status",68,75,143]
[null,null,null,null,null,"Show","dm:hasClassOfPossessor",0,35,35]

{"sheet":"Settings","index":1,"n_rows":87,"n_cols":8,"rows_kept":87,"cut":false,"hidden":true,"merged":[]}
["Setting name","Select name","OnKey","Value","Status","RDLType"]
["Endpoint","RDL2 (15926.org)",null,"http://data.15926.org/rdl/","Current",null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA RDL",null,"http://data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA Staging",null,"http://staging.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA SVRDL",null,"http://svrdl.community.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P4",null,"http://posccaesar.org/p4/sparql",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P12",null,"http://sti.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","Localhost",null,"http://localhost:8890/sparql/",null,null,null,"Note: end address always with a slash (/)"]
[]
["gBaseNamespace",null,"http://data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://staging.data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://svrdl.community.data.posccaesar.org/rdl/","http://svrdl.community.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://posccaesar.org/p4/sparql","http://posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://sti.data.posccaesar.org/rdl/","http://sti.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://localhost:8890/sparql/","http://data.15926.org/rdl/",null,"RDL2"]
["gKeepSettings",null,null,"T"]
["gShowDeprecated",null,null,"F"]
["gColoring",null,null,"F"]
["gNamespaceReplacing",null,null,"F"]
["gHyperlinkReplacing",null,null,"F"]
[]
["Endpoint","aisi",null,"http://data.15926.org/aisi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ansi",null,"http://data.15926.org/ansi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","api",null,"http://data.15926.org/api/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","all",null,"http://data.15926.org/all/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","asme",null,"http://data.15926.org/asme/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","astm",null,"http://data.15926.org/astm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","atex",null,"http://data.15926.org/atex/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","bs",null,"http://data.15926.org/bs/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","din",null,"http://data.15926.org/din/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dm",null,"http://data.15926.org/dm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dnv",null,"http://data.15926.org/dnv/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","edm",null,"http://data.15926.org/edm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","en",null,"http://data.15926.org/en/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","eu",null,"http://data.15926.org/eu/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iec",null,"http://data.15926.org/iec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ieee",null,"http://data.15926.org/ieee/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iso",null,"http://data.15926.org/iso/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","lci",null,"http://data.15926.org/lci/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","mss",null,"http://data.15926.org/mss/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nace",null,"http://data.15926.org/nace/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nec",null,"http://data.15926.org/nec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nema",null,"http://data.15926.org/nema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nfpa",null,"http://data.15926.org/nfpa/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nor",null,"http://data.15926.org/nor/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","rdl",null,"http://data.15926.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sae",null,"http://data.15926.org/sae/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sie",null,"http://data.15926.org/sie/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","tema",null,"http://data.15926.org/tema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","twr",null,"http://data.15926.org/twr/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","uns",null,"http://data.15926.org/uns/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","wits",null,"http://data.15926.org/wits/",null,null,null,"Note: end address always with a slash (/)"]
[]
[]
["gBaseNamespace",null,"http://data.15926.org/aisi/","http://data.15926.org/aisi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ansi/","http://data.15926.org/ansi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/api/","http://data.15926.org/api/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/asme/","http://data.15926.org/asme/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/all/","http://data.15926.org/all/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/astm/","http://data.15926.org/astm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/atex/","http://data.15926.org/atex/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/bs/","http://data.15926.org/bs/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/din/","http://data.15926.org/din/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dm/","http://data.15926.org/dm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dnv/","http://data.15926.org/dnv/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/edm/","http://data.15926.org/edm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/en/","http://data.15926.org/en/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/eu/","http://data.15926.org/eu/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iec/","http://data.15926.org/iec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ieee/","http://data.15926.org/ieee/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iso/","http://data.15926.org/iso/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/lci/","http://data.15926.org/lci/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/mss/","http://data.15926.org/mss/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nace/","http://data.15926.org/nace/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nec/","http://data.15926.org/nec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nema/","http://data.15926.org/nema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nfpa/","http://data.15926.org/nfpa/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nor/","http://data.15926.org/nor/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sae/","http://data.15926.org/sae/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sie/","http://data.15926.org/sie/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/tema/","http://data.15926.org/tema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/twr/","http://data.15926.org/twr/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/uns/","http://data.15926.org/uns/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/wits/","http://data.15926.org/wits/",null,"RDL2"]
["                                          "]

{"sheet":"about","index":2,"n_rows":165,"n_cols":3,"rows_kept":165,"cut":false,"hidden":false,"merged":[]}
["Version 71 changes","2016-07-17","Onno Paap"]
["Aded report button for comparison of RDL2 with a subfolder called views filled with spreadsheets."]
[]
[]
["Version 69 changes","2016-06-16","Onno Paap"]
["Added button: \"errors in definitions\" that lists all classes that have more or less \"<\" brackets than the number of super class relationships + 1. Where the part after the word \"that \"  is ignored in the count of \"<\" brackets."]
[]
["Version 68 changes","2016-06-13","Onno Paap"]
["Updated endpoint of RDL2 sparql "]
[]
["Version 67 changes","2016-05-22","Onno Paap"]
["Added button list subclasses from superclass "]
[]
["Version 65 changes","2016-04-25","Onno Paap"]
["Added checkbox at action dialog \"supress double child occurances\" so that this built-in feature can be switched off"]
[]
["Version 64 changes","2016-04-20","Onno Paap"]
["Made search case-insensitive and added endpoint \"all\""]
[]
["Version 63 changes","2016-09-28","Onno Paap"]
["Made entity list working on P4 endpoint (they changed the database version which was not accepting som sparql setting)"]
["Version 62 changes","2016-09-28","Onno Paap"]
["Applied show deprecated to searched result list"]
[]
["Version 61 changes","2016-08-29","Onno Paap"]
["Added query from pcardl for ClassOfIndirectProperty"]
[]
["Version 60 changes","2016-08-19","Onno Paap"]
["Repaired failing entity reports"]
[]
["Version 59 changes","2016-08-19","Onno Paap"]
["Missing superclasses now queries whole federation of RDL2"]
[]
["Version 58 changes","2016-08-16","Onno Paap"]
["Repaired missing output for entities and doubles in RDL2 endpoints other than rdl"]
[]
["Version 57 changes","2016-08-13","Onno Paap"]
["Doubles report now skips classes that are deprecated"]
[]
["Version 56 changes","2016-07-22","Onno Paap"]
["Made rowheight suitable for longer definitions to example DESIGN BASIS"]
[]
["Version 55 changes","2016-07-19","Onno Paap"]
["Made rowheight suitable for longer definitions"]
[]
["Version 54 changes","2016-07-03","Onno Paap"]
["Entity Type field changed to 6 merged cells."]
[]
["Version 53 changes","2016-06-23","Onno Paap"]
["added lci namespace"]
[]
["Version 52 changes","2016-06-23","Onno Paap"]
["Added deprecated count to list entities"]
[]
["Version 51 changes","2016-06-19","Onno Paap"]
["Updated namespaces of staging RDL"]
[]
["Version 50 changes","2016-06-19","Onno Paap"]
["taxonomy view repaired missing entity type"]
[]
["Version 49 changes","2016-06-14","Onno Paap"]
["Room for 12 superclasses"]
[]
["Version 48 changes","2016-06-14","Onno Paap"]
["Repaired NOR:/RDS  bug"]
[]
["Version 47 changes","2016-06-14","Onno Paap"]
["Repaired endpoint bug"]
[]
["Version 46 changes","2016-06-13","Onno Paap"]
["Updated endpoints"]
[]
["Version 45 changes","2016-06-06","Onno Paap"]
["Completed Missing Superclasses report"]
[]
["Version 44 changes","2016-05-20","Onno Paap"]
["Added Clear Cache button (use on any database changes)"]
[]
["Version 43 changes","2016-05-19","Onno Paap"]
["Changed non-existing super classes to show as \"no label\""]
[]
["Version 42 changes","2016-05-02","Onno Paap"]
["bug fix"]
[]
["Version 41 changes","2016-05-02","Onno Paap"]
["Added setting to show/not show deprecated items. If shown, they are stricken through"]
[]
["Version 40 changes","2016-03-31","Onno Paap"]
["Added  in doubles: two classes having the same label."]
[]
["Version 39 changes","2016-03-21","Onno Paap"]
["Made the query more robust, after the server hass been returning a 404 occasionally"]
[]
["Version 38 changes","2016-03-03","Onno Paap"]
["Repaired bug entity type query on PCA endpoint"]
[]
["Version 37 changes","2016-01-29","Onno Paap"]
["Showing deprecated class in taxonomy with label in strikethrough."]
[]
["Version 36 changes","2016-01-13","Onno Paap"]
["Added the 17 endpoints of http://data.15926.org/rdl"]
[]
["Version 35 changes","2016-01-13","Onno Paap"]
["In taxonomy view, disregard all rdf:type that is not data model.  So only show rdf:type that is dm:"]
[]
["Version 34 changes","2016-01-13","Onno Paap"]
["Solved taxonomy levels regression bug"]
[]
["Version 33 changes","2016-01-11","Onno Paap"]
["Enhanced the doubled query. First 4 columns are about the triple, the rest is info."]
[]
["Repaired bug in entity type query."]
[]
["Version 30 changes","2016-01-03","Onno Paap"]
["Repaired entity type query for old PCA RDL. \nRepaired bug in entity type query where a class that has a superclass of the wanted type as well as  of another type became  the start point of a new taxonomy as well as part in the main taxonomy. (read that again)"]
[]
["Version 29 changes","2016-01-02","Onno Paap"]
["Filtered entity filtered taxonomy to only show the filtered entity not subClassOf of another entity"]
[]
["Version 27 changes","2016-01-01","Onno Paap"]
["few bugs repaired.  Changed entity search into presenting taxonomies. "]
[]
["Version 26 changes","2015-12-26","Onno Paap"]
["few bugs repaired. "]
[]
["Version 25 changes","2015-12-26","Onno Paap"]
["Added Part 12 and localhost endpoints"]
["Added button for selecting double labels and definitions. "]
["Version 24 changes","2015-12-14","Onno Paap"]
["Added button to list all distinct entity data types and their counts, and click to show."]
["Added a button to show all orphans that have a rdfs:label"]
["Version 23 changes"]
["Added endpoint posccaesar.org/p4/sparql"]
["Version 22 changes"]
["Added endpoint staging.data.posccaesar.org/rdl"]
[]
["Version 21 changes"]
["Repaired bug where namespace replace was based upon definition instead of class label"]
[]
["Version 20 changes"]
["Repaired bug where definition did not show up if hyperlink replace was on."]
[]
["Version 19 changes (skip version 16-18)"]
["Settings expanded with persist settings, namespace replacer and hyperlink replacer"]
["Added namespace replacer which will replace the RDL: namespace of the ID with the namespace given in the list on the front page."]
["Added hyperlink replacer which will find terms between single quotes and look them up in the RDL, then add a hyperlink in the text if found. Anchor tag <a></a> used not &hyperlink() so looks ugly."]
[]
["Version 15 changes"]
["Changed browser page Action buttons to hyperlinks because buttons are not equally spaced between Excel versions (Office 2007 versus Office 365)"]
["First row is empty. Move all up."]
["Make stop button for during query taxonomy query execution"]
[]
[]
["Version 14 changes"]
["Aligned buttons on browser page"]
["Made color notification work. Note: switch it on first in settings. Default is off"]
["Top align subclasses in taxonomy"]
["Subclasses made to hyperlink in taxonomy"]
["Subclasses made to increase column width in taxonomy"]
["Made browser search go when hitting enter in search field"]
[]
[]
[]
["todo"]
["Make setting for outputting to other result pages"]

{"sheet":"Results1","index":3,"n_rows":800,"n_cols":31,"rows_kept":800,"cut":false,"hidden":false,"merged":[[0,20,0,21],[0,14,0,19],[0,22,0,27],[0,28,0,31],[1,20,1,21],[1,14,1,19],[1,22,1,27],[1,28,1,31],[6,20,6,21],[6,14,6,19],[6,22,6,27],[6,28,6,31],[7,20,7,21],[7,14,7,19],[7,22,7,27],[7,28,7,31],[4,20,4,21],[4,14,4,19],[4,22,4,27],[4,28,4,31],[5,20,5,21],[5,14,5,19],[5,22,5,27],[5,28,5,31],[2,20,2,21],[2,14,2,19],[2,22,2,27],[2,28,2,31],[3,20,3,21],[3,14,3,19],[3,22,3,27],[3,28,3,31],[12,20,12,21],[12,14,12,19],[12,22,12,27],[12,28,12,31],[13,20,13,21],[13,14,13,19],[13,22,13,27],[13,28,13,31],[10,20,10,21],[10,14,10,19],[10,22,10,27],[10,28,10,31],[11,20,11,21],[11,14,11,19],[11,22,11,27],[11,28,11,31],[8,20,8,21],[8,14,8,19],[8,22,8,27],[8,28,8,31],[9,20,9,21],[9,14,9,19],[9,22,9,27],[9,28,9,31],[18,20,18,21],[18,14,18,19],[18,22,18,27],[18,28,18,31],[19,20,19,21],[19,14,19,19],[19,22,19,27],[19,28,19,31],[16,20,16,21],[16,14,16,19],[16,22,16,27],[16,28,16,31],[17,20,17,21],[17,14,17,19],[17,22,17,27],[17,28,17,31],[14,20,14,21],[14,14,14,19],[14,22,14,27],[14,28,14,31],[15,20,15,21],[15,14,15,19],[15,22,15,27],[15,28,15,31],[24,20,24,21],[24,14,24,19],[24,22,24,27],[24,28,24,31],[25,20,25,21],[25,14,25,19],[25,22,25,27],[25,28,25,31],[22,20,22,21],[22,14,22,19],[22,22,22,27],[22,28,22,31],[23,20,23,21],[23,14,23,19],[23,22,23,27],[23,28,23,31],[20,20,20,21],[20,14,20,19],[20,22,20,27],[20,28,20,31],[21,20,21,21],[21,14,21,19],[21,22,21,27],[21,28,21,31],[30,20,30,21],[30,14,30,19],[30,22,30,27],[30,28,30,31],[31,20,31,21],[31,14,31,19],[31,22,31,27],[31,28,31,31],[28,20,28,21],[28,14,28,19],[28,22,28,27],[28,28,28,31],[29,20,29,21],[29,14,29,19],[29,22,29,27],[29,28,29,31],[26,20,26,21],[26,14,26,19],[26,22,26,27],[26,28,26,31],[27,20,27,21],[27,14,27,19],[27,22,27,27],[27,28,27,31],[36,20,36,21],[36,14,36,19],[36,22,36,27],[36,28,36,31],[37,20,37,21],[37,14,37,19],[37,22,37,27],[37,28,37,31],[34,20,34,21],[34,14,34,19],[34,22,34,27],[34,28,34,31],[35,20,35,21],[35,14,35,19],[35,22,35,27],[35,28,35,31],[32,20,32,21],[32,14,32,19],[32,22,32,27],[32,28,32,31],[33,20,33,21],[33,14,33,19],[33,22,33,27],[33,28,33,31],[42,20,42,21],[42,14,42,19],[42,22,42,27],[42,28,42,31],[43,20,43,21],[43,14,43,19],[43,22,43,27],[43,28,43,31],[40,20,40,21],[40,14,40,19],[40,22,40,27],[40,28,40,31],[41,20,41,21],[41,14,41,19],[41,22,41,27],[41,28,41,31],[38,20,38,21],[38,14,38,19],[38,22,38,27],[38,28,38,31],[39,20,39,21],[39,14,39,19],[39,22,39,27],[39,28,39,31],[48,20,48,21],[48,14,48,19],[48,22,48,27],[48,28,48,31],[49,20,49,21],[49,14,49,19],[49,22,49,27],[49,28,49,31],[46,20,46,21],[46,14,46,19],[46,22,46,27],[46,28,46,31],[47,20,47,21],[47,14,47,19],[47,22,47,27],[47,28,47,31],[44,20,44,21],[44,14,44,19],[44,22,44,27],[44,28,44,31],[45,20,45,21],[45,14,45,19],[45,22,45,27],[45,28,45,31],[54,20,54,21],[54,14,54,19],[54,22,54,27],[54,28,54,31],[55,20,55,21],[55,14,55,19],[55,22,55,27],[55,28,55,31],[52,20,52,21],[52,14,52,19],[52,22,52,27],[52,28,52,31],[53,20,53,21],[53,14,53,19],[53,22,53,27],[53,28,53,31],[50,20,50,21],[50,14,50,19],[50,22,50,27],[50,28,50,31],[51,20,51,21],[51,14,51,19],[51,22,51,27],[51,28,51,31],[60,20,60,21],[60,14,60,19],[60,22,60,27],[60,28,60,31],[61,20,61,21],[61,14,61,19],[61,22,61,27],[61,28,61,31],[58,20,58,21],[58,14,58,19],[58,22,58,27],[58,28,58,31],[59,20,59,21],[59,14,59,19],[59,22,59,27],[59,28,59,31],[56,20,56,21],[56,14,56,19],[56,22,56,27],[56,28,56,31],[57,20,57,21],[57,14,57,19],[57,22,57,27],[57,28,57,31],[66,20,66,21],[66,14,66,19],[66,22,66,27],[66,28,66,31],[67,20,67,21],[67,14,67,19],[67,22,67,27],[67,28,67,31],[64,20,64,21],[64,14,64,19],[64,22,64,27],[64,28,64,31],[65,20,65,21],[65,14,65,19],[65,22,65,27],[65,28,65,31],[62,20,62,21],[62,14,62,19],[62,22,62,27],[62,28,62,31],[63,20,63,21],[63,14,63,19],[63,22,63,27],[63,28,63,31],[72,20,72,21],[72,14,72,19],[72,22,72,27],[72,28,72,31],[73,20,73,21],[73,14,73,19],[73,22,73,27],[73,28,73,31],[70,20,70,21],[70,14,70,19],[70,22,70,27],[70,28,70,31],[71,20,71,21],[71,14,71,19],[71,22,71,27],[71,28,71,31],[68,20,68,21],[68,14,68,19],[68,22,68,27],[68,28,68,31],[69,20,69,21],[69,14,69,19],[69,22,69,27],[69,28,69,31],[78,20,78,21],[78,14,78,19],[78,22,78,27],[78,28,78,31],[79,20,79,21],[79,14,79,19],[79,22,79,27],[79,28,79,31],[76,20,76,21],[76,14,76,19],[76,22,76,27],[76,28,76,31],[77,20,77,21],[77,14,77,19],[77,22,77,27],[77,28,77,31],[74,20,74,21],[74,14,74,19],[74,22,74,27],[74,28,74,31],[75,20,75,21],[75,14,75,19],[75,22,75,27],[75,28,75,31],[84,20,84,21],[84,14,84,19],[84,22,84,27],[84,28,84,31],[85,20,85,21],[85,14,85,19],[85,22,85,27],[85,28,85,31],[82,20,82,21],[82,14,82,19],[82,22,82,27],[82,28,82,31],[83,20,83,21],[83,14,83,19],[83,22,83,27],[83,28,83,31],[80,20,80,21],[80,14,80,19],[80,22,80,27],[80,28,80,31],[81,20,81,21],[81,14,81,19],[81,22,81,27],[81,28,81,31],[90,20,90,21],[90,14,90,19],[90,22,90,27],[90,28,90,31],[91,20,91,21],[91,14,91,19],[91,22,91,27],[91,28,91,31],[88,20,88,21],[88,14,88,19],[88,22,88,27],[88,28,88,31],[89,20,89,21],[89,14,89,19],[89,22,89,27],[89,28,89,31],[86,20,86,21],[86,14,86,19],[86,22,86,27],[86,28,86,31],[87,20,87,21],[87,14,87,19],[87,22,87,27],[87,28,87,31],[96,20,96,21],[96,14,96,19],[96,22,96,27],[96,28,96,31],[97,20,97,21],[97,14,97,19],[97,22,97,27],[97,28,97,31],[94,20,94,21],[94,14,94,19],[94,22,94,27],[94,28,94,31],[95,20,95,21],[95,14,95,19],[95,22,95,27],[95,28,95,31],[92,20,92,21],[92,14,92,19],[92,22,92,27],[92,28,92,31],[93,20,93,21],[93,14,93,19],[93,22,93,27],[93,28,93,31],[102,20,102,21],[102,14,102,19],[102,22,102,27],[102,28,102,31],[103,20,103,21],[103,14,103,19],[103,22,103,27],[103,28,103,31],[100,20,100,21],[100,14,100,19],[100,22,100,27],[100,28,100,31],[101,20,101,21],[101,14,101,19],[101,22,101,27],[101,28,101,31],[98,20,98,21],[98,14,98,19],[98,22,98,27],[98,28,98,31],[99,20,99,21],[99,14,99,19],[99,22,99,27],[99,28,99,31],[108,20,108,21],[108,14,108,19],[108,22,108,27],[108,28,108,31],[109,20,109,21],[109,14,109,19],[109,22,109,27],[109,28,109,31],[106,20,106,21],[106,14,106,19],[106,22,106,27],[106,28,106,31],[107,20,107,21],[107,14,107,19],[107,22,107,27],[107,28,107,31],[104,20,104,21],[104,14,104,19],[104,22,104,27],[104,28,104,31],[105,20,105,21],[105,14,105,19],[105,22,105,27],[105,28,105,31],[114,20,114,21],[114,14,114,19],[114,22,114,27],[114,28,114,31],[115,20,115,21],[115,14,115,19],[115,22,115,27],[115,28,115,31],[112,20,112,21],[112,14,112,19],[112,22,112,27],[112,28,112,31],[113,20,113,21],[113,14,113,19],[113,22,113,27],[113,28,113,31],[110,20,110,21],[110,14,110,19],[110,22,110,27],[110,28,110,31],[111,20,111,21],[111,14,111,19],[111,22,111,27],[111,28,111,31],[120,20,120,21],[120,14,120,19],[120,22,120,27],[120,28,120,31],[121,20,121,21],[121,14,121,19],[121,22,121,27],[121,28,121,31],[118,20,118,21],[118,14,118,19],[118,22,118,27],[118,28,118,31],[119,20,119,21],[119,14,119,19],[119,22,119,27],[119,28,119,31],[116,20,116,21],[116,14,116,19],[116,22,116,27],[116,28,116,31],[117,21,117,22],[117,15,117,20],[117,23,117,28],[117,29,117,32],[126,20,126,21],[126,14,126,19],[126,22,126,27],[126,28,126,31],[127,20,127,21],[127,14,127,19],[127,22,127,27],[127,28,127,31],[124,20,124,21],[124,14,124,19],[124,22,124,27],[124,28,124,31],[125,20,125,21],[125,14,125,19],[125,22,125,27],[125,28,125,31],[122,20,122,21],[122,14,122,19],[122,22,122,27],[122,28,122,31],[123,20,123,21],[123,14,123,19],[123,22,123,27],[123,28,123,31],[132,20,132,21],[132,14,132,19],[132,22,132,27],[132,28,132,31],[133,20,133,21],[133,14,133,19],[133,22,133,27],[133,28,133,31],[130,20,130,21],[130,14,130,19],[130,22,130,27],[130,28,130,31],[131,20,131,21],[131,14,131,19],[131,22,131,27],[131,28,131,31],[128,20,128,21],[128,14,128,19],[128,22,128,27],[128,28,128,31],[129,20,129,21],[129,14,129,19],[129,22,129,27],[129,28,129,31],[138,20,138,21],[138,14,138,19],[138,22,138,27],[138,28,138,31],[139,20,139,21],[139,14,139,19],[139,22,139,27],[139,28,139,31],[136,20,136,21],[136,14,136,19],[136,22,136,27],[136,28,136,31],[137,20,137,21],[137,14,137,19],[137,22,137,27],[137,28,137,31],[134,20,134,21],[134,14,134,19],[134,22,134,27],[134,28,134,31],[135,20,135,21],[135,14,135,19],[135,22,135,27],[135,28,135,31],[144,20,144,21],[144,14,144,19],[144,22,144,27],[144,28,144,31],[145,20,145,21],[145,14,145,19],[145,22,145,27],[145,28,145,31],[142,20,142,21],[142,14,142,19],[142,22,142,27],[142,28,142,31],[143,20,143,21],[143,14,143,19],[143,22,143,27],[143,28,143,31],[140,20,140,21],[140,14,140,19],[140,22,140,27],[140,28,140,31],[141,20,141,21],[141,14,141,19],[141,22,141,27],[141,28,141,31],[150,20,150,21],[150,14,150,19],[150,22,150,27],[150,28,150,31],[151,20,151,21],[151,14,151,19],[151,22,151,27],[151,28,151,31],[148,20,148,21],[148,14,148,19],[148,22,148,27],[148,28,148,31],[149,20,149,21],[149,14,149,19],[149,22,149,27],[149,28,149,31],[146,20,146,21],[146,14,146,19],[146,22,146,27],[146,28,146,31],[147,20,147,21],[147,14,147,19],[147,22,147,27],[147,28,147,31],[156,20,156,21],[156,14,156,19],[156,22,156,27],[156,28,156,31],[157,20,157,21],[157,14,157,19],[157,22,157,27],[157,28,157,31],[154,20,154,21],[154,14,154,19],[154,22,154,27],[154,28,154,31],[155,20,155,21],[155,14,155,19],[155,22,155,27],[155,28,155,31],[152,20,152,21],[152,14,152,19],[152,22,152,27],[152,28,152,31],[153,20,153,21],[153,14,153,19],[153,22,153,27],[153,28,153,31],[162,20,162,21],[162,14,162,19],[162,22,162,27],[162,28,162,31],[163,20,163,21],[163,14,163,19],[163,22,163,27],[163,28,163,31],[160,20,160,21],[160,14,160,19],[160,22,160,27],[160,28,160,31],[161,20,161,21],[161,14,161,19],[161,22,161,27],[161,28,161,31],[158,20,158,21],[158,14,158,19],[158,22,158,27],[158,28,158,31],[159,20,159,21],[159,14,159,19],[159,22,159,27],[159,28,159,31],[168,20,168,21],[168,14,168,19],[168,22,168,27],[168,28,168,31],[169,20,169,21],[169,14,169,19],[169,22,169,27],[169,28,169,31],[166,20,166,21],[166,14,166,19],[166,22,166,27],[166,28,166,31],[167,20,167,21],[167,14,167,19],[167,22,167,27],[167,28,167,31],[164,20,164,21],[164,14,164,19],[164,22,164,27],[164,28,164,31],[165,20,165,21],[165,14,165,19],[165,22,165,27],[165,28,165,31],[174,20,174,21],[174,14,174,19],[174,22,174,27],[174,28,174,31],[175,20,175,21],[175,14,175,19],[175,22,175,27],[175,28,175,31],[172,20,172,21],[172,14,172,19],[172,22,172,27],[172,28,172,31],[173,20,173,21],[173,14,173,19],[173,22,173,27],[173,28,173,31],[170,20,170,21],[170,14,170,19],[170,22,170,27],[170,28,170,31],[171,20,171,21],[171,14,171,19],[171,22,171,27],[171,28,171,31],[180,20,180,21],[180,14,180,19],[180,22,180,27],[180,28,180,31],[181,21,181,22],[181,15,181,20],[181,23,181,28],[181,29,181,32],[178,20,178,21],[178,14,178,19],[178,22,178,27],[178,28,178,31],[179,21,179,22],[179,15,179,20],[179,23,179,28],[179,29,179,32],[176,20,176,21],[176,14,176,19],[176,22,176,27],[176,28,176,31],[177,20,177,21],[177,14,177,19],[177,22,177,27],[177,28,177,31],[186,20,186,21],[186,14,186,19],[186,22,186,27],[186,28,186,31],[187,20,187,21],[187,14,187,19],[187,22,187,27],[187,28,187,31],[184,20,184,21],[184,14,184,19],[184,22,184,27],[184,28,184,31],[185,20,185,21],[185,14,185,19],[185,22,185,27],[185,28,185,31],[182,20,182,21],[182,14,182,19],[182,22,182,27],[182,28,182,31],[183,20,183,21],[183,14,183,19],[183,22,183,27],[183,28,183,31],[192,20,192,21],[192,14,192,19],[192,22,192,27],[192,28,192,31],[193,20,193,21],[193,14,193,19],[193,22,193,27],[193,28,193,31],[190,20,190,21],[190,14,190,19],[190,22,190,27],[190,28,190,31],[191,20,191,21],[191,14,191,19],[191,22,191,27],[191,28,191,31],[188,20,188,21],[188,14,188,19],[188,22,188,27],[188,28,188,31],[189,20,189,21],[189,14,189,19],[189,22,189,27],[189,28,189,31],[198,20,198,21],[198,14,198,19],[198,22,198,27],[198,28,198,31],[199,20,199,21],[199,14,199,19],[199,22,199,27],[199,28,199,31],[196,20,196,21],[196,14,196,19],[196,22,196,27],[196,28,196,31],[197,20,197,21],[197,14,197,19],[197,22,197,27],[197,28,197,31],[194,20,194,21],[194,14,194,19],[194,22,194,27],[194,28,194,31],[195,20,195,21],[195,14,195,19],[195,22,195,27],[195,28,195,31],[204,20,204,21],[204,14,204,19],[204,22,204,27],[204,28,204,31],[205,20,205,21],[205,14,205,19],[205,22,205,27],[205,28,205,31],[202,20,202,21],[202,14,202,19],[202,22,202,27],[202,28,202,31],[203,20,203,21],[203,14,203,19],[203,22,203,27],[203,28,203,31],[200,20,200,21],[200,14,200,19],[200,22,200,27],[200,28,200,31],[201,20,201,21],[201,14,201,19],[201,22,201,27],[201,28,201,31],[210,20,210,21],[210,14,210,19],[210,22,210,27],[210,28,210,31],[211,20,211,21],[211,14,211,19],[211,22,211,27],[211,28,211,31],[208,20,208,21],[208,14,208,19],[208,22,208,27],[208,28,208,31],[209,20,209,21],[209,14,209,19],[209,22,209,27],[209,28,209,31],[206,20,206,21],[206,14,206,19],[206,22,206,27],[206,28,206,31],[207,20,207,21],[207,14,207,19],[207,22,207,27],[207,28,207,31],[216,20,216,21],[216,14,216,19],[216,22,216,27],[216,28,216,31],[217,20,217,21],[217,14,217,19],[217,22,217,27],[217,28,217,31],[214,20,214,21],[214,14,214,19],[214,22,214,27],[214,28,214,31],[215,20,215,21],[215,14,215,19],[215,22,215,27],[215,28,215,31],[212,20,212,21],[212,14,212,19],[212,22,212,27],[212,28,212,31],[213,20,213,21],[213,14,213,19],[213,22,213,27],[213,28,213,31],[222,20,222,21],[222,14,222,19],[222,22,222,27],[222,28,222,31],[223,20,223,21],[223,14,223,19],[223,22,223,27],[223,28,223,31],[220,20,220,21],[220,14,220,19],[220,22,220,27],[220,28,220,31],[221,20,221,21],[221,14,221,19],[221,22,221,27],[221,28,221,31],[218,20,218,21],[218,14,218,19],[218,22,218,27],[218,28,218,31],[219,20,219,21],[219,14,219,19],[219,22,219,27],[219,28,219,31],[228,20,228,21],[228,14,228,19],[228,22,228,27],[228,28,228,31],[229,20,229,21],[229,14,229,19],[229,22,229,27],[229,28,229,31],[226,20,226,21],[226,14,226,19],[226,22,226,27],[226,28,226,31],[227,20,227,21],[227,14,227,19],[227,22,227,27],[227,28,227,31],[224,20,224,21],[224,14,224,19],[224,22,224,27],[224,28,224,31],[225,20,225,21],[225,14,225,19],[225,22,225,27],[225,28,225,31],[234,20,234,21],[234,14,234,19],[234,22,234,27],[234,28,234,31],[235,20,235,21],[235,14,235,19],[235,22,235,27],[235,28,235,31],[232,20,232,21],[232,14,232,19],[232,22,232,27],[232,28,232,31],[233,20,233,21],[233,14,233,19],[233,22,233,27],[233,28,233,31],[230,20,230,21],[230,14,230,19],[230,22,230,27],[230,28,230,31],[231,20,231,21],[231,14,231,19],[231,22,231,27],[231,28,231,31],[240,20,240,21],[240,14,240,19],[240,22,240,27],[240,28,240,31],[241,20,241,21],[241,14,241,19],[241,22,241,27],[241,28,241,31],[238,20,238,21],[238,14,238,19],[238,22,238,27],[238,28,238,31],[239,20,239,21],[239,14,239,19],[239,22,239,27],[239,28,239,31],[236,20,236,21],[236,14,236,19],[236,22,236,27],[236,28,236,31],[237,20,237,21],[237,14,237,19],[237,22,237,27],[237,28,237,31],[246,20,246,21],[246,14,246,19],[246,22,246,27],[246,28,246,31],[247,20,247,21],[247,14,247,19],[247,22,247,27],[247,28,247,31],[244,20,244,21],[244,14,244,19],[244,22,244,27],[244,28,244,31],[245,20,245,21],[245,14,245,19],[245,22,245,27],[245,28,245,31],[242,20,242,21],[242,14,242,19],[242,22,242,27],[242,28,242,31],[243,20,243,21],[243,14,243,19],[243,22,243,27],[243,28,243,31],[252,20,252,21],[252,14,252,19],[252,22,252,27],[252,28,252,31],[253,20,253,21],[253,14,253,19],[253,22,253,27],[253,28,253,31]],"merged_total":3200,"flags":["merged_cut"]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUTE DESIGN PRESSURE",null,null,null,null,null,"rdl:RDS7311150",null,"An <ABSOLUTE DESIGN PRESSURE> is an <IndirectProperty> that refers to a <DESIGN PRESSURE> that is relative to a full vacuum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACCURACY",null,null,null,null,null,"rdl:RDS1416460501",null,"An <ACCURACY> is an <IndirectProperty> that represents the closeness of agreement between the result of a measurement and the (conventional) true value of the quantity being measured",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACCURACY RANGE",null,null,null,null,null,"rdl:RDS1415829671",null,"An <ACCURACY RANGE> is an <IndirectProperty> that represents a <PropertyRange> within which the nominal <ACCURACY> is valid",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACCURACY RATING",null,null,null,null,null,"rdl:RDS5922494",null,"An <ACCURACY RATING> is an <IndirectProperty> that represents the limits within which the inaccuracy of a given model of a device can be guaranteed in its specification",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACHIEVED AVAILABILITY (AA)",null,null,null,null,null,"rdl:RDS14649170",null,"An <ACHIEVED AVAILABILITY (AA)> is an <IndirectProperty> that refers to the probability that a system or equipment, when used under stated conditions in an ideal support environment (i.e., readily available tools, spares, personnel, etc.), will operate satisfactorily at any point in <TIME>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACIDIFICATION CHARACTERIZATION FACTOR",null,null,null,null,null,"rdl:RDS14820093",null,"An <ACIDIFICATION CHARACTERIZATION FACTOR> is an <IndirectProperty> that refers to used to quantify the potential impact per unit of emission",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACIDIFICATION EQUIVALENT",null,null,null,null,null,"rdl:RDS14824615",null,"An <ACIDIFICATION EQUIVALENT> is an <IndirectProperty> that refers to a measure on emission of Nox and SO2 all together",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACTIVITY FACTOR REFERENCED TO HENRY&#39;S LAW",null,null,null,null,null,"rdl:RDS9999006",null,"An <ACTIVITY FACTOR REFERENCED TO HENRY&#39;S LAW> is an <IndirectProperty> where there are three different cases for the activity factor referenced to Henry&#39;s law: molality basis, gamma_m, <CONCENTRATION> basis, gamma_c, and amount-of-substance basis, gamm_z: gamma_m,B = a_m,B/(b_B/b^Theta); gamma_c,B = a_c,B/(c_b/c^Theta); gamma_x,B = a_x,B/x_B",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACTIVITY FACTOR REFERENCED TO RAOULT&#39;S LAW",null,null,null,null,null,"rdl:RDS9999007",null,"An <ACTIVITY FACTOR REFERENCED TO RAOULT&#39;S LAW> is an <IndirectProperty> where f_B = a_B/x_B where a_B is the activity of solute B and x_B is the amount-of-substance fraction of B",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACTIVITY OF SOLUTE B",null,null,null,null,null,"rdl:RDS388664",null,"An <ACTIVITY OF SOLUTE B> is an <IndirectProperty> where, for a solute B in a solution, a_B is proportional to the absolute activity lambda_B, the proportionality factor, which is a function of <TEMPERATURE> and <PRESSURE> only, being determined by the condition that, at constant <TEMPERATURE> and <PRESSURE> a_B divided by the molality <RATIO> m_B/m^Theta, tends to 1 at infinite dilution; b_B is the molality of solute B, and b^Theta is standard molality, usually 1 mol/kg",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACTIVITY OF SOLVENT A",null,null,null,null,null,"rdl:RDS388799",null,"An <ACTIVITY OF SOLUTE A> is an <IndirectProperty> that, for the solvent A in a solution, refers to a <RATIO> of the absolute activity of substance A, lambda_A, to that, lambda*_A, of the pure solvent at the same <TEMPERATURE> and pressure",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ADJUSTABLE LEVEL MEASURING RANGE",null,null,null,null,null,"rdl:RDS1458291861",null,"An <ADJUSTABLE LEVEL MEASURING RANGE> is an <IndirectProperty> of a <LEVEL MEASURING ELEMENT> denoting the <PropertyRange> within which the range can be adjusted",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ADJUSTABLE TEMPERATURE MEASURING RANGE",null,null,null,null,null,"rdl:RDS1458175821",null,"An <ADJUSTABLE TEMPERATURE MEASURING RANGE> is an <IndirectProperty> of a <TEMPERATURE MEASURING ELEMENT> denoting the <PropertyRange> within which the range can be adjusted",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ADJUSTED AMOUNT",null,null,null,null,null,"rdl:RDS482640180",null,"An <ADJUSTED AMOUNT> is an <IndirectProperty> that refers to an <AMOUNT> of a product that has been adjusted (up or down) based on if its quality, proven by lab tests, has shown to be above or below standard",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ADJUSTED MASS",null,null,null,null,null,"rdl:RDS482640362",null,"An <ADJUSTED MASS> is an <IndirectProperty> that refers to a <MASS> of a product that has been adjusted (up or down) due to the quality of the product",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ADJUSTED VOLUME",null,null,null,null,null,"rdl:RDS482640310",null,"An <ADJUSTED VOLUME> is an <IndirectProperty> that refers to a <VOLUME> of a product that has been adjusted (up or down) due to the quality of the product",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ADJUSTMENT REFERENCE TEMPERATURE",null,null,null,null,null,"rdl:RDS7348985",null,"An <ADJUSTMENT REFERENCE TEMPERATURE> is an <IndirectProperty> that refers to a known <TEMPERATURE> which eg. a pointer or scale can be adjusted against",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AFFINITY (OF A CHEMICAL REACTION)",null,null,null,null,null,"rdl:RDS389024",null,"An <AFFINITY (OF A CHEMICAL REACTION)> is an <IndirectProperty> where A = -Sum(nu_B/mu_B) where nu_B is the stoichiometric number of substance B and mu_B the chemical potential of substance B. The summation goes over all substances of B",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ALARM LIMIT",null,null,null,null,null,"rdl:RDS1020232051",null,"An <ALARM LIMIT> is a <IndirectProperty> that denotes the limit of an acceptable value range",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALARM LIMIT HIGH",null,null,null,null,null,"rdl:RDS1020249561",null,"An <ALARM LIMIT HIGH> is an <ALARM LIMIT> for an acceptable high value",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALARM LIMIT HIGH HIGH",null,null,null,null,null,"rdl:RDS1020240091",null,"An <ALARM LIMIT HIGH HIGH> is an <ALARM LIMIT> for an acceptable high-high value",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALARM LIMIT LOW",null,null,null,null,null,"rdl:RDS1020252061",null,"An <ALARM LIMIT LOW> is an <ALARM LIMIT> for an acceptable low value",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALARM LIMIT LOW LOW",null,null,null,null,null,"rdl:RDS1020252711",null,"An <ALARM LIMIT LOW LOW> is an <ALARM LIMIT> for an acceptable low-low value",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOCATED AMOUNT",null,null,null,null,null,"rdl:RDS409510451",null,"An <ALLOCATED AMOUNT> is an <IndirectProperty> that refers to an <AMOUNT> that is an calculated/decided amount (quantity) of a product",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE AXIAL FORCE",null,null,null,null,null,"rdl:RDS14250275",null,"An <ALLOWABLE AXIAL FORCE> is an <IndirectProperty> that refers to a <FORCE> allowable in axial direction for a <COMPONENT>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE AXIAL MOMENT FORCE",null,null,null,null,null,"rdl:RDS14250320",null,"An <ALLOWABLE AXIAL MOMENT FORCE> is an <IndirectProperty> that refers to a <MOMENT OF FORCE> that is allowable around axial axis for a <COMPONENT>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE BACK PRESSURE",null,null,null,null,null,"rdl:RDS8423289",null,"An <ALLOWABLE BACK PRESSURE> is an <Indirect Property> that refers to a <BACK PRESSURE> that an <ARTEFACT> is allowed to have under stated conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE HORIZONTAL 90 DEGREES FORCE",null,null,null,null,null,"rdl:RDS14250410",null,"An <ALLOWABLE HORIZ 90 FORCE> is an <IndirectProperty> that is a <FORCE> allowable for the piping inlet horizontal 90 degrees direction",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE HORIZONTAL 90 DEGREES MOMENT FORCE",null,null,null,null,null,"rdl:RDS14250455",null,"An <ALLOWABLE HORIZ 90 MOMENT FORCE> is an <IndirectProperty> that refers to a <MOMENT OF FORCE> allowable for the piping inlet horizontal 90 degrees direction",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE LOADING PRESSURE",null,null,null,null,null,"rdl:RDS14250725",null,"An <ALLOWABLE LOADING PRESSURE> is an <IndirectProperty> that refers to a <PRESSURE> that is allowed during loading",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE NOZZLE TORQUE",null,null,null,null,null,"rdl:RDS365174",null,"An <ALLOWABLE NOZZLE TORQUE> is an <IndirectProperty> that refers to a <TORQUE> that a <NOZZLE> can accept from the interface piping",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE OVERPRESSURE PERCENTAGE",null,null,null,null,null,"rdl:RDS1470889031",null,"An <ALLOWABLE OVERPRESSURE PERCENTAGE> is an <IndirectProperty> that refers to a <PERCENTAGE> overpressure above the setting pressure of the applicable relief valve",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE PRESSURE DROP GRADIENT",null,null,null,null,null,"rdl:RDS8106300",null,"An <ALLOWABLE PRESSURE DROP GRADIENT> is an <Indirect Property> that refers to a <PRESSURE DROP GRADIENT> an allowable decrease in <PRESSURE> over an interval of <LENGTH>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE STARTING VOLTAGE DROP FACTOR",null,null,null,null,null,"rdl:RDS410894",null,"An <ALLOWABLE STARTING VOLTAGE DROP FACTOR> is an <IndirectProperty> that refers to a <RATIO> of a <MAXIMUM VOLTAGE DROP> to a <NORMAL OPERATING VOLTAGE AT STARTUP>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE STARTING VOLTAGE PERCENTAGE",null,null,null,null,null,"rdl:RDS13658045",null,"An <ALLOWABLE STARTING VOLTAGE PERCENTAGE> is an <IndirectProperty> that refers to a <PERCENTAGE> that is the highest acceptable <RATIO> of <STARTING VOLTAGE> over <RATED VOLTAGE>, expressed in percent",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE TEST LEVEL DISPLACEMENT",null,null,null,null,null,"rdl:RDS14252930",null,"An <ALLOWABLE TEST LEVEL DISPLACEMENT> is an <IndirectProperty> that refers to a <VIBRATION DISPLACEMENT> for allowable test level",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE VERTICAL FORCE",null,null,null,null,null,"rdl:RDS14260850",null,"An <ALLOWABLE VERTICAL FORCE> is an <IndirectProperty> that refers to a <FORCE> that is allowable in vertical direction",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALLOWABLE VERTICAL MOMENT FORCE",null,null,null,null,null,"rdl:RDS14250365",null,"An <ALLOWABLE VERTICAL MOMENT FORCE> is an <IndirectProperty> that refers to a <MOMENT OF FORCE> that is allowable around vertical axis",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AMBIENT OPERATING HUMIDITY RANGE",null,null,null,null,null,"rdl:RDS8499297",null,"An <AMBIENT OPERATING HUMIDITY RANGE> is an <IndirectProperty> that refers to a <HUMIDITY> limited by upper and lower limits within which a member of a physical object class is intended to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AMBIENT OPERATING TEMPERATURE RANGE",null,null,null,null,null,"rdl:RDS1411476491",null,"An <AMBIENT OPERATING TEMPERATURE RANGE> is an <IndirectProperty> that refers to a <TEMPERATURE> limited by upper and lower limits within which a member of a physical object class is intended to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AMBIENT STORAGE HUMIDITY RANGE",null,null,null,null,null,"rdl:RDS8499077",null,"An <AMBIENT STORAGE HUMIDITY RANGE> is an <IndirectProperty> that refers to a <HUMIDITY> limited by upper and lower limits which is the permissible ambient humidity in which a member of a physical object class is intended to be stored when not used for its purpose",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AMBIENT STORAGE TEMPERATURE RANGE",null,null,null,null,null,"rdl:RDS1411582901",null,"An <AMBIENT STORAGE TEMPARATURE RANGE> is an <IndirectProperty> that refers to a <TEMPERATURE> limited by upper and lower limits which is the permissible ambient temperature in which a member of a physical object class is intended to be stored when not used for its purpose",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AMOUNT ADJUSTMENT TRANSACTION",null,null,null,null,null,"rdl:RDS498993203",null,"An <AMOUNT ADJUSTMENT TRANSACTION> is an <IndirectProperty> that refers to an <AMOUNT> that is any change in amount of mass or volume",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANGULAR CROSS-SECTION",null,null,null,null,null,"rdl:RDS392759",null,"An <ANGULAR CROSS-SECTION> is an <IndirectProperty> that refers to a cross section for ejecting or scattering a particle into an elementary cone, divided by a <SOLID ANGLE> d Omega of that cone: sigma = integral (sigma_Omega.d Omega)",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"APPARENT POWER",null,null,null,null,null,"rdl:RDS384434",null,"An <APPARENT POWER> is an <Indirect Property>which is the total power in an AC circuit, both dissipated and absorbed/returned symbolized by the letter S = U.I where U is rms value of <VOLTAGE> and I is rms value of <ELECTRIC CURRENT>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"APPROXIMATE DISCHARGE TIME",null,null,null,null,null,"rdl:RDS6739932",null,"An <APPROXIMATE DISCHARGE TIME> is an <IndirectProperty> that refers to a <TIME> that it normally takes to discharge eg. a <PRESSURE> vessel, a battery or to empty a fire extinguisher",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"APPROXIMATE INSTALLATION WEIGHT",null,null,null,null,null,"rdl:RDS1467625211",null,"An <APPROXIMATE INSTALLATION WEIGHT> is an <IndirectProperty> that refers to an estimated <MASS> for lifting purposes",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"APPROXIMATE OPERATING WEIGHT",null,null,null,null,null,"rdl:RDS1661765921",null,"An <APPROXIMATE OPERATING WEIGHT> is an <IndirectProperty> that refers to an estimated <MASS> of a physical object during operations, so filled with a fluid",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"APPROXIMATE TOTAL HEIGHT",null,null,null,null,null,"rdl:RDS7483159",null,"An <APPROXIMATE TOTAL HEIGHT> is an <IndirectProperty> that refers to an approximate total <HEIGHT> of something",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"APPROXIMATE TOTAL LENGTH",null,null,null,null,null,"rdl:RDS7483114",null,"An <APPROXIMATE TOTAL LENGTH> is an <IndirectProperty> that refers to an approximate total <LENGTH> of something",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"APPROXIMATE TOTAL WIDTH",null,null,null,null,null,"rdl:RDS7483204",null,"An <APPROXIMATE TOTAL WIDTH> is an <IndirectProperty> which is an approximate total <WIDTH> of something",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ARITHMETIC MEAN TEMPERATURE DIFFERENCE",null,null,null,null,null,"rdl:RDS14118190",null,"An <ARITHMETIC MEAN TEMPERATURE DIFFERENCE> is an <IndirectProperty> that refers to an arithmetic mean value of the <DIFFERENTIAL TEMPERATURE> at which heat exchange is calculated to occur",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ARM LENGTH",null,null,null,null,null,"rdl:RDS6480660",null,"An <ARM LENGTH> is an <IndirectProperty> that refers to a <LENGTH> from a centre of rotation to the origin of force",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ASYNCHRONOUS SPEED",null,null,null,null,null,"rdl:RDS12842180",null,"An <ASYNCHRONOUS SPEED> is an <IndirectProperty> that refers to a <ROTATIONAL SPEED> of an AC machine at a given load",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ASYNCHRONOUS SPEED AT 1/1 LOAD",null,null,null,null,null,"rdl:RDS14148914",null,"An <ASYNCHRONOUS SPEED> is an <IndirectProperty> that refers to a <ROTATIONAL SPEED> of an AC machine at full load",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ATOMIC ATTENUATION COEFFICIENT",null,null,null,null,null,"rdl:RDS393299",null,"An <ATOMIC ATTENUATION COEFFICIENT> is an <IndirectProperty> of a <MATERIAL> that refers to a <RATE> of penetration by a beam of light, sound, particles, or other energy or matter as defined in ISO 80000-10 (2009) 10-53",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ATTENUATION COEFFICIENT",null,null,null,null,null,"rdl:RDS381419",null,"An <ATTENUATION COEFFICIENT> is an <IndirectProperty> where, if a field quantity is a function of <DISTANCE> x given by F(x) = Ae^(alpha x).cos[Beta(x-x_0)], then alpha is the attenuation coefficient and beta is the phase coefficient",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AUDITORY THRESHOLD",null,null,null,null,null,"rdl:RDS9999037",null,"An <AUDITORY THRESHOLD> is an <IndirectProperty> that refers to thresholds of sensitivity to auditory signals and other input to the ear or the sense of hearing as defined in ISO 80000-14-2009",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AUTOGENOUS IGNITION TEMPERATURE",null,null,null,null,null,"rdl:RDS7352431",null,"An <AUTOGENOUS IGNITION TEMPERATURE> is an <IndirectProperty> that refers to an ignition <TEMPERATURE> as defined in ISO 1998 def. 2-004",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AUTORECLOSE INTERRUPTION TIME",null,null,null,null,null,"rdl:RDS409904",null,"An <AUTORECLOSE INTERRUPTION TIME> is an <IndirectProperty> that refers to a <DURATION> of automatic reclosing when the power line or phase cannot transfer any power",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AUTORECLOSE OPEN TIME",null,null,null,null,null,"rdl:RDS409859",null,"An <AUTORECLOSE OPEN TIME> is an <IndirectProperty> that refers to a <DURATION> of automatic reclosing when the pole(s) of the associated circuit-breaker is (are) open",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE AREA",null,null,null,null,null,"rdl:RDS16631157",null,"An <AVERAGE AREA> is an <IndirectProperty> that refers to an <AREA> which is the quotient obtained by dividing the total sum of a set of area measurements by the total number of measurements",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE DEPTH",null,null,null,null,null,"rdl:RDS13101798",null,"An <AVERAGE DEPTH> is an <IndirectProperty> that refers to a <DEPTH> which is the quotient obtained by dividing the sum total of a set of depths by the number of dephts",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE ENERGY LOSS PER ION PAIR FORMED",null,null,null,null,null,"rdl:RDS393704",null,"An <AVERAGE ENERGY LOSS PER ION PAIR FORMED> is an <IndirectProperty> as defined in ISO 80000-10 (2009) 10-62",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE FLOW RATE",null,null,null,null,null,"rdl:RDS16630527",null,"An <AVERAGE FLOW RATE> is an <IndirectProperty> that refers to a <FLOW RATE> which is the quotient obtained by dividing the total sum of a set of flow rate measurements by the total number of measurements",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE HEIGHT",null,null,null,null,null,"rdl:RDS8647860",null,"An <AVERAGE HEIGHT>is an <IndirectProperty> that refers to a <HEIGHT> which is the quotient obtained by dividing the sum total of a set of heights by the number of heights",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE INFORMATION RATE",null,null,null,null,null,"rdl:RDS9999038",null,"An <AVERAGE INFORMATION RATE> is an <IndirectProperty> that refers to the expected number of bits of information that may be recovered from an encoded message as defined in ISO-80000.38-2009",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE LOGARITMIC ENERGY DECREMENT",null,null,null,null,null,"rdl:RDS394199",null,"An <AVERAGE LOGARITMIC ENERGY DECREMENT> is an <IndirectProperty> that refers to the Average value of the increase in lethargy in elastic collisions between neutrons and nuclei whose kinetic energy is negligible compared with that of the neutrons",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE MOLECULAR WEIGHT",null,null,null,null,null,"rdl:RDS14256305",null,"An <AVERAGE MOLECULAR WEIGHT> is an <IndirectProperty> that refers to an averaged <MOLECULAR WEIGHT> which is to be given in gas analysis",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE MUTUAL INFORMATION RATE",null,null,null,null,null,"rdl:RDS9999039",null,"An <AVERAGE MUTUAL INFORMATION RATE> is a measure of the amount of information that can be obtained about one random variable by observing another. As defined in ISO 80000-13.40-2009",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE PRESSURE",null,null,null,null,null,"rdl:RDS13117462",null,"An <AVERAGE PRESSURE> is an <IndirectProperty> that refers to a <PRESSURE> which is the quotient obtained by dividing the total sum of a set of <PRESSURE> measurements by the total number of measurements",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE QUANTITY",null,null,null,null,null,"rdl:RDS16629627",null,"An <AVERAGE QUANTITY> is an <IndirectProperty> that refers to a <QUANTITY> which is the quotient obtained by dividing the total sum of a set of quantity measurements by the total number of measurements",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE TEMPERATURE",null,null,null,null,null,"rdl:RDS13108062",null,"An <AVERAGE TEMPERATURE> is an <IndirectProperty> that refers to a <TEMPERATURE> which is the quotient obtained by dividing the total sum of a set of <TEMPERATURE> measurements by the total number of measurements",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE THICKNESS",null,null,null,null,null,"rdl:RDS14119450",null,"An <AVERAGE THICKNESS> is an <IndirectProperty> that refers to a <THICKNESS> that is the average thickness",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE VELOCITY",null,null,null,null,null,"rdl:RDS13107740",null,"An <AVERAGE VELOCITY> is an <IndirectProperty> that refers to a <VELOCITY> which is the quotient obtained by dividing the total sum of a set of <VELOCITY> measurements by the total number of measurements",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE VOLUME",null,null,null,null,null,"rdl:RDS16623687",null,"An <AVERAGE VOLUME> is an <IndirectProperty> that refers to a <VOLUME> which is the quotient obtained by dividing the total sum of a set of volume measurements by the total number of measurements",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE VOLUME FLOW RATE",null,null,null,null,null,"rdl:RDS16628457",null,"An <AVERAGE VOLUME FLOW RATE> is an <IndirectProperty> that refers to a <VOLUME FLOW RATE> which is the quotient obtained by dividing the total sum of a set of <VOLUME FLOW RATE> measurements by the total number of measurements",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AVERAGE WALL THICKNESS SOCKET-WELDING END",null,null,null,null,null,"rdl:RDS376739",null,"An <AVERAGE WALL THICKNESS SOCKET-WELDING END> is an <IndirectProperty> that refers to a <WALL THICKNESS> that refers to an average wall thickness of a <SOCKET WELDING END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"BACKGROUND CORROSION DEPTH",null,null,null,null,null,"rdl:RDS8774623",null,"A <BACKGROUND CORROSION DEPTH> is an <IndirectProperty> that refers to a <DEPTH> that is an estimated <DEPTH> of the METAL LOSS of the areas between the individual METAL LOSS features within a METAL LOSS cluster",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"BETA RATIO",null,null,null,null,null,"rdl:RDS4238768",null,"A <BETA RATIO> is an <IndirectProperty> that is the ratio s/S of the surface of the orifice bore (s) to the cross section (S) of the pipe in which the <ORIFICE PLATE> is installed",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"BLOCKING TEMPERATURE",null,null,null,null,null,"rdl:RDS7352369",null,"A <BLOCKING TEMPERATURE> is an <IndirectProperty> that, in the context of superparamagnetism, refers to the <TEMPERATURE> that is defined in ISO 1998 def. 2-012",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"BRAGG ANGLE",null,null,null,null,null,"rdl:RDS395684",null,"A <BRAGG ANGLE> is an <IndirectProperty> for a plane wave that is diffracted from a family of <LATTICE PLATES> that is the <ANGLE> Î¸ between the wave vector of the incident plane wave, ko, and the lattice planes",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"BRAKE FORCE",null,null,null,null,null,"rdl:RDS7923980",null,"A <BRAKE FORCE> is an <IndirectProperty> that refers to a <FORCE> that is the force needed to retard the motion of a body",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"BRAKE HORSEPOWER",null,null,null,null,null,"rdl:RDS7924042",null,"A <BRAKE HORSEPOWER> is an <IndirectProperty> that refers to a <POWER> which is an effective or useful <POWER> developed by a prime mover or an electric motor, as measured by a <BRAKE> or a <DYNAMOMETER>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"BRAKE MEAN EFFECTIVE PRESSURE",null,null,null,null,null,"rdl:RDS13291466",null,"A <BRAKE MEAN EFFECTIVE PRESSURE> is an <IndirectProperty> that refers to an <AVERAGE PRESSURE> that is that part of the indicated mean effective <PRESSURE> developed in an engine cylinder output equal to A <BRAKE HORSEPOWER> of A <ENGINE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"BREAKDOWN TORQUE",null,null,null,null,null,"rdl:RDS6652260",null,"A <BREAKDOWN TORQUE> is an <IndirectProperty> that refers to the maximum <TORQUE> the motor can produce at full rated voltage and frequency.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"BREAKDOWN TORQUE MULTIPLIER",null,null,null,null,null,"rdl:RDS411569",null,"A <BREAKDOWN TORQUE MULTIPLIER> is an <IndirectProperty> that refers to a <RATIO> of the <UPPER LIMIT TORQUE> which an <ASYNCHRONOUS MOTOR> will produce without an abrupt drop in speed, divided by the full load torque",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"BREAKOUT MOMENT",null,null,null,null,null,"rdl:RDS12147280",null,"A <BREAKOUT MOMENT> is an <IndirectProperty> that refers to a <MOMENT OF FORCE> needed to break open a <CONNECTOR>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"BREAKOUT TORQUE",null,null,null,null,null,"rdl:RDS16741157",null,"A <BREAKOUT TORQUE> is an <IndirectProperty> that refers to a <TORQUE> that must be applied to a rod, e.g. a valve spindle, before it starts turning",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"BUCKLING RESISTANCE",null,null,null,null,null,"rdl:RDS374399",null,"A <BUCKLING RESISTANCE> is an <IndirectProperty> that refers to the resistance against <BUCKLING>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"BURST PRESSURE",null,null,null,null,null,"rdl:RDS8372714",null,"A <BURST PRESSURE> is an <IndirectProperty> that refers to a <PRESSURE> at which something will burst.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED ABSOLUTE OPEN FLOW",null,null,null,null,null,"rdl:RDS8180432",null,"A <CALCULATED ABSOLUTE OPEN FLOW> is an <IndirectProperty> that refers to a <VOLUME FLOW RATE> that is the measurement of the potential of a flowing gas well",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED AREA",null,null,null,null,null,"rdl:RDS8406909",null,"A <CALCULATED AREA> is an <IndirectProperty> that refers to an <AREA(math)> that is based on calculations",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED AVERAGE HEIGHT",null,null,null,null,null,"rdl:RDS8656001",null,"A <CALCULATED AVERAGE HEIGHT> is an <IndirectProperty> that refers to an <AVERAGE HEIGHT> that is determined by calculation",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED CUSTOMARY UNIT VALVE FLOW COEFFICIENT",null,null,null,null,null,"rdl:RDS411119",null,"A <CALCULATED CUSTOMARY UNIT VALVE FLOW COEFFICIENT> is an <IndirectProperty> that refers to a calculated <VALVE FLOW COEFFICIENT> which is the calculated flow of water (at 60 deg F), expressed in US gall/min which can be passed by the valve when a <PRESSURE> drop of 1 psi act across it",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED DIFFERENTIAL PRESSURE RANGE",null,null,null,null,null,"rdl:RDS7478026",null,"A <CALCULATED DIFFERENTIAL PRESSURE RANGE> is a <PRESSURE RANGE> that is limited by the calculated lower and upper differential pressure limit that corresponds to the flow range for a measuring orifice plate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED DRY WEIGHT",null,null,null,null,null,"rdl:RDS14133490",null,"A <CALCULATED DRY WEIGHT> is an <IndirectProperty> that refers to a <DRY WEIGHT> which is <CALCULATED>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED HOOP STRESS",null,null,null,null,null,"rdl:RDS13299220",null,"A <CALCULATED HOOP STRESS> is an <IndirectProperty> that refers to a <HOOP STRESS> as <CALCULATED> from design or operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED METRIC VALVE FLOW COEFFICIENT",null,null,null,null,null,"rdl:RDS411074",null,"A <CALCULATED METRIC VALVE FLOW COEFFICIENT> is an <IndirectProperty> that refers to a <CALCULATED VALVE FLOW COEFFICIENT> which is the <CALCULATED FLOW> of water expressed in cubic metres/hr which can be passed by the valve when a <PRESSURE> drop of 1 bar (actually 0,981bar) act across it",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED OPERATING WEIGHT",null,null,null,null,null,"rdl:RDS1661808291",null,"A <CALCULATED OPERATING WEIGHT> is an <IndirectProperty> that refers to an <OPERATING WEIGHT> which is calculated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED OVERALL HEIGHT",null,null,null,null,null,"rdl:RDS14133805",null,"A <CALCULATED OVERALL HEIGHT> is an <IndirectProperty> that refers to an <OVERALL HEIGHT> which is calculated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED OVERALL LENGTH",null,null,null,null,null,"rdl:RDS14133715",null,"A <CALCULATED OVERALL LENGTH> is an <IndirectProperty> that refers to an <OVERALL LENGTH> which is calculated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED OVERALL WIDTH",null,null,null,null,null,"rdl:RDS14133760",null,"A <CALCULATED OVERALL WIDTH> is an <IndirectProperty> that refers to an <OVERALL WIDTH> which is calculated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED PRESSURE LOSS AT FULL RANGE",null,null,null,null,null,"rdl:RDS7478088",null,"A <CALCULATED PRESSURE LOSS AT FULL RANGE> is an <IndirectProperty> that is apressure drop which is a permanent pressure drop across an item at 100 % of the flow range, established by calculations",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED PRESSURE RISE TO SURGE",null,null,null,null,null,"rdl:RDS14259815",null,"A <CALCULATED PRESSURE RISE TO SURGE> is an <IndirectProperty> that refers to a <CALCULATED PRESSURE RISE> from normal conditions to surge start",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED RUPTURING DISC AREA",null,null,null,null,null,"rdl:RDS8406971",null,"A <CALCULATED RUPTURING DISC AREA> is an <IndirectProperty> that refers to a <CALCULATED AREA> of a <RUPTURING DISC>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED SHIPPING WEIGHT",null,null,null,null,null,"rdl:RDS1658405211",null,"A <CALCULATED SHIPPING WEIGHT> is an <IndirectProperty> that refers to a <SHIPPING WEIGHT> which is calculated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED VALVE FLOW COEFFICIENT RANGE",null,null,null,null,null,"rdl:RDS7509196",null,"A <CALCULATED VALVE FLOW COEFFICIENT RANGE> is an <IndirectProperty> that is a valve flow coefficient range which is determined by calculations",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED VALVE FLOW COEFFICIENT",null,null,null,null,null,"rdl:RDS7508976",null,"A <CALCULATED VALVE FLOW COEFFICIENT> is an <IndirectProperty> that refers to a <VALVE FLOW COEFFICIENT> that is calculated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED WEIGHT",null,null,null,null,null,"rdl:RDS369044",null,"A <CALCULATED WEIGHT> is an <IndirectProperty> that refers to a <WEIGHT> which is calculated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED X COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT",null,null,null,null,null,"rdl:RDS14133310",null,"A <CALCULATED X COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT> is an <IndirectProperty> that refers to A <X COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT> of installed dry condition that is calculated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED Y COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT",null,null,null,null,null,"rdl:RDS14132995",null,"A <CALCULATED Y COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT> is an <IndirectProperty> that refers to a <Y COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT> of installed dry condition that is calculated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALCULATED Z COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT",null,null,null,null,null,"rdl:RDS14133040",null,"A <CALCULATED Z COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT> is an <IndirectProperty> that refers to a <Z COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT> of installed dry condition that is calculated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALIBRATED RANGE",null,null,null,null,null,"rdl:RDS1416382021",null,"A <CALIBRATED RANGE> is an <IndirectProperty> that is the value rsnge of the measured variable to which a device is actually adjusted to measure within a specified accuracy",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALIBRATED RANGE LOWER LIMIT",null,null,null,null,null,"rdl:RDS373635",null,"A <CALIBRATED RANGE LOWER LIMIT> is an <IndirectProperty> that is the lowest value of the measured variable to which a device is actually adjusted to measure within a specified accuracy",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALIBRATED RANGE UPPER LIMIT",null,null,null,null,null,"rdl:RDS373634",null,"A <CALIBRATED RANGE UPPER LIMIT> is an <IndirectProperty> that is the highest value of the measured variable to which a device is actually adjusted to measure within a specified accuracy",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALL INTENSITY",null,null,null,null,null,"rdl:RDS9999044",null,"A <CALL INTENSITY> is an <IndirectProperty> that refers to the <COUNT> of call attempts over a specified time interval",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"CALL INTENSITY",null,null,null,null,null,null,null,null,null,null,null,null,"COMPLETED CALL INTENSITY",null,null,null,null,null,"rdl:RDS9999055",null,"A <COMPLETED CALL INTENSITY is a <CALL INTENSITY> for the call attempts that result in the transmission of an answer signal as defined in ISO 80000-13. 8",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALORIFIC VALUE",null,null,null,null,null,"rdl:RDS13886193",null,"A <CALORIFIC VALUE> is an <IndirectProperty> that refers to the <ENERGY> contained in a <PhysicalObject>, determined by measuring the heat produced by the complete combustion of a specified quantity of it.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALORIFIC VALUE GAS VOLUME",null,null,null,null,null,"rdl:RDS350009",null,"A <CALORIFIC VALUE GAS VOLUME> is an <IndirectProperty> that refers to the amount of <HEAT ENERGY> in a standard <VOLUME> of <GAS>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALORIFIC VALUE MASS BASIS",null,null,null,null,null,"rdl:RDS350054",null,"A <CALORIFIC VALUE MASS BASIS> is an <IndirectProperty> that refers to the quantity of <HEAT ENERGY> in a standard <MASS> of the material",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALORIFIC VALUE MOLE BASIS",null,null,null,null,null,"rdl:RDS350099",null,"A <CALORIFIC VALUE MOLE BASIS> is an <IndirectProperty> that refers to the amount of <HEAT ENERGY> per unit <MOLE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CALORIFIC VALUE SOLID LIQUID VOL",null,null,null,null,null,"rdl:RDS350144",null,"A <CALORIFIC VALUE SOLID LIQUID VOL> is an <IndirectProperty> that refers to the amount of thermal energy in a <STANDARD VOLUME> of a <SOLID> or a <LIQUID>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CANONICAL PARTITION FUNCTION",null,null,null,null,null,"rdl:RDS389339",null,"A <CANONICAL PARTITION FUNCTION> is an <IndirectProperty> that applies to a canonical ensemble, in which a <SYSTEM> is allowed to exchange <HEAT> with the environment at fixed <TEMPERATURE> , volume, and number of particles as defined in ISO 80000-9 (2009) 9-40.2",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CARRIER LIFE TIME",null,null,null,null,null,"rdl:RDS397529",null,"A <CARRIER LIFE TIME> is an <IndirectProperty> that refers to a <DURATION> of recombination or trapping of minority charge carriers in semiconductors",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CHARACTERISTIC IMPEDANCE OF A MEDIUM",null,null,null,null,null,"rdl:RDS386909",null,"A <CHARACTERISTIC IMPEDANCE OF A MEDIUM> is an <IndirectProperty> that refers to at a point of in a non-dissipative medium and for a plane progressive wave, the quotient of a <SOUND PRESSURE> by the component of the sound particle <VELOCITY> in the direction of the wave propagation",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CHARACTERISTIC VOLUME",null,null,null,null,null,"rdl:RDS364679",null,"A <CHARACTERISTIC VOLUME> is an <IndirectProperty> that refers to a <VOLUME> that is a parameter used for calculation of <DENSITY>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CHARPY 2/3 ENERGY",null,null,null,null,null,"rdl:RDS13299130",null,"A <CHARPY 2/3 ENERGY> is an <IndirectProperty> that refers to an <IMPACT ENERGY> obtained from a Charpy fracture toughness test on a 2/3 size specimen",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CHARPY IMPACT U-NOTCH TEST ENERGY",null,null,null,null,null,"rdl:RDS13294060",null,"A <CHARPY IMPACT U-NOTCH TEST ENERGY> is an <IndirectProperty> that refers to an <IMPACT ENERGY> absorbed by the fracture in a charpy impact u-notch test",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CHARPY IMPACT V-NOTCH TEST ENERGY",null,null,null,null,null,"rdl:RDS13106286",null,"A <CHARPY IMPACT V-NOTCH TEST ENERGY> is an <IndirectProperty> that refers to an <IMPACT ENERGY> absorbed by the fracture in a charpy impact v-notch test",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CHEMICAL POTENTIAL OF B",null,null,null,null,null,"rdl:RDS388349",null,"A <CHEMICAL POTENTIAL OF B> is an <IndirectProperty> that refers to the rate of change of a free energy of a thermodynamic system with respect to the change in the number of atoms or molecules of the species that are added to the system; for a mixture of substances i mu_B = (deltaG/delta n_B)_Tau,p,n_i where G is Gibbs energy and n_B is the amount of substance B",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CIRCUMFERENTIAL POSITIONAL ACCURACY",null,null,null,null,null,"rdl:RDS13104157",null,"A <CIRCUMFERENTIAL POSITIONAL ACCURACY> is an <IndirectProperty> that refers to the <ACCURACY> that is the largest allowable deviation between a reported position and the actual position measured along a <CIRCUMFERENCE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CLOSING PRESSURE",null,null,null,null,null,"rdl:RDS7470101",null,"The CLOSING PRESSURE> is an <IndirectProperty> that refers to A <PRESSURE> at which a <VALVE> closes",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"COEFFICIENT OF HEAT TRANSFER",null,null,null,null,null,"rdl:RDS381959",null,"A <COEFFICIENT OF HEAT TRANSFER> is an <IndirectProperty> that refers to the <AREIC FLOW RATE> divided by thermodynamic <TEMPERATURE DIFFERENCE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"COERCIVITY",null,null,null,null,null,"rdl:RDS9999050",null,"A <COERCIVITY> is an <IndirectProperty> that refers to a <MAGNETIC FIELD STRENGTH> to be applied to bring a <MAGNETIC FLUX DENSITY> in a substance from its remaining <MAGNETIC FLUX DENSITY> to zero",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"COHERENCE LENGTH",null,null,null,null,null,"rdl:RDS398294",null,"A <COHERENCE LENGTH> is an <IndirectProperty> that refers to the <DISTANCE> in a superconductor over which the effect of a perturbation is appreciable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"COLD FILTER PLUGGING POINT",null,null,null,null,null,"rdl:RDS7353222",null,"A <COLD FILTER PLUGGING POINT> is an <IndirectProperty> that refers to the lowest <TEMPERATURE> at which a <FLUID> can flow through a standardised <FILTER>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"COLD LOCKED ROTOR TIME",null,null,null,null,null,"rdl:RDS6450064",null,"A <COLD LOCKED ROTOR TIME> is an <IndirectProperty> that refers to the maximum <DURATION> that a cold electric motor with a locked or jammed rotor (not having run for some time) can be fully switched on before its <TEMPERATURE> rises to the level at which the insulation is destroyed. Typically value is 10-14 seconds",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"COLD RECEPTOR THRESHOLD",null,null,null,null,null,"rdl:RDS9999051",null,"A <COLD RECEPTOR THRESHOLD> is an <IndirectProperty> that refers to the smallers difference of <TEMPERATURE> that is sensed by a <COLD RECEPTOR>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"COLOUR STIMULUS FUNCTION",null,null,null,null,null,"rdl:RDS9999052",null,"A <COLOUR STIMULUS FUNCTION> is an <IndirectProperty> that influences the quantification of the physiological color perception; it is calculated using the formula phi_lambda(lambda) = X_lambda(lambda) /R as defined in ISO 80000-7-42 (2009)",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"COMBINED NONEVAPORATIVE HEAT TRANSFER COFFICIENT",null,null,null,null,null,"rdl:RDS9999054",null,"A <COMBINED NONEVAPORATIVE HEAT TRANSFER COFFICIENT> is a <HEAT TRANSFER COEFFICIENT> as defined in ISO 80000-14-11.7",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"COMPRESSIBILITY",null,null,null,null,null,"rdl:RDS350234",null,"A <COMPRESSIBILITY> is an <IndirectProperty> that refers to a measure of the relative <VOLUME> change of a fluid or solid as a response to a <PRESSURE> or meA <MEAN STRESS> change tyoically kappa = -(1/V).dV/dP where V is volume and p pressure",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"COMPRESSION PRESSURE",null,null,null,null,null,"rdl:RDS13310920",null,"A <COMPRESSION PRESSURE> is an <IndirectProperty> that refers to the maximum <PRESSURE> that is the highest <PRESSURE> achieved during compression",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CONDITIONAL INFORMATION CONTENT",null,null,null,null,null,"rdl:RDS9999058",null,"A <CONDITIONAL INFORMATION CONTENT> is an <IndirectProperty> that refers to the <INFORMATION CONTENT> of event x under the condition that y has occurred: as defined in ISO/IEC 2382-16, item 16.04.02",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONSTANT FAILURE RATE PERIOD",null,null,null,null,null,"rdl:RDS14648495",null,"A <CONSTANT FAILURE RATE PERIOD> is an <IndirectProperty> that refers to a <PeriodInTime> in the life of a non-repaired item during which the failure rate is approximately constant",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CONTINUOUS CURRENT CAPACITY",null,null,null,null,null,"rdl:RDS14188580",null,"A <CONTINUOUS CURRENT CAPACITY> is an <IndirectProperty> that refers to a maximum <CURRENT> which can be carried continuously by a <CONDUCTOR> under specified conditions without its steady-state <TEMPERATURE> exceeding a specified value",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CONTROLLABLE VALVE FLOW COEFFICIENT",null,null,null,null,null,"rdl:RDS7509326",null,"A <CONTROLLABLE VALVE FLOW COEFFICIENT> is an <IndirectProperty> that refers to a <VALVE FLOW COEFFICIENT> that is the controllable <FLOW> of water which can be passed by a <VALVLE> when a <PRESSURE DROP> of 1 bar (actually 0,981bar) acts across it",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CONVENTIONAL TOUCH VOLTAGE LIMIT",null,null,null,null,null,"rdl:RDS407564",null,"A <CONVENTIONAL TOUCH VOLTAGE LIMIT> is an <IndirectProperty> that refers to a maximum value of a <TOUCH VOLTAGE> that is permitted to be maintained indefinitely in specified conditions of external influences",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"COOLING DUTY",null,null,null,null,null,"rdl:RDS350684",null,"A <COOLING DUTY> is an <IndirectProperty> that refers to the <RATE> at which sensible and latent heat must be removed from the space to maintain a constant space dry-bulb air temperature and humidity",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CORROSION ALLOWANCE",null,null,null,null,null,"rdl:RDS357344",null,"A <CORROSION ALLOWANCE> is an <IndirectProperty> that is a <THICKNESS> that is the upper limit of allowed corrosion of a metal structure",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CORROSION RATE",null,null,null,null,null,"rdl:RDS350729",null,"A <CORROSION RATE> is an <IndirectProperty> that refers to a <RATE> of decrease in thickness with respect to time",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CURRENT DENSITY OF PARTICLES",null,null,null,null,null,"rdl:RDS393164",null,"A <CURRENT DENSITY OF PARTICLES> is an <IndirectProperty> that refers to is a Vector quantity, the integral of whose normal component over any surface is equal to the net number N of particles passing through that surface in an infinitesimal time interval divided by its duration. Integral J.e_n.dA=dN/dt where e_n.dA is the vector surface element",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CURRENT IN A FAULT",null,null,null,null,null,"rdl:RDS408689",null,"A <CURRENT IN A FAULT> is an <IndirectProperty> that refers to is a <CURRENT> flowing through A <FAULT>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CURRENT IN THE SHORT CIRCUIT",null,null,null,null,null,"rdl:RDS408734",null,"A <CURRENT IN THE SHORT CIRCUIT> is an <IndirectProperty> that refers to is a <CURRENT> flowing through a <SHORT CIRCUIT>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CURRENT LINKAGE",null,null,null,null,null,"rdl:RDS383309",null,"A <CURRENT LINKAGE> is an <IndirectProperty> that refers to is the Net <ELECTRIC CURRENT> through a <SURFACE> delimited by a closed loop",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CURRENT WHEN ACTIVATED",null,null,null,null,null,"rdl:RDS7503900",null,"A <CURRENT WHEN ACTIVATED> is an <IndirectProperty> that refers to is an <ELECTRIC CURRENT> when a limit switch is activated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"CURRENT WHEN NOT ACTIVATED",null,null,null,null,null,"rdl:RDS7503945",null,"A <CURRENT WHEN NOT ACTIVATED> is an <IndirectProperty> that refers to is an <ELECTRIC CURRENT> when a limit switch is not activated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DATA COLLECTION PERIOD",null,null,null,null,null,"rdl:RDS14671950",null,"A <DATA COLLECTION PERIOD> is an <IndirectProperty> that refers to is the A <PERIOD> of time over which <DATA> has been collected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DAYS OF INDEPENDENT OPERATION",null,null,null,null,null,"rdl:RDS14663190",null,"A <DAYS OF INDEPENDENT OPERATION> is an <IndirectProperty> that refers to is a <PERIOD OF TIME> that is the number of days of independent operation without replenishment of spares",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DEAD TIME",null,null,null,null,null,"rdl:RDS409994",null,"A <DEAD TIME> is an <IndirectProperty> that refers to the <DURATION> of automatic reclosing when the power line or phase is not connected to any network voltage",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DEBYE ANGULAR FREQUENCY",null,null,null,null,null,"rdl:RDS398204",null,"A <DEBYE ANGULAR FREQUENCY> is an <IndirectProperty> that refers to is the cutoff <ANGULAR FREQUENCY> in the Debye model of the vibrational spectrum of a <SOLID>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DEBYE ANGULAR REPETENCY",null,null,null,null,null,"rdl:RDS396179",null,"A <DEBYE ANGULAR REPETENCY> is an <IndirectProperty> that refers to is the cutoff <ANGULAR WAVENUMBER> in the Debye model of the vibrational spectrum of a <SOLID>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DEBYE TEMPERATURE",null,null,null,null,null,"rdl:RDS396224",null,"A <DEBYE TEMPERATURE> is an <IndirectProperty> that refers to the <TEMPERATURE> of a crystal&#39;s highest normal mode of vibration, i.e., the highest temperature that can be achieved due to a single normal vibration. It is calculated as Theta_D = h~.omega_D / k where k is the <BOLTZMANN CONSTANT> and h~ is the <PLANCK CONSTANT> , divided by 2.pi, and omega_D is a <DEBYE ANGULAR FREQUENCY>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DEBYE-WALLER FACTOR",null,null,null,null,null,"rdl:RDS396044",null,"A <DEBYE-WALLER FACTOR> is an <IndirectProperty> that refers to the <FACTOR> by which the intensity of a diffraction line is reduced because of the lattice vibrations",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DEFECT DEPTH TOLERANCE 1",null,null,null,null,null,"rdl:RDS13299040",null,"A <DEFECT DEPTH TOLERANCE 1> is an <IndirectProperty> that refers to a <STRAIGHT LINEAR DISTANCE> which is A <DEPTH> tolerance applied to defects which have a <LENGTH> less than or equal to A <DEPTH> tolerance <LENGTH> limit",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DEFECT DEPTH TOLERANCE 2",null,null,null,null,null,"rdl:RDS13299085",null,"A <DEFECT DEPTH TOLERANCE 2> is an <IndirectProperty> that refers to a <STRAIGHT LINEAR DISTANCE> which is A <DEPTH> tolerance applied to defects which have a <LENGTH> greater than A <DEPTH> tolerance <LENGTH> limit",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DEFECT DEPTH TOLERANCE LENGTH LIMIT",null,null,null,null,null,"rdl:RDS13298995",null,"A <DEFECT DEPTH TOLERANCE LENGTH LIMIT> is an <IndirectProperty> that refers to a <STRAIGHT LINEAR DISTANCE> which is the boundary between defect lengths to which <DEPTH> tolerance 1 and <DEPTH> tolerance 2 are applied",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DELAY 1 (MEAN LOGISTIC - MLD)",null,null,null,null,null,"rdl:RDS14648900",null,"A <DELAY 1 (MEAN LOGISTIC - MLD)> is an <IndirectProperty> that refers to the <DURATION> of an expected logistic <DELAY>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DELAY 2 (MEAN ADMINISTRATIVE -MAD)",null,null,null,null,null,"rdl:RDS14648945",null,"A <DELAY 2 (MEAN ADMINISTRATIVE -MAD)> is an <IndirectProperty> that refers to the <DURATION> of an expected administrative <DELAY>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DELAY 3 (ADMINISTRATIVE - CORRECTIVE MAINTENANCE)",null,null,null,null,null,"rdl:RDS14648990",null,"A <DELAY 3 (ADMINISTRATIVE - CORRECTIVE MAINTENANCE)> is an <IndirectProperty> that refers to the <DURATION>of the accumulated time during which an action of corrective maintenance on a faulty item is not performed due to administrative reasons",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DENSITY AT LOWER LIMIT DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS8276009",null,"A <DENSITY AT LOWER LIMIT DIFFERENTIAL PRESSURE> is an <IndirectProperty> that refers to a <DENSITY> at a <LOWER LIMIT DIFFERENTIAL PRESSURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DENSITY AT LOWER LIMIT FLOW RATE",null,null,null,null,null,"rdl:RDS7298282",null,"A <DENSITY AT LOWER LIMIT FLOW RATE> is an <IndirectProperty> that refers to a <DENSITY> at flow condition at a lower limit of a <FLOW RATE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DENSITY AT NORMAL DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS8276054",null,"A <DENSITY AT NORMAL DIFFERENTIAL PRESSURE> is an <IndirectProperty> that refers to a <DENSITY> at flow condition at a normal <DIFFERENTIAL PRESSURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DENSITY AT NORMAL FLOW RATE",null,null,null,null,null,"rdl:RDS7298220",null,"A <DENSITY AT NORMAL FLOW RATE> is an <IndirectProperty> that refers to a <DENSITY> at a normal operating <FLOW RATE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DENSITY AT UPPER LIMIT DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS8276144",null,"A <DENSITY AT UPPER LIMIT DIFFERENTIAL PRESSURE> is an <Indirect Property> that is a <DENSITY> at a lower limit of a <DIFFERENTIAL PRESSURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DENSITY AT UPPER LIMIT FLOW RATE",null,null,null,null,null,"rdl:RDS7298344",null,"A <DENSITY AT UPPER LIMIT FLOW RATE> is an <IndirectProperty> that refers to a <DENSITY> at flow condition at an upper limit <FLOW RATE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DENSITY GRADIENT",null,null,null,null,null,"rdl:RDS1065668921",null,"A <DENSITY GRADIENT> is an <IndirectProperty> that refers to a variation in <DENSITY> of a solution caused by a change in <CONCENTRATION> of a solute in a confined solution",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DENSITY OF STATES",null,null,null,null,null,"rdl:RDS396494",null,"A <DENSITY OF STATES> (DOS) is an <IndirectProperty> that he number of different states at a particular energy level that electrons are allowed to occupy, i.e. the number of electron states per unit volume per unit energy. It is calculated as rho(E) = n_E(E) = (dN(E)/dE).(1/V) where N(E) is the total number of states with energy less than E, and V is <VOLUME>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DESIGN PRESSURE",null,null,null,null,null,"rdl:RDS1470835011",null,"A <DESIGN PRESSURE> is an <IndirectProperty> that is the pressure at the most severe condition of coincident internal or external pressure and temperature (minimum or maximum) expected during service. It is subject to the rules of the applicable code relating to allowances for variations of pressure or temperature or both",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"DESIGN PRESSURE",null,null,null,null,null,null,null,null,null,null,null,null,"OUTLET DESIGN PRESSURE",null,null,null,null,null,"rdl:RDS7471401",null,"An <OUTLET DESIGN PRESSURE> is a <DESIGN PRESSURE> at an <OUTLET>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DESIGN TEMPERATURE",null,null,null,null,null,"rdl:RDS357164",null,"A <DESIGN TEMPERATURE> is an <IndirectProperty> that refers to a <TEMPERATURE>that an object is designed to withstand",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"DESIGN TEMPERATURE",null,null,null,null,null,null,null,null,null,null,null,null,"OUTLET DESIGN TEMPERATURE",null,null,null,null,null,"rdl:RDS7471243",null,"An <OUTLET DESIGN TEMPERATURE> is a <DESIGN TEMPERATURE> at an <OUTLET>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DESIGNATED SPEED",null,null,null,null,null,"rdl:RDS8797566",null,"A <DESIGNATED SPEED> is an <IndirectProperty> that refers to a <ROTATIONAL SPEED> designated for an electric rotating machine",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DETECTION EQUIPMENT COUNT",null,null,null,null,null,"rdl:RDS7054598",null,"A <DETECTION EQUIPMENT COUNT> is an <IndirectProperty> that refers to a <COUNT> of the number of detection equipment within a defined boundary",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DEW POINT",null,null,null,null,null,"rdl:RDS7353160",null,"A <DEW POINT> is an <IndirectProperty> that refers to a <TEMPERATURE> at which condensation of vapour in gas takes place",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DIELECTRIC CONSTANT LOWER LIMIT",null,null,null,null,null,"rdl:RDS1470026581",null,"A <DIELECTRIC CONSTANT LOWER LIMIT> is an <IndirectProperty> that refers to a minimum allowable <DIELECTRIC CONSTANT>.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DIELECTRIC CONSTANT OF FLUID IN LOWER PHASE",null,null,null,null,null,"rdl:RDS7967048",null,"A <DIELECTRICITY, FLUID IN LOWER PHASE> is an <IndirectProperty> that refers to a <DIELECTRIC CONSTANT> of a fluid in the lower phase",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DIELECTRIC CONSTANT OF FLUID IN UPPER PHASE",null,null,null,null,null,"rdl:RDS7967093",null,"A <DIELECTRICITY, FLUID IN UPPER PHASE> is an <IndirectProperty> that refers to a <DIELECTRIC CONSTANT> of a fluid in the upper phase",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL PRESSURE AT NORMAL MASS FLOW RATE",null,null,null,null,null,"rdl:RDS14251355",null,"A <DIFFERENTIAL PRESSURE AT NORMAL MASS FLOW RATE> is an <IndirectProperty> that refers to a <DIFFERENTIAL PRESSURE> that occurs at <NORMAL MASS FLOW RATE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL PRESSURE AT UPPER LIMIT MASS FLOW RATE",null,null,null,null,null,"rdl:RDS14251445",null,"A <DIFFERENTIAL PRESSURE AT UPPER LIMIT MASS FLOW RATE> is an <IndirectProperty> that refers to a <DIFFERENTIAL PRESSURE> that occurs at <UPPER LIMIT MASS FLOW RATE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DIFFUSION AREA",null,null,null,null,null,"rdl:RDS394289",null,"A <DIFFUSION AREA> is an <IndirectProperty> that refers to an infinite homogeneous medium, one-sixth of the mean square <DISTANCE> between the point where a neutron enters a specified class and the point where it leaves this class",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DIFFUSION LENGTH",null,null,null,null,null,"rdl:RDS394424",null,"A <DIFFUSION LENGTH> is an <IndirectProperty> that refers to the <AVERAGE LENGTH> a carrier moves between generation and recombination",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DIRECTION OF EXPLOSION",null,null,null,null,null,"rdl:RDS7051659",null,"A <DIRECTION OF EXPLOSION> is an <IndirectProperty> that refers to the <DIRECTION> of an explosion given in a referance system",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DIRECTION OF FIRE",null,null,null,null,null,"rdl:RDS7051164",null,"A <DIRECTION OF FIRE> is an <IndirectProperty> that refers to the <DIRECTION> of a fire given in a reference system",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DIRECTION OF FLOW",null,null,null,null,null,"rdl:RDS12144470",null,"A <DIRECTION OF FLOW> is an <IndirectProperty> that refers to the <DIRECTION>of a flow given in a referance system",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DIRECTION OF MOVEMENT",null,null,null,null,null,"rdl:RDS16680869",null,"A <DIRECTION OF MOVEMENT> is an <IndirectProperty> that refers to the <DIRECTION> of a movement given in a reference system",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DISTRIBUTION LOSS",null,null,null,null,null,"rdl:RDS14188085",null,"A <DISTRIBUTION LOSS> is an <IndirectProperty> that refers to a <LOSS> due to transport or distribution of electricital energy, heat, natural gas and derived gases. It also includes flaring of manufactured gases as well as pipeline losses",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DONOR NUMBER DENSITY",null,null,null,null,null,"rdl:RDS397349",null,"A <DONOR NUMBER DENSITY> is an <IndirectProperty> that refers to a <COUNT> per <VOLUME> of donor levels",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DOSE EQUIVALENT",null,null,null,null,null,"rdl:RDS395099",null,"A <DOSE EQUIVALENT> is an <IndirectProperty> that refers to an estimate of the biological effect of a <DOSE> of ionizing radiation, calculated by multiplying the dose received by a factor depending on the type of radiation. It is measured in sieverts",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"DYNAMIC HEAD",null,null,null,null,null,"rdl:RDS2220949",null,"A <DYNAMIC HEAD> is an <IndirectProperty> that represents the energy of the fluid due to its bulk motion",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EFFECTIVE MASS",null,null,null,null,null,"rdl:RDS397394",null,"An <EFFECTIVE MASS> is an <IndirectProperty> that refers to the <MASS> that a particle seems to have when responding to forces, or the mass that it seems to have when interacting with other identical particles in a thermal distribution",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EFFICIENCY AT RATED FLOW",null,null,null,null,null,"rdl:RDS14152685",null,"An <EFFICIENCY AT RATED FLOW> is an <EFFICIENCY> at rated flow",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ENERGY LOSS",null,null,null,null,null,"rdl:RDS5965024",null,"An <ENERGY LOSS> is an <IndirectProperty> that refers to a time integral of <POWER LOSS>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ENERGY SHORTFALL",null,null,null,null,null,"rdl:RDS5965148",null,"An <ENERGY SHORTFALL> is an <IndirectProperty> that refers to an <ENERGY> that is lacking with respect to the energy demand over a stated <PeriodInTime>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EQUILIBRIUM CONSTANT ON A CONCENTRATION BASIS",null,null,null,null,null,"rdl:RDS9999102",null,"An <EQUILIBRIUM CONSTANT ON A CONCENTRATION BASIS> is an <IndirectProperty> that refers to An <NUMBER> K that expresses the relationship between the amounts of products and reactants present at equilibrium in a reversible chemical reaction at a given <TEMPERATURE> for solutions as defined in ISO 80000-9 (2009) 9-35",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EQUILIBRIUM CONSTANT ON A PRESSURE BASIS",null,null,null,null,null,"rdl:RDS9999103",null,"An <EQUILIBRIUM CONSTANT ON A PRESSURE BASIS> is an <IndirectProperty> that refers to An <NUMBER> K that expresses the relationship between the amounts of products and reactants present at equilibrium in a reversible chemical reaction at a given <TEMPERATURE> for gases as defined in ISO 80000-9 (2009) 9-34",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EQUIVALENT ABSORPTION AREA OF A SURFACE OR OBJECT",null,null,null,null,null,"rdl:RDS387314",null,"An <EQUIVALENT ABSORPTION AREA OF A SURFACE OR OBJECT> is an <IndirectProperty> that, in a diffuse sound field, refers to an <AREA> of a surface having An <ABSORPTION FACTOR> equal to 1, which, if diffraction effects are neglected, would, in the same diffuse sound field, absorb the same power",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EQUIVALENT BINARY",null,null,null,null,null,"rdl:RDS9999104",null,"An <EQUIVALENT BINARY> is an <Indirectproperty> that refers to the minimum storage capacity of a bit-organized storage device which would contain the amount of data in the given storage device and is equal to the smallest integer greater than or equal to the equivalent binary storage capacity as defined in ISO 80000-13 (2009) 13-10",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EQUIVALENT BINARY DIGIT RATE",null,null,null,null,null,"rdl:RDS9999105",null,"An <EQUIVALENT BINARY DIGIT RATE> is a <BINARY DIGIT RATE> which is equivalent to An <TRANSFER RATE> for the specified data elements as defined in ISO 80000-13 (2009) 13-15",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"Property",null,null,null,null,null,null,null,null,null,null,null,"EQUIVALENT PER MASS",null,null,null,null,null,"rdl:RDS17234502",null,"An <EQUIVALENT PER MASS> is an <IndirectProperty> that refers to a concept of property that is an equivalent divided by mass",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EQUIVOCATION",null,null,null,null,null,"rdl:RDS9999106",null,"An <EQUIVOCATION> is an <IndirectProperty> that refers to a conditional <ENTROPY> of a set X of emitted characters given the set Y of received characters as defined in ISO 80000-13 (2009) 13-33",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EROSION RATE",null,null,null,null,null,"rdl:RDS16757892",null,"An <EROSION RATE> is an <IndirectProperty> that refers to An <RATE> of decrease in <THICKNESS> caused by erosion with respect to time",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ERROR",null,null,null,null,null,"rdl:RDS13886943",null,"An <ERROR> is an <IndirectProperty> that refers to a quantity by which a result obtained by observation or by calculation differs from an accurate determination",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED AGE",null,null,null,null,null,"rdl:RDS13106162",null,"An <ESTIMATED AGE> is an <IndirectProperty> that refers to an estimated <AGE> of a person or a thing",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED AUXILIARIES WEIGHT",null,null,null,null,null,"rdl:RDS14133895",null,"An <ESTIMATED AUXILIARIES WEIGHT> is an <IndirectProperty> that refers to an auxiliaries <WEIGHT> which is estimated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED AVERAGE HEIGHT",null,null,null,null,null,"rdl:RDS8655939",null,"An <ESTIMATED AVERAGE HEIGHT> is an <IndirectProperty> that refers to An <AVERAGE HEIGHT> that is established by an estimate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED DRY WEIGHT",null,null,null,null,null,"rdl:RDS7285516",null,"An <ESTIMATED DRY WEIGHT> is an <IndirectProperty> that refers to An <DRY WEIGHT> that is estimated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED ERROR",null,null,null,null,null,"rdl:RDS13886898",null,"An <ESTIMATED ERROR> is an <IndirectProperty> that refers to an error that is estimated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED INVENTORY WEIGHT",null,null,null,null,null,"rdl:RDS14133940",null,"An <ESTIMATED INVENTORY WEIGHT> is an <IndirectProperty> that refers to an <INVENTORY WEIGHT> which is estimated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED OVERALL HEIGHT",null,null,null,null,null,"rdl:RDS14134075",null,"An <ESTIMATED OVERALL HEIGHT> is an <IndirectProperty> that refers to an <OVERALL HEIGHT> which is estimated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED OVERALL LENGTH",null,null,null,null,null,"rdl:RDS14133985",null,"An <ESTIMATED OVERALL LENGTH> is an <IndirectProperty> that refers to an <OVERALL LENGTH> which is estimated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED OVERALL WIDTH",null,null,null,null,null,"rdl:RDS14134030",null,"An <ESTIMATED OVERALL WIDTH> is an <IndirectProperty> that refers to an overall <WIDTH> which is estimated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED RESERVOIR PORE PRESSURE",null,null,null,null,null,"rdl:RDS17847285",null,"An <ESTIMATED RESERVOIR PORE PRESSURE> is an <IndirectProperty> that refers to An <RESERVOIR PORE PRESSURE> that is based on estimates",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED SHIPPING WEIGHT",null,null,null,null,null,"rdl:RDS1658417191",null,"An <ESTIMATED SHIPPING WEIGHT> is an <IndirectProperty> that refers to An <SHIPPING WEIGHT> that has been estimated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED SURGE FLOW AT ROTATIONAL SPEED",null,null,null,null,null,"rdl:RDS14259770",null,"An <ESTIMATED SURGE FLOW AT ROTATIONAL SPEED> is an <IndirectProperty> that refers to An <VOLUME FLOW RATE> at An <ROTATIONAL SPEED> at which surging is estimated to occur",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED WEIGHT",null,null,null,null,null,"rdl:RDS367514",null,"An <ESTIMATED WEIGHT> is an <IndirectProperty> that refers to a <WEIGHT> based on estimates",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED X COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT",null,null,null,null,null,"rdl:RDS14134120",null,"An <ESTIMATED X COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT> is an <IndirectProperty> that refers to an <X COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT> of installed dry condition that is estimated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED Y COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT",null,null,null,null,null,"rdl:RDS14134165",null,"An <ESTIMATED Y COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT> is an <IndirectProperty> that refers to a <Y COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT> of installed dry condition that is estimated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ESTIMATED Z COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT",null,null,null,null,null,"rdl:RDS14133670",null,"An <ESTIMATED Z COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT> is an <IndirectProperty> that refers to a <Z COORDINATE FOR CENTRE OF GRAVITY RELATIVE TO LOCAL DATUM POINT>of installed dry condition that is estimated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EVAPORATION POINT",null,null,null,null,null,"rdl:RDS7352957",null,"An <EVAPORATION POINT> is an <IndirectProperty> that refers to An <TEMPERATURE> at which <EVAPORATION> starts when a liquid object is heated",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EXCHANGE INTEGRAL",null,null,null,null,null,"rdl:RDS397619",null,"An <EXCHANGE INTEGRAL> is an <IndirectProperty> that refers to a constituent of the interaction <ENERGY> between the spins of adjacent electrons in matter arising from the overlap of electron state functions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EXTERNAL DESIGN PRESSURE",null,null,null,null,null,"rdl:RDS7311195",null,"An <EXTERNAL DESIGN PRESSURE> is an <IndirectProperty> that refers to a <DESIGN PRESSURE> acting on the external surface of an object",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"PRESSURE",null,null,null,null,null,null,null,null,null,null,null,"EXTERNAL PRESSURE",null,null,null,null,null,"rdl:RDS7343982",null,"An <EXTERNAL PRESSURE> is a <PRESSURE> that is acting on the external surface of an object",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EXTERNAL THREAD LOWER LIMIT MAJOR DIAMETER",null,null,null,null,null,"rdl:RDS370394",null,"An <EXTERNAL THREAD LOWER LIMIT MAJOR DIAMETER> is an <IndirectProperty> that refers to an <EXTERNAL THREAD MAJOR DIAMETER> minus <EXTERNAL THREAD ALLOWANCE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EXTERNAL THREAD LOWER LIMIT MINOR DIAMETER",null,null,null,null,null,"rdl:RDS370979",null,"An <EXTERNAL THREAD LOWER LIMIT MINOR DIAMETER> is an <IndirectProperty> that equals <EXTERNAL THREAD LOWER LIMIT PITCH DIAMETER> minus 0.649519P",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EXTERNAL THREAD LOWER LIMIT PITCH DIAMETER",null,null,null,null,null,"rdl:RDS370844",null,"An <EXTERNAL THREAD LOWER LIMIT PITCH DIAMETER> is an <IndirectProperty> that equals <EXTERNAL THREAD UPPER LIMIT PITCH DIAMETER> minus <EXTERNAL THREAD PITCH DIAMETER TOLERANCE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EXTERNAL THREAD MAJOR DIAMETER TOLERANCE",null,null,null,null,null,"rdl:RDS370439",null,"An <EXTERNAL THREAD MAJOR DIAMETER TOLERANCE> is an <IndirectProperty> that refers to the tolerance applicable to an <EXTERNAL THREAD MAJOR DIAMETER>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EXTERNAL THREAD PITCH DIAMETER TOLERANCE",null,null,null,null,null,"rdl:RDS370619",null,"An <EXTERNAL THREAD PITCH DIAMETER TOLERANCE> is an <IndirectProperty> that refers to the tolerance applicable to an <EXTERNAL THREAD PITCH DIAMETER>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EXTERNAL THREAD UPPER LIMIT MAJOR DIAMETER",null,null,null,null,null,"rdl:RDS370349",null,"An <EXTERNAL THREAD UPPER LIMIT MAJOR DIAMETER> is an <IndirectProperty> that refers to An <BASIC THREAD MAJOR DIAMETER> minus <EXTERNAL THREAD ALLOWANCE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"EXTERNAL THREAD UPPER LIMIT PITCH DIAMETER",null,null,null,null,null,"rdl:RDS370799",null,"An <EXTERNAL THREAD UPPER LIMIT PITCH DIAMETER> is an <IndirectProperty> that equals the <BASIC THREAD PITCH DIAMETER> minus the <EXTERNAL THREAD ALLOWANCE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FAILURE PROBABILITY",null,null,null,null,null,"rdl:RDS14643516",null,"A <FAILURE PROBABILITY> is an <IndirectProperty> that refers to a <PROBABILITY of failure",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FAILURE RATE",null,null,null,null,null,"rdl:RDS7068695",null,"A <FAILURE RATE> is an <IndirectProperty> that refers to a <RATE> of failure occurences",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FATIGUE LIMIT",null,null,null,null,null,"rdl:RDS366434",null,"A <FATIGUE LIMIT> is an <IndirectProperty> that refers to a stress limit which is the maximum repeated stress a material can take without breaking, regardless of the number of applied stress cycles. (Ref S-N diagram). For steel that number of cycles are normally set to 10 exp 7",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FERMI ANGULAR REPETENCY",null,null,null,null,null,"rdl:RDS396134",null,"A <FERMI ANGULAR REPETENCY> is an <IndirectProperty> that refers to an <ANGULAR WAVENUMBER> of electrons in states on the Fermi sphere",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"TEMPERATURE",null,null,null,null,null,null,null,null,null,null,null,"FIRE POINT",null,null,null,null,null,"rdl:RDS7353594",null,"A <FIRE POINT> is a <TEMPERATURE> that is defined in ISO 1998 def. 2-015",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FISCAL MEASURED AMOUNT",null,null,null,null,null,"rdl:RDS411745871",null,"A <FISCAL MEASURED AMOUNT> is an <IndiredProperty> that refers to an <AMOUNT> that is generated throug a certified measuring device and has an impact on company revenue and government taxation",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLAME DETECTOR RESPONSE DISTANCE",null,null,null,null,null,"rdl:RDS7469160",null,"A <FLAME DETECTOR RESPONSE DISTANCE> is an <IndirectProperty> that refers to a <STRAIGHT LINEAR DISTANCE> that is the largest distance at which a <FLAME DETECTOR> detects a 1 square feet flame",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"FLOW MEASURING RANGE",null,null,null,null,null,"rdl:RDS7482596",null,"A <FLOW MEASURING RANGE> is an <FLOW RANGE> that is the flow range an instrument is designed to measure",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW RATE AT LOWER LIMIT DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS8276899",null,"A <FLOW RATE AT LOWER LIMIT DIFFERENTIAL PRESSURE> is an <IndirectProperty> that refers to a <VOLUME FLOW RATE> at a lower limit <DIFFERENTIAL PRESSURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW RATE AT LOWER LIMIT FLOW",null,null,null,null,null,"rdl:RDS8276234",null,"A <FLOW RATE AT LOWER LIMIT FLOW> is an <IndirectProperty> that refers to a <VOLUME FLOW RATE> at lower limit flow",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW RATE AT NORMAL DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS8276549",null,"A <FLOW RATE AT NORMAL DIFFERENTIAL PRESSURE> is an <IndirectProperty> that refers to a <VOLUME FLOW RATE> at normal <DIFFERENTIAL PRESSURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW RATE AT UPPER LIMIT DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS8276189",null,"A <FLOW RATE AT UPPER LIMIT DIFFERENTIAL PRESSURE> is an <IndirectProperty> that refers to a <VOLUME FLOW RATE> at an upper limit <DIFFERENTIAL PRESSURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLUID YIELD POINT",null,null,null,null,null,"rdl:RDS17684485",null,"A <FLUID YIELD POINT> is an <IndirectProperty> that refers to the <STRESS> required to a start fluid movement",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FUEL CONSUMPTION",null,null,null,null,null,"rdl:RDS352034",null,"A <FUEL CONSUMPTION> is an <IndirectProperty> that refers to a <FLOW RATE> of <FUEL> that is consumed by a given <PhysicalObject>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FUEL MILEAGE",null,null,null,null,null,"rdl:RDS352079",null,"A <FUEL MILEAGE> is an <IndirectProperty> that refers to a <DISTANCE> travelled by a vehicle per <VOLUME> of fuel",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FUGACITY OF B",null,null,null,null,null,"rdl:RDS388484",null,"A <FUGACITY OD B> of a real gas is an <IndirectProperty> that refers to an effective <PARTIAL PRESSURE> that replaces the mechanical <PARTIAL PRESSURE> in an accurate computation of the chemical equilibrium constant. It is equal to the pressure of an ideal gas which has the same chemical potential as the real gas. For a for a gaseous mixture it is calculated as p~_B is proportional to the absolute activity lambda_B, the proportionality factor, which is a function of <TEMPERATURE> only, being determined by the condition that at constant <TEMPERATURE> and composition p_B/p~_B tends to 1 for an indefinitely dilute gas",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS LIFT VOLUME AVERAGED",null,null,null,null,null,"rdl:RDS16623732",null,"A <GAS LIFT VOLUME AVERAGED> is an <IndirectProperty> that refers to an average volume of a gas lift system",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"RATIO(math)",null,null,null,null,null,null,null,null,null,null,null,"GAS OIL RATIO AT STANDARD CONDITIONS",null,null,null,null,null,"rdl:RDS17034450",null,"A <GAS OIL RATIO AT STANDARD CONDITIONS> is a <RATIO> of dissolved gas compared to the amount of oil at a given temperature and pressure",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"GAS OIL RATIO AT STANDARD CONDITIONS",null,null,null,null,null,null,null,null,null,null,null,null,"GAS-OIL RATIO FOR EXPORT AT STANDARD CONDITIONS",null,null,null,null,null,"rdl:RDS16872001",null,"A <GAS-OIL RATIO FOR EXPORT AT STANDARD CONDITIONS> is a <GAS OIL RATIO AT STANDARD CONDITIONS> at standard conditions that is the ratio of the exported gas volume and the oil volume. Both volume flow rates should be converted to the same pressure and temperature (generally to standard conditions, i.e. 15 deg. C and 1 atm)",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GAS VOLUME",null,null,null,null,null,"rdl:RDS16227880",null,"A <GAS VOLUME> is an <IndirectProperty> that refers to a <VOLUME> of gas at 1.013 bar and boiling point",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GEAR INPUT SHAFT RATED ROTATIONAL SPEED",null,null,null,null,null,"rdl:RDS13233683",null,"A <GEAR INPUT SHAFT RATED ROTATIONAL SPEED> is an <IndirectProperty> that refers to a <RATED ROTATIONAL SPEED> induced on a gear input shaft at full load",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GEAR INPUT SHAFT RATED TORQUE",null,null,null,null,null,"rdl:RDS13233948",null,"A <GEAR INPUT SHAFT RATED TORQUE> is an <IndirectProperty> that refers to a <RATED TORQUE> induced on a gear input shaft at full load",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GEAR INPUT SHAFT UPPER LIMIT ROTATIONAL SPEED",null,null,null,null,null,"rdl:RDS13233824",null,"A <GEAR INPUT SHAFT UPPER LIMIT ROTATIONAL SPEED> is an <IndirectProperty> that refers to an <UPPER LIMIT ROTATIONAL SPEED> induced on a gear input shaft",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GEAR INPUT SHAFT UPPER LIMIT TORQUE",null,null,null,null,null,"rdl:RDS13234072",null,"A <GEAR INPUT SHAFT UPPER LIMIT TORQUE> is an <IndirectProperty> that refers to an <UPPER LIMIT TORQUE> induced on a gear input shaft",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GEAR OUTPUT SHAFT RATED ROTATIONAL SPEED",null,null,null,null,null,"rdl:RDS13233745",null,"A <GEAR OUTPUT SHAFT RATED ROTATIONAL SPEED> is an <IndirectProperty> that refers to a <RATED ROTATIONAL SPEED> transmitted from a gear output shaft at full load",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GEAR OUTPUT SHAFT RATED TORQUE",null,null,null,null,null,"rdl:RDS13234010",null,"A <GEAR OUTPUT SHAFT RATED TORQUE> is an <IndirectProperty> that refers to a <RATED TORQUE> transmitted from a gear output shaft at full load",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GEAR OUTPUT SHAFT UPPER LIMIT ROTATIONAL SPEED",null,null,null,null,null,"rdl:RDS13233886",null,"A <GEAR OUTPUT SHAFT UPPER LIMIT ROTATIONAL SPEED> is an <IndirectProperty> that refers to an <UPPER LIMIT ROTATIONAL SPEED> transmitted from a gear output shaft",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GEAR OUTPUT SHAFT UPPER LIMIT TORQUE",null,null,null,null,null,"rdl:RDS13234134",null,"A <GEAR OUTPUT SHAFT UPPER LIMIT TORQUE> is an <IndirectProperty> that refers to an <UPPER LIMIT TORQUE> transmitted from a gear output shaft",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GENERATED HEAT",null,null,null,null,null,"rdl:RDS403964",null,"A <GENERATED HEAT> is an <IndirectProperty> that refers to <ENERGY> in the form of <HEAT <ENERGY> (J) that is transformed from another <ENERGY> form in a time interval (s)",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GROSS AVERAGE HEAT RATE",null,null,null,null,null,"rdl:RDS14524160",null,"A <GROSS AVERAGE HEAT RATE> is an <IndirectProperty> that refers to a <RATIO> of the <THERMAL ENERGY> of the fuel consumed to the gross <ELECTRIC ENERGY> generated by a unit during the same <PeriodInTime>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GROSS CALORIFIC VALUE",null,null,null,null,null,"rdl:RDS13886283",null,"A <GROSS CALORIFIC VALUE> is an <IndirectProperty> that refers to a <CALORIFIC VALUE> of the heat evolved when all of the products of combustion are cooled to atmospheric <TEMPERATURE> and <PRESSURE> as in a bomb calorimeter",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GROSS HEATING VALUE",null,null,null,null,null,"rdl:RDS365084",null,"A <GROSS HEATING VALUED> is an <IndirectProperty> that refers to the total <HEAT> needed for heating a <PhysicalObject> from one <TEMPERATURE> to another",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GROSS OIL MASS",null,null,null,null,null,"rdl:RDS16711465",null,"A <GROSS OIL MASS> is an <IndirectProperty> that refers to a <MASS> that is the total <MASS> of all petroleum liquids and sediments and water, excluding free water, corrected by the appropriate volume correction factor (Ci1) for the observed <TEMPERATURE> and API gravity, relative density, or <DENSITY> to a standard <TEMPERATURE> such as 60 deg. F or 15 deg. C and also corrected by the applicable <PRESSURE> correction factor (Cp1) and meter factor",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GROSS OUTPUT OF A POWER STATION",null,null,null,null,null,"rdl:RDS14188265",null,"A <GROSS OUTPUT OF A POWER STATION> is an <IndirectProperty> that refers to the electrical <POWER> produced at the terminals of the main and auxiliary generators of a <POWER>station",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GROSS STANDARD OIL VOLUME",null,null,null,null,null,"rdl:RDS16711735",null,"A <GROSS STANDARD OIL VOLUME> is an <IndirectProperty> that refers to a <TOTAL VOLUME> of all petroleum liquids and sediments and water, excluding free water, corrected by the appropriate volume correction factor (Ci1) for the observed <TEMPERATURE> and API gravity, relative density, or density to a standard <TEMPERATURE> such as 60 deg. F or 15 deg. C and also corrected by the applicable <PRESSURE> correction factor (Cp1) and meter factor",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GUARANTEED INNER OIL LEAKAGE RATE",null,null,null,null,null,"rdl:RDS14285175",null,"A <GUARANTEED INNER OIL LEAKAGE RATE> is an <IndirectProperty> that refers to a maximum <INNER OIL LEAKAGE RATE> that is guaranteed at the shaft (or seal)",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"GUARANTEED PRESSURE RISE TO SURGE",null,null,null,null,null,"rdl:RDS14259545",null,"A <GUARANTEED PRESSURE RISE TO SURGE> is an <IndirectProperty> that refers to a <PRESSURE RISE> from normal conditions to where the supplier can guarantee no surge",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"HAMILTONIAN FUNCTION",null,null,null,null,null,"rdl:RDS9999131",null,"A <HAMILTONIAN FUNCTION> of a system is an <IndirectProperty> that refers to its total <ENERGY> that is the sum of its <KINETIC ENERGY> and its <POTENTIAL ENERGY> in terms of the Lagrangian function derived in earlier studies of dynamics and of the position and momentum of each of the particles",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"HARDNESS",null,null,null,null,null,"rdl:RDS366344",null,"A <HARDNESS> is an <IndirectProperty> that refers to an <INDENTATION RESISTANCE> possessed by a substance",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"HEAD",null,null,null,null,null,"rdl:RDS362609",null,"A <HEAD> is an <IndirectProperty> that relates the <ENERGY> in an incompressible <FLUID> to the <HEIGHT> of an equivalent static column of that fluid.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"HEAT OF FUSION AT FREEZING POINT",null,null,null,null,null,"rdl:RDS364769",null,"A <HEAT OF FUSION AT FREEZING POINT> is an <IndirectProperty> that refers to the <THERMAL ENERGY> needed to convert a substance from liquid form to solid form or vice versa",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"HOT LOCKED ROTOR TIME",null,null,null,null,null,"rdl:RDS6450157",null,"A <HOT LOCKED ROTOR TIME> is an <IndirectProperty> that refers to a <DURATION> in which a hot electric motor (recently been run for some time) can be fully switched on when the rotor is locked or jammed before its temperature rises to the level at which the insulation is destroyed. Typical value is 7-10 seconds",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"HUB ANGLE UPPER LIMIT",null,null,null,null,null,"rdl:RDS368054",null,"A <HUB ANGLE UPPER LIMIT> is an <IndirectProperty> that refers to a hub <ANGLE> which is the largest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"HYDROSTATIC TEST PRESSURE PERCENT SMYS",null,null,null,null,null,"rdl:RDS13298770",null,"A <> is an <IndirectProperty> that refers to a hydrostatic test level defined in terms of pipeline hoop stress as a percentage of Specified Minimum Yield Strength (SMYS)",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"HYPERFINE STRUCTURE QUANTUM NUMBER",null,null,null,null,null,"rdl:RDS391544",null,"A <HYPERFINE STRUCTURE QUANTUM NUMBER> is an <IndirectProperty> that refers to a <QUANTUM NUMBER> of an atom describing inclination of the nuclear spin with respect to a quantization axis given by the magnetic field produced by the orbital electrons",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INFINITE MEDIUM MULTIPLICATION FACTOR",null,null,null,null,null,"rdl:RDS394784",null,"An <INFINITE MEDIUM MULTIPLICATION FACTOR> is an <IndirectProperty> that refers to An <MULTIPLICATION FACTOR> for an infinite medium or for an infinite repeating lattice",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INHERENT AVAILABILITY (AI)",null,null,null,null,null,"rdl:RDS14649125",null,"An <INHERENT AVAILABILITY (AI)> is an <IndirectProperty> that refers to the <PROBABILITY> that a system or equipment, when used under stated conditions in an ideal support environment (i.e., readily available tools, spares, maintenance personnel, etc.), will operate satisfactorily at any point in time as required",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INPUT TO STORAGE",null,null,null,null,null,"rdl:RDS4989931926",null,"An <INPUT TO STORAGE> is an <IndirectProperty> that refers to An <VOLUME>, <MASS> or <ENERGY> of a product that has been added to the stock within the report <PERIOD>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INRUSH CURRENT HALF PEAK VALUE TIME",null,null,null,null,null,"rdl:RDS413009",null,"An <INRUSH CURRENT HALF PEAK VALUE TIME> is an <IndirectProperty> that refers to a <DURATION> it takes to reach the half peak value of the inrush current",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTANTANEOUS FAILURE RATE",null,null,null,null,null,"rdl:RDS14648405",null,"An <INSTANTANEOUS FAILURE RATE> is an <IndirectProperty> that refers to the limit, if it exists, of the <RATIO> of the conditional <PROBABILITY> that the instant of a failure of a non-repaired item falls within a given time interval (t, t + Dt) and the <DURATION>of this time interval, Dt, when Dt tends to zero, given that the item has not failed up to the beginning of a time interval",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INTERMITTENT OVERLOAD",null,null,null,null,null,"rdl:RDS13590694",null,"An <INTERMITTENT OVERLOAD> is an <IndirectProperty> that refers to an <UPPER LIMIT CONTINUOUS POWER> that is tolerable for a short <DURATION>, e.g. for 10% of the total running hours between overhaul",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INTERNAL DESIGN PRESSURE",null,null,null,null,null,"rdl:RDS7311240",null,"An <INTERNAL DESIGN PRESSURE> is a <DESIGN PRESSURE> acting on the inside surface of an object",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INTERNAL THREAD LOWER LIMIT MAJOR DIAMETER",null,null,null,null,null,"rdl:RDS370259",null,"An <INTERNAL THREAD LOWER LIMIT MAJOR DIAMETER> is an <IndirectProperty> that equals &#39;basic major diameter&#39; (D bsc.)",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INTERNAL THREAD LOWER LIMIT MINOR DIAMETER",null,null,null,null,null,"rdl:RDS370889",null,"An <INTERNAL THREAD LOWER LIMIT MINOR DIAMETER> is an <IndirectProperty> that equals &#39;<INTERNAL THREAD> minimum pitch diameter&#39; minus H/2",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INTERNAL THREAD LOWER LIMIT PITCH DIAMETER",null,null,null,null,null,"rdl:RDS370709",null,"An <INTERNAL THREAD LOWER LIMIT PITCH DIAMETER> is an <IndirectProperty> that refers to An <DIAMETER> that equals &#39;basic pitch diameter&#39;",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INTERNAL THREAD MINOR DIAMETER TOLERANCE",null,null,null,null,null,"rdl:RDS370484",null,"An <INTERNAL THREAD MINOR DIAMETER TOLERANCE> is an <IndirectProperty> that refers to An <TOLERANCE(engineering)> on an <INTERNAL THREAD MINOR DIAMETER>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INTERNAL THREAD PITCH DIAMETER TOLERANCE",null,null,null,null,null,"rdl:RDS370574",null,"An <INTERNAL THREAD PITCH DIAMETER TOLERANCE> is an <IndirectProperty> that refers to An <TOLERANCE(engineering)> on an <INTERNAL THREAD PITCH DIAMETER>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INTERNAL THREAD UPPER LIMIT MAJOR DIAMETER",null,null,null,null,null,"rdl:RDS370214",null,"An <INTERNAL THREAD UPPER LIMIT MAJOR DIAMETER> is an <IndirectProperty> that refers to the maximum of &#39;<INTERNAL THREAD> major diameter&#39;. ASME B1.1 Sect. 8.3.2 (a): In practice, the Major Diameter of an Inside Thread is satisfactory when accepted by a gauge or gauging method that represents the maximum-material condition of an Outside Thread that has no allowance",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INTERNAL THREAD UPPER LIMIT MINOR DIAMETER",null,null,null,null,null,"rdl:RDS370529",null,"An <INTERNAL THREAD UPPER LIMIT MINOR DIAMETER> is an <IndirectProperty> that Equals &#39;minimum pitch <DIAMETER> of internal thread&#39;, plus &#39;pitch <DIAMETER> tolerance of internal thread&#39;",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"INTERNAL THREAD UPPER LIMIT PITCH DIAMETER",null,null,null,null,null,"rdl:RDS370934",null,"An <INTERNAL THREAD UPPER LIMIT PITCH DIAMETER> is an <IndirectProperty> that equals &#39;<INTERNAL THREAD> minimum minor diameter&#39; plus &#39;<INTERNAL THREAD> minimum <MINOR DIAMETER> tolerance&#39;",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"K FACTOR",null,null,null,null,null,"rdl:RDS8614770",null,"A <K FACTOR> is an <IndirectProperty> that relates a <NUMBER> of pulses to a <QUANTITY> of a material that passes a <FLOW ELEMENT>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LANDAU-GINZBURG NUMBER",null,null,null,null,null,"rdl:RDS398024",null,"A <LANDAU-GINZBURG NUMBER> is an <IndirectProperty> that refers to at zero thermodynamic <TEMPERATURE> kappa = lambda_L/(xi.root 2) where lambda_L is London penetration depth and xi coherence <LENGTH>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO BASE FOR FLANGED BASE FITTING LOWER LIMIT",null,null,null,null,null,"rdl:RDS377954",null,"A <LENGTH CENTER TO BASE FOR FLANGED BASE FITTING LOWER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO BASE FOR FLANGED BASE FITTING> that is the shortest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO BASE FOR FLANGED BASE FITTING UPPER LIMIT",null,null,null,null,null,"rdl:RDS377909",null,"A <LENGTH CENTER TO BASE FOR FLANGED BASE FITTING UPPER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO BASE FOR FLANGED BASE FITTING> that is the longest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO BOTTOM SOCKET WELDING END LOWER LIMIT",null,null,null,null,null,"rdl:RDS379034",null,"A <LENGTH CENTER TO BOTTOM SOCKET WELDING END LOWER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO BOTTOM SOCKET WELDING END> that is the shortest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO BOTTOM SOCKET WELDING END UPPER LIMIT",null,null,null,null,null,"rdl:RDS379079",null,"A <LENGTH CENTER TO BOTTOM SOCKET WELDING END UPPER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO BOTTOM SOCKET WELDING END> that is the longest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO FACE INSIDE THREADED END BAND LOWER LIMIT",null,null,null,null,null,"rdl:RDS379169",null,"A <LENGTH CENTER TO FACE INSIDE THREADED END BAND LOWER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO FACE INSIDE THREADED END BAND> which is the shortest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO FACE INSIDE THREADED END BAND UPPER LIMIT",null,null,null,null,null,"rdl:RDS379214",null,"A <LENGTH CENTER TO FACE INSIDE THREADED END BAND UPPER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO FACE INSIDE THREADED END BAND> which is the longest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO FACE BEVELLED END LOWER LIMIT",null,null,null,null,null,"rdl:RDS378944",null,"A <LENGTH CENTER TO FACE BEVELLED END LOWER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO FACE BEVELLED END> which is the shortest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO FACE BEVELLED END UPPER LIMIT",null,null,null,null,null,"rdl:RDS378899",null,"A <LENGTH CENTER TO FACE BEVELLED END UPPER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO FACE BEVELLED END> which is the longest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO FLANGED END LOWER LIMIT",null,null,null,null,null,"rdl:RDS378674",null,"A <LENGTH CENTER TO FLANGED END LOWER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO FLANGED END> which is the shortest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO FLANGED END UPPER LIMIT",null,null,null,null,null,"rdl:RDS378629",null,"A <LENGTH CENTER TO FLANGED END UPPER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO FLANGED END> which is the longest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO OUTLET END PIPING CROSS LOWER LIMIT",null,null,null,null,null,"rdl:RDS375974",null,"A <LENGTH CENTER TO OUTLET END PIPING CROSS LOWER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO OUTLET END PIPING CROSS> that is the shortest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO OUTLET END PIPING CROSS UPPER LIMIT",null,null,null,null,null,"rdl:RDS16202742",null,"A <LENGTH CENTER TO OUTLET END PIPING CROSS UPPER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO OUTLET END PIPING CROSS> that is the longest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO OUTLET END PIPING TEE LOWER LIMIT",null,null,null,null,null,"rdl:RDS375659",null,"A <LENGTH CENTER TO OUTLET END PIPING TEE LOWER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO OUTLET END PIPING TEE> that is the shortest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO OUTLET END PIPING TEE UPPER LIMIT",null,null,null,null,null,"rdl:RDS16202607",null,"A <LENGTH CENTER TO OUTLET END PIPING TEE UPPER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO OUTLET END PIPING TEE> that is the longest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO RUN END PIPING CROSS LOWER LIMIT",null,null,null,null,null,"rdl:RDS376019",null,"A <LENGTH CENTER TO RUN END PIPING CROSS LOWER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO RUN END PIPING CROSS> that is the shortest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO RUN END PIPING CROSS UPPER LIMIT",null,null,null,null,null,"rdl:RDS16202652",null,"A <LENGTH CENTER TO RUN END PIPING CROSS UPPER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO RUN END PIPING CROSS> that is the longest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO RUN END PIPING TEE LOWER LIMIT",null,null,null,null,null,"rdl:RDS375614",null,"A <LENGTH CENTER TO RUN END PIPING TEE LOWER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO RUN END PIPING TEE> that is the shortest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH CENTER TO RUN END PIPING TEE UPPER LIMIT",null,null,null,null,null,"rdl:RDS16202382",null,"A <LENGTH CENTER TO RUN END PIPING TEE UPPER LIMIT> is an <IndirectProperty> that refers to a <LENGTH CENTER TO RUN END PIPING TEE> that is the longest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH PIPING FLANGE HUB CYLINDER LOWER LIMIT",null,null,null,null,null,"rdl:RDS368324",null,"A <LENGTH PIPING FLANGE HUB CYLINDER LOWER LIMIT> is an <IndirectProperty> that refers to a <LENGTH PIPING FLANGE HUB CYLINDER> which is the shortest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LENGTH PIPING FLANGE HUB CYLINDER UPPER LIMIT",null,null,null,null,null,"rdl:RDS367019",null,"A <LENGTH PIPING FLANGE HUB CYLINDER UPPER LIMIT> is an <IndirectProperty> that refers to a <LENGTH PIPING FLANGE HUB CYLINDER> which is the longest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LINEARITY",null,null,null,null,null,"rdl:RDS7000661",null,"<LINEARITY> is an <IndirectProperty> that refers to the closeness whith which a calibration curve approximates to a specified straight line",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LIQUID VAPOUR HEAD",null,null,null,null,null,"rdl:RDS2220951",null,"A <LIQUID VAPOUR HEAD> is an <IndirectProperty> that is the <VAPOUR PRESSURE> divided by the <SPECIFIC WEIGHT> of the vapour, so the head corresponding to the equilibrium vapor pressure",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOCKED ROTOR TORQUE",null,null,null,null,null,"rdl:RDS6656320",null,"A <LOCKED ROTOR TORQUE> is an <IndirectProperty> that refers to the smallest <TORQUE> that is a motor develops at its shaft when the rotor is locked over all its angular positions at rated voltage and frequency",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOG MEAN TEMPERATURE DIFFERENCE",null,null,null,null,null,"rdl:RDS14119810",null,"A <LOG MEAN TEMPERATURE DIFFERENCE> is an <IndirectProperty> that refers to a <TEMPERATURE> that is the logaritmic meA <TEMPERATURE> difference at which heat exchange is calculated to occur",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOSS FACTOR",null,null,null,null,null,"rdl:RDS384299",null,"A <LOSS FACTOR> is an <IndirectProperty> that refers to the inverse of A <QUALITY FACTOR> d= 1/Q where Q is the quality factor",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT ACCEPTABLE WALL THICKNESS",null,null,null,null,null,"rdl:RDS7014543",null,"A <LOWER LIMIT ACCEPTABLE WALL THICKNESS> is an <IndirectProperty> that refers to a <WALL THICKNESS> that is the thinnest acceptable according to its design code",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT AMBIENT OPERATING HUMIDITY",null,null,null,null,null,"rdl:RDS8499421",null,"A <LOWER LIMIT AMBIENT OPERATING HUMIDITY> is an <IndirectProperty> that refers to a <HUMIDITY> that is a lower limit of an <AMBIENT OPERATING HUMIDITY>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT AMBIENT OPERATING TEMPERATURE",null,null,null,null,null,"rdl:RDS4231846",null,"A <LOWER LIMIT AMBIENT OPERATING TEMPERATURE> is an <IndirectProperty> that refers to a lowest <AMBIENT TEMPERATURE> under which a device is supposed to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT AMBIENT STORAGE HUMIDITY",null,null,null,null,null,"rdl:RDS8499201",null,"A <LOWER LIMIT AMBIENT STORAGE HUMIDITY> is an <IndirectProperty> that refers to a <HUMIDITY> that is a lower limit of an <AMBIENT STORAGE HUMIDITY",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT AMBIENT STORAGE TEMPERATURE",null,null,null,null,null,"rdl:RDS8797962",null,"A <LOWER LIMIT AMBIENT STORAGE TEMPERATURE> is an <IndirectProperty> that refers to an ambient storage <TEMPERATURE> which is the lowest <AMBIENT TEMPERATURE> under which a device is intended to be stored",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT BEVELLED END INNER BEVEL ANGLE",null,null,null,null,null,"rdl:RDS379304",null,"A <LOWER LIMIT BEVELLED END INNER BEVEL ANGLE> is an <IndirectProperty> that refers to the lower limit of the inner <ANGLE> of a <BEVELLED END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT BEVELLED END INNER BEVEL THICKNESS",null,null,null,null,null,"rdl:RDS379394",null,"A <LOWER LIMIT BEVELLED END INNER BEVEL THICKNESS> is an <IndirectProperty> that refers to the lower limit of a <THICKNESS> of the inner part of a compound bevel measured from the inside of a <BEVELLED END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT BEVELLED END OFF ANGLE",null,null,null,null,null,"rdl:RDS379439",null,"A <LOWER LIMIT BEVELLED END OFF ANGLE> is an <IndirectProperty> that refers to the off <ANGLE> of a <BEVELLED END> pipe fitting",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT BEVELLED END OFF PLANE",null,null,null,null,null,"rdl:RDS376514",null,"A <LOWER LIMIT BEVELLED END OFF PLANE> is an <IndirectProperty> that refers to the lower limit of the off plane <DISTANCE> from intended position of a <BEVELLED END> of a <BEVELLED END> pipe fitting",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT BEVELLED END OUTER BEVEL ANGLE",null,null,null,null,null,"rdl:RDS412154",null,"A <LOWER LIMIT BEVELLED END OUTER BEVEL ANGLE> is an <IndirectProperty> that refers to the lower limit of an <ANGLE> of the outer bevel of a compound bevel measured from the plane of the end cut. A top point of an <ANGLE> is at a <DISTANCE> &#39;bevelled end root face thickness&#39;+ &#39;bevelled end inner bevel thickness&#39; from the inside of <BEVELLED END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT BEVELLED END PLAIN BEVEL ANGLE",null,null,null,null,null,"rdl:RDS412334",null,"A <LOWER LIMIT BEVELLED END PLAIN BEVEL ANGLE> is an <IndirectProperty> that refers to a lower limit of an <ANGLE> of the bevel of a plain <BEVELLED END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT BEVELLED END ROOT FACE THICKNESS",null,null,null,null,null,"rdl:RDS412019",null,"A <LOWER LIMIT BEVELLED END ROOT FACE THICKNESS> is an <IndirectProperty> that refers to the lower limit of a <THICKNESS> of a <BEVELLED END> root face",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT BEVELLED END WALL THICKNESS",null,null,null,null,null,"rdl:RDS412109",null,"A <LOWER LIMIT BEVELLED END WALL THICKNESS> is an <IndirectProperty> that refers to the lower limit of A <WALL THICKNESS> of a <BEVELLED END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT BOTTOMHOLE PRESSURE",null,null,null,null,null,"rdl:RDS16631742",null,"A <LOWER LIMIT BOTTOMHOLE PRESSURE> is an <IndirectProperty> that refers to a <PRESSURE> in a <BOTTOMHOLE> which is the lowest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT BOTTOMHOLE TEMPERATURE",null,null,null,null,null,"rdl:RDS16632012",null,"A <LOWER LIMIT BOTTOMHOLE TEMPERATURE> is an <IndirectProperty> that refers to a <TEMPERATURE> in a <BOTTOMHOLE> which is the lowest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT BRAKE FORCE",null,null,null,null,null,"rdl:RDS7925031",null,"A <LOWER LIMIT BRAKE FORCE> is an <IndirectProperty> that refers to a <BRAKE FORCE> that is the least necessary for braking to begin",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CAP THREADED END WALL THICKNESS",null,null,null,null,null,"rdl:RDS379619",null,"A <LOWER LIMIT CALCULATED VALVE FLOW COEFFICIENT> is an <IndirectProperty> that refers to the lower limit of a <WALL THICKNESS> of the end of a threaded type cap",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CAPACITY (volume flow rate)",null,null,null,null,null,"rdl:RDS7354084",null,"A <LOWER LIMIT CAPACITY (volume flow rate)> is an <IndirectProperty> that refers to a <VOLUME FLOW RATE> which is the least possible",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CLEARANCE",null,null,null,null,null,"rdl:RDS4722156",null,"A <LOWER LIMIT CLEARANCE> is an <IndirectProperty> that refers to a <STRAIGHT LINEAR DISTANCE> which is the shortest acceptable between two objects, or between a moving and stationary part of a machine",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CLEARANCE ABOVE",null,null,null,null,null,"rdl:RDS4722353",null,"A <LOWER LIMIT CLEARANCE ABOVE> is an <IndirectProperty> that refers to a <LOWER LIMIT CLEARANCE> above an object",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CLEARANCE BEHIND",null,null,null,null,null,"rdl:RDS4722263",null,"A <LOWER LIMIT CLEARANCE BEHIND> is an <IndirectProperty> that refers to a <LOWER LIMIT CLEARANCE> behind an object",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CLEARANCE FRONT",null,null,null,null,null,"rdl:RDS4722218",null,"A <LOWER LIMIT CLEARANCE FRONT> is an <IndirectProperty> that refers to a <LOWER LIMIT CLEARANCE> in front of an object",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CLEARANCE SIDE",null,null,null,null,null,"rdl:RDS4722308",null,"A <LOWER LIMIT CLEARANCE SIDE> is an <IndirectProperty> that refers to a <LOWER LIMIT CLEARANCE> at the side of an object",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CONTINOUS THERMAL FLOW",null,null,null,null,null,"rdl:RDS402794",null,"A <LOWER LIMIT CONTINOUS THERMAL FLOW> is an <IndirectProperty> that refers to a <HEAT FLOW RATE> which is the least at which an object can operate without its operation being impaired by a <TEMPERATURE RISE> of a pumped liquid",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CONTINUOUS STABLE FLOW",null,null,null,null,null,"rdl:RDS402749",null,"A <LOWER LIMIT CONTINUOUS STABLE FLOW> is an <IndirectProperty> that refers to a <VOLUME FLOW RATE> which is the lowest possible at which no flow recirculation at impeller suction will take place and hence no unwished increase of the vibration level",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CONTROLLABLE VALVE FLOW COEFFICIENT",null,null,null,null,null,"rdl:RDS7509614",null,"A <LOWER LIMIT CONTROLLABLE VALVE FLOW COEFFICIENT> is an <IndirectProperty> that refers to a <CONTROLLABLE VALVE FLOW COEFFICIENT> that is the minimum flow that can pass through the valve",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT COUNTERBORE DIAMETER",null,null,null,null,null,"rdl:RDS367289",null,"A <LOWER LIMIT COUNTERBORE DIAMETER> is an <IndirectProperty> that refers to a <COUNTERBORE DIAMETER> that is the smallest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CRACK DETECTION DEPTH",null,null,null,null,null,"rdl:RDS13111700",null,"A <LOWER LIMIT CRACK DETECTION DEPTH> is an <IndirectProperty> that refers to a <DEPTH> which is the smallest by which a crack can be detected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CRACK DETECTION LENGTH",null,null,null,null,null,"rdl:RDS13111762",null,"A <LOWER LIMIT CRACK DETECTION LENGTH> is an <IndirectProperty> that refers to a <DEPTH> which is the smallest by which a crack can be detected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CROWN RADIUS",null,null,null,null,null,"rdl:RDS371564",null,"A <LOWER LIMIT CROWN RADIUS> is an <IndirectProperty> that refers to a <RADIUS> of a <TORISPHERICAL HEAD> that is the smallest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CROWN THICKNESS",null,null,null,null,null,"rdl:RDS372149",null,"A <LOWER LIMIT CROWN THICKNESS> is an <IndirectProperty> that refers to a <THICKNESS> of a <TORISPHERICAL HEAD> that is the least allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT CYLINDRICAL SECTION THICKNESS",null,null,null,null,null,"rdl:RDS372059",null,"A <LOWER LIMIT CYLINDRICAL SECTION THICKNESS> is an <IndirectProperty> that refers to a <THICKNESS> of a cylindrical section that is the least allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT DESIGN PRESSURE",null,null,null,null,null,"rdl:RDS360674",null,"A <LOWER LIMIT DESIGN PRESSURE> is an <IndirectProperty> that refers to the lowest <PRESSURE> at which a functional or physical object is designed",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT DESIGN TEMPERATURE",null,null,null,null,null,"rdl:RDS360494",null,"A <LOWER LIMIT DESIGN TEMPERATURE> is an <IndirectProperty> that refers to the lowest <TEMPERATURE> at which a functional or physical object is designed",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT DIAMETER FOR BASE OF FLANGED BASE FITTING",null,null,null,null,null,"rdl:RDS378449",null,"A <LOWER LIMIT DIAMETER FOR BASE OF FLANGED BASE FITTING> is an <IndirectProperty> that refers to a <DIAMETER> which is the lower limit of a <DIAMETER> for the base of a flanged base fitting",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT DISPLACEMENT PER REVOLUTION",null,null,null,null,null,"rdl:RDS5957422",null,"A <LOWER LIMIT DISPLACEMENT PER REVOLUTION> is an <IndirectProperty> that refers to a <DISPLACEMENT PER REVOLUTION> which is the smallest volume of liquid a variable displacement pump or hydraulic motor is able to displace or consume per one complete revolution of it&#39;s shaft",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT DYNAMIC PRESSURE RATING",null,null,null,null,null,"rdl:RDS401039",null,"A <LOWER LIMIT DYNAMIC PRESSURE RATING> is an <IndirectProperty> that refers to a <DYNAMIC PRESSURE RATING> that is the lowest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT ELBOW ANGLE",null,null,null,null,null,"rdl:RDS374759",null,"A <LOWER LIMIT ELBOW ANGLE> is an <IndirectProperty> that refers to an <ANGLE> that is the lower limit for A <ANGLE> between centrelines of an <ANGLE> type fitting",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT ELECTRICAL CONDUCTIVITY",null,null,null,null,null,"rdl:RDS7502430",null,"A <LOWER LIMIT ELECTRICAL CONDUCTIVITY> is an <IndirectProperty> that refers to a <ELECTRICAL CONDUCTIVITY> that is the lowest acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT ELECTRICAL CURRENT",null,null,null,null,null,"rdl:RDS5947026",null,"A <LOWER LIMIT ELECTRICAL CURRENT> is an <IndirectProperty> that refers to an electric <CURRENT> that is the lowest <CURRENT> an apparatus is expected to draw from a <POWER SUPPLY>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT ELECTROLYTIC CONDUCTIVITY",null,null,null,null,null,"rdl:RDS1470055261",null,"A <LOWER LIMIT ELECTROLYTIC CONDUCTIVITY> is an <IndirectProperty> that refers to an <ELECTROLYTIC CONDUCTIVITY> that is the lowest acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT END TO END LENGTH",null,null,null,null,null,"rdl:RDS376649",null,"A <LOWER LIMIT END TO END LENGTH>is an <IndirectProperty> that refers to an <END TO END LENGTH> which is the shortest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT FLAMMABILITY CONCENTRATION",null,null,null,null,null,"rdl:RDS364904",null,"A <LOWER LIMIT FLAMMABILITY CONCENTRATION> is an <IndirectProperty> that refers to a <CONCENTRATION> that is the lowest flammability limit of a flammable substance in a mixture with air that can burn",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT FREQUENCY",null,null,null,null,null,"rdl:RDS5956420",null,"A <LOWER LIMIT FREQUENCY>is an <IndirectProperty> that refers to A <ELECTRICAL FREQUENCY> that is the lowest under which a device is designed to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT GAS LIFT PRESSURE",null,null,null,null,null,"rdl:RDS16634757",null,"A <LOWER LIMIT GAS LIFT PRESSURE> is an <IndirectProperty> that refers to a <GAS LIFT PRESSURE> which is the least acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT GAS LIFT TEMPERATURE",null,null,null,null,null,"rdl:RDS16634352",null,"A <LOWER LIMIT GAS LIFT TEMPERATURE> is an <IndirectProperty> that refers to a lower limit <TEMPERATURE> of the gas in a <GAS LIFT> system",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT GAS LIFT VOLUME",null,null,null,null,null,"rdl:RDS16623822",null,"A <LOWER LIMIT GAS LIFT VOLUME> is an <IndirectProperty> that refers to a lower limit volume of a <GAS LIFT> system",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT GASKET CONTACT FACE OUTSIDE DIAMETER",null,null,null,null,null,"rdl:RDS367424",null,"A <LOWER LIMIT GASKET CONTACT FACE OUTSIDE DIAMETER> is an <IndirectProperty> that refers to A <OUTSIDE DIAMETER> of a raised portion of a <GASKET CONTACT FACE> which is the smallest allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT GUARANTEED TORQUE",null,null,null,null,null,"rdl:RDS5947100",null,"A <LOWER LIMIT GUARANTEED TORQUE> is an <IndirectProperty> that refers to a <TORQUE> that is a guaranteed <LOWER LIMIT TORQUE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT HEIGHT",null,null,null,null,null,"rdl:RDS371879",null,"A <LOWER LIMIT HEIGHT> is an <IndirectProperty> that refers to a <HEIGHT> that is the least allowable for the object in focus",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT HYDRAULIC POWER",null,null,null,null,null,"rdl:RDS413234",null,"A <LOWER LIMIT HYDRAULIC POWER> is an <IndirectProperty> that refers to a <HYDRAULIC POWER> which is the least power transmitted to a liquid by a pump when operating at its lower limit capacity, ie at lower limit continuous stable flow",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT IMPACT ENERGY",null,null,null,null,null,"rdl:RDS13696662",null,"A <LOWER LIMIT IMPACT ENERGY> is an <IndirectProperty> that refers to the impact <ENERGY> that is the minimum <ENERGY> accepted by the material specification",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT INLET FLOW RATE",null,null,null,null,null,"rdl:RDS400589",null,"A <LOWER LIMIT INLET FLOW RATE> is an <IndirectProperty> that refers to a <VOLUME FLOW RATE> that is the lowest allowed at an <INLET>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT INLET PRESSURE",null,null,null,null,null,"rdl:RDS2226090",null,"A <LOWER LIMIT INLET PRESSURE> is an <IndirectProperty> that refers to the minimum <PRESSURE> at an <INLET> that is acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT INLET TEMPERATURE",null,null,null,null,null,"rdl:RDS400274",null,"A <LOWER LIMIT INLET TEMPERATURE> is an <IndirectProperty> that refers to a <TEMPERATURE> which is the lowest <TEMPERATURE> at the location of an <INLET>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT INNER KNUCKLE RADIUS",null,null,null,null,null,"rdl:RDS371654",null,"A <LOWER LIMIT INNER KNUCKLE RADIUS> is an <IndirectProperty> that refers to an inner knuckle <RADIUS> that is the smallest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT INSIDE DIAMETER",null,null,null,null,null,"rdl:RDS12223777",null,"A <LOWER LIMIT INSIDE DIAMETER> is an <IndirectProperty> that refers to an <INSIDE DIAMETER> which is the smallest allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT INSPECTION LENGTH",null,null,null,null,null,"rdl:RDS13117276",null,"A <LOWER LIMIT INSPECTION LENGTH> is an <IndirectProperty> that refers to a <LENGTH OF PATH> which is the shortest <LENGTH> by which an inspection can be detected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT LENGTH CENTER TO CENTER RETURN ELBOW",null,null,null,null,null,"rdl:RDS376154",null,"A <LOWER LIMIT LENGTH CENTER TO CENTER RETURN ELBOW> is an <IndirectProperty> that refers to the minimum <LENGTH> from the Return Elbow Center to Center Point",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT LIQUID DENSITY",null,null,null,null,null,"rdl:RDS6718380",null,"A <LOWER LIMIT LIQUID DENSITY> is an <IndirectProperty> that refers to a <DENSITY> that is the lowest a liquid may have",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT LOWERING SPEED",null,null,null,null,null,"rdl:RDS7924726",null,"A <LOWER LIMIT LOWERING SPEED> is an <IndirectProperty> that refers to a <LOWERING SPEED> that is the lowest allowable when lowering an object",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT LUBRICATION OIL PRESSURE",null,null,null,null,null,"rdl:RDS13590444",null,"A <LOWER LIMIT LUBRICATION OIL PRESSURE> is an <IndirectProperty> that refers to an <INLET PRESSURE> of the lubrication oil at an <INLET> that is the lowest allowable.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT MASS FLOW RATE",null,null,null,null,null,"rdl:RDS14118550",null,"A <LOWER LIMIT MASS FLOW RATE> is an <IndirectProperty> that refers to a <MASS FLOW RATE> that is the lowest allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT MEASURING RANGE",null,null,null,null,null,"rdl:RDS373589",null,"The lowest value of the measured variable to which a device can be adjusted to measure within a specified accuracy",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT NPSHA",null,null,null,null,null,"rdl:RDS14331198",null,"A <LOWER LIMIT NPSHA> is an <IndirectProperty> that refers to a <NET POSITIVE SUCTION HEAD AVAILABLE> that is the lower limit (minimum) that can occur",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT OF OUTDOOR STORAGE",null,null,null,null,null,"rdl:RDS14254370",null,"A <LOWER LIMIT OF OUTDOOR STORAGE> is an <IndirectProperty> that refers to a <PERIOD OF TIME> which is the lower limit of outdoor storage",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT OPERATING TEMPERATURE",null,null,null,null,null,"rdl:RDS360584",null,"A <LOWER LIMIT OPERATING TEMPERATURE> is an <IndirectProperty> that refers to a <TEMPERATURE> that is the lowest at which an object is expected to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT OPERATING PRESSURE",null,null,null,null,null,"rdl:RDS1469272681",null,"A <LOWER LIMIT OPERATING PRESSURE> is an <IndirectProperty> that refers to a <PRESSURE> that is the lowest at which an object is expected to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT OPERATING VOLTAGE",null,null,null,null,null,"rdl:RDS7922743",null,"A <LOWER LIMIT OPERATING VOLTAGE> is an <IndirectProperty> that refers to the lowest <VOLTAGE> that can be tolerated under normal working conditions, at a given instant",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT OPERATING VOLUME",null,null,null,null,null,"rdl:RDS360314",null,"A <LOWER LIMIT OPERATING VOLUME> is an <IndirectProperty> that refers to a <VOLUME> that is the lowest under which the object is expected to work",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT OUTLET PRESSURE",null,null,null,null,null,"rdl:RDS2226091",null,"A <LOWER LIMIT OUTLET PRESSURE> is an <IndirectProperty> that is the minimum <PRESSURE> at an <OUTLET> that is acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT OUTLET PRESSURE",null,null,null,null,null,"rdl:RDS7343157",null,"A <LOWER LIMIT OUTLET PRESSURE> is an <IndirectProperty> that refers to an <OUTLET PRESSURE> that is the lowest at the location of an <OUTLET>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT OUTLET TEMPERATURE",null,null,null,null,null,"rdl:RDS14262020",null,"A <LOWER LIMIT OUTLET TEMPERATURE> is an <IndirectProperty> that refers to an <OUTLET TEMPERATURE> that is the lowest at the location of an <OUTLET>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT OUTSIDE DIAMETER",null,null,null,null,null,"rdl:RDS371834",null,"A <LOWER LIMIT OUTSIDE DIAMETER> is an <IndirectProperty> that refers to an <OUTSIDE DIAMETER> that is the smallest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT OUTSIDE DIAMETER FEMALE FACE",null,null,null,null,null,"rdl:RDS12239336",null,"A <LOWER LIMIT OUTSIDE DIAMETER FEMALE FACE> is an <IndirectProperty> that refers to an <OUTSIDE DIAMETER> of the protruding part of a female face that is the smallest allowable or expected.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT OUTSIDE DIAMETER OF FLANGED END",null,null,null,null,null,"rdl:RDS377324",null,"A <LOWER LIMIT OUTSIDE DIAMETER OF FLANGED END> is an <IndirectProperty> that refers to an <OUTSIDE DIAMETER> of a <FLANGED END> that is the smallest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT OUTSIDE DIAMETER RAISED PORTION OF GROOVE FACE",null,null,null,null,null,"rdl:RDS12250283",null,"A <LOWER LIMIT OUTSIDE DIAMETER RAISED PORTION OF GROOVE FACE> is an <IndirectProperty> of the raised portion of a groove face that is the smallest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT PIPE FLANGE THICKNESS",null,null,null,null,null,"rdl:RDS367109",null,"A <LOWER LIMIT PIPE FLANGE THICKNESS> is an <IndirectProperty> that refers to a <THICKNESS> that is the least allowable thickness of the plate of a flanged piping end, excluding the standout for a raised face end",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT POWER CONSUMPTION",null,null,null,null,null,"rdl:RDS8020816",null,"A <LOWER LIMIT POWER CONSUMPTION> is an <IndirectProperty> that refers to a <POWER CONSUMPTION> that is the smallest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT PRESSURE",null,null,null,null,null,"rdl:RDS400859",null,"A <LOWER LIMIT PRESSURE> is an <IndirectProperty> that refers to a <PRESSURE> that is the lowest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT PRESSURE DROP GRADIENT",null,null,null,null,null,"rdl:RDS8221460",null,"A <LOWER LIMIT PRESSURE DROP GRADIENT> is an <IndirectProperty> that refers to a <PRESSURE DROP GRADIENT> that is the lowest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT PROXIMITY DISTANCE",null,null,null,null,null,"rdl:RDS13288379",null,"A <LOWER LIMIT PROXIMITY DISTANCE> is an <IndirectProperty> that refers to an <DISTANCE> between two objects which is the least allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT RAISED PORTION OUTSIDE DIAMETER",null,null,null,null,null,"rdl:RDS368369",null,"A <LOWER LIMIT RAISED PORTION OUTSIDE DIAMETER> is an <IndirectProperty> that refers to an <OUTSIDE DIAMETER> of a raised portion of a ring joint <GASKET CONTACT FACE> which is the smallest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT RATED EFFICIENCY AT 1/1 LOAD",null,null,null,null,null,"rdl:RDS13649965",null,"A <LOWER LIMIT RATED EFFICIENCY AT 1/1 LOAD> is an <IndirectProperty> that refers to a <RATED EFFICIENCY AT 1/1 LOAD> that is the least allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT RATED SPEED AT 1/1 LOAD",null,null,null,null,null,"rdl:RDS13649875",null,"A <LOWER LIMIT RATED SPEED AT 1/1 LOAD> is an <IndirectProperty> that refers to a <RATED SPEED AT 1/1 LOAD> that is the least allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT RATED TORQUE",null,null,null,null,null,"rdl:RDS13649920",null,"A <LOWER LIMIT RATED TORQUE> is a <RATED TORQUE> that is the least allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT RECOMMENDED INSTALLATION TEMPERATURE",null,null,null,null,null,"rdl:RDS6653874",null,"A <LOWER LIMIT RECOMMENDED INSTALLATION TEMPERATURE> is an <IndirectProperty> that refers to an <AMBIENT TEMPERATURE> that is the minimum under which it is recommended to carry out an installation",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT REQUIRED CAPACITY (volume flow rate)",null,null,null,null,null,"rdl:RDS7354640",null,"A <LOWER LIMIT REQUIRED CAPACITY (VOLUME FLOW RATE)> is an <IndirectProperty> that refers to a <CAPACITY (volume flow rate)> which is the lowest required",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT RETURN PRESSURE",null,null,null,null,null,"rdl:RDS14260175",null,"A <LOWER LIMIT RETURN PRESSURE> is an <IndirectProperty> that refers to a <PRESSURE> of a <FLUID STREAM> returning from a device",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT ROTATIONAL SPEED",null,null,null,null,null,"rdl:RDS402704",null,"A <LOWER LIMIT ROTATIONAL SPEED> is an <IndirectProperty> that refers to a <ROTATIONAL SPEED> which is the lowest at which the manufacturer&#39;s design will permit continous operation",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT SOCKET-WELDING END SOCKET DEPTH",null,null,null,null,null,"rdl:RDS376784",null,"A <LOWER LIMIT SOCKET-WELDING END SOCKET DEPTH> is an <IndirectProperty> that refers to a <DEPTH> of a <SOCKET WELDING END> that is the lowest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT SOCKET-WELDING END WALL THICKNESS",null,null,null,null,null,"rdl:RDS377144",null,"A <LOWER LIMIT SOCKET-WELDING END WALL THICKNESS> is an <IndirectProperty> that refers to a <WALL THICKNESS> of a <SOCKET WELDING END> that is the lowest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT SPAN",null,null,null,null,null,"rdl:RDS411839",null,"A <LOWER LIMIT SPAN> is an <IndirectProperty> that refers to a <SPAN> that is a smallest a device can be adjusted to in order to measure within prescribed tolerances",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT SPRING PRESSURE",null,null,null,null,null,"rdl:RDS11553192",null,"A <LOWER LIMIT SPRING PRESSURE> is an <IndirectProperty> that refers to <FORCE> against which a spring is expected to function",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT STARTING TIME",null,null,null,null,null,"rdl:RDS11379264",null,"A <LOWER LIMIT STARTING TIME> is an <IndirectProperty> that refers to a <STARTING TIME> which is the shortest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT STATIC PRESSURE RATING",null,null,null,null,null,"rdl:RDS401084",null,"A <LOWER LIMIT STATIC PRESSURE RATING> is an <IndirectProperty> that refers to a <STATIC PRESSURE RATING> that is the lowest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT SUBMERGENCE",null,null,null,null,null,"rdl:RDS401894",null,"A <LOWER LIMIT SUBMERGENCE> is an <IndirectProperty> that refers to a <DEPTH> which is the minimum required from the lowest liquid level to the suction <INLET> of a pump",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT SUPPLY PRESSURE",null,null,null,null,null,"rdl:RDS7503758",null,"A <LOWER LIMIT SUPPLY PRESSURE> is an <IndirectProperty> that refers to a <SUPPLY PRESSURE> that is the lowest under which an artefact has been designed to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT SUPPLY TEMPERATURE",null,null,null,null,null,"rdl:RDS13599162",null,"A <LOWER LIMIT SUPPLY TEMPERATURE> is an <IndirectProperty> that refers to <TEMPERATURE> that is the lowest under which an artefact has been designed to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT THREADED LENGTH",null,null,null,null,null,"rdl:RDS367244",null,"A <LOWER LIMIT THREADED LENGTH> is an <IndirectProperty> that refers to a <LENGTH> of the threaded part that is the shortest allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT VALUE OF DISPLACEMENT",null,null,null,null,null,"rdl:RDS14260220",null,"A <LOWER LIMIT VALUE OF DISPLACEMENT> is an <IndirectProperty> that refers to a <DISPLACEMENT> that is the lowest allowable or expected.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT VALVE FLOW COEFFICIENT",null,null,null,null,null,"rdl:RDS7509400",null,"A <LOWER LIMIT VALVE FLOW COEFFICIENT> is an <IndirectProperty> that refers to a <VALVE FLOW COEFFICIENT> that is the minimum flow that can pass through the valve",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT VIBRATION DISPLACEMENT",null,null,null,null,null,"rdl:RDS14296343",null,"A <LOWER LIMIT VIBRATION DISPLACEMENT> is an <IndirectProperty> that refers to a <DISPLACEMENT> due to <VIBRATION> that is the lowest allowable or expected.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT VOLTAGE",null,null,null,null,null,"rdl:RDS7922602",null,"A <LOWER LIMIT VOLTAGE> is an <IndirectProperty> that refers to a <VOLTAGE> that is the lowest allowable or expected.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT VOLUME",null,null,null,null,null,"rdl:RDS360404",null,"A <LOWER LIMIT VOLUME> is an <IndirectProperty> that refers to a <VOLUME> that is the lowest allowable or expected for a given set of conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT WALL THICKNESS TOLERANCE",null,null,null,null,null,"rdl:RDS13282842",null,"A <LOWER LIMIT WALL THICKNESS TOLERANCE> is an <IndirectProperty> that refers to a <THICKNESS> which is the maximum allowable reduction of a wall thickness",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWER LIMIT YIELD STRESS",null,null,null,null,null,"rdl:RDS13116780",null,"A <LOWER LIMIT YIELD STRESS> is an <IndirectProperty> that refers to a <YIELD STRESS> which is the lowest allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"LOWEST VOLTAGE OF A SYSTEM",null,null,null,null,null,"rdl:RDS408104",null,"A <LOWEST VOLTAGE OF A SYSTEM> is an <IndirectProperty> that refers to the lowest value of <OPERATING VOLTAGE> that occurs under normal conditions at any time and any point in the system",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM ABSORBED POWER",null,null,null,null,null,"rdl:RDS16808994",null,"A <MAXIMUM ABSORBED POWER> is an <IndirectProperty> that refers to a <POWER> that is the maximum an <ARTEFACT> will absorb",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM ALLOWABLE WORKING PRESSURE (MAWP)",null,null,null,null,null,"rdl:RDS2227070",null,"A <MAXIMUM ALLOWABLE WORKING PRESSURE (MAWP)> is an <IndirectProperty> of a <PRESSURE RATED ARTEFACT> that is highest pressure that it will withstand; this pressure may be higher than the applicable <MAXIMUM DESIGN PRESSURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM ALLOWABLE WORKING PRESSURE",null,null,null,null,null,"rdl:RDS13113437",null,"A <MAXIMUM ALLOWABLE WORKING PRESSURE> is an <IndirectProperty> that refers to a <OPERATING PRESSURE> which is regarded as the upper limit",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM AMBIENT TEMPERATURE",null,null,null,null,null,"rdl:RDS2223545",null,"A <MAXIMUM AMBIENTTEMPERATURE > is an <IndirectProperty> that is a <TEMPERATURE > of a <PLACE> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM BETA PARTICLE ENERGY",null,null,null,null,null,"rdl:RDS392444",null,"A <MAXIMUM BETA PARTICLE ENERGY> is an <IndirectProperty> that refers to a maximum <ENERGY> of an energy spectrum in a beta disintegration process",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS361619",null,"A <MAXIMUM DIFFERENTIAL PRESSURE> is an <IndirectProperty> that is a <DIFFERENTIAL PRESSURE> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM DIFFERENTIAL HEAD",null,null,null,null,null,"rdl:RDS14152220",null,"A <MAXIMUM DIFFERENTIAL HEAD> is an <IndirectProperty> that is a <DIFFERENTIAL HEAD> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM DIFFERENTIAL FORCE",null,null,null,null,null,"rdl:RDS2223171",null,"A <MAXIMUM DIFFERENTIAL FORCE> is an <IndirectProperty> that is a <DIFFERENTIAL FORCE> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM DIFFERENTIAL TEMPERATURE",null,null,null,null,null,"rdl:RDS2223172",null,"A <MAXIMUM DIFFERENTIAL TEMPERATURE> is an <IndirectProperty> that is a <DIFFERENTIAL TEMPERATURE> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM DISCHARGE PRESSURE",null,null,null,null,null,"rdl:RDS14151900",null,"A <MAXIMUM DISCHARGE PRESSURE> is an <IndirectProperty> that is a <DISCHARGE PRESSURE> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM FIRING PRESSURE",null,null,null,null,null,"rdl:RDS13311325",null,"A <MAXIMUM FIRING PRESSURE> is an <IndirectProperty> that refers to a maximum <PRESSURE> that is the highest cylinder <PRESSURE> achieved during and after ignition",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM FREESPAN HEIGHT",null,null,null,null,null,"rdl:RDS8656662",null,"A <MAXIMUM FREESPAN HEIGHT> is an <IndirectProperty> that refers to a <FREESPAN HEIGHT> which is the largest of a set of freespan heights",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM HEIGHT",null,null,null,null,null,"rdl:RDS8655877",null,"A <MAXIMUM HEIGHT> is an <IndirectProperty> that refers to a <HEIGHT> which is the largest of a set of heights",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM INLET PRESSURE",null,null,null,null,null,"rdl:RDS400724",null,"A <MAXIMUM INLET PRESSURE> is an <IndirectProperty> that is a <INLET PRESSURE> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM PRESSURE",null,null,null,null,null,"rdl:RDS7344775",null,"A <MAXIMUM PRESSURE> is an <IndirectProperty> that is a <PRESSURE> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM RELATIVE DENSITY",null,null,null,null,null,"rdl:RDS2229892",null,"A <MAXIMUM RELATIVE DENSITY> is an <IndirectProperty> that is a <RELATIVE DENSITY> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM RELATIVE HUMIDITY",null,null,null,null,null,"rdl:RDS2223547",null,"A <MAXIMUM RELATIVE HUMIDITY> is an <IndirectProperty> that is a <RELATIVE HUMIDITY> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM SPECIFIC GRAVITY",null,null,null,null,null,"rdl:RDS2229777",null,"A <MAXIMUM SPECIFIC GRAVITY> is an <IndirectProperty> that is a <SPECIFIC GRAVITY> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM SPECIFIC HEAT",null,null,null,null,null,"rdl:RDS2229894",null,"A <MAXIMUM SPECIFIC HEAT> is an <IndirectProperty> that is a <SPECIFIC HEAT> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM SPECTRAL LUMINOUS EFFICACY",null,null,null,null,null,"rdl:RDS385649",null,"A <MAXIMUM SPECTRAL LUMINOUS EFFICACY> is an <IndirectProperty> that refers to a maximum value of <SPECTRAL LUMINOUS EFFICACY>, and is calculated as K_m= (683/V.(555,016 nm)).lm /W= 683 lm/W where V(lambda) is the spectral luminous efficacy",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM TEMPERATURE",null,null,null,null,null,"rdl:RDS400184",null,"A <MAXIMUM TEMPERATURE > is an <IndirectProperty> that is a <TEMPERATURE > that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM VAPOR PRESSURE",null,null,null,null,null,"rdl:RDS2229890",null,"A <MAXIMUM VAPOR PRESSURE> is an <IndirectProperty> that is a <VAPOR PRESSURE> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM VISCOSITY",null,null,null,null,null,"rdl:RDS2229896",null,"A <MAXIMUM VISCOSITY> is an <IndirectProperty> that is a <VISCOSITY> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM VOLUME FLOW RATE",null,null,null,null,null,"rdl:RDS7353960",null,"A <MAXIMUM FLOW> is an <IndirectProperty> that is a <VOLUME FLOW RATE> that is expected to occur as a maximum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAXIMUM WAVE HEIGHT",null,null,null,null,null,"rdl:RDS16431965",null,"A <MAXIMUM WAVE HEIGHT> is an <IndirectProperty> that refers to a <HEIGHT> of the highest wave expected to pass during the passing of 1000 waves",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN ACTIVE CORRECTIVE MAINTENANCE TIME",null,null,null,null,null,"rdl:RDS14645075",null,"A <MEAN ACTIVE CORRECTIVE MAINTENANCE TIME> is an <IndirectProperty> that refers to a mean <DURATION> of a <CORRECTIVE MAINTENANCE TIME>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN ENERGY IMPARTED",null,null,null,null,null,"rdl:RDS395009",null,"A <MEAN ENERGY IMPARTED> is an <IndirectProperty> that refers to to a mean value of an <ENERGY IMPARTED>, epsilon~= R_in - R_out + Sum(Q) where R_in is the radiant <ENERGY> of all those charged and uncharged ionizing particles that enter the domain, R_out is the radiant <ENERGY> of all those charged and uncharged ionizing particloes that leave the domain, and Sum(Q) is the sum of all changes of the rest <ENERGY> of nuclei and elementary particles that occur in that domain",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN FAILURE RATE",null,null,null,null,null,"rdl:RDS14648540",null,"A <MEAN FAILURE RATE> is an <IndirectProperty> that refers to the mean of the <INSTANTANEOUS FAILURE RATE > over a given time interval (t1, t2). )",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN FREE PATH",null,null,null,null,null,"rdl:RDS389609",null,"A <MEAN FREE PATH> is an <IndirectProperty> that refers to, for a particle, the average <DISTANCE> between two successive collisions with other molecules",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN INDICATED PRESSURE",null,null,null,null,null,"rdl:RDS13291528",null,"A <MEAN INDICATED PRESSURE> is an <IndirectProperty> that refers to a <PRESSURE> that is the mean value of the cylinder <PRESSURE> measured during an engine cycle",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN MAINTENANCE MAN HOURS",null,null,null,null,null,"rdl:RDS14647550",null,"A <MEAN MAINTENANCE MAN HOURS> is an <IndirectProperty> that refers to a mean value of the <MAN HOUR>s required for maintenance",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN MAN HOURS TO REPAIR",null,null,null,null,null,"rdl:RDS8599152",null,"A <MEAN MAN HOURS TO REPAIR> is an <IndirectProperty> that refers to a mean value of <MAN HOUR>s which includes all maintenance man hours associated with a repair, including make-ready, performing the maintenance actions, data recording, administrative time and put away",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN PREVENTIVE MAINTENANCE TIME",null,null,null,null,null,"rdl:RDS7926696",null,"A <MEAN PREVENTIVE MAINTENANCE TIME> is an <IndirectProperty> that refers to a mean <DURATION> it takes to do preventive maintenance work",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN QUEUE LENGTH",null,null,null,null,null,"rdl:RDS9999222",null,"A <MEAN QUEUE LENGTH> is an <IndirectProperty> that refers to a mean value of queue <LENGTH>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN REPAIR RATE",null,null,null,null,null,"rdl:RDS14647370",null,"A <MEAN REPAIR RATE> is an <IndirectProperty> that refers to the mean of the instantaneous <REPAIR RATE> over a given time interval (t1, t2)",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN REPAIR TIME (MRT)",null,null,null,null,null,"rdl:RDS14644895",null,"A <MEAN REPAIR TIME (MRT)> is an <IndirectProperty> that refers to a <DURATION> of the repair time",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN SEA LEVEL",null,null,null,null,null,"rdl:RDS1751822991",null,"A <MEAN SEA LEVEL> is an <IndirectProperty> that refers to a mean value of the <SEA LEVEL>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN TIME BETWEEN FAILURE (MTBF)",null,null,null,null,null,"rdl:RDS7925234",null,"A <MEAN TIME BETWEEN FAILURE (MTBF)> is an <IndirectProperty> that refers to a mean <DURATION> of an interval between failures",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN TIME BETWEEN MAINTENANCE",null,null,null,null,null,"rdl:RDS7947774",null,"A <MEAN TIME BETWEEN MAINTENANCE> is an <IndirectProperty> that refers to a mean <DURATION> of an interval between maintenances, planned or actual",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN TIME TO FAILURE (MTTF)",null,null,null,null,null,"rdl:RDS7925189",null,"A <MEAN TIME TO FAILURE (MTTF)> is an <IndirectProperty> that refers to a mean <DURATION> until something fails in its function",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN TIME TO RECOVERY",null,null,null,null,null,"rdl:RDS14646515",null,"A <MEAN TIME TO RECOVERY> is an <IndirectProperty> that refers to a mean <DURATION> until restoration",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEAN TIME TO REPAIR",null,null,null,null,null,"rdl:RDS7926634",null,"A <MEAN TIME TO REPAIR> is an <IndirectProperty> that refers to a mean <DURATION> it takes to repair a fault",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"METAL LOSS CLUSTER AVERAGE DEPTH",null,null,null,null,null,"rdl:RDS8774443",null,"A <METAL LOSS CLUSTER AVERAGE DEPTH> is an <IndirectProperty> that refers to a <DEPTH> that is the average of the individual metal loss features included in the metal loss cluster",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"METAL LOSS CLUSTER PEAK AVERAGE PERCENTAGE",null,null,null,null,null,"rdl:RDS13657730",null,"A <METAL LOSS CLUSTER PEAK AVERAGE PERCENTAGE> is an <IndirectProperty> that refers to a <PERCENTAGE> of the METAL LOSS cluster average depth relative to the reference wall thickness for the METAL LOSS cluster",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"DEPTH",null,null,null,null,null,null,null,null,null,null,null,"METAL LOSS DETECTION THRESHOLD",null,null,null,null,null,"rdl:RDS8774668",null,"A <DETECTION THRESHOLD> is a <DEPTH> that is a minimum detectable depth of METAL LOSS",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM AMBIENT TEMPERATURE",null,null,null,null,null,"rdl:RDS2223546",null,"A <MinIMUM AMBIENTTEMPERATURE > is an <IndirectProperty> that is a <TEMPERATURE > of a <PLACE> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS14152080",null,"A <MINIMUM DIFFERENTIAL HEAD> is an <IndirectProperty> that is a <DIFFERENTIAL PRESSURE> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM DIFFERENTIAL HEAD",null,null,null,null,null,"rdl:RDS14152282",null,"A <MINIMUM DIFFERENTIAL HEAD> is an <IndirectProperty> that is a <DIFFERENTIAL HEAD> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM DIFFERENTIAL FORCE",null,null,null,null,null,"rdl:RDS2223173",null,"A <MINIMUM DIFFERENTIAL FORCE> is an <IndirectProperty> that is a <DIFFERENTIAL FORCE> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM DIFFERENTIAL TEMPERATURE",null,null,null,null,null,"rdl:RDS2223174",null,"A <MINIMUM DIFFERENTIAL TEMPERATURE> is an <IndirectProperty>that is a <DIFFERENTIAL TEMPERATURE> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM DISCHARGE PRESSURE",null,null,null,null,null,"rdl:RDS14151962",null,"A <MINIMUM DISCHARGE PRESSURE> is an <IndirectProperty> that is a <DISCHARGE PRESSURE> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM INLET PRESSURE",null,null,null,null,null,"rdl:RDS400769",null,"A <MINIMUM INLET PRESSURE> is an <IndirectProperty> that is a <INLET PRESSURE> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM PRESSURE",null,null,null,null,null,"rdl:RDS7344837",null,"A <MINIMUM PRESSURE> is an <IndirectProperty> that is a <PRESSURE> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM RELATIVE DENSITY",null,null,null,null,null,"rdl:RDS2229893",null,"A <MINIMUM RELATIVE DENSITY> is an <IndirectProperty> that is a <RELATIVE DENSITY> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM RELATIVE HUMIDITY",null,null,null,null,null,"rdl:RDS2223548",null,"A <MINIMUM RELATIVE HUMIDITY> is an <IndirectProperty> that is a <RELATIVE HUMIDITY> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM SPECIFIC GRAVITY",null,null,null,null,null,"rdl:RDS2229775",null,"A <MINIMUM SPECIFIC GRAVITY> is an <IndirectProperty> that is a <SPECIFIC GRAVITY> that is expected to occur as a mimimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM SPECIFIC HEAT",null,null,null,null,null,"rdl:RDS2229895",null,"A <MINIMUM SPECIFIC HEAT> is an <IndirectProperty> that is a <SPECIFIC HEAT> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM TEMPERATURE",null,null,null,null,null,"rdl:RDS400229",null,"A <MINIMUM TEMPERATURE> is an <IndirectProperty> that is a <TEMPERATURE > that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM VAPOR PRESSURE",null,null,null,null,null,"rdl:RDS2229891",null,"A <MINIMUM VAPOR PRESSURE> is an <IndirectProperty> that is a <VAPOR PRESSURE> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM VELOCITY",null,null,null,null,null,"rdl:RDS13107678",null,"A <MINIMUM VELOCITY> is an <IndirectProperty> that refers to a <VELOCITY> which is the minimum velocity that can be held",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM VISCOSITY",null,null,null,null,null,"rdl:RDS2229897",null,"A <MINIMUM VISCOSITY> is an <IndirectProperty> that is a <VISCOSITY> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MINIMUM VOLUME FLOW RATE",null,null,null,null,null,"rdl:RDS400679",null,"A <MINIMUM FLOW> is an <IndirectProperty> that is a <VOLUME FLOW RATE> that is expected to occur as a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MOBILITY",null,null,null,null,null,"rdl:RDS353474",null,"A <MOBILITY> is an <IndirectProperty> that refers to an average drift speed imparted to a charged particle in a medium by an electric field, divided by the <ELECTRIC FIELD STRENGTH>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"MONTH AVERAGE DENSITY",null,null,null,null,null,"rdl:RDS5059502437",null,"A <MONTH AVERAGE DENSITY> is an <IndirectProperty> that refers to a <DENSITY> that is the average of all measured densities during a <DURATION> of one month",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NET POSITIVE SUCTION HEAD",null,null,null,null,null,"rdl:RDS362834",null,"A <NET POSITIVE SUCTION HEAD>(NPSH) is an <IndirectProperty> that refers to the total absolute suction <PRESSURE> determined at the suction nozzle and referred to the datum elevation, minus a <VAPOUR PRESSURE> of the liquid, expressed as a <HEIGHT> of the pumped liquid",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"NET POSITIVE SUCTION HEAD",null,null,null,null,null,null,null,null,null,null,null,null,"NET POSITIVE SUCTION HEAD AVAILABLE",null,null,null,null,null,"rdl:RDS362879",null,"A <NET POSITIVE SUCTION HEAD AVAILABLE>(NPSHA) is a <NET POSITIVE SUCTION HEAD> for a particular pumping system at a certain <FLOW RATE> and <TEMPERATURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"NET POSITIVE SUCTION HEAD",null,null,null,null,null,null,null,null,null,null,null,null,"NET POSITIVE SUCTION HEAD REQUIRED",null,null,null,null,null,"rdl:RDS362924",null,"A <NET POSITIVE SUCTION HEAD REQUIRED>(NPSHR) is a <NET POSITIVE SUCTION HEAD> as required by a pump, determined by the manufacturer to comply with applicable standards",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"NET POSITIVE SUCTION HEAD REQUIRED",null,null,null,null,null,null,null,null,null,null,null,null,null,"NET POSITIVE SUCTION HEAD REQUIRED AT LOWER LIMIT FLOW",null,null,null,null,null,"rdl:RDS404234",null,"A <NET POSITIVE SUCTION HEAD REQUIRED AT LOWER LIMIT FLOW> is a <NET POSITIVE SUCTION HEAD REQUIRED> which is required at lower limit flow",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"NET POSITIVE SUCTION HEAD REQUIRED",null,null,null,null,null,null,null,null,null,null,null,null,null,"NET POSITIVE SUCTION HEAD REQUIRED AT RATED CAPACITY",null,null,null,null,null,"rdl:RDS404189",null,"A <NET POSITIVE SUCTION HEAD REQUIRED AT RATED CAPACITY> is a <NET POSITIVE SUCTION HEAD REQUIRED> which is the required NPSH at rated capacity",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NET STANDARD OIL VOLUME",null,null,null,null,null,"rdl:RDS16682234",null,"A <NET STANDARD OIL VOLUME> is an <IndirectProperty> that refers to a total <VOLUME> of all petroleum liquids excluding sediments and water and free water, corrected by the appropriate <VOLUME> correction factor (Ci1) for the observed <TEMPERATURE> and API gravity, relative density, or density to a standard <TEMPERATURE> such as 60 deg F or 15 deg C and also corrected by the applicabe <PRESSURE> correction factor (Cp1) and meter factor",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NET THERMAL EFFICIENCY",null,null,null,null,null,"rdl:RDS6729217",null,"A <NET THERMAL EFFICIEN> is an <IndirectProperty> that refers to a <RATIO> of the net electrical <ENERGY> generated by a unit to the thermal <ENERGY> of the fuel consumed during a <PeriodInTime> by the same unit",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NET TOTAL WEIGHT",null,null,null,null,null,"rdl:RDS8798340",null,"A <NET TOTAL WEIGHT> is an <IndirectProperty> that refers to a <WEIGHT> of an assembly excluding eg. operating or process fluids if any, <WEIGHT> of packaging material etc",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NEUTRON YIELD PER ABSORPTION",null,null,null,null,null,"rdl:RDS394559",null,"A <NEUTRON YIELD PER ABSORPTION> is an <IndirectProperty> that referes to an average <NUMBER> of fission neutrons, both prompt and delayed, emitted per neutron absorbed in a fissionable nuclide or in a nuclear fuel, as specified",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NEUTRON YIELD PER FISSION",null,null,null,null,null,"rdl:RDS394514",null,"A <NEUTRON YIELD PER FISSION> is an <IndirectProperty> that referes to an average <NUMBER> of fission neutrons, both prompt and delayed, emitted per fission event",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL BOLT CIRCLE DIAMETER",null,null,null,null,null,"rdl:RDS366884",null,"A <NOMINAL BOLT CIRCLE DIAMETER> is an <IndirectProperty> that refers to a <NOMINAL DIAMETER> of bolt circle",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL BOLT DIAMETER",null,null,null,null,null,"rdl:RDS366974",null,"A <NOMINAL BOLT DIAMETER> is an <IndirectProperty> that refers to a <NOMINAL OUTSIDE DIAMETER> of a threaded fastener, ie. a bolt or screw",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL BOLT HOLE DIAMETER",null,null,null,null,null,"rdl:RDS366929",null,"A <NOMINAL BOLT HOLE DIAMETER> is an <IndirectProperty> that refers to a <NOMINAL DIAMETER> of a bolt hole",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL BURST PRESSURE",null,null,null,null,null,"rdl:RDS5912043",null,"A <NOMINAL BURST PRESSURE> is an <IndirectProperty> that refers to a burst <PRESSURE> that is a design/intended burst pressure",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL DESIGN PRESSURE",null,null,null,null,null,"rdl:RDS8652159",null,"A <NOMINAL DESIGN PRESSURE> is an <IndirectProperty> that refers to a <DESIGN PRESSURE> that is determined based on the expected operating pressure",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL DESIGN TEMPERATURE",null,null,null,null,null,"rdl:RDS8652097",null,"A <NOMINAL DESIGN TEMPERATURE> is an <IndirectProperty> that refers to a design <TEMPERATURE> which determined based on a nominal operating <TEMPERATURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"DIAMETER",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL DIAMETER",null,null,null,null,null,"rdl:RDS366794",null,"A <NOMINAL DIAMETER> is a <DIAMETER> that is an expected (theoretical/as designed) diameter that does not necessarily indicate the exact internal diameter. It is used to arrive at the pipe dimensions using standard tables and schedules",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"NOMINAL DIAMETER",null,null,null,null,null,null,null,null,null,null,null,null,"SECONDARY NOMINAL DIAMETER",null,null,null,null,null,"rdl:RDS2226500",null,"A <SECONDARY NOMINAL DIAMETER> is a <NOMINAL DIAMETER> that is the second largest nominal diameter of a <PhysicalObject>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL FREQUENCY",null,null,null,null,null,"rdl:RDS2224476",null,"A <NOMINAL FREQUENCY> is an <IndirectProperty> that is the <FREQUENCY> according to which some item has been named or is generally referred to. Such a nominal value may have no real relation to the item being referred to",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL HANDLE LENGTH",null,null,null,null,null,"rdl:RDS6774557",null,"A <NOMINAL HANDLE LENGTH> is an <IndirectProperty> that refers to a nominal <LENGTH> of a handle",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL HANDLE WIDTH",null,null,null,null,null,"rdl:RDS6775263",null,"A <NOMINAL HANDLE WIDTH> is an <IndirectProperty> that refers to a nominal <WIDTH> of a handle",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL HEIGHT RAISED FACE STANDOUT",null,null,null,null,null,"rdl:RDS367469",null,"A <NOMINAL HEIGHT RAISED FACE STANDOUT> is an <IndirectProperty> that refers to a <HEIGHT> of raised face standout that is the expected (theoretical/as designed) <HEIGHT> of the standout",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL INSIDE DIAMETER",null,null,null,null,null,"rdl:RDS366839",null,"A <NOMINAL INSIDE DIAMETER> is an <IndirectProperty> that refers to an <INSIDE DIAMETER> that is an expected (theoretical/as designed) inside diameter",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL LENGTH",null,null,null,null,null,"rdl:RDS367064",null,"A <NOMINAL LENGTH> is an <IndirectProperty> that refers to a <DISTANCE> that is an expected (theoretical/as designed) distance",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL OPERATING TEMPERATURE",null,null,null,null,null,"rdl:RDS6949510",null,"A <NOMINAL OPERATING TEMPERATURE> is an <IndirectProperty> that refers to a n operating <TEMPERATURE> that is the expected operating <TEMPERATURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL OUTSIDE DIAMETER",null,null,null,null,null,"rdl:RDS366614",null,"A <NOMINAL OUTSIDE DIAMETER> is an <IndirectProperty> that refers to an <OUTSIDE DIAMETER> that is an expected (theoretical/as designed) <OUTSIDE DIAMETER>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL OUTSIDE DIAMETER GASKET CONTACT FACE",null,null,null,null,null,"rdl:RDS367379",null,"A <NOMINAL OUTSIDE DIAMETER GASKET CONTACT FACE> is an <IndirectProperty> that refers to a <NOMINAL OUTSIDE DIAMETER> of a <GASKET CONTACT FACE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL OUTSIDE DIAMETER OF FLANGED END",null,null,null,null,null,"rdl:RDS366659",null,"A <NOMINAL OUTSIDE DIAMETER OF FLANGED END> is an <IndirectProperty> that refers to a <NOMINAL OUTSIDE DIAMETER> of a <FLANGED END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL OUTSIDE DIAMETER OF THE LAST INSTALLED WELL CASING STRING",null,null,null,null,null,"rdl:RDS17659515",null,"A <NOMINAL OUTSIDE DIAMETER OF THE LAST INSTALLED WELL CASING STRING> is an <IndirectProperty> that refers to a nominal outside diameter of a well casing string that is the nominal outside diameter of the last run casing string in a wellbore",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL OUTSIDE DIAMETER OF WELL CASING STRING",null,null,null,null,null,"rdl:RDS17659560",null,"A <NOMINAL OUTSIDE DIAMETER OF WELL CASING STRING> is an <IndirectProperty> that refers to a <NOMINAL OUTSIDE DIAMETER> that is A <NOMINAL OUTSIDE DIAMETER> of a well casing string",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL OUTSIDE STUFFING BOX PACKING DIAMETER",null,null,null,null,null,"rdl:RDS14188720",null,"A <NOMINAL OUTSIDE STUFFING BOX PACKING DIAMETER> is an <IndirectProperty> that refers to a <NOMINAL OUTSIDE DIAMETER> of a stuffing box packing (packing ring)",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL OVERCOVERAGE",null,null,null,null,null,"rdl:RDS13101674",null,"A <NOMINAL OVERCOVERAGE> is an <IndirectProperty> that refers to a <DEPTH> which is the intended or designed <DEPTH> of an overcoverage",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL PIPE FLANGE THICKNESS",null,null,null,null,null,"rdl:RDS7286136",null,"A <NOMINAL PIPE FLANGE THICKNESS> is an <IndirectProperty> that refers to a <PIPE FLANGE THICKNESS> that is the intended thickness of the plate of a flanged piping end, excluding the standout for a raised face end",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL PRESSURE",null,null,null,null,null,"rdl:RDS6949380",null,"A <NOMINAL PRESSURE> is an <IndirectProperty> that refers to a <PRESSURE> that is an expected (theoretical/as designed) <PRESSURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL SIZE",null,null,null,null,null,"rdl:RDS2229888",null,"A <NOMINAL SIZE> is an <IndirectProperty> that is a <SIZE> used for purposes of general identification; the actual size of a part will be approximately the same as the nominal size but need not be exactly the same;",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL SUPPLY FREQUENCY",null,null,null,null,null,"rdl:RDS7510156",null,"A <NOMINAL SUPPLY FREQUENCY> is an <IndirectProperty> that refers to a nominal frequency (at nominal supply voltage) supplied to a motor or actuator",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL SUPPLY VOLTAGE",null,null,null,null,null,"rdl:RDS6606500",null,"A <NOMINAL SUPPLY VOLTAGE> is an <IndirectProperty> that refers to a supply voltage that is the nominal or rated value marked or printed on an apparatus",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL TEMPERATURE",null,null,null,null,null,"rdl:RDS13112512",null,"A <NOMINAL TEMPERATURE> is an <IndirectProperty> that refers to a <TEMPERATURE> which is the intended or planned <TEMPERATURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL THICKNESS",null,null,null,null,null,"rdl:RDS6785160",null,"A <NOMINAL THICKNESS> is an <IndirectProperty> that refers to a <THICKNESS> that is an expected (theoretical/as designed) <THICKNESS>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL VOLTAGE",null,null,null,null,null,"rdl:RDS369449",null,"A <NOMINAL VOLTAGE> is an <IndirectProperty> that is the <VOLTAGE> according to which some item has been named or is generally referred to. Such a nominal value may have no real relation to the item being referred to",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL VOLTAGE OF A SYSTEM",null,null,null,null,null,"rdl:RDS407969",null,"A <NOMINAL VOLTAGE OF A SYSTEM> is an <IndirectProperty> that refers to a suitable approximate value of <VOLTAGE> used to designate or identify a system",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL WALL THICKNESS",null,null,null,null,null,"rdl:RDS13115973",null,"A <NOMINAL WALL THICKNESS> is an <IndirectProperty> that refers to a <WALL THICKNESS> which is the expected / as designed <WALL THICKNESS>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NOMINAL WIDTH",null,null,null,null,null,"rdl:RDS6775201",null,"A <NOMINAL WIDTH> is an <IndirectProperty> that refers to a <WIDTH> that is an expected (theoretical/as designed) <WIDTH>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL ABSORBED POWER",null,null,null,null,null,"rdl:RDS410399",null,"A <NORMAL ABSORBED POWER> is an <IndirectProperty> that refers to a <POWER> which is absorbed at normal operation conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL AMBIENT OPERATING TEMPERATURE",null,null,null,null,null,"rdl:RDS7923460",null,"A <NORMAL AMBIENT OPERATING TEMPERATURE> is an <IndirectProperty> that refers to a n ambient operating <TEMPERATURE> under which a device normally is supposed to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL BACK PRESSURE",null,null,null,null,null,"rdl:RDS7470944",null,"A <NORMAL BACK PRESSURE> is an <IndirectProperty> that refers to a <BACK PRESSURE> based upon static outlet conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL BOILING TEMPERATURE",null,null,null,null,null,"rdl:RDS358694",null,"A <NORMAL BOILING TEMPERATURE> is an <IndirectProperty> that refers to a <BOILING TEMPERATURE> at which fractions of a liquid boils",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL BRAKE FORCE",null,null,null,null,null,"rdl:RDS7925076",null,"A <NORMAL BRAKE FORCE> is an <IndirectProperty> that refers to a <BRAKE FORCE> that is normally applied to the brake",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL CAPACITY (volumetric flow rate)",null,null,null,null,null,"rdl:RDS7354310",null,"A <NORMAL CAPACITY (volumetric flow rate)> is an <IndirectProperty> that refers to a <CAPACITY (volumetric flow rate)> which is normally expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL CAPACITY REQUIRED (volumetric flow rate)",null,null,null,null,null,"rdl:RDS7356304",null,"A <NORMAL CAPACITY REQUIRED (volumetric flow rate)> is an <IndirectProperty> that refers to a <CAPACITY (volumetric flow rate)> which is normally required",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS2223471",null,"A <NORMAL DIFFERENTIAL PRESSURE> is an <IndirectProperty> that is a <DIFFERENTIAL PRESSURE> that is expected to occur under normal conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL DIFFERENTIAL HEAD",null,null,null,null,null,"rdl:RDS2223472",null,"A <NORMAL DIFFERENTIAL HEAD> is an <IndirectProperty> that is a <DIFFERENTIAL HEAD> that is expected to occur under normal conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL DISCHARGE PRESSURE",null,null,null,null,null,"rdl:RDS2229898",null,"A <NORMAL DISCHARGE PRESSURE> is an <IndirectProperty> that is a <DISCHARGE PRESSURE> that is expected to occur under normal conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL FREEZING TEMPERATURE",null,null,null,null,null,"rdl:RDS7352774",null,"A <NORMAL FREEZING TEMPERATURE> is an <IndirectProperty> that refers to a <TFREEZING EMPERATURE> where a liquid material forms solid material under normal conditions&quot;",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL INLET PRESSURE",null,null,null,null,null,"rdl:RDS7343782",null,"A <NORMAL INLET PRESSURE> is an <IndirectProperty> that is a <INLET PRESSURE> that is expected to occur under normal conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL INLET TEMPERATURE",null,null,null,null,null,"rdl:RDS14261975",null,"A <NORMAL INLET TEMPERATURE> is an <IndirectProperty> that refers to an <INLET TEMPERATURE> which is normally expected.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL LOWERING SPEED",null,null,null,null,null,"rdl:RDS7924636",null,"A <NORMAL LOWERING SPEED> is an <IndirectProperty> that refers to a <LOWERING SPEED> which a hoist is designed for",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL MAINTENANCE MANNING",null,null,null,null,null,"rdl:RDS7054058",null,"A <NORMAL MAINTENANCE MANNING> is an <IndirectProperty> that refers to a <NUMBER> of people normally required for Maintenance activities",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL MASS FLOW RATE",null,null,null,null,null,"rdl:RDS14118280",null,"A <NORMAL MASS FLOW RATE> is an <IndirectProperty> that refers to a <MASS FLOW RATE> which is normally expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL OPERATING DENSITY",null,null,null,null,null,"rdl:RDS43168075198",null,"A <NORMAL OPERATING DENSITY> is an <IndirectProperty> that refers to a <DENSITY> at which a designed or actual physical object is expected to operate normally",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL OPERATING PRESSURE",null,null,null,null,null,"rdl:RDS369629",null,"A <NORMAL OPERATING PRESSURE> is an <IndirectProperty> that refers to a <PRESSURE> at which a designed or actual physical object is expected to operate normally",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL OPERATING TORQUE AT BALANCED DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS16761837",null,"A <NORMAL OPERATING TORQUE AT BALANCED DIFFERENTIAL PRESSURE> is an <IndirectProperty> that refers to a <NORMAL OPERATING TORQUE> when the line <DIFFERENTIAL PRESSURE> is equal across the valve",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL OPERATING TORQUE AT MAXIMUM DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS16761940",null,"A <NORMAL OPERATING TORQUE AT MAXIMUM DIFFERENTIAL PRESSURE> is an <IndirectProperty> that refers to a <NORMAL OPERATING TORQUE> when the line <DIFFERENTIAL PRESSURE> is at maximum across the valve",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL OPERATING TORQUE",null,null,null,null,null,"rdl:RDS16741840",null,"A <NORMAL OPERATING TORQUE> is an <IndirectProperty> that refers to a <TORQUE> used under normal operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL OPERATING VOLUME",null,null,null,null,null,"rdl:RDS7355353",null,"A <NORMAL OPERATING VOLUME> is an <IndirectProperty> that refers to a <VOLUME> at which a designed or actual physical object is expected to operate normally",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL OUTLET PRESSURE",null,null,null,null,null,"rdl:RDS14261705",null,"A <NORMAL OUTLET PRESSURE> is an <IndirectProperty> that refers to an <OUTLET PRESSURE> that will occur under normal operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL OUTLET TEMPERATURE",null,null,null,null,null,"rdl:RDS14262065",null,"A <NORMAL OUTLET TEMPERATURE> is an <IndirectProperty> that refers to an <OUTLET TEMPERATURE> that will occur under normal operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL POWER CONSUMPTION",null,null,null,null,null,"rdl:RDS8020878",null,"A <NORMAL POWER CONSUMPTION> is an <IndirectProperty> that refers to a <POWER CONSUMPTION> at normal working conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL PRESSURE",null,null,null,null,null,"rdl:RDS14302040",null,"A <NORMAL PRESSURE> is an <IndirectProperty> that is expected to occur under normal conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL PRESSURE DROP GRADIENT",null,null,null,null,null,"rdl:RDS8221505",null,"A <NORMAL PRESSURE DROP GRADIENT> is an <IndirectProperty> that refers to a <PRESSURE DROP GRADIENT> under normal operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL PROCESS ACTIVITY MANNING",null,null,null,null,null,"rdl:RDS7054013",null,"A <NORMAL PROCESS ACTIVITY MANNING> is an <IndirectProperty> that refers to a <NUMBER> of people required for process activities under normal operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL RAISING SPEED",null,null,null,null,null,"rdl:RDS7924546",null,"A <NORMAL RAISING SPEED> is an <IndirectProperty> that refers to a <RAISING SPEED> which a hoist is designed for when <RAISING> an object.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL REQUIRED TORQUE",null,null,null,null,null,"rdl:RDS13598352",null,"A <NORMAL REQUIRED TORQUE> is an <IndirectProperty> that refers to a <TORQUE> required under normal operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL SPECIFIC GRAVITY",null,null,null,null,null,"rdl:RDS2229776",null,"A <NORMAL SPECIFIC GRAVITY> is an <IndirectProperty> that is a <SPECIFIC GRAVITY> that is expected to occur under normal operating conditions.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL STEAM CONSUMPTION",null,null,null,null,null,"rdl:RDS14261480",null,"A <NORMAL STEAM CONSUMPTION> is an <IndirectProperty> that refers to a <STEAM CONSUMPTION> at normal working conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL STRESS",null,null,null,null,null,"rdl:RDS380249",null,"A <NORMAL STRESS> is an <IndirectProperty> that refers to a <STRESS> at normal working conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL SUPPLY PRESSURE",null,null,null,null,null,"rdl:RDS7503713",null,"A <NORMAL SUPPLY PRESSURE> is an <IndirectProperty> that refers to a <SUPPLY PRESSURE> under which an object has been designed to normally operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL TEMPERATURE",null,null,null,null,null,"rdl:RDS369674",null,"A <NORMAL TEMPERATURE> is an <IndirectProperty> that is a <TEMPERATURE > that is expected to occur under normal conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL VAPOUR PRESSURE",null,null,null,null,null,"rdl:RDS2229885",null,"A <NORMAL VAPOUR PRESSURE> is an <IndirectProperty> that is a <VAPOUR PRESSURE> that is expected to occur under normal operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL VISCOSITY",null,null,null,null,null,"rdl:RDS2229886",null,"A <NORMAL VISCOSITY> is an <IndirectProperty> that is a <VISCOSITY> that is expected to occur under normal operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NORMAL VOLUMETRIC FLOW RATE",null,null,null,null,null,"rdl:RDS8276279",null,"A <NORMAL VOLUMETRIC FLOW RATE> is an <IndirectProperty> that refers to a <VOLUMETRIC FLOW RATE> which is normally expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NPSHA",null,null,null,null,null,"rdl:RDS14331074",null,"An <NPSHA> is an <IndirectProperty> that is the difference between the <SUCTION HEAD>, and the <LIQUID VAPOUR HEAD>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NPSHR",null,null,null,null,null,"rdl:RDS2220952",null,"An <NPSHR> is an <IndirectProperty> that is the minimum pressure required at the suction port of the pump to keep the pump from cavitating.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NUMBER OF STARTS PER DAY",null,null,null,null,null,"rdl:RDS402974",null,"A <NUMBER OF STARTS PER DAY> is an <IndirectProperty> that is the number of starts of a equipment item per day",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"NUMBER OF STARTS PER HOUR",null,null,null,null,null,"rdl:RDS412559",null,"A <NUMBER OF STARTS PER DAY> is an <IndirectProperty> that is the number of starts of a equipment item per hour",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"NUMBER OF STARTS PER HOUR",null,null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT NUMBER OF STARTS PER HOUR",null,null,null,null,null,"rdl:RDS14149462",null,"An <UPPER LIMIT NUMBER OF STARTS PER HOUR> is a <NUMBER OF STARTS PER HOUR> that is the upper limit (maximum) number of starts of an equipment item per hour",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"OPERATING PRESSURE",null,null,null,null,null,"rdl:RDS1469240071",null,"An <OPERATING PRESSURE> is an <IndirectProperty> that refers to a <PRESSURE> under which an object is supposed to work",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"OPERATING TEMPERATURE",null,null,null,null,null,"rdl:RDS357119",null,"An <OPERATING TEMPERATURE> is an <IndirectProperty> that refers to a <TEMPERATURE> under which an object is supposed to work",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"OPERATING TIME",null,null,null,null,null,"rdl:RDS14644985",null,"An <OPERATING TIME> is an <IndirectProperty> that refers to a <DURATION> during which an item is in an operating state",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"OPERATING VOLTAGE",null,null,null,null,null,"rdl:RDS7504137",null,"An <OPERATING VOLTAGE> is an <IndirectProperty> that refers to a <VOLTAGE> under normal working conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"OPERATING VOLUME",null,null,null,null,null,"rdl:RDS356984",null,"An <OPERATING VOLUME> is an <IndirectProperty> that refers to a <VOLUME> that occurs during operation",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"OPERATIONAL READINESS",null,null,null,null,null,"rdl:RDS14646560",null,"An <OPERATIONAL READINESS> is an <IndirectProperty> thar refers to a <DURATION> of the time required to restore an item receiving support to an operational condition (e.g. 24 hours notice for sea)",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"OPFLEX",null,null,null,null,null,"rdl:RDS49899319137",null,"An <OPFLEX> is an <IndirectProperty> that refers to a <VOLUME> or <MASS> of unused and available gas within a gas transportation system and/or at one or many gas producing fields that is accessible by the operator responsible for gas transportation for the purposes of alleviating field curtailment",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"Property",null,null,null,null,null,null,null,null,null,null,null,"OPTIMUM LOAD",null,null,null,null,null,"rdl:RDS103229",null,"An <OPTIMUM LOAD> is a <ClassOfInformationRepresentation> that defines how a load of a network component for which the sum of the present values of cost under given conditions is a minimum",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"OVERLOAD CAPACITY",null,null,null,null,null,"rdl:RDS14187455",null,"An <OVERLOAD CAPACITY> is an <IndirectProperty> that refers to the highest <LOAD> which can be maintained during a short <PeriodInTime>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"PHASE(electric)",null,null,null,null,null,"rdl:RDS2224474",null,"A <PHASE(electric)> is an <IndirectProperty> of an <ELECTRIC CIRCUIT> indicating the number of alternating voltages, that are, if larger than one, displaced in phase by an angle",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"PHASE-TO-EARTH CLEARANCE",null,null,null,null,null,"rdl:RDS406664",null,"A <PHASE-TO-EARTH CLEARANCE> is an <IndirectProperty> that refers to a <CLEARANCE> that is the minimum <DISTANCE> between any live parts and all structures at earth potential",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"PHASE-TO-PHASE CLEARANCE",null,null,null,null,null,"rdl:RDS406619",null,"A <PHASE-TO-PHASE CLEARANCE> is an <IndirectProperty> that refers to a <CLEARANCE> that is the minimum <DISTANCE> between live parts of two adjacent phases taking into account all operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"POLYTROPIC EFFICIENCY",null,null,null,null,null,"rdl:RDS361169",null,"A <POLYTROPIC EFFICIENCY> is an <IndirectProperty> that refers to an <EFFICIENCY> of a compressor; this property is based on an imaginary &quot;polytropic path&quot; which is reversible and non-adiabatic",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"PRESSURE DROP AT FULL RANGE",null,null,null,null,null,"rdl:RDS7478342",null,"A <PRESSURE DROP AT FULL RANGE> is an <IndirectProperty> that is a pressure loss that is a permanent pressure loss across an item at 100 % of the flow range",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROSPECTIVE TOUCH VOLTAGE",null,null,null,null,null,"rdl:RDS407519",null,"A <PROSPECTIVE TOUCH VOLTAGE> is an <IndirectProperty> that refers to a <VOLTAGE> that is the highest liable to appear in the event of a fault of negligible <IMPEDANCE> in an electrical installation",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROXIMITY UPPER LIMIT DISTANCE",null,null,null,null,null,"rdl:RDS13112777",null,"A <PROXIMITY UPPER LIMIT DISTANCE> is an <IndirectProperty> that refers to a <STRAIGHT LINEAR DISTANCE> which is the upper limit <DISTANCE> for which something is considdered to be within the proximity",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED AIR CONSUMPTION",null,null,null,null,null,"rdl:RDS8501608",null,"A <RATED AIR CONSUMPTION> is an <IndirectProperty> that refers to an <AIR CONSUMPTION> that is the rated (nominal) air consumption of a device at rated conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED CAPACITY (volumetric flow rate)",null,null,null,null,null,"rdl:RDS7354389",null,"A <RATED CAPACITY (volumetric flow rate)> is an <IndirectProperty> that refers to a <CAPACITY (volumetric flow rate)> at a specified condition",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED CURRENT",null,null,null,null,null,"rdl:RDS364454",null,"A <RATED CURRENT> is an <IndirectProperty> that refers to an r.m.s. value of an <ALTERNATING CURRENT> for which an apparatus has been designed",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED DEPTH",null,null,null,null,null,"rdl:RDS17611083",null,"A <RATED DEPTH> is an <IndirectProperty> that refers to a <DEPTH> which is the maximum rated working <DEPTH> of a piece of equipment at a given set of operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"RATED DIFFERENTIAL HEAD",null,null,null,null,null,"rdl:RDS14152344",null,"A <RATED DIFFERENTIAL HEAD> is an <IndirectProperty> that is a <DIFFERENTIAL HEAD> that is expected to occur under rated conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"RATED DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS14152142",null,"A <RATED DIFFERENTIAL PRESSURE> is an <IndirectProperty> that is a <DIFFERENTIAL PRESSURE> that is expected to occur under rated conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"RATED DISCHARGE PRESSURE",null,null,null,null,null,"rdl:RDS14151838",null,"A <RATED DISCHARGE PRESSURE> is an <IndirectProperty> that is a <DISCHARGE PRESSURE> that is expected to occur under rated conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED EFFICIENCY",null,null,null,null,null,"rdl:RDS402254",null,"A <RATED EFFICIENCY> is an <IndirectProperty> that refers to a <EFFICIENCY> of a <SYSTEM>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED EFFICIENCY AT 1/1 LOAD",null,null,null,null,null,"rdl:RDS5963820",null,"A <RATED EFFICIENCY AT 1/1 LOAD> is an <IndirectProperty> that refers to a <RATED EFFICIENCY> at 1/1 load (full load)",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED EFFICIENCY AT 1/2 LOAD",null,null,null,null,null,"rdl:RDS14103921",null,"A <RATED EFFICIENCY AT 1/2 LOAD> is an <IndirectProperty> that refers to a <RATED EFFICIENCY> at 1/2 load (50% load)",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED EFFICIENCY AT 3/4 LOAD",null,null,null,null,null,"rdl:RDS9540040",null,"A <RATED EFFICIENCY AT 3/4 LOAD> is an <IndirectProperty> that refers to a <RATED EFFICIENCY> at 3/4 load",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED FREQUENCY",null,null,null,null,null,"rdl:RDS4720960",null,"A <RATED FREQUENCY> is an <IndirectProperty> that refers to an <ELECTRICAL FREQUENCY> of a machine at rated output",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED HYDRAULIC POWER",null,null,null,null,null,"rdl:RDS413189",null,"A <RATED HYDRAULIC POWER> is an <IndirectProperty> that refers to a <HYDRAULIC POWER> that is transmitted to a liquid by a pump when operating at rated capacity and head",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"RATED INLET PRESSURE",null,null,null,null,null,"rdl:RDS2223470",null,"A <RATED INLET PRESSURE> is an <IndirectProperty> that is a <INLET PRESSURE> that is expected to occur under rated conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED INPUT POWER",null,null,null,null,null,"rdl:RDS13283842",null,"A <RATED INPUT POWER> is an <IndirectProperty> that refers to a <POWER> that a machine or an apparatus receives at full load",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED INSTRUMENT AIR CONSUMPTION",null,null,null,null,null,"rdl:RDS14308822",null,"A <RATED INSTRUMENT AIR CONSUMPTION> is an <IndirectProperty> that refers to an <INSTRUMENT AIR CONSUMPTION> that is the rated (nominal) instrument air consumption of a device at rated conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED OPERATING PRESSURE",null,null,null,null,null,"rdl:RDS12839974",null,"A <RATED OPERATING PRESSURE> is an <IndirectProperty> that refers to a <OPERATING PRESSURE> which is the rated (e.g. design) pressure",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"RATED OUTLET PRESSURE",null,null,null,null,null,"rdl:RDS2229032",null,"A <RATED OUTLET PRESSURE> is an <IndirectProperty> that is a <OUTLET PRESSURE> that is expected to occur under rated conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED OUTPUT POWER",null,null,null,null,null,"rdl:RDS369539",null,"A <RATED OUTPUT POWER> is an <IndirectProperty> that refers to a <POWER> that a motor has been designed to deliver under specified conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED OUTPUT SHAFT POWER",null,null,null,null,null,"rdl:RDS13646740",null,"A <RATED OUTPUT SHAFT POWER> is an <IndirectProperty> that refers to a <SHAFT POWER> at rated conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED POWER",null,null,null,null,null,"rdl:RDS13281757",null,"A <RATED POWER> is an <IndirectProperty> that refers to a <POWER> which a machine or apparatus has been designed to deliver at full load operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED POWER CONSUMPTION",null,null,null,null,null,"rdl:RDS6729014",null,"A <RATED POWER CONSUMPTION> is an <IndirectProperty> that refers to a <POWER CONSUMPTION> at rated conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED PRIMARY WINDING CURRENT",null,null,null,null,null,"rdl:RDS4253799",null,"A <RATED PRIMARY WINDING CURRENT> is an <IndirectProperty> that refers to an r.m.s. value of an <ALTERNATING CURRENT> for which an primary winding has been designed",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED PRIMARY WINDING VOLTAGE",null,null,null,null,null,"rdl:RDS412784",null,"A <RATED PRIMARY WINDING VOLTAGE> is an <IndirectProperty> that refers to a <RATED VOLTAGE> between lines at the terminals of the primary winding on a transformer at rated output",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED ROTATIONAL SPEED",null,null,null,null,null,"rdl:RDS13233604",null,"A <RATED ROTATIONAL SPEED> is an <IndirectProperty> that refers to a <ROTATIONAL SPEED> of a rotating machine working at its full load",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED SECONDARY WINDING CURRENT",null,null,null,null,null,"rdl:RDS4253844",null,"A <RATED SECONDARY WINDING CURRENT> is an <IndirectProperty> that refers to an r.m.s. value of an <ALTERNATING CURRENT> for which an secondary winding has been designed",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED SECONDARY WINDING VOLTAGE",null,null,null,null,null,"rdl:RDS412829",null,"A <RATED SECONDARY WINDING VOLTAGE> is an <IndirectProperty> that refers to a <RATED VOLTAGE> that is the voltage between lines at the terminals of the secondary winding on a transformer at rated output",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED SPEED AT 1/1 LOAD",null,null,null,null,null,"rdl:RDS410714",null,"A <RATED SPEED AT 1/1 LOAD> is an <IndirectProperty> that refers to a <ROTATIONAL SPEED> of an electric rotating machine working at its full load",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"RATED TEMPERATURE",null,null,null,null,null,"rdl:RDS2229899",null,"A <RATED TEMPERATURE> is an <IndirectProperty> that is a <TEMPERATURE > that is expected to occur under rated conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED THRUST",null,null,null,null,null,"rdl:RDS7502934",null,"A <RATED THRUST> is an <IndirectProperty> that refers to a <THRUST> at operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED TORQUE",null,null,null,null,null,"rdl:RDS411479",null,"A <RATED TORQUE> is an <IndirectProperty> that refers to a <TORQUE> at operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED VOLTAGE",null,null,null,null,null,"rdl:RDS412874",null,"A <RATED VOLTAGE> is an <IndirectProperty> that refers to a <VOLTAGE> that is the voltage between lines at the terminals of the machine at rated output",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"RATED VOLUME FLOW RATE",null,null,null,null,null,"rdl:RDS4720595",null,"A <RATED FLOW> is an <IndirectProperty> that is a <VOLUME FLOW RATE> that is expected to occur under rated conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESIDUAL CURRENT",null,null,null,null,null,"rdl:RDS407744",null,"A <RESIDUAL CURRENT> is an <IndirectProperty> that refers to an <ELECTRIC CURRENT> that is the algebraic sum of the instantaneous values of <CURRENT> flowing through all live conductors of a circuit at a point of the electrical installation. (current equal to the sum of the phase currents)",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESIDUAL RESISTIVITY",null,null,null,null,null,"rdl:RDS396539",null,"A <RESIDUAL RESISTIVITY> is an <IndirectProperty> that refers to a <RESISTIVITY> extrapolated to zero thermodynamic <TEMPERATURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESIDUAL VOLTAGE",null,null,null,null,null,"rdl:RDS409184",null,"A <RESIDUAL VOLTAGE> is an <IndirectProperty> that refers to a <VOLTAGE> equal to the sum of the phase-to-earth voltages",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ROTATIONAL SPEED RANGE UPPER LIMIT",null,null,null,null,null,"rdl:RDS14258735",null,"A <ROTATIONAL SPEED RANGE UPPER LIMIT> is an <IndirectProperty> that refers to the <ROTATIONAL SPEED> that is the upper limit of a <ROTATIONAL SPEED RANGE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"ROTATIONAL SPEED RANGE LOWER LIMIT",null,null,null,null,null,"rdl:RDS14258690",null,"A <ROTATIONAL SPEED RANGE LOWER LIMIT> is an <IndirectProperty> that refers to the <ROTATIONAL SPEED> that is the lower limit of a <ROTATIONAL SPEED RANGE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTATIONAL TRIP SPEED",null,null,null,null,null,"rdl:RDS14260355",null,"A <ROTATIONAL TRIP SPEED> is an <IndirectProperty> that refers to a <ROTATIONAL SPEED> limit that automatic shut down the device",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAFE WORKING LOAD",null,null,null,null,null,"rdl:RDS362519",null,"A <SAFE WORKING LOAD> is an <IndirectProperty> that refers to a <FORCE> which is the upper limit for which a lifting equipment is certified",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAND CONTENT RATIO AVERAGED",null,null,null,null,null,"rdl:RDS16628817",null,"A <SAND CONTENT RATIO AVERAGED> is an <IndirectProperty> that refers to a <SAND CONTENT RATIO> that is averaged",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SET POINT",null,null,null,null,null,"rdl:RDS1020060331",null,"A <SET POINT> is an <IndirectProperty> that a desired or target value for a <Property> of a system",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHORT CIRCUIT CURRENT - 0,2 SECOND",null,null,null,null,null,"rdl:RDS5956980",null,"The permissible value of the SHORT CIRCUIT current in a given network component for 0,2 second",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHORT CIRCUIT CURRENT - 0,3 SECOND",null,null,null,null,null,"rdl:RDS5957042",null,"The permissible value of the SHORT CIRCUIT current in a given network component for 0,3 second",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHORT CIRCUIT CURRENT - 0,5 SECOND",null,null,null,null,null,"rdl:RDS5957104",null,"The permissible value of the SHORT CIRCUIT current in a given network component for 0,5 second",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHORT CIRCUIT CURRENT - 1 SECOND",null,null,null,null,null,"rdl:RDS4702533",null,"The permissible value of the SHORT CIRCUIT current in a given network component for one second",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHRINKAGE ALLOWANCE",null,null,null,null,null,"rdl:RDS13292305",null,"A <SHRINKAGE ALLOWANCE> is an <IndirectProperty> that refers to a <RADIAL DISTANCE> which is the shrinkage fit, i.e. the difference in <DIAMETER> of the bore in relation to the shaft of the items that is going to be fit together",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"SOUND PRESSURE LEVEL ALLOWED",null,null,null,null,null,"rdl:RDS7469565",null,"A <SOUND PRESSURE LEVEL ALLOWED> is an <IndirectProperty> that refers to a <SOUND PRESSURE LEVEL> that is allowed",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"SPECIFIC SPEED",null,null,null,null,null,"rdl:RDS402839",null,"A <SPECIFIC SPEED> is an <IndirectProperty> that refers to a <ROTATIONAL SPEED> (in rpm) that a geometrically similar impeller would need to operate in order to deliver 1 L/s of fluid at a head of 1 m (US units : 1 USgal/min at a head of 1 ft ). It is calculated as: nq=(N*(Q^0,5))/(H^0,75) where nq=specific speed, N=rotative speed in revolutions per minute, Q=total pump flow in cubic meters per second, H=head per stage in meters",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"STATIC HEAD",null,null,null,null,null,"rdl:RDS2220948",null,"A <STATIC HEAD> is an <IndirectProperty> that is a specific measurement of liquid pressure above a geodetic datum; it is expressed in units of length, that represent the height of an equivalent static column of that fluid",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"SUCTION HEAD",null,null,null,null,null,"rdl:RDS2220950",null,"A <SUCTION HEAD> is an <IndirectProperty> that is the sum of the <STATIC HEAD> and <VELOCITY HEAD>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"SUPPLY VOLTAGE LOWER LIMIT",null,null,null,null,null,"rdl:RDS373814",null,"A <SUPPLY VOLTAGE LOWER LIMIT> is an <IndirectProperty> that refers to a <SUPPLY VOLTAGE > that is the lowest under which an object is designed to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"SUPPLY VOLTAGE RANGE",null,null,null,null,null,"rdl:RDS1411396881",null,"A <SUPPLY VOLTAGE RANGE> is an <IndirectProperty> that refers to a minimum and maximum value of a <SUPPLY VOLTAGE> that is either delivered or required",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"SUPPLY VOLTAGE UPPER LIMIT",null,null,null,null,null,"rdl:RDS373859",null,"A <SUPPLY VOLTAGE UPPER LIMIT> is an <IndirectProperty> that refers to a <SUPPLY VOLTAGE > that is the highest under which an object is designed to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"TEST PRESSURE",null,null,null,null,null,"rdl:RDS7315228",null,"A <TEST PRESSURE> is an <IndirectProperty> that refers to a <PRESSURE> to which an object should be subjected to test for <LEAKAGE> and structural integrity",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"THINNING ALLOWANCE",null,null,null,null,null,"rdl:RDS13175490",null,"A <THINNING ALLOWANCE> is an <IndirectProperty> that refers to a <THICKNESS> which is the allowable reduction caused by bending",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"TORSIONAL CRITICAL SPEED",null,null,null,null,null,null,null,null,null,null,null,"THIRD TORSIONAL CRITICAL SPEED",null,null,null,null,null,"rdl:RDS14252840",null,"A <THIRDTORSIONAL CRITICAL SPEED> is an <IndiredProperty> that refers to the <SPEED> that is a third torsional critical speed",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"TIME-AVERAGED SOUND INTENSITY",null,null,null,null,null,"rdl:RDS9999359",null,"A <TIME-AVERAGED SOUND INTENSITY> is an <IndirectProperty> that refers to an average value of a <SOUND INTENSITY> per <PeriodInTime>. It is calculated as: I = (1/(t_2 - t_1)).integral [t_1, t_2](i(t).dt) where t_1 and t_2 are the starting and ending time for the integral and i is a <SOUND INTENSITY>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"TOLERANCE(engineering)",null,null,null,null,null,"rdl:RDS1415808661",null,"A <TOLERANCE(engineering)> is an <IndirectProperty> that is a permissible limit or limits of variation in: a physical dimension; a measured value or physical property of a material, manufactured object, system, or service; other measured values",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"TOTAL MASS FLOW",null,null,null,null,null,"rdl:RDS369224",null,"A <TOTAL MASS FLOW> is a <MASS> which is the total flown into/through a unit per unit time",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"TURBULENCE COEFFICIENT",null,null,null,null,null,"rdl:RDS356174",null,"A <TURBULENCE COEFFICIENT> is an <IndirectProperty> that refers to a <PRESSURE DROP> across a flow network due to resistance associated with non-laminar flow of the fluid. This term is defined as a rate dependent term, commonly used as part of a rate dependent skin factor",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER CRITICAL MAGNETIC FLUX DENSITY",null,null,null,null,null,"rdl:RDS397889",null,"An <UPPER CRITICAL MAGNETIC FLUX DENSITY>, for type II superconductors, is an <IndirectProperty> that refers to the threshold <MAGNETIC FLUX DENSITY> for disappearance of bulk superconductivity",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT ABSORBED POWER",null,null,null,null,null,"rdl:RDS14148160",null,"An <UPPER LIMIT ABSORBED POWER> is an <IndirectProperty> that refers to a <POWER> that is the highest absorbed <POWER> by an apparatus during abnormal condition",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT ACCEPTABLE CORROSION RATE",null,null,null,null,null,"rdl:RDS403604",null,"An <UPPER LIMIT ACCEPTABLE CORROSION RATE> is an <IndirectProperty> that refers to a <CORROSION RATE> that is the highest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT AIR CONTENT",null,null,null,null,null,"rdl:RDS13106748",null,"An <UPPER LIMIT AIR CONTENT> is an <IndirectProperty> that refers to a measure describing the maximum (upper limit) of air a defined <VOLUME> of gas, liquid or solid is capable to contain",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT ALLOWABLE DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS14261390",null,"An <UPPER LIMIT ALLOWABLE DIFFERENTIAL PRESSURE> is an <IndirectProperty> that refers to a <DIFFERENTIAL PRESSURE> that is allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT AMBIENT DRY BULB OPERATING TEMPERATURE",null,null,null,null,null,"rdl:RDS14255585",null,"An <UPPER LIMIT AMBIENT DRY BULB OPERATING TEMPERATURE> is an <IndirectProperty> that refers to a <AMBIENT DRY BULB OPERATING TEMPERATURE> that is acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT AMBIENT OPERATING HUMIDITY",null,null,null,null,null,"rdl:RDS8499359",null,"An <UPPER LIMIT AMBIENT OPERATING HUMIDITY> is an <IndirectProperty> that refers to a <HUMIDITY> that is an upper limit of an <AMBIENT OPERATING HUMIDITY>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT AMBIENT OPERATING TEMPERATURE",null,null,null,null,null,"rdl:RDS4231801",null,"An <UPPER LIMIT AMBIENT OPERATING TEMPERATURE> is an <IndirectProperty> that refers to a <TEMPERATURE> which is the highest <AMBIENT TEMPERATURE> under which a device is supposed to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT AMBIENT STORAGE HUMIDITY",null,null,null,null,null,"rdl:RDS8499139",null,"An <UPPER LIMIT AMBIENT STORAGE HUMIDITY> is an <IndirectProperty> that refers to a <HUMIDITY> that is an upper limit of an <AMBIENT STORAGE HUMIDITY>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT AMBIENT STORAGE TEMPERATURE",null,null,null,null,null,"rdl:RDS8798024",null,"An <UPPER LIMIT AMBIENT STORAGE TEMPERATURE> is an <IndirectProperty> that refers to a n ambient storage <TEMPERATURE> which is the highest <AMBIENT TEMPERATURE> under which a device is intended to be stored",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT AMBIENT WET BULB OPERATING TEMPERATURE",null,null,null,null,null,"rdl:RDS14255630",null,"An <UPPER LIMIT AMBIENT WET BULB OPERATING TEMPERATURE> is an <IndirectProperty> that refers to an <AMBIENT WET BULB OPERATING TEMPERATURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT AXIAL LOAD",null,null,null,null,null,"rdl:RDS362024",null,"An <UPPER LIMIT AXIAL LOAD> is an <IndirectProperty> that refers to a <FORCE> that is an upper limit that can be applied along the axis of a <PhysicalObject>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT BEVELLED END INNER BEVEL THICKNESS",null,null,null,null,null,"rdl:RDS379349",null,"An <UPPER LIMIT BEVELLED END INNER BEVEL THICKNESS> is an <IndirectProperty> that refers to a <THICKNESS> that is the upper limit of the inner part of a compound bevel measured from the inside of A <BEVELLED END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT BEVELLED END OFF ANGLE",null,null,null,null,null,"rdl:RDS376424",null,"An <UPPER LIMIT BEVELLED END OFF ANGLE> is an <IndirectProperty> that refers to an <ANGLE> that is the upper limit of the off angle of a <BEVELLED END> pipe fitting",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT BEVELLED END OFF PLANE",null,null,null,null,null,"rdl:RDS376469",null,"An <UPPER LIMIT BEVELLED END OFF PLANE> is an <IndirectProperty> that refers to an <ANGLE> that is the upper limit of the off plane <DISTANCE> from intended position of a <BEVELLED END> pipe fitting",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT BEVELLED END OUTER BEVEL ANGLE",null,null,null,null,null,"rdl:RDS412199",null,"An <UPPER LIMIT BEVELLED END OUTER BEVEL ANGLE> is an <IndirectProperty> that refers to an <ANGLE> that is the upper limit of the outer bevel of a compound bevel measured from the plane of the end cut. A top point of an <ANGLE> is at a <DISTANCE> &#39;bevelled end root face thickness&#39;+ &#39;bevelled end inner bevel thickness&#39; from the inside of <BEVELLED END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT BEVELLED END OUTSIDE DIAMETER",null,null,null,null,null,"rdl:RDS379529",null,"An <UPPER LIMIT BEVELLED END OUTSIDE DIAMETER> is an <IndirectProperty> that refers to a <DIAMETER> that is the upper limit of a <BEVELLED END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT BEVELLED END PLAIN BEVEL ANGLE",null,null,null,null,null,"rdl:RDS412244",null,"An <UPPER LIMIT BEVELLED END PLAIN BEVEL ANGLE> is an <IndirectProperty> that refers to an <ANGLE> that is the upper limit of the bevel of a plain <BEVELLED END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT BEVELLED END ROOT FACE THICKNESS",null,null,null,null,null,"rdl:RDS411974",null,"An <UPPER LIMIT BEVELLED END ROOT FACE THICKNESS> is an <IndirectProperty> that refers to a <THICKNESS> that is the upper limit of a <BEVELLED END> root face",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT BEVELLED END WALL THICKNESS",null,null,null,null,null,"rdl:RDS412064",null,"An <UPPER LIMIT BEVELLED END WALL THICKNESS> is an <IndirectProperty> that refers to a <WALL THICKNESS> that is the upper limit of a <BEVELLED END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT BRAKE FORCE",null,null,null,null,null,"rdl:RDS7924986",null,"An <UPPER LIMIT BRAKE FORCE> is an <IndirectProperty> that refers to a <BRAKE FORCE> that is the highest which can be applied without causing damage",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT BREAKDOWN TORQUE MULTIPLIER",null,null,null,null,null,"rdl:RDS13649425",null,"An <UPPER LIMIT BREAKDOWN TORQUE MULTIPLIER> is an <IndirectProperty> that refers to a <BREAKDOWN TORQUE MULTIPLIER> that is the highest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT BREAKOUT TORQUE",null,null,null,null,null,"rdl:RDS16741236",null,"An <UPPER LIMIT BREAKOUT TORQUE> is an <IndirectProperty> that refers to a <BREAKOUT TORQUE> which is the maximum necessary to start turning a valve spindle",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT BREAKOUT TORQUE AT BALANCED DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS16741349",null,"An <UPPER LIMIT BREAKOUT TORQUE AT BALANCED DIFFERENTIAL PRESSURE> is an <IndirectProperty> that refers to a <BREAKOUT TORQUE> that is the maximum allowed when the line <PRESSURE> is equal across the valve",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT BREAKOUT TORQUE AT MAX DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS16741428",null,"An <UPPER LIMIT BREAKOUT TORQUE AT MAX DIFFERENTIAL PRESSURE> is an <IndirectProperty> that refers to a <BREAKOUT TORQUE> that is the maximum allowed when the line <DIFFERENTIAL PRESSURE> is the maximum across the valve",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT CAPACITY (volume flow rate)",null,null,null,null,null,"rdl:RDS7354022",null,"An <UPPER LIMIT CAPACITY (volume flow rate)> is an <IndirectProperty> that refers to a <CAPACITY (volume flow rate)> which is the highest possible",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT CENTER TO BOTTOM OF SOCKET-WELDING END LENGTH",null,null,null,null,null,"rdl:RDS377279",null,"An <UPPER LIMIT CENTER TO BOTTOM OF SOCKET-WELDING END LENGTH> is an <IndirectProperty> that refers to a centre to bottom of socket welding end <LENGTH> that is the upper limit for a <LENGTH> from a centre of a pipe fitting to a bottom of a socket of a <SOCKET WELDING END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT CONDUCTOR CROSS-SECTION AREA",null,null,null,null,null,"rdl:RDS6653680",null,"An <UPPER LIMIT CONDUCTOR CROSS-SECTION AREA> is an <IndirectProperty> that refers to a <CROSS-SECTION AREA> which is the largest <CROSS-SECTION AREA> a cable conductor can have to fit into a terminal clamp",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT CONTINUOUS ROTATIONAL SPEED",null,null,null,null,null,"rdl:RDS13591348",null,"An <UPPER LIMIT CONTINUOUS ROTATIONAL SPEED> is an <IndirectProperty> that refers to a <ROTATIONAL SPEED> which trip the compressor",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT CONTINUOUS STABLE FLOW",null,null,null,null,null,"rdl:RDS7368340",null,"An <UPPER LIMIT CONTINUOUS STABLE FLOW> is an <IndirectProperty> that refers to a <VOLUME FLOW RATE> that is the highest possible rate at which no flow recirculation at impeller suction will take place and hence no unwished increase of the vibration level",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT CONTROLLABLE VALVE FLOW COEFFICIENT",null,null,null,null,null,"rdl:RDS7509704",null,"An <UPPER LIMIT CONTROLLABLE VALVE FLOW COEFFICIENT> is an <IndirectProperty> that refers to a <CONTROLLABLE VALVE FLOW COEFFICIENT> that is the maximum allowable for a <CONTROL VALVE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT CROSS CENTER TO OUTLET END LENGTH",null,null,null,null,null,"rdl:RDS375884",null,"An <UPPER LIMIT CROSS CENTER TO OUTLET END LENGTH> is an <IndirectProperty> that refers to a <CENTER TO END LENGTH> which is the upper limit from a cross center point to an outlet end",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT CROSS CENTER TO RUN END LENGTH",null,null,null,null,null,"rdl:RDS375929",null,"An <UPPER LIMIT CROSS CENTER TO RUN END LENGTH> is an <IndirectProperty> that refers to a <CENTER TO END LENGTH> which is the upper limit from a cross center point to a run end",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT CROWN RADIUS",null,null,null,null,null,"rdl:RDS371519",null,"An <UPPER LIMIT CROWN RADIUS> is an <IndirectProperty> that refers to a <RADIUS> of a <TORISPHERICAL HEAD> that is the largest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT CROWN SECTION THICKNESS",null,null,null,null,null,"rdl:RDS372104",null,"An <UPPER LIMIT CROWN SECTION THICKNESS> is an <IndirectProperty> that refers to a <THICKNESS> that is the largest allowable for a crown section",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT CYLINDRICAL SECTION THICKNESS",null,null,null,null,null,"rdl:RDS372014",null,"An <UPPER LIMIT CYLINDRICAL SECTION THICKNESS> is an <IndirectProperty> that refers to a <THICKNESS> that is the largest allowable for a cylindrical section",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT DIAMETER",null,null,null,null,null,"rdl:RDS2225080",null,"An <UPPER LIMIT DIAMETER> is an <IndirectProperty> that refers to a <DIAMETER> which is the largest acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT DIAMETER FOR BASE OF FLANGED BASE FITTING",null,null,null,null,null,"rdl:RDS378494",null,"An <UPPER LIMIT DIAMETER FOR BASE OF FLANGED BASE FITTING> is an <IndirectProperty> that refers to a <DIAMETER> which is the upper limit for the base of a flanged base fitting",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT DISPLACEMENT",null,null,null,null,null,"rdl:RDS14259860",null,"An <UPPER LIMIT DISPLACEMENT> is an <IndirectProperty> that refers to a <DISPLACEMENT> that is the highest allowed or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT DISPLACEMENT PER REVOLUTION",null,null,null,null,null,"rdl:RDS5957377",null,"An <UPPER LIMIT DISPLACEMENT PER REVOLUTION> is an <IndirectProperty> that refers to a <VOLUME> which is the largest volume of liquid a variable displacement pump or hydraulic motor is able to displace or consume per one complete revolution of its shaft",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT DISTANCE DETECTOR TO TRANSMITTER",null,null,null,null,null,"rdl:RDS7861964",null,"An <UPPER LIMIT DISTANCE DETECTOR TO TRANSMITTER> is an <IndirectProperty> that refers to a <LENGTH OF PATH> that is the largest acceptable distance between a detector and a transmitter",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT DISTANCE FLOW ELEMENT TO TRANSMITTER",null,null,null,null,null,"rdl:RDS7482348",null,"An <UPPER LIMIT DISTANCE FLOW ELEMENT TO TRANSMITTER> is an <IndirectProperty> that refers to a <LENGTH OF PATH> that is the largest acceptable <DISTANCE> between a flow element and a flow transmitter",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT DISTANCE LEVEL ELEMENT TO TRANSMITTER",null,null,null,null,null,"rdl:RDS7843320",null,"An <UPPER LIMIT DISTANCE LEVEL ELEMENT TO TRANSMITTER> is an <IndirectProperty> that refers to a <LENGTH OF PATH> that is the largest acceptable <DISTANCE> between a level element and a level transmitter",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT ELBOW ANGLE",null,null,null,null,null,"rdl:RDS374714",null,"An <UPPER LIMIT ELBOW ANGLE> is an <IndirectProperty> that refers to an <ANGLE> that is the upper limit between centrelines of an <ELBOW>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT ELECTRIC CURRENT",null,null,null,null,null,"rdl:RDS13175670",null,"An <UPPER LIMIT ELECTRIC CURRENT> is an <IndirectProperty> that refers to an <ELECTRIC CURRENT> which is the highest allowable under a set of conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT END TO END LENGTH",null,null,null,null,null,"rdl:RDS376604",null,"An <UPPER LIMIT END TO END LENGTH> is an <IndirectProperty> that refers to an <END TO END LENGTH> that is the longest acceptable length",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT FLAMMABILITY CONCENTRATION",null,null,null,null,null,"rdl:RDS364949",null,"An <UPPER LIMIT FLAMMABILITY CONCENTRATION> is an <IndirectProperty> that refers to a <CONCENTRATION> that is the highest flammability limit of a flammable substance in a mixture with air that can burn",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT FLOW RATE",null,null,null,null,null,"rdl:RDS8276324",null,"An <UPPER LIMIT FLOW RATE> is an <IndirectProperty> to a <VOLUME FLOW RATE> that is the maximum acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT FORCE",null,null,null,null,null,"rdl:RDS12146188",null,"An <UPPER LIMIT FORCE> is an <IndirectProperty> that refers to a <FORCE> which is an upper limit which can be applied to a physical object",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT FREQUENCY",null,null,null,null,null,"rdl:RDS5956465",null,"An <UPPER LIMIT FREQUENCY> is an <IndirectProperty> that refers to an <ELECTRICAL FREQUENCY> that is the highest under which a device is designed to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT GAS LIFT PRESSURE",null,null,null,null,null,"rdl:RDS16634577",null,"An <UPPER LIMIT GAS LIFT PRESSURE> is an <IndirectProperty> that refers to a <GAS LIFT PRESSURE> which is the highest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT GAS LIFT TEMPERATURE",null,null,null,null,null,"rdl:RDS16634307",null,"An <UPPER LIMIT GAS LIFT TEMPERATURE> is an <IndirectProperty> that refers to an <GAS LIFT TEMPERATURE> which is the highest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT GAS LIFT VOLUME",null,null,null,null,null,"rdl:RDS16623777",null,"An <UPPER LIMIT GAS LIFT VOLUME> is an <IndirectProperty> that refers to a <GAS LIFT VOLUME> which is the highest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT HEAD AT RATED SPEED",null,null,null,null,null,"rdl:RDS14251985",null,"An <UPPER LIMIT HEAD AT RATED SPEED> is an <IndirectProperty> that refers to a <HEAD> that is the maximum at rated speed",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT HEAD WITH RATED IMPELLER DIAMETER",null,null,null,null,null,"rdl:RDS404099",null,"An <UPPER LIMIT HEAD WITH RATED IMPELLER DIAMETER> is an <IndirectProperty> that refers to a <HEAD> that is the largest a centrifugal pump can produce when using a impeller with rated diameter",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT HEIGHT",null,null,null,null,null,"rdl:RDS11379636",null,"An <UPPER LIMIT HEIGHT> is an <IndirectProperty> that refers to a <HEIGHT> that is the highest acceptable height",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT HYDRAULIC POWER",null,null,null,null,null,"rdl:RDS413279",null,"An <UPPER LIMIT HYDRAULIC POWER> is an <IndirectProperty> that refers to an <HYDRAULIC POWER> when operating at upper limit capacity of a <PUMP>.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT IMPEDANCE",null,null,null,null,null,"rdl:RDS362204",null,"An <UPPER LIMIT IMPEDANCE> is an <IndirectProperty> that refers to an <IMPEDANCE> that is the allowable upper limit of an external impedance",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT INLET FLOW RATE",null,null,null,null,null,"rdl:RDS400634",null,"An <UPPER LIMIT INLET FLOW RATE> is an <IndirectProperty> that refers to a <VOLUME FLOW RATE> which is the highest allowed at an <INLET>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT INLET TEMPERATURE",null,null,null,null,null,"rdl:RDS400319",null,"An <UPPER LIMIT INLET TEMPERATURE> is an <IndirectProperty> that refers to an <INLET TEMPERATURE> which is the highest allowable at an <INLET>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT INNER KNUCLE RADIUS",null,null,null,null,null,"rdl:RDS371609",null,"An <UPPER LIMIT INNER KNUCLE RADIUS> is an <IndirectProperty> that refers to an inner knuckle <RADIUS> that is the largest acceptable inner knuckle radius",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT INPUT POWER",null,null,null,null,null,"rdl:RDS13285100",null,"An <UPPER LIMIT INPUT POWER> is an <IndirectProperty> that refers to a <POWER> which is the highest tolerable an object or apparatus can receive",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT INSIDE DIAMETER",null,null,null,null,null,"rdl:RDS14187365",null,"An <UPPER LIMIT INSIDE DIAMETER> is an <IndirectProperty> that refers to an <INSIDE DIAMETER> which is the largest allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT LOCKED ROTOR TORQUE MULTIPLIER",null,null,null,null,null,"rdl:RDS13649470",null,"An <UPPER LIMIT LOCKED ROTOR TORQUE MULTIPLIER> is an <IndirectProperty> that refers to a <LOCKED ROTOR TORQUE MULTIPLIER> that is the highest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT LOWERING SPEED",null,null,null,null,null,"rdl:RDS7924681",null,"An <UPPER LIMIT LOWERING SPEED> is an <IndirectProperty> that refers to a <LOWERING SPEED> that is the highest allowable when lowering an object",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT MACH NUMBER",null,null,null,null,null,"rdl:RDS14251940",null,"An <UPPER LIMIT MACH NUMBER> is an <IndirectProperty> that refers to a <MACH NUMBER> that is the maximum allowable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT MAINTENANCE WEIGHT",null,null,null,null,null,"rdl:RDS402389",null,"An <UPPER LIMIT MAINTENANCE WEIGHT> is an <IndirectProperty> that refers to a <WEIGHT> that is the maximum allowed for an equipment in a maintenance operation",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT MASS FLOW RATE",null,null,null,null,null,"rdl:RDS14118640",null,"An <UPPER LIMIT MASS FLOW RATE> is an <IndirectProperty> that refers to a <MASS FLOW RATE> that is the highest expected flow",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT MEASURED OPEN BOREHOLE PRESSURE",null,null,null,null,null,"rdl:RDS17705320",null,"An <UPPER LIMIT MEASURED OPEN BOREHOLE PRESSURE> is an <IndirectProperty> that refers to an open <BOREHOLE PRESSURE> that is the highest measured open borehole pressure in a reporting period measured during a formation pressure test",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT MEASURING RANGE",null,null,null,null,null,"rdl:RDS373544",null,"The highest value of the measured variable to which a device can be adjusted to measure within a specified accuracy",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT NPSHA",null,null,null,null,null,"rdl:RDS14331136",null,"An <UPPER LIMIT NPSHA> is an <IndirectProperty> that refers to a <NPSHA> that is the maximum that can occur",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT NUCLEON DOSE RATE",null,null,null,null,null,"rdl:RDS7943720",null,"An <UPPER LIMIT NUCLEON DOSE RATE> is an <IndirectProperty> that refers to a <NUCLEON DOSE RATE> which is the highest allowed at an surface.",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT NUMBER OF IMPELLERS",null,null,null,null,null,"rdl:RDS14253020",null,"An <UPPER LIMIT NUMBER OF IMPELLERS> is an <IndirectProperty> that refers to a <COUNT> of a maximum numbers of impellers on a <COMPRESSOR>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT NUMBER OF PLATES",null,null,null,null,null,"rdl:RDS14119135",null,"An <UPPER LIMIT NUMBER OF PLATES> is an <IndirectProperty> that refers to a <COUNT> of the number of plates which is the highest allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OF TIP VELOCITY AT RATED TRIP SPEED",null,null,null,null,null,"rdl:RDS14254010",null,"An <UPPER LIMIT OF TIP VELOCITY AT RATED TRIP SPEED> is an <IndirectProperty> that refers to a maximum impeller tip <VELOCITY> at rated trip speed",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OF TIP VELOCITY AT UPPER LIMIT CONTINOUS SPEED",null,null,null,null,null,"rdl:RDS14253560",null,"An <UPPER LIMIT OF TIP VELOCITY AT UPPER LIMIT CONTINOUS SPEED> is an <IndirectProperty> that refers to a maximum impeller tip <VELOCITY> at upper limit continous speed",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OPERATING TEMPERATURE",null,null,null,null,null,"rdl:RDS360539",null,"An <UPPER LIMIT OPERATING TEMPERATURE> is an <IndirectProperty> that refers to an <OPERATING TEMPERATURE> that is the highest at which a functional or physical object is expected to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OPERATING PRESSURE",null,null,null,null,null,"rdl:RDS1469251881",null,"An <UPPER LIMIT OPERATING PRESSURE> is an <IndirectProperty> that refers to an <OPERATING PRESSURE> which is the highest under which an object is designed to operate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OPERATING PRESSURE AT DESIGN TEMPERATURE",null,null,null,null,null,"rdl:RDS402569",null,"An <UPPER LIMIT OPERATING PRESSURE AT DESIGN TEMPERATURE> is an <IndirectProperty> that refers to an <OPERATING PRESSURE> which is the highest under which an object is designed to operate at the highest allowable <TEMPERATURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OPERATING STRESS",null,null,null,null,null,"rdl:RDS13113736",null,"An <UPPER LIMIT OPERATING STRESS> is an <IndirectProperty> that refers to an <OPERATING STRESS> which is the highest stress occuring during operation",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OPERATING VOLTAGE",null,null,null,null,null,"rdl:RDS7922664",null,"An <UPPER LIMIT OPERATING VOLTAGE> is an <IndirectProperty> that refers to a <OPERATING VOLTAGE> that is the maximum that can be tolerated under normal working conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OPERATING VOLUME",null,null,null,null,null,"rdl:RDS360269",null,"An <UPPER LIMIT OPERATING VOLUME> is an <IndirectProperty> that refers to an <OPERATING VOLUME> which is the highest volume under which the object is expected to work",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT ORIFICE BORE DIAMETER",null,null,null,null,null,"rdl:RDS17701245",null,"An <UPPER LIMIT ORIFICE BORE DIAMETER> is an <IndirectProperty> that refers to an <ORIFICE BORE DIAMETER> that is the maximum possible for a given orifice configuration",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OUTLET PRESSURE",null,null,null,null,null,"rdl:RDS402659",null,"An <UPPER LIMIT OUTLET PRESSURE> is an <IndirectProperty> that refers to an <OUTLET PRESSURE> that is the highest acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OUTLET TEMPERATURE",null,null,null,null,null,"rdl:RDS14261255",null,"An <UPPER LIMIT OUTLET TEMPERATURE> is an <IndirectProperty> that refers to an <OUTLET TEMPERATURE> that is the highest acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OUTPUT POWER",null,null,null,null,null,"rdl:RDS13285162",null,"An <UPPER LIMIT OUTPUT POWER> is an <IndirectProperty> that refers to an <OUTPUT POWER> which is the highest tolerable power an object or apparatus can deliver",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OUTSIDE DIAMETER",null,null,null,null,null,"rdl:RDS371744",null,"An <UPPER LIMIT OUTSIDE DIAMETER> is an <IndirectProperty> that refers to an <OUTSIDE DIAMETER> that is the largest allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OUTSIDE DIAMETER OF FLANGED END",null,null,null,null,null,"rdl:RDS377369",null,"An <UPPER LIMIT OUTSIDE DIAMETER OF FLANGED END> is an <IndirectProperty> that refers to an <OUTSIDE DIAMETER> which is the maximum allowable of a <FLANGED END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OVERPRESSURE PROTECTION",null,null,null,null,null,"rdl:RDS7456620",null,"An <UPPER LIMIT OVERPRESSURE PROTECTION> is an <IndirectProperty> that refers to a <PRESSURE> that is the highest an instrument is able to withstand without the need for recalibration",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT OVERTEMPERATURE PROTECTION",null,null,null,null,null,"rdl:RDS7349047",null,"An <UPPER LIMIT OVERTEMPERATURE PROTECTION> is an <IndirectProperty> that refers to a <TEMPERATURE> that is the highest an instrument is able to withstand without the need for recalibration",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT PERMISSIBLE STARTING CURRENT",null,null,null,null,null,"rdl:RDS412649",null,"An <UPPER LIMIT PERMISSIBLE STARTING CURRENT> is an <IndirectProperty> that refers to a <STARTING CURRENT> that is the maximum peak-current occurring when starting an <ELECTRIC ENERGY CONVERTER>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT POWER",null,null,null,null,null,"rdl:RDS410354",null,"An <UPPER LIMIT POWER> is an <IndirectProperty> that refers to a <POWER> which is the highest an object or apparatus can generate, transmit or tolerate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT POWER CONSUMPTION",null,null,null,null,null,"rdl:RDS8020754",null,"An <UPPER LIMIT POWER CONSUMPTION> is an <IndirectProperty> that refers to a <POWER CONSUMPTION> that is the highest amount of power an apparatus will consume",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT POWER CONSUMPTION WITH RATED IMPELLER",null,null,null,null,null,"rdl:RDS4310017",null,"An <UPPER LIMIT POWER CONSUMPTION WITH RATED IMPELLER> is an <IndirectProperty> that refers to a <POWER CONSUMPTION> that is the highest absorbed power by a pump when it is equipped with an impeller with rated diameter",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT PRESSURE",null,null,null,null,null,"rdl:RDS400814",null,"An <UPPER LIMIT PRESSURE> is an <IndirectProperty> that refers to a <PRESSURE> that is the highest allowable pressure",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT PRESSURE DROP",null,null,null,null,null,"rdl:RDS7452620",null,"An <UPPER LIMIT PRESSURE DROP> is an <IndirectProperty> that refers to a <PRESSURE DROP> that is the highest allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT PRESSURE AT DESIGN TEMPERATURE",null,null,null,null,null,"rdl:RDS7477840",null,"An <UPPER LIMIT PRESSURE AT DESIGN TEMPERATURE> is an <IndirectProperty> that refers to a <DESIGN PRESSURE> which is the highest continous (non-shock) <PRESSURE> under which an object is designed to operate at the highest allowable <TEMPERATURE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT PRESSURE DROP AT NORMAL FLOW",null,null,null,null,null,"rdl:RDS14178344",null,"An <UPPER LIMIT PRESSURE DROP AT NORMAL FLOW> is an <IndirectProperty> that refers to a <PRESSURE DROP> at a normal <FLOW RATE>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT PRESSURE RATING-DYNAMIC",null,null,null,null,null,"rdl:RDS400994",null,"An <UPPER LIMIT PRESSURE RATING-DYNAMIC> is an <IndirectProperty> that refers to a <PRESSURE RATING-DYNAMIC> that is the highest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT PRESSURE RATING-STATIC",null,null,null,null,null,"rdl:RDS401129",null,"An <UPPER LIMIT PRESSURE RATING-STATIC> is an <IndirectProperty> that refers to a <PRESSURE RATING-DYNAMIC> that is the highest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT PRESTRESS",null,null,null,null,null,"rdl:RDS12147105",null,"An <UPPER LIMIT PRESTRESS> is an <IndirectProperty> that refers to a prestress <FORCE> that is the maximum allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT RADIAL LOAD",null,null,null,null,null,"rdl:RDS362069",null,"An <UPPER LIMIT RADIAL LOAD> is an <IndirectProperty> that refers to a <RADIAL LOAD> that is the maximum acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT RAISING SPEED",null,null,null,null,null,"rdl:RDS7924501",null,"An <UPPER LIMIT RAISING SPEED> is an <IndirectProperty> that refers to a <RAISING SPEED> that is the highest permissible speed when raising an object",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT RETURN PRESSURE",null,null,null,null,null,"rdl:RDS16759899",null,"An <UPPER LIMIT RETURN PRESSURE> is an <IndirectProperty> that refers to a <RETURN PRESSURE> which is the maximum allowed in a return line",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT RETURN TEMPERATURE",null,null,null,null,null,"rdl:RDS14260400",null,"An <UPPER LIMIT RETURN TEMPERATURE> is an <IndirectProperty> that refers to a <RETURN TEMPERATURE> which is the maximum allowed in a return line",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT RING JOINT GROOVE BOTTOM RADIUS",null,null,null,null,null,"rdl:RDS368639",null,"An <UPPER LIMIT RING JOINT GROOVE BOTTOM RADIUS> is an <IndirectProperty> that refers to a <RING JOINT GROOVE BOTTOM RADIUS> that is the largest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT ROTATIONAL SPEED",null,null,null,null,null,"rdl:RDS402479",null,"An <UPPER LIMIT ROTATIONAL SPEED> is an <IndirectProperty> that refers to a <ROTATIONAL SPEED> which is the highest at which the manufacturer&#39;s design will permit continous operation",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT SHAFT INPUT POWER",null,null,null,null,null,"rdl:RDS13599072",null,"An <UPPER LIMIT SHAFT INPUT POWER> is an <IndirectProperty> that refers to a <SHAFT INPUT POWER> that is the highest required at peak operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT SHUT OFF DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS7498180",null,"An <UPPER LIMIT SHUT OFF DIFFERENTIAL PRESSURE> is an <IndirectProperty> that refers to a <DIFFERENTIAL PRESSURE> that is the maximum acceptable or expected in case of a shut-off",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT SOUND POWER LEVEL AT NOMINAL LOAD",null,null,null,null,null,"rdl:RDS13620210",null,"An <UPPER LIMIT SOUND POWER LEVEL AT NOMINAL LOAD> is an <IndirectProperty> that refers to a <SOUND POWER LEVEL> at nominal load that is the highest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT SOUND PRESSURE LEVEL",null,null,null,null,null,"rdl:RDS7510060",null,"An <UPPER LIMIT SOUND PRESSURE LEVEL> is an <IndirectProperty> that refers to a <SOUND PRESSURE LEVEL> that is the highest allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT SPECIFIC GRAVITY AT TEMPERATURE",null,null,null,null,null,"rdl:RDS404369",null,"An <UPPER LIMIT SPECIFIC GRAVITY AT TEMPERATURE> is an <IndirectProperty> that refers to a <SPECIFIC GRAVITY> that is the highest acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT SPRING FORCE",null,null,null,null,null,"rdl:RDS11553147",null,"An <UPPER LIMIT SPRING FORCE> is an <IndirectProperty> that refers to a <SPRING FORCE> that is the maximum acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT STARTING CURRENT MULTIPLIER",null,null,null,null,null,"rdl:RDS13649740",null,"An <UPPER LIMIT STARTING CURRENT MULTIPLIER> is an <IndirectProperty> that refers to a <STARTING CURRENT MULTIPLIER> that is the highest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT STARTING TIME",null,null,null,null,null,"rdl:RDS412604",null,"An <UPPER LIMIT STARTING TIME> is an <IndirectProperty> that refers to a <STARTING TIME> which is the longest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT STEAM CONSUMPTION",null,null,null,null,null,"rdl:RDS14261525",null,"An <UPPER LIMIT STEAM CONSUMPTION> is an <IndirectProperty> that refers to a <STEAM CONSUMPTION> that is the highest amount of steam an apparatus will consume",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT TAPER ANGLE",null,null,null,null,null,"rdl:RDS367199",null,"An <UPPER LIMIT TAPER ANGLE> is an <IndirectProperty> that refers to a <TAPER ANGLE> that is the largest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT TEE CENTER TO OUTLET END LENGTH",null,null,null,null,null,"rdl:RDS375749",null,"An <UPPER LIMIT TEE CENTER TO OUTLET END LENGTH> is an <IndirectProperty> that refers to a <CENTER TO END LENGTH> which is the upper limit from a tee center point to an outlet end",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT TEE CENTER TO RUN END LENGTH",null,null,null,null,null,"rdl:RDS375704",null,"An <UPPER LIMIT TEE CENTER TO RUN END LENGTH> is an <IndirectProperty> that refers to a center to a <CENTER TO END LENGTH> which is the upper limit from the tee center point to the run end",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT TEMPERATURE RISE",null,null,null,null,null,"rdl:RDS13649560",null,"An <UPPER LIMIT TEMPERATURE RISE> is an <IndirectProperty> that refers to a <TEMPERATURE RISE> that is the highest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT TENSILE STRESS",null,null,null,null,null,"rdl:RDS403829",null,"An <UPPER LIMIT TENSILE STRESS> is an <IndirectProperty> that refers to a <TENSILE STRESS> that is a highest allowable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT THICKNESS OF BASE FOR FLANGED BASE FITTING",null,null,null,null,null,"rdl:RDS378044",null,"An <UPPER LIMIT THICKNESS OF BASE FOR FLANGED BASE FITTING> is an <IndirectProperty> that refers to a <THICKNESS> which is the upper limit of a base for a flanged base fitting",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT THICKNESS OF FLANGED END",null,null,null,null,null,"rdl:RDS377459",null,"An <UPPER LIMIT THICKNESS OF FLANGED END> is an <IndirectProperty> that refers to a <THICKNESS> which is the upper limit for a <FLANGED PIPE END>",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT THICKNESS OF RIBS FOR FLANGED BASE FITTING",null,null,null,null,null,"rdl:RDS378179",null,"An <UPPER LIMIT THICKNESS OF RIBS FOR FLANGED BASE FITTING> is an <IndirectProperty> that refers to a <THICKNESS> which is the upper limit for the ribs for a flanged base fitting",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT THRUST",null,null,null,null,null,"rdl:RDS7502872",null,"An <UPPER LIMIT THRUST> is an <IndirectProperty> that refers to a <THRUST> that is the highest which an object can generate, transmit or tolerate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT TIME CONSTANT MULTIPLIER",null,null,null,null,null,"rdl:RDS13649515",null,"An <UPPER LIMIT TIME CONSTANT MULTIPLIER> is an <IndirectProperty> that refers to a <TIME CONSTANT MULTIPLIER> that is the highest acceptable",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT TORQUE",null,null,null,null,null,"rdl:RDS5925856",null,"An <UPPER LIMIT TORQUE> is an <IndirectProperty> that refers to a <TORQUE> that is the highest which an object can generate, transmit or tolerate",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT TRACTION FORCE",null,null,null,null,null,"rdl:RDS5927042",null,"An <UPPER LIMIT TRACTION FORCE> is an <IndirectProperty> that refers to a <TRACTION FORCE> that is the highest allowed to be exerted on an electrical cable, wire or eg. a backstay bracket",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT VALVE FLOW COEFFICIENT",null,null,null,null,null,"rdl:RDS7509462",null,"An <UPPER LIMIT VALVE FLOW COEFFICIENT> is an <IndirectProperty> that refers to a <VALVE FLOW COEFFICIENT> that is the largest acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT VELOCITY",null,null,null,null,null,"rdl:RDS13107616",null,"An <UPPER LIMIT VELOCITY> is an <IndirectProperty> that refers to a <VELOCITY> which is the highest acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT VELOCITY AT NORMAL FLOW",null,null,null,null,null,"rdl:RDS14176949",null,"An <UPPER LIMIT VELOCITY AT NORMAL FLOW> is an <IndirectProperty> that refers to an <UPPER LIMIT VELOCITY> at a normal flow",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT VIBRATION DISPLACEMENT",null,null,null,null,null,"rdl:RDS14249690",null,"An <UPPER LIMIT VIBRATION DISPLACEMENT> is an <IndirectProperty> that refers to a <VIBRATION DISPLACEMENT> which is the highest acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT VOLTAGE",null,null,null,null,null,"rdl:RDS7922540",null,"An <UPPER LIMIT VOLTAGE> is an <IndirectProperty> that refers to a <VOLTAGE> which is the highest acceptable or expected",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT VOLUME",null,null,null,null,null,"rdl:RDS360359",null,"An <UPPER LIMIT VOLUME> is an <IndirectProperty> that refers to a <VOLUME> that is the largest allowable for a given set of conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"UPPER LIMIT WALL THICKNESS",null,null,null,null,null,"rdl:RDS377639",null,"An <UPPER LIMIT WALL THICKNESS> is an <IndirectProperty> that refers to a <WALL THICKNESS> that is the largest allowable for a given set of conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"W/N FREQUENCY RATIO",null,null,null,null,null,"rdl:RDS4316908428",null,"A <W/N FREQUENCY RATIO> is an <IndirectProperty> that is the <RATIO> between wake frequency and natural frequency under operating conditions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"WEIGHTED AVERAGE BOILING TEMPERATURE",null,null,null,null,null,"rdl:RDS2299438521",null,"A <WEIGHTED AVERAGE BOILING TEMPERATURE> is an <IndirectProperty> that refers to a <BOILING TEMPERATURE> that is the average of the boiling temperatures of a number of fractions, averaged proportional to the weights of those fractions",null,null,null,null,null,"dm:ClassOfIndirectProperty"]
[null,null,"IndirectProperty",null,null,null,null,null,null,null,null,null,null,null,"YEAR AVERAGE DENSITY",null,null,null,null,null,"rdl:RDS5059502425",null,"A <YEAR AVERAGE DENSITY> is an <IndirectProperty> that refers to a <DENSITY> that is the average of all measured densities during a <DURATION> of one year",null,null,null,null,null,"dm:ClassOfIndirectProperty"]