{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["RDL browser","Settings","about","Results1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"RDL browser","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[[0,0,0,4]]}
["RDL2 browser to spreadsheet tool version 75",null,null,null,null,null,"Endpoint: http://data.15926.org/rdl/"]
["Contact: onno.paap@gmail.com",null,null,null,null,"Action","ENERGY STORAGE","http://data.15926.org/rdl/RDS2222105"]
[null,null,null,null,null,"Action","ENERGY STORAGE CAPACITOR","http://data.15926.org/rdl/RDS1090169"]
["Search:","ENERGY STORAGE"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Note: first set coloring on in Settings"]
[null,"Coloring (containing this string will give this color)"]
[null,"ClassOfFunctionalObject"]
[null,"ClassOfInanimatePhysicalObject "]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Namespace replacer (definition containing this string replaces the namespace)"]
[null,"API","API:"]
[null,"ASME","ASME:"]
[null,"ASTM","ASTM:"]
[null,"DIN","DIN:"]
[null,"EN","EN:"]
[null,"ISO","ISO:"]
[null,"NORSOK","NOR:"]
[null,"NPD","NOR:"]
[null,"NS","NOR:"]
[null,"ROSEMOUNT","ROS:"]
[null,"SAE","SAE:"]
[null,"SIEMENS","SIE:"]
[null,"SKOTSELV","SKOT:"]
[null,"TWR","TWR:"]

{"sheet":"Settings","index":1,"n_rows":87,"n_cols":8,"rows_kept":87,"cut":false,"hidden":true,"merged":[]}
["Setting name","Select name","OnKey","Value","Status","RDLType"]
["Endpoint","RDL2 (15926.org)",null,"http://data.15926.org/rdl/","Current",null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA RDL",null,"http://data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA Staging",null,"http://staging.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA SVRDL",null,"http://svrdl.community.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P4",null,"http://posccaesar.org/p4/sparql",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P12",null,"http://sti.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","Localhost",null,"http://localhost:8890/sparql/",null,null,null,"Note: end address always with a slash (/)"]
[]
["gBaseNamespace",null,"http://data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://staging.data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://svrdl.community.data.posccaesar.org/rdl/","http://svrdl.community.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://posccaesar.org/p4/sparql","http://posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://sti.data.posccaesar.org/rdl/","http://sti.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://localhost:8890/sparql/","http://data.15926.org/rdl/",null,"RDL2"]
["gKeepSettings",null,null,"T"]
["gShowDeprecated",null,null,"T"]
["gColoring",null,null,"T"]
["gNamespaceReplacing",null,null,"F"]
["gHyperlinkReplacing",null,null,"F"]
[]
["Endpoint","aisi",null,"http://data.15926.org/aisi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ansi",null,"http://data.15926.org/ansi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","api",null,"http://data.15926.org/api/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","all",null,"http://data.15926.org/all/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","asme",null,"http://data.15926.org/asme/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","astm",null,"http://data.15926.org/astm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","atex",null,"http://data.15926.org/atex/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","bs",null,"http://data.15926.org/bs/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","din",null,"http://data.15926.org/din/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dm",null,"http://data.15926.org/dm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dnv",null,"http://data.15926.org/dnv/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","edm",null,"http://data.15926.org/edm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","en",null,"http://data.15926.org/en/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","eu",null,"http://data.15926.org/eu/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iec",null,"http://data.15926.org/iec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ieee",null,"http://data.15926.org/ieee/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iso",null,"http://data.15926.org/iso/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","lci",null,"http://data.15926.org/lci/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","mss",null,"http://data.15926.org/mss/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nace",null,"http://data.15926.org/nace/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nec",null,"http://data.15926.org/nec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nema",null,"http://data.15926.org/nema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nfpa",null,"http://data.15926.org/nfpa/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nor",null,"http://data.15926.org/nor/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","rdl",null,"http://data.15926.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sae",null,"http://data.15926.org/sae/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sie",null,"http://data.15926.org/sie/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","tema",null,"http://data.15926.org/tema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","twr",null,"http://data.15926.org/twr/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","uns",null,"http://data.15926.org/uns/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","wits",null,"http://data.15926.org/wits/",null,null,null,"Note: end address always with a slash (/)"]
[]
[]
["gBaseNamespace",null,"http://data.15926.org/aisi/","http://data.15926.org/aisi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ansi/","http://data.15926.org/ansi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/api/","http://data.15926.org/api/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/asme/","http://data.15926.org/asme/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/all/","http://data.15926.org/all/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/astm/","http://data.15926.org/astm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/atex/","http://data.15926.org/atex/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/bs/","http://data.15926.org/bs/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/din/","http://data.15926.org/din/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dm/","http://data.15926.org/dm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dnv/","http://data.15926.org/dnv/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/edm/","http://data.15926.org/edm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/en/","http://data.15926.org/en/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/eu/","http://data.15926.org/eu/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iec/","http://data.15926.org/iec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ieee/","http://data.15926.org/ieee/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iso/","http://data.15926.org/iso/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/lci/","http://data.15926.org/lci/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/mss/","http://data.15926.org/mss/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nace/","http://data.15926.org/nace/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nec/","http://data.15926.org/nec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nema/","http://data.15926.org/nema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nfpa/","http://data.15926.org/nfpa/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nor/","http://data.15926.org/nor/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sae/","http://data.15926.org/sae/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sie/","http://data.15926.org/sie/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/tema/","http://data.15926.org/tema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/twr/","http://data.15926.org/twr/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/uns/","http://data.15926.org/uns/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/wits/","http://data.15926.org/wits/",null,"RDL2"]
["                                          "]

{"sheet":"about","index":2,"n_rows":176,"n_cols":3,"rows_kept":176,"cut":false,"hidden":false,"merged":[]}
["Version 75 changes","2018-10-05","Onno Paap"]
["missing superclasses - and orphans- filter no deprecated classes"]
[]
["Version 74 changes","2018-09-30","Onno Paap"]
["Repaired bug missing label"]
[]
["Version 73 changes","2018-05-16","Onno Paap"]
["Repaired bug Deprecated Superclass"]
[]
[]
[]
["Version 71 changes","2016-07-17","Onno Paap"]
["Aded report button for comparison of RDL2 with a subfolder called views filled with spreadsheets."]
[]
[]
["Version 69 changes","2016-06-16","Onno Paap"]
["Added button: \"errors in definitions\" that lists all classes that have more or less \"<\" brackets than the number of super class relationships + 1. Where the part after the word \"that \"  is ignored in the count of \"<\" brackets."]
[]
["Version 68 changes","2016-06-13","Onno Paap"]
["Updated endpoint of RDL2 sparql "]
[]
["Version 67 changes","2016-05-22","Onno Paap"]
["Added button list subclasses from superclass "]
[]
["Version 65 changes","2016-04-25","Onno Paap"]
["Added checkbox at action dialog \"supress double child occurances\" so that this built-in feature can be switched off"]
[]
["Version 64 changes","2016-04-20","Onno Paap"]
["Made search case-insensitive and added endpoint \"all\""]
[]
["Version 63 changes","2016-09-28","Onno Paap"]
["Made entity list working on P4 endpoint (they changed the database version which was not accepting som sparql setting)"]
["Version 62 changes","2016-09-28","Onno Paap"]
["Applied show deprecated to searched result list"]
[]
["Version 61 changes","2016-08-29","Onno Paap"]
["Added query from pcardl for ClassOfIndirectProperty"]
[]
["Version 60 changes","2016-08-19","Onno Paap"]
["Repaired failing entity reports"]
[]
["Version 59 changes","2016-08-19","Onno Paap"]
["Missing superclasses now queries whole federation of RDL2"]
[]
["Version 58 changes","2016-08-16","Onno Paap"]
["Repaired missing output for entities and doubles in RDL2 endpoints other than rdl"]
[]
["Version 57 changes","2016-08-13","Onno Paap"]
["Doubles report now skips classes that are deprecated"]
[]
["Version 56 changes","2016-07-22","Onno Paap"]
["Made rowheight suitable for longer definitions to example DESIGN BASIS"]
[]
["Version 55 changes","2016-07-19","Onno Paap"]
["Made rowheight suitable for longer definitions"]
[]
["Version 54 changes","2016-07-03","Onno Paap"]
["Entity Type field changed to 6 merged cells."]
[]
["Version 53 changes","2016-06-23","Onno Paap"]
["added lci namespace"]
[]
["Version 52 changes","2016-06-23","Onno Paap"]
["Added deprecated count to list entities"]
[]
["Version 51 changes","2016-06-19","Onno Paap"]
["Updated namespaces of staging RDL"]
[]
["Version 50 changes","2016-06-19","Onno Paap"]
["taxonomy view repaired missing entity type"]
[]
["Version 49 changes","2016-06-14","Onno Paap"]
["Room for 12 superclasses"]
[]
["Version 48 changes","2016-06-14","Onno Paap"]
["Repaired NOR:/RDS  bug"]
[]
["Version 47 changes","2016-06-14","Onno Paap"]
["Repaired endpoint bug"]
[]
["Version 46 changes","2016-06-13","Onno Paap"]
["Updated endpoints"]
[]
["Version 45 changes","2016-06-06","Onno Paap"]
["Completed Missing Superclasses report"]
[]
["Version 44 changes","2016-05-20","Onno Paap"]
["Added Clear Cache button (use on any database changes)"]
[]
["Version 43 changes","2016-05-19","Onno Paap"]
["Changed non-existing super classes to show as \"no label\""]
[]
["Version 42 changes","2016-05-02","Onno Paap"]
["bug fix"]
[]
["Version 41 changes","2016-05-02","Onno Paap"]
["Added setting to show/not show deprecated items. If shown, they are stricken through"]
[]
["Version 40 changes","2016-03-31","Onno Paap"]
["Added  in doubles: two classes having the same label."]
[]
["Version 39 changes","2016-03-21","Onno Paap"]
["Made the query more robust, after the server hass been returning a 404 occasionally"]
[]
["Version 38 changes","2016-03-03","Onno Paap"]
["Repaired bug entity type query on PCA endpoint"]
[]
["Version 37 changes","2016-01-29","Onno Paap"]
["Showing deprecated class in taxonomy with label in strikethrough."]
[]
["Version 36 changes","2016-01-13","Onno Paap"]
["Added the 17 endpoints of http://data.15926.org/rdl"]
[]
["Version 35 changes","2016-01-13","Onno Paap"]
["In taxonomy view, disregard all rdf:type that is not data model.  So only show rdf:type that is dm:"]
[]
["Version 34 changes","2016-01-13","Onno Paap"]
["Solved taxonomy levels regression bug"]
[]
["Version 33 changes","2016-01-11","Onno Paap"]
["Enhanced the doubled query. First 4 columns are about the triple, the rest is info."]
[]
["Repaired bug in entity type query."]
[]
["Version 30 changes","2016-01-03","Onno Paap"]
["Repaired entity type query for old PCA RDL. \nRepaired bug in entity type query where a class that has a superclass of the wanted type as well as  of another type became  the start point of a new taxonomy as well as part in the main taxonomy. (read that again)"]
[]
["Version 29 changes","2016-01-02","Onno Paap"]
["Filtered entity filtered taxonomy to only show the filtered entity not subClassOf of another entity"]
[]
["Version 27 changes","2016-01-01","Onno Paap"]
["few bugs repaired.  Changed entity search into presenting taxonomies. "]
[]
["Version 26 changes","2015-12-26","Onno Paap"]
["few bugs repaired. "]
[]
["Version 25 changes","2015-12-26","Onno Paap"]
["Added Part 12 and localhost endpoints"]
["Added button for selecting double labels and definitions. "]
["Version 24 changes","2015-12-14","Onno Paap"]
["Added button to list all distinct entity data types and their counts, and click to show."]
["Added a button to show all orphans that have a rdfs:label"]
["Version 23 changes"]
["Added endpoint posccaesar.org/p4/sparql"]
["Version 22 changes"]
["Added endpoint staging.data.posccaesar.org/rdl"]
[]
["Version 21 changes"]
["Repaired bug where namespace replace was based upon definition instead of class label"]
[]
["Version 20 changes"]
["Repaired bug where definition did not show up if hyperlink replace was on."]
[]
["Version 19 changes (skip version 16-18)"]
["Settings expanded with persist settings, namespace replacer and hyperlink replacer"]
["Added namespace replacer which will replace the RDL: namespace of the ID with the namespace given in the list on the front page."]
["Added hyperlink replacer which will find terms between single quotes and look them up in the RDL, then add a hyperlink in the text if found. Anchor tag <a></a> used not &hyperlink() so looks ugly."]
[]
["Version 15 changes"]
["Changed browser page Action buttons to hyperlinks because buttons are not equally spaced between Excel versions (Office 2007 versus Office 365)"]
["First row is empty. Move all up."]
["Make stop button for during query taxonomy query execution"]
[]
[]
["Version 14 changes"]
["Aligned buttons on browser page"]
["Made color notification work. Note: switch it on first in settings. Default is off"]
["Top align subclasses in taxonomy"]
["Subclasses made to hyperlink in taxonomy"]
["Subclasses made to increase column width in taxonomy"]
["Made browser search go when hitting enter in search field"]
[]
[]
[]
["todo"]
["Make setting for outputting to other result pages"]

{"sheet":"Results1","index":3,"n_rows":57,"n_cols":34,"rows_kept":57,"cut":false,"hidden":false,"merged":[[56,23,56,24],[56,17,56,22],[56,25,56,30],[56,31,56,34],[54,23,54,24],[54,17,54,22],[54,25,54,30],[54,31,54,34],[55,23,55,24],[55,17,55,22],[55,25,55,30],[55,31,55,34],[52,23,52,24],[52,17,52,22],[52,25,52,30],[52,31,52,34],[53,23,53,24],[53,17,53,22],[53,25,53,30],[53,31,53,34],[50,24,50,25],[50,18,50,23],[50,26,50,31],[50,32,50,35],[51,25,51,26],[51,19,51,24],[51,27,51,32],[51,33,51,36],[48,24,48,25],[48,18,48,23],[48,26,48,31],[48,32,48,35],[49,25,49,26],[49,19,49,24],[49,27,49,32],[49,33,49,36],[46,24,46,25],[46,18,46,23],[46,26,46,31],[46,32,46,35],[47,23,47,24],[47,17,47,22],[47,25,47,30],[47,31,47,34],[44,23,44,24],[44,17,44,22],[44,25,44,30],[44,31,44,34],[45,23,45,24],[45,17,45,22],[45,25,45,30],[45,31,45,34],[42,23,42,24],[42,17,42,22],[42,25,42,30],[42,31,42,34],[43,22,43,23],[43,16,43,21],[43,24,43,29],[43,30,43,33],[40,23,40,24],[40,17,40,22],[40,25,40,30],[40,31,40,34],[41,23,41,24],[41,17,41,22],[41,25,41,30],[41,31,41,34],[38,22,38,23],[38,16,38,21],[38,24,38,29],[38,30,38,33],[39,23,39,24],[39,17,39,22],[39,25,39,30],[39,31,39,34],[36,23,36,24],[36,17,36,22],[36,25,36,30],[36,31,36,34],[37,23,37,24],[37,17,37,22],[37,25,37,30],[37,31,37,34],[34,23,34,24],[34,17,34,22],[34,25,34,30],[34,31,34,34],[35,23,35,24],[35,17,35,22],[35,25,35,30],[35,31,35,34],[33,23,33,24],[33,17,33,22],[33,25,33,30],[33,31,33,34],[32,25,32,26],[32,19,32,24],[32,27,32,32],[32,33,32,36],[30,25,30,26],[30,19,30,24],[30,27,30,32],[30,33,30,36],[31,25,31,26],[31,19,31,24],[31,27,31,32],[31,33,31,36],[28,25,28,26],[28,19,28,24],[28,27,28,32],[28,33,28,36],[29,25,29,26],[29,19,29,24],[29,27,29,32],[29,33,29,36],[26,23,26,24],[26,17,26,22],[26,25,26,30],[26,31,26,34],[27,24,27,25],[27,18,27,23],[27,26,27,31],[27,32,27,35],[24,23,24,24],[24,17,24,22],[24,25,24,30],[24,31,24,34],[25,23,25,24],[25,17,25,22],[25,25,25,30],[25,31,25,34],[22,23,22,24],[22,17,22,22],[22,25,22,30],[22,31,22,34],[23,23,23,24],[23,17,23,22],[23,25,23,30],[23,31,23,34],[20,23,20,24],[20,17,20,22],[20,25,20,30],[20,31,20,34],[21,23,21,24],[21,17,21,22],[21,25,21,30],[21,31,21,34],[18,23,18,24],[18,17,18,22],[18,25,18,30],[18,31,18,34],[19,23,19,24],[19,17,19,22],[19,25,19,30],[19,31,19,34],[16,24,16,25],[16,18,16,23],[16,26,16,31],[16,32,16,35],[17,23,17,24],[17,17,17,22],[17,25,17,30],[17,31,17,34],[14,24,14,25],[14,18,14,23],[14,26,14,31],[14,32,14,35],[15,24,15,25],[15,18,15,23],[15,26,15,31],[15,32,15,35],[12,24,12,25],[12,18,12,23],[12,26,12,31],[12,32,12,35],[13,24,13,25],[13,18,13,23],[13,26,13,31],[13,32,13,35],[10,24,10,25],[10,18,10,23],[10,26,10,31],[10,32,10,35],[11,23,11,24],[11,17,11,22],[11,25,11,30],[11,31,11,34],[8,24,8,25],[8,18,8,23],[8,26,8,31],[8,32,8,35],[9,24,9,25],[9,18,9,23],[9,26,9,31],[9,32,9,35],[6,23,6,24],[6,17,6,22],[6,25,6,30],[6,31,6,34],[7,24,7,25],[7,18,7,23],[7,26,7,31],[7,32,7,35],[4,24,4,25],[4,18,4,23],[4,26,4,31],[4,32,4,35],[5,24,5,25],[5,18,5,23],[5,26,5,31],[5,32,5,35],[2,22,2,23],[2,16,2,21],[2,24,2,29],[2,30,2,33],[3,23,3,24],[3,17,3,22],[3,25,3,30],[3,31,3,34],[0,20,0,21],[0,14,0,19],[0,22,0,27],[0,28,0,31],[1,21,1,22],[1,15,1,20],[1,23,1,28],[1,29,1,32]]}
[null,null,"FunctionalObject",null,null,null,null,null,null,null,null,null,null,null,"ENERGY STORAGE",null,null,null,null,null,"rdl:RDS2222105",null,"An <ENERGY STORAGE> is a <FunctionalObject> that is capable of <ENERGY STORING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ACCUMULATOR","ENERGY STORAGE",null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL ACCUMULATOR",null,null,null,null,null,"rdl:RDS281384",null,"An <ELECTRICAL ACCUMULATOR> is an <ACCUMULATOR> and an <ENERGY STORAGE> that converts chemical energy into electrical energy by reversible chemical reactions and that may be recharged by passing a current through it in the direction opposite to that of its discharge",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","ELECTRICAL ACCUMULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC BATTERY",null,null,null,null,null,"rdl:RDS478124",null,"An <ELECTRIC BATTERY> is an <ARTEFACT> and an <ELECTRICAL ACCUMULATOR> that comprises one or more electric battery cells",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR-METAL BATTERY",null,null,null,null,null,"rdl:RDS869939",null,"An <AIR-METAL BATTERY> is an <ELECTRIC BATTERY> in which atmospheric oxygen serves as the active material at the positive electrode and a metal as the negative electrode",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AIR-METAL BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALKALINE AIR-ZINC BATTERY",null,null,null,null,null,"rdl:RDS5856972",null,"An <ALKALINE AIR-ZINC BATTERY> is an <AIR-METAL BATTERY> with an alkaline electrolyte and a negative electrode of zinc.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AIR-METAL BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NEUTRAL-ELECTROLYTE AIR-ZINC BATTERY",null,null,null,null,null,"rdl:RDS5857017",null,"A <NEUTRAL-ELECTROLYTE AIR-ZINC BATTERY> is an <AIR-METAL BATTERY> with a saline electrolyte and a negative electrode of zinc.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALKALINE PRIMARY BATTERY",null,null,null,null,null,"rdl:RDS868139",null,"An <ALKALINE PRIMARY BATTERY> is an <ELECTRIC BATTERY> containing an alkaline electrolyte",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALKALINE PRIMARY BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALKALINE MANGANESE DIOXIDE-ZINC BATTERY",null,null,null,null,null,"rdl:RDS5857096",null,"An <ALKALINE MANGANESE DIOXIDE-ZINC BATTERY> is an <ALKALINE PRIMARY BATTERY> with an alkaline electrolyte, a positive electrode containing manganese dioxide and a negative electrode of zinc.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALKALINE PRIMARY BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COPPER OXIDE-ZINC BATTERY",null,null,null,null,null,"rdl:RDS5857141",null,"A <COPPER OXIDE-ZINC BATTERY> is an <ALKALINE PRIMARY BATTERY> with a positive electrode containing copper oxide as active material and a negative electrode of zinc.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALKALINE PRIMARY BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MERCURIC OXIDE-ZINC BATTERY",null,null,null,null,null,"rdl:RDS5857186",null,"A <MERCURIC OXIDE-ZINC BATTERY> is an <ALKALINE PRIMARY BATTERY> with a positive electrode containing mercuric oxide as active material and a negative electrode of zinc.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALKALINE PRIMARY BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ZINC SILVER OXIDE BATTERY",null,null,null,null,null,"rdl:RDS5857231",null,"A <ZINC SILVER OXIDE BATTERY> is an <ALKALINE PRIMARY BATTERY> with an alkaline electrolyte, a positive electrode containing silver oxide and a negative electrode of zinc.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALKALINE SECONDARY BATTERY",null,null,null,null,null,"rdl:RDS869894",null,"An <ALKALINE SECONDARY BATTERY> is an <ELECTRIC BATTERY> in which the electrolyte is an alkaline solution",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALKALINE SECONDARY BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NICKEL-CADMIUM BATTERY",null,null,null,null,null,"rdl:RDS5856662",null,"A <NICKEL-CADMIUM BATTERY> is an <ALKALINE SECONDARY BATTERY> with an alkaline electrolyte, a positive electrode containing nickel oxide and a negative electrode of cadmium.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALKALINE SECONDARY BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NICKEL-IRON BATTERY",null,null,null,null,null,"rdl:RDS5856707",null,"A <NICKEL-IRON BATTERY> is an <ALKALINE SECONDARY BATTERY> with an alkaline electrolyte, a positive electrode containing nickel oxide and a negative electrode of iron.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALKALINE SECONDARY BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NICKEL-ZINC BATTERY",null,null,null,null,null,"rdl:RDS5856752",null,"A <NICKEL-ZINC BATTERY> is an <ALKALINE SECONDARY BATTERY> with an alkaline electrolyte, a positive electrode containing nickel oxide and a negative electrode of zinc.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALKALINE SECONDARY BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SILVER OXIDE CADMIUM BATTERY",null,null,null,null,null,"rdl:RDS5856797",null,"A <SILVER OXIDE CADMIUM BATTERY> is an <ALKALINE SECONDARY BATTERY> with an alkaline electrolyte, a positive electrode containing silver oxide and a negative electrode of cadmium.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALKALINE SECONDARY BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SILVER-ZINC BATTERY",null,null,null,null,null,"rdl:RDS5856842",null,"A <SILVER-ZINC BATTERY> is an <ALKALINE SECONDARY BATTERY> with an alkaline electrolyte, a positive electrode containing silver and a negative electrode of zinc.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CARBON-ZINC BATTERY",null,null,null,null,null,"rdl:RDS869849",null,"A <CARBON-ZINC BATTERY> is an <ELECTRIC BATTERY> such as Leclanch or zinc chloride batteries",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CUPROUS CHLORIDE-MAGNESIUM BATTERY",null,null,null,null,null,"rdl:RDS478169",null,"A <CUPROUS CHLORIDE-MAGNESIUM BATTERY> is an <ELECTRIC BATTERY> with a positive electrode containing cuprous chloride as active material, a negative electrode of magnesium and a salt solution as electrolyte",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DRY PRIMARY BATTERY",null,null,null,null,null,"rdl:RDS5855980",null,"A <DRY PRIMARY BATTERY> is an <ELECTRIC BATTERY> containing an immobilized electrolyte",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEAD-ACID BATTERY",null,null,null,null,null,"rdl:RDS478214",null,"A <LEAD-ACID BATTERY> is an <ELECTRIC BATTERY> with an aqueous electrolyte based on dilute sulphuric acid, a positive electrode of lead dioxide and a negative electrode of lead",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LECLANCHE BATTERY",null,null,null,null,null,"rdl:RDS5856042",null,"A <LECLANCHE BATTERY> is an <ELECTRIC BATTERY> with a saline electrolyte based on ammonium chloride and zinc chloride, a positive electrode containing manganese dioxide and a negative electrode of zinc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAINTENANCE-FREE BATTERY",null,null,null,null,null,"rdl:RDS5855422",null,"An <MAINTENANCE-FREE BATTERY> is an <ELECTRIC BATTERY> that, during its service life, requires no maintenance provided specified operating conditions are fulfilled",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MANGANESE DIOXIDE-MAGNESIUM BATTERY",null,null,null,null,null,"rdl:RDS5856104",null,"A <MANGANESE DIOXIDE-MAGNESIUM BATTERY> is an <ELECTRIC BATTERY> with a positive electrode containing manganese dioxide as active material, a negative electrode of magnesium and a salt solution as electrolyte",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOLTEN SALT BATTERY",null,null,null,null,null,"rdl:RDS5856166",null,"A <MOLTEN SALT BATTERY> is an <ELECTRIC BATTERY> with an electrolyte consisting of one or more anhydrous molten salts",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MONOBLOC BATTERY",null,null,null,null,null,"rdl:RDS890819",null,"A <MONOBLOC BATTERY> is an <ELECTRIC BATTERY> in which multiple separate but electrically connected cell compartments each of which is designed to house an assembly of electrodes, electrolyte, terminals or interconnections and possible separators",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-AQUEOUS BATTERY",null,null,null,null,null,"rdl:RDS5856228",null,"A <NON-AQUEOUS BATTERY> is an <ELECTRIC BATTERY> having an electrolyte made from a non-aqueous liquid solvent",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"NON-AQUEOUS BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-AQUEOUS LITHIUM BATTERY",null,null,null,null,null,"rdl:RDS5856290",null,"A <NON-AQUEOUS LITHIUM BATTERY> is a <NON-AQUEOUS BATTERY> with a negative electrode of lithium or containing lithium.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"NON-AQUEOUS LITHIUM BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHROMIUM OXIDE-LITHIUM BATTERY",null,null,null,null,null,"rdl:RDS5856397",null,"A <CHROMIUM OXIDE-LITHIUM BATTERY> is a <NON-AQUEOUS LITHIUM BATTERY> with a positive electrode containing chromium oxide as active material, a negative electrode of lithium and a non-aqueous, organic solution as electrolyte.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"NON-AQUEOUS LITHIUM BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LITHIUM CARBON MONOFLUORIDE BATTERY",null,null,null,null,null,"rdl:RDS5856352",null,"A <LITHIUM CARBON MONOFLUORIDE BATTERY> is a <NON-AQUEOUS LITHIUM BATTERY> with a positive electrode containing carbon monofluoride and a negative electrode of lithium.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"NON-AQUEOUS LITHIUM BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LITHIUM COPPER OXIDE BATTERY",null,null,null,null,null,"rdl:RDS5856442",null,"A <LITHIUM COPPER OXIDE BATTERY> is a <NON-AQUEOUS LITHIUM BATTERY> with a positive electrode containing copper oxide and a negative electrode of lithium.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"NON-AQUEOUS LITHIUM BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LITHIUM MANGANESE DIOXIDE BATTERY",null,null,null,null,null,"rdl:RDS5856487",null,"A <LITHIUM MANGANESE DIOXIDE BATTERY> is a <NON-AQUEOUS LITHIUM BATTERY> with a positive electrode containing manganese dioxide and a negative electrode of lithium.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"NON-AQUEOUS LITHIUM BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LITHIUM THIONYL CHLORIDE BATTERY",null,null,null,null,null,"rdl:RDS5856532",null,"A <LITHIUM THIONYL CHLORIDE BATTERY> is a <NON-AQUEOUS LITHIUM BATTERY> with a non-aqueous inorganic electrolyte, a positive electrode containing thionyl chloride and a negative electrode of lithium.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEALED PRIMARY BATTERY",null,null,null,null,null,"rdl:RDS5855783",null,"A <SEALED PRIMARY BATTERY> is an <ELECTRIC BATTERY> that remains closed and does not release either gas or liquid when operated within the limits specified by the manufacturer",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SILVER CHLORIDE-MAGNESIUM BATTERY",null,null,null,null,null,"rdl:RDS5760553",null,"A <SILVER CHLORIDE-MAGNESIUM BATTERY> is an <ELECTRIC BATTERY> with a positive electrode containing silver chloride as active material, a negative electrode of magnesium and a salt solution as electrolyte",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID ELECTROLYTE BATTERY",null,null,null,null,null,"rdl:RDS5855845",null,"A <SOLID ELECTROLYTE BATTERY> is an <ELECTRIC BATTERY> with an ionically conducting solid as electrolyte",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WET PRIMARY BATTERY",null,null,null,null,null,"rdl:RDS5760615",null,"A <WET PRIMARY BATTERY> is an <ELECTRIC BATTERY> in which the electrolyte is in liquid and mobile form",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ZINC CHLORIDE BATTERY",null,null,null,null,null,"rdl:RDS5760491",null,"A <ZINC CHLORIDE BATTERY> is an <ELECTRIC BATTERY> with a saline electrolyte based on zinc chloride, a positive electrode containing manganese dioxide and a negative electrode of zinc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ACCUMULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC BATTERY BANK",null,null,null,null,null,"rdl:RDS17859310",null,"An <ELECTRIC BATTERY BANK> is an <ARTEFACT> and an <ELECTRICAL ACCUMULATOR> that consisting of a number of electric batteries connected together to store and supply electrical energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY BANK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PARALLEL CONNECTED BATTERY BANK",null,null,null,null,null,"rdl:RDS5858140",null,"A <PARALLEL CONNECTED BATTERY BANK> is an <ELECTRIC BATTERY BANK> in which all the positive battery terminals are connected together and all the negative battery terminals are connected together",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY BANK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PARALLEL-SERIES CONNECTED BATTERY BANK",null,null,null,null,null,"rdl:RDS5858095",null,"A <PARALLEL-SERIES CONNECTED BATTERY BANK> is an <ELECTRIC BATTERY BANK> in which parallel connected groups of batteries are connected in series",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY BANK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SERIES CONNECTED BATTERY BANK",null,null,null,null,null,"rdl:RDS5858230",null,"A <SERIES CONNECTED BATTERY BANK> is an <ELECTRIC BATTERY BANK> in which the positive terminal of each battery is connected to the negative terminal of the next battery in sequence",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY BANK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SERIES-PARALLEL CONNECTED BATTERY BANK",null,null,null,null,null,"rdl:RDS5858185",null,"A <SERIES-PARALLEL CONNECTED BATTERY BANK> is an <ELECTRIC BATTERY BANK> in which series connected groups of batteries are connected in parallel",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL ACCUMULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC BATTERY CELL",null,null,null,null,null,"rdl:RDS483614",null,"An <ELECTRIC BATTERY CELL> is an <ARTEFACT> and an <ELECTRICAL ACCUMULATOR> and that is a single electrochemical system, consisting of positive and negative electrodes and an electrolyte to transport ions between them",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLAT BATTERY CELL",null,null,null,null,null,"rdl:RDS5857360",null,"A <FLAT BATTERY CELL> is an <ELECTRIC BATTERY CELL> with flat, stratified electrode geometry",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GASTIGHT SEALED BATTERY CELL",null,null,null,null,null,"rdl:RDS5857405",null,"A <GASTIGHT SEALED BATTERY CELL> is an <ELECTRIC BATTERY CELL> that remains closed and does not release either gas or liquid when operated within the limits of charge and temperature specified by the manufacturer",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GASTIGHT SEALED BATTERY CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HERMETICALLY SEALED BATTERY CELL",null,null,null,null,null,"rdl:RDS5857732",null,"A <HERMETICALLY SEALED BATTERY CELL> is a <GASTIGHT SEALED BATTERY CELL> without pressure release device.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRIMARY CELL",null,null,null,null,null,"rdl:RDS870209",null,"A <PRIMARY CELL> is an <ELECTRIC BATTERY CELL> that is not designed to be recharged",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PRIMARY CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FUEL CELL",null,null,null,null,null,"rdl:RDS5857794",null,"A <FUEL CELL> is a <PRIMARY CELL> that consumes fuel continuously and converts its chemical energy directly into electrical energy.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FUEL CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OXYGEN-HYDROGEN FUEL CELL",null,null,null,null,null,"rdl:RDS5857856",null,"An <OXYGEN-HYDROGEN FUEL CELL> is a <FUEL CELL> in which the active materials are oxygen and hydrogen.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PRIMARY CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STANDARD BATTERY CELL",null,null,null,null,null,"rdl:RDS5857954",null,"A <STANDARD BATTERY CELL> is a <PRIMARY CELL> having, at a specified temperature, an invariant and specific open-circuit voltage, used as a reference voltage.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STANDARD BATTERY CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WESTON STANDARD CELL",null,null,null,null,null,"rdl:RDS5858033",null,"A <WESTON STANDARD CELL> is a <STANDARD BATTERY CELL> with a saline electrolyte saturated with cadmium sulphate, a positive electrode of mercury and solid mercurous sulphate, and a negative electrode of amalgamated cadmium and solid cadmium sulphate.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROUND BATTERY CELL",null,null,null,null,null,"rdl:RDS5857450",null,"A <ROUND BATTERY CELL> is an <ELECTRIC BATTERY CELL> with a cylindrical shape, in which the overall height is equal to or greater than the diameter",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SECONDARY CELL",null,null,null,null,null,"rdl:RDS870164",null,"A <SECONDARY CELL> is an <ELECTRIC BATTERY CELL> that is designed to be electrically recharged",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UNSPILLABLE BATTERY CELL",null,null,null,null,null,"rdl:RDS5857495",null,"A <UNSPILLABLE BATTERY CELL> is an <ELECTRIC BATTERY CELL> from which electrolyte cannot escape regardless of its orientation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE REGULATED LEAD ACID BATTERY CELL",null,null,null,null,null,"rdl:RDS5857540",null,"A <VALVE REGULATED LEAD ACID BATTERY CELL> is an <ELECTRIC BATTERY CELL> that is closed but have a valve which allows the escape of gas if the internal pressure exceeds a predetermined value",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC BATTERY CELL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VENTED BATTERY CELL",null,null,null,null,null,"rdl:RDS5857585",null,"A <VENTED BATTERY CELL> is an <ELECTRIC BATTERY CELL> having a cover provided with an opening through which products of electrolysis and evaporation are allowed to escape freely from the cell to the atmosphere",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]