{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["RDL browser","Settings","about","Results1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"RDL browser","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[[0,0,0,4]]}
["RDL2 browser to spreadsheet tool version 75",null,null,null,null,null,"Endpoint: http://data.15926.org/rdl/"]
["Contact: onno.paap@gmail.com",null,null,null,null,"Action","INSTRUMENTATION FUNCTION","http://data.15926.org/rdl/RDS2225050"]
[]
["Search:","INSTRUMENTATION FUNCTION"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Note: first set coloring on in Settings"]
[null,"Coloring (containing this string will give this color)"]
[null,"ClassOfFunctionalObject"]
[null,"ClassOfInanimatePhysicalObject "]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Namespace replacer (definition containing this string replaces the namespace)"]
[null,"API","API:"]
[null,"ASME","ASME:"]
[null,"ASTM","ASTM:"]
[null,"DIN","DIN:"]
[null,"EN","EN:"]
[null,"ISO","ISO:"]
[null,"NORSOK","NOR:"]
[null,"NPD","NOR:"]
[null,"NS","NOR:"]
[null,"ROSEMOUNT","ROS:"]
[null,"SAE","SAE:"]
[null,"SIEMENS","SIE:"]
[null,"SKOTSELV","SKOT:"]
[null,"TWR","TWR:"]

{"sheet":"Settings","index":1,"n_rows":87,"n_cols":8,"rows_kept":87,"cut":false,"hidden":true,"merged":[]}
["Setting name","Select name","OnKey","Value","Status","RDLType"]
["Endpoint","RDL2 (15926.org)",null,"http://data.15926.org/rdl/","Current",null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA RDL",null,"http://data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA Staging",null,"http://staging.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA SVRDL",null,"http://svrdl.community.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P4",null,"http://posccaesar.org/p4/sparql",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P12",null,"http://sti.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","Localhost",null,"http://localhost:8890/sparql/",null,null,null,"Note: end address always with a slash (/)"]
[]
["gBaseNamespace",null,"http://data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://staging.data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://svrdl.community.data.posccaesar.org/rdl/","http://svrdl.community.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://posccaesar.org/p4/sparql","http://posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://sti.data.posccaesar.org/rdl/","http://sti.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://localhost:8890/sparql/","http://data.15926.org/rdl/",null,"RDL2"]
["gKeepSettings",null,null,"T"]
["gShowDeprecated",null,null,"F"]
["gColoring",null,null,"T"]
["gNamespaceReplacing",null,null,"F"]
["gHyperlinkReplacing",null,null,"F"]
[]
["Endpoint","aisi",null,"http://data.15926.org/aisi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ansi",null,"http://data.15926.org/ansi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","api",null,"http://data.15926.org/api/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","all",null,"http://data.15926.org/all/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","asme",null,"http://data.15926.org/asme/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","astm",null,"http://data.15926.org/astm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","atex",null,"http://data.15926.org/atex/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","bs",null,"http://data.15926.org/bs/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","din",null,"http://data.15926.org/din/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dm",null,"http://data.15926.org/dm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dnv",null,"http://data.15926.org/dnv/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","edm",null,"http://data.15926.org/edm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","en",null,"http://data.15926.org/en/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","eu",null,"http://data.15926.org/eu/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iec",null,"http://data.15926.org/iec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ieee",null,"http://data.15926.org/ieee/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iso",null,"http://data.15926.org/iso/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","lci",null,"http://data.15926.org/lci/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","mss",null,"http://data.15926.org/mss/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nace",null,"http://data.15926.org/nace/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nec",null,"http://data.15926.org/nec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nema",null,"http://data.15926.org/nema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nfpa",null,"http://data.15926.org/nfpa/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nor",null,"http://data.15926.org/nor/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","rdl",null,"http://data.15926.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sae",null,"http://data.15926.org/sae/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sie",null,"http://data.15926.org/sie/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","tema",null,"http://data.15926.org/tema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","twr",null,"http://data.15926.org/twr/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","uns",null,"http://data.15926.org/uns/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","wits",null,"http://data.15926.org/wits/",null,null,null,"Note: end address always with a slash (/)"]
[]
[]
["gBaseNamespace",null,"http://data.15926.org/aisi/","http://data.15926.org/aisi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ansi/","http://data.15926.org/ansi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/api/","http://data.15926.org/api/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/asme/","http://data.15926.org/asme/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/all/","http://data.15926.org/all/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/astm/","http://data.15926.org/astm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/atex/","http://data.15926.org/atex/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/bs/","http://data.15926.org/bs/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/din/","http://data.15926.org/din/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dm/","http://data.15926.org/dm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dnv/","http://data.15926.org/dnv/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/edm/","http://data.15926.org/edm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/en/","http://data.15926.org/en/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/eu/","http://data.15926.org/eu/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iec/","http://data.15926.org/iec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ieee/","http://data.15926.org/ieee/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iso/","http://data.15926.org/iso/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/lci/","http://data.15926.org/lci/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/mss/","http://data.15926.org/mss/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nace/","http://data.15926.org/nace/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nec/","http://data.15926.org/nec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nema/","http://data.15926.org/nema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nfpa/","http://data.15926.org/nfpa/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nor/","http://data.15926.org/nor/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sae/","http://data.15926.org/sae/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sie/","http://data.15926.org/sie/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/tema/","http://data.15926.org/tema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/twr/","http://data.15926.org/twr/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/uns/","http://data.15926.org/uns/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/wits/","http://data.15926.org/wits/",null,"RDL2"]
["                                          "]

{"sheet":"about","index":2,"n_rows":176,"n_cols":3,"rows_kept":176,"cut":false,"hidden":false,"merged":[]}
["Version 75 changes","2018-10-05","Onno Paap"]
["missing superclasses - and orphans- filter no deprecated classes"]
[]
["Version 74 changes","2018-09-30","Onno Paap"]
["Repaired bug missing label"]
[]
["Version 73 changes","2018-05-16","Onno Paap"]
["Repaired bug Deprecated Superclass"]
[]
[]
[]
["Version 71 changes","2016-07-17","Onno Paap"]
["Aded report button for comparison of RDL2 with a subfolder called views filled with spreadsheets."]
[]
[]
["Version 69 changes","2016-06-16","Onno Paap"]
["Added button: \"errors in definitions\" that lists all classes that have more or less \"<\" brackets than the number of super class relationships + 1. Where the part after the word \"that \"  is ignored in the count of \"<\" brackets."]
[]
["Version 68 changes","2016-06-13","Onno Paap"]
["Updated endpoint of RDL2 sparql "]
[]
["Version 67 changes","2016-05-22","Onno Paap"]
["Added button list subclasses from superclass "]
[]
["Version 65 changes","2016-04-25","Onno Paap"]
["Added checkbox at action dialog \"supress double child occurances\" so that this built-in feature can be switched off"]
[]
["Version 64 changes","2016-04-20","Onno Paap"]
["Made search case-insensitive and added endpoint \"all\""]
[]
["Version 63 changes","2016-09-28","Onno Paap"]
["Made entity list working on P4 endpoint (they changed the database version which was not accepting som sparql setting)"]
["Version 62 changes","2016-09-28","Onno Paap"]
["Applied show deprecated to searched result list"]
[]
["Version 61 changes","2016-08-29","Onno Paap"]
["Added query from pcardl for ClassOfIndirectProperty"]
[]
["Version 60 changes","2016-08-19","Onno Paap"]
["Repaired failing entity reports"]
[]
["Version 59 changes","2016-08-19","Onno Paap"]
["Missing superclasses now queries whole federation of RDL2"]
[]
["Version 58 changes","2016-08-16","Onno Paap"]
["Repaired missing output for entities and doubles in RDL2 endpoints other than rdl"]
[]
["Version 57 changes","2016-08-13","Onno Paap"]
["Doubles report now skips classes that are deprecated"]
[]
["Version 56 changes","2016-07-22","Onno Paap"]
["Made rowheight suitable for longer definitions to example DESIGN BASIS"]
[]
["Version 55 changes","2016-07-19","Onno Paap"]
["Made rowheight suitable for longer definitions"]
[]
["Version 54 changes","2016-07-03","Onno Paap"]
["Entity Type field changed to 6 merged cells."]
[]
["Version 53 changes","2016-06-23","Onno Paap"]
["added lci namespace"]
[]
["Version 52 changes","2016-06-23","Onno Paap"]
["Added deprecated count to list entities"]
[]
["Version 51 changes","2016-06-19","Onno Paap"]
["Updated namespaces of staging RDL"]
[]
["Version 50 changes","2016-06-19","Onno Paap"]
["taxonomy view repaired missing entity type"]
[]
["Version 49 changes","2016-06-14","Onno Paap"]
["Room for 12 superclasses"]
[]
["Version 48 changes","2016-06-14","Onno Paap"]
["Repaired NOR:/RDS  bug"]
[]
["Version 47 changes","2016-06-14","Onno Paap"]
["Repaired endpoint bug"]
[]
["Version 46 changes","2016-06-13","Onno Paap"]
["Updated endpoints"]
[]
["Version 45 changes","2016-06-06","Onno Paap"]
["Completed Missing Superclasses report"]
[]
["Version 44 changes","2016-05-20","Onno Paap"]
["Added Clear Cache button (use on any database changes)"]
[]
["Version 43 changes","2016-05-19","Onno Paap"]
["Changed non-existing super classes to show as \"no label\""]
[]
["Version 42 changes","2016-05-02","Onno Paap"]
["bug fix"]
[]
["Version 41 changes","2016-05-02","Onno Paap"]
["Added setting to show/not show deprecated items. If shown, they are stricken through"]
[]
["Version 40 changes","2016-03-31","Onno Paap"]
["Added  in doubles: two classes having the same label."]
[]
["Version 39 changes","2016-03-21","Onno Paap"]
["Made the query more robust, after the server hass been returning a 404 occasionally"]
[]
["Version 38 changes","2016-03-03","Onno Paap"]
["Repaired bug entity type query on PCA endpoint"]
[]
["Version 37 changes","2016-01-29","Onno Paap"]
["Showing deprecated class in taxonomy with label in strikethrough."]
[]
["Version 36 changes","2016-01-13","Onno Paap"]
["Added the 17 endpoints of http://data.15926.org/rdl"]
[]
["Version 35 changes","2016-01-13","Onno Paap"]
["In taxonomy view, disregard all rdf:type that is not data model.  So only show rdf:type that is dm:"]
[]
["Version 34 changes","2016-01-13","Onno Paap"]
["Solved taxonomy levels regression bug"]
[]
["Version 33 changes","2016-01-11","Onno Paap"]
["Enhanced the doubled query. First 4 columns are about the triple, the rest is info."]
[]
["Repaired bug in entity type query."]
[]
["Version 30 changes","2016-01-03","Onno Paap"]
["Repaired entity type query for old PCA RDL. \nRepaired bug in entity type query where a class that has a superclass of the wanted type as well as  of another type became  the start point of a new taxonomy as well as part in the main taxonomy. (read that again)"]
[]
["Version 29 changes","2016-01-02","Onno Paap"]
["Filtered entity filtered taxonomy to only show the filtered entity not subClassOf of another entity"]
[]
["Version 27 changes","2016-01-01","Onno Paap"]
["few bugs repaired.  Changed entity search into presenting taxonomies. "]
[]
["Version 26 changes","2015-12-26","Onno Paap"]
["few bugs repaired. "]
[]
["Version 25 changes","2015-12-26","Onno Paap"]
["Added Part 12 and localhost endpoints"]
["Added button for selecting double labels and definitions. "]
["Version 24 changes","2015-12-14","Onno Paap"]
["Added button to list all distinct entity data types and their counts, and click to show."]
["Added a button to show all orphans that have a rdfs:label"]
["Version 23 changes"]
["Added endpoint posccaesar.org/p4/sparql"]
["Version 22 changes"]
["Added endpoint staging.data.posccaesar.org/rdl"]
[]
["Version 21 changes"]
["Repaired bug where namespace replace was based upon definition instead of class label"]
[]
["Version 20 changes"]
["Repaired bug where definition did not show up if hyperlink replace was on."]
[]
["Version 19 changes (skip version 16-18)"]
["Settings expanded with persist settings, namespace replacer and hyperlink replacer"]
["Added namespace replacer which will replace the RDL: namespace of the ID with the namespace given in the list on the front page."]
["Added hyperlink replacer which will find terms between single quotes and look them up in the RDL, then add a hyperlink in the text if found. Anchor tag <a></a> used not &hyperlink() so looks ugly."]
[]
["Version 15 changes"]
["Changed browser page Action buttons to hyperlinks because buttons are not equally spaced between Excel versions (Office 2007 versus Office 365)"]
["First row is empty. Move all up."]
["Make stop button for during query taxonomy query execution"]
[]
[]
["Version 14 changes"]
["Aligned buttons on browser page"]
["Made color notification work. Note: switch it on first in settings. Default is off"]
["Top align subclasses in taxonomy"]
["Subclasses made to hyperlink in taxonomy"]
["Subclasses made to increase column width in taxonomy"]
["Made browser search go when hitting enter in search field"]
[]
[]
[]
["todo"]
["Make setting for outputting to other result pages"]

{"sheet":"Results1","index":3,"n_rows":825,"n_cols":35,"rows_kept":825,"cut":false,"hidden":false,"merged":[[824,21,824,22],[824,15,824,20],[824,23,824,28],[824,29,824,32],[822,21,822,22],[822,15,822,20],[822,23,822,28],[822,29,822,32],[823,21,823,22],[823,15,823,20],[823,23,823,28],[823,29,823,32],[820,22,820,23],[820,16,820,21],[820,24,820,29],[820,30,820,33],[821,22,821,23],[821,16,821,21],[821,24,821,29],[821,30,821,33],[818,22,818,23],[818,16,818,21],[818,24,818,29],[818,30,818,33],[819,22,819,23],[819,16,819,21],[819,24,819,29],[819,30,819,33],[816,22,816,23],[816,16,816,21],[816,24,816,29],[816,30,816,33],[817,21,817,22],[817,15,817,20],[817,23,817,28],[817,29,817,32],[814,22,814,23],[814,16,814,21],[814,24,814,29],[814,30,814,33],[815,22,815,23],[815,16,815,21],[815,24,815,29],[815,30,815,33],[812,22,812,23],[812,16,812,21],[812,24,812,29],[812,30,812,33],[813,22,813,23],[813,16,813,21],[813,24,813,29],[813,30,813,33],[810,22,810,23],[810,16,810,21],[810,24,810,29],[810,30,810,33],[811,22,811,23],[811,16,811,21],[811,24,811,29],[808,21,808,22],[808,15,808,20],[808,23,808,28],[808,29,808,32],[809,22,809,23],[809,16,809,21],[809,24,809,29],[809,30,809,33],[806,22,806,23],[806,16,806,21],[806,24,806,29],[806,30,806,33],[807,22,807,23],[807,16,807,21],[807,24,807,29],[807,30,807,33],[804,22,804,23],[804,16,804,21],[804,24,804,29],[804,30,804,33],[805,21,805,22],[805,15,805,20],[805,23,805,28],[805,29,805,32],[802,21,802,22],[802,15,802,20],[802,23,802,28],[802,29,802,32],[803,21,803,22],[803,15,803,20],[803,23,803,28],[803,29,803,32],[800,23,800,24],[800,17,800,22],[800,25,800,30],[800,31,800,34],[801,23,801,24],[801,17,801,22],[801,25,801,30],[801,31,801,34],[798,22,798,23],[798,16,798,21],[798,24,798,29],[798,30,798,33],[799,23,799,24],[799,17,799,22],[799,25,799,30],[799,31,799,34],[796,22,796,23],[796,16,796,21],[796,24,796,29],[796,30,796,33],[797,22,797,23],[797,16,797,21],[797,24,797,29],[797,30,797,33],[794,21,794,22],[794,15,794,20],[794,23,794,28],[794,29,794,32],[795,22,795,23],[795,16,795,21],[795,24,795,29],[795,30,795,33],[792,23,792,24],[792,17,792,22],[792,25,792,30],[792,31,792,34],[793,22,793,23],[793,16,793,21],[793,24,793,29],[793,30,793,33],[790,22,790,23],[790,16,790,21],[790,24,790,29],[790,30,790,33],[791,22,791,23],[791,16,791,21],[791,24,791,29],[791,30,791,33],[788,22,788,23],[788,16,788,21],[788,24,788,29],[788,30,788,33],[789,22,789,23],[789,16,789,21],[789,24,789,29],[789,30,789,33],[786,23,786,24],[786,17,786,22],[786,25,786,30],[786,31,786,34],[787,24,787,25],[787,18,787,23],[787,26,787,31],[787,32,787,35],[784,22,784,23],[784,16,784,21],[784,24,784,29],[784,30,784,33],[785,22,785,23],[785,16,785,21],[785,24,785,29],[785,30,785,33],[782,23,782,24],[782,17,782,22],[782,25,782,30],[782,31,782,34],[783,22,783,23],[783,16,783,21],[783,24,783,29],[783,30,783,33],[780,22,780,23],[780,16,780,21],[780,24,780,29],[780,30,780,33],[781,22,781,23],[781,16,781,21],[781,24,781,29],[781,30,781,33],[778,23,778,24],[778,17,778,22],[778,25,778,30],[778,31,778,34],[779,22,779,23],[779,16,779,21],[779,24,779,29],[779,30,779,33],[776,23,776,24],[776,17,776,22],[776,25,776,30],[776,31,776,34],[777,22,777,23],[777,16,777,21],[777,24,777,29],[777,30,777,33],[774,21,774,22],[774,15,774,20],[774,23,774,28],[774,29,774,32],[775,22,775,23],[775,16,775,21],[775,24,775,29],[775,30,775,33],[772,23,772,24],[772,17,772,22],[772,25,772,30],[772,31,772,34],[773,23,773,24],[773,17,773,22],[773,25,773,30],[773,31,773,34],[770,23,770,24],[770,17,770,22],[770,25,770,30],[770,31,770,34],[771,23,771,24],[771,17,771,22],[771,25,771,30],[771,31,771,34],[768,23,768,24],[768,17,768,22],[768,25,768,30],[768,31,768,34],[769,23,769,24],[769,17,769,22],[769,25,769,30],[769,31,769,34],[766,24,766,25],[766,18,766,23],[766,26,766,31],[766,32,766,35],[767,23,767,24],[767,17,767,22],[767,25,767,30],[767,31,767,34],[764,24,764,25],[764,18,764,23],[764,26,764,31],[764,32,764,35],[765,24,765,25],[765,18,765,23],[765,26,765,31],[765,32,765,35],[762,23,762,24],[762,17,762,22],[762,25,762,30],[762,31,762,34],[763,23,763,24],[763,17,763,22],[763,25,763,30],[763,31,763,34],[760,23,760,24],[760,17,760,22],[760,25,760,30],[760,31,760,34],[761,23,761,24],[761,17,761,22],[761,25,761,30],[761,31,761,34],[758,24,758,25],[758,18,758,23],[758,26,758,31],[758,32,758,35],[759,24,759,25],[759,18,759,23],[759,26,759,31],[759,32,759,35],[756,24,756,25],[756,18,756,23],[756,26,756,31],[756,32,756,35],[757,24,757,25],[757,18,757,23],[757,26,757,31],[757,32,757,35],[754,24,754,25],[754,18,754,23],[754,26,754,31],[754,32,754,35],[755,24,755,25],[755,18,755,23],[755,26,755,31],[755,32,755,35],[752,23,752,24],[752,17,752,22],[752,25,752,30],[752,31,752,34],[753,23,753,24],[753,17,753,22],[753,25,753,30],[753,31,753,34],[750,24,750,25],[750,18,750,23],[750,26,750,31],[750,32,750,35],[751,24,751,25],[751,18,751,23],[751,26,751,31],[751,32,751,35],[748,24,748,25],[748,18,748,23],[748,26,748,31],[748,32,748,35],[749,24,749,25],[749,18,749,23],[749,26,749,31],[749,32,749,35],[746,23,746,24],[746,17,746,22],[746,25,746,30],[746,31,746,34],[747,24,747,25],[747,18,747,23],[747,26,747,31],[747,32,747,35],[744,22,744,23],[744,16,744,21],[744,24,744,29],[744,30,744,33],[745,23,745,24],[745,17,745,22],[745,25,745,30],[745,31,745,34],[742,23,742,24],[742,17,742,22],[742,25,742,30],[742,31,742,34],[743,23,743,24],[743,17,743,22],[743,25,743,30],[743,31,743,34],[740,23,740,24],[740,17,740,22],[740,25,740,30],[740,31,740,34],[741,23,741,24],[741,17,741,22],[741,25,741,30],[741,31,741,34],[738,23,738,24],[738,17,738,22],[738,25,738,30],[738,31,738,34],[739,23,739,24],[739,17,739,22],[739,25,739,30],[739,31,739,34],[736,23,736,24],[736,17,736,22],[736,25,736,30],[736,31,736,34],[737,23,737,24],[737,17,737,22],[737,25,737,30],[737,31,737,34],[734,22,734,23],[734,16,734,21],[734,24,734,29],[734,30,734,33],[735,23,735,24],[735,17,735,22],[735,25,735,30],[735,31,735,34],[732,23,732,24],[732,17,732,22],[732,25,732,30],[732,31,732,34],[733,23,733,24],[733,17,733,22],[733,25,733,30],[733,31,733,34],[730,23,730,24],[730,17,730,22],[730,25,730,30],[730,31,730,34],[731,23,731,24],[731,17,731,22],[731,25,731,30],[731,31,731,34],[728,23,728,24],[728,17,728,22],[728,25,728,30],[728,31,728,34],[729,23,729,24],[729,17,729,22],[729,25,729,30],[729,31,729,34],[726,23,726,24],[726,17,726,22],[726,25,726,30],[726,31,726,34],[727,23,727,24],[727,17,727,22],[727,25,727,30],[727,31,727,34],[724,23,724,24],[724,17,724,22],[724,25,724,30],[724,31,724,34],[725,23,725,24],[725,17,725,22],[725,25,725,30],[725,31,725,34],[722,23,722,24],[722,17,722,22],[722,25,722,30],[722,31,722,34],[723,23,723,24],[723,17,723,22],[723,25,723,30],[723,31,723,34],[720,23,720,24],[720,17,720,22],[720,25,720,30],[720,31,720,34],[721,23,721,24],[721,17,721,22],[721,25,721,30],[721,31,721,34],[718,23,718,24],[718,17,718,22],[718,25,718,30],[718,31,718,34],[719,23,719,24],[719,17,719,22],[719,25,719,30],[719,31,719,34],[716,23,716,24],[716,17,716,22],[716,25,716,30],[716,31,716,34],[717,23,717,24],[717,17,717,22],[717,25,717,30],[717,31,717,34],[714,23,714,24],[714,17,714,22],[714,25,714,30],[714,31,714,34],[715,23,715,24],[715,17,715,22],[715,25,715,30],[715,31,715,34],[712,23,712,24],[712,17,712,22],[712,25,712,30],[712,31,712,34],[713,23,713,24],[713,17,713,22],[713,25,713,30],[713,31,713,34],[710,23,710,24],[710,17,710,22],[710,25,710,30],[710,31,710,34],[711,22,711,23],[711,16,711,21],[711,24,711,29],[711,30,711,33],[708,23,708,24],[708,17,708,22],[708,25,708,30],[708,31,708,34],[709,23,709,24],[709,17,709,22],[709,25,709,30],[709,31,709,34],[706,23,706,24],[706,17,706,22],[706,25,706,30],[706,31,706,34],[707,23,707,24],[707,17,707,22],[707,25,707,30],[707,31,707,34],[704,24,704,25],[704,18,704,23],[704,26,704,31],[704,32,704,35],[705,24,705,25],[705,18,705,23],[705,26,705,31],[705,32,705,35],[702,24,702,25],[702,18,702,23],[702,26,702,31],[702,32,702,35],[703,24,703,25],[703,18,703,23],[703,26,703,31],[703,32,703,35],[700,24,700,25],[700,18,700,23],[700,26,700,31],[700,32,700,35],[701,24,701,25],[701,18,701,23],[701,26,701,31],[701,32,701,35],[698,24,698,25],[698,18,698,23],[698,26,698,31],[698,32,698,35],[699,24,699,25],[699,18,699,23],[699,26,699,31],[699,32,699,35],[696,24,696,25],[696,18,696,23],[696,26,696,31],[696,32,696,35],[697,24,697,25],[697,18,697,23],[697,26,697,31],[697,32,697,35],[694,24,694,25],[694,18,694,23],[694,26,694,31],[694,32,694,35],[695,24,695,25],[695,18,695,23],[695,26,695,31],[695,32,695,35],[692,24,692,25],[692,18,692,23],[692,26,692,31],[692,32,692,35],[693,24,693,25],[693,18,693,23],[693,26,693,31],[693,32,693,35],[690,23,690,24],[690,17,690,22],[690,25,690,30],[690,31,690,34],[691,24,691,25],[691,18,691,23],[691,26,691,31],[691,32,691,35],[688,23,688,24],[688,17,688,22],[688,25,688,30],[688,31,688,34],[689,23,689,24],[689,17,689,22],[689,25,689,30],[689,31,689,34],[686,23,686,24],[686,17,686,22],[686,25,686,30],[686,31,686,34],[687,22,687,23],[687,16,687,21],[687,24,687,29],[687,30,687,33],[684,23,684,24],[684,17,684,22],[684,25,684,30],[684,31,684,34],[685,23,685,24],[685,17,685,22],[685,25,685,30],[685,31,685,34],[682,23,682,24],[682,17,682,22],[682,25,682,30],[682,31,682,34],[683,23,683,24],[683,17,683,22],[683,25,683,30],[683,31,683,34],[680,23,680,24],[680,17,680,22],[680,25,680,30],[680,31,680,34],[681,23,681,24],[681,17,681,22],[681,25,681,30],[681,31,681,34],[678,23,678,24],[678,17,678,22],[678,25,678,30],[678,31,678,34],[679,23,679,24],[679,17,679,22],[679,25,679,30],[679,31,679,34],[676,23,676,24],[676,17,676,22],[676,25,676,30],[676,31,676,34],[677,23,677,24],[677,17,677,22],[677,25,677,30],[677,31,677,34],[674,23,674,24],[674,17,674,22],[674,25,674,30],[674,31,674,34],[675,23,675,24],[675,17,675,22],[675,25,675,30],[675,31,675,34],[672,23,672,24],[672,17,672,22],[672,25,672,30],[672,31,672,34],[673,23,673,24],[673,17,673,22],[673,25,673,30],[673,31,673,34],[670,23,670,24],[670,17,670,22],[670,25,670,30],[670,31,670,34],[671,23,671,24],[671,17,671,22],[671,25,671,30],[671,31,671,34],[668,23,668,24],[668,17,668,22],[668,25,668,30],[668,31,668,34],[669,23,669,24],[669,17,669,22],[669,25,669,30],[669,31,669,34],[666,23,666,24],[666,17,666,22],[666,25,666,30],[666,31,666,34],[667,23,667,24],[667,17,667,22],[667,25,667,30],[667,31,667,34],[664,23,664,24],[664,17,664,22],[664,25,664,30],[664,31,664,34],[665,23,665,24],[665,17,665,22],[665,25,665,30],[665,31,665,34],[662,23,662,24],[662,17,662,22],[662,25,662,30],[662,31,662,34],[663,23,663,24],[663,17,663,22],[663,25,663,30],[663,31,663,34],[660,24,660,25],[660,18,660,23],[660,26,660,31],[660,32,660,35],[661,24,661,25],[661,18,661,23],[661,26,661,31],[661,32,661,35],[658,24,658,25],[658,18,658,23],[658,26,658,31],[658,32,658,35],[659,24,659,25],[659,18,659,23],[659,26,659,31],[659,32,659,35],[656,24,656,25],[656,18,656,23],[656,26,656,31],[656,32,656,35],[657,24,657,25],[657,18,657,23],[657,26,657,31],[657,32,657,35],[654,24,654,25],[654,18,654,23],[654,26,654,31],[654,32,654,35],[655,24,655,25],[655,18,655,23],[655,26,655,31],[655,32,655,35],[652,23,652,24],[652,17,652,22],[652,25,652,30],[652,31,652,34],[653,23,653,24],[653,17,653,22],[653,25,653,30],[653,31,653,34],[650,24,650,25],[650,18,650,23],[650,26,650,31],[650,32,650,35],[651,23,651,24],[651,17,651,22],[651,25,651,30],[651,31,651,34],[648,24,648,25],[648,18,648,23],[648,26,648,31],[648,32,648,35],[649,24,649,25],[649,18,649,23],[649,26,649,31],[649,32,649,35],[646,24,646,25],[646,18,646,23],[646,26,646,31],[646,32,646,35],[647,24,647,25],[647,18,647,23],[647,26,647,31],[647,32,647,35],[644,24,644,25],[644,18,644,23],[644,26,644,31],[644,32,644,35],[645,24,645,25],[645,18,645,23],[645,26,645,31],[645,32,645,35],[642,23,642,24],[642,17,642,22],[642,25,642,30],[642,31,642,34],[643,23,643,24],[643,17,643,22],[643,25,643,30],[643,31,643,34],[640,23,640,24],[640,17,640,22],[640,25,640,30],[640,31,640,34],[641,22,641,23],[641,16,641,21],[641,24,641,29],[641,30,641,33],[638,23,638,24],[638,17,638,22],[638,25,638,30],[638,31,638,34],[639,23,639,24],[639,17,639,22],[639,25,639,30],[639,31,639,34],[636,23,636,24],[636,17,636,22],[636,25,636,30],[636,31,636,34],[637,23,637,24],[637,17,637,22],[637,25,637,30],[637,31,637,34],[634,23,634,24],[634,17,634,22],[634,25,634,30],[634,31,634,34],[635,23,635,24],[635,17,635,22],[635,25,635,30],[635,31,635,34],[632,23,632,24],[632,17,632,22],[632,25,632,30],[632,31,632,34],[633,23,633,24],[633,17,633,22],[633,25,633,30],[633,31,633,34],[630,23,630,24],[630,17,630,22],[630,25,630,30],[630,31,630,34],[631,23,631,24],[631,17,631,22],[631,25,631,30],[631,31,631,34],[628,23,628,24],[628,17,628,22],[628,25,628,30],[628,31,628,34],[629,23,629,24],[629,17,629,22],[629,25,629,30],[629,31,629,34],[626,23,626,24],[626,17,626,22],[626,25,626,30],[626,31,626,34],[627,23,627,24],[627,17,627,22],[627,25,627,30],[627,31,627,34],[624,23,624,24],[624,17,624,22],[624,25,624,30],[624,31,624,34],[625,23,625,24],[625,17,625,22],[625,25,625,30],[625,31,625,34],[622,24,622,25],[622,18,622,23],[622,26,622,31],[622,32,622,35],[623,23,623,24],[623,17,623,22],[623,25,623,30],[623,31,623,34],[620,24,620,25],[620,18,620,23],[620,26,620,31],[620,32,620,35],[621,24,621,25],[621,18,621,23],[621,26,621,31],[621,32,621,35],[618,23,618,24],[618,17,618,22],[618,25,618,30],[618,31,618,34],[619,23,619,24],[619,17,619,22],[619,25,619,30],[619,31,619,34],[616,21,616,22],[616,15,616,20],[616,23,616,28],[616,29,616,32],[617,22,617,23],[617,16,617,21],[617,24,617,29],[617,30,617,33],[614,21,614,22],[614,15,614,20],[614,23,614,28],[614,29,614,32],[615,22,615,23],[615,16,615,21],[615,24,615,29],[615,30,615,33],[612,22,612,23],[612,16,612,21],[612,24,612,29],[612,30,612,33],[613,22,613,23],[613,16,613,21],[613,24,613,29],[613,30,613,33],[610,22,610,23],[610,16,610,21],[610,24,610,29],[610,30,610,33],[611,22,611,23],[611,16,611,21],[611,24,611,29],[611,30,611,33],[608,24,608,25],[608,18,608,23],[608,26,608,31],[608,32,608,35],[609,22,609,23],[609,16,609,21],[609,24,609,29],[609,30,609,33],[606,24,606,25],[606,18,606,23],[606,26,606,31],[606,32,606,35],[607,24,607,25],[607,18,607,23],[607,26,607,31],[607,32,607,35],[604,25,604,26],[604,19,604,24],[604,27,604,32],[604,33,604,36],[605,24,605,25],[605,18,605,23],[605,26,605,31],[605,32,605,35],[602,24,602,25],[602,18,602,23],[602,26,602,31],[602,32,602,35],[603,24,603,25],[603,18,603,23],[603,26,603,31],[603,32,603,35],[600,25,600,26],[600,19,600,24],[600,27,600,32],[600,33,600,36],[601,24,601,25],[601,18,601,23],[601,26,601,31],[601,32,601,35],[598,26,598,27],[598,20,598,25],[598,28,598,33],[598,34,598,37],[599,26,599,27],[599,20,599,25],[599,28,599,33],[599,34,599,37],[596,25,596,26],[596,19,596,24],[596,27,596,32],[596,33,596,36],[597,25,597,26],[597,19,597,24],[597,27,597,32],[597,33,597,36],[594,26,594,27],[594,20,594,25],[594,28,594,33],[594,34,594,37],[595,26,595,27],[595,20,595,25],[595,28,595,33],[595,34,595,37],[592,25,592,26],[592,19,592,24],[592,27,592,32],[592,33,592,36],[593,25,593,26],[593,19,593,24],[593,27,593,32],[593,33,593,36],[590,26,590,27],[590,20,590,25],[590,28,590,33],[590,34,590,37],[591,26,591,27],[591,20,591,25],[591,28,591,33],[591,34,591,37],[588,25,588,26],[588,19,588,24],[588,27,588,32],[588,33,588,36],[589,25,589,26],[589,19,589,24],[589,27,589,32],[589,33,589,36],[586,26,586,27],[586,20,586,25],[586,28,586,33],[586,34,586,37],[587,26,587,27],[587,20,587,25],[587,28,587,33],[587,34,587,37],[584,26,584,27],[584,20,584,25],[584,28,584,33],[584,34,584,37],[585,26,585,27],[585,20,585,25],[585,28,585,33],[585,34,585,37],[582,24,582,25],[582,18,582,23],[582,26,582,31],[582,32,582,35],[583,25,583,26],[583,19,583,24],[583,27,583,32],[583,33,583,36],[580,25,580,26],[580,19,580,24],[580,27,580,32],[580,33,580,36],[581,23,581,24],[581,17,581,22],[581,25,581,30],[581,31,581,34],[578,25,578,26],[578,19,578,24],[578,27,578,32],[578,33,578,36],[579,24,579,25],[579,18,579,23],[579,26,579,31],[579,32,579,35],[576,25,576,26],[576,19,576,24],[576,27,576,32],[576,33,576,36],[577,25,577,26],[577,19,577,24],[577,27,577,32],[577,33,577,36],[574,24,574,25],[574,18,574,23],[574,26,574,31],[574,32,574,35],[575,24,575,25]],"merged_total":3290,"flags":["merged_cut"]}
[null,null,"FunctionalObject",null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENTATION FUNCTION",null,null,null,null,null,"rdl:RDS2225050",null,"An <INSTRUMENTATION FUNCTION> is a <FunctionalObject> that is capable of one or more of the following activities: <ACTUATING>, <COMPUTING>, <CONTROLLING>, <DETECTING>, <EXECUTING BOOLEAN LOGIC>, <INDICATING>, <MEASURING>, <MONITORING>, <PROTECTING>, <RECORDING>, <REGULATING>, <SIGNAL AMPLIFYING>, <SIGNAL CONVERTING>, <SIGNAL CONVEYING>, <SWITCHING>, <TRANSDUCING>, <TRANSMITTING>, and <WARNING> related to physical variables (quantities)",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,"BOOLEAN LOGIC FUNCTION",null,null,null,null,null,"rdl:RDS222482",null,"A <BOOLEAN LOGIC FUNCTION> is an <INSTRUMENTATION FUNCTION> that is capable of <EXECUTING BOOLEAN LOGIC>.",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"BOOLEAN LOGIC FUNCTION","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"LOGIC ARTEFACT",null,null,null,null,null,"rdl:RDS220111",null,"A <LOGIC ARTEFACT> is an <INSTRUMENTATION ITEM> and a <BOOLEAN LOGIC FUNCTION> that executes Boolean logic and timig functions as required in the process industries",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LOGIC ARTEFACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INTERLOCKING DEVICE",null,null,null,null,null,"rdl:RDS955664",null,"An <INTERLOCKING DEVICE> is a <LOGIC ARTEFACT> that makes the operation of a piece of equipment dependent upon the condition, position or operation of one or more other pieces of equipment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LOGIC ARTEFACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROCESS LOGIC ARTEFACT",null,null,null,null,null,"rdl:RDS222483",null,"A <PROCESS LOGIC ARTEFACT> is a <LOGIC ARTEFACT> that executes Boolean logic and timig functions as required in the process industries",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PROCESS LOGIC ARTEFACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANTI PUMPING ARTEFACT",null,null,null,null,null,"rdl:RDS955619",null,"An <ANTI PUMPING ARTEFACT> is a <PROCESS LOGIC ARTEFACT> that prevents reclosing after a close-open operation as long as the device initiating closing is maintained in the position for closing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LOGIC ARTEFACT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROGRAMMABLE LOGIC CONTROLLER",null,null,null,null,null,"rdl:RDS1008584",null,"A <PROGRAMMABLE LOGIC CONTROLLER> is a <LOGIC ARTEFACT> that continuously monitors the state of input devices and makes decisions based upon a custom program to control the state of output devices",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,"CONTROLLER",null,null,null,null,null,"rdl:RDS289844",null,"A <CONTROLLER> is an <INSTRUMENTATION FUNCTION> that is capable of <CONTROLLING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"CONTROLLER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"ANTI SURGE CONTROLLER",null,null,null,null,null,"rdl:RDS5981292",null,"An <ANTI SURGE CONTROLLER> is a <PROCESS INSTRUMENTATION ITEM> and a <CONTROLLER> that continuously measures and provides multi-variable proximity-to-surge calculations in order to protect the compressor against surge; it is specifically designed for this purpose",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"BURNER CONTROLLER",null,null,null,null,null,"rdl:RDS6535671",null,"A <BURNER CONTROLLER> is an <INSTRUMENTATION ITEM> and a <CONTROLLER> that is designed and programmed to control the operation of a burner",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"CHARGE CONTROLLER",null,null,null,null,null,"rdl:RDS5764044",null,"A <CHARGE CONTROLLER> is a <INSTRUMENTATION ITEM> and a <CONTROLLER> for controlling the quantity of unbalanced electricity in a body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLER","SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,"CONTROL SYSTEM",null,null,null,null,null,"rdl:RDS13610030",null,"A <CONTROL SYSTEM> is a <SYSTEM> and a <CONTROLLER> intended to control the operation of a machine, unit or process",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"CONTROL SYSTEM","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"CENTRIFUGAL COMPRESSOR BUFFER GAS CONTROL SYSTEM",null,null,null,null,null,"rdl:RDS14214727",null,"A <CENTRIFUGAL COMPRESSOR BUFFER GAS CONTROL SYSTEM> is an <INSTRUMENTATION ITEM> and a <CONTROL SYSTEM> intended to control the buffer gas system on a centrifugal compressor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SYSTEM","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"CENTRIFUGAL COMPRESSOR PROCESS CONTROL",null,null,null,null,null,"rdl:RDS14207329",null,"A <CENTRIFUGAL COMPRESSOR PROCESS CONTROL> is an <INSTRUMENTATION ITEM> and a <CONTROL SYSTEM> that is intended for use on a centrifugal compressor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SYSTEM","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"CRANE MASTER",null,null,null,null,null,"rdl:RDS1066965381",null,"A <CRANE MASTER> is an <INSTRUMENTATION ITEM> and a <CONTROL SYSTEM> intended to control a crane",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SYSTEM","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"FUEL INJECTION CONTROL SYSTEM",null,null,null,null,null,"rdl:RDS13662846",null,"A <FUEL INJECTION CONTROL SYSTEM> is an <INSTRUMENTATION ITEM> and a <CONTROL SYSTEM> intended to control the operation of the fuel injection on an internal combustion engine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SYSTEM","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"INLET GUIDE VANE CONTROL",null,null,null,null,null,"rdl:RDS407109371",null,"An <INLET GUIDE VANE CONTROL> is an <INSTRUMENTATION ITEM> and a <CONTROL SYSTEM> that uses the adjustment of the angle in order to position the inlet guide vanes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SYSTEM","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"REMOTE-OPERATED CONTROL UNIT",null,null,null,null,null,"rdl:RDS5761886",null,"A <REMOTE-OPERATED CONTROL UNIT> is an <INSTRUMENTATION ITEM> and a <CONTROL SYSTEM> that can be operated in remote",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SYSTEM","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"SPEED GOVERNOR SYSTEM",null,null,null,null,null,"rdl:RDS13310290",null,"A <SPEED GOVERNOR SYSTEM> is an <INSTRUMENTATION ITEM> and a <CONTROL SYSTEM> intended to control a speed by means of a governor and related equipment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SYSTEM","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA PRODUCTION CONTROL SYSTEM",null,null,null,null,null,"rdl:RDS16761080",null,"A <SUBSEA PRODUCTION CONTROL SYSTEM> is an <INSTRUMENTATION ITEM> and a <CONTROL SYSTEM> that is a well production control system intended to be installed in a subsea environment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SYSTEM","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"WELL PRODUCTION CONTROL SYSTEM",null,null,null,null,null,"rdl:RDS16761001",null,"A <WELL PRODUCTION CONTROL SYSTEM> is an <INSTRUMENTATION ITEM> and a <CONTROL SYSTEM> intended to control equipment during production and/or injection operations in wells",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC CONTROLLER",null,null,null,null,null,"rdl:RDS879839",null,"An <ELECTRONIC CONTROLLER> is an <INSTRUMENTATION ITEM> and a <CONTROLLER> that uses in-built algorithms executed by electronic circuitry to perform its function",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CONTROLLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUS CONTROLLER",null,null,null,null,null,"rdl:RDS6536046",null,"A <BUS CONTROLLER> is an <ELECTRONIC CONTROLLER> that is intended to control the data traffic of a bus",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CONTROLLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMMUNICATIONS CONTROLLER",null,null,null,null,null,"rdl:RDS6535566",null,"A <COMMUNICATIONS CONTROLLER> is an <ELECTRONIC CONTROLLER> that is intended to act as a node in a communication network",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CONTROLLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DISK CONTROLLER",null,null,null,null,null,"rdl:RDS6535716",null,"A <DISK CONTROLLER> is an <ELECTRONIC CONTROLLER> that is intended to control a hard disk drive",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CONTROLLER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VDU CONTROLLER",null,null,null,null,null,"rdl:RDS6536151",null,"A <VDU CONTROLLER> is an <ELECTRONIC CONTROLLER> that is intended to control a visual display unit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC CONTROLLER",null,null,null,null,null,"rdl:RDS880514",null,"A <HYDRAULIC CONTROLLER> is an <INSTRUMENTATION ITEM> and a <CONTROLLER> that is designed or can be programmed to operate and control hydraulic operated systems",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"MANUAL LOADING STATION",null,null,null,null,null,"rdl:RDS880829",null,"A <MANUAL LOADING STATION> is an <INSTRUMENTATION ITEM> and a <CONTROLLER> that is dedicated to manually manipulate a final control device",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","CONTROLLER",null,null,null,null,null,null,null,null,null,null,null,null,"MODULATING CONTROLLER",null,null,null,null,null,"rdl:RDS270224",null,"An <MODULATING CONTROLLER> is an <ARTEFACT> and a <CONTROLLER> which has the capability OF <MODULATING CONTROLLING>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLER",null,null,null,null,null,null,null,null,null,null,null,null,null,"MOTOR CONTROLLER",null,null,null,null,null,"rdl:RDS1008359",null,"A <MOTOR CONTROLLER> is a <CONTROLLER> that serves to govern in some predetermined manner the performance of an electric motor",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","CONTROLLER",null,null,null,null,null,null,null,null,null,null,null,null,"ON OFF CONTROLLER",null,null,null,null,null,"rdl:RDS270269",null,"An <ON OFF CONTROLLER> is an <ARTEFACT> and a <CONTROLLER> that is a two step controller in which one of the steps is assigned the value zero",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC CONTROLLER",null,null,null,null,null,"rdl:RDS882179",null,"A <PNEUMATIC CONTROLLER> is an <INSTRUMENTATION ITEM> and a <CONTROLLER> that is using pneumatic components to execute its function",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","CONTROLLER",null,null,null,null,null,null,null,null,null,null,null,null,"SAFEGUARD CONTROLLER",null,null,null,null,null,"rdl:RDS325529",null,"A <SAFEGUARD CONTROLLER> is an <ARTEFACT> and a <CONTROLLER> which has the capability to drive the output to High or Low upon an unwanted state of a <PLANT> or a component thereof",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","CONTROLLER",null,null,null,null,null,null,null,null,null,null,null,null,"SETPOINT CHOKE VALVE CONTROLLER",null,null,null,null,null,"rdl:RDS325619",null,"A <SETPOINT CHOKE VALVE CONTROLLER> is an <ARTEFACT> and a <CONTROLLER> which has the capability to control the Choke valve position automatically to a given setpoint",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","CONTROLLER",null,null,null,null,null,null,null,null,null,null,null,null,"SPEED GOVERNOR",null,null,null,null,null,"rdl:RDS5760378",null,"A <SPEED GOVERNOR> is an <ARTEFACT> and a <CONTROLLER> that consists of those elements that respond directly to speed and that actuate the position of other parts of the speed governor system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPEED GOVERNOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONSTANT SPEED GOVERNOR",null,null,null,null,null,"rdl:RDS13284662",null,"A <CONSTANT SPEED GOVERNOR> is a <SPEED GOVERNOR> which monitors and adjusts the rotational speed of a machine to a fixed predetermined value",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPEED GOVERNOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC GOVERNOR",null,null,null,null,null,"rdl:RDS403477161",null,"An <ELECTRONIC GOVERNOR> is a <SPEED GOVERNOR> utilizing an electronic control system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPEED GOVERNOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC GOVERNOR",null,null,null,null,null,"rdl:RDS815039",null,"A <HYDRAULIC GOVERNOR> is a <SPEED GOVERNOR> that is provided with a special centrifugal pump as speed-sensing element",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPEED GOVERNOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ISOCHRONOUS GOVERNOR",null,null,null,null,null,"rdl:RDS408009261",null,"An <ISOCHRONOUS GOVERNOR> is a <SPEED GOVERNOR> that holds the speed constant at all loads",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPEED GOVERNOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MECHANICAL SPEED GOVERNOR",null,null,null,null,null,"rdl:RDS815669",null,"A <MECHANICAL SPEED GOVERNOR> is a <SPEED GOVERNOR> that contains flyweights intended to move the spring loaded speeder rod and activate the speed changer/control mechanism",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPEED GOVERNOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RELAYED SPEED GOVERNOR",null,null,null,null,null,"rdl:RDS6539864",null,"A <RELAYED SPEED GOVERNOR> is a <SPEED GOVERNOR> that needs an amplification such as pilot valve, servomotor or differently in order to move the control valve(s)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPEED GOVERNOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TURBINE SPEED GOVERNOR",null,null,null,null,null,"rdl:RDS816794",null,"A <TURBINE SPEED GOVERNOR> is a <SPEED GOVERNOR> intended to adjust the intake valves of the turbine in order to maintain the speed of rotation at a required value",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPEED GOVERNOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VARIABLE SPEED GOVERNOR",null,null,null,null,null,"rdl:RDS13284724",null,"A <VARIABLE SPEED GOVERNOR> is a <SPEED GOVERNOR> which monitors and adjusts the rotational speed of a machine to an optional value",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLER","INSTRUMENTATION ITEM","STANDARD SIGNAL RECEIVER","STANDARD SIGNAL SENDER",null,null,null,null,null,null,null,null,null,null,"STANDARD SIGNAL CONTROLLER",null,null,null,null,null,"rdl:RDS2223257",null,"A <STANDARD SIGNAL CONTROLLER> is an <INSTRUMENTATION ITEM> and a <CONTROLLER> and a <STANDARD SIGNAL RECEIVER> and a <STANDARD SIGNAL SENDER>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"START CONTROLLER",null,null,null,null,null,"rdl:RDS6810820",null,"A <START CONTROLLER> is an <INSTRUMENTATION ITEM> and a <CONTROLLER> intended to control the starting of an engine or motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","CONTROLLER",null,null,null,null,null,null,null,null,null,null,null,null,"STEP CONTROLLER",null,null,null,null,null,"rdl:RDS324314",null,"A <STEP CONTROLLER> is an <ARTEFACT> and a <CONTROLLER> which has the capability to control a <CHOKE VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,"FINAL CONTROL FUNCTION",null,null,null,null,null,"rdl:RDS2220650",null,"A <FINAL CONTROL FUNCTION> is an <INSTRUMENTATION FUNCTION> that physically changes a process in response to a change in the output from a <CONTROLLER>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"FINAL CONTROL FUNCTION","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,"CONTROL VALVE",null,null,null,null,null,"rdl:RDS297539",null,"A <CONTROL VALVE> is a <VALVE> and an <FINAL CONTROL FUNCTION>, operated by an <ACTUATOR> that can be used to modify (regulate) the fluid flow rate in response to a signal from a <PROCESS CONTROL DEVICE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANGLE VALVE","CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"ANGLE CONTROL VALVE",null,null,null,null,null,"rdl:RDS5791021",null,"An <ANGLE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and an <ANGLE VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"ANTI CAVITATION CONTROL VALVE",null,null,null,null,null,"rdl:RDS11273555",null,"An <ANTI CAVITATION CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that can be used to prevent cavitation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BIDIRECTIONAL VALVE","CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"BI-DIRECTIONAL CONTROL VALVE",null,null,null,null,null,"rdl:RDS16744700",null,"A <BI-DIRECTIONAL CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <BI-DIRECTIONAL VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BI-DIRECTIONAL CONTROL VALVE","THREE WAY CONTROL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHANGE-OVER CONTROL VALVE",null,null,null,null,null,"rdl:RDS16744813",null,"A <CHANGE-OVER CONTROL VALVE> is a <BI-DIRECTIONAL CONTROL VALVE> and a <THREE WAY CONTROL VALVE> with two inlet ports and one outlet port, enabling changing between dual supplies",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BUTTERFLY VALVE","CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"BUTTERFLY CONTROL VALVE",null,null,null,null,null,"rdl:RDS5791128",null,"A <BUTTERFLY CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <BUTTERFLY VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"CAGE TRIM CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142445",null,"A <CAGE TRIM CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that has a cage trim, which is a cylinder with openings in the wall, and which surrounds and guides the plug closure member of a plug type globe valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"CHEMICAL INJECTION DOSING CONTROL VALVE",null,null,null,null,null,"rdl:RDS16757390",null,"A <CHEMICAL INJECTION DOSING CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> which is used to control the rate and amount of the chemicals injection into the well or flowline",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"CIRCULATION CONTROL VALVE",null,null,null,null,null,"rdl:RDS17609942",null,"A <CIRCULATION CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> normally placed across a circulation point to allow isolation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","CRYOGENIC VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"CRYOGENIC CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142580",null,"A <CRYOGENIC CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <CRYOGENIC VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"DELUGE CONTROL VALVE",null,null,null,null,null,"rdl:RDS6329587",null,"A <DELUGE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that is intended to operate at high temperature, and admit water into a deluge system. It is fail safe, kept closed by pressurised gas, and is typically made of bronze",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DELUGE CONTROL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DELUGE VALVE WITH AFFF",null,null,null,null,null,"rdl:RDS297854",null,"A <DELUGE VALVE WITH AFFF> is a <DELUGE VALVE> that is installed in a deluge sprinkler system, which spreads <AFFF> (Aqueous Film Forming Foam) out in an area of an installation in case of fire",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECTIONAL CONTROL VALVE",null,null,null,null,null,"rdl:RDS16744139",null,"A <DIRECTIONAL CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that operates in one direction, having a reset function",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"ECCENTRIC ROTATING DISC CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142670",null,"An <ECCENTRIC ROTATING DISC CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that uses a rotating disc as closing element, and with a design that causes the disc to take a slightly eccentric path during actuation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","GATE VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"GATE CONTROL VALVE",null,null,null,null,null,"rdl:RDS17079788",null,"A <GATE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <GATE VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","GLOBE VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"GLOBE CONTROL VALVE",null,null,null,null,null,"rdl:RDS5767330",null,"A <GLOBE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <GLOBE VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"HIGH DIFFERENTIAL PRESSURE CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142085",null,"A <HIGH DIFFERENTIAL PRESSURE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that is intended to operate when the downstream pressure is much lower than the upstream pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"HIGH TEMPERATURE CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142130",null,"A <HIGH TEMPERATURE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that is intended to withstand high temperature operating conditions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM","SLIDE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC DIRECTIONAL CONTROL VALVE",null,null,null,null,null,"rdl:RDS5800454",null,"A <HYDRAULIC DIRECTIONAL CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <SLIDE VALVE> that is designed to operate in a hydraulic system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"LOW NOISE CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142175",null,"A <LOW NOISE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that is designed to generate low noise levels during operation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM","MEMBRANE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,"MEMBRANE CONTROL VALVE",null,null,null,null,null,"rdl:RDS11215886",null,"A <MEMBRANE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <MEMBRANE VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"MIXING CONTROL VALVE",null,null,null,null,null,"rdl:RDS11273885",null,"A <MIXING CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that usually is self-operating and can use a control element to regulate flow input(s)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM","MULTIPLE SEAT VALVE",null,null,null,null,null,null,null,null,null,null,null,null,"MULTIPLE SEAT CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142355",null,"A <MULTIPLE SEAT CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <MULTIPLE SEAT VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"ON-OFF CONTROL VALVE",null,null,null,null,null,"rdl:RDS11141905",null,"An <ON-OFF CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that only has two defined positions, being fully open and fully closed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM","PLUG VALVE",null,null,null,null,null,null,null,null,null,null,null,null,"PLUG CONTROL VALVE",null,null,null,null,null,"rdl:RDS5791353",null,"A <PLUG CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <PLUG VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"SEALING STEAM CONTROL VALVE",null,null,null,null,null,"rdl:RDS418634441",null,"A <SEALING STEAM CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that reduces the steam supply pressure from the admission steam valve to a very slight overpressure to avoid air inrush into the shaft labyrinths of a condensing steam turbine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"SLAM SHUT CONTROL VALVE",null,null,null,null,null,"rdl:RDS646964",null,"A <SLAM SHUT CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that has a disc which is held open against the flow and closes automatically when released",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM","THREE WAY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,"THREE WAY CONTROL VALVE",null,null,null,null,null,"rdl:RDS293894",null,"A <THREE WAY CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <THREE WAY VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATOR","FINAL CONTROL FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,"CONTROLLED ACTUATOR",null,null,null,null,null,"rdl:RDS2220505",null,"A <CONTROLLED ACTUATOR> is an <ACTUATOR> and a <FINAL CONTROL FUNCTION> that is remotely operated",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"CONTROLLED ACTUATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"DIAPHRAGM ACTUATOR",null,null,null,null,null,"rdl:RDS6491422",null,"A <DIAPHRAGM ACTUATOR> is an <INSTRUMENTATION ITEMT> and a <CONTROLLED ACTUATOR> that is using a <DIAPHRAGM>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIAPHRAGM ACTUATOR","PNEUMATIC ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC DIAPHRAGM ACTUATOR",null,null,null,null,null,"rdl:RDS430109",null,"A <PNEUMATIC DIAPHRAGM ACTUATOR> is a <CONTROLLED ACTUATOR> and a <PNEUMATIC ACTUATOR> that is operated using low-pressure air supply",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOUBLE ACTING ACTUATOR","PNEUMATIC DIAPHRAGM ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE ACTING PNEUMATIC DIAPHRAGM ACTUATOR",null,null,null,null,null,"rdl:RDS6625398",null,"A <DOUBLE ACTING PNEUMATIC DIAPHRAGM ACTUATOR> is a <PNEUMATIC DIAPHRAGM ACTUATOR> and a <DOUBLE ACTING ACTUATOR> that is actuated by low-pressure air and is driven in both directions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PNEUMATIC DIAPHRAGM ACTUATOR","SINGLE ACTING ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE ACTING PNEUMATIC DIAPHRAGM ACTUATOR",null,null,null,null,null,"rdl:RDS6625443",null,"A <SINGLE ACTING PNEUMATIC DIAPHRAGM ACTUATOR> is a <PNEUMATIC DIAPHRAGM ACTUATOR> and a <SINGLE ACTING ACTUATOR> that is actuated by low-pressure air and is driven in one direction only",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"DIGITAL ACTUATOR",null,null,null,null,null,"rdl:RDS16144733",null,"A <DIGITAL ACTUATOR is an <INSTRUMENTATION ITEM> and a <CONTROLLED ACTUATOR> that is controlled by a digital signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE ACTING ACTUATOR",null,null,null,null,null,"rdl:RDS6594380",null,"A <DOUBLE ACTING ACTUATOR is an <INSTRUMENTATION ITEM> and a <CONTROLLED ACTUATOR> that is able to operate in both directions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOUBLE ACTING ACTUATOR","HYDRAULIC PISTON ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE ACTING HYDRAULIC PISTON ACTUATOR",null,null,null,null,null,"rdl:RDS6625578",null,"A <DOUBLE ACTING HYDRAULIC PISTON ACTUATOR> is a <HYDRAULIC PISTON ACTUATOR> and a <DOUBLE ACTING ACTUATOR> that is a hydraulic piston actuator that is actuated by hydraulic fluid and is driven in both directions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOUBLE ACTING ACTUATOR","PNEUMATIC PISTON ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE ACTING PNEUMATIC PISTON ACTUATOR",null,null,null,null,null,"rdl:RDS6625488",null,"A <DOUBLE ACTING PNEUMATIC PISTON ACTUATOR> is a <PNEUMATIC PISTON ACTUATOR> and a <DOUBLE ACTING ACTUATOR> that is a pneumatic piston actuator that is actuated by low-pressure air and is driven in two directions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","ELECTRICAL APPARATUS","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC ACTUATOR",null,null,null,null,null,"rdl:RDS430379",null,"An <ELECTRIC ACTUATOR> is an <INSTRUMENTATION ITEM> and an <ELECTRICAL APPARATUS> and a <CONTROLLED ACTUATOR> that produces a specified movement when actuated by electrical energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC ACTUATOR WITH HANDWHEEL",null,null,null,null,null,"rdl:RDS11507710",null,"An <ELECTRIC ACTUATOR WITH HANDWHEEL> is an <ELECTRIC ACTUATOR> with a handwheel for operating the valve manually",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ACTUATOR","HYDRAULIC ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC HYDRAULIC ACTUATOR",null,null,null,null,null,"rdl:RDS7195780",null,"An <ELECTRIC HYDRAULIC ACTUATOR> is an <ELECTRIC ACTUATOR> and a <HYDRAULIC ACTUATOR> having a fluid pump driven by an electric motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC HYDRAULIC ACTUATOR","VALVE ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRO-HYDRAULIC VALVE ACTUATOR",null,null,null,null,null,"rdl:RDS16742011",null,"An <ELECTRO-HYDRAULIC VALVE ACTUATOR> is a <VALVE ACTUATOR> and a <ELECTRIC HYDRAULIC ACTUATOR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ACTUATOR","VALVE ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC VALVE ACTUATOR",null,null,null,null,null,"rdl:RDS7028560",null,"An <ELECTRIC VALVE ACTUATOR> is an <ELECTRIC ACTUATOR> and a <VALVE ACTUATOR> that is a valve actuator that is intended to be driven by an electric motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLENOID ACTUATOR",null,null,null,null,null,"rdl:RDS7191376",null,"A <SOLENOID ACTUATOR> is an <ELECTRIC ACTUATOR> that is utilizing a continuous duty linear solenoid to convert electrical energy into mechanical power via a plunger with an axial stroke in either a push or pull action",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLENOID ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DUAL SOLENOID ACTUATOR",null,null,null,null,null,"rdl:RDS7191440",null,"A <DUAL SOLENOID ACTUATOR> is a <SOLENOID ACTUATOR> with two solenoids that are energized one at a time, each causing a move in an opposite direction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLENOID ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PILOT AIR OPERATED SOLENOID ACTUATOR",null,null,null,null,null,"rdl:RDS7191609",null,"A <PILOT AIR OPERATED SOLENOID ACTUATOR> is a <SOLENOID ACTUATOR> in which operation is boosted by an external supply of pilot air",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLENOID ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE SOLENOID ACTUATOR",null,null,null,null,null,"rdl:RDS7191502",null,"A <SINGLE SOLENOID ACTUATOR> is a <SOLENOID ACTUATOR> with one solenoid where the two opposite positions are for energized vs de-energized",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","HYDRAULIC TO MECHANICAL ENERGY CONVERTER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC ACTUATOR",null,null,null,null,null,"rdl:RDS430154",null,"A <HYDRAULIC ACTUATOR> is an <INSTRUMENTATION ITEM> and a <CONTROLLED ACTUATOR> and a <HYDRAULIC TO MECHANICAL ENERGY CONVERTER>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC PISTON ACTUATOR",null,null,null,null,null,"rdl:RDS884879",null,"A <HYDRAULIC PISTON ACTUATOR> is a <HYDRAULIC ACTUATOR> that is intended to operate by a displacement of a piston using hydraulic energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC PISTON ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC PISTON ACTUATOR SPRING RETURN",null,null,null,null,null,"rdl:RDS11507614",null,"A <HYDRAULIC PISTON ACTUATOR SPRING RETURN> is a <HYDRAULIC PISTON ACTUATOR> with a spring acting on one side of the piston",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC PISTON ACTUATOR","SINGLE ACTING ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE ACTING HYDRAULIC PISTON ACTUATOR",null,null,null,null,null,"rdl:RDS6625353",null,"A <SINGLE ACTING HYDRAULIC PISTON ACTUATOR> is a <HYDRAULIC PISTON ACTUATOR> that is actuated by hydraulic fluid and is driven in one direction only",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC ACTUATOR","VALVE ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC VALVE ACTUATOR",null,null,null,null,null,"rdl:RDS7503442",null,"A <HYDRAULIC VALVE ACTUATOR> is a <HYDRAULIC ACTUATOR> and a <VALVE ACTUATOR> that is designed to operate a valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"MAGNETIC ACTUATOR",null,null,null,null,null,"rdl:RDS7195887",null,"A <MAGNETIC ACTUATOR> is an <INSTRUMENTATION ITEM> and a <CONTROLLED ACTUATOR> where the force is provided by magnetic forces",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"MODULATING ACTUATOR",null,null,null,null,null,"rdl:RDS1458713041",null,"A <MODULATING ACTUATOR> is an <INSTRUMENTATION ITEM> and a <CONTROLLED ACTUATOR> that can take any position between the limits",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"MOTOR ACTUATOR",null,null,null,null,null,"rdl:RDS16145021",null,"A <MOTOR ACTUATOR> is an <INSTRUMENTATION ITEM> and a <CONTROLLED ACTUATOR> powered by a motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"ONE CYLINDER ACTUATOR",null,null,null,null,null,"rdl:RDS6607127",null,"An <ONE CYLINDER ACTUATOR> is an <INSTRUMENTATION ITEM> and a <CONTROLLED ACTUATOR> which has got one cylinder acting on the actuator driving sleeve creating torque",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"PILOT ACTUATOR",null,null,null,null,null,"rdl:RDS16145280",null,"A <PILOT ACTUATOR> is an <INSTRUMENTATION ITEM> and a <CONTROLLED ACTUATOR> which operation is controlled by a pilot signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"PISTON ACTUATOR",null,null,null,null,null,"rdl:RDS6631280",null,"A <PISTON ACTUATOR> is an <INSTRUMENTATION ITEM> and a <CONTROLLED ACTUATOR> intended to operate by displacement of a piston by the use of pneumatic or hydraulic energy",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PISTON ACTUATOR","PNEUMATIC ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC PISTON ACTUATOR",null,null,null,null,null,"rdl:RDS476864",null,"A <PNEUMATIC PISTON ACTUATOR> is a <PISTON ACTUATOR> that is operated by compressed air",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PNEUMATIC PISTON ACTUATOR","SINGLE ACTING ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE ACTING PNEUMATIC PISTON ACTUATOR",null,null,null,null,null,"rdl:RDS6625533",null,"A <SINGLE ACTING PNEUMATIC PISTON ACTUATOR> is a <PNEUMATIC PISTON ACTUATOR> that is actuated by low-pressure air and is driven in one direction only",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC ACTUATOR",null,null,null,null,null,"rdl:RDS430334",null,"A <PNEUMATIC ACTUATOR> is an <INSTRUMENTATION ITEM> and a <CONTROLLED ACTUATOR> that is intended to be operated by pneumatic power",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PNEUMATIC ACTUATOR","VALVE ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC VALVE ACTUATOR",null,null,null,null,null,"rdl:RDS7503487",null,"A <PNEUMATIC VALVE ACTUATOR> is a <VALVE ACTUATOR> and a <PNEUMATIC ACTUATOR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"STEPPING ACTUATOR",null,null,null,null,null,"rdl:RDS370725574",null,"A <STEPPING ACTUATOR> is an <INSTRUMENTATION ITEM> and a <CONTROLLED ACTUATOR> that can be moved in discrete steps",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STEPPING ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL STEPPING ACTUATOR",null,null,null,null,null,"rdl:RDS370725624",null,"An <ELECTRICAL STEPPING ACTUATOR> is a <STEPPING ACTUATOR> having an electrical motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STEPPING ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC STEPPING ACTUATOR",null,null,null,null,null,"rdl:RDS3707255912",null,"A <HYDRAULIC STEPPING ACTUATOR> is a <STEPPING ACTUATOR> having a hydraulic motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROLLED ACTUATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE ACTUATOR",null,null,null,null,null,"rdl:RDS7019057",null,"A <VALVE ACTUATOR> is an <INSTRUMENTATION ITEM> and a <CONTROLLED ACTUATOR> intended to change and/or maintain the position of the closing member of a valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPRESSOR UNLOAD VALVE ACTUATOR",null,null,null,null,null,"rdl:RDS7028035",null,"A <COMPRESSOR UNLOAD VALVE ACTUATOR> is a <VALVE ACTUATOR> that is operating a suction valve or clearance pocket valve on a reciprocating compressor, in order to have the compressor run at part-load or at no-load condition",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOTOR OPERATED VALVE ACTUATOR",null,null,null,null,null,"rdl:RDS11142310",null,"A <MOTOR OPERATED VALVE ACTUATOR> is a <VALVE ACTUATOR> that is driven by an electrical motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPRING CONTROLLED VALVE ACTUATOR",null,null,null,null,null,"rdl:RDS11141275",null,"An <SPRING CONTROLLED VALVE ACTUATOR> is a <VALVE ACTUATOR> that has a spring which acts as the trigger to open or close the valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE CLOSING ACTUATOR",null,null,null,null,null,"rdl:RDS313829",null,"A <VALVE CLOSING ACTUATOR> is a <VALVE ACTUATOR> that only closes a valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE ACTUATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE OPENING ACTUATOR",null,null,null,null,null,"rdl:RDS313964",null,"A <VALVE OPENING ACTUATOR> is a <VALVE ACTUATOR> that only opens a valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FINAL CONTROL FUNCTION","INSTRUMENTATION ITEM","SYSTEM",null,null,null,null,null,null,null,null,null,null,null,"FINAL CONTROL ASSEMBLY",null,null,null,null,null,"rdl:RDS2229978",null,"A <FINAL CONTROL ASSEMBLY> is an <INSTRUMENTATION ITEM> and a <FINAL CONTROL FUNCTION> and a <SYSTEM> that is the assembly of a <CONTROL VALVE>, <CONTROLLED ACTUATOR>, <POSITIONER>, or <VARIABLE SPEED DRIVE UNIT> and all necessary piping, tubing, wiring, power supply, and other accessories around it",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FINAL CONTROL FUNCTION","STANDARD SIGNAL RECEIVER",null,null,null,null,null,null,null,null,null,null,null,null,"POSITIONER",null,null,null,null,null,"rdl:RDS415844",null,"A <POSITIONER> is a <FINAL CONTROL FUNCTION> and a <STANDARD SIGNAL RECEIVER> that is intended to position a given item in proportion with a <STANDARD SIGNAL>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","POSITIONER",null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE POSITIONER",null,null,null,null,null,"rdl:RDS2229945",null,"A <VALVE POSITIONER> is an <INSTRUMENTATION ITEM> and a <POSITIONER> for a <CONTROL VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","FINAL CONTROL FUNCTION","STANDARD SIGNAL RECEIVER",null,null,null,null,null,null,null,null,null,null,null,"VARIABLE FREQUENCY DRIVE",null,null,null,null,null,"rdl:RDS2226607",null,"A <VARIABLE FREQUENCY DRIVE> (VFD) is an <ARTEFACT> and a <FINAL CONTROL FUNCTION> and a <STANDARD SIGNAL RECEIVER> that controls the rotational speed of an <ALTERNATING CURRENT MOTOR> by controlling the <FREQUENCY> and <VOLTAGE> of the electrical power supplied to that motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","FINAL CONTROL FUNCTION","STANDARD SIGNAL RECEIVER",null,null,null,null,null,null,null,null,null,null,null,"VARIABLE SPEED DRIVE UNIT",null,null,null,null,null,"rdl:RDS860444",null,"A <VARIABLE SPEED DRIVE UNIT> is an <ARTEFACT> and a <FINAL CONTROL FUNCTION> and a <STANDARD SIGNAL RECEIVER> that consists of an electric motor and controller that is used to adjust the motors operating speed in proportion with a <STANDARD SIGNAL>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,"INDICATOR",null,null,null,null,null,"rdl:RDS418499",null,"An <INDICATOR> is an <INSTRUMENTATION FUNCTION> that has a capability of <INDICATING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INDICATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"ANALOGUE INDICATOR",null,null,null,null,null,"rdl:RDS671084",null,"An <ANALOGUE INDICATOR> is an <INSTRUMENTATION ITEM> and an <INDICATOR> that gives a visual indication of a measured variable by a pointer on a dial",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDICATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"DIRECT ACTING INDICATOR",null,null,null,null,null,"rdl:RDS933704",null,"A <DIRECT ACTING INDICATOR> is an <INSTRUMENTATION ITEM> and an <INDICATOR> in which the indicator is mechanically connected to, and actuated by, the moving element",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW INDICATOR",null,null,null,null,null,"rdl:RDS268379",null,"A <FLOW INDICATOR> IS AN <INDICATOR> that measures flow"]
[null,null,"FLOW INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POSITIVE DISPLACEMENT TYPE FLOW TOTALIZING INDICATOR",null,null,null,null,null,"rdl:RDS308654",null,"A <POSITIVE DISPLACEMENT TYPE FLOW TOTALIZING INDICATOR> is a <FLOW INDICATOR> that is a hydraulic motor with high volumetric efficiency that absorbs a small amount of energy (which actually is a pressure drop) from the flowing stream. Total flow can be calculated from the rotation and pressure drop"]
[null,null,"INDICATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"INDIRECT ACTING INDICATOR",null,null,null,null,null,"rdl:RDS933749",null,"An <INDIRECT ACTING INDICATOR> is an <INSTRUMENTATION ITEM> and an <INDICATOR> in which the indicating or recording device is driven by a motor or other device, as a function of the value of the measurand",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDICATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT WITH OPTICAL INDEX",null,null,null,null,null,"rdl:RDS933569",null,"An <INSTRUMENT WITH OPTICAL INDEX> is an <INSTRUMENTATION ITEM> and an <INDICATOR> in which the indications are given by the displacement of an optical index over a scale which may be a part of the instrument or may be separate from it",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDICATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"MOVING-SCALE INSTRUMENT",null,null,null,null,null,"rdl:RDS933614",null,"A <MOVING-SCALE INSTRUMENT> is an <INSTRUMENTATION ITEM> and an <INDICATOR> in which the scale moves relative to a fixed index",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDICATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"MULTI POINT INDICATOR",null,null,null,null,null,"rdl:RDS1009349",null,"A <MULTI POINT INDICATOR> is an <INSTRUMENTATION ITEM> and an <INDICATOR> that is intended to indicate more than one property at the same time",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDICATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"POINTER INSTRUMENT",null,null,null,null,null,"rdl:RDS933524",null,"A <POINTER INSTRUMENT> is an <INSTRUMENTATION ITEM> and an <INDICATOR> in which the index is a pointer moving over a fixed scale",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,"POSITION INDICATOR",null,null,null,null,null,"rdl:RDS416024",null,"A <POSITION INDICATOR> is an <ARTEFACT> and an <INDICATOR> that measures position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"POSITION INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE POSITION INDICATOR",null,null,null,null,null,"rdl:RDS16742860",null,"A <VALVE POSITION INDICATOR> is a <POSITION INDICATOR> intended to display the position of a valve element",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE INDICATOR",null,null,null,null,null,"rdl:RDS268334",null,"A <PRESSURE INDICATOR> IS AN <INDICATOR> that measures pressure"]
[null,null,"PRESSURE INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL PRESSURE INDICATOR",null,null,null,null,null,"rdl:RDS5786050",null,"A <DIFFERENTIAL PRESSURE INDICATOR> is a <PRESSURE INDICATOR> that is indicating the difference between two fluid pressures applied to it"]
[null,null,"INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"PROCESS VARIABLE METER",null,null,null,null,null,"rdl:RDS2229045",null,"A <PROCESS VARIABLE METER> is an<INDICATOR> that is stand-alone and that has been specifically designed for the given service",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AREOMETER",null,null,null,null,null,"rdl:RDS8180060",null,"An <AREOMETER> is a <PROCESS VARIABLE METER> consisting of a graduated glass tube terminating in a loaded bulb, for measuring the specific gravity of fluids",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONDUCTIVITY METER",null,null,null,null,null,"rdl:RDS878714",null,"A <CONDUCTIVITY METER> is a <PROCESS VARIABLE METER> that is used for measuring electrical conductivity in fluids",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CORROSION METER",null,null,null,null,null,"rdl:RDS5859071",null,"A <CORROSION METER> is a <PROCESS VARIABLE METER> intended to measure and indicate and/or produce a signal which represents the rate or degree of corrosion",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COULOMETER",null,null,null,null,null,"rdl:RDS915479",null,"A <COULOMETER> is a <PROCESS VARIABLE METER> for determining the amount of a substance released during electrolysis by measuring the electrical charge",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DENSITOMETER",null,null,null,null,null,"rdl:RDS884789",null,"A <DENSITOMETER> is a <PROCESS VARIABLE METER> that measures the degree of darkness in photographic or semitransparent material. The densitometer is basically a light source aimed at a photoelectric cell which determines the density of the sample from differences in the readings",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL PRESSURE METER",null,null,null,null,null,"rdl:RDS879299",null,"A <DIFFERENTIAL PRESSURE METER> is a <PROCESS VARIABLE METER> that is intended to measure and indicate and/or produce a signal which represent a measured differential pressure",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DYNAMOMETER",null,null,null,null,null,"rdl:RDS7924104",null,"A <DYNAMOMETER> is a <PROCESS VARIABLE METER> that is intended for measuring the brake horsepower of a prime mover or engine",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RATED CAPACITY INDICATOR",null,null,null,null,null,"rdl:RDS1325731911",null,"A <RATED CAPACITY INDICATOR> is a <PROCESS VARIABLE METER> using a <WEIGHT MEASURING ELEMENT>, that provides a crane operator with information required to operate a crane within safe working limits",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOUND LEVEL METER",null,null,null,null,null,"rdl:RDS6635318",null,"A <SOUND LEVEL METER> is a <PROCESS VARIABLE METER> for the measurement of sound level with a standard frequency weighting and a standard exponential time weighting",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPEED METER",null,null,null,null,null,"rdl:RDS883124",null,"A <SPEED METER> is a <MEASURING INSTRUMENT> that is intended to measure the upload and download speed of a internet connection",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TACHOMETER",null,null,null,null,null,"rdl:RDS884834",null,"A <TACHOMETER> is a <PROCESS MEASURING INSTRUMENT> that is intended to measure and indicate and/or produce a signal which represents the measured speed of rotation",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TOTAL PRESSURE INSTRUMENT",null,null,null,null,null,"rdl:RDS5770755",null,"A <TOTAL PRESSURE INSTRUMENT> is a <PROCESS MEASURING INSTRUMENT> that is intended for activating and read pneumatic piezometers, total pressure cells and settlement cells",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VIBRATION METER",null,null,null,null,null,"rdl:RDS883664",null,"A <VIBRATION METER> is a <PROCESS MEASURING INSTRUMENT> for vibration measurements (frequency and amplitude), consisting of an instrument part and a vibration probe",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WEIGHT INDICATOR",null,null,null,null,null,"rdl:RDS317609",null,"A <WEIGHT INDICATOR> is a <PROCESS VARIABLE INDICATOR> using a <WEIGHT MEASURING ELEMENT> that displays the weight of materials or products",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","WEIGHT INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WEIGHT LOAD INDICATOR",null,null,null,null,null,"rdl:RDS1325747151",null,"A <WEIGHT LOAD INDICATOR> is an <ARTEFACT> and a <WEIGHT INDICATOR> that displays the weight of materials or products being lifted",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDICATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"SHADOW COLUMN INSTRUMENT",null,null,null,null,null,"rdl:RDS933659",null,"A <SHADOW COLUMN INSTRUMENT> is an <INSTRUMENTATION ITEM> and an <INDICATOR> in which the indications are given by a shadow column on an illuminated scale which can be a part of the instrument or may be separate from it",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDICATOR","INSTRUMENTATION ITEM","STANDARD SIGNAL RECEIVER",null,null,null,null,null,null,null,null,null,null,null,"STANDARD SIGNAL INDICATOR",null,null,null,null,null,"rdl:RDS222468",null,"A <STANDARD SIGNAL INDICATOR> is an <INSTRUMENTATION ITEM> and a <INDICATOR> and a <STANDARD SIGNAL RECEIVER> that gives an indication that is proportional with a standard input signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE INDICATOR",null,null,null,null,null,"rdl:RDS268289",null,"A <TEMPERATURE INDICATOR> IS AN <INDICATOR> that measures temperature"]
[null,null,"TEMPERATURE INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BIMETALLIC TEMPERATURE INDICATOR",null,null,null,null,null,"rdl:RDS5771099",null,"A <BIMETALLIC TEMPERATURE INDICATOR> is a <TEMPERATURE INDICATOR> that is powered and uses a bimetallic temperature element as the primary element"]
[null,null,"TEMPERATURE INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIGITAL TEMPERATURE INDICATOR",null,null,null,null,null,"rdl:RDS7349490",null,"A <DIGITAL TEMPERATURE INDICATOR> is a <TEMPERATURE INDICATOR> that is powered and is displaying the temperature in a digital way"]
[null,null,"TEMPERATURE INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESISTANCE TEMPERATURE INDICATOR",null,null,null,null,null,"rdl:RDS5771144",null,"A <RESISTANCE TEMPERATURE INDICATOR> is a <TEMPERATURE INDICATOR> that is powered and uses a resistance element as sensor"]
[null,null,"TEMPERATURE INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SQUARE ROOT TEMPERATURE INDICATOR",null,null,null,null,null,"rdl:RDS7349704",null,"A <SQUARE ROOT TEMPERATURE INDICATOR> is a <TEMPERATURE INDICATOR> with square root function ???????? that is loop powered"]
[null,null,"INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"TIME INDICATOR",null,null,null,null,null,"rdl:RDS17602760",null,"A <TIME INDICATOR> is a <INDICATOR> that indicates time",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","TIME INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"CLOCK",null,null,null,null,null,"rdl:RDS6588455",null,"A <CLOCK> is an <INSTRUMENTATION ITEM> and a <TIME INDICATOR> for the measurement and indication of time",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","TIME INDICATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"TIMER",null,null,null,null,null,"rdl:RDS5768480",null,"A <TIMER> is an <INSTRUMENTATION ITEM> and a <TIME INDICATOR> that measures a time interval and signals its end; a time switch",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","TIMER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC TIMER",null,null,null,null,null,"rdl:RDS6590405",null,"An <ELECTRIC TIMER> is a <TIMER> and an <ELECTRICAL APPARATUS> that is electrically powered/",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION FUNCTION","SIGNAL CIRCUIT","SYSTEM",null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP",null,null,null,null,null,"rdl:RDS222493",null,"An <INSTRUMENT LOOP> is an <INSTRUMENTATION FUNCTION> and a <SIGNAL CIRCUIT> and a <SYSTEM> that has two or more interlinked <INSTRUMENTATION FUNCTION>s",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC INSTRUMENT LOOP",null,null,null,null,null,"rdl:RDS2223298",null,"An <ELECTRONIC INSTRUMENT LOOP> is an <INSTRUMENTATION ITEM> and an <INSTRUMENT LOOP> composed of two or more <CURRENT SIGNAL LOOP ELEMENT>s",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR ANALYSIS",null,null,null,null,null,"rdl:RDS2221126",null,"An <INSTRUMENT LOOP FOR ANALYSIS> is an <INSTRUMENT LOOP> for <ANALYSIS>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR DISPLACEMENT",null,null,null,null,null,"rdl:RDS2229101",null,"An <INSTRUMENT LOOP FOR DISPLACEMENT> is an <INSTRUMENT LOOP> for <DISPLACEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR DUST DETECTION",null,null,null,null,null,"rdl:RDS2229102",null,"An <INSTRUMENT LOOP FOR DUST DETECTION> is an <INSTRUMENT LOOP> for <DUST DETECTION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR ELECTRICAL VARIABLE",null,null,null,null,null,"rdl:RDS2229103",null,"An <INSTRUMENT LOOP FOR ELECTRICAL VARIABLE> is an <INSTRUMENT LOOP> for <ELECTRICAL VARIABLE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR EROSION DETECTION",null,null,null,null,null,"rdl:RDS2229104",null,"An <INSTRUMENT LOOP FOR EROSION DETECTION> is an <INSTRUMENT LOOP> for <EROSION DETECTION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR FIRE DETECTION",null,null,null,null,null,"rdl:RDS2229105",null,"An <INSTRUMENT LOOP FOR FIRE DETECTION> is an <INSTRUMENT LOOP> for <FIRE DETECTION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR FLOW RATE",null,null,null,null,null,"rdl:RDS2221122",null,"An <INSTRUMENT LOOP FOR FLOW RATE> is an <INSTRUMENT LOOP> for <FLOW RATE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR FORCE",null,null,null,null,null,"rdl:RDS2229106",null,"An <INSTRUMENT LOOP FOR FORCE> is an <INSTRUMENT LOOP> for <FORCE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR GAS DETECTION",null,null,null,null,null,"rdl:RDS2229107",null,"An <INSTRUMENT LOOP FOR GAS DETECTION> is an <INSTRUMENT LOOP> for <GAS DETECTION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR LEAK DETECTION",null,null,null,null,null,"rdl:RDS2229108",null,"An <INSTRUMENT LOOP FOR LEAK DETECTION> is an <INSTRUMENT LOOP> for <LEAK DETECTION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR LEVEL",null,null,null,null,null,"rdl:RDS2221123",null,"An <INSTRUMENT LOOP FOR LEVEL> is an <INSTRUMENT LOOP> for liquid <LEVEL>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR MIST DETECTION",null,null,null,null,null,"rdl:RDS2229109",null,"An <INSTRUMENT LOOP FOR MIST DETECTION> is an <INSTRUMENT LOOP> for <MIST DETECTION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR POSITION",null,null,null,null,null,"rdl:RDS2229110",null,"An <INSTRUMENT LOOP FOR POSITION> is an <INSTRUMENT LOOP> for <POSITION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR PRESSURE",null,null,null,null,null,"rdl:RDS2221124",null,"An <INSTRUMENT LOOP FOR PRESSURE> is an <INSTRUMENT LOOP> for <PRESSURE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR PROXIMITY",null,null,null,null,null,"rdl:RDS2229111",null,"An <INSTRUMENT LOOP FOR PROXIMITY> is an <INSTRUMENT LOOP> for <PROXIMITY>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR RADIATION",null,null,null,null,null,"rdl:RDS2229112",null,"An <INSTRUMENT LOOP FOR RADIATION> is an <INSTRUMENT LOOP> for <RADIATION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR SAND DETECTION",null,null,null,null,null,"rdl:RDS2229113",null,"An <INSTRUMENT LOOP FOR SAND DETECTION> is an <INSTRUMENT LOOP> for <SAND DETECTION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR SPEED",null,null,null,null,null,"rdl:RDS2229114",null,"An <INSTRUMENT LOOP FOR SPEED> is an <INSTRUMENT LOOP> for <SPEED>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR TEMPERATURE",null,null,null,null,null,"rdl:RDS2221125",null,"An <INSTRUMENT LOOP FOR TEMPERATURE> is an <INSTRUMENT LOOP> for <TEMPERATURE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR WATER DETECTION",null,null,null,null,null,"rdl:RDS2229117",null,"An <INSTRUMENT LOOP FOR WATER DETECTION> is an <INSTRUMENT LOOP> for detection of presence of water",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR WEIGHT",null,null,null,null,null,"rdl:RDS2229118",null,"An <INSTRUMENT LOOP FOR WEIGHT> is an <INSTRUMENT LOOP> for <WEIGHT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP FOR ANTI SURGE PROTECTION",null,null,null,null,null,"rdl:RDS2220946",null,"An <INSTRUMENT LOOP FOR ANTI SURGE> is an <INSTRUMENT LOOP> for <ANTI SURGE PROTECTION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC INSTRUMENT LOOP",null,null,null,null,null,"rdl:RDS2224303",null,"A <PNEUMATIC INSTRUMENT LOOP> is an <INSTRUMENTATION ITEM> and an <INSTRUMENT LOOP> composed of two or more <PNEUMATIC SIGNAL LOOP ELEMENT>s",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION FUNCTION","SIGNAL CIRCUIT ELEMENT",null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT LOOP ELEMENT",null,null,null,null,null,"rdl:RDS222220",null,"An <INSTRUMENT LOOP ELEMENT> is a <INSTRUMENTATION FUNCTION> and a <SIGNAL CIRCUIT ELEMENT> capable of operating as a part in an <INSTRUMENT LOOP>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENT LOOP ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"3-15 PSIG SIGNAL LOOP ELEMENT",null,null,null,null,null,"rdl:RDS2224302",null,"A <3-15 PSIG SIGNAL LOOP ELEMENT> is an <INSTRUMENTATION ITEM> and an <INSTRUMENT LOOP ELEMENT> that can be installed in a <PNEUMATIC INSTRUMENT LOOP SYSTEM>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL ELEMENT","INSTRUMENT LOOP ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT SIGNAL LOOP ELEMENT",null,null,null,null,null,"rdl:RDS2221029",null,"A <CURRENT SIGNAL LOOP ELEMENT> is an <INSTRUMENT LOOP ELEMENT> and an <ELECTRICAL ELEMENT> that has the capability of <PARTAKING> in an <ANALOG CURRENT LOOP>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"CURRENT SIGNAL LOOP ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"10-50 mA SIGNAL LOOP ELEMENT",null,null,null,null,null,"rdl:RDS1422806811",null,"A <10-50 mA SIGNAL LOOP ELEMENT> is an <INSTRUMENTATION ITEM> and a <CURRENT SIGNAL LOOP ELEMENT> that can be installed in a <10-50 mA SIGNAL LOOP>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT SIGNAL LOOP ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"4-20 mA SIGNAL LOOP ELEMENT",null,null,null,null,null,"rdl:RDS1422805611",null,"A <4-20 mA SIGNAL LOOP ELEMENT> is an <INSTRUMENTATION ITEM> and a <CURRENT SIGNAL LOOP ELEMENT> that can be installed in a <4-20 mA SIGNAL LOOP>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","INSTRUMENTATION FUNCTION",null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENTATION ITEM",null,null,null,null,null,"rdl:RDS2220012",null,"A <INSTRUMENTATION ITEM> is an <ARTEFACT> and a <INSTRUMENTATION FUNCTION>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE GAUGE",null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUTE PRESSURE GAUGE",null,null,null,null,null,"rdl:RDS850122",null,"An <ABSOLUTE PRESSURE GAUGE> is an <INSTRUMENTATION ITEM> and a <PRESSURE GAUGE> using a <ABSOLUTE PRESSURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUTE PRESSURE MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS222588",null,"An <ABSOLUTE PRESSURE MEASURING ELEMENT> is an <INSTRUMENTATION ITEM> and a <PRESSURE MEASURING ELEMENT> for the measurement of <ABSOLUTE PRESSURE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ABSOLUTE PRESSURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUTE PRESSURE MEASURING ELEMENT - DIAPHRAGM",null,null,null,null,null,"rdl:RDS222589",null,"An <ABSOLUTE PRESSURE MEASURING ELEMENT - DIAPHRAGM> is an <ABSOLUTE PRESSURE MEASURING ELEMENT> that is a diaphragm with a reference chamber on the side of that diaphragm that not subject to pressure. In that reference chamber an absolute vacuum is given as reference pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROXIMITY MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"ACOUSTIC PROXIMITY PROBE",null,null,null,null,null,"rdl:RDS1466004581",null,"An <ACOUSTIC PROXIMITY PROBE> is an <INSTRUMENTATION ITEM> and a <PROXIMITY MEASURING ELEMENT> where acoustic signals are sent out, with the time of echo return being a measure of distance to an obstacle",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SAND DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,"ACOUSTIC SAND DETECTOR",null,null,null,null,null,"rdl:RDS16757717",null,"An <ACOUSTIC SAND DETECTOR> is an <INSTRUMENTATION ITEM> and a <SAND DETECTOR> using acoustic signalling",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"AIR PRESSURE REGULATOR",null,null,null,null,null,"rdl:RDS5794822",null,"An <AIR PRESSURE REGULATOR> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that is intended to control the air supply pressure to a consumer and keeping it invariable independent of the air consumption",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"AIR PRESSURE REGULATOR AND FILTER",null,null,null,null,null,"rdl:RDS5794965",null,"An <AIR PRESSURE REGULATOR AND FILTER> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that is an assembly of an air pressure regulator and an air filter",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","STATE WARNER",null,null,null,null,null,null,null,null,null,null,null,null,"ALARM",null,null,null,null,null,"rdl:RDS13611830",null,"An <ALARM> is an <INSTRUMENTATION ITEM> and a <STATE WARNER> that is an audible or visual signal indicating that a failure condition has occured",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALARM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANNUNCIATOR",null,null,null,null,null,"rdl:RDS13611605",null,"An <ANNUNCIATOR> is an <ALARM> that is an electronically controlled device that signals or sounds an alarm when conditions deviate from normal or from predetermined levels of pressure, heat, or speed in a process or in operating equipment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALARM","SOUNDER",null,null,null,null,null,null,null,null,null,null,null,null,null,"AUDIBLE ALARM",null,null,null,null,null,"rdl:RDS13611560",null,"An <AUDIBLE ALARM> is an <ALARM> and a <SOUNDER>, giving audible signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALARM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BURST ALARM UNIT",null,null,null,null,null,"rdl:RDS8373148",null,"A <BURST ALARM UNIT> is an <ALARM> intended for use with a rupture disc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALARM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CO2 PREDISCHARGE ALARM",null,null,null,null,null,"rdl:RDS296954",null,"A <CO2 PREDISCHARGE ALARM> is an <ALARM> which is activated prior to discharge of CO2 into an area",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALARM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HALON CO2 ALARM HORN",null,null,null,null,null,"rdl:RDS303749",null,"A <HALON CO2 ALARM HORN> is an <ALARM> which is a horn which is actvated when halon or CO2 is released in an area/room",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALARM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MANUAL FIRE ALARM",null,null,null,null,null,"rdl:RDS306134",null,"A <MANUAL FIRE ALARM> is an <ALARM> that is a fire alarm that is activated manually",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALARM","LAMP",null,null,null,null,null,null,null,null,null,null,null,null,null,"WARNING LAMP",null,null,null,null,null,"rdl:RDS314774",null,"A <WARNING LAMP> is an <ALARM> and a <LAMP> that is activated when something abnormal occurs in a system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC VARIABLE METER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"AMPEREMETER",null,null,null,null,null,"rdl:RDS870569",null,"An <AMPEREMETER> is an <INSTRUMENTATION ITEM> and an <ELECTRIC VARIABLE METER> that is intended to measure the value of an electric current",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"AMPEREMETER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"DYNAMOMETER AMMETER",null,null,null,null,null,"rdl:RDS7924183",null,"A <DYNAMOMETER AMMETER> is an <INSTRUMENTATION ITEM> and an <AMPEREMETER> operating according to the dynamometric principle",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AMPEREMETER","INSTRUMENTATION ITEM","INTEGRATING METER",null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRATING AMPEREMETER",null,null,null,null,null,"rdl:RDS871154",null,"An <INTEGRATING AMPEREMETER> is an <INSTRUMENTATION ITEM> and an <AMPEREMETER> and an <INTEGRATING METER> that is measuring the time integral of ampere",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"ANALOGUE TO DIGITAL SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS851354",null,"An <ANALOGUE TO DIGITALL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert an analogue input signal into a digital output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ASTATIC","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"ASTATIC INSTRUMENT",null,null,null,null,null,"rdl:RDS916604",null,"An <ASTATIC INSTRUMENT> is an <INSTRUMENTATION ITEM> having an <ASTATIC> (Status)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISPLACEMENT MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"AXIAL DISPLACEMENT PROBE",null,null,null,null,null,"rdl:RDS6500874",null,"An <AXIAL DISPLACEMENT PROBE> is an <INSTRUMENTATION ITEM> and a <DISPLACEMENT MEASURING ELEMENT> for measurement of <AXIAL DISPLACEMENT>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","POSITION DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,"AXIAL POSITION DETECTOR",null,null,null,null,null,"rdl:RDS14216032",null,"An <AXIAL POSITION DETECTOR> is an <INSTRUMENTATION ITEM> and a <POSITION DETECTOR> intended to detect a displacement in the axial direction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AXIAL POSITION DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CENTRIFUGAL COMPRESSOR AXIAL POSITION DETECTOR",null,null,null,null,null,"rdl:RDS14216077",null,"A <CENTRIFUGAL COMPRESSOR AXIAL POSITION DETECTOR> is an <AXIAL POSITION DETECTOR> that is intended used on a centrifugal compressor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"BACK PRESSURE REGULATOR",null,null,null,null,null,"rdl:RDS1011194",null,"A <BACK PRESSURE REGULATOR> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that uses the up-stream pressure to control the valve trim position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","TEMPERATURE DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,"BEARING TEMPERATURE DETECTOR",null,null,null,null,null,"rdl:RDS327779",null,"A <BEARING TEMPERATURE DETECTOR> is an <INSTRUMENTATION ITEM> and a <TEMPERATURE DETECTOR> that is designed to detect the temperature in a bearing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLAME DETECTOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"BURNER FLAME DETECTOR",null,null,null,null,null,"rdl:RDS1336292351",null,"A <BURNER FLAME DETECTOR> is an <INSTRUMENTATION ITEM> and a <FLAME DETECTOR> that is designed to detect the presence of a burner flame",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MOISTURE SENSING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"CAPACITANCE MOISTURE SENSOR",null,null,null,null,null,"rdl:RDS11468322",null,"A <CAPACITANCE MOISTURE SENSOR> is a <MOISTURE SENSING ELEMENT> intended to determine moisture based on the capacitance principle",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","WEIGHT MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"CAPACITIVE LOAD CELL",null,null,null,null,null,"rdl:RDS222600",null,"A <CAPACITIVE LOAD CELL> is an <INSTRUMENTATION ITEM> and a <WEIGHT MEASURING ELEMENT where the capacitance of a capacitor changes as the load presses the two plates of a capacitor closer together",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROXIMITY MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"CAPACITIVE PROXIMITY PROBE",null,null,null,null,null,"rdl:RDS11479520",null,"A <CAPACITIVE PROXIMITY PROBE> is an <INSTRUMENTATION ITEM> and a <PROXIMITY MEASURING ELEMENT> in which when power is applied to the sensor, an electrostatic field is generated and reacts to changes in capacitance caused by the presence of a target",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS ANALYSER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"CATALYTIC ANALYSER",null,null,null,null,null,"rdl:RDS1066499",null,"A <CATALYTIC ANALYSER>is an <INSTRUMENTATION ITEM> and a <GAS ANALYSER> that is using catalytic combustion of gases in air or oxygen",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","VIBRATION DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,"CENTRIFUGAL COMPRESSOR VIBRATION DETECTOR",null,null,null,null,null,"rdl:RDS14216122",null,"A <CENTRIFUGAL COMPRESSOR VIBRATION DETECTOR> is an <INSTRUMENTATION ITEM> and a <VIBRATION DETECTOR> for a centrifugal compressor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CENTRIFUGAL COMPRESSOR VIBRATION DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CENTRIFUGAL COMPRESSOR VIBRATION OSCILLATOR-DETECTOR",null,null,null,null,null,"rdl:RDS14216167",null,"A <CENTRIFUGAL COMPRESSOR VIBRATION OSCILLATOR-DETECTOR> is a <CENTRIFUGAL COMPRESSOR VIBRATION DETECTOR> of oscillating type for a centrifugal compressor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"CHART RECORDER",null,null,null,null,null,"rdl:RDS6588185",null,"A <CHART RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> that is <RECORDING> on a chart",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHART RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STRIP CHART RECORDER",null,null,null,null,null,"rdl:RDS915929",null,"A <STRIP CHART RECORDER> is an <CHART RECORDER> in which the chart is a strip driven by the chart driving mechanism",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","POSITION DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,"CHOKE VALVE POSITION DETECTOR",null,null,null,null,null,"rdl:RDS16758040",null,"A <CHOKE VALVE POSITION DETECTOR> is an <INSTRUMENTATION ITEM> and a <POSITION DETECTOR> designed to measure a position of a <CHOKE VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPASS",null,null,null,null,null,"rdl:RDS13611245",null,"A <COMPASS> is an <INSTRUMENTATION ITEM> and a <DIRECTING DEVICE> that indicates either a) magnetic bearings by alignment of its needle on the magnetic poles, or b) reference bearing by radio signal, or c) change of orientation in relation to a gyromaintained line",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COMPASS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GYROCOMPASS",null,null,null,null,null,"rdl:RDS13621304",null,"A <GYROCOMPASS> is a <COMPASS> consisting of a driven high speed wheel, specially mounted, so that its axis remains parallel to that of the earth",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COMPASS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAGNETIC COMPASS",null,null,null,null,null,"rdl:RDS13621180",null,"A <MAGNETIC COMPASS> is a <COMPASS> consisting of a magnetized needle turning freely on a pivot, used for determing magnetic bearings by alignment of its needle to the magnetic poles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COMPASS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIO COMPASS",null,null,null,null,null,"rdl:RDS13621242",null,"A <RADIO COMPASS> is a <COMPASS> that use signals from radio beacons for determining a bearing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DEW POINT ANALYSER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"CONDENSATION DEW POINT ANALYSER",null,null,null,null,null,"rdl:RDS1007909",null,"A <CONDENSATION DEW POINT ANALYSER> is an <INSTRUMENTATION ITEM> and a <DEW POINT ANALYSER> that detects the first appearance of condense to determine a dew point",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONDUCTIVITY CELL","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"CONDUCTIVITY CELL - CONTACTING",null,null,null,null,null,"rdl:RDS222502",null,"A <CONDUCTIVITY CELL - CONTACTING> is an <INSTRUMENTATION ITEM> and a <CONDUCTIVITY CELL> that consist of two metal electrodes, usually stainless steel or titanium, in contact with the electrolyte solution",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"CONSTANT VOLUME REGULATOR",null,null,null,null,null,"rdl:RDS297494",null,"A <CONSTANT VOLUME REGULATOR> is an <ARTEFACT> and a <REGULATOR> ensuring constant volume in a HVAC system to reduce noise",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"CONTINUOUS LINE RECORDER",null,null,null,null,null,"rdl:RDS916424",null,"A <CONTINUOUS LINE RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> that is capable of recording slowly changing measured signals/quantities",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT TO CURRENT SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS5762894",null,"A <CURRENT TO CURRENTL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a current input signal to a current output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT TO PRESSURE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS460484",null,"A <CURRENT TO PRESSUREL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a current input signal to a proportional linear pneumatic output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT TO VOLTAGE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS851219",null,"A <CURRENT TO VOLTAGEL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a current input signal to a proportional voltage output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","TRANSDUCER",null,null,null,null,null,null,null,null,null,null,null,null,"DIAPHRAGM SEAL",null,null,null,null,null,"rdl:RDS298079",null,"A <DIAPHRAGM SEAL> is an <INSTRUMENTATION ITEM> and a <TRANSDUCER> that provides a <BARRIER> between two substance using an impenetrable membrane or <DIAPHRAGM>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FORCE MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL FORCE SENSOR",null,null,null,null,null,"rdl:RDS1337128971",null,"A <DIFFERENTIAL FORCE SENSOR> is an <INSTRUMENTATION ITEM> and a <FORCE MEASURING ELEMENT> that is sensing a difference in force and produces a corresponding output",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE GAUGE",null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL PRESSURE GAUGE",null,null,null,null,null,"rdl:RDS850814",null,"A <DIFFERENTIAL PRESSURE GAUGE> is an <INSTRUMENTATION ITEM> and a <PRESSURE GAUGE> using a <DIFFERENTIAL PRESSURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL PRESSURE REGULATOR",null,null,null,null,null,"rdl:RDS879344",null,"A <DIFFERENTIAL PRESSURE REGULATOR> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that uses the differential pressure to control the valve trim and regulate the pressure in a process system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL PRESSURE MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS5770524",null,"A <DIFFERENTIAL PRESSURE MEASURING ELEMENT> is an <INSTRUMENTATION ITEM> and a <PRESSURE MEASURING ELEMENT> for the measurement of <DIFFERENTIAL PRESSURE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIFFERENTIAL PRESSURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL PRESSURE MEASURING ELEMENT - BELLOWS",null,null,null,null,null,"rdl:RDS222591",null,"A <DIFFERENTIAL PRESSURE MEASURING ELEMENT - BELLOWS> is a <DIFFERENTIAL PRESSURE MEASURING ELEMENT> that is a bellows. The pressure of the media acts on both sides of this bellows upon which it moves, and this movement is a measurement for the pressure difference",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIFFERENTIAL PRESSURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL PRESSURE MEASURING ELEMENT - DIAPHRAGM",null,null,null,null,null,"rdl:RDS222590",null,"A <DIFFERENTIAL PRESSURE MEASURING ELEMENT - DIAPHRAGM> is a <DIFFERENTIAL PRESSURE MEASURING ELEMENT> where two sealed media chambers are separated by a diaphragm. The deflection caused in this way is used as a measurement for the pressure difference",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"DIGITAL TO ANALOGUE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS851399",null,"A <DIGITAL TO ANALOGUEL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a digital input signal into an analogue output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"DIRECT OPERATED PRESSURE REGULATOR",null,null,null,null,null,"rdl:RDS879524",null,"A <DIRECT OPERATED PRESSURE REGULATOR> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that is using direct feed back of the outlet pressure to correct the valve trim position and maintain a constant outlet pressure independent of the flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"DISC RECORDER",null,null,null,null,null,"rdl:RDS916064",null,"A <DISC RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> that records data on a rotating recordable disc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS ANALYSER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"DISPERSIVE INFRA-RED GAS ANALYSER",null,null,null,null,null,"rdl:RDS1066634",null,"A <DISPERSIVE INFRA-RED GAS ANALYSER>is an <INSTRUMENTATION ITEM> and a <GAS ANALYSER> in which the absorption of a specific wavelength or <IR> radiation is measured by dispersing the <IR> radiation from a source through a prism, grating, or filter before passing it through the gas, and detecting this radiation by a broad band sensor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"DRUM RECORDER",null,null,null,null,null,"rdl:RDS915974",null,"A <DRUM RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> in which the chart is wrapped as a single turn around a cylindrical drum which is rotated by the chart driving mechanism",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","VOLTMETER",null,null,null,null,null,null,null,null,null,null,null,null,"DYNAMOMETER VOLTMETER",null,null,null,null,null,"rdl:RDS7924279",null,"A <DYNAMOMETER VOLTMETER> is an <INSTRUMENTATION ITEM> and a <VOLTMETER> operating on the dynamometric principle",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","WATTMETER",null,null,null,null,null,null,null,null,null,null,null,null,"DYNAMOMETER WATTMETER",null,null,null,null,null,"rdl:RDS7924377",null,"A <DYNAMOMETER WATTMETER> is an <INSTRUMENTATION ITEM> and a <WATTMETER> operating on the dynamometric principle",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","OHMMETER",null,null,null,null,null,null,null,null,null,null,null,null,"EARTH RESISTANCE METER",null,null,null,null,null,"rdl:RDS915344",null,"An <EARTH RESISTANCE METER> is an <INSTRUMENTATION ITEM> and an <OHMMETER> intended to measure the resistance of an earth connection",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL TO OPTICAL SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS1066703201",null,"An <ELECTRICAL TO OPTICALL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that converts an electrical input signal to an optical output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","INSTRUMENTATION ITEM","TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL TRANSMITTER",null,null,null,null,null,"rdl:RDS1455527751",null,"An <ELECTRICAL TRANSMITTER> is an <INSTRUMENTATION ITEM> and a <TRANSMITTER> and an <ELECTRICAL APPARATUS>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","WATT-HOUR METER",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRODYNAMIC METER",null,null,null,null,null,"rdl:RDS932444",null,"An <ELECTRODYNAMIC METER> is an <INSTRUMENTATION ITEM> and a <WATT-HOUR METER> that operates by the rotation of the moving coil of an electrodynamic measuring element",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","VOLTMETER",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTROSCOPE",null,null,null,null,null,"rdl:RDS918044",null,"An <ELECTROSCOPE> is an <INSTRUMENTATION ITEM> and a <VOLTMETER> for ascertaining the presence of electricity, and its quantity if present",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","VOLTMETER",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTROSTATIC INSTRUMENT",null,null,null,null,null,"rdl:RDS915839",null,"An <ELECTROSTATIC INSTRUMENT> is an <INSTRUMENTATION ITEM> and a <VOLTMETER> intended to determine potential difference which operates by means of electrostatic forces between fixed and moveable charged electrodes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","INSTRUMENTATION SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,"EMERGENCY SHUT DOWN SYSTEM",null,null,null,null,null,"rdl:RDS276929",null,"An <EMERGENCY SHUT DOWN SYSTEM> is an <INSTRUMENTATION ITEM> and an <INSTRUMENTATION SYSTEM> that gives the possibility of bringing the whole plant or part of it with one or few manipulations into a safe pre-determined position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","INSTRUMENTATION SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,"ENVIRONMENTAL CONTROL SYSTEM",null,null,null,null,null,"rdl:RDS276884",null,"A <ENVIRONMENTAL CONTROL SYSTEM> is an <INSTRUMENTATION ITEM> and an <INSTRUMENTATION SYSTEM> that includes monitoring of the plant environment by supervising air, water and soil conditions in accordance with the applicable regulations for pollution",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EROSION DETECTING MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"EROSION PROBE",null,null,null,null,null,"rdl:RDS5781161",null,"An <EROSION PROBE> is an <INSTRUMENTATION ITEM> and an <EROSION DETECTING MEASURING ELEMENT> that is detecting accumulated erosion directly",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"EVENT RECORDER",null,null,null,null,null,"rdl:RDS916469",null,"A <EVENT RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> that records the presence or absence of a quantity, or the state of a two-state device, as a function of time",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","WATT-HOUR METER",null,null,null,null,null,null,null,null,null,null,null,null,"EXCESS ENERGY METER",null,null,null,null,null,"rdl:RDS932534",null,"An <EXCESS ENERGY METER> is an <INSTRUMENTATION ITEM> and a <WATT-HOUR METER> intended to measure the excess energy when the power exceeds a pre-determined value",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"FLOAT CHAMBER",null,null,null,null,null,"rdl:RDS5782529",null,"A <FLOAT CHAMBER> is an <INSTRUMENTATION ITEM> and a <LEVEL REGULATOR> which is a device for automatically regulating the supply of a liquid to a system using a valve operated by a float inside a chamber",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOAT CHAMBER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRAP",null,null,null,null,null,"rdl:RDS7455439",null,"A <TRAP> is a <FLOAT CHAMBER> for collection and discharge of unwanted condensate from an air-, gas- or steam-flow in pipes, jackets or reservoirs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRAP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR RELEASE TRAP",null,null,null,null,null,"rdl:RDS294839",null,"An <AIR RELEASE TRAP> is a <TRAP> that is accumulating unwanted air in a closed system and release it",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRAP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR TRAP",null,null,null,null,null,"rdl:RDS648809",null,"An <AIR TRAP> is a <TRAP> which, by a water seal, prevents foul air from rising from sinks, wash basins, drains, sewers etc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRAP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STEAM TRAP",null,null,null,null,null,"rdl:RDS5782388",null,"A <STEAM TRAP> is a <TRAP> that consists of a chamber into which condensed steam from steam pipes etc. is allowed to drain, and which automatically ejects it without permitting the escape of steam",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"FLOAT VALVE",null,null,null,null,null,"rdl:RDS553184",null,"A <FLOAT VALVE> is an <INSTRUMENTATION ITEM> and a <LEVEL REGULATOR> that usually is operated by a float mechanism to regulate or maintain a liquid level in a tank",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOAT VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR RELEASE VALVE",null,null,null,null,null,"rdl:RDS7027945",null,"An <AIR RELEASE VALVE> is a <FLOAT VALVE> that is made for gas or vapour release from a liquid system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOAT VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOAT VALVE (INTERNAL)",null,null,null,null,null,"rdl:RDS11142265",null,"A <FLOAT VALVE (INTERNAL)> is a <FLOAT VALVE> that is operated by an internal float mechanism",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LIMITER",null,null,null,null,null,null,null,null,null,null,null,null,"FLOW LIMITER",null,null,null,null,null,"rdl:RDS1011329",null,"A <FLOW LIMITER> is an <INSTRUMENTATION ITEM> and a <LIMITER> that normally use the differential pressure across an orifice to control a valve trim and limit the flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FORCE MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"FORCE SENSOR",null,null,null,null,null,"rdl:RDS222546",null,"A <FORCE SENSOR> is an <INSTRUMENTATION ITEM> and a <FORCE MEASURING ELEMENT that is a piezoresistive force sensor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FORCE SENSOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STRAIN GAUGE LOAD CELL",null,null,null,null,null,"rdl:RDS5770253",null,"A <STRAIN GAUGE LOAD CELL> is a <FORCE SENSOR> that measures the deformation (strain) as a change in electrical resistance, which is a measure of the strain and hence the applied forces",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"FREQUENCY TO CURRENT SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS1011104",null,"A <FREQUENCY TO CURRENTL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a frequency or rotational speed input signal into a current output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"FREQUENCY TO VOLTAGE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS1011149",null,"A <FREQUENCY TO VOLTAGEL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a frequency or rotational speed input signal into a voltage output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"GALVANOMETER",null,null,null,null,null,"rdl:RDS915029",null,"A <GALVANOMETER> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> for detecting the existence and determining the direction and intensity of a galvanic current (direct current)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GALVANOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BALLISTIC GALVANOMETER",null,null,null,null,null,"rdl:RDS932219",null,"A <BALLISTIC GALVANOMETER> is a <GALVANOMETER> intended to measure the value of an electric energy by reading the amplitude of the first swing of its moving element",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GALVANOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENCE GALVANOMETER",null,null,null,null,null,"rdl:RDS932309",null,"A <DIFFERENCE GALVANOMETER> is a <GALVANOMETER> intended to measure the difference between two currents",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GALVANOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOVING-COIL GALVANOMETER",null,null,null,null,null,"rdl:RDS932174",null,"A <MOVING-COIL GALVANOMETER> is a <GALVANOMETER> in which a coil carrying a current moves in the field of a permanent magnet",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GALVANOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STRING GALVANOMETER",null,null,null,null,null,"rdl:RDS932264",null,"A <STRING GALVANOMETER> is a <GALVANOMETER> in which the moving element is a conductive thread which is able to move between the pole pieces of a permanent magnet or of an electromagnet",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GALVANOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VIBRATION GALVANOMETER",null,null,null,null,null,"rdl:RDS932354",null,"A <VIBRATION GALVANOMETER> is a <GALVANOMETER> in which the natural frequency of the moving element is adjusted to resonate with the frequency of the current to be measured or detected",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RADIATION MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"GAMMA DETECTING MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS880199",null,"A <GAMMA DETECTING MEASURING ELEMENT> is an <INSTRUMENTATION ITEM> and a <RADIATION MEASURING ELEMENT> for measurement of the level of gamma radiation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHROMATOGRAPH","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"GAS CHROMATOGRAPH",null,null,null,null,null,"rdl:RDS1007639",null,"A <GAS CHROMATOGRAPH> is an <INSTRUMENTATION ITEM> and a <CHROMATOGRAPH> where gas is injected directly into one or more separation columns",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS CHROMATOGRAPH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ON-LINE PROCESS GAS CHROMATOGRAPH",null,null,null,null,null,"rdl:RDS1066724",null,"An <ON-LINE PROCESS GAS CHROMATOGRAPH> is a <GAS CHROMATOGRAPH> that is able to measure the concentration of one or several components of a chemical mixture repetitively, by regularly sampling the process mixture and transmitting the resulting information for control purposes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DENSITY ANALYSER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"GAS DENSITY ANALYSER",null,null,null,null,null,"rdl:RDS1007819",null,"A <GAS DENSITY ANALYSER> is an <INSTRUMENTATION ITEM> and a <DENSITY ANALYSER> that is intended for analysing the density of gas and vapour",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS DETECTING MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"GAS DETECTING MEASURING ELEMENT - ELECTROCHEMICAL",null,null,null,null,null,"rdl:RDS222547",null,"A <GAS DETECTING MEASURING ELEMENT - ELECTROCHEMICAL> is an <INSTRUMENTATION ITEM> and a <GAS DETECTING MEASURING ELEMENT> where gases are allowed to diffuse through a porous membrane to an electrode where it is either chemically oxidized or reduced. The amount of current produced is determined by how much of the gas is oxidized at the electrode,[3] indicating the concentration of the gas",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS DETECTING MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"GAS DETECTING MEASURING ELEMENT - HOLOGRAPHIC",null,null,null,null,null,"rdl:RDS222548",null,"A <GAS DETECTING MEASURING ELEMENT - HOLOGRAPHIC> is an <INSTRUMENTATION ITEM> and a <GAS DETECTING MEASURING ELEMENT>using light reflection to detect changes in a polymer film matrix containing a hologram. Since holograms reflect light at certain wavelengths, a change in their composition can generate a colorful reflection indicating the presence of a gas molecule",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS DETECTING MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"GAS DETECTING MEASURING ELEMENT - INFRARED IMAGING",null,null,null,null,null,"rdl:RDS222549",null,"A <GAS DETECTING MEASURING ELEMENT - INFRARED IMAGING> is an <INSTRUMENTATION ITEM> and a <GAS DETECTING MEASURING ELEMENT> that can be an active or passive system. For active sensing, IR imaging sensors typically scan a laser across the field of view of a scene and look for backscattered light at the absorption line wavelength of a specific target gas. Passive IR imaging sensors measure spectral changes at each pixel in an image and look for specific spectral signatures that indicate the presence of target gases",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS DETECTING MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"GAS DETECTING MEASURING ELEMENT - SEMICONDUCTOR",null,null,null,null,null,"rdl:RDS222550",null,"A <GAS DETECTING MEASURING ELEMENT - SEMICONDUCTOR> is an <INSTRUMENTATION ITEM> and a <GAS DETECTING MEASURING ELEMENT> using a chemical reaction that takes place, causing the electrical resistance in the sensor to be decreased when it comes in contact with the monitored gas",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS DETECTING MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"GAS DETECTING MEASURING ELEMENT - ULTRASONIC",null,null,null,null,null,"rdl:RDS222551",null,"A <GAS DETECTING MEASURING ELEMENT - ULTRASONIC> is an <INSTRUMENTATION ITEM> and a <GAS DETECTING MEASURING ELEMENT> using acoustic sensors to detect changes in the background noise of its environment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS DETECTING MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"GAS DETECTING MEASURING ELEMENT - INFRARED POINT",null,null,null,null,null,"rdl:RDS7477380",null,"A <GAS DETECTING MEASURING ELEMENT - INFRARED POINT> is an <INSTRUMENTATION ITEM> and a <GAS DETECTING MEASURING ELEMENT> using radiation passing through a known volume of gas; energy from the sensor beam is absorbed at certain wavelengths, depending on the properties of the specific gas",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHROMATOGRAPH","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"GAS LIQUID CHROMATOGRAPH",null,null,null,null,null,"rdl:RDS1007684",null,"A <GAS LIQUID CHROMATOGRAPH> is an <INSTRUMENTATION ITEM> and a <CHROMATOGRAPH> where a liquid sample is injected and evaporated and subsequently carried to one or more separation columns",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE GAUGE",null,null,null,null,null,null,null,null,null,null,null,null,"GAUGE PRESSURE GAUGE",null,null,null,null,null,"rdl:RDS416159",null,"A <GAUGE PRESSURE GAUGE> is an <INSTRUMENTATION ITEM> and a <PRESSURE GAUGE> using a <GAUGE PRESSURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"GAUGE PRESSURE MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS1322274131",null,"A <GAUGE PRESSURE MEASURING ELEMENT> is an <INSTRUMENTATION ITEM> and a <PRESSURE MEASURING ELEMENT> for the measurement of <GAUGE PRESSURE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAUGE PRESSURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIAPHRAGM SEAL ASSEMBLY",null,null,null,null,null,"rdl:RDS1469940001",null,"A <DIAPHRAGM SEAL ASSEMBLY> is a <GAUGE PRESSURE MEASURING ELEMENT> that consists of a <DIAPHRAGM SEAL> and additional parts like <CAPILLARY TUBE> required to transfer the pressure from the fluid to the process connection of the device in focus",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIAPHRAGM SEAL ASSEMBLY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TWO REMOTE SEALS DIAPHRAGM SEAL ASSEMBLY",null,null,null,null,null,"rdl:RDS1469942981",null,"A <TWO REMOTE SEALS DIAPHRAGM SEAL ASSEMBLY> is a <DIAPHRAGM SEAL ASSEMBLY> that consists of two <DIAPHRAGM SEAL>s and <CAPILLARY TUBE>s, and additional parts required for the connection",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAUGE PRESSURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAUGE PRESSURE MEASURING ELEMENT - DIAPHRAGM",null,null,null,null,null,"rdl:RDS708344",null,"A <GAUGE PRESSURE MEASURING ELEMENT - DIAPHRAGM> is a <GAUGE PRESSURE MEASURING ELEMENT> that is a circular-shaped, corrugated membrane, either clamped around the rim between two flanges or welded and subject to the pressure of the media acting on one side. The deflection caused in this way is used as a measurement for pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAUGE PRESSURE MEASURING ELEMENT - DIAPHRAGM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAUGE PRESSURE TRANSDUCER",null,null,null,null,null,"rdl:RDS222594",null,"A <GAUGE PRESSURE TRANSDUCER> is a <GAUGE PRESSURE MEASURING ELEMENT - DIAPHRAGM> where pressure applied to a pressure transducer that produces a deflection of a <DIAPHRAGM> which introduces strain to strain gages. The strain gages produce an electrical resistance change proportional to the pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAUGE PRESSURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAUGE PRESSURE MEASURING ELEMENT - BELLOWS",null,null,null,null,null,"rdl:RDS222592",null,"A <GAUGE PRESSURE MEASURING ELEMENT - BELLOWS> is a <GAUGE PRESSURE MEASURING ELEMENT> that is a bellows. The pressure of the media acts on the inside of this bellows upon which it moves, and this movement is a measurement for the pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAUGE PRESSURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAUGE PRESSURE MEASURING ELEMENT - BOURDON",null,null,null,null,null,"rdl:RDS462239",null,"A <GAUGE PRESSURE MEASURING ELEMENT - BOURDON> is a <GAUGE PRESSURE MEASURING ELEMENT> that is a radially-formed tube with an oval crosssection. The pressure of the media acts on the inside of this tube. The end of the tube which is not fixed moves, and this movement is a measurement for the pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAUGE PRESSURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAUGE PRESSURE MEASURING ELEMENT - CAPSULE",null,null,null,null,null,"rdl:RDS222593",null,"A <GAUGE PRESSURE MEASURING ELEMENT - CAPSULE> is a <GAUGE PRESSURE MEASURING ELEMENT> that is an element that comprises two circular-shaped, corrugated diaphragms, joined together around the rim with a pressure-tight seal. The pressure acts on the inside of this capsule and the generated stroke movement is indicated by means of a movement as a measurement of pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS DETECTOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"H2S DETECTOR",null,null,null,null,null,"rdl:RDS1008764",null,"An <H2S DETECTOR> is an <INSTRUMENTATION ITEM> and a <GAS DETECTOR> that is designed for detecting Hydrogen Sulfide",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"GAS DETECTOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"HC GAS INFRARED POINT DETECTOR",null,null,null,null,null,"rdl:RDS7057881",null,"An <HC GAS INFRARED POINT DETECTOR> is an <INSTRUMENTATION ITEM> and a <GAS DETECTOR> that is designed for detecting Hydrocarbon Gas",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"HEAT DETECTOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"HEAT DETECTOR FOR SURFACE MOUNTING",null,null,null,null,null,"rdl:RDS6718927",null,"A <HEAT DETECTOR FOR SURFACE MOUNTING> is an <INSTRUMENTATION ITEM> and a <HEAT DETECTOR> that is intended to be mounted onto a surface in such a way that it protrudes into the volume of which it is intended to detect heat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS DETECTOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"HF IN AIR DETECTOR",null,null,null,null,null,"rdl:RDS6599262",null,"An <HF IN AIR DETECTOR> is an <INSTRUMENTATION ITEM> and a <GAS DETECTOR> that is intended to detect the presence of hydrogen fluoride (fluoric acid) in air",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","WEIGHT MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC LOAD CELL",null,null,null,null,null,"rdl:RDS222601",null,"A <HYDRAULIC LOAD CELL> is an <INSTRUMENTATION ITEM> and a <WEIGHT MEASURING ELEMENT that is a conventional piston and cylinder arrangement",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLUID LEAK DETECTOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"HYDROCARBON LEAK DETECTOR",null,null,null,null,null,"rdl:RDS16553373",null,"A <HYDROCARBON LEAK DETECTOR> is an <INSTRUMENTATION ITEM> and a <FLUID LEAK DETECTOR> designed to detect hydrocarbons",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","WATT-HOUR METER",null,null,null,null,null,null,null,null,null,null,null,null,"INDUCTION METER",null,null,null,null,null,"rdl:RDS932489",null,"An <INDUCTION METER> is an <INSTRUMENTATION ITEM> and a <WATT-HOUR METER> that operates by the rotation of the disc of an induction measuring element",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROXIMITY MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"INDUCTIVE PROXIMITY PROBE",null,null,null,null,null,"rdl:RDS11468260",null,"An <INDUCTIVE PROXIMITY PROBE> is an <INSTRUMENTATION ITEM> and a <PROXIMITY MEASURING ELEMENT> that senses proximity based on the use of induced magnetic fields",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"INFRARED ANALYSER",null,null,null,null,null,"rdl:RDS6466119",null,"An <INFRARED ANALYSER> is an <INSTRUMENTATION ITEM> and a <PROCESS ANALYSER> that applies the principle of infrared analysis",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLAME DETECTOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"INFRARED FLAME DETECTOR",null,null,null,null,null,"rdl:RDS613214",null,"An <INFRARED FLAME DETECTOR> is an <INSTRUMENTATION ITEM> and a <FLAME DETECTOR> that is based on detection of infrared radiation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROXIMITY MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"INFRARED PROXIMITY PROBE",null,null,null,null,null,"rdl:RDS1466002331",null,"An <INFRARED PROXIMITY PROBE> is an <INSTRUMENTATION ITEM> and a <PROXIMITY MEASURING ELEMENT> that operates by sending out a beam of IR light, and then computing the distance to any nearby objects from characteristics of the returned (reflected) signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"INK JET RECORDER",null,null,null,null,null,"rdl:RDS916289",null,"A <INK JET RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> that is using an ink-jet printing head to record data on a chart",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT WITH LIMIT SWITCHES",null,null,null,null,null,"rdl:RDS953639",null,"An <INSTRUMENT WITH LIMIT SWITCHES> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> in which the moving element operates switches at certain predetermined positions or values",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT WITH LOCKING DEVICE",null,null,null,null,null,"rdl:RDS916649",null,"An <INSTRUMENT WITH LOCKING DEVICE> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> in which a device can lock the moving element in the position where it stands at a given time",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","OHMMETER",null,null,null,null,null,null,null,null,null,null,null,null,"INSULATION RESISTANCE METER",null,null,null,null,null,"rdl:RDS915389",null,"An <INSULATION RESISTANCE METER> is an <INSTRUMENTATION ITEM> and an <OHMMETER> intended to measure insulation resistance",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC VARIABLE METER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRATING METER",null,null,null,null,null,"rdl:RDS870749",null,"An <INTEGRATING METER> is an <INSTRUMENTATION ITEM> and an <ELECTRIC VARIABLE METER> that measures the time integral of the named quantity",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTEGRATING METER","POWER METER",null,null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRATING POWER METER",null,null,null,null,null,"rdl:RDS871019",null,"An <INTEGRATING POWER METER> is an <INTEGRATING METER> and a <POWER METER> that is measuring the time integral of electrical power (kWh meter)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTEGRATING METER","REACTIVE POWER METER",null,null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRATING REACTIVE POWER METER",null,null,null,null,null,"rdl:RDS871064",null,"An <INTEGRATING REACTIVE POWER METER> is an <INTEGRATING METER> and a <REACTIVE POWER METER> that is measuring the time integral of reactive electrical power",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTEGRATING METER","VOLTMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRATING VOLT METER",null,null,null,null,null,"rdl:RDS871199",null,"An <INTEGRATING VOLT METER> is an <INTEGRATING METER> and a <VOLTMETER> that is measuring the time integral of voltage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTEGRATING METER","VOLT-AMPERE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRATING VOLT-AMPERE METER",null,null,null,null,null,"rdl:RDS871109",null,"An <INTEGRATING VOLT-AMPERE METER> is an <INTEGRATING METER> and a <VOLT-AMPERE METER> that is measuring the time integral of volt-ampere",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLAME DETECTOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"IONISATION FLAME DETECTOR",null,null,null,null,null,"rdl:RDS1008674",null,"An <IONISATION FLAME DETECTOR> is an <INSTRUMENTATION ITEM> and a <FLAME DETECTOR> designed to detect a flame by measuring a degree of ionisation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SMOKE DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,"IONIZATION SMOKE DETECTOR",null,null,null,null,null,"rdl:RDS7064769",null,"An <IONIZATION SMOKE DETECTOR> is an <INSTRUMENTATION ITEM> and a <SMOKE DETECTOR> that is using an ionization chamber and a source of ionizing radiation (Americium-241) to detect smoke",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL GAUGE",null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL GAUGE GLASS",null,null,null,null,null,"rdl:RDS430199",null,"A <LEVEL GAUGE GLASS> is an <INSTRUMENTATION ITEM> and a <LEVEL GAUGE> that is a glass tubular device or vertical cylindrical device, often graduated, that indicates the level or amount of liquid in a tank or vessel",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - DISPLACER",null,null,null,null,null,"rdl:RDS222553",null,"A <LEVEL MEASURING ELEMENT - DISPLACER> is an <INSTRUMENTATION ITEM> and a <LEVEL MEASURING ELEMENT> that uses the buoyancy force from a suspended displacer that is immersed in the liquid",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - ELECTRIC PROPERTY",null,null,null,null,null,"rdl:RDS222554",null,"A <LEVEL MEASURING ELEMENT - ELECTRIC PROPERTY> is an <INSTRUMENTATION ITEM> and a <LEVEL MEASURING ELEMENT> that uses the electric properties of a process material to measure its level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - ELECTRIC PROPERTY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - CONDUCTANCE",null,null,null,null,null,"rdl:RDS222555",null,"A <LEVEL MEASURING ELEMENT - CONDUCTANCE> is a <LEVEL MEASURING ELEMENT - ELECTRIC PROPERTY> that uses a low-voltage, current-limited power source applied across separate electrodes. The power supply is matched to the conductivity of the liquid, with higher voltage versions designed to operate in less conductive (higher resistance) mediums. A conductive liquid contacting both the longest probe (common) and a shorter probe (return) completes a conductive circuit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - ELECTRIC PROPERTY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - RF ADMITTANCE",null,null,null,null,null,"rdl:RDS222559",null,"A <LEVEL MEASURING ELEMENT - RF ADMITTANCE> is a <LEVEL MEASURING ELEMENT - ELECTRIC PROPERTY> that uses a rod probe and RF source to measures the change in admittance (a measure of how easily a circuit will allow a current to flow). When the level changes around the probe, a corresponding change in the di-electric is observed. This changes the admittance of this imperfect capacitor and this change is measured to detect change of level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - ELECTRIC PROPERTY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - CAPACITANCE",null,null,null,null,null,"rdl:RDS6500394",null,"A <LEVEL MEASURING ELEMENT - CAPACITANCE> is a <LEVEL MEASURING ELEMENT - ELECTRIC PROPERTY> that senses the presence of a wide variety of solids, aqueous and organic liquids, and slurries. The technique is frequently referred to as RF for the radio frequency signals applied to the capacitance circuit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - HYDROSTATIC PRESSURE",null,null,null,null,null,"rdl:RDS222563",null,"A <LEVEL MEASURING ELEMENT - HYDROSTATIC PRESSURE> is an <INSTRUMENTATION ITEM> and a <LEVEL MEASURING ELEMENT> that is a submersible or externally mounted pressure sensor that senses increasing pressure with depth",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - HYDROSTATIC PRESSURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS222564",null,"A <LEVEL MEASURING ELEMENT - DIFFERENTIAL PRESSURE> is a <LEVEL MEASURING ELEMENT - HYDROSTATIC PRESSURE> that is measuring liquid level by sensing pressure difference between two points, e.g. the hydrostatic pressure at the bottom of a tank to the atmosphere pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - HYDROSTATIC PRESSURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - PRESSURE",null,null,null,null,null,"rdl:RDS222565",null,"A <LEVEL MEASURING ELEMENT - PRESSURE> is a <LEVEL MEASURING ELEMENT - HYDROSTATIC PRESSURE> that uses gauge pressure to measure level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - PRESSURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - AIR BUBBLER SYSTEM",null,null,null,null,null,"rdl:RDS222566",null,"A <LEVEL MEASURING ELEMENT - AIR BUBBLER SYSTEM> is a <LEVEL MEASURING ELEMENT - PRESSURE> that uses a tube with an opening below the surface of the liquid level. A fixed flow of air is passed through the tube. Pressure in the tube is proportional to the depth (and density) of the liquid over the outlet of the tube",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - PRESSURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - IMMERSION",null,null,null,null,null,"rdl:RDS222567",null,"A <LEVEL MEASURING ELEMENT - IMMERSION> is a <LEVEL MEASURING ELEMENT - PRESSURE> the sensing element of which is immersed in the liquid to be measured",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - MECHANICAL",null,null,null,null,null,"rdl:RDS222568",null,"A <LEVEL MEASURING ELEMENT - MECHANICAL> is an <INSTRUMENTATION ITEM> and a <LEVEL MEASURING ELEMENT> that uses mechanical means to measure level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - MECHANICAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - PLUMB BOB",null,null,null,null,null,"rdl:RDS222569",null,"A <LEVEL MEASURING ELEMENT - PLUMB BOB> is a <LEVEL MEASURING ELEMENT - MECHANICAL> that uses a wire or tape with a body as sensing element to measure level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - MECHANICAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - ROTATING PADDLE",null,null,null,null,null,"rdl:RDS222570",null,"A <LEVEL MEASURING ELEMENT - ROTATING PADDLE> is a <LEVEL MEASURING ELEMENT - MECHANICAL> that is an established technique for bulk solid point level indication. It uses a low-speed gear motor that rotates a paddle wheel. When the paddle is stalled by solid materials, the motor is rotated on its shaft by its own torque until a flange mounted on the motor contacts a mechanical switch",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - MECHANICAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - SERVO",null,null,null,null,null,"rdl:RDS222571",null,"A <LEVEL MEASURING ELEMENT - SERVO> is a <LEVEL MEASURING ELEMENT - MECHANICAL> that uses a float and a wire fed by a servo motor to measure level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - MECHANICAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - SINGLE PROBE VIBRATING",null,null,null,null,null,"rdl:RDS222572",null,"A <LEVEL MEASURING ELEMENT - SINGLE PROBE VIBRATING> is a <LEVEL MEASURING ELEMENT - MECHANICAL> that is for bulk powder level measurement. It is not affected by dust, static-charge build-up from dielectric powders, or changes in conductivity, temperature, pressure, humidity or moisture content. Since only one sensing element contacts the powder, bridging between two probe elements is eliminated and media build-up is minimized",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - MECHANICAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - TUNING FORK VIBRATING",null,null,null,null,null,"rdl:RDS222573",null,"A <LEVEL MEASURING ELEMENT - TUNING FORK VIBRATING> is a <LEVEL MEASURING ELEMENT - MECHANICAL> for bulk powder level measurement. It is not affected by dust, static-charge build-up from dielectric powders, or changes in conductivity, temperature, pressure, humidity or moisture content, but it is prone to material buildup between the tines",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - NUCLEAR",null,null,null,null,null,"rdl:RDS222574",null,"A <LEVEL MEASURING ELEMENT - NUCLEAR> is an <INSTRUMENTATION ITEM> and a <LEVEL MEASURING ELEMENT> that uses the absorption of gamma radiation by process material to measure level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - OPTICAL",null,null,null,null,null,"rdl:RDS222575",null,"A <LEVEL MEASURING ELEMENT - OPTICAL> is an <INSTRUMENTATION ITEM> and a <LEVEL MEASURING ELEMENT> that uses the transmission, reflection or refraction of light by the process material to measure level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - OPTICAL INFRARED",null,null,null,null,null,"rdl:RDS222576",null,"A <LEVEL MEASURING ELEMENT - OPTICAL INFRARED> is an <INSTRUMENTATION ITEM> and a <LEVEL MEASURING ELEMENT> that is used for point level sensing of sediments, liquids with suspended solids, and liquid-liquid interfaces. These sensors sense the decrease or change in transmission of infrared light emitted from an infrared diode (LED)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - OPTICAL LASER",null,null,null,null,null,"rdl:RDS222577",null,"A <LEVEL MEASURING ELEMENT - OPTICAL LASER> is an <INSTRUMENTATION ITEM> and a <LEVEL MEASURING ELEMENT> that involves the use of a laser. Laser light reflects off most solid, liquid surfaces. The time of flight can be measured with precise timing circuitry, to determine the range or distance of the surface from the sensor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - OPTICAL LASER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - OPTICAL REFRACTION",null,null,null,null,null,"rdl:RDS222578",null,"A <LEVEL MEASURING ELEMENT - OPTICAL REFRACTION> is a <LEVEL MEASURING ELEMENT - OPTICAL LASER> that uses the difference between the refractive index of the process fluid and the material of the sensing element to measure level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - WAVE",null,null,null,null,null,"rdl:RDS222579",null,"A <LEVEL MEASURING ELEMENT - WAVE> is an <INSTRUMENTATION ITEM> and a <LEVEL MEASURING ELEMENT> that measures the level by detecting either a propagation time or a damping of a propagation phenomenon of waves",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - WAVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - FREE-SPACE RADAR",null,null,null,null,null,"rdl:RDS222580",null,"A <LEVEL MEASURING ELEMENT - FREE-SPACE RADAR> is a <LEVEL MEASURING ELEMENT - WAVE> that uses the travelling time of a radar beam to measure level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - FREE-SPACE RADAR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - CONTINUOUS-WAVE RADAR",null,null,null,null,null,"rdl:RDS222581",null,"A <LEVEL MEASURING ELEMENT - CONTINUOUS-WAVE RADAR> is a <LEVEL MEASURING ELEMENT - FREE-SPACE RADAR> that uses a continuous radar wave to measure level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - FREE-SPACE RADAR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - PULSED-WAVE RADAR",null,null,null,null,null,"rdl:RDS222582",null,"A <LEVEL MEASURING ELEMENT - PULSED-WAVE RADAR> is a <LEVEL MEASURING ELEMENT - FREE-SPACE RADAR> that uses a pulsed radar wave to measure level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - WAVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - GAMMA RAY",null,null,null,null,null,"rdl:RDS222583",null,"A <LEVEL MEASURING ELEMENT - GAMMA RAY> is a <LEVEL MEASURING ELEMENT - WAVE> that measures level by the attenuation of gamma rays passing through a process vessel. The technique is used to regulate the level of molten steel in a continuous casting process of steelmaking",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - WAVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - GUIDED-WAVE RADAR",null,null,null,null,null,"rdl:RDS222584",null,"A <LEVEL MEASURING ELEMENT - GUIDED-WAVE RADAR> is a <LEVEL MEASURING ELEMENT - WAVE> that emits a wave that is guided by a rod, cable or rope to the surface of process material and uses the time of flight of the reflected wave to measure level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - WAVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - PULSED MICROWAVE",null,null,null,null,null,"rdl:RDS222585",null,"A <LEVEL MEASURING ELEMENT - PULSED MICROWAVE> is a <LEVEL MEASURING ELEMENT - WAVE> that using a Pulsed Reflectometry signal processing technique",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - WAVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - TDR MICROWAVE",null,null,null,null,null,"rdl:RDS222586",null,"A <LEVEL MEASURING ELEMENT - TDR MICROWAVE> is a <LEVEL MEASURING ELEMENT - WAVE> using a Time-Domain Reflectometry signal processing technique which is a measurement of time of flight divided by the speed of light",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - WAVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - ULTRASONIC",null,null,null,null,null,"rdl:RDS11468384",null,"A <LEVEL MEASURING ELEMENT - ULTRASONIC> is a <LEVEL MEASURING ELEMENT - WAVE> that is used for non-contact level sensing of liquids and bulk solids. It emits high frequency (20 kHz to 200 kHz) acoustic waves that are reflected back to and detected by the emitting transducer. Ultrasonic sensors can be designed to provide point level control, continuous monitoring or both",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - FLOAT",null,null,null,null,null,"rdl:RDS851039",null,"A <LEVEL MEASURING ELEMENT - FLOAT> is an <INSTRUMENTATION ITEM> and a <LEVEL MEASURING ELEMENT> that involves the actuation of a mechanical switch actuated by a float",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - FLOAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - FLOAT - MAGNET",null,null,null,null,null,"rdl:RDS222561",null,"A <LEVEL MEASURING ELEMENT - FLOAT - MAGNET> is a <LEVEL MEASURING ELEMENT - FLOAT> that uses a magnet and resistors to determine the position of the float",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - FLOAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - FLOAT - RESISTIVE CHAIN",null,null,null,null,null,"rdl:RDS222562",null,"A <LEVEL MEASURING ELEMENT - FLOAT - RESISTIVE CHAIN> is a <LEVEL MEASURING ELEMENT - FLOAT> where a permanent magnet, sealed inside a float, moves up and down a stem in which closely spaced switches and resistors are sealed. When the switches are closed, the resistance is summed and converted to current or voltage signals that are proportional to the level of the liquid",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - FLOAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - MAGNETORESISTIVE FLOAT",null,null,null,null,null,"rdl:RDS222556",null,"A <LEVEL MEASURING ELEMENT - MAGNETORESISTIVE FLOAT> is a <LEVEL MEASURING ELEMENT - FLOAT> where a permanent magnet pair is sealed inside the float arm pivot. As the float moves up the motion and location are transmitted as the angular position of the magnetic field",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - FLOAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - MAGNETOSTRICTIVE",null,null,null,null,null,"rdl:RDS222560",null,"A <LEVEL MEASURING ELEMENT - MAGNETOSTRICTIVE> is a <LEVEL MEASURING ELEMENT -> <FLOAT> that uses the magnetostrictive effect to determine the position of the float",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LEVEL MEASURING ELEMENT - FLOAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT - MAGNETOSTRICTIVE FLOAT",null,null,null,null,null,"rdl:RDS222557",null,"A <LEVEL MEASURING ELEMENT - MAGNETOSTRICTIVE FLOAT> is a <LEVEL MEASURING ELEMENT - FLOAT> where a permanent magnet, sealed inside a float, travels up and down a stem in which a magnetostrictive wire is sealed. For high-accuracy, continuous level measurement of a wide variety of liquids",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","POSITION SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,"LIMIT SWITCH",null,null,null,null,null,"rdl:RDS418814",null,"A <LIMIT SWITCH> is an <INSTRUMENTATION ITEM> and a <POSITION SWITCH> that is a switch preventing the travel of an object in a mechanism past some predetermined point, mechanically operated by the motion of the object itself",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","POSITION MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"LIMIT SWITCH SENSOR",null,null,null,null,null,"rdl:RDS1325720321",null,"A <LIMIT SWITCH SENSOR> is an <INSTRUMENTATION ITEM> and a <POSITION MEASURING ELEMENT> that is used in conjunction with a <LIMIT SWITCH>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","VOLTAGE DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,"LINE VOLTAGE DETECTOR",null,null,null,null,null,"rdl:RDS916874",null,"A <LINE VOLTAGE DETECTOR> is an <INSTRUMENTATION ITEM> and a <VOLTAGE DETECTOR> for <LINE VOLTAGE>, i.e. phase-to-phase voltage difference",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DENSITY ANALYSER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"LIQUID DENSITY ANALYSER",null,null,null,null,null,"rdl:RDS1007864",null,"A <LIQUID DENSITY ANALYSER> is an <INSTRUMENTATION ITEM> and a <DENSITY ANALYSER> that is intended for analysing the density of liquid",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"MAGNETOMETER",null,null,null,null,null,"rdl:RDS915749",null,"A <MAGNETOMETER> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> that is intended to measure the value of a magnetic flux density in a given direction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE GAUGE",null,null,null,null,null,null,null,null,null,null,null,null,"MANOMETER",null,null,null,null,null,"rdl:RDS880874",null,"A <MANOMETER> is an <INSTRUMENTATION ITEM> and a <PRESSURE GAUGE> for low pressure measurement",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MANOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BAROMETER",null,null,null,null,null,"rdl:RDS13611695",null,"A <BAROMETER> is a <MANOMETER> that is an instrument used for the measurement of atmospheric pressure. The mercury barometer is preferable if the highest accuracy of readings is important, but where compactness has to be considered, the aneroid barometer is often used",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MANOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"U-TUBE MANOMETER",null,null,null,null,null,"rdl:RDS883394",null,"A <U-TUBE MANOMETER> is a <MANOMETER> that is a vertical or inclined U-shaped tube half-full of liquid where the measured pressure is applied to one side of the tube whilst the reference pressure (which might be of the atmosphere) is applied to the other. The difference in liquid level represents the applied pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOW MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"MASS FLOW MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS222509",null,"A <MASS FLOW MEASURING ELEMENT> is an <INSTRUMENTATION ITEM> and a <FLOW MEASURING ELEMENT> that is used to measure <MASS FLOW RATE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MASS FLOW MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MASS FLOW MEASURING ELEMENT - CORIOLIS",null,null,null,null,null,"rdl:RDS613394",null,"A <MASS FLOW MEASURING ELEMENT - CORIOLIS> is a <MASS FLOW MEASURING ELEMENT> that uses the Coriolis effect that causes a laterally vibrating tube to distort, giving a direct measurement of mass flow. Furthermore, a direct measure of the density of the fluid is obtained",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MASS FLOW MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MASS FLOW MEASURING ELEMENT - THERMAL",null,null,null,null,null,"rdl:RDS883304",null,"A <MASS FLOW MEASURING ELEMENT - THERMAL> is a <MASS FLOW MEASURING ELEMENT> that uses combinations of heated elements and temperature sensors to measure the difference between static and flowing heat transfer to a fluid and infer its flow with a knowledge of the fluids specific heat and density. The fluid temperature is also measured and compensated for. If the density and specific heat characteristics of the fluid are constant, the meter can provide a direct mass flow readout, and does not need any additional pressure temperature compensation over their specified range",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS ANALYSER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"MERCAPTAN ANALYSER",null,null,null,null,null,"rdl:RDS6599637",null,"A <MERCAPTAN ANALYSER>is an <INSTRUMENTATION ITEM> and a <GAS ANALYSER> intended to determine the mercaptan concentration in a fluid",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","WATT-HOUR METER",null,null,null,null,null,null,null,null,null,null,null,null,"MERCURY MOTOR METER",null,null,null,null,null,"rdl:RDS932399",null,"A <MERCURY MOTOR METER> is an <INSTRUMENTATION ITEM> and a <WATT-HOUR METER> or a coulometer having a disk immersed in mercury and rotating in the field produced by an electromagnet or a permanent magnet",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","WATT-HOUR METER",null,null,null,null,null,null,null,null,null,null,null,null,"METER WITH MAXIMUM DEMAND INDICATOR",null,null,null,null,null,"rdl:RDS932579",null,"A <METER WITH MAXIMUM DEMAND INDICATOR> is an <INSTRUMENTATION ITEM> and a <WATT-HOUR METER> fitted with a means to indicate the highest average value of the power during successive time intervals of equal duration",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"MOVING COIL METER",null,null,null,null,null,"rdl:RDS7034915",null,"A <MOVING COIL METER> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> and a tight coil of copper wire, wrapped round an iron core, mounted in between the poles of a permanent magnet; when an electric current is passed through that coil is deflects proportiaonally to the current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"MULTI-FUNCTION METER",null,null,null,null,null,"rdl:RDS914534",null,"A <MULTI-FUNCTION METER> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> having a single indicating device, intended to measure more than one kind of quantity",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"MULTI-RANGE INSTRUMENT",null,null,null,null,null,"rdl:RDS914399",null,"A <MULTI-RANGE INSTRUMENT> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> having more than one measuring range",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","WATT-HOUR METER",null,null,null,null,null,null,null,null,null,null,null,null,"MULTI-RATE METER",null,null,null,null,null,"rdl:RDS932624",null,"A <MULTI-RATE METER> is an <INSTRUMENTATION ITEM> and a <WATT-HOUR METER> provided with a number of registers, each becoming operative at specified time intervals corresponding to different tariffs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"MULTI-SCALE INSTRUMENT",null,null,null,null,null,"rdl:RDS914444",null,"A <MULTI-SCALE INSTRUMENT> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> having more than one scale",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"MULTIMETER",null,null,null,null,null,"rdl:RDS873539",null,"A <MULTIMETER> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> that is a hand-held multi-range multi-function measuring instrument intended for measuring voltage, current and sometimes other electrical quantities such as resistance",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOW MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"MULTIPHASE METER",null,null,null,null,null,"rdl:RDS1318334201",null,"A <MULTIPHASE METER> is an <INSTRUMENTATION ITEM> and a <FLOW MEASURING ELEMENT> for multiphase <METERING> of <LIQUID> and <GAS> flows",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"MULTIPOINT RECORDER",null,null,null,null,null,"rdl:RDS881729",null,"A <MULTIPOINT RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> that is able to record more than one variable at the same time",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS ANALYSER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"NON-DISPERSIVE INFRA-RED GAS ANALYSER",null,null,null,null,null,"rdl:RDS1066589",null,"A <NON-DISPERSIVE INFRA-RED GAS ANALYSER> is an <INSTRUMENTATION ITEM> and a <GAS ANALYSER> in which the absorption of a specific wavelength of infrared radiation is measured by radiating broadband an infrared through the gas and selecting a specific band by using a wavelength selective sensor as detector",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS ANALYSER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"NOX ANALYSER",null,null,null,null,null,"rdl:RDS6466209",null,"A <NOX ANALYSER> is an <INSTRUMENTATION ITEM> and a <GAS ANALYSER> intended to determine the nitrogen oxide concentration in gaseous compound",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"NUCLEAR MAGNETIC RESONANCE SPECTROSCOPY ANALYSER",null,null,null,null,null,"rdl:RDS6466254",null,"A <NUCLEAR MAGNETIC RESONANCE SPECTROSCOPY ANALYSER> is an <INSTRUMENTATION ITEM> and a <PROCESS ANALYSER> often used in physical and analytical chemistry for the identification of substances",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"OFF-LINE ANALYSER",null,null,null,null,null,"rdl:RDS6466344",null,"An <OFF-LINE ANALYSER> is an <INSTRUMENTATION ITEM> and a <PROCESS ANALYSER> intended for measuring on samples and not to be directly coupled to a process for continuous measuring",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MIST DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,"OIL MIST DETECTOR",null,null,null,null,null,"rdl:RDS1008989",null,"An <OIL MIST DETECTOR> is an <INSTRUMENTATION ITEM> and a <MIST DETECTOR> for detection of an oil mist",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"ON-LINE ANALYSER",null,null,null,null,null,"rdl:RDS6466389",null,"An <ON-LINE ANALYSER> is an <INSTRUMENTATION ITEM> and a <PROCESS ANALYSER> intended to be directly coupled to a process for continuous measuring",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SMOKE DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,"OPTICAL SMOKE DETECTOR",null,null,null,null,null,"rdl:RDS7064814",null,"An <OPTICAL SMOKE DETECTOR> is an <INSTRUMENTATION ITEM> and a <SMOKE DETECTOR> that is using a light source and a sensor to detect smoke",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"OPTICAL TO ELECTRICAL SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS1066704961",null,"An <OPTICAL TO ELECTRICALL SIGNAL CONVERTER > is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that converts an optical input signal to an electrical output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOW MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"ORIFICE PLATE FLOWMETER ASSEMBLY",null,null,null,null,null,"rdl:RDS881909",null,"An <ORIFICE PLATE FLOWMETER ASSEMBLY> is an <INSTRUMENTATION ITEM> and a <FLOW MEASURING ELEMENT> that is an assembly of an orifice plate, carrier rings, flanges ans manifold as its main components",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"OSCILLOSCOPE",null,null,null,null,null,"rdl:RDS914759",null,"An <OSCILLOSCOPE> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> in which a moving spot on the screen of a cathode-ray tube represents by its position the relationship between two variables",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"PANEL MOUNTED INSTRUMENT",null,null,null,null,null,"rdl:RDS881999",null,"A <PANEL MOUNTED INSTRUMENT> is an <INSTRUMENTATION ITEM> that has a special shape intended to be mounted on or in a flat rigid surface,",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS ANALYSER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"PARAMETRIC OXYGEN ANALYSER",null,null,null,null,null,"rdl:RDS1066544",null,"A <PARAMETRIC OXYGEN ANALYSER> is an <INSTRUMENTATION ITEM> and a <GAS ANALYSER> making use of the magnetic property of oxygen to measure its concentration",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","VOLTMETER",null,null,null,null,null,null,null,null,null,null,null,null,"PEAK VOLTMETER",null,null,null,null,null,"rdl:RDS915164",null,"A <PEAK VOLTMETER> is an <INSTRUMENTATION ITEM> and a <VOLTMETER> that measures the peak value of an alternating voltage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"PEN RECORDER",null,null,null,null,null,"rdl:RDS916109",null,"A <PEN RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> that is using a pen supplied with ink to record data on a chart",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PEN RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE PEN RECORDER",null,null,null,null,null,"rdl:RDS6623058",null,"A <SINGLE PEN RECORDER> is a <PEN RECORDER> that is equipped with only one pen",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","WEIGHT MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"PIEZOELECTRIC LOAD CELL",null,null,null,null,null,"rdl:RDS222602",null,"A <PIEZOELECTRIC LOAD CELL> is an <INSTRUMENTATION ITEM> and a <WEIGHT MEASURING ELEMENT that works on the same principle of deformation as the strain gauge load cells, but a voltage output is generated by the basic piezoelectric material - proportional to the deformation of load cell",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"PILOT OPERATED REGULATOR",null,null,null,null,null,"rdl:RDS882134",null,"A <PILOT OPERATED REGULATOR> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> where a diaphragm responds quickly to the downstream pressure, causing an immediate correction of the main valve plug position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"PLOTTER",null,null,null,null,null,"rdl:RDS13610795",null,"A <PLOTTER> is an <INSTRUMENTATION ITEM> and a <RECORDER> that is a pen based graph printing device",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","WEIGHT MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC LOAD CELL",null,null,null,null,null,"rdl:RDS222603",null,"A <PNEUMATIC LOAD CELL> is an <INSTRUMENTATION ITEM> and a <WEIGHT MEASURING ELEMENT that has a diaphragm working on a force-balance principle",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PNEUMATIC APPARATUS","TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC TRANSMITTER",null,null,null,null,null,"rdl:RDS2222220",null,"A <PNEUMATIC TRANSMITTER> is an <INSTRUMENTATION ITEM> and a <TRANSMITTER> and an <PNEUMATIC APPARATUS>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"PORTABLE INSTRUMENT",null,null,null,null,null,"rdl:RDS914309",null,"A <PORTABLE INSTRUMENT> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> designed to be easily carried by hand and to be disconnected by the user",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","WATT-HOUR METER",null,null,null,null,null,null,null,null,null,null,null,null,"PREPAYMENT METER",null,null,null,null,null,"rdl:RDS932669",null,"A <PREPAYMENT METER> is an <INSTRUMENTATION ITEM> and a <WATT-HOUR METER> provided with a mechanism which, by insertion of suitable payment means (e.g. coin, token or credit card), connects a supply of electricity and then disconnects it after the consumption of a predetermined amount of energy or after a predetermined duration",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE REDUCING VALVE",null,null,null,null,null,"rdl:RDS646199",null,"A <PRESSURE REDUCING VALVE> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that is equipped with an internal pressure sensing element that reduces the upstream line pressure to a set level downstream, and maintains the reduced pressure irrespective of changes in upstream pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE REGULATOR VALVE",null,null,null,null,null,"rdl:RDS309284",null,"A <PRESSURE REGULATOR VALVE> is an <INSTRUMENTATION ITEM> and a <REGULATOR> that can be used to regulate the pressure in a container or system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE TO CURRENT SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS460439",null,"A <PRESSURE TO CURRENTL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a pressure input signal to a current output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE TO VOLTAGE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS851264",null,"A <PRESSURE TO VOLTAGEL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a pressure input signal into a voltage output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE RELIEF DEVICE","VACUUM RELIEF DEVICE",null,null,null,null,null,null,null,null,null,null,null,"PRESSURE VACUUM RELIEF VALVE",null,null,null,null,null,"rdl:RDS6330659",null,"A <PRESSURE VACUUM RELIEF VALVE> is an <INSTRUMENTATION ITEM> and a <PRESSURE RELIEF DEVICE> and a <VACUUM RELIEF DEVICE> that automatically releases excess pressure or admits pressure to prevent a vacuum",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"PRINTING RECORDER",null,null,null,null,null,"rdl:RDS916334",null,"A <PRINTING RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> that produces characters or graphic symbols on paper or other medium",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PRINTING RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOTTED LINE RECORDER",null,null,null,null,null,"rdl:RDS916379",null,"A <DOTTED LINE RECORDER> is a <PRINTING RECORDER> in which the record comprises a series of points, numerals, etc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","INSTRUMENTATION SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,"PROCESS DATA ACQUISITION AND CONTROL SYSTEM",null,null,null,null,null,"rdl:RDS276749",null,"A <PROCESS DATA ACQUISITION AND CONTROL SYSTEM> is an <INSTRUMENTATION ITEM> and an <INSTRUMENTATION SYSTEM> that measures and controls the main plant computerized operational system, where all process, utility and off site activities are monitored. The system is located in the main control room",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROCESS SIGNAL GENERATING FUNCTION","SYSTEM",null,null,null,null,null,null,null,null,null,null,null,"PROCESS SIGNAL GENERATING SYSTEM",null,null,null,null,null,"rdl:RDS222435",null,"A <PROCESS SIGNAL GENERATING SYSTEM> is an <INSTRUMENTATION ITEM> and a <PROCESS SIGNAL GENERATING FUNCTION> and a <SYSTEM> that is the assembly of a <DETECTOR>, <SWITCH>, or <TRANSMITTER> and all necessary piping, tubing, wiring, and other accessories around it",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","POSITION SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,"PROXIMITY SWITCH",null,null,null,null,null,"rdl:RDS851084",null,"A <PROXIMITY SWITCH> is a <POSITION SWITCH> and a <PROXIMITY MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTROMETER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"QUADRANT ELECTROMETER",null,null,null,null,null,"rdl:RDS918089",null,"A <QUADRANT ELECTROMETER> is an <INSTRUMENTATION ITEM> and an <ELECTROMETER> in which the moving element is actuated by electrostatic forces between that element and fixed elements in the form of quadrants",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"QUOTIENT-METER",null,null,null,null,null,"rdl:RDS914939",null,"A <QUOTIENT-METER> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> intended to measure the ratio or the quotient of the values of two quantities",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISPLACEMENT MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL DISPLACEMENT PROBE",null,null,null,null,null,"rdl:RDS6500499",null,"An <RADIAL DISPLACEMENT PROBE> is an <INSTRUMENTATION ITEM> and a <DISPLACEMENT MEASURING ELEMENT> for measurement of <RADIAL DISPLACEMENT>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"RATIO-METER",null,null,null,null,null,"rdl:RDS914894",null,"A <RATIO-METER> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> intended to measure the ratio or the quotient of the values of two quantities",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","POWER METER",null,null,null,null,null,null,null,null,null,null,null,null,"REACTIVE POWER METER",null,null,null,null,null,"rdl:RDS870884",null,"A <REACTIVE POWER METER> is an <INSTRUMENTATION ITEM> and a <POWER METER> that is measuring the reactive electrical power (VAr)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DENSITY ANALYSER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"RELATIVE DENSITY GAS ANALYSER",null,null,null,null,null,"rdl:RDS6600192",null,"A <RELATIVE DENSITY GAS ANALYSER> is an <INSTRUMENTATION ITEM> and a <DENSITY ANALYSER> that is intended to determine the density of a gas relative to another gas",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE RELIEF DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"RELIEF VALVE",null,null,null,null,null,"rdl:RDS416699",null,"A <RELIEF VALVE> is an <INSTRUMENTATION ITEM> and a <PRESSURE RELIEF DEVICE> that is set to open at a certain pressure level to prevent the pressure in a container or system from reaching unsafe levels",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BALANCED RELIEF VALVE",null,null,null,null,null,"rdl:RDS6333340",null,"A <BALANCED RELIEF VALVE> is a <RELIEF VALVE> that incorporates means of minimizing the effect of back pressure on the operational characteristics of the valve (opening pressure, closing pressure and relieving capacity)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALANCED RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BALANCED RELIEF VALVE COMBINED",null,null,null,null,null,"rdl:RDS7461715",null,"A <BALANCED RELIEF VALVE COMBINED> is a <BALANCED RELIEF VALVE> that is equipped with balancing bellows and an auxiliary balancing piston",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALANCED RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BALANCED RELIEF VALVE USING BELLOWS",null,null,null,null,null,"rdl:RDS7461670",null,"A <BALANCED RELIEF VALVE USING BELLOWS> is a <BALANCED RELIEF VALVE> that is equipped with balancing bellows. The balancing bellows minimizes the effects of backpressure and prevents the process fluid from entering the spring chamber",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALANCED RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BALANCED RELIEF VALVE USING PISTON",null,null,null,null,null,"rdl:RDS7461625",null,"A <BALANCED RELIEF VALVE USING PISTON> is a <BALANCED RELIEF VALVE> that is equipped with a balancing piston. The balanced piston design minimizes the effects of backpressure and prevents the process fluid from entering the spring chamber",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONVENTIONAL RELIEF VALVE",null,null,null,null,null,"rdl:RDS885239",null,"A <CONVENTIONAL RELIEF VALVE> is a <RELIEF VALVE> that has its closing force provided by a spring",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONVENTIONAL SAFETY RELIEF VALVE",null,null,null,null,null,"rdl:RDS7461501",null,"A <CONVENTIONAL SAFETY RELIEF VALVE> is a <RELIEF VALVE> that is equipped with vented bonnet where its performance characteristics are directly affected by changes of the back pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HIGH PRESSURE RELIEF VALVE",null,null,null,null,null,"rdl:RDS428309",null,"A <HIGH PRESSURE RELIEF VALVE> is a <RELIEF VALVE> that is venting off high pressure gas to the atmosphere",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PILOT-OPERATED RELIEF VALVE",null,null,null,null,null,"rdl:RDS885194",null,"A <PILOT-OPERATED RELIEF VALVE> is a <RELIEF VALVE> that uses a pilot valve to indirectly activate the main valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE RELIEF VALVE",null,null,null,null,null,"rdl:RDS7461439",null,"A <PRESSURE RELIEF VALVE> is a <RELIEF VALVE> that is an automatic pressure relieving device actuated by the static pressure upstream of the valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE","SAFETY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"SAFETY RELIEF VALVE",null,null,null,null,null,"rdl:RDS6330862",null,"A <SAFETY RELIEF VALVE> is a <SAFETY VALVE> and a <RELIEF VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SAFETY RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CRANKCASE SAFETY RELIEF VALVE",null,null,null,null,null,"rdl:RDS13310425",null,"A <CRANKCASE SAFETY RELIEF VALVE> is a <SAFETY RELIEF VALVE> to release pressure in case of a crankcase explosion",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SAFETY RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOWNHOLE SAFETY RELIEF VALVE",null,null,null,null,null,"rdl:RDS16552132",null,"A <DOWNHOLE SAFETY VALVE> is a <SAFETY RELEIF VALVE> insertable into the well tubing to act as a well barrier",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOWNHOLE SAFETY RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SURFACE CONTROLLED SUBSURFACE SAFETY RELEIF VALVE",null,null,null,null,null,"rdl:RDS16756786",null,"A <SURFACE CONTROLLED SUBSURFACE SAFETY RELIEF VALVE> is a <DOWNHOLE SAFETY VALVE> located in a well and operated from the surface that, when it is activated, is designed to prevent uncontrolled flow up the well",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WEIGHT-OPERATED RELIEF VALVE",null,null,null,null,null,"rdl:RDS11215931",null,"A <WEIGHT-OPERATED RELIEF VALVE> is a <RELIEF VALVE> in which the closure member is held against the seat by a static weight",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"YARWAY RELIEF VALVE",null,null,null,null,null,"rdl:RDS11141545",null,"A <YARWAY RELIEF VALVE> is a <RELIEF VALVE> that is a valve installed in a bypass line on the discharge header of a pump that is recirculating the minimum flow required back to the pump suction in cases of closed discharge line",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"RESISTANCE TO CURRENT SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS5763018",null,"A <RESISTANCE TO CURRENTL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended to convert a measured resistance as input into a current output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE RELIEF DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"SAFETY VALVE",null,null,null,null,null,"rdl:RDS309374",null,"A <SAFETY VALVE> is an <INSTRUMENTATION ITEM> and a <PRESSURE RELIEF DEVICE> that is used in gas service",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SAFETY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RELIEF POP-OFF VALVE",null,null,null,null,null,"rdl:RDS17157050",null,"A <RELIEF POP-OFF VALVE> is a <SAFETY VALVE> that is designed to be used in breathing circuits. The relief pop-off valve is venting gas to the atmosphere when the pressure of the gas in the breathing circuit reaches a certain level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SAFETY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STRAIGHT THROUGH SAFETY VALVE",null,null,null,null,null,"rdl:RDS6331313",null,"A <STRAIGHT THROUGH SAFETY VALVE> is a <SAFETY VALVE> that is a relief valve of straight body design, usually with small bore for instrumentation purposes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"SEQUENCE OF EVENTS RECORDER",null,null,null,null,null,"rdl:RDS6622878",null,"A <SEQUENCE OF EVENTS RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> intended to record time stamped events",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOW GAUGE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"SIGHT FLOW INDICATOR",null,null,null,null,null,"rdl:RDS5771573",null,"A <SIGHT FLOW INDICATOR> is an <INSTRUMENTATION ITEM> and a <FLOW GAUGE> that is a transparent flow gauge indicating whether there is a flow or not",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVEYOR",null,null,null,null,null,null,null,null,null,null,null,null,"SIGNAL CONVEYING ITEM",null,null,null,null,null,"rdl:RDS2220500",null,"A <PROCESS SIGNAL CONVEYING ITEM> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVEYOR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIGITAL LOOP","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"FIELDBUS",null,null,null,null,null,"rdl:RDS2222904",null,"A <FIELDBUS> is a <SIGNAL CONVEYING ITEM> and a <DIGITAL LOOP> that is an all-digital, serial, two-way communications system that serves as the base-level network in a plant or factory automation environment. It is an open architecture, developed and administered by the Fieldbus Foundation. It is targeted for applications using basic and advanced regulatory control, and for much of the discrete control associated with those functions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FIELDBUS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOUNDATION Fieldbus H1",null,null,null,null,null,"rdl:RDS2222905",null,"A <FOUNDATION Fieldbus H1> is a <FIELDBUS> that operates at 31.25 kbit/s and is generally used to connect to field devices and host systems. It provides communication and power over standard stranded twisted-pair wiring in both conventional and intrinsic safety applications. H1 is currently the most common implementation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FIELDBUS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HIGH SPEED ETHERNET (HSE)",null,null,null,null,null,"rdl:RDS2222906",null,"A <HIGH SPEED ETHERNET (HSE)> is a <FIELDBUS> that operates at 100/1000 Mbit/s and generally connects input/output subsystems, host systems, linking devices and gateways. It does not currently provide power over the cable, although work is under way to address this using the IEEE802.3af Power over Ethernet (PoE) standard",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIGITAL LOOP","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"HART",null,null,null,null,null,"rdl:RDS2222903",null,"A <HART> is a <SIGNAL CONVEYING ITEM> and a <DIGITAL LOOP> that is compliant with the HART Communications Protocol (Highway Addressable Remote Transducer)and is an early implementation of <FIELDBUS>. Its most notable advantage is that it can communicate over legacy 4-20 mA analog instrumentation wiring, sharing the pair of wires used by the older system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIGITAL LOOP","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"MODBUS RS-485",null,null,null,null,null,"rdl:RDS2222910",null,"A <MODBUS RS-485> is a <SIGNAL CONVEYING ITEM> and a <DIGITAL LOOP> that is compliant with TIA-495 that is a standard defining the electrical characteristics of drivers and receivers for use in balanced digital multipoint systems. The standard is published by the Telecommunications Industry Association/Electronic Industries Alliance (TIA/EIA). Digital communications networks implementing the standard can be used effectively over long distances and in electrically noisy environments. Multiple receivers may be connected to such a network in a linear, multi-drop configuration. These characteristics make such networks useful in industrial environments and similar applications",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OPTICAL FIBRE",null,null,null,null,null,"rdl:RDS514214",null,"An <OPTICAL FIBRE> is a <SIGNAL CONVEYING ITEM> that is a flexible, transparent fiber made by drawing glass (silica) or plastic to a diameter slightly thicker than that of a human hair; Optical fibers are used most often as a means to transmit light between the two ends of the fiber and find wide usage in fiber-optic communications, where they permit transmission over longer distances and at higher bandwidths (data rates) than wire cables",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OPTICAL FIBRE CABLE",null,null,null,null,null,"rdl:RDS475829",null,"An <OPTICAL FIBRE CABLE> is a <SIGNAL CONVEYING ITEM> that is an assembly comprising one or more <OPTICAL FIBRE>s or fibre bundles inside a common covering designed to protect them against mechanical stresses and other environmental influences while retaining the transmission quality of the fibres",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIGITAL LOOP","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"PROFIBUS",null,null,null,null,null,"rdl:RDS2222907",null,"A <PROFIBUS> is a <SIGNAL CONVEYING ITEM> and a <DIGITAL LOOP> that is a standard for fieldbus communication in automation technology and was first promoted in 1989 by BMBF (German department of education and research); it is openly published as part of IEC 61158. It has two variations: PA (Process Automation) and DP (Decentralised Peripherals). PA uses the same protocol as DP, and can be linked to a DP network using a coupler device. The much faster DP acts as a backbone network for transmitting process signals to the controller. This means that DP and PA can work tightly together, especially in hybrid applications where process and factory automation networks operate side by side",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PROFIBUS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROFIBUS DP",null,null,null,null,null,"rdl:RDS2222908",null,"A <PROFIBUS DP> is a <PROFIBUS> that is used to operate sensors and actuators via a centralised controller in production (factory) automation applications. The many standard diagnostic options, in particular, are focused on here",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PROFIBUS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROFIBUS PA",null,null,null,null,null,"rdl:RDS2222909",null,"A <PROFIBUS PA> is a <PROFIBUS> that is used to monitor measuring equipment via a process control system in process automation applications. This variant is designed for use in explosion/hazardous areas (Ex-zone 0 and 1). The Physical Layer (i.e. the cable) conforms to IEC 61158-2, which allows power to be delivered over the bus to field instruments, while limiting current flows so that explosive conditions are not created, even if a malfunction occurs. The number of devices attached to a PA segment is limited by this feature. PA has a data transmission rate of 31.25 kbit/s",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"SHIELDED CABLE",null,null,null,null,null,"rdl:RDS6459144",null,"A <SHIELDED CABLE> is a <SIGNAL CONVEYING ITEM> and a <ELECTRICAL CABLE> that contains a cable shield",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMOCOUPLE COMPENSATION CABLE",null,null,null,null,null,"rdl:RDS6459234",null,"A <THERMOCOUPLE COMPENSATION CABLE> is a <SIGNAL CONVEYING ITEM> and a <ELECTRICAL CABLE> having conductors differing in nature or quality from that of the thermocouple, but having thermoelectric characteristics such that the resulting error is within specified limits for a given temperature range",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CABLE","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMOCOUPLE EXTENSION CABLE",null,null,null,null,null,"rdl:RDS6459279",null,"A <THERMOCOUPLE EXTENSION CABLE> is a <SIGNAL CONVEYING ITEM> and a <ELECTRICAL CABLE> consisting of conductors of the same nature as the thermocouple elements, extending it to the reference junction and having the same thermo-electric properties as those of the thermocouple within the whole temperature range of utilisation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","STANDARD SIGNAL RECEIVER","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"SIGNAL SWITCH",null,null,null,null,null,"rdl:RDS222463",null,"A <SIGNAL SWITCH> is a <INSTRUMENTATION ITEM> and a <STANDARD SIGNAL RECEIVER> and a <SWITCHING DEVICE> that operates when an input standard signal reaches a preset criterium",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE FUNCTION INSTRUMENT",null,null,null,null,null,"rdl:RDS914489",null,"A <SINGLE FUNCTION INSTRUMENT> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> intended for the measurement of one kind of quantity only",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE RANGE INSTRUMENT",null,null,null,null,null,"rdl:RDS914354",null,"A <SINGLE RANGE INSTRUMENT> is an <INSTRUMENTATION ITEM> and a <MEASURING INSTRUMENT> having only one measuring range",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","OXYGEN CONTENT ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"SOLID ELECTROLYTE OXYGEN ANALYSER",null,null,null,null,null,"rdl:RDS1066679",null,"A <SOLID ELECTROLYTE OXYGEN ANALYSER> is an <INSTRUMENTATION ITEM> and an <OXYGEN CONTENT ANALYSER> using the electrochemical behaviour of a solid, e.g. zirconia, at high temperature to determine the oxygen content of a fluid",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","VOLTMETER",null,null,null,null,null,null,null,null,null,null,null,null,"SPARK GAP METER",null,null,null,null,null,"rdl:RDS917999",null,"A <SPARK GAP METER> is an <INSTRUMENTATION ITEM> and a <VOLTMETER> intended to measure peak voltage as a function of the flashover distance between its two electrodes, generally spheres",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"SPOT RECORDER",null,null,null,null,null,"rdl:RDS916199",null,"A <SPOT RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> that is using an optical head for projecting a light beam (visible or invisible) on a light-sensitive chart",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"SPRING-LOADED CONSTANT DOWNSTREAM PRESSURE VALVE",null,null,null,null,null,"rdl:RDS11141815",null,"An <SPRING-LOADED CONSTANT DOWNSTREAM PRESSURE VALVE> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that acts against a spring pressure to maintain a constant downstream pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOW REGULATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"SPRINKLER CONTROL VALVE",null,null,null,null,null,"rdl:RDS312074",null,"An <SPRINKLER CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <FLOW REGULATOR> that can be used to control the flow of fluid to a sprinkler system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER","STANDARD SIGNAL RECEIVER",null,null,null,null,null,null,null,null,null,null,null,"STANDARD SIGNAL RECORDER",null,null,null,null,null,"rdl:RDS222472",null,"A <STANDARD SIGNAL RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> and a <STANDARD SIGNAL RECEIVER> that produces a record that is proportional with a standard input signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"STYLUS RECORDER",null,null,null,null,null,"rdl:RDS916154",null,"A <STYLUS RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> in which the record on the chart is made by a stylus not requiring ink",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SULPHUR ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"SULPHUR IN GAS ANALYSER",null,null,null,null,null,"rdl:RDS6623898",null,"A <SULPHUR IN GAS ANALYSER> is an <INSTRUMENTATION ITEM> and a <SULPHUR ANALYSER> that is intended to determine the sulphur concentration in gas",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SULPHUR ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"SULPHUR IN OIL ANALYSER",null,null,null,null,null,"rdl:RDS6624003",null,"A <SULPHUR IN OIL ANALYSER> is an <INSTRUMENTATION ITEM> and a <SULPHUR ANALYSER> that is intended to determine the sulphur concentration in oil",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS DETECTOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"SURFACE MOUNTED GAS DETECTOR",null,null,null,null,null,"rdl:RDS6720917",null,"A <SURFACE MOUNTED GAS DETECTOR> is an <INSTRUMENTATION ITEM> and a <GAS DETECTOR> that is designed to be mounted onto a surface such that it protrudes into the volume of which it is intended to detect gas",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC VARIABLE METER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"SYNCHRONOSCOPE",null,null,null,null,null,"rdl:RDS870389",null,"A <SYNCHRONOSCOPE> is an <INSTRUMENTATION ITEM> and an <ELECTRIC VARIABLE METER> that is intended to indicate if two a.c. voltages or polyphase voltage systems have the same frequency and are in phase",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","TEMPERATURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE MEASURING ELEMENT - BIMETAL",null,null,null,null,null,"rdl:RDS445184",null,"A <TEMPERATURE MEASURING ELEMENT - BIMETAL> is an <INSTRUMENTATION ITEM> and a <TEMPERATURE MEASURING ELEMENT> that is composed of two separate metals joined together and which convert a temperature change into mechanical displacement",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","TEMPERATURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE MEASURING ELEMENT - FILLED BULB",null,null,null,null,null,"rdl:RDS1029959",null,"A <TEMPERATURE MEASURING ELEMENT - FILLED BULB> is an <INSTRUMENTATION ITEM> and a <TEMPERATURE MEASURING ELEMENT> that uses the principle of fluid expansion to measure temperature",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","TEMPERATURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE MEASURING ELEMENT - INFRARED",null,null,null,null,null,"rdl:RDS222595",null,"A <TEMPERATURE MEASURING ELEMENT - INFRARED> is an <INSTRUMENTATION ITEM> and a <TEMPERATURE MEASURING ELEMENT> that infers temperature from a portion of the thermal radiation sometimes called blackbody radiation emitted by the object being measured",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","TEMPERATURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE MEASURING ELEMENT - RESISTANCE",null,null,null,null,null,"rdl:RDS445274",null,"A <TEMPERATURE MEASURING ELEMENT - RESISTANCE> is an <INSTRUMENTATION ITEM> and a <TEMPERATURE MEASURING ELEMENT> that is a sensing element that operate on the principle of changes in electrical resistance of pure metals (sintered semiconductor material) and are characterized by an almost linear positive change in resistance with temperature",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - RESISTANCE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NEGATIVE RESISTANCE TEMPERATURE ELEMENT",null,null,null,null,null,"rdl:RDS445364",null,"A <NEGATIVE RESISTANCE TEMPERATURE ELEMENT> is a <TEMPERATURE MEASURING ELEMENT - RESISTANCE> that has a negative temperature coefficient which means that the electrical resistance decreases with increasing temperature",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - RESISTANCE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POSITIVE RESISTANCE TEMPERATURE ELEMENT",null,null,null,null,null,"rdl:RDS445319",null,"A <POSITIVE RESISTANCE TEMPERATURE ELEMENT> is a <TEMPERATURE MEASURING ELEMENT - RESISTANCE> that has a positive temperature coefficient which means that the electrical resistance increases with increasing temperature",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - RESISTANCE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PT100 RESISTANCE THERMOMETER",null,null,null,null,null,"rdl:RDS890324",null,"A <PT100 RESISTANCE THERMOMETER> is a <TEMPERATURE MEASURING ELEMENT - RESISTANCE> made of platinum that has the resistance of 100 ohm at 0 deg. Celsius",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PT100 RESISTANCE THERMOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WINDING TEMPERATURE SENSOR",null,null,null,null,null,"rdl:RDS1186559",null,"A <WINDING TEMPERATURE SENSOR> is a <PT100 RESISTANCE THERMOMETER> that is designed for winding temperature measurement",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - RESISTANCE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PT1000 RESISTANCE THERMOMETER",null,null,null,null,null,"rdl:RDS1464287521",null,"A <PT1000 RESISTANCE THERMOMETER> is a <TEMPERATURE MEASURING ELEMENT - RESISTANCE> made of platinum that has the resistance of 1000 ohm at 0 deg. Celsius",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - RESISTANCE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMISTOR",null,null,null,null,null,"rdl:RDS6624243",null,"A <THERMISTOR> is a <TEMPERATURE MEASURING ELEMENT - RESISTANCE> that use a semiconductor device to change resistance that increases with increasing temperature, and is used for the sensitive measurement and control",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","TEMPERATURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE",null,null,null,null,null,"rdl:RDS445229",null,"A <TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE> is an <INSTRUMENTATION ITEM> and a <TEMPERATURE MEASURING ELEMENT> that is a temperature sensing element in which a pair of wires of dissimilar metals (as copper and iron) are joined and the free ends of the wires are connected to an instrument (as a voltmeter) that measures the difference in potential created at the junction of the two metals",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TYPE B THERMOCOUPLE",null,null,null,null,null,"rdl:RDS12171850",null,"A <TYPE B THERMOCOUPLE> is a <TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE> made of 70%Pt/30%Rhâ€“94%Pt/6%Rh, by weight",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TYPE C THERMOCOUPLE",null,null,null,null,null,"rdl:RDS12171895",null,"A <TYPE C THERMOCOUPLE> is a <TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE> made of 95%W/5%Reâ€“74%W/26%Re, by weight",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TYPE D THERMOCOUPLE",null,null,null,null,null,"rdl:RDS12171940",null,"A <TYPE D THERMOCOUPLE> is a <TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE> made of 97%W/3%Reâ€“75%W/25%Re, by weight",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TYPE E THERMOCOUPLE",null,null,null,null,null,"rdl:RDS12171985",null,"A <TYPE E THERMOCOUPLE> is a <TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE> made of chromel-constantan",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TYPE G THERMOCOUPLE",null,null,null,null,null,"rdl:RDS12172030",null,"A <TYPE G THERMOCOUPLE> is a <TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE> made of Wâ€“74%W/26%Re, by weight",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TYPE J THERMOCOUPLE",null,null,null,null,null,"rdl:RDS12172075",null,"A <TYPE J THERMOCOUPLE> is a <TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE> made of iron-constantan",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TYPE K THERMOCOUPLE",null,null,null,null,null,"rdl:RDS12171355",null,"A <TYPE K THERMOCOUPLE> is a <TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE> made of chromel-alumel",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TYPE M THERMOCOUPLE",null,null,null,null,null,"rdl:RDS222596",null,"A <TYPE M THERMOCOUPLE> is a <TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE> made of 82%Ni/18%Moâ€“99.2%Ni/0.8%Co%, by weight",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TYPE N THERMOCOUPLE",null,null,null,null,null,"rdl:RDS222597",null,"A <TYPE N THERMOCOUPLE> is a <TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE> made of Nicrosil-Nisil",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TYPE R THERMOCOUPLE",null,null,null,null,null,"rdl:RDS12170905",null,"A <TYPE R THERMOCOUPLE> is a <TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE> made of 87%Pt/13%Rhâ€“Pt, by weight",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TYPE S THERMOCOUPLE",null,null,null,null,null,"rdl:RDS12170950",null,"A <TYPE S THERMOCOUPLE> is a <TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE> made of 90%Pt/10%Rhâ€“Pt, by weight",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TYPE T THERMOCOUPLE",null,null,null,null,null,"rdl:RDS12170995",null,"A <TYPE T THERMOCOUPLE> is a <TEMPERATURE MEASURING ELEMENT - THERMOCOUPLE> made of copper-constantan",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"THERMAL CONDUCTIVITY ANALYSER",null,null,null,null,null,"rdl:RDS1008089",null,"A <THERMAL CONDUCTIVITY ANALYSER>is a <PROCESS ANALYSER> that is intended to determine a physical property that is named thermal conductivity",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"GAS ANALYSER","INSTRUMENTATION ITEM","THERMAL CONDUCTIVITY ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"THERMAL CONDUCTIVITY GAS ANALYSER",null,null,null,null,null,"rdl:RDS1066454",null,"A <THERMAL CONDUCTIVITY GAS ANALYSER>is an <INSTRUMENTATION ITEM> and a <GAS ANALYSER> and a <THERMAL CONDUCTIVITY ANALYSER> intended to provide on-line gas-composition analysis based on the measured thermal conductivity of the gases in a mixture",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","TEMPERATURE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"THERMAL ELEMENT BULB",null,null,null,null,null,"rdl:RDS7350739",null,"A <THERMAL ELEMENT BULB> is an <INSTRUMENTATION ITEM> and a <TEMPERATURE MEASURING ELEMENT> that is a closed metal bulb containing a temperature responsive fluid",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"THERMAL RECORDER",null,null,null,null,null,"rdl:RDS916244",null,"A <THERMAL RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> that is using thermal pen(s) to record data on a chart",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","TEMPERATURE GAUGE",null,null,null,null,null,null,null,null,null,null,null,null,"THERMOMETER",null,null,null,null,null,"rdl:RDS5779382",null,"A <THERMOMETER> is an <INSTRUMENTATION ITEM> and a <TEMPERATURE GAUGE>, typically one consisting of a narrow, hermetically sealed glass tube marked with graduations and having at one end a bulb containing mercury or alcohol which extends along the tube as it expands",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMOMETER 135 DEGREES LEFT",null,null,null,null,null,"rdl:RDS1471868161",null,"A <THERMOMETER 135 DEGREES LEFT> is a <THERMOMETER> where the stem is at a 135 degree angle with the axis of the <GAUGE>, pointing left",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMOMETER 135 DEGREES RIGHT",null,null,null,null,null,"rdl:RDS1471868951",null,"A <THERMOMETER 135 DEGREES RIGHT> is a <THERMOMETER> where the stem is at a 135 degree angle with the axis of the <GAUGE>, pointing right",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMOMETER STRAIGHT",null,null,null,null,null,"rdl:RDS1471867731",null,"A <THERMOMETER STRAIGHT> is a <THERMOMETER> where the stem is aligned with the axis of the thermometer",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMOMETER WITH CELSIUS TEMPERATURE SCALE",null,null,null,null,null,"rdl:RDS1471721551",null,"A <THERMOMETER WITH CELSIUS TEMPERATURE SCALE> is a <THERMOMETER> that has a celsius temperature indicator scale",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMOMETER WITH CELSIUS-FARENHEIT TEMPERATURE SCALE",null,null,null,null,null,"rdl:RDS1471722991",null,"A <THERMOMETER WITH CELSIUS-FARENHEIT TEMPERATURE SCALE> is a <THERMOMETER> that has a celsius-farenheit temperature indicator scale",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMOMETER WITH FARENHEIT TEMPERATURE SCALE",null,null,null,null,null,"rdl:RDS1471722181",null,"A <THERMOMETER WITH FARENHEIT TEMPERATURE SCALE> is a <THERMOMETER> that has a farenheit temperature indicator scale",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMOMETER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"V-SHAPED THERMOMETER",null,null,null,null,null,"rdl:RDS1471891631",null,"A <THERMOMETER V-SHAPE> is a <THERMOMETER> where the opening in the upper case has a V-shape",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","TEMPERATURE SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,"THERMOSTAT",null,null,null,null,null,"rdl:RDS964664",null,"A <THERMOSTAT> is an <INSTRUMENTATION ITEM> and a <TEMPERATURE SWITCH> whose function is controlled by variations of temperature and whose contacts make or break automatically a load circuit when the temperature of the ambient space in which its sensing element placed or the temperature of the surface on which it is fixed reaches a predetermined value",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMOSTAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ADJUSTABLE THERMOSTAT",null,null,null,null,null,"rdl:RDS964709",null,"An <ADJUSTABLE THERMOSTAT> is a <THERMOSTAT> whose operating temperature may be varied by the user by adjusting the actuating mechanism, the position of which can be readily identified",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ADJUSTABLE THERMOSTAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MECHANICALLY ADJUSTABLE THERMOSTAT",null,null,null,null,null,"rdl:RDS1462231991",null,"A <MECHANICALLY ADJUSTABLE THERMOSTAT> is an <ADJUSTABLE THERMOSTAT> where the settings must be changed via mechanical means",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ADJUSTABLE THERMOSTAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROGRAMMABLE ADJUSTABLE THERMOSTAT",null,null,null,null,null,"rdl:RDS1462230971",null,"A <PROGRAMMABLE ADJUSTABLE THERMOSTAT> is an <ADJUSTABLE THERMOSTAT> that is programmable; i.e. the settings can be changed in software",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMOSTAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AMBIENT THERMOSTAT",null,null,null,null,null,"rdl:RDS964754",null,"An <AMBIENT THERMOSTAT> is a <THERMOSTAT> that responds to changes in the temperature of the space into which its sensing element penetrates or is housed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMOSTAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-ADJUSTABLE THERMOSTAT",null,null,null,null,null,"rdl:RDS964799",null,"A <NON-ADJUSTABLE THERMOSTAT> is a <THERMOSTAT> whose operating temperature is determined by a permanent setting carried out by the manufacturer",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","TEMPERATURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"THERMOSTATIC MIXING ASSEMBLY",null,null,null,null,null,"rdl:RDS312839",null,"A <THERMOSTATIC MIXING ASSEMBLY> is an <INSTRUMENTATION ITEM> and a <TEMPERATURE REGULATOR> that maintains and limits mixed hot water to a desired, selectable temperature, helping to minimize thermal shock",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"TOC ANALYSER",null,null,null,null,null,"rdl:RDS6466569",null,"A <TOC ANALYSER>is a <PROCESS ANALYSER> intended to determine the total organic carbon content in a substance",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","POSITION SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,"TRAVEL STOP",null,null,null,null,null,"rdl:RDS7773461",null,"A <TRAVEL STOP> is a <POSITION SWITCH> that terminates a rotation when a predefined position has been reached",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"TREND RECORDER",null,null,null,null,null,"rdl:RDS1029869",null,"A <TREND RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> that enables the recording of historical data at a reduced sampling rate, to be retrieved for trend and power quality analysis",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HEAT DETECTOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"TRIMPLATE PNEUMATIC HEAT DETECTION",null,null,null,null,null,"rdl:RDS313154",null,"A <TRIMPLATE PNEUMATIC HEAT DETECTION> is an <INSTRUMENTATION ITEM> and a <HEAT DETECTOR> for detection of heat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"TURBIDITY ANALYSER",null,null,null,null,null,"rdl:RDS6466614",null,"A <TURBIDITY ANALYSER>is a <PROCESS ANALYSER> for measuring turbidity (clarity) of liquids using the nephelometric principal to compare the light scattered due to contamination with the light scattering from a standard reference suspension",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"FLAME DETECTOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"TWIN BEAM FLAME DETECTOR",null,null,null,null,null,"rdl:RDS7152045",null,"A <TWIN BEAM FLAME DETECTOR> is an <INSTRUMENTATION ITEM> and a <FLAME DETECTOR> which is utilizing twin beams",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLAME DETECTOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"ULTRAVIOLET FLAME DETECTOR",null,null,null,null,null,"rdl:RDS613169",null,"An <ULTRAVIOLET FLAME DETECTOR> is an <INSTRUMENTATION ITEM> and a <FLAME DETECTOR> that is designed to detect flame based on absorption of ultraviolet radiation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","VACUUM RELIEF DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"VACUUM RELIEF VALVE",null,null,null,null,null,"rdl:RDS6331685",null,"A <VACUUM RELIEF VALVE> is an <INSTRUMENTATION ITEM> and a <VACUUM RELIEF DEVICE> that is used for pressure compensation purposes by admitting (letting in) a pressure to prevent that vacuum is forming when filling or emptying a system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","VACUUM RELIEF DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"VACUUM SAFETY VALVE",null,null,null,null,null,"rdl:RDS646289",null,"A <VACUUM SAFETY VALVE> is an <INSTRUMENTATION ITEM> and a <VACUUM RELIEF DEVICE> that automatically releases excess pressure or admits pressure to prevent a vacuum",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DEW POINT ANALYSER","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"VAPOUR PRESSURE DEW POINT ANALYSER",null,null,null,null,null,"rdl:RDS1007954",null,"A <VAPOUR PRESSURE DEW POINT ANALYSER> is an <INSTRUMENTATION ITEM> and a <DEW POINT ANALYSER> that uses vapour pressure to determine a dew point",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOW GAUGE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"VARIABLE AREA FLOW INDICATOR",null,null,null,null,null,"rdl:RDS883529",null,"A <VARIABLE AREA FLOW INDICATOR> is an <INSTRUMENTATION ITEM> and a <FLOW GAUGE> where a weighted float rises in a tapered tube as the flow rate increases; the float stops rising when area between float and tube is large enough that the weight of the float is balanced by the drag of fluid flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACCELERATION MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"VELOCITY PICKUP",null,null,null,null,null,"rdl:RDS5480833728",null,"A <VELOCITY PICKUP> is an <INSTRUMENTATION ITEM> and a <VELOCITY MEASURING ELEMENT> that uses the principle set forth in ISO 2041",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","WEIGHT MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,"VIBRATING WIRE LOAD CELL",null,null,null,null,null,"rdl:RDS222604",null,"A <VIBRATING WIRE LOAD CELL> is an <INSTRUMENTATION ITEM> and a <WEIGHT MEASURING ELEMENT that measures force (a mechanical load) using a wire that vibrates at a high frequency. The applied external force changes the tension on the wire, this changes the frequency",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","OSCILLATOR","VIBRATION DETECTOR",null,null,null,null,null,null,null,null,null,null,null,"VIBRATION OSCILLATOR-DETECTOR",null,null,null,null,null,"rdl:RDS14206609",null,"A <VIBRATION OSCILLATOR-DETECTOR> is an <INSTRUMENTATION ITEM> and a <VIBRATION DETECTOR> and an <OSCILLATOR> that detects motion that can be translated into a signal which can be displayed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"VISCOMETER",null,null,null,null,null,"rdl:RDS5766901",null,"A <VISCOMETER>is a <PROCESS ANALYSER> for measuring the viscosity of liquids",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"VISCOSITY ANALYSER",null,null,null,null,null,"rdl:RDS6466659",null,"A <VISCOSITY ANALYSER>is a <PROCESS ANALYSER> intended to determine the viscosity of a fluid",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE TO CURRENT SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS851174",null,"A <VOLTAGE TO CURRENTL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended for converting an input voltage signal into a current output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE TO PRESSURE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS851309",null,"A <VOLTAGE TO PRESSUREL SIGNAL CONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended for converting a voltage input signal into proportional linear pneumatic output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","SIGNAL CONVERTER",null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE TO VOLTAGE SIGNAL CONVERTER",null,null,null,null,null,"rdl:RDS5762939",null,"A <VOLTAGE TO VOLTAGEL SIGNALCONVERTER> is an <INSTRUMENTATION ITEM> and a <SIGNAL CONVERTER> that is intended for converting a voltage input signal to a voltage output signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOW MEASURING ELEMENT","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS222510",null,"A <VOLUME FLOW MEASURING ELEMENT> is an <INSTRUMENTATION ITEM> and a <FLOW MEASURING ELEMENT> that is used to measure <VOLUME FLOW RATE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - POSITIVE DISPLACEMENT",null,null,null,null,null,"rdl:RDS418094",null,"A <VOLUME FLOW MEASURING ELEMENT - POSITIVE DISPLACEMENT> is a <VOLUME FLOW MEASURING ELEMENT> that measures the volumetric flow rate of a liquid or gas by separating the flow stream into known volumes and counting them over time",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - POSITIVE DISPLACEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - GEAR",null,null,null,null,null,"rdl:RDS222528",null,"A <VOLUME FLOW MEASURING ELEMENT - GEAR> is a <VOLUME FLOW MEASURING ELEMENT - POSITIVE DISPLACEMENT> that uses gears to divide and meter the flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - GEAR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - HELICAL GEAR",null,null,null,null,null,"rdl:RDS222529",null,"A <VOLUME FLOW MEASURING ELEMENT - HELICAL GEAR> is a <VOLUME FLOW MEASURING ELEMENT - GEAR> that is a flow meter that gets its name from the shape of its gears or rotors. These rotors resemble the shape of a helix, which is a spiral-shaped structure. As the fluid flows through the meter, it enters the compartments in the rotors, causing the rotors to rotate. Flowrate is calculated from the speed of rotation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - GEAR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - OVAL GEAR",null,null,null,null,null,"rdl:RDS880424",null,"A <VOLUME FLOW MEASURING ELEMENT - OVAL GEAR> is a <VOLUME FLOW MEASURING ELEMENT - GEAR> that is a positive displacement meter that uses two or more oblong gears configured to rotate at right angles to one another, forming a T shape",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - POSITIVE DISPLACEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - HELIX",null,null,null,null,null,"rdl:RDS222530",null,"A <VOLUME FLOW MEASURING ELEMENT - HELIX> is a <VOLUME FLOW MEASURING ELEMENT - POSITIVE DISPLACEMENT> that is a type of turbine flow meter that comprises a rotor with helical blades inserted axially in the flow, much like a ducted fan",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - POSITIVE DISPLACEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - ROTARY",null,null,null,null,null,"rdl:RDS222531",null,"A <VOLUME FLOW MEASURING ELEMENT - ROTARY> is a <VOLUME FLOW MEASURING ELEMENT - POSITIVE DISPLACEMENT> that uses eccentrically mounted drums to divide and meter the flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - POSITIVE DISPLACEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - NUTATING DISC",null,null,null,null,null,"rdl:RDS881819",null,"A <VOLUME FLOW MEASURING ELEMENT - NUTATING DISC> is a <VOLUME FLOW MEASURING ELEMENT - POSITIVE DISPLACEMENT> that uses a disk which fits closely in a measuring chamber. As the fluid enters one side of the partition and leaves through the other side, it makes the disk to wobble. The number of revolutions made by a small shaft attached to the disk will indicate the volume of flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - POSITIVE DISPLACEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - PISTON",null,null,null,null,null,"rdl:RDS812114",null,"A <VOLUME FLOW MEASURING ELEMENT - PISTON> is a <VOLUME FLOW MEASURING ELEMENT - POSITIVE DISPLACEMENT> that is utilizing a piston closely fitted into a cylindrical chamber with a pair of slots that are progressively uncovered as the pressure differential makes the piston oscillate/spin around a control roller in the centre of the chamber",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - FORCE-BALANCE",null,null,null,null,null,"rdl:RDS222516",null,"A <VOLUME FLOW MEASURING ELEMENT - FORCE-BALANCE> is a <VOLUME FLOW MEASURING ELEMENT> that measures the force exerted by a fluid in order to calculate its flow rate",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - FORCE-BALANCE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - IMPACT",null,null,null,null,null,"rdl:RDS222517",null,"A <VOLUME FLOW MEASURING ELEMENT - IMPACT> is a <VOLUME FLOW MEASURING ELEMENT - FORCE-BALANCE> that measures the impact force of a fluid on a plate and outputs a signal representative of flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - FORCE-BALANCE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - TARGET",null,null,null,null,null,"rdl:RDS222518",null,"A <VOLUME FLOW MEASURING ELEMENT - TARGET> is a <VOLUME FLOW MEASURING ELEMENT - FORCE-BALANCE> that uses a target, with force bar, as MEASURING ELEMENT",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - FORCE-BALANCE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - VANE",null,null,null,null,null,"rdl:RDS222519",null,"A <VOLUME FLOW MEASURING ELEMENT - VANE> is a <VOLUME FLOW MEASURING ELEMENT - FORCE-BALANCE> that uses one or more vanes in a measuring chamber to measure flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - VARIABLE AREA",null,null,null,null,null,"rdl:RDS222515",null,"A <VOLUME FLOW MEASURING ELEMENT - VARIABLE AREA> is a <VOLUME FLOW MEASURING ELEMENT> that measures fluid flow by allowing the cross sectional area of the device to vary in response to the flow, causing some measurable effect that indicates the rate",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VARIABLE AREA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOAT COLLAR",null,null,null,null,null,"rdl:RDS5786112",null,"A <FLOAT COLLAR> is a <VOLUME FLOW MEASURING ELEMENT - VARIABLE AREA> that is a specially formed float for use in variable area flow meters and variable area flow indicators that has a collar or flange on the top",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VARIABLE AREA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - ROTAMETER",null,null,null,null,null,"rdl:RDS882719",null,"A <VOLUME FLOW MEASURING ELEMENT - ROTAMETER> is a <VOLUME FLOW MEASURING ELEMENT - VARIABLE AREA> that consists of a tapered tube, typically made of glass, with a float inside that is pushed up by fluid flow and pulled down by gravity. As flow rate increases, greater viscous and pressure forces on the float cause it to rise until it becomes stationary at a location in the tube that is wide enough for the forces to balance",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,"rdl:RDS222532",null,"A <VOLUME FLOW MEASURING ELEMENT - VELOCITY> is a <VOLUME FLOW MEASURING ELEMENT> that measures the velocity of a fluid in order to calculate its flow rate",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - ACOUSTIC DOPPLER",null,null,null,null,null,"rdl:RDS222533",null,"A <VOLUME FLOW MEASURING ELEMENT - ACOUSTIC DOPPLER> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> measuring the velocity of particles in a remote sampling volume based upon the Doppler shift effect; records velocity components at a single point with a relatively high frequency",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - ELECTROMAGNETIC",null,null,null,null,null,"rdl:RDS1009664",null,"A <VOLUME FLOW MEASURING ELEMENT - ELECTROMAGNETIC> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> that uses a magnetic field applied to the metering tube, which results in a potential difference proportional to the flow velocity perpendicular to the flux lines. The potential difference is sensed by electrodes aligned perpendicular to the flow and the applied magnetic field. The physical principle at work is Faraday&amp;#39;s law of electromagnetic induction. The magnetic flow meter requires a conducting fluid and a nonconducting pipe liner",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - LASER DOPPLER",null,null,null,null,null,"rdl:RDS222535",null,"A <VOLUME FLOW MEASURING ELEMENT - LASER DOPPLER> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> that uses a beam of laser light impinging on a moving particle; the light will be partially scattered with a change in wavelength proportional to the particles speed (the Doppler effect)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - MULTIPLE JET",null,null,null,null,null,"rdl:RDS222536",null,"A <VOLUME FLOW MEASURING ELEMENT - MULTIPLE JET> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> that is a velocity type meter that has an impeller that rotates horizontally on a vertical shaft. The impeller element is in a housing in which multiple inlet ports direct the fluid flow at the impeller causing it to rotate in a specific direction in proportion to the flow velocity. This meter works mechanically much like a single jet meter except that the ports direct the flow at the impeller equally from several points around the circumference of the element, not just one point; this minimizes uneven wear on the impeller and its shaft",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - OPTICAL",null,null,null,null,null,"rdl:RDS222537",null,"A <VOLUME FLOW MEASURING ELEMENT - OPTICAL> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> that is a flow meter that uses light to determine flow rate. Small particles which accompany natural and industrial gases pass through two laser beams focused a short distance apart in the flow path. Laser light is scattered when a particle crosses the first beam. The detecting optics collects scattered light on a photodetector, which then generates a pulse signal. As the same particle crosses the second beam, the detecting optics collect scattered light on a second photodetector, which converts the incoming light into a second electrical pulse. By measuring the time interval between these pulses, the gas velocity is calculated",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT",null,null,null,null,null,"rdl:RDS222540",null,"A <VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> that uses the rotation of a shaped element to measure flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - PADDLE INSERTION",null,null,null,null,null,"rdl:RDS222541",null,"A <VOLUME FLOW MEASURING ELEMENT - PADDLE INSERTION> is a <VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT> that uses the rotation of a paddle wheel to measure flow at a point inside the process",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - PROPELLER",null,null,null,null,null,"rdl:RDS222542",null,"A <VOLUME FLOW MEASURING ELEMENT - PROPELLER> is a <VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT> that uses the rotation of a propeller to measure flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - RADIAL TURBINE",null,null,null,null,null,"rdl:RDS222543",null,"A <VOLUME FLOW MEASURING ELEMENT - RADIAL TURBINE> is a <VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT> where a Pelton wheel rotates in the liquid flow around an axis into a user-readable rate of flow. The Pelton wheel tends to have all the flow traveling around it with the inlet flow focused on the blades by a jet",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - ROTATING VANE",null,null,null,null,null,"rdl:RDS222544",null,"A <VOLUME FLOW MEASURING ELEMENT - ROTATING VANE> is a <VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT> that uses the rotation of a vane to measure flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - TURBINE",null,null,null,null,null,"rdl:RDS417914",null,"A <VOLUME FLOW MEASURING ELEMENT - TURBINE> is a <VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT> that translates the mechanical action of the turbine rotating in the liquid flow around an axis into a user-readable rate of flow (gpm, lpm, etc.). The turbine tends to have all the flow traveling around it. The turbine wheel is set in the path of a fluid stream",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - PADDLE WHEEL",null,null,null,null,null,"rdl:RDS882809",null,"A <VOLUME FLOW MEASURING ELEMENT - PADDLE WHEEL> is a <VOLUME FLOW MEASURING ELEMENT - ROTATING ELEMENT> that consists of an impeller is small with respect to the width of the pipe, and projects only partially into the flow, like the paddle wheel",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - SINGLE JET",null,null,null,null,null,"rdl:RDS222539",null,"A <VOLUME FLOW MEASURING ELEMENT - SINGLE JET> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> that consists of an impeller with radial vanes, impinged upon by a single jet",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - SWIRL",null,null,null,null,null,"rdl:RDS222545",null,"A <VOLUME FLOW MEASURING ELEMENT - SWIRL> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> that uses swirls generated by fixed spiral vanes to measure flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - ULTRASONIC DOPPLER",null,null,null,null,null,"rdl:RDS1009799",null,"A <VOLUME FLOW MEASURING ELEMENT - ULTRASONIC DOPPLER> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> that measures the Doppler shift resulting from reflecting an ultrasonic beam off the particulates in flowing fluid. The frequency of the transmitted beam is affected by the movement of the particles; this frequency shift can be used to calculate the fluid velocity. For the Doppler principle to work there must be a high enough density of sonically reflective materials such as solid particles or air bubbles suspended in the fluid",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - VORTEX",null,null,null,null,null,"rdl:RDS418184",null,"A <VOLUME FLOW MEASURING ELEMENT - VORTEX> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> that involves placing a bluff body (called a shedder bar) in the path of the fluid. As the fluid passes this bar, disturbances in the flow called vortices are created. The vortices trail behind the cylinder, alternatively from each side of the bluff body. The frequency at which these vortices alternate sides is essentially proportional to the flow rate of the fluid. Inside, atop, or downstream of the shedder bar is a sensor for measuring the frequency of the vortex shedding. This sensor is often a piezoelectric crystal, which produces a small, but measurable, voltage pulse every time a vortex is created. Since the frequency of such a voltage pulse is also proportional to the fluid velocity, a volumetric flow rate is calculated using the cross sectional area of the flow meter",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - ULTRASONIC TRANSIT TIME",null,null,null,null,null,"rdl:RDS418139",null,"A <VOLUME FLOW MEASURING ELEMENT - ULTRASONIC TRANSIT TIME> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> that measures the difference of the transit time of ultrasonic pulses propagating in and against the direction of flow. This time difference is a measure for the average velocity of the fluid along the path of the ultrasonic beam",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - ULTRASONIC TRANSIT TIME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TIME OF FLIGHT ULTRASONIC FLOW METER",null,null,null,null,null,"rdl:RDS883349",null,"A <TIME OF FLIGHT ULTRASONIC FLOW METER> is an <ULTRASONIC FLOW METER> that use the time for the sound to travel between <A TRANSMITTER> and a receiver to measure a flow rate",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - ELECTROMAGNETIC INSERTION",null,null,null,null,null,"rdl:RDS222534",null,"A <VOLUME FLOW MEASURING ELEMENT - ELECTROMAGNETIC INSERTION> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> that uses electromagnetic principles to measure flow at a point inside the process",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - ANEMOMETRIC",null,null,null,null,null,"rdl:RDS5773048",null,"A <VOLUME FLOW MEASURING ELEMENT - ANEMOMETRIC> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> that can be the sensing element of an ANEMOMETER or wind gauge",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - ULTRASONIC IN-LINE",null,null,null,null,null,"rdl:RDS880559",null,"A <VOLUME FLOW MEASURING ELEMENT - ULTRASONIC IN-LINE> is a <VOLUME FLOW MEASURING ELEMENT - VELOCITY> that is mounted in-line with a pipeline",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - LEVEL-TO-FLOW OPEN CHANNEL",null,null,null,null,null,"rdl:RDS222520",null,"A <VOLUME FLOW MEASURING ELEMENT - LEVEL-TO-FLOW OPEN CHANNEL> is a <VOLUME FLOW MEASURING ELEMENT< where behind a <WEIR> or in a <FLUME> the level of the water is measured at a designated point in a hydraulic structure using various secondary devices (bubblers, ultrasonic, float, and differential pressure are common methods). This level is converted to a flow rate",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - LEVEL-TO-FLOW OPEN CHANNEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - CURRENT",null,null,null,null,null,"rdl:RDS222521",null,"A <VOLUME FLOW MEASURING ELEMENT - CURRENT> is a <VOLUME FLOW MEASURING ELEMENT - LEVEL-TO-FLOW OPEN> CHANNEL that where a propeller is traversed over the area of a channel and velocities averaged to calculate total flow. This may be on the order of hundreds of cubic meters per second. The flow must be kept steady during the traverse of the current meters. Methods for testing hydroelectric turbines are given in IEC standard 60041",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - LEVEL-TO-FLOW OPEN CHANNEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - FLUME",null,null,null,null,null,"rdl:RDS222522",null,"A <VOLUME FLOW MEASURING ELEMENT - FLUME> is a <VOLUME FLOW MEASURING ELEMENT - LEVEL-TO-FLOW OPEN> CHANNEL that is a specially shaped, fixed hydraulic structure that under free-flow conditions forces flow to accelerate in such a manner that the flow rate through the flume can be characterized by a level-to-flow relationship as applied to a single head (level) measurement within the flume. Acceleration is accomplished through a convergence of the sidewalls, a change in floor elevation, or a combination of the two",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - LEVEL-TO-FLOW OPEN CHANNEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - WEIR",null,null,null,null,null,"rdl:RDS222524",null,"A <VOLUME FLOW MEASURING ELEMENT - WEIR> is a <VOLUME FLOW MEASURING ELEMENT - LEVEL-TO-FLOW OPEN> CHANNEL that is an obstruction in the flow path in an open channel. The weir will cause an increase in the water depth as the water flows over the weir. In general, the greater the flow rate, the greater will be the increase in depth of flow, The height of water above the top of the weir is the measurement usually used to correlate with flow rate",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - WEIR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - BROAD-CRESTED WEIR",null,null,null,null,null,"rdl:RDS222525",null,"A <VOLUME FLOW MEASURING ELEMENT - BROAD-CRESTED WEIR> is a <VOLUME FLOW MEASURING ELEMENT - WEIR> that is a flat-crested structure, with a long crest compared to the flow thickness",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - WEIR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - SHARP-CRESTED WEIR",null,null,null,null,null,"rdl:RDS222526",null,"A <VOLUME FLOW MEASURING ELEMENT - SHARP-CRESTED WEIR> is a <VOLUME FLOW MEASURING ELEMENT - WEIR> that is allowing the fluid to fall cleanly away from the weir. Sharp crested weirs are typically 1/4 inch or thinner metal plates",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - WEIR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - V-NOTCH WEIR",null,null,null,null,null,"rdl:RDS222527",null,"A <VOLUME FLOW MEASURING ELEMENT - V-NOTCH WEIR> is a <VOLUME FLOW MEASURING ELEMENT - WEIR> that is a triangular channel section, used to measure small discharge values. The upper edge of the section is always above the water level, so the channel is always triangular simplifying calculation of the cross-sectional area",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - LEVEL-TO-FLOW OPEN CHANNEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - AREA-VELOCITY",null,null,null,null,null,"rdl:RDS881864",null,"A <VOLUME FLOW MEASURING ELEMENT - AREA-VELOCITY> is a <VOLUME FLOW MEASURING ELEMENT - LEVEL-TO-FLOW OPEN> CHANNEL that calculates flow in an open channel by measuring the level to determine the cross section, and it measures the fluid velocity; subequently these two values are multiplied to arrive at the <VOLUME FLOW RATE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - AREA-VELOCITY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WEIR FLOW METER",null,null,null,null,null,"rdl:RDS883754",null,"A <WEIR FLOW METER> is an <OPEN CHANNEL FLOW METER> utilizing some kind of weir as obstruction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE",null,null,null,null,null,"rdl:RDS222511",null,"A <VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE> is a <VOLUME FLOW MEASURING ELEMENT> that measures the differential pressure across a MEASURING ELEMENT in order to measure flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ORIFICE PLATE",null,null,null,null,null,"rdl:RDS418364",null,"An <ORIFICE PLATE> is a <VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE> that is a plate with a hole through it, placed in the flow; it constricts the flow, and measuring the pressure differential across the constriction gives the flow rate. It is basically a crude form of Venturi meter, but with higher energy losses. There are three type of orifice: concentric, eccentric, and segmental",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONCENTRIC HOLE ORIFICE PLATE",null,null,null,null,null,"rdl:RDS7199620",null,"A <CONCENTRIC HOLE ORIFICE PLATE> is an <ORIFICE PLATE> with a circular orifice that is coaxial with the conduit and is concentric to the conduit axis",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONCENTRIC HOLE ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONICAL CONCENTRIC ORIFICE PLATE",null,null,null,null,null,"rdl:RDS7199744",null,"A <CONICAL CONCENTRIC ORIFICE PLATE> is a <CONCENTRIC HOLE ORIFICE PLATE> of which the orifice is conical",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONCENTRIC HOLE ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CYLINDRICAL CONCENTRIC ORIFICE PLATE",null,null,null,null,null,"rdl:RDS7200382",null,"A <CYLINDRICAL CONCENTRIC ORIFICE PLATE> is a <CONCENTRIC HOLE ORIFICE PLATE> of which the orifice is cylindrical",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONCENTRIC HOLE ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"QUARTER-CIRCLE CONCENTRIC ORIFICE PLATE",null,null,null,null,null,"rdl:RDS7200320",null,"A <QUARTER-CIRCLE CONCENTRIC ORIFICE PLATE> is a <CONCENTRIC HOLE ORIFICE PLATE> of which the orifice is a quarter of the circumference of a circle",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONCENTRIC HOLE ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SQUARE-EDGED CONCENTRIC ORIFICE PLATE",null,null,null,null,null,"rdl:RDS7199682",null,"A <SQUARE-EDGED CONCENTRIC ORIFICE PLATE> is a <CONCENTRIC HOLE ORIFICE PLATE> of which the orifice is square-shaped",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECCENTRIC HOLE ORIFICE PLATE",null,null,null,null,null,"rdl:RDS7199806",null,"An <ECCENTRIC HOLE ORIFICE PLATE> is an <ORIFICE PLATE> with an orifice that is circular and coaxial with the conduit, but eccentric to the conduit axis",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PADDLE ORIFICE PLATE",null,null,null,null,null,"rdl:RDS6759480",null,"A <PADDLE ORIFICE PLATE> is an <ORIFICE PLATE> with an integrated paddle or handle to facilitate installation between flanges",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PADDLE ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRAL PADDLE ORIFICE PLATE",null,null,null,null,null,"rdl:RDS7211344",null,"An <INTEGRAL PADDLE ORIFICE PLATE> is a <PADDLE ORIFICE PLATE> that is made from one piece",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PADDLE ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WELDED PADDLE ORIFICE PLATE",null,null,null,null,null,"rdl:RDS7211282",null,"A <WELDED PADDLE ORIFICE PLATE> is a <PADDLE ORIFICE PLATE> where the orifce plate and the paddle (handle) is assembled through welding",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"QUARTER CIRCLE ORIFICE PLATE",null,null,null,null,null,"rdl:RDS7022320",null,"A <QUARTER CIRCLE ORIFICE PLATE> is an <ORIFICE PLATE> with an orifice that has the shape of a quarter circle",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESTRICTION ORIFICE",null,null,null,null,null,"rdl:RDS882629",null,"A <RESTRICTION ORIFICE> is an <ORIFICE PLATE> that is intended for use as a restrictor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RESTRICTION ORIFICE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTI-HOLE RESTRICTION ORIFICE",null,null,null,null,null,"rdl:RDS1465077151",null,"A <MULTI-HOLE RESTRICTION ORIFICE> is a <RESTRICTION ORIFICE> with more than one hole",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RESTRICTION ORIFICE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE-HOLE RESTRICTION ORIFICE",null,null,null,null,null,"rdl:RDS1465078021",null,"A <SINGLE-HOLE RESTRICTION ORIFICE> is a <RESTRICTION ORIFICE PLATE> with one hole",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEAL ORIFICE",null,null,null,null,null,"rdl:RDS7042877",null,"A <SEAL ORIFICE> is an <ORIFICE PLATE> intended to limit the flow of seal flush to the seal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEGMENTAL ORIFICE PLATE",null,null,null,null,null,"rdl:RDS7199868",null,"A <SEGMENTAL ORIFICE PLATE> is an <ORIFICE PLATE> with an orifice that has the form of a segment of a circle",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEGMENTAL ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEGMENTAL ORIFICE PLATE FOR DIRTY GAS",null,null,null,null,null,"rdl:RDS7199960",null,"A <SEGMENTAL ORIFICE PLATE FOR DIRTY GAS> is a <SEGMENTAL ORIFICE PLATE> that is in the form of a segment of a circle, the cord of which is vertical. The hole is tangential to the side of the conduit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEGMENTAL ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEGMENTAL ORIFICE PLATE FOR DIRTY LIQUID",null,null,null,null,null,"rdl:RDS7200022",null,"A <SEGMENTAL ORIFICE PLATE FOR DIRTY LIQUID> is a <SEGMENTAL ORIFICE PLATE> that is in the form of a segment of a circle, the cord of which is horizontal. The hole is tangential to the bottom of the conduit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ORIFICE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UNIVERSAL TYPE ORIFICE PLATE",null,null,null,null,null,"rdl:RDS6759638",null,"A <UNIVERSAL TYPE ORIFICE PLATE> is an <ORIFICE PLATE> with a circular design that is fit for use in orifice fittings or in the plate holders of ring-type joint (RTJ) orifice flanges",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VENTURI TUBE ASSEMBLY",null,null,null,null,null,"rdl:RDS7940784",null,"A <VENTURI TUBE ASSEMBLY> is a <VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE> that is an assembly of a venturi tube, flow straightener and meter tube as its main components",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - CONE",null,null,null,null,null,"rdl:RDS222512",null,"A <VOLUME FLOW MEASURING ELEMENT - CONE> is a <VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE> that works with the same basic principles as Venturi and Orifice type DP meters, but don&amp;#226;&#226;â€š&#172;&#226;â€ž&#162;t require the same upstream and downstream piping. The cone acts as a conditioning device as well as a differential pressure producer",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - PITOT TUBE",null,null,null,null,null,"rdl:RDS418274",null,"A <VOLUME FLOW MEASURING ELEMENT - PITOT TUBE> is a <VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE> that is a pressure measuring device used to measure fluid flow velocity by determining the stagnation pressure and static pressure. Bernoulli&amp;amp;amp;amp;#39;s equation used to calculate the dynamic pressure and hence fluid velocity",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - PITOT TUBE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTIPORT PITOT TUBE",null,null,null,null,null,"rdl:RDS418319",null,"A <MULTIPORT PITOT TUBE> is a <VOLUME FLOW MEASURING ELEMENT - PITOT TUBE> that has multiple impact pressure ports normal to the flow direction on the exterior tube",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - SEGMENTAL WEDGE",null,null,null,null,null,"rdl:RDS222513",null,"A <VOLUME FLOW MEASURING ELEMENT - SEGMENTAL WEDGE> is a <VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE> that consists of a cylindrical pressure vessel into which a constriction is fabricated thereby leaving an open segment of a known height. Pressure taps on either side of the wedge provide the differential signal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - V-CONE",null,null,null,null,null,"rdl:RDS222514",null,"A <VOLUME FLOW MEASURING ELEMENT - V-CONE> is a <VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE> that uses a conical body as MEASURING ELEMENT",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - DALL TUBE",null,null,null,null,null,"rdl:RDS7023655",null,"A <VOLUME FLOW MEASURING ELEMENT - DALL TUBE> is a <VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE> that is a shortened version of a Venturi meter, with a lower pressure drop than an orifice plate. As with these flow meters the flow rate in a Dall tube is determined by measuring the pressure drop caused by restriction in the conduit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLUME FLOW MEASURING ELEMENT - VENTURI TUBE",null,null,null,null,null,"rdl:RDS648044",null,"A <VOLUME FLOW MEASURING ELEMENT - VENTURI TUBE> is a <VOLUME FLOW MEASURING ELEMENT - DIFFERENTIAL PRESSURE> that constricts the flow in some fashion, and pressure sensors measure the differential pressure before and within the constriction. This method is widely used to measure flow rate in the transmission of gas through pipelines",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"WATER FRACTION METER",null,null,null,null,null,"rdl:RDS16553283",null,"A <WATER FRACTION METER>is a <PROCESS ANALYSER> designed to measure the water fraction in a fluid",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"WET GAS METER",null,null,null,null,null,"rdl:RDS16553328",null,"A <WET GAS METER>is a <PROCESS ANALYSER> that measures the amount of liquid, i.e. condensate and water in a gas",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","TEMPERATURE DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,"WINDING TEMPERATURE DETECTOR",null,null,null,null,null,"rdl:RDS17820411",null,"A <WINDING TEMPERATURE DETECTOR> is an <INSTRUMENTATION ITEM> and a <TEMPERATURE DETECTOR that is designed to measure the temperature in a stator winding",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,"WOBBE INDEX METER",null,null,null,null,null,"rdl:RDS1008134",null,"A <WOBBE INDEX METER>is a <PROCESS ANALYSER> intended to determine the wobbe index of a gas or gas mixture",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"XY RECORDER",null,null,null,null,null,"rdl:RDS914984",null,"A <XY RECORDER> is an <INSTRUMENTATION ITEM> and a <RECORDER> in which a marking device is moved along two orthogonal axes by two separate travelling devices, to each of which the quantity to be recorded is applied",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION FUNCTION","SYSTEM",null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENTATION SYSTEM",null,null,null,null,null,"rdl:RDS222491",null,"An <INSTRUMENTATION SYSTEM> is a <INSTRUMENTATION FUNCTION> and a <SYSTEM>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","INSTRUMENTATION SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,"CONTROL MODULE",null,null,null,null,null,"rdl:RDS5773641",null,"A <CONTROL MODULE> is an <ARTEFACT> and a <INSTRUMENTATION SYSTEM> where the control and process functions are housed in a special container",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,"MEASURING FUNCTION",null,null,null,null,null,"rdl:RDS1415826371",null,"A <MEASURING FUNCTION> is an <INSTRUMENTATION FUNCTION> that is capable of <MEASURING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING FUNCTION","PROCESS SIGNAL GENERATING FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,"DETECTOR",null,null,null,null,null,"rdl:RDS17604520",null,"A <DETECTOR> is an <MEASURING FUNCTION> and a <PROCESS SIGNAL GENERATING FUNCTION> that is capable of <DETECTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"ASPIRATED DETECTOR",null,null,null,null,null,"rdl:RDS1317199411",null,"An <ASPIRATED DETECTOR> is an <ARTEFACT> and a <DETECTOR> that incorporates a device to draw or force exterior ambient atmosphere into the detector",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC VARIABLE DETECTOR",null,null,null,null,null,"rdl:RDS2223219",null,"An <ELECTRIC VARIABLE DETECTOR> is a <DETECTOR> using an <ELECTRIC VARIABLE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTH LEAKAGE DETECTOR",null,null,null,null,null,"rdl:RDS916829",null,"An <EARTH LEAKAGE DETECTOR> is an <ELECTRIC VARIABLE DETECTOR> using an <EARTH LEAKAGE MEASURING ELEMENT> for detecting a leakage <CURRENT> to earth",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSULATION FAULT DETECTOR",null,null,null,null,null,"rdl:RDS916784",null,"An <INSULATION FAULT DETECTOR> is an <ELECTRIC VARIABLE DETECTOR> using an <INSULATION FAULT MEASURING ELEMENT> for detecting faults in electrical insulation",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE DETECTOR",null,null,null,null,null,"rdl:RDS1336298951",null,"A <VOLTAGE DETECTOR> is an <ELECTRIC VARIABLE DETECTOR> using a <VOLTAGE MEASURING ELEMENT> that is designed to detect the presence of an <ELECTRIC POTENTIAL>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EROSION DETECTOR",null,null,null,null,null,"rdl:RDS2223220",null,"An <EROSION DETECTOR> is a <DETECTOR> using an <EROSION PROBE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLAME DETECTOR",null,null,null,null,null,"rdl:RDS477044",null,"A <FLAME DETECTOR> is a <DETECTOR> using a <FLAME DETECTING MEASURING ELEMENT> that is designed to detect the presence of a flame",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW DETECTOR",null,null,null,null,null,"rdl:RDS1008719",null,"A <FLOW DETECTOR> is a <DETECTOR> using a <FLOW MEASURING ELEMENT> that is designed to detect whether a fluid flow exists",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLUID LEAK DETECTOR",null,null,null,null,null,"rdl:RDS880604",null,"A <FLUID LEAK DETECTOR> is a <DETECTOR> using a <FLUID LEAK DETECTION MEASURING ELEMENT> designed to detect fluid leaks",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS DETECTOR",null,null,null,null,null,"rdl:RDS2223230",null,"A <GAS DETECTOR> is a <DETECTOR> using a <GAS DETECTING MEASURING ELEMENT> that is intended to sense the presence of a specified concentration of a gas",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HEAT DETECTOR",null,null,null,null,null,"rdl:RDS477089",null,"A <HEAT DETECTOR> is a <DETECTOR> using a <HEAT DETECTING MEASURING ELEMENT> that is a fire alarm device designed to respond when the convected thermal energy of a fire increases the temperature of a heat sensitive element. The thermal mass and conductivity of the element regulate the rate flow of heat into the element. All heat detectors have this thermal lag. (source: Wikipedia)",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HUMIDITY DETECTOR",null,null,null,null,null,"rdl:RDS880469",null,"A <HUMIDITY DETECTOR> is a<DETECTOR> using a <HUMIDITY MEASURING ELEMENT> that is intended to detect ambient humidity",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL DETECTOR",null,null,null,null,null,"rdl:RDS7920754",null,"A <LEVEL DETECTOR> is a<DETECTOR> using a <LEVEL MEASURING ELEMENT> that is intended to detect that a level exceeds a preset value",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIST DETECTOR",null,null,null,null,null,"rdl:RDS2223221",null,"A <MIST DETECTOR> is a <DETECTOR> using a <MIST DETECTION MEASURING ELEMENT> for the detection of a mist",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOISTURE DETECTOR",null,null,null,null,null,"rdl:RDS1008944",null,"A <MOISTURE DETECTOR> is a <DETECTOR> using a <MOISTURE SENSING ELEMENT> for the detection of moisture",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OIL-IN-WATER DETECTOR",null,null,null,null,null,"rdl:RDS1008809",null,"An <OIL-IN-WATER DETECTOR> is a <DETECTOR> using an <ANALYSIS MEASURING ELEMENT> for detection of hydrocarbons in water",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PIG DETECTOR",null,null,null,null,null,"rdl:RDS416249",null,"A <PIG INDICATOR> is a <DETECTOR> using a <PROXIMITY MEASURING ELEMENT> that is showing when/if the <PIG> is inside a <PIG RECEIVER>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POSITION DETECTOR",null,null,null,null,null,"rdl:RDS1009034",null,"A <POSITION DETECTOR> is a <DETECTOR> using a <POSITION MEASURING ELEMENT> for the detection of a particular physical <POSITION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAND DETECTOR",null,null,null,null,null,"rdl:RDS850724",null,"A <SAND DETECTOR> is a <DETECTOR> using a <SAND DETECTION MEASURING ELEMENT> that is intended to detect sand in a liquid",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SMOKE DETECTOR",null,null,null,null,null,"rdl:RDS476999",null,"An <SMOKE DETECTOR> is a <DETECTOR> using a <SMOKE DETECTING MEASURING ELEMENT> typically as an indication of fire",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE DETECTOR",null,null,null,null,null,"rdl:RDS2220080",null,"A <TEMPERATURE DETECTOR> is a <DETECTOR> using a <TEMPERATURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VIBRATION DETECTOR",null,null,null,null,null,"rdl:RDS850769",null,"A <VIBRATION DETECTOR> is a <DETECTOR> using a <VIBRATION MEASURING ELEMENT> that is intended to detect the level of <VIBRATION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"DETECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WATER HARDNESS DETECTOR",null,null,null,null,null,"rdl:RDS6501054",null,"A <WATER HARDNESS DETECTOR> is a <DETECTOR> using a <WATER HARDNESS MEASURING ELEMENT> that is intended to detect a preset hardness of <WATER>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS222444",null,"A <MEASURING ELEMENT> is a <MEASURING FUNCTION> used for the measurement of a <Property>. It is defined independently from any other <INSTRUMENTATION DEVICE> that is handling that measurement result and that may or may not house that <MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACCELERATION MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS222500",null,"An <ACCELERATION MEASURING ELEMENT> is a <MEASURING ELEMENT> for <ACCELERATION> measurement",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANALYSIS MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS222501",null,"An <ANALYSIS MEASURING ELEMENT> is a <MEASURING ELEMENT> for <ANALYSIS> purposes",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANALYSIS MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUTE HUMIDITY PROBE",null,null,null,null,null,"rdl:RDS222504",null,"An <ABSOLUTE HUMIDITY PROBE> is an <ANALYSIS MEASURING ELEMENT> for measurement of <ABSOLUTE HUMIDITY>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANALYSIS MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONDUCTIVITY CELL",null,null,null,null,null,"rdl:RDS5770462",null,"An <CONDUCTIVITY CELL> is an <ANALYSIS MEASURING ELEMENT> for measurement of <CONDUCTIVITY>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANALYSIS MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CORROSION PROBE",null,null,null,null,null,"rdl:RDS648179",null,"A <CORROSION PROBE> is an <ANALYSIS MEASURING ELEMENT> that is a piece of suitable metal meant to corrode and give an indication of the corrosion rate",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANALYSIS MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KNOCK SENSOR",null,null,null,null,null,"rdl:RDS6466164",null,"A <KNOCK SENSOR> is an <ANALYSIS MEASURING ELEMENT> that is intended to detect engine knock in a combustion engine",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANALYSIS MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOISTURE SENSING ELEMENT",null,null,null,null,null,"rdl:RDS5772924",null,"A <MOISTURE SENSING ELEMENT> is an <ANALYSIS MEASURING ELEMENT> for measurement of <MOISTURE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANALYSIS MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PH ELECTRODE",null,null,null,null,null,"rdl:RDS222505",null,"A <PH ELECTRODE> is an <ANALYSIS MEASURING ELEMENT> that is an electrode that uses a specially formulated, pH sensitive glass in contact with the solution, that develops a potential (voltage) proportional to the pH of the solution",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANALYSIS MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RELATIVE HUMITITY PROBE",null,null,null,null,null,"rdl:RDS5772862",null,"A <RELATIVE HUMITITY PROBE> is an <ANALYSIS MEASURING ELEMENT> for measurement of <RELATIVE HUMITITY>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DISPLACEMENT MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS5480833840",null,"A <DISPLACEMENT MEASURING ELEMENT> is a <MEASURING ELEMENT> for measurement of <DISPLACEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DUST MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS1299047481",null,"A <DUST MEASURING ELEMENT> is a <MEASURING ELEMENT> for measuring the velocity, mass, charge, flight direction, and number of dust particles in space",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC VARIABLE MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS222506",null,"An <ELECTRIC VARIABLE MEASURING ELEMENT> is a <MEASURING ELEMENT> for measurement of <ELECTRIC VARIABLE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS222507",null,"A <CURRENT MEASURING ELEMENT> is an <ELECTRIC VARIABLE MEASURING ELEMENT> for measurement of <CURRENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTH LEAKAGE MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS2229115",null,"An <EARTH LEAKAGE MEASURING ELEMENT> is an <ELECTRIC VARIABLE MEASURING ELEMENT> for measurement of <EARTH LEAKAGE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FREQUENCY MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS2222222",null,"A <FREQUENCY MEASURING ELEMENT> is an <ELECTRIC VARIABLE MEASURING ELEMENT> for measurement of <FREQUENCY>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSULATION FAULT MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS2229116",null,"An <INSULATION FAULT MEASURING ELEMENT> is an <ELECTRIC VARIABLE MEASURING ELEMENT> for measurement of <INSULATION FAULT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER FACTOR MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS222508",null,"A <POWER FACTOR MEASURING ELEMENT> is an <ELECTRIC VARIABLE MEASURING ELEMENT> for measurement of <POWER FACTOR>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS1337135221",null,"A <POWER MEASURING ELEMENT> is an <ELECTRIC VARIABLE MEASURING ELEMENT> for measurement of <POWER>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESISTANCE MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS2222223",null,"A <RESISTANCE MEASURING ELEMENT> is an <ELECTRIC VARIABLE MEASURING ELEMENT> for measurement of <RESISTANCE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS1287147001",null,"A <VOLTAGE MEASURING ELEMENT> is an <ELECTRIC VARIABLE MEASURING ELEMENT> for measurement of <VOLTAGE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EROSION DETECTING MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS16757813",null,"An <EROSION DETECTING MEASURING ELEMENT> is a <MEASURING ELEMENT> that is designed to detect <EROSION>, e.g. caused by particles in a fluid",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIRE DETECTING MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS1008629",null,"A <FIRE DETECTING MEASURING ELEMENT> is a <MEASURING ELEMENT> for detecting a <FIRE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLAME DETECTING MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS2220149",null,"A <FLAME DETECTING MEASURING ELEMENT> is a <MEASURING ELEMENT> for detecting a <FLAME>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS461834",null,"A <FLOW MEASURING ELEMENT> is a <MEASURING ELEMENT> that is used to measure <FLOW RATE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLUID LEAK DETECTION MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS222552",null,"A <FLUID LEAK DETECTION MEASURING ELEMENT> is a <MEASURING ELEMENT> for the detection of a fluid leak",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FORCE MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS1337126251",null,"A <FORCE MEASURING ELEMENT> is a <MEASURING ELEMENT> for the measurement of <FORCE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS DETECTING MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS477134",null,"A <GAS DETECTING MEASURING ELEMENT> is a <MEASURING ELEMENT> for the detection of the presence of a specified concentration of a gas",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HEAT DETECTION MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS2229121",null,"A <HEAT DETECTION MEASURING ELEMENT> is a <MEASURING ELEMENT> for the detection of a rising heat",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HUMIDITY MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS2229123",null,"A <HUMIDITY MEASURING ELEMENT> is a <MEASURING ELEMENT> for the detection of a <HUMIDITY>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS880784",null,"A <LEVEL MEASURING ELEMENT> is a <MEASURING ELEMENT> for measuring a <LEVEL>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIST DETECTION MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS1008899",null,"A <MIST DETECTION MEASURING ELEMENT> is a <MEASURING ELEMENT> for the detection of a mist",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POSITION MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS222587",null,"A <POSITION MEASURING ELEMENT> is a <MEASURING ELEMENT> for the measurement of physical <POSITION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS462104",null,"A <PRESSURE MEASURING ELEMENT> is a <MEASURING ELEMENT> for the measurement of <PRESSURE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROXIMITY MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS850904",null,"A <PROXIMITY MEASURING ELEMENT> is a <MEASURING ELEMENT> for the measurement of <PROXIMITY>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIATION MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS1336333241",null,"A <RADIATION MEASURING ELEMENT> is a <MEASURING ELEMENT> for detecting the level of nuclear <RADIATION>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTATIONAL SPEED MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS5773110",null,"A <ROTATIONAL SPEED MEASURING ELEMENT> is a <MEASURING ELEMENT> for the measurement of <ROTATIONAL SPEED>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAND DETECTION MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS5781223",null,"A <SAND DETECTION MEASURING ELEMENT> is a <MEASURING ELEMENT> for sand detection in a pipeline",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SMOKE DETECTION MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS5781225",null,"A <SMOKE DETECTION MEASURING ELEMENT> is a <MEASURING ELEMENT> for the detection of smoke",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS445454",null,"A <TEMPERATURE MEASURING ELEMENT> is a <MEASURING ELEMENT> for the measurement of <TEMPERATURE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VELOCITY MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS54808340199",null,"A <VELOCITY MEASURING ELEMENT> is a <MEASURING ELEMENT> that is sensing velocity (vibration) conforming ISO2041",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VIBRATION MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS435959",null,"A <VIBRATION MEASURING ELEMENT> is a <MEASURING ELEMENT> that senses vibration",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WATER DETECTING MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS883709",null,"A <WATER DETECTING MEASURING ELEMENT> is a <MEASURING ELEMENT> that is designed to detect the presence of water and provide input to an alert to allow the prevention of water damage. A common design is a small cable or device that lies flat on a floor and relies on the electrical conductivity of water to decrease the resistance across two contacts",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WATER HARDNESS MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS2229120",null,"A <WATER HARDNESS MEASURING ELEMENT> is a <MEASURING ELEMENT> for the measurement of <HARDNESS> of <WATER>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WAVE HEIGHT SENSOR",null,null,null,null,null,"rdl:RDS1300144801",null,"A <WAVE HEIGHT SENSOR> is a <MEASURING ELEMENT> that senses wave hights and produces an output signal to represent the measured height",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WEIGHT MEASURING ELEMENT",null,null,null,null,null,"rdl:RDS222599",null,"A <WEIGHT MEASURING ELEMENT> is a <MEASURING ELEMENT> for the measurement of <WEIGHT> (mass)",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"MEASURING INSTRUMENT",null,null,null,null,null,"rdl:RDS2220105",null,"A <MEASURING INSTRUMENT> is a <MEASURING FUNCTION> that is a portable meter",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALIGNMENT INSTRUMENT",null,null,null,null,null,"rdl:RDS6569135",null,"An <ALIGNMENT INSTRUMENT> is a <MEASURING INSTRUMENT> that is intended to measure and indicate the position of equipment relative to each other",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANEMOMETER",null,null,null,null,null,"rdl:RDS6635693",null,"An <ANEMOMETER> is a <MEASURING INSTRUMENT> for recording wind speed and possibly wind direction",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,"rdl:RDS913904",null,"An <ELECTRIC VARIABLE METER> is a <MEASURING INSTRUMENT> intended to measure an electric variable",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AMPERE-HOUR METER",null,null,null,null,null,"rdl:RDS915524",null,"An <AMPERE-HOUR METER> is an <ELECTRIC VARIABLE METER> that is intended to measure a quantity of electricity by integrating current with respect to time",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTROMETER",null,null,null,null,null,"rdl:RDS915119",null,"An <ELECTROMETER> is an <ELECTRIC VARIABLE METER> for ascertaining the quality and quantity of electricity in an electrified body",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OHMMETER",null,null,null,null,null,"rdl:RDS915299",null,"An <OHMMETER> is an <ELECTRIC VARIABLE METER> for measuring electrical resistance in ohms",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PERMEAMETER",null,null,null,null,null,"rdl:RDS953504",null,"A <PERMEAMETER> is an <ELECTRIC VARIABLE METER> for measuring the magnetic permeability of a substance or object",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PHASE METER",null,null,null,null,null,"rdl:RDS915434",null,"A <PHASE METER> is an <ELECTRIC VARIABLE METER> that measures the phase difference between two oscillations having the same frequency, especially that between an alternating current and the corresponding voltage (hence giving the power factor)",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PHASE SEQUENCE METER",null,null,null,null,null,"rdl:RDS916739",null,"A <PHASE SEQUENCE METER> is an <ELECTRIC VARIABLE METER> that indicates, on a polyphase system, the sequence in which the instantaneous voltage of the phase conductors reach their maximum value",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POLARITY METER",null,null,null,null,null,"rdl:RDS916694",null,"A <POLARITY METER> is an <ELECTRIC VARIABLE METER> that indicates the polarity of one conductor with reference to another",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER FACTOR METER",null,null,null,null,null,"rdl:RDS870839",null,"A <POWER FACTOR METER> is an <<ELECTRIC VARIABLE METER> intended to measure the ratio of the active to the apparent power in an electrical circuit",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER METER",null,null,null,null,null,"rdl:RDS870794",null,"A <POWER METER> is an <<ELECTRIC VARIABLE METER> intended to measure electrical power in watt",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VAR-HOUR METER",null,null,null,null,null,"rdl:RDS915614",null,"A <VAR-HOUR METER> is an <<ELECTRIC VARIABLE METER> intended to measure reactive energy by integrating reactive power with respect to time",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLT-AMPERE METER",null,null,null,null,null,"rdl:RDS915254",null,"A <VOLT-AMPERE METER> is an <ELECTRIC VARIABLE METER> intended to measure apparent power (volt-ampere)",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLT-AMPERE-HOUR METER",null,null,null,null,null,"rdl:RDS915659",null,"A <VOLT-AMPERE-HOUR METER> is an <ELECTRIC VARIABLE METER> intended to measure apparent energy by integrating apparent power with respect to time",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLTMETER",null,null,null,null,null,"rdl:RDS870974",null,"A <VOLTMETER> is an <ELECTRIC VARIABLE METER> for measuring the pressure of electricity in volts",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WATT-HOUR METER",null,null,null,null,null,"rdl:RDS915569",null,"A <WATT-HOUR METER> is an <ELECTRIC VARIABLE METER> intended to measure active energy by integrating active power with respect to time",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRIC VARIABLE METER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WATTMETER",null,null,null,null,null,"rdl:RDS915209",null,"A <WATTMETER> is an <ELECTRIC VARIABLE METER> for measuring electric energy",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,"MEASURING BRIDGE",null,null,null,null,null,"rdl:RDS915794",null,"A <MEASURING BRIDGE> is an <ARTEFACT> and a <MEASURING INSTRUMENT> consisting of at least four branches (arms) or groups of circuit elements (resistors, inductors, capacitors, etc.) connected in a quadrilateral, one of whose diagonals is supplied by a source and the other connected to a null detector or a measuring instrument",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOISTURE METER",null,null,null,null,null,"rdl:RDS5770693",null,"A <MOISTURE METER> is a <MEASURING INSTRUMENT>, usually a hand-held or portable instrument consisting of a digital display and a moisture sensing element, that is intended to measure and indicate a measured moisture",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRAVEL INDICATOR",null,null,null,null,null,"rdl:RDS5771285",null,"A <TRAVEL INDICATOR> is a <MEASURING INSTRUMENT> that is powered and indicates the length or rotational movement",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VIBRATION INDICATOR",null,null,null,null,null,"rdl:RDS317654",null,"A <VIBRATION INDICATOR> is an <MEASURING INSTRUMENT> that indicates a measured vibration",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING INSTRUMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WEIGHING SCALE",null,null,null,null,null,"rdl:RDS6621783",null,"A <WEIGHING SCALE> is a <MEASURING INSTRUMENT> that is intended to measure and indicate the weight of an object",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"PROCESS ANALYSER",null,null,null,null,null,"rdl:RDS624014",null,"An <PROCESS ANALYSER> is a <MEASURING FUNCTION> that is intended to analyse a substance for its composition and/or properties, and where the distinction between the primary element and the measuring instrument cannot be made easily",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACETIC ACID ANALYSER",null,null,null,null,null,"rdl:RDS6568985",null,"An <ACETIC ACID ANALYSER> is a <PROCESS ANALYSER> that measures the amount of <ACETIC ACID>s in liquid streams or liquid samples",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BOILING POINT ANALYSER",null,null,null,null,null,"rdl:RDS878489",null,"A <BOILING POINT ANALYSER> is a <PROCESS ANALYSER> that determines the <BOILING POINT> or <BOILING RANGE> of a fluid",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CARBON DIOXIDE ANALYSER",null,null,null,null,null,"rdl:RDS1007729",null,"A <CARBON DIOXIDE ANALYSER> is a <PROCESS ANALYSER> that determines the concentration of carbon dioxide",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHEMICAL COLORIMETRY ANALYSER",null,null,null,null,null,"rdl:RDS6588290",null,"A <CHEMICAL COLORIMETRY ANALYSER> is a <PROCESS ANALYSER> that measures <ALKALINITY> by colorimetric pH determination in a buffered sample",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHROMATOGRAPH",null,null,null,null,null,"rdl:RDS878669",null,"A <CHROMATOGRAPH> is a <PROCESS ANALYSER> that analyses the molecular composition of a substance",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CLOUD POINT ANALYSER",null,null,null,null,null,"rdl:RDS6588560",null,"A <CLOUD POINT ANALYSER> is a <PROCESS ANALYSER> that determines the <CLOUD POINT> of a fluid",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DENSITY ANALYSER",null,null,null,null,null,"rdl:RDS1007774",null,"A <DENSITY ANALYSER> is a <PROCESS ANALYSER> intended to determine the density of a substance",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DEW POINT ANALYSER",null,null,null,null,null,"rdl:RDS879254",null,"A <DEW POINT ANALYSER> is a <PROCESS ANALYSER> intended to determine the dew point of a substance",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLAME IONISATION ANALYSER",null,null,null,null,null,"rdl:RDS6599217",null,"A <FLAME IONISATION ANALYSER> is a <PROCESS ANALYSER> that is using the flame ionisation principle for analysing hydro carbons, also called TOC and a UHC",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLASH POINT ANALYSER",null,null,null,null,null,"rdl:RDS1007999",null,"A <FLASH POINT ANALYSER> is a <PROCESS ANALYSER> intended to determine the flash point of a substance",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS ANALYSER",null,null,null,null,null,"rdl:RDS850679",null,"A <GAS ANALYSER> is a <PROCESS ANALYSER> that analyses the composition of a gaseous mixture with two or more components",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H2S ANALYSER",null,null,null,null,null,"rdl:RDS6466434",null,"An <H2S ANALYSER>is a <PROCESS ANALYSER> intended to analyse the concentration of <H2S> in a fluid stream",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HARDNESS ANALYSER",null,null,null,null,null,"rdl:RDS6466074",null,"A <HARDNESS ANALYSER>is a <PROCESS ANALYSER> intended to determine the hardness of a solid compound",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OCTANE NUMBER ANALYSER",null,null,null,null,null,"rdl:RDS6466299",null,"An <OCTANE NUMBER ANALYSER>is a <PROCESS ANALYSER> intended to determine the octane number of gasoline or diesel oil",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OIL IN WATER ANALYSER",null,null,null,null,null,"rdl:RDS647999",null,"An <OIL IN WATER ANALYSER>is a <PROCESS ANALYSER> intended to determine the oil content in water",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OXYGEN CONTENT ANALYSER",null,null,null,null,null,"rdl:RDS647954",null,"An <OXYGEN CONTENT ANALYSER>is a <PROCESS ANALYSER> intended to determine the oxygen concentration in a fluid",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PH ANALYSER",null,null,null,null,null,"rdl:RDS850634",null,"A <PH ANALYSER>is a <PROCESS ANALYSER> intended to measure and indicate and/or produce a signal which represents the measured alkalinity / acidity in a fluid or matter",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PNA-METER",null,null,null,null,null,"rdl:RDS6466704",null,"A <PNA-METER>is a <PROCESS ANALYSER> intended to measure and indicate and/or produce a signal which represents the measured parafinic and naphtenic and aromatic content of a fluid",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POUR POINT ANALYSER",null,null,null,null,null,"rdl:RDS6466479",null,"A <POUR POINT ANALYSER>is a <PROCESS ANALYSER> intended to determine the pour point of a fluid, i.e. the lowest temperature at which an oil or other liquid will pour under given conditions",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REFRACTIVE INDEX ANALYSER",null,null,null,null,null,"rdl:RDS1008044",null,"A <REFRACTIVE INDEX ANALYSER>is a <PROCESS ANALYSER> intended to determine the refractive index for a medium",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SALINOMETER",null,null,null,null,null,"rdl:RDS5772800",null,"A <SALINOMETER>is a <PROCESS ANALYSER> for measuring the amount of salt in a solution",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS ANALYSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SULPHUR ANALYSER",null,null,null,null,null,"rdl:RDS6466524",null,"A <SULPHUR ANALYSER>is a <PROCESS ANALYSER> intended to determine the sulphur concentration in a fluid",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING FUNCTION","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"PROCESS SWITCH",null,null,null,null,null,"rdl:RDS7210156",null,"A <PROCESS SWITCH> is an <MEASURING FUNCTION> and a <SWITCHING DEVICE> that operates when the output of a <MEASURING ELEMENT> reaches a preset criterium",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DUST SWITCH",null,null,null,null,null,"rdl:RDS2220007",null,"A <DUST SWITCH> is a <PROCESS SWITCH> using a <DUST MEASURING ELEMENT> that switches when the dust concentration in a gas flow has reached a preset value",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW SWITCH",null,null,null,null,null,"rdl:RDS302894",null,"A <FLOW SWITCH> is a <PROCESS SWITCH> using a <FLOW MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL SWITCH",null,null,null,null,null,"rdl:RDS316754",null,"A <LEVEL SWITCH> is a <PROCESS SWITCH> using a <LEVEL MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POSITION SWITCH",null,null,null,null,null,"rdl:RDS935594",null,"A <POSITION SWITCH> isa <PROCESS SWITCH> using a <POSITION MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE SWITCH",null,null,null,null,null,"rdl:RDS309419",null,"A <PRESSURE SWITCH> isa <PROCESS SWITCH> using a <PRESSURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTATIONAL SPEED SWITCH",null,null,null,null,null,"rdl:RDS317159",null,"A <ROTATIONAL SPEED SWITCH> isa <PROCESS SWITCH> using a <ROTATIONAL SPEED MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE SWITCH",null,null,null,null,null,"rdl:RDS2229401",null,"A <TEMPERATURE SWITCH> isa <PROCESS SWITCH> using a <TEMPERATURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VIBRATION SWITCH",null,null,null,null,null,"rdl:RDS317204",null,"A <VIBRATION SWITCH> isa <PROCESS SWITCH> using a <VIBRATION MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WEIGHT SWITCH",null,null,null,null,null,"rdl:RDS317249",null,"A <WEIGHT SWITCH> isa <PROCESS SWITCH> using a <WEIGHT MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MEASURING FUNCTION","PROCESS SIGNAL GENERATING FUNCTION","TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,"rdl:RDS2220501",null,"A < PROCESS VARIABLE TRANSMITTER> is a <MEASURING FUNCTION> and a <PROCESS SIGNAL GENERATING FUNCTION> and a <TRANSMITTER> for a <PROCESS VARIABLE> measurement",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACCELLERATION TRANSMITTER",null,null,null,null,null,"rdl:RDS2229100",null,"An <ACCELLERATION TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <ACCELLERATION> measurement, using an <ACCELERATION MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANALYSIS TRANSMITTER",null,null,null,null,null,"rdl:RDS2229319",null,"An <ANALYSIS TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <ANALYSIS> measurement",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANALYSIS TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUTE HUMIDITY TRANSMITTER",null,null,null,null,null,"rdl:RDS6501474",null,"An <ABSOLUTE HUMIDITY TRANSMITTER> is an <ANALYSIS TRANSMITTER> for <ABSOLUTE HUMIDITY> measurement, using a <HUMIDITY MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANALYSIS TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONCENTRATION TRANSMITTER",null,null,null,null,null,"rdl:RDS1455523211",null,"A <CONCENTRATION TRANSMITTER> is an <ANALYSIS TRANSMITTER> using an <ANALYSIS MEASURING ELEMENT> measuring how much of a given substance there is mixed with another substance and transmit a signal proportional to the measured level",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANALYSIS TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONDUCTIVITY TRANSMITTER",null,null,null,null,null,"rdl:RDS6501159",null,"A <CONDUCTIVITY TRANSMITTER> is an <ANALYSIS TRANSMITTER> using an <ANALYSIS MEASURING ELEMENT> for <CONDUCTIVITY> measurement",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANALYSIS TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PH TRANSMITTER",null,null,null,null,null,"rdl:RDS6501579",null,"A <PH TRANSMITTER> is an <ANALYSIS TRANSMITTER> using an <ANALYSIS MEASURING ELEMENT> for pH measurement",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ANALYSIS TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RELATIVE HUMIDITY TRANSMITTER",null,null,null,null,null,"rdl:RDS6501684",null,"A <RELATIVE HUMIDITY TRANSMITTER> is an <ANALYSIS TRANSMITTER> using a <HUMIDITY MEASURING ELEMENT> for <RELATIVE HUMIDITY> measurement",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DISPLACEMENT TRANSMITTER",null,null,null,null,null,"rdl:RDS2229301",null,"A <DISPLACEMENT TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <DISPLACEMENT> measurement, using a <DISPLACEMENT MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL VARIABLE TRANSMITTER",null,null,null,null,null,"rdl:RDS2229303",null,"An <ELECTRICAL VARIABLE TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <ELECTRICAL VARIABLE> measurement",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRICAL VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT TRANSMITTER",null,null,null,null,null,"rdl:RDS6501264",null,"A <CURRENT TRANSMITTER> is an < ELECTRICAL VARIABLE TRANSMITTER> for <CURRENT> measurement, using a <CURRENT MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRICAL VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FREQUENCY TRANSMITTER",null,null,null,null,null,"rdl:RDS6501369",null,"A <FREQUENCY TRANSMITTER> is an < ELECTRICAL VARIABLE TRANSMITTER> for <FREQUENCY> measurement, using a <FREQUENCY MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRICAL VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER FACTOR TRANSMITTER",null,null,null,null,null,"rdl:RDS2222219",null,"A <POWER FACTOR TRANSMITTER> is an < ELECTRICAL VARIABLE TRANSMITTER> for <POWER FACTOR> measurement, using a <POWER FACTOR MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRICAL VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER TRANSMITTER",null,null,null,null,null,"rdl:RDS2222218",null,"A <POWER TRANSMITTER> is an < ELECTRICAL VARIABLE TRANSMITTER> for <POWER> measurement, using a <POWER MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRICAL VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESISTANCE TRANSMITTER",null,null,null,null,null,"rdl:RDS6501789",null,"A <RESISTANCE TRANSMITTER> is an < ELECTRICAL VARIABLE TRANSMITTER> for <RESISTANCE> measurement, using a <RESISTANCE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRICAL VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE TRANSMITTER",null,null,null,null,null,"rdl:RDS1287137911",null,"A <VOLTAGE TRANSMITTER> is an < ELECTRICAL VARIABLE TRANSMITTER> for <VOLTAGE> measurement, using a <VOLTAGE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW TRANSMITTER",null,null,null,null,null,"rdl:RDS880154",null,"A <FLOW TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <FLOW RATE> measurement, using a <FLOW MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL TRANSMITTER",null,null,null,null,null,"rdl:RDS418544",null,"A <LEVEL TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for liquid <LEVEL> measurement, using a <LEVEL MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POSITION TRANSMITTER",null,null,null,null,null,"rdl:RDS5769450",null,"A <POSITION TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <POSITION> measurement, using a <POSITION MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE TRANSMITTER",null,null,null,null,null,"rdl:RDS743399",null,"A <PRESSURE TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <PRESSURE> measurement, using a <PRESSURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PRESSURE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABSOLUTE PRESSURE TRANSMITTER",null,null,null,null,null,"rdl:RDS819044",null,"An <ABSOLUTE PRESSURE TRANSMITTER> is a <PRESSURE TRANSMITTER> for <ABSOLUTE PRESSURE> measurement, using a <ABSOLUTE PRESSURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PRESSURE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL PRESSURE TRANSMITTER",null,null,null,null,null,"rdl:RDS428849",null,"A <DIFFERENTIAL PRESSURE TRANSMITTER> is a <PRESSURE TRANSMITTER> for <DIFFERENTIAL PRESSURE> measurement, using a <DIFFERENTIAL PRESSURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PRESSURE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAUGE PRESSURE TRANSMITTER",null,null,null,null,null,"rdl:RDS818999",null,"A <GAUGE PRESSURE TRANSMITTER> is a <PRESSURE TRANSMITTER> for <GAUGE PRESSURE> measurement, using a <GAUGE PRESSURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROXIMITY TRANSMITTER",null,null,null,null,null,"rdl:RDS2229311",null,"A <PROXIMITY TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <PROXIMITY> measurement, using a <PROXIMITY MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIATION TRANSMITTER",null,null,null,null,null,"rdl:RDS2229312",null,"A <RADIATION TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <RADIATION> measurement, using a <RADIATION MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTATIONAL SPEED TRANSMITTER",null,null,null,null,null,"rdl:RDS5769822",null,"A <ROTATIONAL SPEED TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <ROTATIONAL SPEED> measurement, using a <ROTATIONAL SPEED MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE TRANSMITTER",null,null,null,null,null,"rdl:RDS418004",null,"A <TEMPERATURE TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <TEMPERATURE> measurement, using a <TEMPERATURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VELOCITY TRANSMITTER",null,null,null,null,null,"rdl:RDS2223228",null,"A <VELOCITY TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <VELOCITY> measurement, using a <VELOCITY MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VIBRATION TRANSMITTER",null,null,null,null,null,"rdl:RDS6501999",null,"A <VIBRATION TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <VIBRATION> measurement, using a <VIBRATION MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS VARIABLE TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WEIGHT TRANSMITTER",null,null,null,null,null,"rdl:RDS6502104",null,"A <WEIGHT TRANSMITTER>is a <PROCESS VARIABLE TRANSMITTER> for <WEIGHT> measurement, using a <WEIGHT MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,"MONITOR",null,null,null,null,null,"rdl:RDS13175715",null,"A <MONITOR> is an <INSTRUMENTATION FUNCTION> that is capable of <MONITORING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","MONITOR","SYSTEM","WARNER",null,null,null,null,null,null,null,null,null,null,"ALARM SYSTEM",null,null,null,null,null,"rdl:RDS13310335",null,"An <ALARM SYSTEM> is an <ARTEFACT> and a <MONITOR> and a <WARNER> and a <SYSTEM> giving alarm if measured values get outside set values",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ALARM SYSTEM","PUBLIC ADDRESS SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"PUBLIC ADDRESS AND ALARM SYSTEM",null,null,null,null,null,"rdl:RDS1300133871",null,"A <PUBLIC ADDRESS AND ALARM SYSTEM> is an <ALARM SYSTEM> and a <PUBLIC ADDRESS SYSTEM>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","MONITOR","SYSTEM",null,null,null,null,null,null,null,null,null,null,null,"CONDITION MONITORING UNIT",null,null,null,null,null,"rdl:RDS271304",null,"A <CONDITION MONITORING UNIT> is an <ARTEFACT> and a <MONITOR> and a <SYSTEM> that is capable of observing one or more parameters in a system/process, or a part of a system/process, and report on status and functioning",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONDITION MONITORING UNIT","PROTECTION SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"CORROSION MONITORING UNIT",null,null,null,null,null,"rdl:RDS11855725",null,"A <CORROSION MONITORING SYSTEM> is a <CONDITION MONITORING UNIT> and a <PROTECTION SYSTEM> intended to monitor a corrosion process of an item",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MONITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"FIRE FOAM MONITOR",null,null,null,null,null,"rdl:RDS301139",null,"A <FIRE FOAM MONITOR> is a <MONITOR> for monitoring the status of fire foam",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MONITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"FIRE MONITOR",null,null,null,null,null,"rdl:RDS5775365",null,"A <FIRE MONITOR> is a <MONITOR> with the capability of receiveing and displaying information about fire and/or firefighting system",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MONITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"FIRE WATER MONITOR",null,null,null,null,null,"rdl:RDS301319",null,"A <FIRE WATER MONITOR> is a <MONITOR> that is capable of monitoring operation of firewater",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","FIRE WATER MONITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"FIRE WATER RELEASE MONITOR",null,null,null,null,null,"rdl:RDS7057656",null,"A <FIRE WATER RELEASE MONITOR> is an <ARTEFACT> and a <FIRE WATER MONITOR> intended to show the state of fire water release",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","MONITOR",null,null,null,null,null,null,null,null,null,null,null,null,"FIREWATER MONITOR",null,null,null,null,null,"rdl:RDS485549",null,"A <FIREWATER MONITOR> is an <ARTEFACT> and a <MONITOR> that is a firewater discharge controller",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MONITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"POSITION MONITOR",null,null,null,null,null,"rdl:RDS5775444",null,"A <POSITION MONITOR> is a <MONITOR> with the capability of receiveing and displaying information about position",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MONITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"PROCESS MONITORING DEVICE",null,null,null,null,null,"rdl:RDS2220082",null,"A <PROCESS MONITORING DEVICE> is a <MONITOR> that is capable of <MONITORING> a process facility",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","PROCESS MONITORING DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,null,"PROCESS MONITORING SYSTEM",null,null,null,null,null,"rdl:RDS2220083",null,"A <PROCESS MONITORING SYSTEM> is an <ARTEFACT> and a <PROCESS MONITORING DEVICE> that is used to monitor a process facility",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PROCESS MONITORING SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SCADA SYSTEM",null,null,null,null,null,"rdl:RDS2220084",null,"A <SCADA SYSTEM> is a <PROCESS MONITORING SYSTEM> that monitors and controls industrial infrastructure or facility processes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MONITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"SAND DETECTION MONITOR",null,null,null,null,null,"rdl:RDS5775602",null,"A <SAND DETECTION MONITOR> is a <MONITOR> with the capability of receiveing signals and displaying information about sand detection",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MONITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"SPEED MONITOR",null,null,null,null,null,"rdl:RDS5775681",null,"A <SPEED MONITOR> is a <MONITOR> with the capability of receiveing signals and displaying information about speed",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"MONITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE MONITOR",null,null,null,null,null,"rdl:RDS5775726",null,"A <TEMPERATURE MONITOR> is a <MONITOR> with the capability of receiveing signals and displaying information about temperature",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","MONITOR",null,null,null,null,null,null,null,null,null,null,null,null,"VIDEO MONITOR",null,null,null,null,null,"rdl:RDS5775540",null,"A <VIDEO MONITOR> is an <ARTEFACT> and a <MONITOR> that displays the output of a video-generating device, such as a media playout server, IRD, video camera, VCR, or DVD player",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VIDEO MONITOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CCTV MONITOR",null,null,null,null,null,"rdl:RDS1322344611",null,"A <CCTV MONITOR> is a <VIDEO MONITOR> in a closed-circuit television circuit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","MONITOR",null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE MONITOR",null,null,null,null,null,"rdl:RDS5775867",null,"A <VOLTAGE MONITOR> is an <ARTEFACT> and a <MONITOR> with the capability of receiveing signals and displaying information about voltage level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAUGE","INSTRUMENTATION FUNCTION",null,null,null,null,null,null,null,null,null,null,null,"PROCESS GAUGE",null,null,null,null,null,"rdl:RDS462644",null,"A <PROCESS GAUGE> is a <INSTRUMENTATION FUNCTION> and a <GAUGE> that is a stand-alone device for measuring or sighting a process variable",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS GAUGE",null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW GAUGE",null,null,null,null,null,"rdl:RDS879929",null,"A <FLOW GAUGE> is a <PROCESS GAUGE> using a <FLOW MEASURING ELEMENT> intended to indicate a liquid or gas flow",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS GAUGE",null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL GAUGE",null,null,null,null,null,"rdl:RDS462689",null,"A <LEVEL GAUGE> is a <PROCESS GAUGE> using a <LEVEL MEASURING ELEMENT>, that is intended to display a representation of a measured level",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS GAUGE",null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE GAUGE",null,null,null,null,null,"rdl:RDS1459688721",null,"A <PRESSURE GAUGE> is a <PROCESS GAUGE> using a <PRESSURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS GAUGE",null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE GAUGE",null,null,null,null,null,"rdl:RDS417824",null,"A <TEMPERATURE GAUGE> is a <PROCESS GAUGE> using a <TEMPERATURE MEASURING ELEMENT> that is intended to measure and indicate a <TEMPERATURE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","TEMPERATURE GAUGE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BIMETALLIC TEMPERATURE GAUGE CENTRE BACK STEM",null,null,null,null,null,"rdl:RDS1471947541",null,"A <BIMETALLIC TEMPERATURE GAUGE CENTRE BACK STEM> is an <ARTEFACT> and a <TEMPERATURE GAUGE> with a <TEMPERATURE MEASURING ELEMENT - BIMETAL> where the stem is protuding from the centre of the back of the housing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TEMPERATURE GAUGE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BIMETALLIC TEMPERATURE GAUGE RADIAL BOTTOM STEM",null,null,null,null,null,"rdl:RDS1471952771",null,"A <BIMETALLIC TEMPERATURE GAUGE RADIAL BOTTOM STEM> is an <ARTEFACT> and a <TEMPERATURE GAUGE> with a <TEMPERATURE MEASURING ELEMENT - BIMETAL> where the stem is protuding radially from the bottom of the housing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","TEMPERATURE GAUGE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BIMETALLIC TEMPERATURE GAUGE CENTRE BACK STEM EVERY ANGLE",null,null,null,null,null,"rdl:RDS1471956011",null,"A <BIMETALLIC TEMPERATURE GAUGE CENTRE BACK STEM EVERY ANGLE> is an <ARTEFACT> and a <TEMPERATURE GAUGE> with a <TEMPERATURE MEASURING ELEMENT - BIMETAL> where the stem is protuding from the centre of the back of the housing, and that can be mounted at any angle",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,"PROCESS SIGNAL GENERATING FUNCTION",null,null,null,null,null,"rdl:RDS2220983",null,"A <PROCESS SIGNAL GENERATING FUNCTION> is an <INSTRUMENTATION FUNCTION> that generates a <SIGNAL> that represents the magnitude of a process variable",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,"READER",null,null,null,null,null,"rdl:RDS2224301",null,"A <READER> is an <INSTRUMENTATION FUNCTION> that has the capability of <READING> some <CODE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","READER",null,null,null,null,null,null,null,null,null,null,null,null,"RFID READER",null,null,null,null,null,"rdl:RDS1319206451",null,"A <PROXIMITY READER> is an <ARTEFACT> and a <READER> that reads passive rfid tags without mechanical contact with the tag",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION FUNCTION",null,null,null,null,null,null,null,null,null,null,null,null,"RECORDER",null,null,null,null,null,"rdl:RDS282059",null,"A <RECORDER> is an <INSTRUMENTATION FUNCTION> that is capable of <RECORDING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"OSCILLOGRAPH",null,null,null,null,null,"rdl:RDS914804",null,"A <OSCILLOGRAPH> is an <ARTEFACT> and a <RECORDER> that is intended to record, in the form of a permanent trace, instantaneous values of measured quantities",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","RECORDER",null,null,null,null,null,null,null,null,null,null,null,null,"VIDEO RECORDER",null,null,null,null,null,"rdl:RDS5780016",null,"A <VIDEO RECORDER> is an <ARTEFACT> and a <RECORDER> that is recording signals originated by a TV camera on a moving magnetic tape for subsequent reproduction or transmission",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION FUNCTION","VALVE",null,null,null,null,null,null,null,null,null,null,null,"SELF-OPERATING VALVE",null,null,null,null,null,"rdl:RDS7018938",null,"A <SELF-OPERATING VALVE> is an <INSTRUMENTATION FUNCTION> and a <VALVE> that includes a means of operation (e.g. spring / gravity / fluid pressure / counter balance), and is not depending on an external source of energy",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW REGULATOR",null,null,null,null,null,"rdl:RDS880109",null,"A <FLOW REGULATOR> is a <SELF-OPERATING VALVE> for fluid flow",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL REGULATOR",null,null,null,null,null,"rdl:RDS880739",null,"A <LEVEL REGULATOR> is a <SELF-OPERATING VALVE> for level",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"OVERPRESSURE PROTECTOR","SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,"OVERPRESSURE PROTECTION VALVE",null,null,null,null,null,"rdl:RDS16207641",null,"An <OVERPRESSURE PROTECTION VALVE> is a <SELF-OPERATING VALVE> and an <OVERPRESSURE PROTECTOR>"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE REGULATOR",null,null,null,null,null,"rdl:RDS309149",null,"A <PRESSURE REGULATOR> is a <SELF-OPERATING VALVE> for pressure",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE RELIEF DEVICE",null,null,null,null,null,"rdl:RDS309329",null,"A <PRESSURE RELIEF DEVICE> is a <SELF-OPERATING VALVE>, that relieves pressure from an exclosed space when the pressure reaches a predetermined value",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE REGULATOR",null,null,null,null,null,"rdl:RDS1011284",null,"A <TEMPERATURE REGULATOR> is a <SELF-OPERATING VALVE> for temperature regulation",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMAL RELIEF DEVICE",null,null,null,null,null,"rdl:RDS1336338491",null,"A <THERMAL RELIEF DEVICE> is a <<SELF-OPERATING VALVE> that relieves fluid from an exclosed space when the temperature reaches a predetermined value",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"VACUUM RELIEF DEVICE",null,null,null,null,null,"rdl:RDS313784",null,"A <VACUUM RELIEF DEVICE> is a <SELF-OPERATING VALVE> that opens up and aligns the pressure when the underpressure of a container reaches a predetermined level",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"CONVEYOR","INSTRUMENTATION FUNCTION",null,null,null,null,null,null,null,null,null,null,null,"SIGNAL CONVEYOR",null,null,null,null,null,"rdl:RDS222448",null,"A <SIGNAL CONVEYOR> is an <INSTRUMENTATION FUNCTION> and a <CONVEYOR> for a <SIGNAL>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"SIGNAL CONVEYOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC SIGNAL CONVEYOR",null,null,null,null,null,"rdl:RDS2220161",null,"A < SIGNAL CONVEYOR> is a <SIGNAL CONVEYOR> that are capable of <CONVEYOR> one or more < SIGNAL>s",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"SIGNAL CONVEYOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTROMAGNETIC SIGNAL CONVEYOR",null,null,null,null,null,"rdl:RDS2220164",null,"A < SIGNAL CONVEYOR> is a <SIGNAL CONVEYOR> that are capable of <CONVEYOR> one or more < SIGNAL>s",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"SIGNAL CONVEYOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC SIGNAL CONVEYOR",null,null,null,null,null,"rdl:RDS2220163",null,"A < SIGNAL CONVEYOR> is a <SIGNAL CONVEYOR> that are capable of <CONVEYOR> one or more < SIGNAL>s",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"SIGNAL CONVEYOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC SIGNAL CONVEYOR",null,null,null,null,null,"rdl:RDS2220162",null,"A < SIGNAL CONVEYOR> is a <SIGNAL CONVEYOR> that are capable of <CONVEYOR> one or more < SIGNAL>s",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION FUNCTION","SIGNAL RECEIVER",null,null,null,null,null,null,null,null,null,null,null,"STANDARD SIGNAL RECEIVER",null,null,null,null,null,"rdl:RDS222805",null,"A <STANDARD SIGNAL RECEIVER> is a <INSTRUMENTATION FUNCTION> and a <SIGNAL RECEIVER> that is capable of <RECEIVING> a <STANDARD SIGNAL>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION FUNCTION","SIGNAL SENDER",null,null,null,null,null,null,null,null,null,null,null,"STANDARD SIGNAL SENDER",null,null,null,null,null,"rdl:RDS2223258",null,"A <STANDARD SIGNAL SENDER> is a <INSTRUMENTATION FUNCTION> and a <SIGNAL SENDER> that is capable of <SENDING> a <STANDARD SIGNAL>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION FUNCTION","WARNER",null,null,null,null,null,null,null,null,null,null,null,"STATE WARNER",null,null,null,null,null,"rdl:RDS2220118",null,"A <STATE WARNER> is an <INSTRUMENTATION FUNCTION> and a <WARNER> of an unwanted state change",null,null,null,null,null,"dm:ClassOfFunctionalObject"]