{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["RDL browser","Settings","about","Results1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"RDL browser","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[[0,0,0,4]]}
["RDL2 browser to spreadsheet tool version 75",null,null,null,null,null,"Endpoint: http://data.15926.org/rdl/"]
["Contact: onno.paap@gmail.com",null,null,null,null,"Action","DATA COMMUNICATION AND NETWORK EQUIPMENT CLASS","http://data.15926.org/rdl/RDS1322281111"]
[null,null,null,null,null,"Action","ELECTRICAL NETWORK","http://data.15926.org/rdl/RDS1293939661"]
["Search:","NETWORK",null,null,null,"Action","EQUIVALENT NETWORK SYSTEM","http://data.15926.org/rdl/RDS7009975"]
[null,null,null,null,null,"Action","NETWORK","http://data.15926.org/rdl/RDS1293947091"]
[null,null,null,null,null,"Action","NETWORK CALCULATING","http://data.15926.org/rdl/RDS7014210"]
[null,null,null,null,null,"Action","NETWORK CARD","http://data.15926.org/rdl/RDS1318193371"]
[null,null,null,null,null,"Action","NETWORK CONVERTING","http://data.15926.org/rdl/RDS30644"]
[null,null,null,null,null,"Action","NETWORK DIAGRAM","http://data.15926.org/rdl/RDS346184"]
[null,null,null,null,null,"Action","NETWORK SPLITTING","http://data.15926.org/rdl/RDS31859"]
[null,null,null,null,null,"Action","NETWORK TOPOLOGY","http://data.15926.org/rdl/RDS17919025"]
[null,null,null,null,null,"Action","PIPING NETWORK BRANCH","http://data.15926.org/rdl/RDS267659"]
[null,"Note: first set coloring on in Settings",null,null,null,"Action","PIPING NETWORK CONNECTOR","http://data.15926.org/rdl/RDS270989"]
[null,"Coloring (containing this string will give this color)",null,null,null,"Action","PIPING NETWORK SEGMENT","http://data.15926.org/rdl/RDS267704"]
[null,"ClassOfFunctionalObject",null,null,null,"Action","PIPING NETWORK SYSTEM","http://data.15926.org/rdl/RDS270359"]
[null,"ClassOfInanimatePhysicalObject ",null,null,null,"Action","PIPING NETWORK TERMINATOR","http://data.15926.org/rdl/RDS270944"]
[null,null,null,null,null,"Action","RADIAL OPERATION (OF A PART OF A NETWORK)","http://data.15926.org/rdl/RDS32174"]
[null,null,null,null,null,"Action","RING OPERATION OF A PART OF A NETWORK","http://data.15926.org/rdl/RDS32129"]
[null,null,null,null,null,"Action","SEPARATE NETWORK OPERATION","http://data.15926.org/rdl/RDS31994"]
[]
[]
[]
[]
[]
[null,"Namespace replacer (definition containing this string replaces the namespace)"]
[null,"API","API:"]
[null,"ASME","ASME:"]
[null,"ASTM","ASTM:"]
[null,"DIN","DIN:"]
[null,"EN","EN:"]
[null,"ISO","ISO:"]
[null,"NORSOK","NOR:"]
[null,"NPD","NOR:"]
[null,"NS","NOR:"]
[null,"ROSEMOUNT","ROS:"]
[null,"SAE","SAE:"]
[null,"SIEMENS","SIE:"]
[null,"SKOTSELV","SKOT:"]
[null,"TWR","TWR:"]

{"sheet":"Settings","index":1,"n_rows":87,"n_cols":8,"rows_kept":87,"cut":false,"hidden":true,"merged":[]}
["Setting name","Select name","OnKey","Value","Status","RDLType"]
["Endpoint","RDL2 (15926.org)",null,"http://data.15926.org/rdl/","Current",null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA RDL",null,"http://data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA Staging",null,"http://staging.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA SVRDL",null,"http://svrdl.community.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P4",null,"http://posccaesar.org/p4/sparql",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P12",null,"http://sti.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","Localhost",null,"http://localhost:8890/sparql/",null,null,null,"Note: end address always with a slash (/)"]
[]
["gBaseNamespace",null,"http://data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://staging.data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://svrdl.community.data.posccaesar.org/rdl/","http://svrdl.community.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://posccaesar.org/p4/sparql","http://posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://sti.data.posccaesar.org/rdl/","http://sti.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://localhost:8890/sparql/","http://data.15926.org/rdl/",null,"RDL2"]
["gKeepSettings",null,null,"T"]
["gShowDeprecated",null,null,"F"]
["gColoring",null,null,"T"]
["gNamespaceReplacing",null,null,"F"]
["gHyperlinkReplacing",null,null,"F"]
[]
["Endpoint","aisi",null,"http://data.15926.org/aisi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ansi",null,"http://data.15926.org/ansi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","api",null,"http://data.15926.org/api/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","all",null,"http://data.15926.org/all/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","asme",null,"http://data.15926.org/asme/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","astm",null,"http://data.15926.org/astm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","atex",null,"http://data.15926.org/atex/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","bs",null,"http://data.15926.org/bs/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","din",null,"http://data.15926.org/din/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dm",null,"http://data.15926.org/dm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dnv",null,"http://data.15926.org/dnv/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","edm",null,"http://data.15926.org/edm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","en",null,"http://data.15926.org/en/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","eu",null,"http://data.15926.org/eu/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iec",null,"http://data.15926.org/iec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ieee",null,"http://data.15926.org/ieee/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iso",null,"http://data.15926.org/iso/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","lci",null,"http://data.15926.org/lci/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","mss",null,"http://data.15926.org/mss/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nace",null,"http://data.15926.org/nace/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nec",null,"http://data.15926.org/nec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nema",null,"http://data.15926.org/nema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nfpa",null,"http://data.15926.org/nfpa/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nor",null,"http://data.15926.org/nor/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","rdl",null,"http://data.15926.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sae",null,"http://data.15926.org/sae/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sie",null,"http://data.15926.org/sie/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","tema",null,"http://data.15926.org/tema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","twr",null,"http://data.15926.org/twr/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","uns",null,"http://data.15926.org/uns/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","wits",null,"http://data.15926.org/wits/",null,null,null,"Note: end address always with a slash (/)"]
[]
[]
["gBaseNamespace",null,"http://data.15926.org/aisi/","http://data.15926.org/aisi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ansi/","http://data.15926.org/ansi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/api/","http://data.15926.org/api/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/asme/","http://data.15926.org/asme/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/all/","http://data.15926.org/all/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/astm/","http://data.15926.org/astm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/atex/","http://data.15926.org/atex/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/bs/","http://data.15926.org/bs/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/din/","http://data.15926.org/din/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dm/","http://data.15926.org/dm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dnv/","http://data.15926.org/dnv/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/edm/","http://data.15926.org/edm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/en/","http://data.15926.org/en/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/eu/","http://data.15926.org/eu/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iec/","http://data.15926.org/iec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ieee/","http://data.15926.org/ieee/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iso/","http://data.15926.org/iso/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/lci/","http://data.15926.org/lci/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/mss/","http://data.15926.org/mss/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nace/","http://data.15926.org/nace/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nec/","http://data.15926.org/nec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nema/","http://data.15926.org/nema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nfpa/","http://data.15926.org/nfpa/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nor/","http://data.15926.org/nor/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sae/","http://data.15926.org/sae/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sie/","http://data.15926.org/sie/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/tema/","http://data.15926.org/tema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/twr/","http://data.15926.org/twr/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/uns/","http://data.15926.org/uns/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/wits/","http://data.15926.org/wits/",null,"RDL2"]
["                                          "]

{"sheet":"about","index":2,"n_rows":176,"n_cols":3,"rows_kept":176,"cut":false,"hidden":false,"merged":[]}
["Version 75 changes","2018-10-05","Onno Paap"]
["missing superclasses - and orphans- filter no deprecated classes"]
[]
["Version 74 changes","2018-09-30","Onno Paap"]
["Repaired bug missing label"]
[]
["Version 73 changes","2018-05-16","Onno Paap"]
["Repaired bug Deprecated Superclass"]
[]
[]
[]
["Version 71 changes","2016-07-17","Onno Paap"]
["Aded report button for comparison of RDL2 with a subfolder called views filled with spreadsheets."]
[]
[]
["Version 69 changes","2016-06-16","Onno Paap"]
["Added button: \"errors in definitions\" that lists all classes that have more or less \"<\" brackets than the number of super class relationships + 1. Where the part after the word \"that \"  is ignored in the count of \"<\" brackets."]
[]
["Version 68 changes","2016-06-13","Onno Paap"]
["Updated endpoint of RDL2 sparql "]
[]
["Version 67 changes","2016-05-22","Onno Paap"]
["Added button list subclasses from superclass "]
[]
["Version 65 changes","2016-04-25","Onno Paap"]
["Added checkbox at action dialog \"supress double child occurances\" so that this built-in feature can be switched off"]
[]
["Version 64 changes","2016-04-20","Onno Paap"]
["Made search case-insensitive and added endpoint \"all\""]
[]
["Version 63 changes","2016-09-28","Onno Paap"]
["Made entity list working on P4 endpoint (they changed the database version which was not accepting som sparql setting)"]
["Version 62 changes","2016-09-28","Onno Paap"]
["Applied show deprecated to searched result list"]
[]
["Version 61 changes","2016-08-29","Onno Paap"]
["Added query from pcardl for ClassOfIndirectProperty"]
[]
["Version 60 changes","2016-08-19","Onno Paap"]
["Repaired failing entity reports"]
[]
["Version 59 changes","2016-08-19","Onno Paap"]
["Missing superclasses now queries whole federation of RDL2"]
[]
["Version 58 changes","2016-08-16","Onno Paap"]
["Repaired missing output for entities and doubles in RDL2 endpoints other than rdl"]
[]
["Version 57 changes","2016-08-13","Onno Paap"]
["Doubles report now skips classes that are deprecated"]
[]
["Version 56 changes","2016-07-22","Onno Paap"]
["Made rowheight suitable for longer definitions to example DESIGN BASIS"]
[]
["Version 55 changes","2016-07-19","Onno Paap"]
["Made rowheight suitable for longer definitions"]
[]
["Version 54 changes","2016-07-03","Onno Paap"]
["Entity Type field changed to 6 merged cells."]
[]
["Version 53 changes","2016-06-23","Onno Paap"]
["added lci namespace"]
[]
["Version 52 changes","2016-06-23","Onno Paap"]
["Added deprecated count to list entities"]
[]
["Version 51 changes","2016-06-19","Onno Paap"]
["Updated namespaces of staging RDL"]
[]
["Version 50 changes","2016-06-19","Onno Paap"]
["taxonomy view repaired missing entity type"]
[]
["Version 49 changes","2016-06-14","Onno Paap"]
["Room for 12 superclasses"]
[]
["Version 48 changes","2016-06-14","Onno Paap"]
["Repaired NOR:/RDS  bug"]
[]
["Version 47 changes","2016-06-14","Onno Paap"]
["Repaired endpoint bug"]
[]
["Version 46 changes","2016-06-13","Onno Paap"]
["Updated endpoints"]
[]
["Version 45 changes","2016-06-06","Onno Paap"]
["Completed Missing Superclasses report"]
[]
["Version 44 changes","2016-05-20","Onno Paap"]
["Added Clear Cache button (use on any database changes)"]
[]
["Version 43 changes","2016-05-19","Onno Paap"]
["Changed non-existing super classes to show as \"no label\""]
[]
["Version 42 changes","2016-05-02","Onno Paap"]
["bug fix"]
[]
["Version 41 changes","2016-05-02","Onno Paap"]
["Added setting to show/not show deprecated items. If shown, they are stricken through"]
[]
["Version 40 changes","2016-03-31","Onno Paap"]
["Added  in doubles: two classes having the same label."]
[]
["Version 39 changes","2016-03-21","Onno Paap"]
["Made the query more robust, after the server hass been returning a 404 occasionally"]
[]
["Version 38 changes","2016-03-03","Onno Paap"]
["Repaired bug entity type query on PCA endpoint"]
[]
["Version 37 changes","2016-01-29","Onno Paap"]
["Showing deprecated class in taxonomy with label in strikethrough."]
[]
["Version 36 changes","2016-01-13","Onno Paap"]
["Added the 17 endpoints of http://data.15926.org/rdl"]
[]
["Version 35 changes","2016-01-13","Onno Paap"]
["In taxonomy view, disregard all rdf:type that is not data model.  So only show rdf:type that is dm:"]
[]
["Version 34 changes","2016-01-13","Onno Paap"]
["Solved taxonomy levels regression bug"]
[]
["Version 33 changes","2016-01-11","Onno Paap"]
["Enhanced the doubled query. First 4 columns are about the triple, the rest is info."]
[]
["Repaired bug in entity type query."]
[]
["Version 30 changes","2016-01-03","Onno Paap"]
["Repaired entity type query for old PCA RDL. \nRepaired bug in entity type query where a class that has a superclass of the wanted type as well as  of another type became  the start point of a new taxonomy as well as part in the main taxonomy. (read that again)"]
[]
["Version 29 changes","2016-01-02","Onno Paap"]
["Filtered entity filtered taxonomy to only show the filtered entity not subClassOf of another entity"]
[]
["Version 27 changes","2016-01-01","Onno Paap"]
["few bugs repaired.  Changed entity search into presenting taxonomies. "]
[]
["Version 26 changes","2015-12-26","Onno Paap"]
["few bugs repaired. "]
[]
["Version 25 changes","2015-12-26","Onno Paap"]
["Added Part 12 and localhost endpoints"]
["Added button for selecting double labels and definitions. "]
["Version 24 changes","2015-12-14","Onno Paap"]
["Added button to list all distinct entity data types and their counts, and click to show."]
["Added a button to show all orphans that have a rdfs:label"]
["Version 23 changes"]
["Added endpoint posccaesar.org/p4/sparql"]
["Version 22 changes"]
["Added endpoint staging.data.posccaesar.org/rdl"]
[]
["Version 21 changes"]
["Repaired bug where namespace replace was based upon definition instead of class label"]
[]
["Version 20 changes"]
["Repaired bug where definition did not show up if hyperlink replace was on."]
[]
["Version 19 changes (skip version 16-18)"]
["Settings expanded with persist settings, namespace replacer and hyperlink replacer"]
["Added namespace replacer which will replace the RDL: namespace of the ID with the namespace given in the list on the front page."]
["Added hyperlink replacer which will find terms between single quotes and look them up in the RDL, then add a hyperlink in the text if found. Anchor tag <a></a> used not &hyperlink() so looks ugly."]
[]
["Version 15 changes"]
["Changed browser page Action buttons to hyperlinks because buttons are not equally spaced between Excel versions (Office 2007 versus Office 365)"]
["First row is empty. Move all up."]
["Make stop button for during query taxonomy query execution"]
[]
[]
["Version 14 changes"]
["Aligned buttons on browser page"]
["Made color notification work. Note: switch it on first in settings. Default is off"]
["Top align subclasses in taxonomy"]
["Subclasses made to hyperlink in taxonomy"]
["Subclasses made to increase column width in taxonomy"]
["Made browser search go when hitting enter in search field"]
[]
[]
[]
["todo"]
["Make setting for outputting to other result pages"]

{"sheet":"Results1","index":3,"n_rows":64,"n_cols":35,"rows_kept":64,"cut":false,"hidden":false,"merged":[[62,23,62,24],[62,17,62,22],[62,25,62,30],[62,31,62,34],[63,23,63,24],[63,17,63,22],[63,25,63,30],[63,31,63,34],[60,23,60,24],[60,17,60,22],[60,25,60,30],[60,31,60,34],[61,23,61,24],[61,17,61,22],[61,25,61,30],[61,31,61,34],[58,23,58,24],[58,17,58,22],[58,25,58,30],[58,31,58,34],[59,23,59,24],[59,17,59,22],[59,25,59,30],[59,31,59,34],[56,23,56,24],[56,17,56,22],[56,25,56,30],[56,31,56,34],[57,23,57,24],[57,17,57,22],[57,25,57,30],[57,31,57,34],[54,24,54,25],[54,18,54,23],[54,26,54,31],[54,32,54,35],[55,25,55,26],[55,19,55,24],[55,27,55,32],[55,33,55,36],[52,24,52,25],[52,18,52,23],[52,26,52,31],[52,32,52,35],[53,25,53,26],[53,19,53,24],[53,27,53,32],[53,33,53,36],[50,25,50,26],[50,19,50,24],[50,27,50,32],[50,33,50,36],[51,24,51,25],[51,18,51,23],[51,26,51,31],[51,32,51,35],[48,24,48,25],[48,18,48,23],[48,26,48,31],[48,32,48,35],[49,24,49,25],[49,18,49,23],[49,26,49,31],[49,32,49,35],[46,23,46,24],[46,17,46,22],[46,25,46,30],[46,31,46,34],[47,23,47,24],[47,17,47,22],[47,25,47,30],[47,31,47,34],[44,24,44,25],[44,18,44,23],[44,26,44,31],[44,32,44,35],[45,23,45,24],[45,17,45,22],[45,25,45,30],[45,31,45,34],[42,25,42,26],[42,19,42,24],[42,27,42,32],[42,33,42,36],[43,24,43,25],[43,18,43,23],[43,26,43,31],[43,32,43,35],[40,25,40,26],[40,19,40,24],[40,27,40,32],[40,33,40,36],[41,25,41,26],[41,19,41,24],[41,27,41,32],[41,33,41,36],[38,25,38,26],[38,19,38,24],[38,27,38,32],[38,33,38,36],[39,24,39,25],[39,18,39,23],[39,26,39,31],[39,32,39,35],[36,23,36,24],[36,17,36,22],[36,25,36,30],[36,31,36,34],[37,24,37,25],[37,18,37,23],[37,26,37,31],[37,32,37,35],[34,23,34,24],[34,17,34,22],[34,25,34,30],[34,31,34,34],[35,22,35,23],[35,16,35,21],[35,24,35,29],[35,30,35,33],[32,22,32,23],[32,16,32,21],[32,24,32,29],[32,30,32,33],[33,22,33,23],[33,16,33,21],[33,24,33,29],[33,30,33,33],[30,22,30,23],[30,16,30,21],[30,24,30,29],[30,30,30,33],[31,21,31,22],[31,15,31,20],[31,23,31,28],[31,29,31,32],[28,23,28,24],[28,17,28,22],[28,25,28,30],[28,31,28,34],[29,22,29,23],[29,16,29,21],[29,24,29,29],[29,30,29,33],[26,23,26,24],[26,17,26,22],[26,25,26,30],[26,31,26,34],[27,24,27,25],[27,18,27,23],[27,26,27,31],[27,32,27,35],[24,24,24,25],[24,18,24,23],[24,26,24,31],[24,32,24,35],[25,24,25,25],[25,18,25,23],[25,26,25,31],[25,32,25,35],[22,26,22,27],[22,20,22,25],[22,28,22,33],[22,34,22,37],[23,26,23,27],[23,20,23,25],[23,28,23,33],[23,34,23,37],[20,25,20,26],[20,19,20,24],[20,27,20,32],[20,33,20,36],[21,25,21,26],[21,19,21,24],[21,27,21,32],[21,33,21,36],[18,26,18,27],[18,20,18,25],[18,28,18,33],[18,34,18,37],[19,25,19,26],[19,19,19,24],[19,27,19,32],[19,33,19,36],[16,25,16,26],[16,19,16,24],[16,27,16,32],[16,33,16,36],[17,26,17,27],[17,20,17,25],[17,28,17,33],[17,34,17,37],[14,25,14,26],[14,19,14,24],[14,27,14,32],[14,33,14,36],[15,24,15,25],[15,18,15,23],[15,26,15,31],[15,32,15,35],[12,24,12,25],[12,18,12,23],[12,26,12,31],[12,32,12,35],[13,24,13,25],[13,18,13,23],[13,26,13,31],[13,32,13,35],[10,26,10,27],[10,20,10,25],[10,28,10,33],[10,34,10,37],[11,26,11,27],[11,20,11,25],[11,28,11,33],[11,34,11,37],[8,24,8,25],[8,18,8,23],[8,26,8,31],[8,32,8,35],[9,25,9,26],[9,19,9,24],[9,27,9,32],[9,33,9,36],[6,24,6,25],[6,18,6,23],[6,26,6,31],[6,32,6,35],[7,23,7,24],[7,17,7,22],[7,25,7,30],[7,31,7,34],[4,23,4,24],[4,17,4,22],[4,25,4,30],[4,31,4,34],[5,23,5,24],[5,17,5,22],[5,25,5,30],[5,31,5,34],[2,22,2,23],[2,16,2,21],[2,24,2,29],[2,30,2,33],[3,23,3,24],[3,17,3,22],[3,25,3,30],[3,31,3,34],[0,20,0,21],[0,14,0,19],[0,22,0,27],[0,28,0,31],[1,21,1,22],[1,15,1,20],[1,23,1,28],[1,29,1,32]]}
[null,null,"FunctionalObject",null,null,null,null,null,null,null,null,null,null,null,"NETWORK",null,null,null,null,null,"rdl:RDS1293947091",null,"A <NETWORK> is a <FunctionalObject> that is a group or system of interconnected people or things",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"NETWORK",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL NETWORK",null,null,null,null,null,"rdl:RDS1293939661",null,"An <ELECTRICAL NETWORK> is a <NETWORK>that is an interconnection of <ELECTRIC ELEMENT>s",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRICAL NETWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC CIRCUIT",null,null,null,null,null,"rdl:RDS5036404627",null,"An <ELECTRIC CIRCUIT> is an <ELECTRICAL NETWORK> that is an arrangement of devices, media, or both, forming one or more conductive paths and where these devices and media can have capacitive and inductive coupling",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","ELECTRIC CIRCUIT",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC ARC WELDING CIRCUIT",null,null,null,null,null,"rdl:RDS1293889471",null,"An <ELECTRIC ARC WELDING CIRCUIT> is an <ELECTRIC CIRCUIT> intended for electric arc welding",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRIC CIRCUIT",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC HEAT TRACING CIRCUIT",null,null,null,null,null,"rdl:RDS1293924881",null,"A <HEAT TRACING CIRCUIT> is an <ARTEFACT> and a <ELECTRIC CIRCUIT> intended for electric heat tracing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRIC CIRCUIT","ENERGY TRANSMITTER",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRIC LINE",null,null,null,null,null,"rdl:RDS1009889",null,"An <ELECTRIC LINE> is an <ENERGY TRANSMITTER> and an <ELECTRIC CIRCUIT> that is an arrangement of conductors, insulating materials and accessories for transferring electricity between two points of a system",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","ELECTRIC LINE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS INSULATED ELECTRIC LINE",null,null,null,null,null,"rdl:RDS1009979",null,"A <GAS INSULATED ELECTRI LINE> is an <ARTEFACT> and a <ELECTRIC LINE> whose conductors are contained in an enclosure and insulated with a compressed gas",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRIC CIRCUIT",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC CIRCUIT",null,null,null,null,null,"rdl:RDS1293967931",null,"An <ELECTRONIC CIRCUIT> is an <ARTEFACT> and a <ELECTRIC CIRCUIT> formed by the interconnection of electronic components through which an electric current can flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANALOG LOOP",null,null,null,null,null,"rdl:RDS1423275251",null,"An <ANALOG LOOP> is an <ELECTRONIC CIRCUIT> in which data is represented by continuously variable physical quantities, usually amplitude or frequency, that is varied in direct proportion to the quantity which it is desired to communicate.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANALOG LOOP","CURRENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANALOG CURRENT LOOP",null,null,null,null,null,"rdl:RDS1422795061",null,"An <ANALOG CURRENT LOOP> is an <ANALOG LOOP> and a <CURRENT LOOP> in which current may vary continuously with time to correspond to the information being represented.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANALOG CURRENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10-50 mA SIGNAL LOOP",null,null,null,null,null,"rdl:RDS1422803261",null,"A <10-50 mA SIGNAL LOOP> is an <ANALOG CURRENT LOOP> where 10 mA is representing 0 percent of measurement, 50 mA is representing 100 percent.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANALOG CURRENT LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4-20 mA SIGNAL LOOP",null,null,null,null,null,"rdl:RDS1422802561",null,"A <4-20 mA SIGNAL LOOP> is an <ANALOG CURRENT LOOP> where 4 mA is representing 0 percent of measurement, 20 mA is representing 100 percent.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONTROL LOOP",null,null,null,null,null,"rdl:RDS290249",null,"A <CONTROL LOOP> is an <ELECTRONIC CIRCUIT> that is an assembly of elements comprising a comparing element, the corresponding forward path and the corresponding feedback path.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT LOOP",null,null,null,null,null,"rdl:RDS1422782601",null,"A <CURRENT LOOP> is an <ELECTRONIC CIRCUIT> that uses current for signaling.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CURRENT LOOP","DIGITAL LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIGITAL CURRENT LOOP",null,null,null,null,null,"rdl:RDS1422793541",null,"A <DIGITAL CURRENT LOOP> is a <DIGITAL LOOP> and a <CURENT LOOP> where the electric signals take on discrete values to represent logical and numeric values.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIGITAL LOOP",null,null,null,null,null,"rdl:RDS1423277371",null,"A <DIGITAL LOOP> is an <ELECTRONIC CIRCUIT> in which data is represented by trains of pulses.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIGITAL LOOP","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIELDBUS",null,null,null,null,null,"rdl:RDS2222904",null,"A <FIELDBUS> is a <SIGNAL CONVEYING ITEM> and a <DIGITAL LOOP> that is an all-digital, serial, two-way communications system that serves as the base-level network in a plant or factory automation environment. It is an open architecture, developed and administered by the Fieldbus Foundation. It is targeted for applications using basic and advanced regulatory control, and for much of the discrete control associated with those functions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FIELDBUS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOUNDATION Fieldbus H1",null,null,null,null,null,"rdl:RDS2222905",null,"A <FOUNDATION Fieldbus H1> is a <FIELDBUS> that operates at 31.25 kbit/s and is generally used to connect to field devices and host systems. It provides communication and power over standard stranded twisted-pair wiring in both conventional and intrinsic safety applications. H1 is currently the most common implementation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FIELDBUS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HIGH SPEED ETHERNET (HSE)",null,null,null,null,null,"rdl:RDS2222906",null,"A <HIGH SPEED ETHERNET (HSE)> is a <FIELDBUS> that operates at 100/1000 Mbit/s and generally connects input/output subsystems, host systems, linking devices and gateways. It does not currently provide power over the cable, although work is under way to address this using the IEEE802.3af Power over Ethernet (PoE) standard",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIGITAL LOOP","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HART",null,null,null,null,null,"rdl:RDS2222903",null,"A <HART> is a <SIGNAL CONVEYING ITEM> and a <DIGITAL LOOP> that is compliant with the HART Communications Protocol (Highway Addressable Remote Transducer)and is an early implementation of <FIELDBUS>. Its most notable advantage is that it can communicate over legacy 4-20 mA analog instrumentation wiring, sharing the pair of wires used by the older system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIGITAL LOOP","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MODBUS RS-485",null,null,null,null,null,"rdl:RDS2222910",null,"A <MODBUS RS-485> is a <SIGNAL CONVEYING ITEM> and a <DIGITAL LOOP> that is compliant with TIA-495 that is a standard defining the electrical characteristics of drivers and receivers for use in balanced digital multipoint systems. The standard is published by the Telecommunications Industry Association/Electronic Industries Alliance (TIA/EIA). Digital communications networks implementing the standard can be used effectively over long distances and in electrically noisy environments. Multiple receivers may be connected to such a network in a linear, multi-drop configuration. These characteristics make such networks useful in industrial environments and similar applications",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIGITAL LOOP","SIGNAL CONVEYING ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROFIBUS",null,null,null,null,null,"rdl:RDS2222907",null,"A <PROFIBUS> is a <SIGNAL CONVEYING ITEM> and a <DIGITAL LOOP> that is a standard for fieldbus communication in automation technology and was first promoted in 1989 by BMBF (German department of education and research); it is openly published as part of IEC 61158. It has two variations: PA (Process Automation) and DP (Decentralised Peripherals). PA uses the same protocol as DP, and can be linked to a DP network using a coupler device. The much faster DP acts as a backbone network for transmitting process signals to the controller. This means that DP and PA can work tightly together, especially in hybrid applications where process and factory automation networks operate side by side",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PROFIBUS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROFIBUS DP",null,null,null,null,null,"rdl:RDS2222908",null,"A <PROFIBUS DP> is a <PROFIBUS> that is used to operate sensors and actuators via a centralised controller in production (factory) automation applications. The many standard diagnostic options, in particular, are focused on here",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PROFIBUS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROFIBUS PA",null,null,null,null,null,"rdl:RDS2222909",null,"A <PROFIBUS PA> is a <PROFIBUS> that is used to monitor measuring equipment via a process control system in process automation applications. This variant is designed for use in explosion/hazardous areas (Ex-zone 0 and 1). The Physical Layer (i.e. the cable) conforms to IEC 61158-2, which allows power to be delivered over the bus to field instruments, while limiting current flows so that explosive conditions are not created, even if a malfunction occurs. The number of devices attached to a PA segment is limited by this feature. PA has a data transmission rate of 31.25 kbit/s",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OPEN LOOP",null,null,null,null,null,"rdl:RDS290294",null,"An <OPEN LOOP> is an <ELECTRONIC CIRCUIT> where a signal path has no feedback path.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE LOOP",null,null,null,null,null,"rdl:RDS1422784941",null,"A <VOLTAGE LOOP> is an <ELECTRONIC CIRCUIT> that uses voltage for signaling.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRIC CIRCUIT",null,null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRATED CIRCUIT",null,null,null,null,null,"rdl:RDS7024354",null,"An <INTEGRATED CIRCUIT> is an <ARTEFACT> and an <ELECTRIC CIRCUIT> that is made as a single indivisible structure (such as a chip) and is electrically equivalent to a conventional circuit of many separate components",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTEGRATED CIRCUIT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEMORY CHIP",null,null,null,null,null,"rdl:RDS7022905",null,"A <MEMORY CHIP> is an <INTEGRATED CIRCUIT> that is intended to store computerized information",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRIC CIRCUIT",null,null,null,null,null,null,null,null,null,null,null,null,null,"INTRINSICALLY SAFE CIRCUIT",null,null,null,null,null,"rdl:RDS5036404640",null,"An <INTRINSICALLY SAFE CIRCUIT> is an <ARTEFACT> and a <ELECTRIC CIRCUIT> in which any spark or thermal effect produced either normally or in specified fault conditions is incapable, in the specified test conditions, of causing ignition of a given gas or vapour",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL NETWORK",null,null,null,null,null,null,null,null,null,null,null,null,"EQUIVALENT NETWORK SYSTEM",null,null,null,null,null,"rdl:RDS7009975",null,"An <EQUIVALENT NETWORK SYSTEM> is an <ARTEFACT> and an <ELECTRICAL NETWORK> that may replace a given network without changing the state variables at specified boundary nodes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ELECTRICAL NETWORK",null,null,null,null,null,null,null,null,null,null,null,null,"NETWORK TOPOLOGY",null,null,null,null,null,"rdl:RDS17919025",null,"A <NETWORK TOPOLOGY> is an <ARTEFACT> and an <ELECTRICAL NETWORK> where the relative positions of the ideal elements are representing an electrical network",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLUID SYSTEM","NETWORK",null,null,null,null,null,null,null,null,null,null,null,"PIPING NETWORK SYSTEM",null,null,null,null,null,"rdl:RDS270359",null,"A <PIPING NETWORK SYSTEM> is a <NETWORK> and a <FLUID SYSTEM> of interconnected piping network branches limited by Unit Operation Inlet/Outlet and Piping Network Terminators. In this context Piping includes e.g. plumbing and tubing",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","PIPING NETWORK SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,"LINE(fluid)",null,null,null,null,null,"rdl:RDS2223299",null,"A <LINE(fluid)> is an <ARTEFACT> and a <PIPING NETWORK SYSTEM> that is a part of the <PIPING NETWORK> of a plant that has the same function, pipe class, and Line Number",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","PIPING NETWORK SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,"PIPING STANDARD ASSEMBLY",null,null,null,null,null,"rdl:RDS369443411",null,"A <PIPING STANDARD ASSEMBLY> is an <ARTEFACT> and a <PIPING NETWORK SYSTEM> that is a standardised assembly of e.g. pipes, tubes, pipe fittings, pipe flanges and valves designed to perform standardised operations",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPING STANDARD ASSEMBLY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXHAUST PIPING STANDARD ASSEMBLY",null,null,null,null,null,"rdl:RDS403501741",null,"An <EXHAUST PIPING STANDARD ASSEMBLY> is a <PIPING STANDARD ASSEMBLY> that is intended to transport exhaust gas or steam.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","PIPING NETWORK SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,"PIPING SYSTEM",null,null,null,null,null,"rdl:RDS6809993",null,"A <PIPING SYSTEM> is an <ARTEFACT> and a <PIPING NETWORK SYSTEM> that is designed for conveyance of fluids by use of pipes, tubes, pipe fittings, valves etc. and connected process equipment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPING SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHRISTMAS TREE",null,null,null,null,null,"rdl:RDS16663020",null,"A <CHRISTMAS TREE> is a <PIPING SYSTEM> that is an assembly of pipes and piping parts, with valves and associated control equipment that is connected to the top of a wellhead and is intended for control of fluid from a well.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHRISTMAS TREE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HORIZONTAL CHRISTMAS TREE",null,null,null,null,null,"rdl:RDS16447332",null,"A <HORIZONTAL CHRISTMAS TREE> is a <CHRISTMAS TREE> configured with the master valves and flow-control equipment on a horizontal axis off the tree bore.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HORIZONTAL CHRISTMAS TREE","SURFACE CHRISTMAS TREE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SURFACE HORIZONTAL CHRISTMAS TREE",null,null,null,null,null,"rdl:RDS16663433",null,"A <SURFACE HORIZONTAL CHRISTMAS TREE> is a <HORIZONTAL CHRISTMAS TREE> and a <SURFACE CHRISTMAS TREE>, where the valves are normally bolted on.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHRISTMAS TREE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA CHRISTMAS TREE",null,null,null,null,null,"rdl:RDS7168366",null,"A <SUBSEA CHRISTMAS TREE> is a <CHRISTMAS TREE> for use in a subsea environment that will normally comprise a hollow, pressure rated body with the valves either built in or bolted on.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA CHRISTMAS TREE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA CHRISTMAS TREE HUB END",null,null,null,null,null,"rdl:RDS16679787",null,"A <SUBSEA CHRISTMAS TREE HUB END> is a <SUBSEA CHRISTMAS TREE> where at least one of the ends is a hub end.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA CHRISTMAS TREE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA CHRISTMAS TREE MANDREL END",null,null,null,null,null,"rdl:RDS16679897",null,"A <SUBSEA CHRISTMAS TREE MANDREL END> is a <SUBSEA CHRISTMAS TREE> where at least one of the ends is a mandrel end.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA CHRISTMAS TREE","VERTICAL CHRISTMAS TREE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA VERTICAL CHRISTMAS TREE",null,null,null,null,null,"rdl:RDS16663478",null,"A <SUBSEA VERTICAL CHRISTMAS TREE> is a <SUBSEA CHRISTMAS TREE> and a <VERTICAL CHRISTMAS TREE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHRISTMAS TREE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SURFACE CHRISTMAS TREE",null,null,null,null,null,"rdl:RDS16663133",null,"A <SURFACE CHRISTMAS TREE> is a <CHRISTMAS TREE> for use on land that will normally comprise a number of assembled parts, e.g. casing spools, with the valves bolted onto the outside.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHRISTMAS TREE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VERTICAL CHRISTMAS TREE",null,null,null,null,null,"rdl:RDS16447377",null,"A <VERTICAL CHRISTMAS TREE> is a <CHRISTMAS TREE> configured with the master valves and flow-control equipment on a vertical axis that is the main axis of the tree.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPING SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COOLING WATER PIPING SYSTEM",null,null,null,null,null,"rdl:RDS16768989",null,"A <COOLING WATER PIPING SYSTEM> is a <PIPING SYSTEM> that is intended to transport cooling water to and from equipment.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPING SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DISCHARGE PIPING SYSTEM",null,null,null,null,null,"rdl:RDS402645721",null,"A <DISCHARGE PIPING SYSTEM> is a <PIPING SYSTEM> that is located at the discharge of subject equipment through which pressurized fluid is transported.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPING SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW LOOP",null,null,null,null,null,"rdl:RDS16695458",null,"A <FLOW LOOP> is a <PIPING SYSTEM> consisting of a short length of pipe, for connecting between two fixed points.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOW LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CROSSOVER FLOW LOOP",null,null,null,null,null,"rdl:RDS16556343",null,"A <CROSSOVER FLOW LOOP> is a <FLOW LOOP> intended for connecting the production bore with the annulus bore on a subsea christmas tree.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOW LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS INJECTION FLOW LOOP",null,null,null,null,null,"rdl:RDS16695639",null,"A <GAS INJECTION FLOW LOOP> is a <FLOW LOOP> on a christmas tree for gas injection.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS INJECTION FLOW LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS INJECTION FLOW LOOP NPS 3",null,null,null,null,null,"rdl:RDS16695735",null,"A <GAS INJECTION FLOW LOOP NPS 3> is a <GAS INJECTION FLOW LOOP> that has a nominal ID of 3 inches.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOW LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MY FLOW LOOP TYPE",null,null,null,null,null,"rdl:RDS2299404481",null,"A <MY FLOW LOOP TYPE> is a <FLOW LOOP> consisting of a short length of pipe, for connecting between two fixed points.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOW LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PIG LOOP",null,null,null,null,null,"rdl:RDS16556388",null,"A <PIG LOOP> is a <FLOW LOOP> having a U-shape that allows a pipeline pig to move from one pipe to another.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIG LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA PIG LOOP",null,null,null,null,null,"rdl:RDS16556433",null,"A <SUBSEA PIG LOOP> is a <PIG LOOP> connected to a subsea structure.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOW LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRODUCTION FLOW LOOP",null,null,null,null,null,"rdl:RDS16693900",null,"A <PRODUCTION FLOW LOOP> is a <FLOW LOOP> consisting of a length of pipe extending from the production outlet on a christmas tree to the wing hub.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PRODUCTION FLOW LOOP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRODUCTION FLOW LOOP NPS 5",null,null,null,null,null,"rdl:RDS16694013",null,"A <PRODUCTION FLOW LOOP NPS 5> is a <PRODUCTION FLOW LOOP> with a nominal ID of 5 inches.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPING SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PIPING AND VALVES SYSTEM",null,null,null,null,null,"rdl:RDS412404361",null,"A <PIPING AND VALVES SYSTEM> is a <PIPING SYSTEM> that is a collection or one or more assemblies of piping as well as piping components together with valves.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPING SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PIPING ASSEMBLY",null,null,null,null,null,"rdl:RDS4723320",null,"A <PIPING ASSEMBLY> is a <PIPING SYSTEM> designed and mounted on a machine or equipment in order to perform a defined auxilary function.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPING SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PURGE PIPING SYSTEM",null,null,null,null,null,"rdl:RDS414093041",null,"A <PURGE PIPING SYSTEM> is a <PIPING SYSTEM> that is situated within the frame and distributes purge gas inside the frame.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPING SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEAL FLUSHING PIPING SYSTEM",null,null,null,null,null,"rdl:RDS418573241",null,"A <SEAL FLUSHING PIPING SYSTEM> is a <PIPING SYSTEM> that consists of piping and piping components belonging to a seal flush system.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPING SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEAL PIPING SYSTEM",null,null,null,null,null,"rdl:RDS418619971",null,"A <SEAL PIPING SYSTEM> is a <PIPING SYSTEM> intended to be used to transport sealing fluid.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPING SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STEAM PIPING SYSTEM",null,null,null,null,null,"rdl:RDS424694371",null,"A <STEAM PIPING SYSTEM> is a <PIPING SYSTEM> through which steam is transported.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPING SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUCTION PIPING SYSTEM",null,null,null,null,null,"rdl:RDS426402071",null,"A <SUCTION PIPING SYSTEM> is a <PIPING SYSTEM> through which fluid is transported to the suction side of any piece of equipment.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPING SYSTEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUCTION VALVE UNLOADING SYSTEM",null,null,null,null,null,"rdl:RDS426407281",null,"A <SUCTION VALVE UNLOADING SYSTEM> is a <PIPING SYSTEM> that is a control system that contains the manual/automatic setpoint operators in conjunction with the electronic/pneumatic control logic.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]