{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["RDL browser","Settings","about","Results1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"RDL browser","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[[0,0,0,4]]}
["RDL2 browser to spreadsheet tool version 75",null,null,null,null,null,"Endpoint: http://data.15926.org/rdl/"]
["Contact: onno.paap@gmail.com",null,null,null,null,"Action","AIR PRESSURE REGULATOR","http://data.15926.org/rdl/RDS5794822"]
[null,null,null,null,null,"Action","AIR PRESSURE REGULATOR AND FILTER","http://data.15926.org/rdl/RDS5794965"]
["Search:","REGULATOR",null,null,null,"Action","BACK PRESSURE REGULATOR","http://data.15926.org/rdl/RDS1011194"]
[null,null,null,null,null,"Action","CONSTANT VOLUME REGULATOR","http://data.15926.org/rdl/RDS297494"]
[null,null,null,null,null,"Action","CURRENT REGULATOR","http://data.15926.org/rdl/RDS7124120"]
[null,null,null,null,null,"Action","DAILY ESTIM LOSS OF PRODUCTION DUE TO REGULATORY REFERENCE - SM3 DEFINITION","http://data.15926.org/rdl/RDS16977246"]
[null,null,null,null,null,"Action","DAILY ESTIMATED LOSS OF PRODUCTION VOLUME DUE TO REGULATORY REASONS DEFINITION","http://data.15926.org/rdl/RDS16977291"]
[null,null,null,null,null,"Action","DIFFERENTIAL PRESSURE REGULATOR","http://data.15926.org/rdl/RDS879344"]
[null,null,null,null,null,"Action","DIRECT OPERATED PRESSURE REGULATOR","http://data.15926.org/rdl/RDS879524"]
[null,null,null,null,null,"Action","FLOW REGULATOR","http://data.15926.org/rdl/RDS880109"]
[null,null,null,null,null,"Action","FLUID REGULATOR","http://data.15926.org/rdl/RDS278369"]
[null,"Note: first set coloring on in Settings",null,null,null,"Action","FLUID REGULATOR CAP","http://data.15926.org/rdl/RDS13036125"]
[null,"Coloring (containing this string will give this color)",null,null,null,"Action","FLUID REGULATOR EQUIPMENT CLASS","http://data.15926.org/rdl/RDS202814"]
[null,"ClassOfFunctionalObject",null,null,null,"Action","LEGAL REGULATORY AND SOCIAL CONSTRAINTS","http://data.15926.org/rdl/RDS330344"]
[null,"ClassOfInanimatePhysicalObject ",null,null,null,"Action","LEVEL REGULATOR","http://data.15926.org/rdl/RDS880739"]
[null,null,null,null,null,"Action","PILOT OPERATED REGULATOR","http://data.15926.org/rdl/RDS882134"]
[null,null,null,null,null,"Action","PRESSURE REGULATOR","http://data.15926.org/rdl/RDS309149"]
[null,null,null,null,null,"Action","PRESSURE REGULATOR VALVE","http://data.15926.org/rdl/RDS309284"]
[null,null,null,null,null,"Action","REGULATOR","http://data.15926.org/rdl/RDS7198580"]
[null,null,null,null,null,"Action","REGULATOR(manager)","http://data.15926.org/rdl/RDS2220906"]
[null,null,null,null,null,"Action","REGULATORY AGREEMENT","http://data.15926.org/rdl/RDS330929"]
[null,null,null,null,null,"Action","REGULATORY AUTHORIZATIONS","http://data.15926.org/rdl/RDS334034"]
[null,null,null,null,null,"Action","REGULATORY BODY","http://data.15926.org/rdl/RDS283544"]
[null,"Namespace replacer (definition containing this string replaces the namespace)",null,null,null,"Action","REGULATORY COMPLYING","http://data.15926.org/rdl/RDS10795609"]
[null,"API","API:",null,null,"Action","REGULATORY REQUIREMENT DEFINITION","http://data.15926.org/rdl/RDS330884"]
[null,"ASME","ASME:",null,null,"Action","REGULATORY REQUIREMENT SPECIFICATION","http://data.15926.org/rdl/RDS14162370"]
[null,"ASTM","ASTM:",null,null,"Action","TEMPERATURE REGULATOR","http://data.15926.org/rdl/RDS1011284"]
[null,"DIN","DIN:",null,null,"Action","VOLTAGE REGULATOR","http://data.15926.org/rdl/RDS7124200"]
[null,"EN","EN:",null,null,"Action","VOLTAGE-REGULATOR DIODE","http://data.15926.org/rdl/RDS6646900"]
[null,"ISO","ISO:"]
[null,"NORSOK","NOR:"]
[null,"NPD","NOR:"]
[null,"NS","NOR:"]
[null,"ROSEMOUNT","ROS:"]
[null,"SAE","SAE:"]
[null,"SIEMENS","SIE:"]
[null,"SKOTSELV","SKOT:"]
[null,"TWR","TWR:"]

{"sheet":"Settings","index":1,"n_rows":87,"n_cols":8,"rows_kept":87,"cut":false,"hidden":true,"merged":[]}
["Setting name","Select name","OnKey","Value","Status","RDLType"]
["Endpoint","RDL2 (15926.org)",null,"http://data.15926.org/rdl/","Current",null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA RDL",null,"http://data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA Staging",null,"http://staging.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA SVRDL",null,"http://svrdl.community.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P4",null,"http://posccaesar.org/p4/sparql",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P12",null,"http://sti.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","Localhost",null,"http://localhost:8890/sparql/",null,null,null,"Note: end address always with a slash (/)"]
[]
["gBaseNamespace",null,"http://data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://staging.data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://svrdl.community.data.posccaesar.org/rdl/","http://svrdl.community.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://posccaesar.org/p4/sparql","http://posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://sti.data.posccaesar.org/rdl/","http://sti.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://localhost:8890/sparql/","http://data.15926.org/rdl/",null,"RDL2"]
["gKeepSettings",null,null,"T"]
["gShowDeprecated",null,null,"F"]
["gColoring",null,null,"T"]
["gNamespaceReplacing",null,null,"F"]
["gHyperlinkReplacing",null,null,"F"]
[]
["Endpoint","aisi",null,"http://data.15926.org/aisi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ansi",null,"http://data.15926.org/ansi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","api",null,"http://data.15926.org/api/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","all",null,"http://data.15926.org/all/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","asme",null,"http://data.15926.org/asme/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","astm",null,"http://data.15926.org/astm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","atex",null,"http://data.15926.org/atex/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","bs",null,"http://data.15926.org/bs/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","din",null,"http://data.15926.org/din/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dm",null,"http://data.15926.org/dm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dnv",null,"http://data.15926.org/dnv/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","edm",null,"http://data.15926.org/edm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","en",null,"http://data.15926.org/en/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","eu",null,"http://data.15926.org/eu/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iec",null,"http://data.15926.org/iec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ieee",null,"http://data.15926.org/ieee/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iso",null,"http://data.15926.org/iso/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","lci",null,"http://data.15926.org/lci/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","mss",null,"http://data.15926.org/mss/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nace",null,"http://data.15926.org/nace/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nec",null,"http://data.15926.org/nec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nema",null,"http://data.15926.org/nema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nfpa",null,"http://data.15926.org/nfpa/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nor",null,"http://data.15926.org/nor/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","rdl",null,"http://data.15926.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sae",null,"http://data.15926.org/sae/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sie",null,"http://data.15926.org/sie/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","tema",null,"http://data.15926.org/tema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","twr",null,"http://data.15926.org/twr/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","uns",null,"http://data.15926.org/uns/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","wits",null,"http://data.15926.org/wits/",null,null,null,"Note: end address always with a slash (/)"]
[]
[]
["gBaseNamespace",null,"http://data.15926.org/aisi/","http://data.15926.org/aisi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ansi/","http://data.15926.org/ansi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/api/","http://data.15926.org/api/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/asme/","http://data.15926.org/asme/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/all/","http://data.15926.org/all/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/astm/","http://data.15926.org/astm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/atex/","http://data.15926.org/atex/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/bs/","http://data.15926.org/bs/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/din/","http://data.15926.org/din/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dm/","http://data.15926.org/dm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dnv/","http://data.15926.org/dnv/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/edm/","http://data.15926.org/edm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/en/","http://data.15926.org/en/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/eu/","http://data.15926.org/eu/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iec/","http://data.15926.org/iec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ieee/","http://data.15926.org/ieee/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iso/","http://data.15926.org/iso/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/lci/","http://data.15926.org/lci/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/mss/","http://data.15926.org/mss/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nace/","http://data.15926.org/nace/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nec/","http://data.15926.org/nec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nema/","http://data.15926.org/nema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nfpa/","http://data.15926.org/nfpa/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nor/","http://data.15926.org/nor/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sae/","http://data.15926.org/sae/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sie/","http://data.15926.org/sie/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/tema/","http://data.15926.org/tema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/twr/","http://data.15926.org/twr/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/uns/","http://data.15926.org/uns/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/wits/","http://data.15926.org/wits/",null,"RDL2"]
["                                          "]

{"sheet":"about","index":2,"n_rows":176,"n_cols":3,"rows_kept":176,"cut":false,"hidden":false,"merged":[]}
["Version 75 changes","2018-10-05","Onno Paap"]
["missing superclasses - and orphans- filter no deprecated classes"]
[]
["Version 74 changes","2018-09-30","Onno Paap"]
["Repaired bug missing label"]
[]
["Version 73 changes","2018-05-16","Onno Paap"]
["Repaired bug Deprecated Superclass"]
[]
[]
[]
["Version 71 changes","2016-07-17","Onno Paap"]
["Aded report button for comparison of RDL2 with a subfolder called views filled with spreadsheets."]
[]
[]
["Version 69 changes","2016-06-16","Onno Paap"]
["Added button: \"errors in definitions\" that lists all classes that have more or less \"<\" brackets than the number of super class relationships + 1. Where the part after the word \"that \"  is ignored in the count of \"<\" brackets."]
[]
["Version 68 changes","2016-06-13","Onno Paap"]
["Updated endpoint of RDL2 sparql "]
[]
["Version 67 changes","2016-05-22","Onno Paap"]
["Added button list subclasses from superclass "]
[]
["Version 65 changes","2016-04-25","Onno Paap"]
["Added checkbox at action dialog \"supress double child occurances\" so that this built-in feature can be switched off"]
[]
["Version 64 changes","2016-04-20","Onno Paap"]
["Made search case-insensitive and added endpoint \"all\""]
[]
["Version 63 changes","2016-09-28","Onno Paap"]
["Made entity list working on P4 endpoint (they changed the database version which was not accepting som sparql setting)"]
["Version 62 changes","2016-09-28","Onno Paap"]
["Applied show deprecated to searched result list"]
[]
["Version 61 changes","2016-08-29","Onno Paap"]
["Added query from pcardl for ClassOfIndirectProperty"]
[]
["Version 60 changes","2016-08-19","Onno Paap"]
["Repaired failing entity reports"]
[]
["Version 59 changes","2016-08-19","Onno Paap"]
["Missing superclasses now queries whole federation of RDL2"]
[]
["Version 58 changes","2016-08-16","Onno Paap"]
["Repaired missing output for entities and doubles in RDL2 endpoints other than rdl"]
[]
["Version 57 changes","2016-08-13","Onno Paap"]
["Doubles report now skips classes that are deprecated"]
[]
["Version 56 changes","2016-07-22","Onno Paap"]
["Made rowheight suitable for longer definitions to example DESIGN BASIS"]
[]
["Version 55 changes","2016-07-19","Onno Paap"]
["Made rowheight suitable for longer definitions"]
[]
["Version 54 changes","2016-07-03","Onno Paap"]
["Entity Type field changed to 6 merged cells."]
[]
["Version 53 changes","2016-06-23","Onno Paap"]
["added lci namespace"]
[]
["Version 52 changes","2016-06-23","Onno Paap"]
["Added deprecated count to list entities"]
[]
["Version 51 changes","2016-06-19","Onno Paap"]
["Updated namespaces of staging RDL"]
[]
["Version 50 changes","2016-06-19","Onno Paap"]
["taxonomy view repaired missing entity type"]
[]
["Version 49 changes","2016-06-14","Onno Paap"]
["Room for 12 superclasses"]
[]
["Version 48 changes","2016-06-14","Onno Paap"]
["Repaired NOR:/RDS  bug"]
[]
["Version 47 changes","2016-06-14","Onno Paap"]
["Repaired endpoint bug"]
[]
["Version 46 changes","2016-06-13","Onno Paap"]
["Updated endpoints"]
[]
["Version 45 changes","2016-06-06","Onno Paap"]
["Completed Missing Superclasses report"]
[]
["Version 44 changes","2016-05-20","Onno Paap"]
["Added Clear Cache button (use on any database changes)"]
[]
["Version 43 changes","2016-05-19","Onno Paap"]
["Changed non-existing super classes to show as \"no label\""]
[]
["Version 42 changes","2016-05-02","Onno Paap"]
["bug fix"]
[]
["Version 41 changes","2016-05-02","Onno Paap"]
["Added setting to show/not show deprecated items. If shown, they are stricken through"]
[]
["Version 40 changes","2016-03-31","Onno Paap"]
["Added  in doubles: two classes having the same label."]
[]
["Version 39 changes","2016-03-21","Onno Paap"]
["Made the query more robust, after the server hass been returning a 404 occasionally"]
[]
["Version 38 changes","2016-03-03","Onno Paap"]
["Repaired bug entity type query on PCA endpoint"]
[]
["Version 37 changes","2016-01-29","Onno Paap"]
["Showing deprecated class in taxonomy with label in strikethrough."]
[]
["Version 36 changes","2016-01-13","Onno Paap"]
["Added the 17 endpoints of http://data.15926.org/rdl"]
[]
["Version 35 changes","2016-01-13","Onno Paap"]
["In taxonomy view, disregard all rdf:type that is not data model.  So only show rdf:type that is dm:"]
[]
["Version 34 changes","2016-01-13","Onno Paap"]
["Solved taxonomy levels regression bug"]
[]
["Version 33 changes","2016-01-11","Onno Paap"]
["Enhanced the doubled query. First 4 columns are about the triple, the rest is info."]
[]
["Repaired bug in entity type query."]
[]
["Version 30 changes","2016-01-03","Onno Paap"]
["Repaired entity type query for old PCA RDL. \nRepaired bug in entity type query where a class that has a superclass of the wanted type as well as  of another type became  the start point of a new taxonomy as well as part in the main taxonomy. (read that again)"]
[]
["Version 29 changes","2016-01-02","Onno Paap"]
["Filtered entity filtered taxonomy to only show the filtered entity not subClassOf of another entity"]
[]
["Version 27 changes","2016-01-01","Onno Paap"]
["few bugs repaired.  Changed entity search into presenting taxonomies. "]
[]
["Version 26 changes","2015-12-26","Onno Paap"]
["few bugs repaired. "]
[]
["Version 25 changes","2015-12-26","Onno Paap"]
["Added Part 12 and localhost endpoints"]
["Added button for selecting double labels and definitions. "]
["Version 24 changes","2015-12-14","Onno Paap"]
["Added button to list all distinct entity data types and their counts, and click to show."]
["Added a button to show all orphans that have a rdfs:label"]
["Version 23 changes"]
["Added endpoint posccaesar.org/p4/sparql"]
["Version 22 changes"]
["Added endpoint staging.data.posccaesar.org/rdl"]
[]
["Version 21 changes"]
["Repaired bug where namespace replace was based upon definition instead of class label"]
[]
["Version 20 changes"]
["Repaired bug where definition did not show up if hyperlink replace was on."]
[]
["Version 19 changes (skip version 16-18)"]
["Settings expanded with persist settings, namespace replacer and hyperlink replacer"]
["Added namespace replacer which will replace the RDL: namespace of the ID with the namespace given in the list on the front page."]
["Added hyperlink replacer which will find terms between single quotes and look them up in the RDL, then add a hyperlink in the text if found. Anchor tag <a></a> used not &hyperlink() so looks ugly."]
[]
["Version 15 changes"]
["Changed browser page Action buttons to hyperlinks because buttons are not equally spaced between Excel versions (Office 2007 versus Office 365)"]
["First row is empty. Move all up."]
["Make stop button for during query taxonomy query execution"]
[]
[]
["Version 14 changes"]
["Aligned buttons on browser page"]
["Made color notification work. Note: switch it on first in settings. Default is off"]
["Top align subclasses in taxonomy"]
["Subclasses made to hyperlink in taxonomy"]
["Subclasses made to increase column width in taxonomy"]
["Made browser search go when hitting enter in search field"]
[]
[]
[]
["todo"]
["Make setting for outputting to other result pages"]

{"sheet":"Results1","index":3,"n_rows":404,"n_cols":37,"rows_kept":404,"cut":false,"hidden":false,"merged":[[402,24,402,25],[402,18,402,23],[402,26,402,31],[402,32,402,35],[403,21,403,22],[403,15,403,20],[403,23,403,28],[403,29,403,32],[400,23,400,24],[400,17,400,22],[400,25,400,30],[400,31,400,34],[401,23,401,24],[401,17,401,22],[401,25,401,30],[401,31,401,34],[398,23,398,24],[398,17,398,22],[398,25,398,30],[398,31,398,34],[399,23,399,24],[399,17,399,22],[399,25,399,30],[399,31,399,34],[396,23,396,24],[396,17,396,22],[396,25,396,30],[396,31,396,34],[397,23,397,24],[397,17,397,22],[397,25,397,30],[397,31,397,34],[394,23,394,24],[394,17,394,22],[394,25,394,30],[394,31,394,34],[395,23,395,24],[395,17,395,22],[395,25,395,30],[395,31,395,34],[392,23,392,24],[392,17,392,22],[392,25,392,30],[392,31,392,34],[393,23,393,24],[393,17,393,22],[393,25,393,30],[393,31,393,34],[390,23,390,24],[390,17,390,22],[390,25,390,30],[390,31,390,34],[391,23,391,24],[391,17,391,22],[391,25,391,30],[391,31,391,34],[388,23,388,24],[388,17,388,22],[388,25,388,30],[388,31,388,34],[389,23,389,24],[389,17,389,22],[389,25,389,30],[389,31,389,34],[386,24,386,25],[386,18,386,23],[386,26,386,31],[386,32,386,35],[387,25,387,26],[387,19,387,24],[387,27,387,32],[387,33,387,36],[384,24,384,25],[384,18,384,23],[384,26,384,31],[384,32,384,35],[385,24,385,25],[385,18,385,23],[385,26,385,31],[385,32,385,35],[382,23,382,24],[382,17,382,22],[382,25,382,30],[382,31,382,34],[383,23,383,24],[383,17,383,22],[383,25,383,30],[383,31,383,34],[380,23,380,24],[380,17,380,22],[380,25,380,30],[380,31,380,34],[381,24,381,25],[381,18,381,23],[381,26,381,31],[381,32,381,35],[378,25,378,26],[378,19,378,24],[378,27,378,32],[378,33,378,36],[379,23,379,24],[379,17,379,22],[379,25,379,30],[379,31,379,34],[376,24,376,25],[376,18,376,23],[376,26,376,31],[376,32,376,35],[377,25,377,26],[377,19,377,24],[377,27,377,32],[377,33,377,36],[374,25,374,26],[374,19,374,24],[374,27,374,32],[374,33,374,36],[375,24,375,25],[375,18,375,23],[375,26,375,31],[375,32,375,35],[372,26,372,27],[372,20,372,25],[372,28,372,33],[372,34,372,37],[373,24,373,25],[373,18,373,23],[373,26,373,31],[373,32,373,35],[370,25,370,26],[370,19,370,24],[370,27,370,32],[370,33,370,36],[371,26,371,27],[371,20,371,25],[371,28,371,33],[371,34,371,37],[368,26,368,27],[368,20,368,25],[368,28,368,33],[368,34,368,37],[369,26,369,27],[369,20,369,25],[369,28,369,33],[369,34,369,37],[366,27,366,28],[366,21,366,26],[366,29,366,34],[366,35,366,38],[367,28,367,29],[367,22,367,27],[367,30,367,35],[367,36,367,39],[364,26,364,27],[364,20,364,25],[364,28,364,33],[364,34,364,37],[365,27,365,28],[365,21,365,26],[365,29,365,34],[365,35,365,38],[362,26,362,27],[362,20,362,25],[362,28,362,33],[362,34,362,37],[363,26,363,27],[363,20,363,25],[363,28,363,33],[363,34,363,37],[360,26,360,27],[360,20,360,25],[360,28,360,33],[360,34,360,37],[361,26,361,27],[361,20,361,25],[361,28,361,33],[361,34,361,37],[358,27,358,28],[358,21,358,26],[358,29,358,34],[358,35,358,38],[359,26,359,27],[359,20,359,25],[359,28,359,33],[359,34,359,37],[356,27,356,28],[356,21,356,26],[356,29,356,34],[356,35,356,38],[357,27,357,28],[357,21,357,26],[357,29,357,34],[357,35,357,38],[354,25,354,26],[354,19,354,24],[354,27,354,32],[354,33,354,36],[355,26,355,27],[355,20,355,25],[355,28,355,33],[355,34,355,37],[352,24,352,25],[352,18,352,23],[352,26,352,31],[352,32,352,35],[353,25,353,26],[353,19,353,24],[353,27,353,32],[353,33,353,36],[350,25,350,26],[350,19,350,24],[350,27,350,32],[350,33,350,36],[351,25,351,26],[351,19,351,24],[351,27,351,32],[351,33,351,36],[348,25,348,26],[348,19,348,24],[348,27,348,32],[348,33,348,36],[349,25,349,26],[349,19,349,24],[349,27,349,32],[349,33,349,36],[346,25,346,26],[346,19,346,24],[346,27,346,32],[346,33,346,36],[347,25,347,26],[347,19,347,24],[347,27,347,32],[347,33,347,36],[344,25,344,26],[344,19,344,24],[344,27,344,32],[344,33,344,36],[345,25,345,26],[345,19,345,24],[345,27,345,32],[345,33,345,36],[342,24,342,25],[342,18,342,23],[342,26,342,31],[342,32,342,35],[343,25,343,26],[343,19,343,24],[343,27,343,32],[343,33,343,36],[340,26,340,27],[340,20,340,25],[340,28,340,33],[340,34,340,37],[341,24,341,25],[341,18,341,23],[341,26,341,31],[338,25,338,26],[338,19,338,24],[338,27,338,32],[338,33,338,36],[339,26,339,27],[339,20,339,25],[339,28,339,33],[339,34,339,37],[336,27,336,28],[336,21,336,26],[336,29,336,34],[336,35,336,38],[337,27,337,28],[337,21,337,26],[337,29,337,34],[337,35,337,38],[334,26,334,27],[334,20,334,25],[334,28,334,33],[334,34,334,37],[335,27,335,28],[335,21,335,26],[335,29,335,34],[335,35,335,38],[332,24,332,25],[332,18,332,23],[332,26,332,31],[332,32,332,35],[333,25,333,26],[333,19,333,24],[333,27,333,32],[333,33,333,36],[330,24,330,25],[330,18,330,23],[330,26,330,31],[330,32,330,35],[331,25,331,26],[331,19,331,24],[331,27,331,32],[331,33,331,36],[328,23,328,24],[328,17,328,22],[328,25,328,30],[328,31,328,34],[329,23,329,24],[329,17,329,22],[329,25,329,30],[329,31,329,34],[326,25,326,26],[326,19,326,24],[326,27,326,32],[326,33,326,36],[327,24,327,25],[327,18,327,23],[327,26,327,31],[327,32,327,35],[324,26,324,27],[324,20,324,25],[324,28,324,33],[324,34,324,37],[325,26,325,27],[325,20,325,25],[325,28,325,33],[325,34,325,37],[322,25,322,26],[322,19,322,24],[322,27,322,32],[322,33,322,36],[323,26,323,27],[323,20,323,25],[323,28,323,33],[323,34,323,37],[320,25,320,26],[320,19,320,24],[320,27,320,32],[320,33,320,36],[321,26,321,27],[321,20,321,25],[321,28,321,33],[321,34,321,37],[318,24,318,25],[318,18,318,23],[318,26,318,31],[318,32,318,35],[319,25,319,26],[319,19,319,24],[319,27,319,32],[319,33,319,36],[316,25,316,26],[316,19,316,24],[316,27,316,32],[316,33,316,36],[317,26,317,27],[317,20,317,25],[317,28,317,33],[317,34,317,37],[314,25,314,26],[314,19,314,24],[314,27,314,32],[314,33,314,36],[315,25,315,26],[315,19,315,24],[315,27,315,32],[315,33,315,36],[312,25,312,26],[312,19,312,24],[312,27,312,32],[312,33,312,36],[313,24,313,25],[313,18,313,23],[313,26,313,31],[313,32,313,35],[310,26,310,27],[310,20,310,25],[310,28,310,33],[310,34,310,37],[311,26,311,27],[311,20,311,25],[311,28,311,33],[311,34,311,37],[308,25,308,26],[308,19,308,24],[308,27,308,32],[308,33,308,36],[309,26,309,27],[309,20,309,25],[309,28,309,33],[309,34,309,37],[306,25,306,26],[306,19,306,24],[306,27,306,32],[306,33,306,36],[307,25,307,26],[307,19,307,24],[307,27,307,32],[307,33,307,36],[304,25,304,26],[304,19,304,24],[304,27,304,32],[304,33,304,36],[305,25,305,26],[305,19,305,24],[305,27,305,32],[305,33,305,36],[302,26,302,27],[302,20,302,25],[302,28,302,33],[302,34,302,37],[303,26,303,27],[303,20,303,25],[303,28,303,33],[303,34,303,37],[300,26,300,27],[300,20,300,25],[300,28,300,33],[300,34,300,37],[301,26,301,27],[301,20,301,25],[301,28,301,33],[301,34,301,37],[298,25,298,26],[298,19,298,24],[298,27,298,32],[298,33,298,36],[299,25,299,26],[299,19,299,24],[299,27,299,32],[299,33,299,36],[296,25,296,26],[296,19,296,24],[296,27,296,32],[296,33,296,36],[297,25,297,26],[297,19,297,24],[297,27,297,32],[297,33,297,36],[294,23,294,24],[294,17,294,22],[294,25,294,30],[294,31,294,34],[295,24,295,25],[295,18,295,23],[295,26,295,31],[295,32,295,35],[292,23,292,24],[292,17,292,22],[292,25,292,30],[292,31,292,34],[293,23,293,24],[293,17,293,22],[293,25,293,30],[293,31,293,34],[290,25,290,26],[290,19,290,24],[290,27,290,32],[290,33,290,36],[291,25,291,26],[291,19,291,24],[291,27,291,32],[291,33,291,36],[288,23,288,24],[288,17,288,22],[288,25,288,30],[288,31,288,34],[289,24,289,25],[289,18,289,23],[289,26,289,31],[289,32,289,35],[286,24,286,25],[286,18,286,23],[286,26,286,31],[286,32,286,35],[287,24,287,25],[287,18,287,23],[287,26,287,31],[287,32,287,35],[284,25,284,26],[284,19,284,24],[284,27,284,32],[284,33,284,36],[285,23,285,24],[285,17,285,22],[285,25,285,30],[285,31,285,34],[282,23,282,24],[282,17,282,22],[282,25,282,30],[282,31,282,34],[283,24,283,25],[283,18,283,23],[283,26,283,31],[283,32,283,35],[279,34,279,37],[280,26,280,27],[280,20,280,25],[280,28,280,33],[280,34,280,37],[281,26,281,27],[281,20,281,25],[281,28,281,33],[281,34,281,37],[278,25,278,26],[278,19,278,24],[278,27,278,32],[279,26,279,27],[279,20,279,25],[279,28,279,33],[276,24,276,25],[276,18,276,23],[276,26,276,31],[276,32,276,35],[277,24,277,25],[277,18,277,23],[277,26,277,31],[277,32,277,35],[274,26,274,27],[274,20,274,25],[274,28,274,33],[274,34,274,37],[275,24,275,25],[275,18,275,23],[275,26,275,31],[275,32,275,35],[272,27,272,28],[272,21,272,26],[272,29,272,34],[272,35,272,38],[273,27,273,28],[273,21,273,26],[273,29,273,34],[273,35,273,38],[270,27,270,28],[270,21,270,26],[270,29,270,34],[270,35,270,38],[271,27,271,28],[271,21,271,26],[271,29,271,34],[271,35,271,38],[268,27,268,28],[268,21,268,26],[268,29,268,34],[268,35,268,38],[269,27,269,28],[269,21,269,26],[269,29,269,34],[269,35,269,38],[266,27,266,28],[266,21,266,26],[266,29,266,34],[266,35,266,38],[267,27,267,28],[267,21,267,26],[267,29,267,34],[267,35,267,38],[264,26,264,27],[264,20,264,25],[264,28,264,33],[264,34,264,37],[265,27,265,28],[265,21,265,26],[265,29,265,34],[265,35,265,38],[262,25,262,26],[262,19,262,24],[262,27,262,32],[262,33,262,36],[263,25,263,26],[263,19,263,24],[263,27,263,32],[263,33,263,36],[260,25,260,26],[260,19,260,24],[260,27,260,32],[260,33,260,36],[261,25,261,26],[261,19,261,24],[261,27,261,32],[261,33,261,36],[258,27,258,28],[258,21,258,26],[258,29,258,34],[258,35,258,38],[259,27,259,28],[259,21,259,26],[259,29,259,34],[259,35,259,38],[256,27,256,28],[256,21,256,26],[256,29,256,34],[256,35,256,38],[257,26,257,27],[257,20,257,25],[257,28,257,33],[257,34,257,37],[254,26,254,27],[254,20,254,25],[254,28,254,33],[254,34,254,37],[255,27,255,28],[255,21,255,26],[255,29,255,34],[255,35,255,38],[252,25,252,26],[252,19,252,24],[252,27,252,32],[252,33,252,36],[253,25,253,26],[253,19,253,24],[253,27,253,32],[253,33,253,36],[250,25,250,26],[250,19,250,24],[250,27,250,32],[250,33,250,36],[251,25,251,26],[251,19,251,24],[251,27,251,32],[251,33,251,36],[248,25,248,26],[248,19,248,24],[248,27,248,32],[248,33,248,36],[249,25,249,26],[249,19,249,24],[249,27,249,32],[249,33,249,36],[246,23,246,24],[246,17,246,22],[246,25,246,30],[246,31,246,34],[247,24,247,25],[247,18,247,23],[247,26,247,31],[247,32,247,35],[244,24,244,25],[244,18,244,23],[244,26,244,31],[244,32,244,35],[245,24,245,25],[245,18,245,23],[245,26,245,31],[245,32,245,35],[242,23,242,24],[242,17,242,22],[242,25,242,30],[242,31,242,34],[243,24,243,25],[243,18,243,23],[243,26,243,31],[243,32,243,35],[240,25,240,26],[240,19,240,24],[240,27,240,32],[240,33,240,36],[241,23,241,24],[241,17,241,22],[241,25,241,30],[241,31,241,34],[238,25,238,26],[238,19,238,24],[238,27,238,32],[238,33,238,36],[239,24,239,25],[239,18,239,23],[239,26,239,31],[239,32,239,35],[236,24,236,25],[236,18,236,23],[236,26,236,31],[236,32,236,35],[237,25,237,26],[237,19,237,24],[237,27,237,32],[237,33,237,36],[234,23,234,24],[234,17,234,22],[234,25,234,30],[234,31,234,34],[235,24,235,25],[235,18,235,23],[235,26,235,31],[235,32,235,35],[232,23,232,24],[232,17,232,22],[232,25,232,30],[232,31,232,34],[233,23,233,24],[233,17,233,22],[233,25,233,30],[233,31,233,34],[230,24,230,25],[230,18,230,23],[230,26,230,31],[230,32,230,35],[231,23,231,24],[231,17,231,22],[231,25,231,30],[231,31,231,34],[228,24,228,25],[228,18,228,23],[228,26,228,31],[228,32,228,35],[229,24,229,25],[229,18,229,23],[229,26,229,31],[229,32,229,35],[226,25,226,26],[226,19,226,24],[226,27,226,32],[226,33,226,36],[227,25,227,26],[227,19,227,24],[227,27,227,32],[227,33,227,36],[224,23,224,24],[224,17,224,22],[224,25,224,30],[224,31,224,34],[225,24,225,25],[225,18,225,23],[225,26,225,31],[225,32,225,35],[222,24,222,25],[222,18,222,23],[222,26,222,31],[222,32,222,35],[223,23,223,24],[223,17,223,22],[223,25,223,30],[223,31,223,34],[220,23,220,24],[220,17,220,22],[220,25,220,30],[220,31,220,34],[221,24,221,25],[221,18,221,23],[221,26,221,31],[221,32,221,35],[218,23,218,24],[218,17,218,22],[218,25,218,30],[218,31,218,34],[219,23,219,24],[219,17,219,22],[219,25,219,30],[219,31,219,34],[216,23,216,24],[216,17,216,22],[216,25,216,30],[216,31,216,34],[217,23,217,24],[217,17,217,22],[217,25,217,30],[217,31,217,34],[214,23,214,24],[214,17,214,22],[214,25,214,30],[214,31,214,34],[215,23,215,24],[215,17,215,22],[215,25,215,30],[215,31,215,34],[212,24,212,25],[212,18,212,23],[212,26,212,31],[212,32,212,35],[213,24,213,25],[213,18,213,23],[213,26,213,31],[213,32,213,35],[210,24,210,25],[210,18,210,23],[210,26,210,31],[210,32,210,35],[211,24,211,25],[211,18,211,23],[211,26,211,31],[211,32,211,35],[208,24,208,25],[208,18,208,23],[208,26,208,31],[208,32,208,35],[209,24,209,25],[209,18,209,23],[209,26,209,31],[209,32,209,35],[206,25,206,26],[206,19,206,24],[206,27,206,32],[206,33,206,36],[207,25,207,26],[207,19,207,24],[207,27,207,32],[207,33,207,36],[204,25,204,26],[204,19,204,24],[204,27,204,32],[204,33,204,36],[205,25,205,26],[205,19,205,24],[205,27,205,32],[205,33,205,36],[202,25,202,26],[202,19,202,24],[202,27,202,32],[202,33,202,36],[203,24,203,25],[203,18,203,23],[203,26,203,31],[203,32,203,35],[200,24,200,25],[200,18,200,23],[200,26,200,31],[200,32,200,35],[201,25,201,26],[201,19,201,24],[201,27,201,32],[201,33,201,36],[198,23,198,24],[198,17,198,22],[198,25,198,30],[198,31,198,34],[199,23,199,24],[199,17,199,22],[199,25,199,30],[199,31,199,34],[196,25,196,26],[196,19,196,24],[196,27,196,32],[196,33,196,36],[197,26,197,27],[197,20,197,25],[197,28,197,33],[197,34,197,37],[194,27,194,28],[194,21,194,26],[194,29,194,34],[194,35,194,38],[195,27,195,28],[195,21,195,26],[195,29,195,34],[195,35,195,38],[192,27,192,28],[192,21,192,26],[192,29,192,34],[192,35,192,38],[193,27,193,28],[193,21,193,26],[193,29,193,34],[193,35,193,38],[190,27,190,28],[190,21,190,26],[190,29,190,34],[190,35,190,38],[191,26,191,27],[191,20,191,25],[191,28,191,33],[191,34,191,37],[188,28,188,29],[188,22,188,27],[188,30,188,35],[188,36,188,39],[189,27,189,28],[189,21,189,26],[189,29,189,34],[189,35,189,38],[186,27,186,28],[186,21,186,26],[186,29,186,34],[186,35,186,38],[187,28,187,29],[187,22,187,27],[187,30,187,35],[187,36,187,39],[184,26,184,27],[184,20,184,25],[184,28,184,33],[184,34,184,37],[185,27,185,28],[185,21,185,26],[185,29,185,34],[185,35,185,38],[182,25,182,26],[182,19,182,24],[182,27,182,32],[182,33,182,36],[183,25,183,26],[183,19,183,24],[183,27,183,32],[183,33,183,36],[180,28,180,29],[180,22,180,27],[180,30,180,35],[180,36,180,39],[181,25,181,26],[181,19,181,24],[181,27,181,32],[181,33,181,36],[178,27,178,28],[178,21,178,26],[178,29,178,34],[178,35,178,38],[179,28,179,29],[179,22,179,27],[179,30,179,35],[179,36,179,39],[176,27,176,28],[176,21,176,26],[176,29,176,34],[176,35,176,38],[177,27,177,28],[177,21,177,26],[177,29,177,34],[177,35,177,38],[174,26,174,27],[174,20,174,25],[174,28,174,33],[174,34,174,37],[175,27,175,28],[175,21,175,26],[175,29,175,34],[175,35,175,38],[172,28,172,29],[172,22,172,27],[172,30,172,35],[172,36,172,39],[173,27,173,28],[173,21,173,26],[173,29,173,34],[173,35,173,38],[170,27,170,28],[170,21,170,26],[170,29,170,34],[170,35,170,38],[171,28,171,29],[171,22,171,27],[171,30,171,35],[171,36,171,39],[168,26,168,27],[168,20,168,25],[168,28,168,33],[168,34,168,37],[169,27,169,28],[169,21,169,26],[169,29,169,34],[169,35,169,38],[166,24,166,25],[166,18,166,23],[166,26,166,31],[166,32,166,35],[167,25,167,26],[167,19,167,24],[167,27,167,32],[167,33,167,36],[164,24,164,25],[164,18,164,23],[164,26,164,31],[164,32,164,35],[165,24,165,25],[165,18,165,23],[165,26,165,31],[165,32,165,35],[162,24,162,25],[162,18,162,23],[162,26,162,31],[162,32,162,35],[163,24,163,25],[163,18,163,23],[163,26,163,31],[163,32,163,35],[160,25,160,26],[160,19,160,24],[160,27,160,32],[160,33,160,36],[161,26,161,27],[161,20,161,25],[161,28,161,33],[161,34,161,37],[158,24,158,25],[158,18,158,23],[158,26,158,31],[158,32,158,35],[159,24,159,25],[159,18,159,23],[159,26,159,31],[159,32,159,35],[156,24,156,25],[156,18,156,23],[156,26,156,31],[156,32,156,35],[157,24,157,25],[157,18,157,23],[157,26,157,31],[157,32,157,35],[154,24,154,25],[154,18,154,23],[154,26,154,31],[154,32,154,35],[155,24,155,25],[155,18,155,23],[155,26,155,31],[155,32,155,35],[152,24,152,25],[152,18,152,23]],"merged_total":1614,"flags":["merged_cut"]}
[null,null,"FunctionalObject",null,null,null,null,null,null,null,null,null,null,null,"REGULATOR",null,null,null,null,null,"rdl:RDS7198580",null,"A <REGULATOR> is a <FunctionalObject> that is capable of <REGULATING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","REGULATOR",null,null,null,null,null,null,null,null,null,null,null,"CONSTANT VOLUME REGULATOR",null,null,null,null,null,"rdl:RDS297494",null,"A <CONSTANT VOLUME REGULATOR> is an <ARTEFACT> and a <REGULATOR> ensuring constant volume in a HVAC system to reduce noise",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT REGULATOR",null,null,null,null,null,"rdl:RDS7124120",null,"A <CURRENT REGULATOR> is a <REGULATOR> to control the electrical current supplied to a unit",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"FLUID REGULATOR",null,null,null,null,null,"rdl:RDS278369",null,"A <FLUID REGULATOR> is a <REGULATOR> that is intended to permit, obstruct, regulate or divert fluid flow",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"FLUID REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"LOUVRE",null,null,null,null,null,"rdl:RDS477359",null,"A <LOUVRE> is a <FLUID REGULATOR> which contains fins or vanes intended to control a flow of air. Typically also to separate water droplets from an air stream",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","LOUVRE",null,null,null,null,null,null,null,null,null,null,null,null,null,"WEATHER LOUVRE",null,null,null,null,null,"rdl:RDS315314",null,"A <WEATHER LOUVRE> is an <ARTEFACT> and a <LOUVRE> for the inlet or outlet of air used for ventilation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BLOCKER","FLUID REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"SLUICE",null,null,null,null,null,"rdl:RDS11588635",null,"An <SLUICE> is a <BLOCKER> and a <FLUID REGULATOR> that is a channel for a fluid to flow through, fitted with a valve or gate for stopping or regulating flow",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","SLUICE",null,null,null,null,null,null,null,null,null,null,null,null,null,"SLAG SLUICE",null,null,null,null,null,"rdl:RDS16054884",null,"A <SLAG SLUICE> is an <ARTEFACT> and a <SLUICE> that is intended (designed) for removing <SLAG>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DAMPER","FLUID REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"THROTTLING DAMPER",null,null,null,null,null,"rdl:RDS313019",null,"A <THROTTLING DAMPER> is a <DAMPER> and a <FLUID REGULATOR> that throttles a gas flow by means of a damper",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"FLUID REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE",null,null,null,null,null,"rdl:RDS292589",null,"A <VALVE> is a <FLUID REGULATOR> that can be used to control (i.e. permit, obstruct, regulate or divert) a fluid stream",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR INLET VALVE",null,null,null,null,null,"rdl:RDS13659922",null,"An <AIR INLET VALVE> is an <ARTEFACT> and a <VALVE> that is assigned to let combustion air, or the mixture of air and fuel, into the combustion chamber of an internal combustion engine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"ANGLE VALVE",null,null,null,null,null,"rdl:RDS5789384",null,"An <ANGLE VALVE> is an <ARTEFACT> and a <VALVE> that has valve ports which are not in-line",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANGLE VALVE","CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANGLE CHECK VALVE",null,null,null,null,null,"rdl:RDS6327442",null,"An <ANGLE CHECK VALVE> is a <CHECK VALVE> and an <ANGLE VALVE> that deviates from the in-line design, i.e. with a body shape designed to adjust the flow direction with a specified angle relative to the straight through-flow an in-line valve would have provided for",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANGLE VALVE","CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"ANGLE CONTROL VALVE",null,null,null,null,null,"rdl:RDS5791021",null,"An <ANGLE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and an <ANGLE VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANGLE VALVE","GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANGLE GLOBE VALVE",null,null,null,null,null,"rdl:RDS882944",null,"An <ANGLE GLOBE VALVE> is a <GLOBE VALVE> and an <ANGLE VALVE> that deviates from the in-line design, i.e. with a body shape designed to adjust the flow direction with a specified angle relative to the straight through-flow an in-line valve would have provided for",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANGLE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANGLE VALVE 45 DEGREE",null,null,null,null,null,"rdl:RDS5789519",null,"An <ANGLE VALVE 45 DEGREE> is an <ANGLE VALVE> that has valve port ends at 45 degrees angle to each other",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANGLE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANGLE VALVE 60 DEGREE",null,null,null,null,null,"rdl:RDS5789474",null,"An <ANGLE VALVE 60 DEGREE> is an <ANGLE VALVE> that has valve port ends at 60 degrees angle to each other",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANGLE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANGLE VALVE 90 DEGREE",null,null,null,null,null,"rdl:RDS5789429",null,"An <ANGLE VALVE 90 DEGREE> is an <ANGLE VALVE> that has valve port ends at 90 degrees angle to each other",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE WITH MANUAL OVERRIDE","ANGLE VALVE 90 DEGREE","CAGE TRIM CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA INSERT CHOKE",null,null,null,null,null,"rdl:RDS370725510",null,"A <SUBSEA INSERT CHOKE> is an <ANGLE VALVE 90 DEGREE> and a <CAGE TRIM CHOKE VALVE> and an <ACTUATED VALVE WITH MANUAL OVERRIDE> where the valve body is fixed to a subsea structure and the trim and actuator is retrievable",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BARE STEM VALVE",null,null,null,null,null,"rdl:RDS14113820",null,"A <BARE STEM VALVE is an <ARTEFACT> and a <VALVE> without operating device",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BARSTOCK VALVE",null,null,null,null,null,"rdl:RDS6329463",null,"A <BARSTOCK VALVE is an <ARTEFACT> and a <VALVE> that has a body machined from a piece of solid material - usually a needle or globe valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BIDIRECTIONAL VALVE",null,null,null,null,null,"rdl:RDS5792062",null,"A <BIDIRECTIONAL VALVE is an <ARTEFACT> and a <VALVE> that is used to regulate fluid flow in either direction of flow through the valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BIDIRECTIONAL VALVE","CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"BI-DIRECTIONAL CONTROL VALVE",null,null,null,null,null,"rdl:RDS16744700",null,"A <BI-DIRECTIONAL CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <BI-DIRECTIONAL VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BI-DIRECTIONAL CONTROL VALVE","THREE WAY CONTROL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHANGE-OVER CONTROL VALVE",null,null,null,null,null,"rdl:RDS16744813",null,"A <CHANGE-OVER CONTROL VALVE> is a <BI-DIRECTIONAL CONTROL VALVE> and a <THREE WAY CONTROL VALVE> with two inlet ports and one outlet port, enabling changing between dual supplies",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BLEED VALVE",null,null,null,null,null,"rdl:RDS11274650",null,"A <BLEED VALVE is an <ARTEFACT> and a <VALVE> that can be used to draw off a fluid",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BLEED VALVE","BLOCK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BLOCK AND BLEED VALVE",null,null,null,null,null,"rdl:RDS431594",null,"A <BLOCK AND BLEED VALVE> is a <BLOCK VALVE> and a <BLEED VALVE> that has one seat which provides a seal, and a bleeder line and valve that are tapped into the block valves bonnet",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BLOCK AND BLEED VALVE","DOUBLE BLOCK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE BLOCK AND BLEED VALVE",null,null,null,null,null,"rdl:RDS552689",null,"A <DOUBLE BLOCK AND BLEED VALVE> is a <BLOCK AND BLEED VALVE> and a <DOUBLE BLOCK VALVE> that is incorporating two seats, each of which provides a seal, and a means of venting the space between the seats. The seats may isolate with the pressure differential acting in the same or in opposite directions depending on the design",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BLENDING VALVE",null,null,null,null,null,"rdl:RDS11274380",null,"A <BLENDING VALVE is an <ARTEFACT> and a <VALVE> that can be used to regulate flow input(s), typically of multi-port design",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BLOCK VALVE",null,null,null,null,null,"rdl:RDS280979",null,"A <BLOCK VALVE is an <ARTEFACT> and a <VALVE> that can be used to isolate possible leaks in case of an emergency situation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BLOCK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE BLOCK VALVE",null,null,null,null,null,"rdl:RDS552734",null,"A <DOUBLE BLOCK VALVE> is a <BLOCK VALVE> that has two seats, each of which provides a seal. The seats may isolate with the pressure differential acting in the same or in the opposite directions, depending on the design",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BLOW DOWN VALVE",null,null,null,null,null,"rdl:RDS283859",null,"A <BLOW DOWN VALVE is an <ARTEFACT> and a <VALVE> that can be used for rapid depressurizing of a high pressure system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BYPASS VALVE",null,null,null,null,null,"rdl:RDS6712675",null,"A <BYPASS VALVE is an <ARTEFACT> and a <VALVE> that can be mounted in a bypass loop where a stream of fluid can be directed through, i.e. shunted past fluid functional unit(s) where the flow normally goes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"CHECK VALVE",null,null,null,null,null,"rdl:RDS292229",null,"A <CHECK VALVE> is an <ARTEFACT> and a <VALVE> that permits fluid to flow in one direction only",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHECK VALVE PILOT OPERATED TO CLOSE",null,null,null,null,null,"rdl:RDS296639",null,"A <CHECK VALVE PILOT OPERATED TO CLOSE> is a <CHECK VALVE> that is opened by means of a pilot valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHECK VALVE PILOT OPERATED TO OPEN",null,null,null,null,null,"rdl:RDS296684",null,"A <CHECK VALVE PILOT OPERATED TO OPEN> is a <CHECK VALVE> that is closed by means of a pilot valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHECK VALVE","DIAPHRAGM VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIAPHRAGM CHECK VALVE",null,null,null,null,null,"rdl:RDS552644",null,"A <DIAPHRAGM CHECK VALVE> is a <CHECK VALVE> and a <DIAPHRAGM VALVE> in which the closure member is a specially shaped diaphragm allowing forward flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOOT VALVE",null,null,null,null,null,"rdl:RDS17079043",null,"A <FOOT VALVE> is a <CHECK VALVE> that is intended to provide an open inlet for total immersion on a pump suction line. Often fitted with a filter or strainer",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FOOT VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOOT VALVE WITH STRAINER",null,null,null,null,null,"rdl:RDS11141995",null,"A <FOOT VALVE WITH STRAINER> is a <FOOT VALVE> that is intended to provide an open inlet for total immersion on a pump suction line",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIFT CHECK VALVE",null,null,null,null,null,"rdl:RDS645119",null,"A <LIFT CHECK VALVE> is a <CHECK VALVE> in which the closure member is lifted from the seat during forward flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LIFT CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BALL CHECK VALVE",null,null,null,null,null,"rdl:RDS552104",null,"A <BALL CHECK VALVE> is a <LIFT CHECK VALVE> that is having a free spring loaded ball closing on a spherical seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE BALL CHECK VALVE",null,null,null,null,null,"rdl:RDS7027900",null,"A <DOUBLE BALL CHECK VALVE> is a <BALL CHECK VALVE> that is provided with two balls",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LIFT CHECK VALVE","PISTON VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PISTON CHECK VALVE",null,null,null,null,null,"rdl:RDS645794",null,"A <PISTON CHECK VALVE> is a <LIFT CHECK VALVE> and a <PISTON VALVE> that has a free gravity or spring loaded piston type closure member",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PISTON CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AXIAL PISTON VALVE",null,null,null,null,null,"rdl:RDS551879",null,"An <AXIAL PISTON VALVE> is a <PISTON CHECK VALVE> that has the piston axis in the line of flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LIFT CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STOP CHECK VALVE",null,null,null,null,null,"rdl:RDS644804",null,"A <STOP CHECK VALVE> is a <LIFT CHECK VALVE> that is combining the self-acting operation of a <CHECK VALVE> with the manual action of a <GLOBE VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-RETURN VALVE",null,null,null,null,null,"rdl:RDS16308005",null,"A <NON-RETURN VALVE> is a <CHECK VALVE> that allows flow in one direction only",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"NON-RETURN VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPRESSOR VALVE",null,null,null,null,null,"rdl:RDS397703521",null,"A <COMPRESSOR VALVE> is a <NON-RETURN VALVE> intended to open and close at each piston stroke and which is mounted in the valve chamber of a reciprocating compressor between cylinder volume and inlet/outlet channel or clearance pocket",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COMPRESSOR VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DISCHARGE COMPRESSOR VALVE",null,null,null,null,null,"rdl:RDS402635861",null,"A <DISCHARGE COMPRESSOR VALVE> is a <COMPRESSOR VALVE> that can be located only at the discharge side of a reciprocating compressor cylinder",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COMPRESSOR VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RING-TYPE COMPRESSOR VALVE",null,null,null,null,null,"rdl:RDS414826151",null,"A <RING-TYPE COMPRESSOR VALVE> is a <COMPRESSOR VALVE> that uses plastic (peek) valve rings to seal off the valve ports in the valve seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PLATE CHECK VALVE",null,null,null,null,null,"rdl:RDS645884",null,"A <PLATE CHECK VALVE> is a <CHECK VALVE> that has several metallic membranes which allow forward flow, but close to prevent reverse flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SCREW DOWN CHECK VALVE",null,null,null,null,null,"rdl:RDS8984380",null,"A <SCREW DOWN CHECK VALVE> is a <CHECK VALVE> where the closure member can be tightened against the seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SWING CHECK VALVE",null,null,null,null,null,"rdl:RDS610424",null,"A <SWING CHECK VALVE> is a <CHECK VALVE> where the closure member is a disc which swings freely on a hinge and which opens automatically when flow is established and closes automatically when flow ceases or is reversed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWING CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONVENTIONAL SWING CHECK VALVE",null,null,null,null,null,"rdl:RDS6327885",null,"A <CONVENTIONAL SWING CHECK VALVE> is a <SWING CHECK VALVE> that has the swing arm hinged outside the flow path",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONVENTIONAL SWING CHECK VALVE","SINGLE PLATE WAFER CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE PLATE WAFER CHECK VALVE LONG PATTERN",null,null,null,null,null,"rdl:RDS429254",null,"A <SINGLE PLATE WAFER CHECK VALVE LONG PATTERN> is a <SINGLE PLATE WAFER CHECK VALVE> and a <CONVENTIONAL SWING CHECK VALVE> with long pattern design",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONVENTIONAL SWING CHECK VALVE","SINGLE PLATE WAFER CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE PLATE WAFER CHECK VALVE SHORT PATTERN",null,null,null,null,null,"rdl:RDS429344",null,"A <SINGLE PLATE WAFER CHECK VALVE SHORT PATTERN> is a <SINGLE PLATE WAFER CHECK VALVE> and a <CONVENTIONAL SWING CHECK VALVE> with short pattern design",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWING CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DUAL DISC SWING CHECK VALVE",null,null,null,null,null,"rdl:RDS6328026",null,"A <DUAL DISC SWING CHECK VALVE> is a <SWING CHECK VALVE> that is equipped with two half discs mounted on a shaft transverse to the center of the valve. The discs respond automatically to the fluid flow, permitting fluid to flow in one direction only",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DUAL DISC SWING CHECK VALVE","WAFER CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DUAL PLATE WAFER CHECK VALVE LONG PATTERN",null,null,null,null,null,"rdl:RDS429299",null,"A <DUAL PLATE WAFER CHECK VALVE LONG PATTERN> is a <DUAL DISC SWING CHECK VALVE> and a <WAFER CHECK VALVE> that is equipped with fluid flow swing open dual discs/plates, and has long pattern design",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWING CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLAP VALVE",null,null,null,null,null,"rdl:RDS553049",null,"A <FLAP VALVE> is a <SWING CHECK VALVE> that is equipped with a hinged disc or flap, sometimes leather or rubber faced, intended for low pressure applications",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FULL BORE VALVE","SWING CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FULL OPENING SWING CHECK VALVE",null,null,null,null,null,"rdl:RDS429209",null,"A <FULL OPENING SWING CHECK VALVE> is a <SWING CHECK VALVE> and a <FULL BORE VALVE> that has a disc which swings completely clear of the bore in the open position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"REDUCED BORE VALVE","SWING CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REDUCED BORE CHECK VALVE",null,null,null,null,null,"rdl:RDS429164",null,"A <REDUCED BORE CHECK VALVE> is a <SWING CHECK VALVE> and a <REDUCED BORE VALVE> that has a smaller opening (by flap seat) than full bore",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWING CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SWING CHECK VALVE WITH OUTSIDE LEVER AND WEIGHT ATTACHMENT",null,null,null,null,null,"rdl:RDS11141365",null,"A <SWING CHECK VALVE WITH OUTSIDE LEVER AND WEIGHT ATTACHMENT> is a <SWING CHECK VALVE> that is a swing check valve whose action is controlled by an outside lever and external weight to provide additional force",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWING CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TILTING DISC CHECK VALVE",null,null,null,null,null,"rdl:RDS6327947",null,"A <TILTING DISC CHECK VALVE> is a <SWING CHECK VALVE> that has a tilting disc, pivoted near its horizontal diameter",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHECK VALVE","WAFER PATTERN VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WAFER CHECK VALVE",null,null,null,null,null,"rdl:RDS6327600",null,"A <WAFER CHECK VALVE> is a <CHECK VALVE> and a <WAFER PATTERN VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WAFER CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DUAL PLATE WAFER CHECK VALVE",null,null,null,null,null,"rdl:RDS647324",null,"A <DUAL PLATE WAFER CHECK VALVE> is a <WAFER CHECK VALVE> that is equipped with two half discs mounted on a shaft transverse to the center of the valve. The discs respond automatically to the fluid flow, permitting fluid to flow in one direction only",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WAFER CHECK VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE PLATE WAFER CHECK VALVE",null,null,null,null,null,"rdl:RDS11141185",null,"A <SINGLE PLATE WAFER CHECK VALVE> is a <WAFER CHECK VALVE> that has a single plate and is intended to be installed between flanges",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"CHOKE VALVE",null,null,null,null,null,"rdl:RDS292364",null,"A <CHOKE VALVE> is an <ARTEFACT> and a <VALVE> in which a solid cylinder is raised and lowered, and which is placed around or inside another cylinder that has holes or slots. The design of a choke valve means fluids flowing through the cage are coming from all sides and that the streams of flow (through the holes or slots) collide with each other at the center of the cage cylinder, thereby dissipating the energy of the fluid through flow impingement. The main advantage of choke valves is that they can be designed to be totally linear in their flow rate. (source: Wikipedia)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ADJUSTABLE CHOKE VALVE",null,null,null,null,null,"rdl:RDS6712472",null,"An <ADJUSTABLE CHOKE VALVE> is a <CHOKE VALVE> that is made with adjustable flow/pressure restriction (i.e. has a valve operator by which it can be adjusted)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ADJUSTABLE CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAGE CHOKE VALVE",null,null,null,null,null,"rdl:RDS16702500",null,"A <CAGE CHOKE VALVE> is an <ADJUSTABLE CHOKE VALVE> having an orifice configuration using a plug and cage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ADJUSTABLE CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTISTAGE CHOKE VALVE",null,null,null,null,null,"rdl:RDS16702658",null,"A <MULTISTAGE CHOKE VALVE> is an <ADJUSTABLE CHOKE VALVE> having an orifice configuration using a slotted sliding sleeve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ADJUSTABLE CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NEEDLE CHOKE VALVE",null,null,null,null,null,"rdl:RDS16702421",null,"A <NEEDLE CHOKE VALVE> is an <ADJUSTABLE CHOKE VALVE> having an orifice configuration using a needle and seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE","ADJUSTABLE CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE COMPENSATED ADJUSTABLE FLOW CONTROL VALVE WITH BYPASS",null,null,null,null,null,"rdl:RDS6712551",null,"A <PRESSURE COMPENSATED ADJUSTABLE FLOW CONTROL VALVE WITH BYPASS> is an <ACTUATED VALVE> and an <ADJUSTABLE CHOKE VALVE> that is pressure compensated and has a bypass",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ADJUSTABLE CHOKE VALVE","CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTATING DISC CHOKE VALVE",null,null,null,null,null,"rdl:RDS16702325",null,"A <ROTATING DISC CHOKE VALVE> is an <ADJUSTABLE CHOKE VALVE> having an orifice configuration using rotating discs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ADJUSTABLE CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLEEVE CHOKE VALVE",null,null,null,null,null,"rdl:RDS16702579",null,"An <SLEEVE CHOKE VALVE> is an <ADJUSTABLE CHOKE VALVE> having an orifice configuration using a holed sliding sleeve and seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAGE TRIM CHOKE VALVE",null,null,null,null,null,"rdl:RDS370725798",null,"A <CAGE TRIM CHOKE VALVE> is a <CHOKE VALVE> that has a cage trim, which is a cylinder with openings in the wall, and having a cylindrical closure member which surrounds the cage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIXED CHOKE VALVE",null,null,null,null,null,"rdl:RDS6329914",null,"A <FIXED CHOKE VALVE> is a <CHOKE VALVE> that has no valve operator by which it can be adjusted, i.e. where the flow/pressure restriction is fixed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FIXED CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POSITIVE CHOKE VALVE",null,null,null,null,null,"rdl:RDS16702246",null,"A <POSITIVE CHOKE VALVE> is a <FIXED CHOKE VALVE> accommodating replaceable parts of fixed orifice dimernsions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHOKE VALVE","REDUCTION VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REDUCTION VALVE SELF ACTING",null,null,null,null,null,"rdl:RDS310454",null,"A <REDUCTION VALVE SELF ACTING> is a <CHOKE VALVE> and a <REDUCTION VALVE> activated by the backpressure in the system it is operating",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA CHOKE VALVE",null,null,null,null,null,"rdl:RDS6331375",null,"A <SUBSEA CHOKE VALVE> is a <CHOKE VALVE> that is specifically intended by design for use in a subsea service",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA GAS LIFT CHOKE VALVE",null,null,null,null,null,"rdl:RDS16757012",null,"A <SUBSEA GAS LIFT CHOKE VALVE> is a <SUBSEA CHOKE VALVE> specifically intended to be used in the gas lift line to regulate the pressure of the gas used for gas lift",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA INJECTION CHOKE VALVE",null,null,null,null,null,"rdl:RDS16757091",null,"A <SUBSEA INJECTION CHOKE VALVE> is a <SUBSEA CHOKE VALVE> specifically intended to be used in the injection line to regulate the pressure of the fluid .injected into a well",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA CHOKE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA PRODUCTION CHOKE VALVE",null,null,null,null,null,"rdl:RDS16756933",null,"A <SUBSEA PRODUCTION CHOKE VALVE> is a <SUBSEA CHOKE VALVE> specifically intended to be used in the production line",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"CHRISTMAS TREE VALVE",null,null,null,null,null,"rdl:RDS16706768",null,"A <CHRISTMAS TREE VALVE> is an <ARTEFACT> and a <VALVE> that is located on a christmas tree, for injection or fluid control",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHRISTMAS TREE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANNULUS CIRCULATION VALVE",null,null,null,null,null,"rdl:RDS16553058",null,"An <ANNULUS CIRCULATION VALVE> is a <CHRISTMAS TREE VALVE> that is located in the annulus outlet of the christmas tree for use when circulating in the well",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHRISTMAS TREE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANNULUS MASTER VALVE",null,null,null,null,null,"rdl:RDS16552934",null,"An <ANNULUS MASTER VALVE> is a <CHRISTMAS TREE VALVE> that is located in the annulus outlet of the christmas tree being the main annulus barrier valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHRISTMAS TREE VALVE","VENT VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANNULUS VENT VALVE",null,null,null,null,null,"rdl:RDS16703649",null,"An <ANNULUS VENT VALVE> is a <CHRISTMAS TREE VALVE> and a <VENT VALVE> that is located in the annulus outlet of the christmas tree for venting overpressure from the well annulus",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHRISTMAS TREE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANNULUS WING VALVE",null,null,null,null,null,"rdl:RDS16553013",null,"An <ANNULUS WING VALVE> is a <CHRISTMAS TREE VALVE> that is located in the annulus outlet of the christmas tree being the secondary annulus barrier valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHRISTMAS TREE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHEMICAL INJECTION VALVE",null,null,null,null,null,"rdl:RDS16551664",null,"A <CHEMICAL INJECTION VALVE> is a <CHRISTMAS TREE VALVE> that is used to control injection of chemicals into the well or flowline",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHEMICAL INJECTION VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHEMICAL INJECTION THROTTLE VALVE",null,null,null,null,null,"rdl:RDS16763375",null,"A <CHEMICAL INJECTION THROTTLE VALVE> is a <CHEMICAL INJECTION VALVE> of the throttle type used to control the rate and amount of chemical injection fluids",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHEMICAL INJECTION VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CORROSION INHIBITOR VALVE",null,null,null,null,null,"rdl:RDS16757260",null,"A <CORROSION INHIBITOR VALVE> is a <CHEMICAL INJECTION VALVE> that is used to control injection of a corrosion inhibitor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHEMICAL INJECTION VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"METHANOL INJECTION VALVE",null,null,null,null,null,"rdl:RDS16551751",null,"A <METHANOL INJECTION VALVE> is a <CHEMICAL INJECTION VALVE> that is used to control injection of Methanol into the well production fluid stream",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHEMICAL INJECTION VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SCALE INHIBITOR VALVE",null,null,null,null,null,"rdl:RDS16551851",null,"A <SCALE INHIBITOR VALVE> is a <CHEMICAL INJECTION VALVE> that is used to control injection of a scale inhibitor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHRISTMAS TREE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CROSSOVER VALVE",null,null,null,null,null,"rdl:RDS16553103",null,"A <CROSSOVER VALVE> is a <CHRISTMAS TREE VALVE> that which is located in the crossover loop",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHRISTMAS TREE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRODUCTION MASTER VALVE",null,null,null,null,null,"rdl:RDS16552776",null,"A <PRODUCTION MASTER VALVE> is a <CHRISTMAS TREE VALVE> that is located in the production outlet of the christmas tree being the main production barrier valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CHRISTMAS TREE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRODUCTION WING VALVE",null,null,null,null,null,"rdl:RDS16552864",null,"A <PRODUCTION WING VALVE> is a <CHRISTMAS TREE VALVE> that is located in the production outlet of the christmas tree being the secondary production barrier valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"CONDUIT VALVE",null,null,null,null,null,"rdl:RDS11711657",null,"A <CONDUIT VALVE> is an <ARTEFACT> and a <VALVE> with a circular hole in the closure member that will pass a sphere no smaller than specified for the applicable nominal size (less the tolerance), except that the end preparation of weld-end valves may require a smaller bore at the weld end to properly mate with the <PIPE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONDUIT VALVE","GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONDUIT GATE VALVE",null,null,null,null,null,"rdl:RDS11711719",null,"A <CONDUIT GATE VALVE> is a <CONDUIT VALVE> and a <GATE VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONDUIT GATE VALVE","FULL BORE VALVE","PARALLEL GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THROUGH CONDUIT GATE VALVE",null,null,null,null,null,"rdl:RDS552554",null,"A <THROUGH CONDUIT GATE VALVE> is a <CONDUIT GATE VALVE> and a <FULL BORE VALVE> and a <PARALLEL GATE VALVE> with full bore that is having a continuous, uninterrupted and unobstructed port through the valve when fully open",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THROUGH CONDUIT GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONDUIT RISING STEM GATE VALVE",null,null,null,null,null,"rdl:RDS429119",null,"A <CONDUIT RISING STEM GATE VALVE> is a <THROUGH CONDUIT GATE VALVE> that is equipped with a rising stem",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THROUGH CONDUIT GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXPANDING CONDUIT GATE VALVE",null,null,null,null,null,"rdl:RDS6328440",null,"An <EXPANDING CONDUIT GATE VALVE> is a <THROUGH CONDUIT GATE VALVE> that has an expanding slab",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THROUGH CONDUIT GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLAB GATE VALVE",null,null,null,null,null,"rdl:RDS487214",null,"A <SLAB GATE VALVE> is a <THROUGH CONDUIT GATE VALVE> that has a single parallel sided gate normally sealed by floating seats",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"CONE VALVE",null,null,null,null,null,"rdl:RDS11142535",null,"A <CONE VALVE> is an <ARTEFACT> and a <VALVE> where the valve seat is conically shaped",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FINAL CONTROL FUNCTION","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"CONTROL VALVE",null,null,null,null,null,"rdl:RDS297539",null,"A <CONTROL VALVE> is a <VALVE> and an <FINAL CONTROL FUNCTION>, operated by an <ACTUATOR> that can be used to modify (regulate) the fluid flow rate in response to a signal from a <PROCESS CONTROL DEVICE>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANTI CAVITATION CONTROL VALVE",null,null,null,null,null,"rdl:RDS11273555",null,"An <ANTI CAVITATION CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that can be used to prevent cavitation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BUTTERFLY VALVE","CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"BUTTERFLY CONTROL VALVE",null,null,null,null,null,"rdl:RDS5791128",null,"A <BUTTERFLY CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <BUTTERFLY VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAGE TRIM CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142445",null,"A <CAGE TRIM CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that has a cage trim, which is a cylinder with openings in the wall, and which surrounds and guides the plug closure member of a plug type globe valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHEMICAL INJECTION DOSING CONTROL VALVE",null,null,null,null,null,"rdl:RDS16757390",null,"A <CHEMICAL INJECTION DOSING CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> which is used to control the rate and amount of the chemicals injection into the well or flowline",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CIRCULATION CONTROL VALVE",null,null,null,null,null,"rdl:RDS17609942",null,"A <CIRCULATION CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> normally placed across a circulation point to allow isolation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","CRYOGENIC VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"CRYOGENIC CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142580",null,"A <CRYOGENIC CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <CRYOGENIC VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DELUGE CONTROL VALVE",null,null,null,null,null,"rdl:RDS6329587",null,"A <DELUGE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that is intended to operate at high temperature, and admit water into a deluge system. It is fail safe, kept closed by pressurised gas, and is typically made of bronze",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DELUGE CONTROL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DELUGE VALVE WITH AFFF",null,null,null,null,null,"rdl:RDS297854",null,"A <DELUGE VALVE WITH AFFF> is a <DELUGE VALVE> that is installed in a deluge sprinkler system, which spreads <AFFF> (Aqueous Film Forming Foam) out in an area of an installation in case of fire",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECTIONAL CONTROL VALVE",null,null,null,null,null,"rdl:RDS16744139",null,"A <DIRECTIONAL CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that operates in one direction, having a reset function",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECCENTRIC ROTATING DISC CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142670",null,"An <ECCENTRIC ROTATING DISC CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that uses a rotating disc as closing element, and with a design that causes the disc to take a slightly eccentric path during actuation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","GATE VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"GATE CONTROL VALVE",null,null,null,null,null,"rdl:RDS17079788",null,"A <GATE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <GATE VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","GLOBE VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,"GLOBE CONTROL VALVE",null,null,null,null,null,"rdl:RDS5767330",null,"A <GLOBE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <GLOBE VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HIGH DIFFERENTIAL PRESSURE CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142085",null,"A <HIGH DIFFERENTIAL PRESSURE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that is intended to operate when the downstream pressure is much lower than the upstream pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HIGH TEMPERATURE CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142130",null,"A <HIGH TEMPERATURE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that is intended to withstand high temperature operating conditions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM","SLIDE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC DIRECTIONAL CONTROL VALVE",null,null,null,null,null,"rdl:RDS5800454",null,"A <HYDRAULIC DIRECTIONAL CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <SLIDE VALVE> that is designed to operate in a hydraulic system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LOW NOISE CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142175",null,"A <LOW NOISE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that is designed to generate low noise levels during operation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM","MEMBRANE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"MEMBRANE CONTROL VALVE",null,null,null,null,null,"rdl:RDS11215886",null,"A <MEMBRANE CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <MEMBRANE VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIXING CONTROL VALVE",null,null,null,null,null,"rdl:RDS11273885",null,"A <MIXING CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that usually is self-operating and can use a control element to regulate flow input(s)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM","MULTIPLE SEAT VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTIPLE SEAT CONTROL VALVE",null,null,null,null,null,"rdl:RDS11142355",null,"A <MULTIPLE SEAT CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <MULTIPLE SEAT VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ON-OFF CONTROL VALVE",null,null,null,null,null,"rdl:RDS11141905",null,"An <ON-OFF CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that only has two defined positions, being fully open and fully closed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM","PLUG VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"PLUG CONTROL VALVE",null,null,null,null,null,"rdl:RDS5791353",null,"A <PLUG CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <PLUG VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEALING STEAM CONTROL VALVE",null,null,null,null,null,"rdl:RDS418634441",null,"A <SEALING STEAM CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that reduces the steam supply pressure from the admission steam valve to a very slight overpressure to avoid air inrush into the shaft labyrinths of a condensing steam turbine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLAM SHUT CONTROL VALVE",null,null,null,null,null,"rdl:RDS646964",null,"A <SLAM SHUT CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> that has a disc which is held open against the flow and closes automatically when released",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL VALVE","INSTRUMENTATION ITEM","THREE WAY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE WAY CONTROL VALVE",null,null,null,null,null,"rdl:RDS293894",null,"A <THREE WAY CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <CONTROL VALVE> and a <THREE WAY VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","CRYOGENIC DEVICE","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,"CRYOGENIC VALVE",null,null,null,null,null,"rdl:RDS14114045",null,"A <CRYOGENIC VALVE> is an <ARTEFACT> and a <VALVE> and a <CRYOGENIC DEVICE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"DEPRESSURISING VALVE",null,null,null,null,null,"rdl:RDS11274470",null,"A <DEPRESSURISING VALVE> is an <ARTEFACT> and a <VALVE> that can be used to depressurise a system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","DIVERTER","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,"DIVERTER VALVE",null,null,null,null,null,"rdl:RDS6329649",null,"A <DIVERTER VALVE> is an <ARTEFACT> and a <VALVE> and a <DIVERTER> that is a valve with multiple ports intended to divert flow in several directions and prevent intermixing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE SEATED VALVE",null,null,null,null,null,"rdl:RDS7019199",null,"A <DOUBLE SEATED VALVE> is an <ARTEFACT> and a <VALVE> that has two valve seats",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"DOWNSTREAM SEATED VALVE",null,null,null,null,null,"rdl:RDS14114000",null,"A <DOWNSTREAM SEATED VALVE> is an <ARTEFACT> and a <VALVE> where the upstream line pressure loads the closure member against the downstream seat with differential pressure across the valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"DRAIN VALVE",null,null,null,null,null,"rdl:RDS11274515",null,"A <DRAIN VALVE> is an <ARTEFACT> and a <VALVE> that can be used to drain empty a piping system, storage tank, or similar. The drain valve is typically installed at the lowest point of the system to allow draining by gravity",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DRAIN VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DRIP DRAIN VALVE",null,null,null,null,null,"rdl:RDS11273510",null,"A <DRIP DRAIN VALVE> is a <DRAIN VALVE> that can be fitted to a drip leg (or other type of condensate trap) to allow blowdown (evacuation of condensate from system)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"ECCENTRIC ROTATING DISC VALVE",null,null,null,null,null,"rdl:RDS11142715",null,"An <ECCENTRIC ROTATING DISC VALVE> is an <ARTEFACT> and a <VALVE> that has a closing member which is an eccentric rotating disc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"EXCESS FLOW VALVE",null,null,null,null,null,"rdl:RDS553004",null,"An <EXCESS FLOW VALVE> is an <ARTEFACT> and a <VALVE> that is designed to close automatically when the flow exceeds a specified rate",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"EXHAUST VALVE",null,null,null,null,null,"rdl:RDS13659798",null,"An <EXHAUST VALVE> is an <ARTEFACT> and a <VALVE> that is assigned to relieve the combustion gases from the cylinder of an internal combustion engine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EXHAUST VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXHAUST VALVE FOR CYLINDER HEAD WITH BUILT ON VALVE HOUSING",null,null,null,null,null,"rdl:RDS13704300",null,"An <EXHAUST VALVE FOR CYLINDER HEAD WITH BUILT ON VALVE HOUSING> is an <EXHAUST VALVE> that is designed for being utilized on a cylinder cover with built on valve housing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EXHAUST VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXHAUST VALVE FOR CYLINDER HEAD WITH INTEGRATED VALVES",null,null,null,null,null,"rdl:RDS13704238",null,"An <EXHAUST VALVE FOR CYLINDER HEAD WITH INTEGRATED VALVES> is an <EXHAUST VALVE> that is designed for being utilized on a cylinder cover with integrated valves",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FAIL CLOSE ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"FAIL CLOSE VALVE",null,null,null,null,null,"rdl:RDS297584",null,"A <FAIL CLOSE VALVE> is an <ARTEFACT> and a <VALVE> and a <PROTECTOR> that is designed to automaticallly return to closed position/condition in the event of a failure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE","FAIL CLOSE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE WITH AUTOMATIC ACTUATOR FAIL CLOSE",null,null,null,null,null,"rdl:RDS314144",null,"A <VALVE WITH AUTOMATIC ACTUATOR FAIL CLOSE> is an <ACTUATED VALVE> and a <FAIL CLOSE VALVE> that, in the case of failure of the actuator, automatically goes to closed position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FAIL OPEN ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"FAIL OPEN VALVE",null,null,null,null,null,"rdl:RDS297629",null,"A <FAIL OPEN VALVE> is an <ARTEFACT> and a <VALVE> and a <PROTECTOR> that is designed to automatically return to open position/condition in the event of a failure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE","FAIL OPEN VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE WITH AUTOMATIC ACTUATOR FAIL OPEN",null,null,null,null,null,"rdl:RDS314189",null,"A <VALVE WITH AUTOMATIC ACTUATOR FAIL OPEN> is an <ACTUATED VALVE> and a <FAIL OPEN VALVE> that, in the case of failure of the actuator, automatically goes to open position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"FIRE TEST CERTIFIED VALVE",null,null,null,null,null,"rdl:RDS13021719",null,"A <FIRE TEST CERTIFIED VALVE> is an <ARTEFACT> and a <VALVE> that conforms to an accepted fire test",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"FUEL INJECTION VALVE",null,null,null,null,null,"rdl:RDS13659984",null,"A <FUEL INJECTION VALVE> is an <ARTEFACT> and a <VALVE> that is assigned to spray fuel into the combustion chamber of an internal combustion engine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FUEL INJECTION VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FUEL INJECTION VALVE FOR CYLINDER HEAD WITH INTEGRATED VALVES",null,null,null,null,null,"rdl:RDS13704362",null,"A <FUEL INJECTION VALVE FOR CYLINDER HEAD WITH INTEGRATED VALVES> is a <FUEL INJECTION VALVE> that is designed for being utilized on cylinder heads with integrated valves",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FUEL INJECTION VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FUEL INJECTION VALVE FOR CYLINDER HEAD WITH BUILT ON VALVE HOUSING",null,null,null,null,null,"rdl:RDS13704424",null,"A <FUEL INJECTION VALVE FOR CYLINDER HEAD WITH BUILT ON VALVE HOUSING> is a <FUEL INJECTION VALVE> that is designed for being utilized on cylinder heads with built on valve housing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"FULL BORE VALVE",null,null,null,null,null,"rdl:RDS14111030",null,"A <FULL BORE VALVE> is an <ARTEFACT> and a <VALVE> in which the opening of the closure member is large enough to allow a sphere equal to the valve nominal size to pass through the closure member",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE","FULL BORE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FULL BORE BALL VALVE",null,null,null,null,null,"rdl:RDS6689022",null,"A <FULL BORE BALL VALVE> is a <FULL BORE VALVE> and a <BALL VALVE> that has a full bore ball closure member",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ECCENTRIC BALL VALVE","FULL BORE BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FULL BORE ECCENTRIC BALL VALVE",null,null,null,null,null,"rdl:RDS14113595",null,"A <FULL BORE ECCENTRIC BALL VALVE> is an <ECCENTRIC BALL VALVE> and a <FULL BORE BALL VALVE> where the closure member is pivoted off centre to provide cam action which urges it against the seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOATING BALL VALVE","FULL BORE BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FULL BORE FLOATING BALL VALVE",null,null,null,null,null,"rdl:RDS14113280",null,"A <FULL BORE FLOATING BALL VALVE> is a <FLOATING BALL VALVE> and a <FULL BORE BALL VALVE> where the ball closure member is supported by seat rings, and free to move relative to the stem",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FULL BORE BALL VALVE","TRUNNION BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FULL BORE TRUNNION BALL VALVE",null,null,null,null,null,"rdl:RDS14113145",null,"A <FULL BORE TRUNNION BALL VALVE> is a <TRUNNION BALL VALVE> and a <FULL BORE BALL VALVE> where the valve is supported by a trunnion where the opening of the closure member is big enough to allow a sphere of a given size to pass through the closure member. (Bore approximately equivalent to the pipe bore)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIAPHRAGM VALVE","FULL BORE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FULL BORE DIAPHRAGM VALVE",null,null,null,null,null,"rdl:RDS14113550",null,"A <FULL BORE DIAPHRAGM VALVE> is a <FULL BORE VALVE> and a <DIAPHRAGM VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FULL BORE VALVE","GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FULL BORE GLOBE VALVE",null,null,null,null,null,"rdl:RDS14113055",null,"A <FULL BORE GLOBE VALVE> is a <FULL BORE VALVE> and a <GLOBE VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FULL BORE VALVE","PLUG VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FULL BORE PLUG VALVE",null,null,null,null,null,"rdl:RDS14113100",null,"A <FULL BORE PLUG VALVE> is a <FULL BORE VALVE> and a <PLUG VALVE> with a full cylindrical bore through the valve as opposed to standard patterns with trapezoidal ports",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"GATE VALVE",null,null,null,null,null,"rdl:RDS416519",null,"A <GATE VALVE> is an <ARTEFACT> and a <VALVE> that is a valve where the closure member is a gate or disc with a linear motion parallel, or nearly parallel, to the plane of flat seats, which are transverse to the direction of flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BELLOW SEALED GATE VALVE",null,null,null,null,null,"rdl:RDS552149",null,"A <BELLOW SEALED GATE VALVE> is a <GATE VALVE> that is having a bellow-sealed gland",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CLAMP GATE VALVE",null,null,null,null,null,"rdl:RDS552464",null,"A <CLAMP GATE VALVE> is a <GATE VALVE> that has body and bonnet held together by a <U->bolt clamp which facilitates stripdown for overhaul",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPACT GATE VALVE",null,null,null,null,null,"rdl:RDS552509",null,"A <COMPACT GATE VALVE> is a <GATE VALVE> that is having compact dimensions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HOSE GATE VALVE",null,null,null,null,null,"rdl:RDS882989",null,"A <HOSE GATE VALVE> is a <GATE VALVE> that has inlet and/or outlet connections intended for hose attachment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KNIFE GATE VALVE",null,null,null,null,null,"rdl:RDS645029",null,"A <KNIFE GATE VALVE> is a <GATE VALVE> that has a narrow parallel gate with a shaped edge indented to cut through glutenous media or slurries when closing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PARALLEL GATE VALVE",null,null,null,null,null,"rdl:RDS645614",null,"A <PARALLEL GATE VALVE> is a <GATE VALVE> that is equipped with a parallel slide gate or disc closure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PARALLEL GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PARALLEL SLIDE VALVE",null,null,null,null,null,"rdl:RDS883034",null,"A <PARALLEL SLIDE VALVE> is a <PARALLEL GATE VALVE> that is equipped with a spring-loaded double disc closure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PARALLEL SLIDE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTARY DISC VALVE",null,null,null,null,null,"rdl:RDS646379",null,"A <ROTARY DISC VALVE> is a <PARALLEL SLIDE VALVE> that has an offset shaft which slides a disc across the valve seat to open or close",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PENSTOCK VALVE",null,null,null,null,null,"rdl:RDS645704",null,"A <PENSTOCK VALVE> is a <GATE VALVE> that is intended to handle large volumes of water, designed with a rectangular gate mounted in a frame fixed to a wall or bulkhead",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTARY GATE VALVE",null,null,null,null,null,"rdl:RDS883079",null,"A <ROTARY GATE VALVE> is a <GATE VALVE> that is manually operated by a lever",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLIDE GATE VALVE",null,null,null,null,null,"rdl:RDS11141230",null,"A <SLIDE GATE VALVE> is a <GATE VALVE> that opens and closes a passageway by sliding over a port",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPLIT GATE VALVE",null,null,null,null,null,"rdl:RDS16683560",null,"An <SPLIT GATE VALVE> is a <GATE VALVE> where the gate or disk is made of two or more pieces which are capable of being energized to seal both upstream and downstream at the same time",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WEDGE GATE VALVE",null,null,null,null,null,"rdl:RDS851579",null,"A <WEDGE GATE VALVE> is a <GATE VALVE> that has a wedge closure member",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WEDGE GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE GATE VALVE",null,null,null,null,null,"rdl:RDS553094",null,"A <FLEXIBLE WEDGE GATE VALVE> is a <WEDGE GATE VALVE> that has a gate designed to permit flexing of sealing faces to ensure alignment parallel with their seats and to avoid thermal wedging",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE WEDGE GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE INSIDE SCREW RISING STEM GATE VALVE",null,null,null,null,null,"rdl:RDS852569",null,"A <FLEXIBLE WEDGE INSIDE SCREW RISING STEM GATE VALVE> is a <FLEXIBLE WEDGE GATE VALVE> that has the threaded portion of the stem under the gland packing. The stem rises via threads in the valve body/bonnet",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE WEDGE INSIDE SCREW RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE INSIDE SCREW RISING STEM FLANGED END GATE VALVE",null,null,null,null,null,"rdl:RDS11141095",null,"A <FLEXIBLE WEDGE INSIDE SCREW RISING STEM FLANGED END GATE VALVE> is a <FLEXIBLE WEDGE INSIDE SCREW RISING STEM GATE VALVE> that has flanged ends",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE WEDGE INSIDE SCREW RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE INSIDE SCREW RISING STEM BUTT WELDING END GATE VALVE",null,null,null,null,null,"rdl:RDS11141050",null,"A <FLEXIBLE WEDGE INSIDE SCREW RISING STEM BUTT WELDING END GATE VALVE> is a <FLEXIBLE WEDGE INSIDE SCREW RISING STEM GATE VALVE> that has butt welding ends",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE WEDGE INSIDE SCREW RISING STEM BUTT WELDING END GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE INSIDE SCREW RISING STEM WELDED PLAIN END GATE VALVE",null,null,null,null,null,"rdl:RDS11140825",null,"A <FLEXIBLE WEDGE INSIDE SCREW RISING STEM WELDED PLAIN END GATE VALVE> is a <FLEXIBLE WEDGE INSIDE SCREW RISING STEM BUTT WELDING END GATE VALVE> that has a welded plain end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE WEDGE INSIDE SCREW RISING STEM BUTT WELDING END GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE INSIDE SCREW RISING STEM WELDED BEVELLED END GATE VALVE",null,null,null,null,null,"rdl:RDS11141005",null,"A <FLEXIBLE WEDGE INSIDE SCREW RISING STEM WELDED BEVELLED END GATE VALVE> is a <FLEXIBLE WEDGE INSIDE SCREW RISING STEM BUTT WELDING END GATE VALVE> that has a welded bevelled end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE WEDGE INSIDE SCREW RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE INSIDE SCREW RISING STEM THREADED END GATE VALVE",null,null,null,null,null,"rdl:RDS11141140",null,"A <FLEXIBLE WEDGE INSIDE SCREW RISING STEM THREADED END GATE VALVE> is a <FLEXIBLE WEDGE INSIDE SCREW RISING STEM GATE VALVE> that has threaded ends",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE WEDGE GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE",null,null,null,null,null,"rdl:RDS852299",null,"A <FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE> is a <FLEXIBLE WEDGE GATE VALVE> that has a threaded portion of the stem isolated from the process media by the gland packing, and the stem rises via a threaded nut in the yoke",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE OS &amp;amp; Y RISING STEM THREADED END GATE VALVE",null,null,null,null,null,"rdl:RDS852389",null,"A <FLEXIBLE WEDGE OS &amp;amp; Y RISING STEM THREADED END GATE VALVE> is a <FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE> with threaded ends",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM FLANGED END GATE VALVE",null,null,null,null,null,"rdl:RDS11140915",null,"A <FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM FLANGED END GATE VALVE> is a <FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE> that has flanged ends",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM THREADED END GATE VALVE",null,null,null,null,null,"rdl:RDS11140960",null,"A <FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM THREADED END GATE VALVE> is a <FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE> that has threaded ends",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM BUTT WELDING END GATE VALVE",null,null,null,null,null,"rdl:RDS11140870",null,"A <FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM BUTT WELDING END GATE VALVE> is a <FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE> that has butt welding ends",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM BUTT WELDING END GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM WELDED BEVELLED END GATE VALVE",null,null,null,null,null,"rdl:RDS11140780",null,"A <FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM WELDED BEVELLED END GATE VALVE> is a <FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM WELDED BEVELLED END GATE VALVE> that has butt welded bevelled end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM BUTT WELDING END GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM WELDED PLAIN END GATE VALVE",null,null,null,null,null,"rdl:RDS11140735",null,"A <FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM WELDED PLAIN END GATE VALVE> is a <FLEXIBLE WEDGE OUTSIDE SCREW AND YOKE RISING STEM WELDED BEVELLED END GATE VALVE> that has butt welded plain end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WEDGE GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RUBBER SEATED WEDGE GATE VALVE",null,null,null,null,null,"rdl:RDS646469",null,"A <RUBBER SEATED WEDGE GATE VALVE> is a <WEDGE GATE VALVE> that has a rubber coated wedge closure that seals against the valve port",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WEDGE GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOFT SEATED WEDGE GATE VALVE",null,null,null,null,null,"rdl:RDS647054",null,"A <SOFT SEATED WEDGE GATE VALVE> is a <WEDGE GATE VALVE> that has primary seats manufactured from elastomer, polymers and similar resilient or semi-resilient materials",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WEDGE GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID WEDGE GATE VALVE",null,null,null,null,null,"rdl:RDS851624",null,"A <SOLID WEDGE GATE VALVE> is a <WEDGE GATE VALVE> that has a solid (non flexible) wedge and stem in one piece",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLID WEDGE GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID WEDGE INSIDE SCREW RISING STEM GATE VALVE",null,null,null,null,null,"rdl:RDS851714",null,"A <SOLID WEDGE INSIDE SCREW RISING STEM GATE VALVE> is a <SOLID WEDGE GATE VALVE> that has a conical wedge with a threaded portion of the stem under the gland packing. The stem rises via threads in the valve body/bonnet",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLID WEDGE INSIDE SCREW RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID WEDGE INSIDE SCREW RISING STEM FLANGED END GATE VALVE",null,null,null,null,null,"rdl:RDS11140555",null,"A <SOLID WEDGE INSIDE SCREW RISING STEM FLANGED END GATE VALVE> is a <SOLID WEDGE INSIDE SCREW RISING STEM GATE VALVE> that has a flanged end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLID WEDGE INSIDE SCREW RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID WEDGE INSIDE SCREW RISING STEM WELDED END GATE VALVE",null,null,null,null,null,"rdl:RDS11140240",null,"A <SOLID WEDGE INSIDE SCREW RISING STEM WELDED END GATE VALVE> is a <SOLID WEDGE INSIDE SCREW RISING STEM GATE VALVE> that has a welded end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLID WEDGE INSIDE SCREW RISING STEM WELDED END GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID WEDGE INSIDE SCREW RISING STEM WELDED BEVELLED END GATE VALVE",null,null,null,null,null,"rdl:RDS11140420",null,"A <SOLID WEDGE INSIDE SCREW RISING STEM WELDED BEVELLED END GATE VALVE> is a <SOLID WEDGE INSIDE SCREW RISING STEM WELDED END GATE VALVE> that has a welded bevelled end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLID WEDGE INSIDE SCREW RISING STEM WELDED END GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID WEDGE INSIDE SCREW RISING STEM WELDED PLAIN END GATE VALVE",null,null,null,null,null,"rdl:RDS11140285",null,"A <SOLID WEDGE INSIDE SCREW RISING STEM WELDED PLAIN END GATE VALVE> is a <SOLID WEDGE INSIDE SCREW RISING STEM WELDED END GATE VALVE> that has a welded plain end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLID WEDGE INSIDE SCREW RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID WEDGE INSIDE SCREW RISING STEM THREADED END GATE VALVE",null,null,null,null,null,"rdl:RDS11140600",null,"A <SOLID WEDGE INSIDE SCREW RISING STEM THREADED END GATE VALVE> is a <SOLID WEDGE INSIDE SCREW RISING STEM GATE VALVE> that has a threaded end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLID WEDGE INSIDE SCREW RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID WEDGE INSIDE SCREW RISING STEM EXTENDED END GATE VALVE",null,null,null,null,null,"rdl:RDS11140510",null,"A <SOLID WEDGE INSIDE SCREW RISING STEM EXTENDED END GATE VALVE> is a <SOLID WEDGE INSIDE SCREW RISING STEM GATE VALVE> that has an extended end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLID WEDGE GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE",null,null,null,null,null,"rdl:RDS851669",null,"A <SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE> is a <SOLID WEDGE GATE VALVE> that has a threaded portion of the stem isolated from the process medium by the gland packing. The stem rises via a threaded nut in the yoke",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM THREADED END GATE VALVE",null,null,null,null,null,"rdl:RDS11140195",null,"A <SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM THREADED END GATE VALVE> is a <SOLID WEDGE GATE VALVE> that is a solid wedge outside screw and yoke rising stem gate valve that has a threaded end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM FLANGED END GATE VALVE",null,null,null,null,null,"rdl:RDS11140465",null,"A <SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM FLANGED END GATE VALVE> is a <SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM EXTENDED END GATE VALVE> that has a flanged end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM BUTT WELDING END GATE VALVE",null,null,null,null,null,"rdl:RDS11140330",null,"A <SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM BUTT WELDING END GATE VALVE> is a <SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE> that has a butt welding end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM EXTENDED END GATE VALVE",null,null,null,null,null,"rdl:RDS11140375",null,"A <SOLID WEDGE OUTSIDE SCREW AND YOKE RISING STEM EXTENDED END GATE VALVE> is a <SOLID WEDGE GATE VALVE> that is a solid wedge outside screw and yoke rising stem gate valve that has an extended end body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WEDGE GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPLIT WEDGE GATE VALVE",null,null,null,null,null,"rdl:RDS647144",null,"An <SPLIT WEDGE GATE VALVE> is a <WEDGE GATE VALVE> that is having a wedge comprising of two parts in order to provide flexibility and resistance to thermal wedging",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPLIT WEDGE GATE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXPANDING WEDGE GATE VALVE",null,null,null,null,null,"rdl:RDS487259",null,"An <EXPANDING WEDGE GATE VALVE> is an <SPLIT WEDGE GATE VALVE> that has a closure member which consists of two parallel faced gates, separated by an expanding wedge, which loads each gate against its fixed seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"GAUGE VALVE",null,null,null,null,null,"rdl:RDS17080622",null,"A <GAUGE VALVE> is an <ARTEFACT> and a <VALVE> that can be used in connection with an INDICATOR, for instance an isolating valve for a level gauge",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"GLOBE VALVE",null,null,null,null,null,"rdl:RDS416204",null,"A <GLOBE VALVE> is an <ARTEFACT> and a <VALVE> where the closure member is a disc or piston operating with linear motion normal to the flat or shaped seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAGE GUIDED GLOBE VALVE",null,null,null,null,null,"rdl:RDS6328239",null,"A <CAGE GUIDED GLOBE VALVE> is a <GLOBE VALVE> that has a cage guided closure member",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAGE GUIDED GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAGE GUIDED PISTON VALVE",null,null,null,null,null,"rdl:RDS6328301",null,"A <CAGE GUIDED PISTON VALVE> is a <CAGE GUIDED GLOBE VALVE> that is a cage guided globe valve where the plug is a piston",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAGE GUIDED GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DRAG VALVE",null,null,null,null,null,"rdl:RDS552869",null,"A <DRAG VALVE> is a <CAGE GUIDED GLOBE VALVE> that is equipped with a perforated cage trim intended for high pressure drop, low noise applications",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DISC GLOBE VALVE",null,null,null,null,null,"rdl:RDS7018548",null,"A <DISC GLOBE VALVE> is a <GLOBE VALVE> that has a disc type plug closure member",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISC GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPOSITION DISC GLOBE VALVE",null,null,null,null,null,"rdl:RDS882314",null,"A <COMPOSITION DISC GLOBE VALVE> is a <DISC GLOBE VALVE> that is intended for coarse regulation and tight shutoff in services contaminated with solid particles. (Particles will embed in soft disc and seal whilst preventing seat damage.)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISC GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE DISC GLOBE VALVE",null,null,null,null,null,"rdl:RDS882494",null,"A <DOUBLE DISC GLOBE VALVE> is a <DISC GLOBE VALVE> that has two disc type plug closure members",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISC GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POPPET VALVE",null,null,null,null,null,"rdl:RDS645974",null,"A <POPPET VALVE> is a <DISC GLOBE VALVE> that is a disc globe valve where the operating mechanism is a non-rotating linear action",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISC GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REGULAR DISC GLOBE VALVE",null,null,null,null,null,"rdl:RDS882854",null,"A <REGULAR DISC GLOBE VALVE> is a <DISC GLOBE VALVE> that has a flat disc closure element",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLUSH BOTTOM VALVE",null,null,null,null,null,"rdl:RDS882539",null,"A <FLUSH BOTTOM VALVE> is a <GLOBE VALVE> that is designed to minimise pocketing, primarily for discharging liquid from low point of tank",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HOSE GLOBE VALVE",null,null,null,null,null,"rdl:RDS882584",null,"A <HOSE GLOBE VALVE> is a <GLOBE VALVE> that has inlet and/or outlet connections intended for hose attachment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NEEDLE VALVE",null,null,null,null,null,"rdl:RDS421064",null,"A <NEEDLE VALVE> is a <GLOBE VALVE> that has a closure member with the shape of a conical plug (needle) which closes into a small seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PISTON VALVE",null,null,null,null,null,"rdl:RDS645839",null,"A <PISTON VALVE> is a <GLOBE VALVE> that is a globe valve where the closure member is a piston",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GLOBE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PLUG GLOBE VALVE",null,null,null,null,null,"rdl:RDS882764",null,"A <PLUG GLOBE VALVE> is a <GLOBE VALVE> that is a globe valve in which the closure member is a tapered plug",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GLOBE VALVE","Y-PATTERN VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y-GLOBE VALVE",null,null,null,null,null,"rdl:RDS7461140",null,"A <Y-GLOBE VALVE> is a <GLOBE VALVE> and a <Y-PATTERN VALVE> that has in-line ports and stem emerging at about 45 degrees to the centerline, hence the name Y",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"GOVERNOR VALVE",null,null,null,null,null,"rdl:RDS11274605",null,"A <GOVERNOR VALVE> is an <ARTEFACT> and a <VALVE> that can be used to control a flow, and can be either of single or multi-port design",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"INLET VALVE",null,null,null,null,null,"rdl:RDS11274695",null,"An <INLET VALVE> is an <ARTEFACT> and a <VALVE> that can be located in an inlet",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSERT CHOKE VALVE CARTRIDGE",null,null,null,null,null,"rdl:RDS370725674",null,"An <INSERT CHOKE VALVE CARTRIDGE> is an <ARTEFACT> and a <VALVE> with a cylindrical sleeve housing the trim of an insert choke",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSERT CHOKE VALVE FLOW NOZZLE",null,null,null,null,null,"rdl:RDS370725698",null,"An <INSERT CHOKE VALVE FLOW NOZZLE> is an <ARTEFACT> and a <VALVE> with a cylindrical sleeve with holes being the valve orifce of an insert choke",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT VALVE",null,null,null,null,null,"rdl:RDS16207506",null,"An <INSTRUMENT VALVE> is an <ARTEFACT> and a <VALVE> that is intended to enable or prevent a fluid condition to be in direct conTact with a fluid stream",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"IRIS VALVE",null,null,null,null,null,"rdl:RDS644984",null,"An <IRIS VALVE> is an <ARTEFACT> and a <VALVE> that has a multiple leaved closure member which can be moved towards the centre of the valve bore until it forms a tight, solid barrier",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"ISOLATION VALVE",null,null,null,null,null,"rdl:RDS16207551",null,"An <ISOLATION VALVE> is an <ARTEFACT> and a <VALVE> used for isolationg all or part of a pipeline system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ISOLATION VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANNULUS ISOLATION VALVE",null,null,null,null,null,"rdl:RDS4858923032",null,"An <ANNULUS ISOLATION VALVE> is an <ISOLATION VALVE> for annulus.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ISOLATION VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TUBING ISOLATION VALVE",null,null,null,null,null,"rdl:RDS48589229281",null,"A <TUBING ISOLATION VALVE> is an <ISOLATION VALVE> for tubing.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"JACKETED VALVE",null,null,null,null,null,"rdl:RDS6330377",null,"A <JACKETED VALVE> is an <ARTEFACT> and a <VALVE> that has a jacket to allow heating/cooling medium to be applied to the valve to maintain some properties of the fluid",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"MEMBRANE VALVE",null,null,null,null,null,"rdl:RDS871739",null,"A <MEMBRANE VALVE> is an <ARTEFACT> and a <VALVE> that is a valve where the closure member is a flexible membrane",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MEMBRANE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIAPHRAGM VALVE",null,null,null,null,null,"rdl:RDS421019",null,"A <DIAPHRAGM VALVE> is a <MEMBRANE VALVE> where the closure member is a resilient diaphragm being forced against a port",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIAPHRAGM VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LINED DIAPHRAGM VALVE",null,null,null,null,null,"rdl:RDS645299",null,"A <LINED DIAPHRAGM VALVE> is a <DIAPHRAGM VALVE> that has the body internally lined",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIAPHRAGM VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAUNDERS DIAPHRAGM VALVE",null,null,null,null,null,"rdl:RDS6328945",null,"A <SAUNDERS DIAPHRAGM VALVE> is a <DIAPHRAGM VALVE> that is made according to Saunders original design, or equivalent",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MEMBRANE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PINCH VALVE",null,null,null,null,null,"rdl:RDS645749",null,"A <PINCH VALVE> is a <MEMBRANE VALVE> that is comprising a flexible tube, either exposed or enclosed in a body. The tube is pinched to close by mechanical means",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MEMBRANE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPIRAL SOCK VALVE",null,null,null,null,null,"rdl:RDS6331251",null,"A <SPIRAL SOCK VALVE> is a <MEMBRANE VALVE> that controls flow of powders by means of a twisted fabric tube or sock",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MEMBRANE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SQUEEZE VALVE",null,null,null,null,null,"rdl:RDS7019137",null,"A <SQUEEZE VALVE> is a <MEMBRANE VALVE> that consists of a flexible tube enclosed in a body. The tube is pinched to close by a pressurising fluid in the body cavity",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"MUD DISCHARGE VALVE",null,null,null,null,null,"rdl:RDS11273930",null,"A <MUD DISCHARGE VALVE> is an <ARTEFACT> and a <VALVE> that is designed to relieve muddy substances",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"MUD TANK PLUG VALVE",null,null,null,null,null,"rdl:RDS11273975",null,"A <MUD TANK PLUG VALVE> is an <ARTEFACT> and a <VALVE> that is assigned to handle muddy substances, and is connected to a mud tank",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"MUD VALVE",null,null,null,null,null,"rdl:RDS11274020",null,"A <MUD VALVE> is an <ARTEFACT> and a <VALVE> that is commonly used as a drain valve in the bottom of water and wastewater treatment basins and tanks, but is also used in industrial applications with spill or overflow containment basins",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTI WAY VALVE",null,null,null,null,null,"rdl:RDS6330104",null,"A <MULTI WAY VALVE> is an <ARTEFACT> and a <VALVE> that has multiple paths of flow through itself",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTI WAY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOUR WAY VALVE",null,null,null,null,null,"rdl:RDS6689411",null,"A <FOUR WAY VALVE> is a <MULTI WAY VALVE> that is made with four separate paths of flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTI WAY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE WAY VALVE",null,null,null,null,null,"rdl:RDS6331499",null,"A <THREE WAY VALVE> is a <MULTI WAY VALVE> that is made with three separate paths of flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE","THREE WAY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE WAY BALL VALVE",null,null,null,null,null,"rdl:RDS11141410",null,"A <THREE WAY BALL VALVE> is a <THREE WAY VALVE> that is <A BALL VALVE> with three paths of flow through the valve body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLUG VALVE","THREE WAY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE WAY PLUG VALVE",null,null,null,null,null,"rdl:RDS7019601",null,"A <THREE WAY PLUG VALVE> is a <PLUG VALVE> and a <THREE WAY VALVE> that is a plug valve with three paths of flow through the valve body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTI WAY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TWO WAY VALVE",null,null,null,null,null,"rdl:RDS6331623",null,"A <TWO WAY VALVE> is a <MULTI WAY VALVE> that is made with two separate paths of flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE","TWO WAY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TWO WAY BALL VALVE",null,null,null,null,null,"rdl:RDS6689332",null,"A <TWO WAY BALL VALVE> is a <TWO WAY VALVE> that is <A BALL VALVE> with two paths of flow through the valve body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTIPLE SEAT VALVE",null,null,null,null,null,"rdl:RDS6330042",null,"A <MULTIPLE SEAT VALVE> is an <ARTEFACT> and a <VALVE> that has more than two seats",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTIPORT VALVE",null,null,null,null,null,"rdl:RDS6329980",null,"A <MULTIPORT VALVE> is an <ARTEFACT> and a <VALVE> that has three or more ports arranged to switch flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTIPORT VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOUR PORT VALVE",null,null,null,null,null,"rdl:RDS6330166",null,"A <FOUR PORT VALVE> is a <MULTIPORT VALVE> that has four ports",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTIPORT VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE PORT VALVE",null,null,null,null,null,"rdl:RDS6331437",null,"A <THREE PORT VALVE> is a <MULTIPORT VALVE> that has three ports",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MULTIPORT VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TWO PORT VALVE",null,null,null,null,null,"rdl:RDS11506315",null,"A <TWO PORT VALVE> is a <MULTIPORT VALVE> that has two ports",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"OPERATED VALVE",null,null,null,null,null,"rdl:RDS11141590",null,"An <OPERATED VALVE> is an <ARTEFACT> and a <VALVE> that includes an external means of operation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"OPERATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACTUATED VALVE",null,null,null,null,null,"rdl:RDS430649",null,"An <ACTUATED VALVE> is an <OPERATED VALVE> where the operator is an <ACTUATOR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACTUATED VALVE WITH MANUAL OVERRIDE",null,null,null,null,null,"rdl:RDS16744303",null,"An <ACTUATED VALVE WITH MANUAL OVERRIDE> is an <ACTUATED VALVE > having means for overriding the actuator and operating the valve manually",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICALLY ACTUATED VALVE",null,null,null,null,null,"rdl:RDS16742668",null,"An <ELECTRICALLY ACTUATED VALVE> is an <ACTUATED VALVE> with an electric (motor) actuator",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EMERGENCY SHUT DOWN VALVE",null,null,null,null,null,"rdl:RDS11274560",null,"An <EMERGENCY SHUT DOWN VALVE> is an <ACTUATED VALVE> that is assigned to act in case of emergency",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULICALLY ACTUATED VALVE",null,null,null,null,null,"rdl:RDS16742764",null,"A <HYDRAULICALLY ACTUATED VALVE> is an <ACTUATED VALVE> operated by an hydraulic actuator",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE","ELECTRICAL APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOTOR OPERATED VALVE",null,null,null,null,null,"rdl:RDS11142220",null,"A <MOTOR OPERATED VALVE> is an <ACTUATED VALVE> and an <ELECTRICAL APPARATUS> that is opened and closed with a motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PILOT OPERATED VALVE",null,null,null,null,null,"rdl:RDS11501880",null,"A <PILOT OPERATED VALVE> is an <ACTUATED VALVE> intended to be opened and closed using another (pilot) valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PILOT OPERATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PILOT OPERATED CONTROL VALVE",null,null,null,null,null,"rdl:RDS16743608",null,"A <PILOT OPERATED CONTROL VALVE> is a <PILOT OPERATED VALVE> with a shear seal type slide valve as the main stage and a solenoid valve as the pilot stage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PILOT OPERATED CONTROL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PILOT OPERATED DIRECTIONAL CONTROL VALVE",null,null,null,null,null,"rdl:RDS16743774",null,"A <PILOT OPERATED DIRECTIONAL CONTROL VALVE> is a <PILOT OPERATED CONTROL VALVE> that has a reset spring for returning the control valve to its closed position if the supply pressure drops below the reset pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PILOT OPERATED CONTROL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PILOT OPERATED ENERGIZED DIRECTIONAL CONTROL VALVE",null,null,null,null,null,"rdl:RDS16743853",null,"A <PILOT OPERATED ENERGIZED DIRECTIONAL CONTROL VALVE> is a <PILOT OPERATED CONTROL VALVE> using a directional solenoid for returning the control valve to its closed position if the solenoid power is switched off or the pilot supply pressure drops below the minimum required pilot pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PILOT OPERATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STARTING AIR VALVE",null,null,null,null,null,"rdl:RDS13659860",null,"A <STARTING AIR VALVE> is a <PILOT OPERATED VALVE> that is assigned to let start air into the cylinder of an internal combustion engine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STARTING AIR VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STARTING AIR VALVE FOR CYLINDER HEAD WITH INTEGRATED VALVES",null,null,null,null,null,"rdl:RDS13704486",null,"A <STARTING AIR VALVE FOR CYLINDER HEAD WITH INTEGRATED VALVES> is a <STARTING AIR VALVE> that is designed for being utilized on cylinder heads with integrated valves",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STARTING AIR VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STARTING AIR VALVE FOR CYLINDER HEAD WITH BUILT ON VALVE HOUSING",null,null,null,null,null,"rdl:RDS13704548",null,"A <STARTING AIR VALVE FOR CYLINDER HEAD WITH BUILT ON VALVE HOUSING> is a <STARTING AIR VALVE> that is designed for being utilized on cylinder heads with built on valve housing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PILOT VALVE",null,null,null,null,null,"rdl:RDS7456999",null,"A <PILOT VALVE> is an <ACTUATED VALVE> that can be used in fluid systems to control the supply of driving fluid to an actuator (i.e. of another valve)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE","PNEUMATIC APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATICALLY ACTUATED VALVE",null,null,null,null,null,"rdl:RDS16743529",null,"A <PNEUMATICALLY ACTUATED VALVE> is an <ACTUATED VALVE> and a <PNEUMATIC APPARATUS> operated by an pneumatic actuator",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REMOTE OPERATED VALVE",null,null,null,null,null,"rdl:RDS11141500",null,"A <REMOTE OPERATED VALVE> is an <ACTUATED VALVE> that can be opened and closed via a non-local control system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ACTUATED VALVE","ELECTRICAL ELEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLENOID VALVE",null,null,null,null,null,"rdl:RDS431279",null,"A <SOLENOID VALVE> is a <VALVE> and an <ACTUATED VALVE> and an <ELECTRIC ELEMENT> with a linear action, fitted with a solenoid for quick operation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,"rdl:RDS5791925",null,"A <DIRECTIONAL SOLENOID VALVE> is a <SOLENOID VALVE> that operates in only one direction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CORE-DISC SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1460612641",null,"A <CORE-DISC SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a core-disc valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECTIONAL SPOOL SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465954351",null,"A <DIRECTIONAL SPOOL SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a directional spool valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLAPPER DISC SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465901811",null,"A <FLAPPER DISC SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a swing check valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOATING DIAPHRAGM SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465915931",null,"A <FLOATING DIAPHRAGM SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a floating diaphragm valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HUNG DIAPHRAGM SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465943841",null,"A <HUNG DIAPHRAGM SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a hung diaphragm valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVER DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465939741",null,"A <LEVER DIRECTIONAL SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a lever operated valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PISTON SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465946921",null,"A <PISTON SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a piston valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POPPET DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1460663261",null,"A <POPPET DIRECTIONAL SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a poppet valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLIDE DISC DIRECTIONAL SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1465952771",null,"A <SLIDE DISC DIRECTIONAL SOLENOID VALVE> is a <DIRECTIONAL SOLENOID VALVE> where the valve is a sliding disc valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SOLENOID VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPRING RETURN SOLENOID VALVE",null,null,null,null,null,"rdl:RDS1472598331",null,"An <SPRING RETURN SOLENOID VALVE> is an <ARTEFACT> and a <SOLENOID VALVE> equipped with a spring reurn mechanism that closes the valve when de-enegized",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"OPERATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVER OPERATED VALVE",null,null,null,null,null,"rdl:RDS11501122",null,"A <LEVER OPERATED VALVE> is an <OPERATED VALVE> intended to be opened and closed by a lever",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"OPERATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MANUALLY OPERATED VALVE",null,null,null,null,null,"rdl:RDS292499",null,"A <MANUALLY OPERATED VALVE> is an <OPERATED VALVE> that is regulated with hand power",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"OPERATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROV OPERATED SUBSEA VALVE",null,null,null,null,null,"rdl:RDS16704580",null,"A <ROV OPERATED SUBSEA VALVE> is an <OPERATED VALVE> having means enabling the operation of the valve using a remote operated torque tool",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROV OPERATED SUBSEA VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROV OPERATED BALL VALVE",null,null,null,null,null,"rdl:RDS16742171",null,"A <ROV OPERATED BALL VALVE> is a <ROV OPERATED SUBSEA VALVE> that is <A BALL VALVE>"]
[null,null,"ROV OPERATED BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROV OPERATED BALL VALVE 10 INS",null,null,null,null,null,"rdl:RDS16742312",null,"A <ROV OPERATED BALL VALVE 10 INS> is an <ROV OPERATED BALL VALVE> having a nominal bore of 10 inches",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROV OPERATED BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROV OPERATED BALL VALVE 12 INS",null,null,null,null,null,"rdl:RDS16742250",null,"A <ROV OPERATED BALL VALVE 12 INS> is an <ROV OPERATED BALL VALVE> having a nominal bore of 12 inches",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROV OPERATED BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROV OPERATED BALL VALVE 14 INS",null,null,null,null,null,"rdl:RDS16742374",null,"A <ROV OPERATED BALL VALVE 14 INS> is an <ROV OPERATED BALL VALVE> having a nominal bore of 14 inches",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"PIGGABLE VALVE",null,null,null,null,null,"rdl:RDS14113685",null,"A <PIGGABLE VALVE> is an <ARTEFACT> and a <VALVE> that is a full bore valve suitable for the passage of pigs and spheres",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE","PIGGABLE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRUNNION BALL VALVE",null,null,null,null,null,"rdl:RDS903509",null,"A <TRUNNION BALL VALVE> is a <PIGGABLE VALVE> and a <BALL VALVE> that has a trunnion mounted ball closure member",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"REDUCED BORE BALL VALVE","TRUNNION BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REDUCED BORE TRUNNION BALL VALVE",null,null,null,null,null,"rdl:RDS14113415",null,"A <REDUCED BORE TRUNNION BALL VALVE> is a <TRUNNION BALL VALVE> and a <REDUCED BORE BALL VALVE> where the ball closure member is supported by a trunnion and where the opening of the closure member is too small to allow a sphere of a given size to pass through the closure member. (Diameter of the bore is reduced to the pipe bore)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"QUICK ACTING VALVE",null,null,null,null,null,"rdl:RDS14113730",null,"A <QUICK ACTING VALVE> is an <ARTEFACT> and a <VALVE> that is designed to act quickly",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"QUICK ACTING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"QUICK DUMP VALVE",null,null,null,null,null,"rdl:RDS16760396",null,"A <QUICK DUMP VALVE> is a <QUICK ACTING VALVE> used for quick bleed down of fluid from a hydraulic fluid line or hydrtaulic actuator",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"QUICK ACTING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"QUICK EXHAUST VALVE",null,null,null,null,null,"rdl:RDS11141860",null,"A <QUICK EXHAUST VALVE> is a <QUICK ACTING VALVE> that is connected to a special actuator on a second valve to enable quick exhaust",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"REDUCED BORE VALVE",null,null,null,null,null,"rdl:RDS14113460",null,"A <REDUCED BORE VALVE> is an <ARTEFACT> and a <VALVE> of which the bore is one pipe size smaller than the valves pipe size resulting in flow area being smaller than pipe",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE","REDUCED BORE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REDUCED BORE BALL VALVE",null,null,null,null,null,"rdl:RDS6689146",null,"A <REDUCED BORE BALL VALVE> is a <REDUCED BORE VALVE> and a <BALL VALVE> that has a reduced bore ball closure member, i.e. where a sphere of opening size can not pass through the valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ECCENTRIC BALL VALVE","REDUCED BORE BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REDUCED BORE ECCENTRIC BALL VALVE",null,null,null,null,null,"rdl:RDS14113640",null,"A <REDUCED BORE ECCENTRIC BALL VALVE> is a <REDUCED BORE BALL VALVE> and an <ECCENTRIC BALL VALVE> where the ball closure member is pivoted off centre to provide cam action which urges it against the seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOATING BALL VALVE","REDUCED BORE BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REDUCED BORE FLOATING BALL VALVE",null,null,null,null,null,"rdl:RDS14113370",null,"A <REDUCED BORE FLOATING BALL VALVE> is a <FLOATING BALL VALVE> and a <REDUCED BORE BALL VALVE> where the ball closure member is supported by seat rings, and free to move relative to the stem",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"REDUCTION VALVE",null,null,null,null,null,"rdl:RDS309914",null,"A <REDUCTION VALVE> is an <ARTEFACT> and a <VALVE> that can be used to reduce the pressure of the medium flowing through the valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTARY STAR VALVE",null,null,null,null,null,"rdl:RDS881684",null,"A <ROTARY STAR VALVE> is an <ARTEFACT> and a <VALVE> that has vanes intended to control streams of solids. It is usually motor driven",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTARY VALVE",null,null,null,null,null,"rdl:RDS7018814",null,"A <ROTARY VALVE> is an <ARTEFACT> and a <VALVE> that is a valve where the closure member has a rotating action. The axis of rotation is usually normal to the flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROTARY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BALL VALVE",null,null,null,null,null,"rdl:RDS416654",null,"A <BALL VALVE> is a <ROTARY VALVE> which uses a hollow, perforated and pivoting ball (called a &amp;quot;floating ball&amp;quot;) to control flow through it. It is open when the balls hole is in line with the flow and closed when it is pivoted 90-degrees by the valve handle",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECCENTRIC BALL VALVE",null,null,null,null,null,"rdl:RDS552914",null,"An <ECCENTRIC BALL VALVE> is a <BALL VALVE> where the ball has an off centre trunnion and/or stem to provide cam action which loads it against the seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOATING BALL VALVE",null,null,null,null,null,"rdl:RDS553139",null,"A <FLOATING BALL VALVE> is a <BALL VALVE> that has a floating ball closure member",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HARD SEATED BALL VALVE",null,null,null,null,null,"rdl:RDS903734",null,"A <HARD SEATED BALL VALVE> is a <BALL VALVE> that has primary seating of metallic, ceramic, composition (Carbon/metal), or other non-resilient materials to provide hard wearing faces",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ONE PIECE BALL VALVE",null,null,null,null,null,"rdl:RDS646919",null,"An <ONE PIECE BALL VALVE> is a <BALL VALVE> that has the body in one piece; the ball being assembled from one end and held by a retainer ring which may also include a valve seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ONE PIECE BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BOTTOM ENTRY BALL VALVE",null,null,null,null,null,"rdl:RDS903869",null,"A <BOTTOM ENTRY BALL VALVE> is a <ONE PIECE BALL VALVE> that has a single piece body in which the ball is assembled from the opposite side to the stem and held in position by a seat/retainer ring fastened to the body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ONE PIECE BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"END ENTRY BALL VALVE",null,null,null,null,null,"rdl:RDS552959",null,"An <END ENTRY BALL VALVE> is a <ONE PIECE BALL VALVE> that is a one piece ball valve that has the ball assembled from one end of the bore and held in position by a seat/retainer ring fastened to the body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ONE PIECE BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEALED ONE PIECE BALL VALVE",null,null,null,null,null,"rdl:RDS903914",null,"A <SEALED ONE PIECE BALL VALVE> is an <ONE PIECE BALL VALVE> that has a single piece body in a welded construction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ONE PIECE BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TOP ENTRY BALL VALVE",null,null,null,null,null,"rdl:RDS903824",null,"A <TOP ENTRY BALL VALVE> is an <ONE PIECE BALL VALVE> that has the ball assembled from the top of the bore and held in position by a seat/retainer ring fastened to the body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE","SINGLE SEATED VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RISING STEM BALL VALVE",null,null,null,null,null,"rdl:RDS430514",null,"A <RISING STEM BALL VALVE> is a <BALL VALVE> and a <SINGLE SEATED VALVE> that is designed to seal by using the valve stem to mechanically wedge the valve ball into a stationary seat effecting a bubble tight seal",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SCREWED BODY BALL VALVE",null,null,null,null,null,"rdl:RDS904139",null,"A <SCREWED BODY BALL VALVE> is a <BALL VALVE> that has a screwed valve body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SIDE ENTRY BALL VALVE",null,null,null,null,null,"rdl:RDS14113505",null,"A <SIDE ENTRY BALL VALVE> is a <BALL VALVE> that is a two or tree piece body ball valve in which the ball is assembled via the bore of one of the body pieces",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SOFT SEATED BALL VALVE",null,null,null,null,null,"rdl:RDS903689",null,"A <SOFT SEATED BALL VALVE> is a <BALL VALVE> that has primary seats manufactured from elastomer, polymers and similar resilient or semi-resilient materials",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPLIT BODY BALL VALVE",null,null,null,null,null,"rdl:RDS903959",null,"An <SPLIT BODY BALL VALVE> is a <BALL VALVE> that has a body which can be split into two or more pieces, allowing service to be performed on the closure member, valve interior, etc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPLIT BODY BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BOLTED BODY BALL VALVE",null,null,null,null,null,"rdl:RDS904094",null,"A <BOLTED BODY BALL VALVE> is an <SPLIT BODY BALL VALVE> that has the body parts bolted together",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPLIT BODY BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE PIECE BALL VALVE",null,null,null,null,null,"rdl:RDS904049",null,"A <THREE PIECE BALL VALVE> is an <SPLIT BODY BALL VALVE> that has a body which can be split into three parts, comprising body and body end connectors including the pipe flanges",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SPLIT BODY BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TWO PIECE BALL VALVE",null,null,null,null,null,"rdl:RDS904004",null,"A <TWO PIECE BALL VALVE> is an <SPLIT BODY BALL VALVE> that can be split into two parts, comprising body and body connector",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"V BALL VALVE",null,null,null,null,null,"rdl:RDS6327380",null,"A <V BALL VALVE> is a <BALL VALVE> that has a V-shaped port in the ball",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROTARY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUTTERFLY VALVE",null,null,null,null,null,"rdl:RDS416609",null,"A <BUTTERFLY VALVE> is a <ROTARY VALVE> that has a closure member of a disc type with a shaft parallel, or near parallel, to the plane of the disc, with an axis of rotation transverse to the flow direction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BUTTERFLY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE DISC BUTTERFLY VALVE",null,null,null,null,null,"rdl:RDS552824",null,"A <DOUBLE DISC BUTTERFLY VALVE> is a <BUTTERFLY VALVE> that has two disc closure members",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BUTTERFLY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECCENTRIC BUTTERFLY VALVE",null,null,null,null,null,"rdl:RDS644894",null,"An <ECCENTRIC BUTTERFLY VALVE> is a <BUTTERFLY VALVE> that is a butterfly valve with the closure disc offset or double offset from the stem polar axis",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BUTTERFLY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LINED BUTTERFLY VALVE",null,null,null,null,null,"rdl:RDS645344",null,"A <LINED BUTTERFLY VALVE> is a <BUTTERFLY VALVE> that has the body internally lined",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LINED BUTTERFLY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RUBBER LINED BUTTERFLY VALVE",null,null,null,null,null,"rdl:RDS646424",null,"A <RUBBER LINED BUTTERFLY VALVE> is a <LINED BUTTERFLY VALVE> that has the rotational axis of the disc concentric with the shaft axis, and where the rubber lining of the body forms the valve seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROTARY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PLUG VALVE",null,null,null,null,null,"rdl:RDS421109",null,"A <PLUG VALVE> is a <ROTARY VALVE> that has a quarter turn action in which the closure member is a cylindrical or tapered plug which operates by rotating on its axis and sealing against a downstream seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLUG VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAGE GUIDED VALVE",null,null,null,null,null,"rdl:RDS11142400",null,"A <CAGE GUIDED VALVE> is a <PLUG VALVE> that is a valve where the plug is guided by a cage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLUG VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LUBRICATED PLUG VALVE",null,null,null,null,null,"rdl:RDS645254",null,"A <LUBRICATED PLUG VALVE> is a <PLUG VALVE> that has grooved seating areas and passageways for lubricant injection which reduces operating torque and assist sealing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LUBRICATED PLUG VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE BALANCED PLUG VALVE",null,null,null,null,null,"rdl:RDS646019",null,"A <PRESSURE BALANCED PLUG VALVE> is a <LUBRICATED PLUG VALVE> that has internal passageways designed to reduce the unbalanced pressure load on the plug in order to ease operation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLUG VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON LUBRICATED PLUG VALVE",null,null,null,null,null,"rdl:RDS645389",null,"A <NON LUBRICATED PLUG VALVE> is a <PLUG VALVE> that is not depending on the injection of lubricant or sealant for operation and seating",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"NON LUBRICATED PLUG VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LINED PLUG VALVE",null,null,null,null,null,"rdl:RDS645209",null,"A <LINED PLUG VALVE> is a <NON LUBRICATED PLUG VALVE> that has a body which is internally lined",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"NON LUBRICATED PLUG VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PLUG VALVE WITH LIFTING PLUG",null,null,null,null,null,"rdl:RDS645164",null,"A <PLUG VALVE WITH LIFTING PLUG> is a <NON LUBRICATED PLUG VALVE> that contains a plug that is lifted clear of the seat during rotation from open to close to reduce operating torque",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"NON LUBRICATED PLUG VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLEEVE LINED PLUG VALVE",null,null,null,null,null,"rdl:RDS647009",null,"An <SLEEVE LINED PLUG VALVE> is a <NON LUBRICATED PLUG VALVE> that has a sleeve of PTFE or similar polymer material fitted into the valve body in the plug seating and sealing area",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLUG VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PARALLEL PLUG VALVE",null,null,null,null,null,"rdl:RDS645659",null,"A <PARALLEL PLUG VALVE> is a <PLUG VALVE> that is equipped with a parallel valve plug",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROTARY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"QUARTER TURN VALVE",null,null,null,null,null,"rdl:RDS7018876",null,"A <QUARTER TURN VALVE> is a <ROTARY VALVE> that is a rotary valve where the rotation of the operating mechanism is limited to 90 degrees",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"SAMPLING VALVE",null,null,null,null,null,"rdl:RDS11274110",null,"A <SAMPLING VALVE> is an <ARTEFACT> and a <VALVE> that can be used to take samples from a vessel or piping system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION FUNCTION","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"SELF-OPERATING VALVE",null,null,null,null,null,"rdl:RDS7018938",null,"A <SELF-OPERATING VALVE> is an <INSTRUMENTATION FUNCTION> and a <VALVE> that includes a means of operation (e.g. spring / gravity / fluid pressure / counter balance), and is not depending on an external source of energy",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW REGULATOR",null,null,null,null,null,"rdl:RDS880109",null,"A <FLOW REGULATOR> is a <SELF-OPERATING VALVE> for fluid flow",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"FLOW REGULATOR","INSTRUMENTATION ITEM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPRINKLER CONTROL VALVE",null,null,null,null,null,"rdl:RDS312074",null,"An <SPRINKLER CONTROL VALVE> is an <INSTRUMENTATION ITEM> and a <FLOW REGULATOR> that can be used to control the flow of fluid to a sprinkler system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL REGULATOR",null,null,null,null,null,"rdl:RDS880739",null,"A <LEVEL REGULATOR> is a <SELF-OPERATING VALVE> for level",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOAT CHAMBER",null,null,null,null,null,"rdl:RDS5782529",null,"A <FLOAT CHAMBER> is an <INSTRUMENTATION ITEM> and a <LEVEL REGULATOR> which is a device for automatically regulating the supply of a liquid to a system using a valve operated by a float inside a chamber",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOAT CHAMBER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRAP",null,null,null,null,null,"rdl:RDS7455439",null,"A <TRAP> is a <FLOAT CHAMBER> for collection and discharge of unwanted condensate from an air-, gas- or steam-flow in pipes, jackets or reservoirs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRAP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR RELEASE TRAP",null,null,null,null,null,"rdl:RDS294839",null,"An <AIR RELEASE TRAP> is a <TRAP> that is accumulating unwanted air in a closed system and release it",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRAP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR TRAP",null,null,null,null,null,"rdl:RDS648809",null,"An <AIR TRAP> is a <TRAP> which, by a water seal, prevents foul air from rising from sinks, wash basins, drains, sewers etc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRAP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STEAM TRAP",null,null,null,null,null,"rdl:RDS5782388",null,"A <STEAM TRAP> is a <TRAP> that consists of a chamber into which condensed steam from steam pipes etc. is allowed to drain, and which automatically ejects it without permitting the escape of steam",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","LEVEL REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOAT VALVE",null,null,null,null,null,"rdl:RDS553184",null,"A <FLOAT VALVE> is an <INSTRUMENTATION ITEM> and a <LEVEL REGULATOR> that usually is operated by a float mechanism to regulate or maintain a liquid level in a tank",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOAT VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR RELEASE VALVE",null,null,null,null,null,"rdl:RDS7027945",null,"An <AIR RELEASE VALVE> is a <FLOAT VALVE> that is made for gas or vapour release from a liquid system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOAT VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOAT VALVE (INTERNAL)",null,null,null,null,null,"rdl:RDS11142265",null,"A <FLOAT VALVE (INTERNAL)> is a <FLOAT VALVE> that is operated by an internal float mechanism",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"OVERPRESSURE PROTECTOR","SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OVERPRESSURE PROTECTION VALVE",null,null,null,null,null,"rdl:RDS16207641",null,"An <OVERPRESSURE PROTECTION VALVE> is a <SELF-OPERATING VALVE> and an <OVERPRESSURE PROTECTOR>"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE REGULATOR",null,null,null,null,null,"rdl:RDS309149",null,"A <PRESSURE REGULATOR> is a <SELF-OPERATING VALVE> for pressure",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR PRESSURE REGULATOR",null,null,null,null,null,"rdl:RDS5794822",null,"An <AIR PRESSURE REGULATOR> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that is intended to control the air supply pressure to a consumer and keeping it invariable independent of the air consumption",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR PRESSURE REGULATOR AND FILTER",null,null,null,null,null,"rdl:RDS5794965",null,"An <AIR PRESSURE REGULATOR AND FILTER> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that is an assembly of an air pressure regulator and an air filter",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BACK PRESSURE REGULATOR",null,null,null,null,null,"rdl:RDS1011194",null,"A <BACK PRESSURE REGULATOR> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that uses the up-stream pressure to control the valve trim position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL PRESSURE REGULATOR",null,null,null,null,null,"rdl:RDS879344",null,"A <DIFFERENTIAL PRESSURE REGULATOR> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that uses the differential pressure to control the valve trim and regulate the pressure in a process system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECT OPERATED PRESSURE REGULATOR",null,null,null,null,null,"rdl:RDS879524",null,"A <DIRECT OPERATED PRESSURE REGULATOR> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that is using direct feed back of the outlet pressure to correct the valve trim position and maintain a constant outlet pressure independent of the flow",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PILOT OPERATED REGULATOR",null,null,null,null,null,"rdl:RDS882134",null,"A <PILOT OPERATED REGULATOR> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> where a diaphragm responds quickly to the downstream pressure, causing an immediate correction of the main valve plug position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE REDUCING VALVE",null,null,null,null,null,"rdl:RDS646199",null,"A <PRESSURE REDUCING VALVE> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that is equipped with an internal pressure sensing element that reduces the upstream line pressure to a set level downstream, and maintains the reduced pressure irrespective of changes in upstream pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE REGULATOR VALVE",null,null,null,null,null,"rdl:RDS309284",null,"A <PRESSURE REGULATOR VALVE> is an <INSTRUMENTATION ITEM> and a <REGULATOR> that can be used to regulate the pressure in a container or system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPRING-LOADED CONSTANT DOWNSTREAM PRESSURE VALVE",null,null,null,null,null,"rdl:RDS11141815",null,"An <SPRING-LOADED CONSTANT DOWNSTREAM PRESSURE VALVE> is an <INSTRUMENTATION ITEM> and a <PRESSURE REGULATOR> that acts against a spring pressure to maintain a constant downstream pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE RELIEF DEVICE",null,null,null,null,null,"rdl:RDS309329",null,"A <PRESSURE RELIEF DEVICE> is a <SELF-OPERATING VALVE>, that relieves pressure from an exclosed space when the pressure reaches a predetermined value",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE RELIEF DEVICE","VACUUM RELIEF DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE VACUUM RELIEF VALVE",null,null,null,null,null,"rdl:RDS6330659",null,"A <PRESSURE VACUUM RELIEF VALVE> is an <INSTRUMENTATION ITEM> and a <PRESSURE RELIEF DEVICE> and a <VACUUM RELIEF DEVICE> that automatically releases excess pressure or admits pressure to prevent a vacuum",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE RELIEF DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RELIEF VALVE",null,null,null,null,null,"rdl:RDS416699",null,"A <RELIEF VALVE> is an <INSTRUMENTATION ITEM> and a <PRESSURE RELIEF DEVICE> that is set to open at a certain pressure level to prevent the pressure in a container or system from reaching unsafe levels",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BALANCED RELIEF VALVE",null,null,null,null,null,"rdl:RDS6333340",null,"A <BALANCED RELIEF VALVE> is a <RELIEF VALVE> that incorporates means of minimizing the effect of back pressure on the operational characteristics of the valve (opening pressure, closing pressure and relieving capacity)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALANCED RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BALANCED RELIEF VALVE COMBINED",null,null,null,null,null,"rdl:RDS7461715",null,"A <BALANCED RELIEF VALVE COMBINED> is a <BALANCED RELIEF VALVE> that is equipped with balancing bellows and an auxiliary balancing piston",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALANCED RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BALANCED RELIEF VALVE USING BELLOWS",null,null,null,null,null,"rdl:RDS7461670",null,"A <BALANCED RELIEF VALVE USING BELLOWS> is a <BALANCED RELIEF VALVE> that is equipped with balancing bellows. The balancing bellows minimizes the effects of backpressure and prevents the process fluid from entering the spring chamber",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALANCED RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BALANCED RELIEF VALVE USING PISTON",null,null,null,null,null,"rdl:RDS7461625",null,"A <BALANCED RELIEF VALVE USING PISTON> is a <BALANCED RELIEF VALVE> that is equipped with a balancing piston. The balanced piston design minimizes the effects of backpressure and prevents the process fluid from entering the spring chamber",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONVENTIONAL RELIEF VALVE",null,null,null,null,null,"rdl:RDS885239",null,"A <CONVENTIONAL RELIEF VALVE> is a <RELIEF VALVE> that has its closing force provided by a spring",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONVENTIONAL SAFETY RELIEF VALVE",null,null,null,null,null,"rdl:RDS7461501",null,"A <CONVENTIONAL SAFETY RELIEF VALVE> is a <RELIEF VALVE> that is equipped with vented bonnet where its performance characteristics are directly affected by changes of the back pressure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HIGH PRESSURE RELIEF VALVE",null,null,null,null,null,"rdl:RDS428309",null,"A <HIGH PRESSURE RELIEF VALVE> is a <RELIEF VALVE> that is venting off high pressure gas to the atmosphere",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PILOT-OPERATED RELIEF VALVE",null,null,null,null,null,"rdl:RDS885194",null,"A <PILOT-OPERATED RELIEF VALVE> is a <RELIEF VALVE> that uses a pilot valve to indirectly activate the main valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE RELIEF VALVE",null,null,null,null,null,"rdl:RDS7461439",null,"A <PRESSURE RELIEF VALVE> is a <RELIEF VALVE> that is an automatic pressure relieving device actuated by the static pressure upstream of the valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE","SAFETY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAFETY RELIEF VALVE",null,null,null,null,null,"rdl:RDS6330862",null,"A <SAFETY RELIEF VALVE> is a <SAFETY VALVE> and a <RELIEF VALVE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SAFETY RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CRANKCASE SAFETY RELIEF VALVE",null,null,null,null,null,"rdl:RDS13310425",null,"A <CRANKCASE SAFETY RELIEF VALVE> is a <SAFETY RELIEF VALVE> to release pressure in case of a crankcase explosion",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SAFETY RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOWNHOLE SAFETY RELIEF VALVE",null,null,null,null,null,"rdl:RDS16552132",null,"A <DOWNHOLE SAFETY VALVE> is a <SAFETY RELEIF VALVE> insertable into the well tubing to act as a well barrier",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOWNHOLE SAFETY RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SURFACE CONTROLLED SUBSURFACE SAFETY RELEIF VALVE",null,null,null,null,null,"rdl:RDS16756786",null,"A <SURFACE CONTROLLED SUBSURFACE SAFETY RELIEF VALVE> is a <DOWNHOLE SAFETY VALVE> located in a well and operated from the surface that, when it is activated, is designed to prevent uncontrolled flow up the well",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WEIGHT-OPERATED RELIEF VALVE",null,null,null,null,null,"rdl:RDS11215931",null,"A <WEIGHT-OPERATED RELIEF VALVE> is a <RELIEF VALVE> in which the closure member is held against the seat by a static weight",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"YARWAY RELIEF VALVE",null,null,null,null,null,"rdl:RDS11141545",null,"A <YARWAY RELIEF VALVE> is a <RELIEF VALVE> that is a valve installed in a bypass line on the discharge header of a pump that is recirculating the minimum flow required back to the pump suction in cases of closed discharge line",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","PRESSURE RELIEF DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAFETY VALVE",null,null,null,null,null,"rdl:RDS309374",null,"A <SAFETY VALVE> is an <INSTRUMENTATION ITEM> and a <PRESSURE RELIEF DEVICE> that is used in gas service",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SAFETY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RELIEF POP-OFF VALVE",null,null,null,null,null,"rdl:RDS17157050",null,"A <RELIEF POP-OFF VALVE> is a <SAFETY VALVE> that is designed to be used in breathing circuits. The relief pop-off valve is venting gas to the atmosphere when the pressure of the gas in the breathing circuit reaches a certain level",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SAFETY VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STRAIGHT THROUGH SAFETY VALVE",null,null,null,null,null,"rdl:RDS6331313",null,"A <STRAIGHT THROUGH SAFETY VALVE> is a <SAFETY VALVE> that is a relief valve of straight body design, usually with small bore for instrumentation purposes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE REGULATOR",null,null,null,null,null,"rdl:RDS1011284",null,"A <TEMPERATURE REGULATOR> is a <SELF-OPERATING VALVE> for temperature regulation",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","TEMPERATURE REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMOSTATIC MIXING ASSEMBLY",null,null,null,null,null,"rdl:RDS312839",null,"A <THERMOSTATIC MIXING ASSEMBLY> is an <INSTRUMENTATION ITEM> and a <TEMPERATURE REGULATOR> that maintains and limits mixed hot water to a desired, selectable temperature, helping to minimize thermal shock",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMAL RELIEF DEVICE",null,null,null,null,null,"rdl:RDS1336338491",null,"A <THERMAL RELIEF DEVICE> is a <<SELF-OPERATING VALVE> that relieves fluid from an exclosed space when the temperature reaches a predetermined value",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"SELF-OPERATING VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VACUUM RELIEF DEVICE",null,null,null,null,null,"rdl:RDS313784",null,"A <VACUUM RELIEF DEVICE> is a <SELF-OPERATING VALVE> that opens up and aligns the pressure when the underpressure of a container reaches a predetermined level",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","VACUUM RELIEF DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VACUUM RELIEF VALVE",null,null,null,null,null,"rdl:RDS6331685",null,"A <VACUUM RELIEF VALVE> is an <INSTRUMENTATION ITEM> and a <VACUUM RELIEF DEVICE> that is used for pressure compensation purposes by admitting (letting in) a pressure to prevent that vacuum is forming when filling or emptying a system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","VACUUM RELIEF DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VACUUM SAFETY VALVE",null,null,null,null,null,"rdl:RDS646289",null,"A <VACUUM SAFETY VALVE> is an <INSTRUMENTATION ITEM> and a <VACUUM RELIEF DEVICE> that automatically releases excess pressure or admits pressure to prevent a vacuum",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE SEATED VALVE",null,null,null,null,null,"rdl:RDS6330941",null,"A <SINGLE SEATED VALVE> is an <ARTEFACT> and a <VALVE> that has only one seat",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"SLIDE VALVE",null,null,null,null,null,"rdl:RDS873224",null,"A <SLIDE VALVE> is an <ARTEFACT> and a <VALVE> that opens and closes a passageway by sliding over a port",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SLIDE VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLIDING SLEEVE",null,null,null,null,null,"rdl:RDS5802062",null,"A <SLIDING SLEEVE> is a <SLIDE VALVE> that is a flow control device located in the production tubing string. It provides a means of controlling fluid flow between the production tubing and the casing annulus",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"STRAIGHTWAY VALVE",null,null,null,null,null,"rdl:RDS9390905",null,"A <STRAIGHTWAY VALVE> is an <ARTEFACT> and a <VALVE> that is straight, i.e. the centerlines perpendicular to the ends are in-line with no offset",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA MANIFOLD VALVE",null,null,null,null,null,"rdl:RDS16703028",null,"A <SUBSEA MANIFOLD VALVE> is an <ARTEFACT> and a <VALVE> that is located in the subsea manifold piping system, for isolation or fluid control",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA MANIFOLD VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA MANIFOLD VALVE 12 INS",null,null,null,null,null,"rdl:RDS16706440",null,"A <SUBSEA MANIFOLD VALVE 12 INS> is a <SUBSEA MANIFOLD VALVE> with 12 inch orifice size",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA MANIFOLD VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA MANIFOLD VALVE 2 1/16 INS",null,null,null,null,null,"rdl:RDS16706327",null,"A <SUBSEA MANIFOLD VALVE 2 1/16 INS> is a <SUBSEA MANIFOLD VALVE> with 2 1/16 inch orifice size",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA MANIFOLD VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA MANIFOLD VALVE 5 1/8 INS",null,null,null,null,null,"rdl:RDS16706214",null,"A <SUBSEA MANIFOLD VALVE 5 1/8 INS> is a <SUBSEA MANIFOLD VALVE> with 5 1/8 inch orifice size",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA MANIFOLD VALVE 5 1/8 INS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRODUCTION MANIFOLD VALVE 5 1/8 INS",null,null,null,null,null,"rdl:RDS16704460",null,"A <PRODUCTION MANIFOLD VALVE 5 1/8 INS> is a <SUBSEA MANIFOLD VALVE 5 1/8 INS> that is a production manifold valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"TANK VALVE",null,null,null,null,null,"rdl:RDS11274155",null,"A <TANK VALVE> is an <ARTEFACT> and a <VALVE> that can be used in connection with a hook-up to a (storage) tank",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"TAP",null,null,null,null,null,"rdl:RDS312569",null,"A <TAP> is an <ARTEFACT> and a <VALVE> that controls the flow of liquid or gas from a pipe or container. Taps are often attached to a sink or bath",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"TIGHT SHUT OFF VALVE",null,null,null,null,null,"rdl:RDS6331561",null,"A <TIGHT SHUT OFF VALVE> is an <ARTEFACT> and a <VALVE> that has a low leakage characteristic",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"UNI-DIRECTIONAL VALVE",null,null,null,null,null,"rdl:RDS5792107",null,"A <UNI-DIRECTIONAL VALVE> is an <ARTEFACT> and a <VALVE> that is designed to seal in one flow direction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE NORMALLY CLOSED",null,null,null,null,null,"rdl:RDS2229154",null,"A <VALVE NORMALLY CLOSED> is an <ARTEFACT> and a <VALVE> that is normally in an <CLOSED> position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE NORMALLY OPEN",null,null,null,null,null,"rdl:RDS313919",null,"A <VALVE NORMALLY OPEN> is an <ARTEFACT> and a <VALVE> that is normally in an <OPEN> position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE THAT REMAINS IN POSITION IN FAILURE MODE",null,null,null,null,null,"rdl:RDS314009",null,"A <VALVE THAT REMAINS IN POSITION IN FAILURE MODE> is an <ARTEFACT> and a <VALVE> that is designed to keep the valve opening (as regulated by the valve closure member) in an unchanged position in case of failure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE THAT REMAINS IN POSITION AT LOSS OF AIR SUPPLY",null,null,null,null,null,"rdl:RDS314054",null,"A <VALVE THAT REMAINS IN POSITION AT LOSS OF AIR SUPPLY> is an <ARTEFACT> and a <VALVE> that is controlled and also usually powered by the use of pressurised air, and that is designed to keep the valve opening (as regulated by the closure member) in an unchanged position in case of loss of air supply",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"VENT VALVE",null,null,null,null,null,"rdl:RDS11274290",null,"A <VENT VALVE> is an <ARTEFACT> and a <VALVE> that can be used for ventilation purposes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"WAFER PATTERN VALVE",null,null,null,null,null,"rdl:RDS6327521",null,"A <WAFER PATTERN VALVE> is an <ARTEFACT> and a <VALVE> that has a short and flangeless body intended for installation directly between piping flanges",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"WEIGHT-LOADED VALVE",null,null,null,null,null,"rdl:RDS315404",null,"A <WEIGHT-LOADED VALVE> is an <ARTEFACT> and a <VALVE> in which the closure member is held against the seat by a static weight. The valve opens when the internal fluid pressure the valve is exposed to is higher than the force the weight creates in the valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"WELLHEAD SEAL TESTING VALVE",null,null,null,null,null,"rdl:RDS4858923021",null,"A <WELLHEAD SEAL TESTING VALVE> is an <ARTEFACT> and a <VALVE> for wellhead seal testing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"WET PIPE SPRINKLER VALVE SET",null,null,null,null,null,"rdl:RDS315584",null,"A <WET PIPE SPRINKLER VALVE SET> is an <ARTEFACT> and a <VALVE> that is a set of valves which can be used in a wet pipe sprinkler system to put out a possible fire",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,"Y-PATTERN VALVE",null,null,null,null,null,"rdl:RDS6331900",null,"A <Y-PATTERN VALVE> is an <ARTEFACT> and a <VALVE> that has in-line ports and stem emerging at an angle of approx 45 degrees",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"Y-PATTERN VALVE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OBLIQUE PATTERN VALVE, WYE-BODY VALVE",null,null,null,null,null,"rdl:RDS14111345",null,"An <OBLIQUE PATTERN VALVE, WYE-BODY VALVE> is a <Y-PATTERN VALVE> that has inline ports and a stem emerging at an angle approx 45 degrees",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"REGULATOR",null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE REGULATOR",null,null,null,null,null,"rdl:RDS7124200",null,"A <VOLTAGE REGULATOR> is a <REGULATOR> designed to automatically maintain a constant voltage level",null,null,null,null,null,"dm:ClassOfFunctionalObject"]