{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["RDL browser","Settings","about","Results1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"RDL browser","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[[0,0,0,4]]}
["RDL2 browser to spreadsheet tool version 75",null,null,null,null,null,"Endpoint: http://data.15926.org/rdl/"]
["Contact: onno.paap@gmail.com",null,null,null,null,"Action","ASSOCIATED PHASE LAYOUT SUBSTATION","http://data.15926.org/rdl/RDS959084"]
[null,null,null,null,null,"Action","ATTENDED SUBSTATION","http://data.15926.org/rdl/RDS959219"]
["Search:","SUBSTATION",null,null,null,"Action","CONVERTER SUBSTATION","http://data.15926.org/rdl/RDS958229"]
[null,null,null,null,null,"Action","DOUBLE BUSBAR SUBSTATION","http://data.15926.org/rdl/RDS958634"]
[null,null,null,null,null,"Action","FOUR-SWITCH MESH SUBSTATION","http://data.15926.org/rdl/RDS958814"]
[null,null,null,null,null,"Action","FOUR-SWITCH MESH SUBSTATION WITH MESH OPENING DISCONNECTORS","http://data.15926.org/rdl/RDS958949"]
[null,null,null,null,null,"Action","FREQUENCY CONVERTER SUBSTATION","http://data.15926.org/rdl/RDS958274"]
[null,null,null,null,null,"Action","GAS INSULATED METAL-ENCLOSED SUBSTATION","http://data.15926.org/rdl/RDS959309"]
[null,null,null,null,null,"Action","INDOOR SUBSTATION","http://data.15926.org/rdl/RDS959354"]
[null,null,null,null,null,"Action","KIOSK SUBSTATION","http://data.15926.org/rdl/RDS959444"]
[null,null,null,null,null,"Action","MANNED SUBSTATION","http://data.15926.org/rdl/RDS958319"]
[null,"Note: first set coloring on in Settings",null,null,null,"Action","MASTER SUBSTATION","http://data.15926.org/rdl/RDS958499"]
[null,"Coloring (containing this string will give this color)",null,null,null,"Action","MESH SUBSTATION","http://data.15926.org/rdl/RDS958769"]
[null,"ClassOfFunctionalObject",null,null,null,"Action","MIXED PHASE LAYOUT SUBSTATION","http://data.15926.org/rdl/RDS959174"]
[null,"ClassOfInanimatePhysicalObject ",null,null,null,"Action","OPEN TYPE SUBSTATION","http://data.15926.org/rdl/RDS959264"]
[null,null,null,null,null,"Action","OUTDOOR SUBSTATION","http://data.15926.org/rdl/RDS959399"]
[null,null,null,null,null,"Action","PERMANENTLY MANNED SUBSTATION","http://data.15926.org/rdl/RDS958409"]
[null,null,null,null,null,"Action","POLE-MOUNTED SUBSTATION","http://data.15926.org/rdl/RDS959534"]
[null,null,null,null,null,"Action","REMOTELY CONTROLLED SUBSTATION","http://data.15926.org/rdl/RDS958454"]
[null,null,null,null,null,"Action","RING SUBSTATION","http://data.15926.org/rdl/RDS958724"]
[null,null,null,null,null,"Action","SATELLITE SUBSTATION","http://data.15926.org/rdl/RDS958544"]
[null,null,null,null,null,"Action","SEPARATED PHASE LAYOUT SUBSTATION","http://data.15926.org/rdl/RDS959129"]
[null,null,null,null,null,"Action","SINGLE BUSBAR SUBSTATION","http://data.15926.org/rdl/RDS958589"]
[null,"Namespace replacer (definition containing this string replaces the namespace)",null,null,null,"Action","STEP-DOWN SUBSTATION","http://data.15926.org/rdl/RDS958139"]
[null,"API","API:",null,null,"Action","STEP-UP SUBSTATION","http://data.15926.org/rdl/RDS958094"]
[null,"ASME","ASME:",null,null,"Action","SUBSTATION","http://data.15926.org/rdl/RDS957959"]
[null,"ASTM","ASTM:",null,null,"Action","SUBSTATION BAY","http://data.15926.org/rdl/RDS1005524"]
[null,"DIN","DIN:",null,null,"Action","SWITCHING SUBSTATION","http://data.15926.org/rdl/RDS958004"]
[null,"EN","EN:",null,null,"Action","TAPPED SUBSTATION","http://data.15926.org/rdl/RDS1011689"]
[null,"ISO","ISO:",null,null,"Action","THREE-SWITCH MESH SUBSTATION WITH BYPASS","http://data.15926.org/rdl/RDS958859"]
[null,"NORSOK","NOR:",null,null,"Action","TRACTION SUBSTATION","http://data.15926.org/rdl/RDS958184"]
[null,"NPD","NOR:",null,null,"Action","TRANSFORMER SUBSTATION","http://data.15926.org/rdl/RDS958049"]
[null,"NS","NOR:",null,null,"Action","TRIPLE BUSBAR SUBSTATION","http://data.15926.org/rdl/RDS958679"]
[null,"ROSEMOUNT","ROS:",null,null,"Action","UNDERGROUND SUBSTATION","http://data.15926.org/rdl/RDS959489"]
[null,"SAE","SAE:",null,null,"Action","UNMANNED SUBSTATION","http://data.15926.org/rdl/RDS958364"]
[null,"SIEMENS","SIE:"]
[null,"SKOTSELV","SKOT:"]
[null,"TWR","TWR:"]

{"sheet":"Settings","index":1,"n_rows":87,"n_cols":8,"rows_kept":87,"cut":false,"hidden":true,"merged":[]}
["Setting name","Select name","OnKey","Value","Status","RDLType"]
["Endpoint","RDL2 (15926.org)",null,"http://data.15926.org/rdl/","Current",null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA RDL",null,"http://data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA Staging",null,"http://staging.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA SVRDL",null,"http://svrdl.community.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P4",null,"http://posccaesar.org/p4/sparql",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P12",null,"http://sti.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","Localhost",null,"http://localhost:8890/sparql/",null,null,null,"Note: end address always with a slash (/)"]
[]
["gBaseNamespace",null,"http://data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://staging.data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://svrdl.community.data.posccaesar.org/rdl/","http://svrdl.community.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://posccaesar.org/p4/sparql","http://posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://sti.data.posccaesar.org/rdl/","http://sti.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://localhost:8890/sparql/","http://data.15926.org/rdl/",null,"RDL2"]
["gKeepSettings",null,null,"T"]
["gShowDeprecated",null,null,"F"]
["gColoring",null,null,"T"]
["gNamespaceReplacing",null,null,"F"]
["gHyperlinkReplacing",null,null,"F"]
[]
["Endpoint","aisi",null,"http://data.15926.org/aisi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ansi",null,"http://data.15926.org/ansi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","api",null,"http://data.15926.org/api/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","all",null,"http://data.15926.org/all/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","asme",null,"http://data.15926.org/asme/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","astm",null,"http://data.15926.org/astm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","atex",null,"http://data.15926.org/atex/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","bs",null,"http://data.15926.org/bs/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","din",null,"http://data.15926.org/din/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dm",null,"http://data.15926.org/dm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dnv",null,"http://data.15926.org/dnv/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","edm",null,"http://data.15926.org/edm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","en",null,"http://data.15926.org/en/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","eu",null,"http://data.15926.org/eu/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iec",null,"http://data.15926.org/iec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ieee",null,"http://data.15926.org/ieee/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iso",null,"http://data.15926.org/iso/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","lci",null,"http://data.15926.org/lci/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","mss",null,"http://data.15926.org/mss/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nace",null,"http://data.15926.org/nace/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nec",null,"http://data.15926.org/nec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nema",null,"http://data.15926.org/nema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nfpa",null,"http://data.15926.org/nfpa/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nor",null,"http://data.15926.org/nor/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","rdl",null,"http://data.15926.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sae",null,"http://data.15926.org/sae/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sie",null,"http://data.15926.org/sie/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","tema",null,"http://data.15926.org/tema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","twr",null,"http://data.15926.org/twr/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","uns",null,"http://data.15926.org/uns/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","wits",null,"http://data.15926.org/wits/",null,null,null,"Note: end address always with a slash (/)"]
[]
[]
["gBaseNamespace",null,"http://data.15926.org/aisi/","http://data.15926.org/aisi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ansi/","http://data.15926.org/ansi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/api/","http://data.15926.org/api/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/asme/","http://data.15926.org/asme/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/all/","http://data.15926.org/all/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/astm/","http://data.15926.org/astm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/atex/","http://data.15926.org/atex/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/bs/","http://data.15926.org/bs/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/din/","http://data.15926.org/din/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dm/","http://data.15926.org/dm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dnv/","http://data.15926.org/dnv/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/edm/","http://data.15926.org/edm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/en/","http://data.15926.org/en/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/eu/","http://data.15926.org/eu/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iec/","http://data.15926.org/iec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ieee/","http://data.15926.org/ieee/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iso/","http://data.15926.org/iso/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/lci/","http://data.15926.org/lci/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/mss/","http://data.15926.org/mss/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nace/","http://data.15926.org/nace/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nec/","http://data.15926.org/nec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nema/","http://data.15926.org/nema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nfpa/","http://data.15926.org/nfpa/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nor/","http://data.15926.org/nor/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sae/","http://data.15926.org/sae/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sie/","http://data.15926.org/sie/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/tema/","http://data.15926.org/tema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/twr/","http://data.15926.org/twr/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/uns/","http://data.15926.org/uns/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/wits/","http://data.15926.org/wits/",null,"RDL2"]
["                                          "]

{"sheet":"about","index":2,"n_rows":176,"n_cols":3,"rows_kept":176,"cut":false,"hidden":false,"merged":[]}
["Version 75 changes","2018-10-05","Onno Paap"]
["missing superclasses - and orphans- filter no deprecated classes"]
[]
["Version 74 changes","2018-09-30","Onno Paap"]
["Repaired bug missing label"]
[]
["Version 73 changes","2018-05-16","Onno Paap"]
["Repaired bug Deprecated Superclass"]
[]
[]
[]
["Version 71 changes","2016-07-17","Onno Paap"]
["Aded report button for comparison of RDL2 with a subfolder called views filled with spreadsheets."]
[]
[]
["Version 69 changes","2016-06-16","Onno Paap"]
["Added button: \"errors in definitions\" that lists all classes that have more or less \"<\" brackets than the number of super class relationships + 1. Where the part after the word \"that \"  is ignored in the count of \"<\" brackets."]
[]
["Version 68 changes","2016-06-13","Onno Paap"]
["Updated endpoint of RDL2 sparql "]
[]
["Version 67 changes","2016-05-22","Onno Paap"]
["Added button list subclasses from superclass "]
[]
["Version 65 changes","2016-04-25","Onno Paap"]
["Added checkbox at action dialog \"supress double child occurances\" so that this built-in feature can be switched off"]
[]
["Version 64 changes","2016-04-20","Onno Paap"]
["Made search case-insensitive and added endpoint \"all\""]
[]
["Version 63 changes","2016-09-28","Onno Paap"]
["Made entity list working on P4 endpoint (they changed the database version which was not accepting som sparql setting)"]
["Version 62 changes","2016-09-28","Onno Paap"]
["Applied show deprecated to searched result list"]
[]
["Version 61 changes","2016-08-29","Onno Paap"]
["Added query from pcardl for ClassOfIndirectProperty"]
[]
["Version 60 changes","2016-08-19","Onno Paap"]
["Repaired failing entity reports"]
[]
["Version 59 changes","2016-08-19","Onno Paap"]
["Missing superclasses now queries whole federation of RDL2"]
[]
["Version 58 changes","2016-08-16","Onno Paap"]
["Repaired missing output for entities and doubles in RDL2 endpoints other than rdl"]
[]
["Version 57 changes","2016-08-13","Onno Paap"]
["Doubles report now skips classes that are deprecated"]
[]
["Version 56 changes","2016-07-22","Onno Paap"]
["Made rowheight suitable for longer definitions to example DESIGN BASIS"]
[]
["Version 55 changes","2016-07-19","Onno Paap"]
["Made rowheight suitable for longer definitions"]
[]
["Version 54 changes","2016-07-03","Onno Paap"]
["Entity Type field changed to 6 merged cells."]
[]
["Version 53 changes","2016-06-23","Onno Paap"]
["added lci namespace"]
[]
["Version 52 changes","2016-06-23","Onno Paap"]
["Added deprecated count to list entities"]
[]
["Version 51 changes","2016-06-19","Onno Paap"]
["Updated namespaces of staging RDL"]
[]
["Version 50 changes","2016-06-19","Onno Paap"]
["taxonomy view repaired missing entity type"]
[]
["Version 49 changes","2016-06-14","Onno Paap"]
["Room for 12 superclasses"]
[]
["Version 48 changes","2016-06-14","Onno Paap"]
["Repaired NOR:/RDS  bug"]
[]
["Version 47 changes","2016-06-14","Onno Paap"]
["Repaired endpoint bug"]
[]
["Version 46 changes","2016-06-13","Onno Paap"]
["Updated endpoints"]
[]
["Version 45 changes","2016-06-06","Onno Paap"]
["Completed Missing Superclasses report"]
[]
["Version 44 changes","2016-05-20","Onno Paap"]
["Added Clear Cache button (use on any database changes)"]
[]
["Version 43 changes","2016-05-19","Onno Paap"]
["Changed non-existing super classes to show as \"no label\""]
[]
["Version 42 changes","2016-05-02","Onno Paap"]
["bug fix"]
[]
["Version 41 changes","2016-05-02","Onno Paap"]
["Added setting to show/not show deprecated items. If shown, they are stricken through"]
[]
["Version 40 changes","2016-03-31","Onno Paap"]
["Added  in doubles: two classes having the same label."]
[]
["Version 39 changes","2016-03-21","Onno Paap"]
["Made the query more robust, after the server hass been returning a 404 occasionally"]
[]
["Version 38 changes","2016-03-03","Onno Paap"]
["Repaired bug entity type query on PCA endpoint"]
[]
["Version 37 changes","2016-01-29","Onno Paap"]
["Showing deprecated class in taxonomy with label in strikethrough."]
[]
["Version 36 changes","2016-01-13","Onno Paap"]
["Added the 17 endpoints of http://data.15926.org/rdl"]
[]
["Version 35 changes","2016-01-13","Onno Paap"]
["In taxonomy view, disregard all rdf:type that is not data model.  So only show rdf:type that is dm:"]
[]
["Version 34 changes","2016-01-13","Onno Paap"]
["Solved taxonomy levels regression bug"]
[]
["Version 33 changes","2016-01-11","Onno Paap"]
["Enhanced the doubled query. First 4 columns are about the triple, the rest is info."]
[]
["Repaired bug in entity type query."]
[]
["Version 30 changes","2016-01-03","Onno Paap"]
["Repaired entity type query for old PCA RDL. \nRepaired bug in entity type query where a class that has a superclass of the wanted type as well as  of another type became  the start point of a new taxonomy as well as part in the main taxonomy. (read that again)"]
[]
["Version 29 changes","2016-01-02","Onno Paap"]
["Filtered entity filtered taxonomy to only show the filtered entity not subClassOf of another entity"]
[]
["Version 27 changes","2016-01-01","Onno Paap"]
["few bugs repaired.  Changed entity search into presenting taxonomies. "]
[]
["Version 26 changes","2015-12-26","Onno Paap"]
["few bugs repaired. "]
[]
["Version 25 changes","2015-12-26","Onno Paap"]
["Added Part 12 and localhost endpoints"]
["Added button for selecting double labels and definitions. "]
["Version 24 changes","2015-12-14","Onno Paap"]
["Added button to list all distinct entity data types and their counts, and click to show."]
["Added a button to show all orphans that have a rdfs:label"]
["Version 23 changes"]
["Added endpoint posccaesar.org/p4/sparql"]
["Version 22 changes"]
["Added endpoint staging.data.posccaesar.org/rdl"]
[]
["Version 21 changes"]
["Repaired bug where namespace replace was based upon definition instead of class label"]
[]
["Version 20 changes"]
["Repaired bug where definition did not show up if hyperlink replace was on."]
[]
["Version 19 changes (skip version 16-18)"]
["Settings expanded with persist settings, namespace replacer and hyperlink replacer"]
["Added namespace replacer which will replace the RDL: namespace of the ID with the namespace given in the list on the front page."]
["Added hyperlink replacer which will find terms between single quotes and look them up in the RDL, then add a hyperlink in the text if found. Anchor tag <a></a> used not &hyperlink() so looks ugly."]
[]
["Version 15 changes"]
["Changed browser page Action buttons to hyperlinks because buttons are not equally spaced between Excel versions (Office 2007 versus Office 365)"]
["First row is empty. Move all up."]
["Make stop button for during query taxonomy query execution"]
[]
[]
["Version 14 changes"]
["Aligned buttons on browser page"]
["Made color notification work. Note: switch it on first in settings. Default is off"]
["Top align subclasses in taxonomy"]
["Subclasses made to hyperlink in taxonomy"]
["Subclasses made to increase column width in taxonomy"]
["Made browser search go when hitting enter in search field"]
[]
[]
[]
["todo"]
["Make setting for outputting to other result pages"]

{"sheet":"Results1","index":3,"n_rows":36,"n_cols":32,"rows_kept":36,"cut":false,"hidden":false,"merged":[[34,22,34,23],[34,16,34,21],[34,24,34,29],[34,30,34,33],[35,23,35,24],[35,17,35,22],[35,25,35,30],[35,31,35,34],[32,21,32,22],[32,15,32,20],[32,23,32,28],[32,29,32,32],[33,21,33,22],[33,15,33,20],[33,23,33,28],[33,29,33,32],[30,22,30,23],[30,16,30,21],[30,24,30,29],[30,30,30,33],[31,21,31,22],[31,15,31,20],[31,23,31,28],[31,29,31,32],[28,21,28,22],[28,15,28,20],[28,23,28,28],[28,29,28,32],[29,22,29,23],[29,16,29,21],[29,24,29,29],[29,30,29,33],[26,21,26,22],[26,15,26,20],[26,23,26,28],[26,29,26,32],[27,21,27,22],[27,15,27,20],[27,23,27,28],[27,29,27,32],[24,22,24,23],[24,16,24,21],[24,24,24,29],[24,30,24,33],[25,21,25,22],[25,15,25,20],[25,23,25,28],[25,29,25,32],[22,23,22,24],[22,17,22,22],[22,25,22,30],[22,31,22,34],[23,23,23,24],[23,17,23,22],[23,25,23,30],[23,31,23,34],[20,22,20,23],[20,16,20,21],[20,24,20,29],[20,30,20,33],[21,23,21,24],[21,17,21,22],[21,25,21,30],[21,31,21,34],[18,21,18,22],[18,15,18,20],[18,23,18,28],[18,29,18,32],[19,21,19,22],[19,15,19,20],[19,23,19,28],[19,29,19,32],[16,21,16,22],[16,15,16,20],[16,23,16,28],[16,29,16,32],[17,22,17,23],[17,16,17,21],[17,24,17,29],[17,30,17,33],[14,21,14,22],[14,15,14,20],[14,23,14,28],[14,29,14,32],[15,21,15,22],[15,15,15,20],[15,23,15,28],[15,29,15,32],[12,22,12,23],[12,16,12,21],[12,24,12,29],[12,30,12,33],[13,22,13,23],[13,16,13,21],[13,24,13,29],[13,30,13,33],[10,21,10,22],[10,15,10,20],[10,23,10,28],[10,29,10,32],[11,21,11,22],[11,15,11,20],[11,23,11,28],[11,29,11,32],[8,21,8,22],[8,15,8,20],[8,23,8,28],[8,29,8,32],[9,21,9,22],[9,15,9,20],[9,23,9,28],[9,29,9,32],[6,22,6,23],[6,16,6,21],[6,24,6,29],[6,30,6,33],[7,21,7,22],[7,15,7,20],[7,23,7,28],[7,29,7,32],[4,21,4,22],[4,15,4,20],[4,23,4,28],[4,29,4,32],[5,22,5,23],[5,16,5,21],[5,24,5,29],[5,30,5,33],[2,21,2,22],[2,15,2,20],[2,23,2,28],[2,29,2,32],[3,21,3,22],[3,15,3,20],[3,23,3,28],[3,29,3,32],[0,20,0,21],[0,14,0,19],[0,22,0,27],[0,28,0,31],[1,21,1,22],[1,15,1,20],[1,23,1,28],[1,29,1,32]]}
[null,null,"FunctionalObject",null,null,null,null,null,null,null,null,null,null,null,"SUBSTATION",null,null,null,null,null,"rdl:RDS957959",null,"A <SUBSTATION> is a <FunctionalObject> at which electrical current is switched, transformed, or converted, intermediate in rank between a generating station and a low-tension distribution network",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"ASSOCIATED PHASE LAYOUT SUBSTATION",null,null,null,null,null,"rdl:RDS959084",null,"An <ASSOCIATED PHASE LAYOUT SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> having a layout in which the conductors relating to the three phases of the same circuit are located side by side",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"ATTENDED SUBSTATION",null,null,null,null,null,"rdl:RDS959219",null,"An <ATTENDED SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> that is operated by personnel during the normal working hours and otherwise as necessary",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"CONVERTER SUBSTATION",null,null,null,null,null,"rdl:RDS958229",null,"A <CONVERTER SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> including converters and the main function of which is to convert alternating current into direct current or vice versa",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"DOUBLE BUSBAR SUBSTATION",null,null,null,null,null,"rdl:RDS958634",null,"A <DOUBLE BUSBAR SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> in which the lines and transformers are connected via two busbars by means of selectors",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOUBLE BUSBAR SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,"ONE-AND-A-HALF BREAKER ARRANGEMENT",null,null,null,null,null,"rdl:RDS959039",null,"An <ONE-AND-A-HALF BREAKER ARRANGEMENT> is a <DOUBLE BUSBAR SUBSTATION> where, for two circuits, three circuit-breakers are connected in series between the two busbars, the circuits being connected on each side of the central circuit-breaker.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOUBLE BUSBAR SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,"TWO-BREAKER ARRANGEMENT",null,null,null,null,null,"rdl:RDS958994",null,"A <TWO-BREAKER ARRANGEMENT> is a <DOUBLE BUSBAR SUBSTATION> in which the selectors are circuit-breakers.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"FREQUENCY CONVERTER SUBSTATION",null,null,null,null,null,"rdl:RDS958274",null,"A <FREQUENCY CONVERTER SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> in which an ac current at a given frequency is converted into an ac current at another frequency",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"GAS INSULATED METAL-ENCLOSED SUBSTATION",null,null,null,null,null,"rdl:RDS959309",null,"A <GAS INSULATED METAL-ENCLOSED SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> that is made up with only gas insulated metal enclosed switchgear",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"INDOOR SUBSTATION",null,null,null,null,null,"rdl:RDS959354",null,"An <INDOOR SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> sheltered from external weather conditions by being installed within a building",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"KIOSK SUBSTATION",null,null,null,null,null,"rdl:RDS959444",null,"A <KIOSK SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> that is compact, often prefabricated and used only for distribution purposes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"MANNED SUBSTATION",null,null,null,null,null,"rdl:RDS958319",null,"A <MANNED SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> that is locally operated by personnel working within the substation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MANNED SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,"MASTER SUBSTATION",null,null,null,null,null,"rdl:RDS958499",null,"A <MASTER SUBSTATION> is a <MANNED SUBSTATION> from which remotely controlled substations are controlled.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MANNED SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,"PERMANENTLY MANNED SUBSTATION",null,null,null,null,null,"rdl:RDS958409",null,"A <PERMANENTLY MANNED SUBSTATION> is a <MANNED SUBSTATION> that is continuously controlled by personnel who are stationed at the substation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"MIXED PHASE LAYOUT SUBSTATION",null,null,null,null,null,"rdl:RDS959174",null,"A <MIXED PHASE LAYOUT SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> and a layout in which the busbars are arranged as a separated phase layout but the bay circuits are arranged as associated phase layout",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"OPEN TYPE SUBSTATION",null,null,null,null,null,"rdl:RDS959264",null,"An <OPEN TYPE SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> in which the insulation to earth and between phase conductors is mainly provided by air at atmospheric pressure and in which some live parts are not enclosed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"OUTDOOR SUBSTATION",null,null,null,null,null,"rdl:RDS959399",null,"An <OUTDOOR SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> that is designed and installed to withstand external weather conditions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"OUTDOOR SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,"POLE-MOUNTED SUBSTATION",null,null,null,null,null,"rdl:RDS959534",null,"A <POLE-MOUNTED SUBSTATION> is an <OUTDOOR SUBSTATION> that is a distribution substation, mounted on one or more poles.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"SEPARATED PHASE LAYOUT SUBSTATION",null,null,null,null,null,"rdl:RDS959129",null,"A <SEPARATED PHASE LAYOUT SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> having a layout in which the conductors of different circuits, relating to the same phase, are located side by side",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"SINGLE BUSBAR SUBSTATION",null,null,null,null,null,"rdl:RDS958589",null,"A <SINGLE BUSBAR SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> in which the lines and transformers are connected to one busbar only",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SINGLE BUSBAR SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,"MESH SUBSTATION",null,null,null,null,null,"rdl:RDS958769",null,"A <MESH SUBSTATION> is a <SINGLE BUSBAR SUBSTATION> in which the busbar is formed as a closed loop with circuit breakers in series within the loop.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MESH SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOUR-SWITCH MESH SUBSTATION",null,null,null,null,null,"rdl:RDS958814",null,"A <FOUR-SWITCH MESH SUBSTATION> is a <MESH SUBSTATION> having a busbar of square configuration with a switch or a circuit-breaker within each side.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MESH SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOUR-SWITCH MESH SUBSTATION WITH MESH OPENING DISCONNECTORS",null,null,null,null,null,"rdl:RDS958949",null,"A <FOUR-SWITCH MESH SUBSTATION WITH MESH OPENING DISCONNECTORS> is a <MESH SUBSTATION>, the busbar of which comprises both circuit-breakers and disconnectors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MESH SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE-SWITCH MESH SUBSTATION WITH BYPASS",null,null,null,null,null,"rdl:RDS958859",null,"A <THREE-SWITCH MESH SUBSTATION WITH BYPASS> is a <MESH SUBSTATION> with usually two feeders and two transformers, the fourth circuit-breaker of the four-switch mesh substation is replaced by a bypass with one or two disconnectors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SINGLE BUSBAR SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,"RING SUBSTATION",null,null,null,null,null,"rdl:RDS958724",null,"A <RING SUBSTATION> is a <SINGLE BUSBAR SUBSTATION> in which the busbar is formed as a closed loop with only disconnectors in series within the loop.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"SWITCHING SUBSTATION",null,null,null,null,null,"rdl:RDS958004",null,"A <SWITCHING SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> that includes switchgear and usually busbars, but no power transformers",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"TAPPED SUBSTATION",null,null,null,null,null,"rdl:RDS1011689",null,"A <TAPPED SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> that is a single supply substation fed from a single branch line",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"TRACTION SUBSTATION",null,null,null,null,null,"rdl:RDS958184",null,"A <TRACTION SUBSTATION> is an <ARTEFACT> and a <SUBSTATION>, the main function of which is to supply a traction system",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"TRANSFORMER SUBSTATION",null,null,null,null,null,"rdl:RDS958049",null,"A <TRANSFORMER SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> containing power transformers interconnecting two or more networks of different voltages",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,"STEP-DOWN SUBSTATION",null,null,null,null,null,"rdl:RDS958139",null,"A <STEP-DOWN SUBSTATION> is a <TRANSFORMER SUBSTATION> in which the outgoing power from the transformers is at a lower voltage than the incoming power.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSFORMER SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,"STEP-UP SUBSTATION",null,null,null,null,null,"rdl:RDS958094",null,"A <STEP-UP SUBSTATION> is a <TRANSFORMER SUBSTATION> in which the outgoing power from the transformers is at a higher voltage than the incoming power.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"TRIPLE BUSBAR SUBSTATION",null,null,null,null,null,"rdl:RDS958679",null,"A <TRIPLE BUSBAR SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> in which the lines and transformers are connected via three busbars by means of selectors",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"UNDERGROUND SUBSTATION",null,null,null,null,null,"rdl:RDS959489",null,"A <UNDERGROUND SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> that is built to operate underground",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,"UNMANNED SUBSTATION",null,null,null,null,null,"rdl:RDS958364",null,"A <UNMANNED SUBSTATION> is an <ARTEFACT> and a <SUBSTATION> that is operated by personnel who are not stationed at the substation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"UNMANNED SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,"REMOTELY CONTROLLED SUBSTATION",null,null,null,null,null,"rdl:RDS958454",null,"A <REMOTELY CONTROLLED SUBSTATION> is a <UNMANNED SUBSTATION> that is controlled by means of telecontrol devices.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"REMOTELY CONTROLLED SUBSTATION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SATELLITE SUBSTATION",null,null,null,null,null,"rdl:RDS958544",null,"A <SATELLITE SUBSTATION> is a <REMOTELY CONTROLLED SUBSTATION>, controlled by a master substation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]