{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["RDL browser","Settings","about","Results1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"RDL browser","index":0,"n_rows":103,"n_cols":8,"rows_kept":103,"cut":false,"hidden":false,"merged":[[0,0,0,4]]}
["RDL2 browser to spreadsheet tool version 75",null,null,null,null,null,"Endpoint: http://data.15926.org/rdl/"]
["Contact: onno.paap@gmail.com",null,null,null,null,"Action","AC GENERATOR SPECIAL SUPPORT AND TEST EQUIPMENT CLASS","http://data.15926.org/rdl/RDS8924646"]
[null,null,null,null,null,"Action","ADJUSTABLE PIPE SUPPORT","http://data.15926.org/rdl/RDS1300656381"]
["Search:","SUPPORT",null,null,null,"Action","ANGLE SUPPORT","http://data.15926.org/rdl/RDS43164553132"]
[null,null,null,null,null,"Action","BRUSH HOLDER SUPPORTING STRUCTURE","http://data.15926.org/rdl/RDS7248380"]
[null,null,null,null,null,"Action","CAISSON SUPPORT","http://data.15926.org/rdl/RDS286514"]
[null,null,null,null,null,"Action","CLOSED BEAM SUPPORT FRAME","http://data.15926.org/rdl/RDS5677782"]
[null,null,null,null,null,"Action","CONDUCTOR SUPPORT","http://data.15926.org/rdl/RDS286334"]
[null,null,null,null,null,"Action","DAVIT SUPPORT CLIP","http://data.15926.org/rdl/RDS4316635265"]
[null,null,null,null,null,"Action","DEMISTER SUPPORT TRAY","http://data.15926.org/rdl/RDS13035285"]
[null,null,null,null,null,"Action","DIVIDED SUPPORT DISCONNECTOR","http://data.15926.org/rdl/RDS934604"]
[null,null,null,null,null,"Action","DIVIDED SUPPORT EARTHING SWITCH","http://data.15926.org/rdl/RDS934649"]
[null,"Note: first set coloring on in Settings",null,null,null,"Action","FIREPROOFING SUPPORT CLIP","http://data.15926.org/rdl/RDS4316636042"]
[null,"Coloring (containing this string will give this color)",null,null,null,"Action","FLEXIBLE SUPPORTED COMMON FRAME","http://data.15926.org/rdl/RDS13703336"]
[null,"ClassOfFunctionalObject",null,null,null,"Action","FLEXIBLE SUPPORTED ENGINE","http://data.15926.org/rdl/RDS13703274"]
[null,"ClassOfInanimatePhysicalObject ",null,null,null,"Action","FOOT SUPPORT","http://data.15926.org/rdl/RDS403701211"]
[null,null,null,null,null,"Action","GENERATOR SUPPORT AND TEST EQUIPMENT CLASS","http://data.15926.org/rdl/RDS8894395"]
[null,null,null,null,null,"Action","GENERATOR SUPPORT AND TEST EQUIPMENT LEVEL 1 CLASS","http://data.15926.org/rdl/RDS8894440"]
[null,null,null,null,null,"Action","GENERATOR SUPPORT AND TEST EQUIPMENT LEVEL 2 CLASS","http://data.15926.org/rdl/RDS8894485"]
[null,null,null,null,null,"Action","GENERATOR SUPPORT AND TEST EQUIPMENT LEVEL 3 CLASS","http://data.15926.org/rdl/RDS8894530"]
[null,null,null,null,null,"Action","GRID SUPPORT BEAM","http://data.15926.org/rdl/RDS43167560154"]
[null,null,null,null,null,"Action","IDENTIFICATION BY SUPPORT NUMBER","http://data.15926.org/rdl/RDS2229904"]
[null,null,null,null,null,"Action","IMPELLER SUPPORT - BETWEEN BEARINGS","http://data.15926.org/rdl/RDS2229060"]
[null,null,null,null,null,"Action","IMPELLER SUPPORT - OVERHUNG","http://data.15926.org/rdl/RDS2229059"]
[null,"Namespace replacer (definition containing this string replaces the namespace)",null,null,null,"Action","INSULATION SUPPORT BRACKET","http://data.15926.org/rdl/RDS444194"]
[null,"API","API:",null,null,"Action","INSULATION SUPPORT CLIP","http://data.15926.org/rdl/RDS4316756328"]
[null,"ASME","ASME:",null,null,"Action","INSULATION SUPPORT RING","http://data.15926.org/rdl/RDS437489"]
[null,"ASTM","ASTM:",null,null,"Action","INTEGRATED EQUIPMENT SUPPORT CLASS","http://data.15926.org/rdl/RDS5859174"]
[null,"DIN","DIN:",null,null,"Action","J-TUBE SUPPORT","http://data.15926.org/rdl/RDS286424"]
[null,"EN","EN:",null,null,"Action","J-TUBE SUPPORT FRAME","http://data.15926.org/rdl/RDS286469"]
[null,"ISO","ISO:",null,null,"Action","LADDER SUPPORT","http://data.15926.org/rdl/RDS4316790417"]
[null,"NORSOK","NOR:",null,null,"Action","LADDER SUPPORT CLIP","http://data.15926.org/rdl/RDS437624"]
[null,"NPD","NOR:",null,null,"Action","LOGISTICS SUPPORT CANDIDATE","http://data.15926.org/rdl/RDS8924151"]
[null,"NS","NOR:",null,null,"Action","MAINTENANCE SUPPORT PERFORMANCE","http://data.15926.org/rdl/RDS14647505"]
[null,"ROSEMOUNT","ROS:",null,null,"Action","MAINTENANCE SUPPORTING","http://data.15926.org/rdl/RDS10799569"]
[null,"SAE","SAE:",null,null,"Action","NATURAL PIPELINE SUPPORT MATERIAL","http://data.15926.org/rdl/RDS13116718"]
[null,"SIEMENS","SIE:",null,null,"Action","NON-TUBULAR HEAT EXCHANGER SUPPORT","http://data.15926.org/rdl/RDS14066865"]
[null,"SKOTSELV","SKOT:",null,null,"Action","OPEN BEAM SUPPORT FRAME","http://data.15926.org/rdl/RDS5677720"]
[null,"TWR","TWR:",null,null,"Action","PACKING SUPPORT","http://data.15926.org/rdl/RDS43168246105"]
[null,null,null,null,null,"Action","PACKING SUPPORT GRID","http://data.15926.org/rdl/RDS43168246119"]
[null,null,null,null,null,"Action","PERCENTAGE UNSUPPORTED LENGTH","http://data.15926.org/rdl/RDS13657865"]
[null,null,null,null,null,"Action","PIPE SUPPORT","http://data.15926.org/rdl/RDS286559"]
[null,null,null,null,null,"Action","PIPE SUPPORT CLIP","http://data.15926.org/rdl/RDS4316824851"]
[null,null,null,null,null,"Action","PIPE SUPPORT DETAIL","http://data.15926.org/rdl/RDS2221141"]
[null,null,null,null,null,"Action","PIPELINE SPAN SUPPORT","http://data.15926.org/rdl/RDS8775568"]
[null,null,null,null,null,"Action","PIPELINE SUPPORT MATERIAL","http://data.15926.org/rdl/RDS13116240"]
[null,null,null,null,null,"Action","PLATFORM SUPPORT","http://data.15926.org/rdl/RDS43168248148"]
[null,null,null,null,null,"Action","PLATFORM SUPPORT CLIP","http://data.15926.org/rdl/RDS43168248162"]
[null,null,null,null,null,"Action","PUSNES WINCH SPECIAL SUPPORT AND TEST EQUIPMENT CLASS","http://data.15926.org/rdl/RDS8619520"]
[null,null,null,null,null,"Action","REACTOR BED SUPPORT","http://data.15926.org/rdl/RDS43168514122"]
[null,null,null,null,null,"Action","RESILIANT ENGINE SUPPORT ARRANGEMENT","http://data.15926.org/rdl/RDS13659420"]
[null,null,null,null,null,"Action","RIGID ENGINE SUPPORT ARRANGEMENT","http://data.15926.org/rdl/RDS13659482"]
[null,null,null,null,null,"Action","RIGID SUPPORT ON ADJUSTABLE STEEL CHOCKS","http://data.15926.org/rdl/RDS13659606"]
[null,null,null,null,null,"Action","RIGID SUPPORT ON EPOXY RESIN CHOCKS","http://data.15926.org/rdl/RDS13659544"]
[null,null,null,null,null,"Action","RIGID SUPPORTED COMMON FRAME","http://data.15926.org/rdl/RDS13703212"]
[null,null,null,null,null,"Action","RISER SUPPORT","http://data.15926.org/rdl/RDS286379"]
[null,null,null,null,null,"Action","SADDLE SUPPORT","http://data.15926.org/rdl/RDS418904"]
[null,null,null,null,null,"Action","SERVICE SUPPORT PERFORMANCE","http://data.15926.org/rdl/RDS14645930"]
[null,null,null,null,null,"Action","SLIDING SUPPORT","http://data.15926.org/rdl/RDS431686359"]
[null,null,null,null,null,"Action","SPECIAL SUPPORT AND TEST EQUIPMENT CLASS","http://data.15926.org/rdl/RDS8614708"]
[null,null,null,null,null,"Action","SUBSEA FLOWLINE CONNECTOR SUPPORT FRAME","http://data.15926.org/rdl/RDS16680316"]
[null,null,null,null,null,"Action","SUBSEA MANIFOLD SUPPORT FRAME","http://data.15926.org/rdl/RDS16705128"]
[null,null,null,null,null,"Action","SUPPORT","http://data.15926.org/rdl/RDS6728598"]
[null,null,null,null,null,"Action","SUPPORT AND TEST EQUIPMENT CLASS","http://data.15926.org/rdl/RDS8614894"]
[null,null,null,null,null,"Action","SUPPORT AND TEST EQUIPMENT LEVEL 1 CLASS","http://data.15926.org/rdl/RDS8625957"]
[null,null,null,null,null,"Action","SUPPORT AND TEST EQUIPMENT LEVEL 2 CLASS","http://data.15926.org/rdl/RDS8626036"]
[null,null,null,null,null,"Action","SUPPORT AND TEST EQUIPMENT LEVEL 3 CLASS","http://data.15926.org/rdl/RDS8626115"]
[null,null,null,null,null,"Action","SUPPORT ASSEMBLY","http://data.15926.org/rdl/RDS13703020"]
[null,null,null,null,null,"Action","SUPPORT BRACKET","http://data.15926.org/rdl/RDS43168639266"]
[null,null,null,null,null,"Action","SUPPORT CLASS","http://data.15926.org/rdl/RDS6728218"]
[null,null,null,null,null,"Action","SUPPORT COLUMN","http://data.15926.org/rdl/RDS426413221"]
[null,null,null,null,null,"Action","SUPPORT EQUIPMENT CLASS","http://data.15926.org/rdl/RDS8614939"]
[null,null,null,null,null,"Action","SUPPORT GRID","http://data.15926.org/rdl/RDS43168639280"]
[null,null,null,null,null,"Action","SUPPORT ISOLATING","http://data.15926.org/rdl/RDS9699317"]
[null,null,null,null,null,"Action","SUPPORT LEG","http://data.15926.org/rdl/RDS280889"]
[null,null,null,null,null,"Action","SUPPORT LOAD","http://data.15926.org/rdl/RDS365264"]
[null,null,null,null,null,"Action","SUPPORT PAD","http://data.15926.org/rdl/RDS5859338"]
[null,null,null,null,null,"Action","SUPPORT PERIOD FOR ONSHORE RESOURCES","http://data.15926.org/rdl/RDS14663055"]
[null,null,null,null,null,"Action","SUPPORT RING","http://data.15926.org/rdl/RDS431686404"]
[null,null,null,null,null,"Action","SUPPORT SERVICE","http://data.15926.org/rdl/RDS9698957"]
[null,null,null,null,null,"Action","SUPPORT TRAY","http://data.15926.org/rdl/RDS13034700"]
[null,null,null,null,null,"Action","SUPPORT TYPE CURRENT TRANSFORMER","http://data.15926.org/rdl/RDS6455972"]
[null,null,null,null,null,"Action","SUPPORTABILITY 1","http://data.15926.org/rdl/RDS14645795"]
[null,null,null,null,null,"Action","SUPPORTABILITY 2","http://data.15926.org/rdl/RDS14645660"]
[null,null,null,null,null,"Action","SUPPORTABILITY 3","http://data.15926.org/rdl/RDS14645480"]
[null,null,null,null,null,"Action","SUPPORTABILITY 4","http://data.15926.org/rdl/RDS14645525"]
[null,null,null,null,null,"Action","SUPPORTABILITY 5","http://data.15926.org/rdl/RDS14645570"]
[null,null,null,null,null,"Action","SUPPORTABILITY 6","http://data.15926.org/rdl/RDS14645615"]
[null,null,null,null,null,"Action","SUPPORTED OBJECT","http://data.15926.org/rdl/RDS2227061"]
[null,null,null,null,null,"Action","SUPPORTING","http://data.15926.org/rdl/RDS9653147"]
[null,null,null,null,null,"Action","SUPPORTING OBJECT","http://data.15926.org/rdl/RDS2223575"]
[null,null,null,null,null,"Action","SUPPORTING STRUCTURE","http://data.15926.org/rdl/RDS13310380"]
[null,null,null,null,null,"Action","THRUSTER SUPPORT AND TEST EQUIPMENT LEVEL 1 CLASS","http://data.15926.org/rdl/RDS8877458"]
[null,null,null,null,null,"Action","THRUSTER SUPPORT AND TEST EQUIPMENT CLASS","http://data.15926.org/rdl/RDS8877413"]
[null,null,null,null,null,"Action","THRUSTER SUPPORT AND TEST EQUIPMENT LEVEL 2 CLASS","http://data.15926.org/rdl/RDS8877503"]
[null,null,null,null,null,"Action","THRUSTER SUPPORT AND TEST EQUIPMENT LEVEL 3 CLASS","http://data.15926.org/rdl/RDS8877548"]
[null,null,null,null,null,"Action","TOPSIDE SUPPORT STRUCTURE","http://data.15926.org/rdl/RDS284534"]
[null,null,null,null,null,"Action","TRAY SUPPORT BEAM","http://data.15926.org/rdl/RDS13034295"]
[null,null,null,null,null,"Action","TUBE BUNDLE SUPPORT PLATE","http://data.15926.org/rdl/RDS11159934"]
[null,null,null,null,null,"Action","WINCH SUPPORT AND TEST EQUIPMENT LEVEL 1 CLASS","http://data.15926.org/rdl/RDS8885918"]
[null,null,null,null,null,"Action","WINCH SUPPORT AND TEST EQUIPMENT CLASS","http://data.15926.org/rdl/RDS8885873"]
[null,null,null,null,null,"Action","WINCH SUPPORT AND TEST EQUIPMENT LEVEL 2 CLASS","http://data.15926.org/rdl/RDS8885963"]
[null,null,null,null,null,"Action","WINCH SUPPORT AND TEST EQUIPMENT LEVEL 3 CLASS","http://data.15926.org/rdl/RDS8886008"]

{"sheet":"Settings","index":1,"n_rows":87,"n_cols":8,"rows_kept":87,"cut":false,"hidden":true,"merged":[]}
["Setting name","Select name","OnKey","Value","Status","RDLType"]
["Endpoint","RDL2 (15926.org)",null,"http://data.15926.org/rdl/","Current",null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA RDL",null,"http://data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA Staging",null,"http://staging.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA SVRDL",null,"http://svrdl.community.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P4",null,"http://posccaesar.org/p4/sparql",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P12",null,"http://sti.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","Localhost",null,"http://localhost:8890/sparql/",null,null,null,"Note: end address always with a slash (/)"]
[]
["gBaseNamespace",null,"http://data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://staging.data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://svrdl.community.data.posccaesar.org/rdl/","http://svrdl.community.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://posccaesar.org/p4/sparql","http://posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://sti.data.posccaesar.org/rdl/","http://sti.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://localhost:8890/sparql/","http://data.15926.org/rdl/",null,"RDL2"]
["gKeepSettings",null,null,"T"]
["gShowDeprecated",null,null,"F"]
["gColoring",null,null,"T"]
["gNamespaceReplacing",null,null,"F"]
["gHyperlinkReplacing",null,null,"F"]
[]
["Endpoint","aisi",null,"http://data.15926.org/aisi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ansi",null,"http://data.15926.org/ansi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","api",null,"http://data.15926.org/api/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","all",null,"http://data.15926.org/all/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","asme",null,"http://data.15926.org/asme/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","astm",null,"http://data.15926.org/astm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","atex",null,"http://data.15926.org/atex/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","bs",null,"http://data.15926.org/bs/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","din",null,"http://data.15926.org/din/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dm",null,"http://data.15926.org/dm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dnv",null,"http://data.15926.org/dnv/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","edm",null,"http://data.15926.org/edm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","en",null,"http://data.15926.org/en/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","eu",null,"http://data.15926.org/eu/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iec",null,"http://data.15926.org/iec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ieee",null,"http://data.15926.org/ieee/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iso",null,"http://data.15926.org/iso/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","lci",null,"http://data.15926.org/lci/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","mss",null,"http://data.15926.org/mss/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nace",null,"http://data.15926.org/nace/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nec",null,"http://data.15926.org/nec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nema",null,"http://data.15926.org/nema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nfpa",null,"http://data.15926.org/nfpa/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nor",null,"http://data.15926.org/nor/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","rdl",null,"http://data.15926.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sae",null,"http://data.15926.org/sae/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sie",null,"http://data.15926.org/sie/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","tema",null,"http://data.15926.org/tema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","twr",null,"http://data.15926.org/twr/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","uns",null,"http://data.15926.org/uns/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","wits",null,"http://data.15926.org/wits/",null,null,null,"Note: end address always with a slash (/)"]
[]
[]
["gBaseNamespace",null,"http://data.15926.org/aisi/","http://data.15926.org/aisi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ansi/","http://data.15926.org/ansi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/api/","http://data.15926.org/api/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/asme/","http://data.15926.org/asme/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/all/","http://data.15926.org/all/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/astm/","http://data.15926.org/astm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/atex/","http://data.15926.org/atex/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/bs/","http://data.15926.org/bs/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/din/","http://data.15926.org/din/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dm/","http://data.15926.org/dm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dnv/","http://data.15926.org/dnv/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/edm/","http://data.15926.org/edm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/en/","http://data.15926.org/en/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/eu/","http://data.15926.org/eu/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iec/","http://data.15926.org/iec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ieee/","http://data.15926.org/ieee/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iso/","http://data.15926.org/iso/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/lci/","http://data.15926.org/lci/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/mss/","http://data.15926.org/mss/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nace/","http://data.15926.org/nace/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nec/","http://data.15926.org/nec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nema/","http://data.15926.org/nema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nfpa/","http://data.15926.org/nfpa/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nor/","http://data.15926.org/nor/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sae/","http://data.15926.org/sae/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sie/","http://data.15926.org/sie/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/tema/","http://data.15926.org/tema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/twr/","http://data.15926.org/twr/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/uns/","http://data.15926.org/uns/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/wits/","http://data.15926.org/wits/",null,"RDL2"]
["                                          "]

{"sheet":"about","index":2,"n_rows":176,"n_cols":3,"rows_kept":176,"cut":false,"hidden":false,"merged":[]}
["Version 75 changes","2018-10-05","Onno Paap"]
["missing superclasses - and orphans- filter no deprecated classes"]
[]
["Version 74 changes","2018-09-30","Onno Paap"]
["Repaired bug missing label"]
[]
["Version 73 changes","2018-05-16","Onno Paap"]
["Repaired bug Deprecated Superclass"]
[]
[]
[]
["Version 71 changes","2016-07-17","Onno Paap"]
["Aded report button for comparison of RDL2 with a subfolder called views filled with spreadsheets."]
[]
[]
["Version 69 changes","2016-06-16","Onno Paap"]
["Added button: \"errors in definitions\" that lists all classes that have more or less \"<\" brackets than the number of super class relationships + 1. Where the part after the word \"that \"  is ignored in the count of \"<\" brackets."]
[]
["Version 68 changes","2016-06-13","Onno Paap"]
["Updated endpoint of RDL2 sparql "]
[]
["Version 67 changes","2016-05-22","Onno Paap"]
["Added button list subclasses from superclass "]
[]
["Version 65 changes","2016-04-25","Onno Paap"]
["Added checkbox at action dialog \"supress double child occurances\" so that this built-in feature can be switched off"]
[]
["Version 64 changes","2016-04-20","Onno Paap"]
["Made search case-insensitive and added endpoint \"all\""]
[]
["Version 63 changes","2016-09-28","Onno Paap"]
["Made entity list working on P4 endpoint (they changed the database version which was not accepting som sparql setting)"]
["Version 62 changes","2016-09-28","Onno Paap"]
["Applied show deprecated to searched result list"]
[]
["Version 61 changes","2016-08-29","Onno Paap"]
["Added query from pcardl for ClassOfIndirectProperty"]
[]
["Version 60 changes","2016-08-19","Onno Paap"]
["Repaired failing entity reports"]
[]
["Version 59 changes","2016-08-19","Onno Paap"]
["Missing superclasses now queries whole federation of RDL2"]
[]
["Version 58 changes","2016-08-16","Onno Paap"]
["Repaired missing output for entities and doubles in RDL2 endpoints other than rdl"]
[]
["Version 57 changes","2016-08-13","Onno Paap"]
["Doubles report now skips classes that are deprecated"]
[]
["Version 56 changes","2016-07-22","Onno Paap"]
["Made rowheight suitable for longer definitions to example DESIGN BASIS"]
[]
["Version 55 changes","2016-07-19","Onno Paap"]
["Made rowheight suitable for longer definitions"]
[]
["Version 54 changes","2016-07-03","Onno Paap"]
["Entity Type field changed to 6 merged cells."]
[]
["Version 53 changes","2016-06-23","Onno Paap"]
["added lci namespace"]
[]
["Version 52 changes","2016-06-23","Onno Paap"]
["Added deprecated count to list entities"]
[]
["Version 51 changes","2016-06-19","Onno Paap"]
["Updated namespaces of staging RDL"]
[]
["Version 50 changes","2016-06-19","Onno Paap"]
["taxonomy view repaired missing entity type"]
[]
["Version 49 changes","2016-06-14","Onno Paap"]
["Room for 12 superclasses"]
[]
["Version 48 changes","2016-06-14","Onno Paap"]
["Repaired NOR:/RDS  bug"]
[]
["Version 47 changes","2016-06-14","Onno Paap"]
["Repaired endpoint bug"]
[]
["Version 46 changes","2016-06-13","Onno Paap"]
["Updated endpoints"]
[]
["Version 45 changes","2016-06-06","Onno Paap"]
["Completed Missing Superclasses report"]
[]
["Version 44 changes","2016-05-20","Onno Paap"]
["Added Clear Cache button (use on any database changes)"]
[]
["Version 43 changes","2016-05-19","Onno Paap"]
["Changed non-existing super classes to show as \"no label\""]
[]
["Version 42 changes","2016-05-02","Onno Paap"]
["bug fix"]
[]
["Version 41 changes","2016-05-02","Onno Paap"]
["Added setting to show/not show deprecated items. If shown, they are stricken through"]
[]
["Version 40 changes","2016-03-31","Onno Paap"]
["Added  in doubles: two classes having the same label."]
[]
["Version 39 changes","2016-03-21","Onno Paap"]
["Made the query more robust, after the server hass been returning a 404 occasionally"]
[]
["Version 38 changes","2016-03-03","Onno Paap"]
["Repaired bug entity type query on PCA endpoint"]
[]
["Version 37 changes","2016-01-29","Onno Paap"]
["Showing deprecated class in taxonomy with label in strikethrough."]
[]
["Version 36 changes","2016-01-13","Onno Paap"]
["Added the 17 endpoints of http://data.15926.org/rdl"]
[]
["Version 35 changes","2016-01-13","Onno Paap"]
["In taxonomy view, disregard all rdf:type that is not data model.  So only show rdf:type that is dm:"]
[]
["Version 34 changes","2016-01-13","Onno Paap"]
["Solved taxonomy levels regression bug"]
[]
["Version 33 changes","2016-01-11","Onno Paap"]
["Enhanced the doubled query. First 4 columns are about the triple, the rest is info."]
[]
["Repaired bug in entity type query."]
[]
["Version 30 changes","2016-01-03","Onno Paap"]
["Repaired entity type query for old PCA RDL. \nRepaired bug in entity type query where a class that has a superclass of the wanted type as well as  of another type became  the start point of a new taxonomy as well as part in the main taxonomy. (read that again)"]
[]
["Version 29 changes","2016-01-02","Onno Paap"]
["Filtered entity filtered taxonomy to only show the filtered entity not subClassOf of another entity"]
[]
["Version 27 changes","2016-01-01","Onno Paap"]
["few bugs repaired.  Changed entity search into presenting taxonomies. "]
[]
["Version 26 changes","2015-12-26","Onno Paap"]
["few bugs repaired. "]
[]
["Version 25 changes","2015-12-26","Onno Paap"]
["Added Part 12 and localhost endpoints"]
["Added button for selecting double labels and definitions. "]
["Version 24 changes","2015-12-14","Onno Paap"]
["Added button to list all distinct entity data types and their counts, and click to show."]
["Added a button to show all orphans that have a rdfs:label"]
["Version 23 changes"]
["Added endpoint posccaesar.org/p4/sparql"]
["Version 22 changes"]
["Added endpoint staging.data.posccaesar.org/rdl"]
[]
["Version 21 changes"]
["Repaired bug where namespace replace was based upon definition instead of class label"]
[]
["Version 20 changes"]
["Repaired bug where definition did not show up if hyperlink replace was on."]
[]
["Version 19 changes (skip version 16-18)"]
["Settings expanded with persist settings, namespace replacer and hyperlink replacer"]
["Added namespace replacer which will replace the RDL: namespace of the ID with the namespace given in the list on the front page."]
["Added hyperlink replacer which will find terms between single quotes and look them up in the RDL, then add a hyperlink in the text if found. Anchor tag <a></a> used not &hyperlink() so looks ugly."]
[]
["Version 15 changes"]
["Changed browser page Action buttons to hyperlinks because buttons are not equally spaced between Excel versions (Office 2007 versus Office 365)"]
["First row is empty. Move all up."]
["Make stop button for during query taxonomy query execution"]
[]
[]
["Version 14 changes"]
["Aligned buttons on browser page"]
["Made color notification work. Note: switch it on first in settings. Default is off"]
["Top align subclasses in taxonomy"]
["Subclasses made to hyperlink in taxonomy"]
["Subclasses made to increase column width in taxonomy"]
["Made browser search go when hitting enter in search field"]
[]
[]
[]
["todo"]
["Make setting for outputting to other result pages"]

{"sheet":"Results1","index":3,"n_rows":616,"n_cols":35,"rows_kept":616,"cut":false,"hidden":false,"merged":[[614,22,614,23],[614,16,614,21],[614,24,614,29],[614,30,614,33],[615,22,615,23],[615,16,615,21],[615,24,615,29],[615,30,615,33],[612,22,612,23],[612,16,612,21],[612,24,612,29],[612,30,612,33],[613,21,613,22],[613,15,613,20],[613,23,613,28],[613,29,613,32],[610,22,610,23],[610,16,610,21],[610,24,610,29],[610,30,610,33],[611,22,611,23],[611,16,611,21],[611,24,611,29],[611,30,611,33],[608,21,608,22],[608,15,608,20],[608,23,608,28],[608,29,608,32],[609,22,609,23],[609,16,609,21],[609,24,609,29],[609,30,609,33],[606,22,606,23],[606,16,606,21],[606,24,606,29],[606,30,606,33],[607,21,607,22],[607,15,607,20],[607,23,607,28],[607,29,607,32],[604,21,604,22],[604,15,604,20],[604,23,604,28],[604,29,604,32],[605,22,605,23],[605,16,605,21],[605,24,605,29],[605,30,605,33],[602,22,602,23],[602,16,602,21],[602,24,602,29],[602,30,602,33],[603,22,603,23],[603,16,603,21],[603,24,603,29],[603,30,603,33],[600,23,600,24],[600,17,600,22],[600,25,600,30],[600,31,600,34],[601,21,601,22],[601,15,601,20],[601,23,601,28],[601,29,601,32],[598,23,598,24],[598,17,598,22],[598,25,598,30],[598,31,598,34],[599,23,599,24],[599,17,599,22],[599,25,599,30],[599,31,599,34],[596,22,596,23],[596,16,596,21],[596,24,596,29],[596,30,596,33],[597,23,597,24],[597,17,597,22],[597,25,597,30],[597,31,597,34],[594,21,594,22],[594,15,594,20],[594,23,594,28],[594,29,594,32],[595,21,595,22],[595,15,595,20],[595,23,595,28],[595,29,595,32],[592,22,592,23],[592,16,592,21],[592,24,592,29],[592,30,592,33],[593,21,593,22],[593,15,593,20],[593,23,593,28],[593,29,593,32],[590,21,590,22],[590,15,590,20],[590,23,590,28],[590,29,590,32],[591,22,591,23],[591,16,591,21],[591,24,591,29],[591,30,591,33],[588,22,588,23],[588,16,588,21],[588,24,588,29],[588,30,588,33],[589,22,589,23],[589,16,589,21],[589,24,589,29],[589,30,589,33],[586,22,586,23],[586,16,586,21],[586,24,586,29],[586,30,586,33],[587,21,587,22],[587,15,587,20],[587,23,587,28],[587,29,587,32],[584,21,584,22],[584,15,584,20],[584,23,584,28],[584,29,584,32],[585,22,585,23],[585,16,585,21],[585,24,585,29],[585,30,585,33],[582,21,582,22],[582,15,582,20],[582,23,582,28],[582,29,582,32],[583,22,583,23],[583,16,583,21],[583,24,583,29],[583,30,583,33],[580,24,580,25],[580,18,580,23],[580,26,580,31],[580,32,580,35],[581,24,581,25],[581,18,581,23],[581,26,581,31],[581,32,581,35],[578,23,578,24],[578,17,578,22],[578,25,578,30],[578,31,578,34],[579,24,579,25],[579,18,579,23],[579,26,579,31],[579,32,579,35],[576,24,576,25],[576,18,576,23],[576,26,576,31],[576,32,576,35],[577,24,577,25],[577,18,577,23],[577,26,577,31],[577,32,577,35],[574,22,574,23],[574,16,574,21],[574,24,574,29],[574,30,574,33],[575,23,575,24],[575,17,575,22],[575,25,575,30],[575,31,575,34],[572,22,572,23],[572,16,572,21],[572,24,572,29],[572,30,572,33],[573,21,573,22],[573,15,573,20],[573,23,573,28],[573,29,573,32],[570,23,570,24],[570,17,570,22],[570,25,570,30],[570,31,570,34],[571,23,571,24],[571,17,571,22],[571,25,571,30],[571,31,571,34],[568,23,568,24],[568,17,568,22],[568,25,568,30],[568,31,568,34],[569,23,569,24],[569,17,569,22],[569,25,569,30],[569,31,569,34],[566,24,566,25],[566,18,566,23],[566,26,566,31],[566,32,566,35],[567,22,567,23],[567,16,567,21],[567,24,567,29],[567,30,567,33],[564,24,564,25],[564,18,564,23],[564,26,564,31],[564,32,564,35],[565,24,565,25],[565,18,565,23],[565,26,565,31],[565,32,565,35],[562,25,562,26],[562,19,562,24],[562,27,562,32],[562,33,562,36],[563,25,563,26],[563,19,563,24],[563,27,563,32],[563,33,563,36],[560,26,560,27],[560,20,560,25],[560,28,560,33],[560,34,560,37],[561,24,561,25],[561,18,561,23],[561,26,561,31],[561,32,561,35],[558,24,558,25],[558,18,558,23],[558,26,558,31],[558,32,558,35],[559,25,559,26],[559,19,559,24],[559,27,559,32],[559,33,559,36],[556,23,556,24],[556,17,556,22],[556,25,556,30],[556,31,556,34],[557,23,557,24],[557,17,557,22],[557,25,557,30],[557,31,557,34],[554,23,554,24],[554,17,554,22],[554,25,554,30],[554,31,554,34],[555,23,555,24],[555,17,555,22],[555,25,555,30],[555,31,555,34],[552,21,552,22],[552,15,552,20],[552,23,552,28],[552,29,552,32],[553,22,553,23],[553,16,553,21],[553,24,553,29],[553,30,553,33],[550,21,550,22],[550,15,550,20],[550,23,550,28],[550,29,550,32],[551,21,551,22],[551,15,551,20],[551,23,551,28],[551,29,551,32],[548,22,548,23],[548,16,548,21],[548,24,548,29],[548,30,548,33],[549,23,549,24],[549,17,549,22],[549,25,549,30],[549,31,549,34],[546,22,546,23],[546,16,546,21],[546,24,546,29],[546,30,546,33],[547,22,547,23],[547,16,547,21],[547,24,547,29],[547,30,547,33],[544,21,544,22],[544,15,544,20],[544,23,544,28],[544,29,544,32],[545,22,545,23],[545,16,545,21],[545,24,545,29],[545,30,545,33],[542,21,542,22],[542,15,542,20],[542,23,542,28],[542,29,542,32],[543,22,543,23],[543,16,543,21],[543,24,543,29],[543,30,543,33],[540,21,540,22],[540,15,540,20],[540,23,540,28],[540,29,540,32],[541,21,541,22],[541,15,541,20],[541,23,541,28],[541,29,541,32],[538,21,538,22],[538,15,538,20],[538,23,538,28],[538,29,538,32],[539,22,539,23],[539,16,539,21],[539,24,539,29],[539,30,539,33],[536,21,536,22],[536,15,536,20],[536,23,536,28],[536,29,536,32],[537,21,537,22],[537,15,537,20],[537,23,537,28],[537,29,537,32],[534,21,534,22],[534,15,534,20],[534,23,534,28],[534,29,534,32],[535,22,535,23],[535,16,535,21],[535,24,535,29],[535,30,535,33],[532,22,532,23],[532,16,532,21],[532,24,532,29],[532,30,532,33],[533,22,533,23],[533,16,533,21],[533,24,533,29],[533,30,533,33],[530,21,530,22],[530,15,530,20],[530,23,530,28],[530,29,530,32],[531,21,531,22],[531,15,531,20],[531,23,531,28],[531,29,531,32],[528,21,528,22],[528,15,528,20],[528,23,528,28],[528,29,528,32],[529,21,529,22],[529,15,529,20],[529,23,529,28],[529,29,529,32],[526,21,526,22],[526,15,526,20],[526,23,526,28],[526,29,526,32],[527,21,527,22],[527,15,527,20],[527,23,527,28],[527,29,527,32],[524,21,524,22],[524,15,524,20],[524,23,524,28],[524,29,524,32],[525,21,525,22],[525,15,525,20],[525,23,525,28],[525,29,525,32],[522,22,522,23],[522,16,522,21],[522,24,522,29],[522,30,522,33],[523,22,523,23],[523,16,523,21],[523,24,523,29],[523,30,523,33],[520,21,520,22],[520,15,520,20],[520,23,520,28],[520,29,520,32],[521,22,521,23],[521,16,521,21],[521,24,521,29],[521,30,521,33],[518,21,518,22],[518,15,518,20],[518,23,518,28],[518,29,518,32],[519,22,519,23],[519,16,519,21],[519,24,519,29],[519,30,519,33],[516,21,516,22],[516,15,516,20],[516,23,516,28],[516,29,516,32],[517,22,517,23],[517,16,517,21],[517,24,517,29],[517,30,517,33],[514,22,514,23],[514,16,514,21],[514,24,514,29],[514,30,514,33],[515,22,515,23],[515,16,515,21],[515,24,515,29],[515,30,515,33],[512,21,512,22],[512,15,512,20],[512,23,512,28],[512,29,512,32],[513,21,513,22],[513,15,513,20],[513,23,513,28],[513,29,513,32],[510,21,510,22],[510,15,510,20],[510,23,510,28],[510,29,510,32],[511,22,511,23],[511,16,511,21],[511,24,511,29],[511,30,511,33],[508,22,508,23],[508,16,508,21],[508,24,508,29],[508,30,508,33],[509,21,509,22],[509,15,509,20],[509,23,509,28],[509,29,509,32],[506,23,506,24],[506,17,506,22],[506,25,506,30],[506,31,506,34],[507,23,507,24],[507,17,507,22],[507,25,507,30],[507,31,507,34],[504,23,504,24],[504,17,504,22],[504,25,504,30],[504,31,504,34],[505,23,505,24],[505,17,505,22],[505,25,505,30],[505,31,505,34],[502,24,502,25],[502,18,502,23],[502,26,502,31],[502,32,502,35],[503,23,503,24],[503,17,503,22],[503,25,503,30],[503,31,503,34],[500,24,500,25],[500,18,500,23],[500,26,500,31],[500,32,500,35],[501,24,501,25],[501,18,501,23],[501,26,501,31],[501,32,501,35],[498,24,498,25],[498,18,498,23],[498,26,498,31],[498,32,498,35],[499,25,499,26],[499,19,499,24],[499,27,499,32],[499,33,499,36],[496,24,496,25],[496,18,496,23],[496,26,496,31],[496,32,496,35],[497,24,497,25],[497,18,497,23],[497,26,497,31],[497,32,497,35],[494,23,494,24],[494,17,494,22],[494,25,494,30],[494,31,494,34],[495,23,495,24],[495,17,495,22],[495,25,495,30],[495,31,495,34],[492,21,492,22],[492,15,492,20],[492,23,492,28],[492,29,492,32],[493,22,493,23],[493,16,493,21],[493,24,493,29],[493,30,493,33],[490,21,490,22],[490,15,490,20],[490,23,490,28],[490,29,490,32],[491,21,491,22],[491,15,491,20],[491,23,491,28],[491,29,491,32],[488,21,488,22],[488,15,488,20],[488,23,488,28],[488,29,488,32],[489,21,489,22],[489,15,489,20],[489,23,489,28],[489,29,489,32],[486,22,486,23],[486,16,486,21],[486,24,486,29],[486,30,486,33],[487,22,487,23],[487,16,487,21],[487,24,487,29],[487,30,487,33],[484,23,484,24],[484,17,484,22],[484,25,484,30],[484,31,484,34],[485,22,485,23],[485,16,485,21],[485,24,485,29],[485,30,485,33],[482,23,482,24],[482,17,482,22],[482,25,482,30],[482,31,482,34],[483,23,483,24],[483,17,483,22],[483,25,483,30],[483,31,483,34],[480,21,480,22],[480,15,480,20],[480,23,480,28],[480,29,480,32],[481,22,481,23],[481,16,481,21],[481,24,481,29],[481,30,481,33],[478,23,478,24],[478,17,478,22],[478,25,478,30],[478,31,478,34],[479,21,479,22],[479,15,479,20],[479,23,479,28],[479,29,479,32],[476,22,476,23],[476,16,476,21],[476,24,476,29],[476,30,476,33],[477,22,477,23],[477,16,477,21],[477,24,477,29],[477,30,477,33],[474,21,474,22],[474,15,474,20],[474,23,474,28],[474,29,474,32],[475,22,475,23],[475,16,475,21],[475,24,475,29],[475,30,475,33],[472,22,472,23],[472,16,472,21],[472,24,472,29],[472,30,472,33],[473,21,473,22],[473,15,473,20],[473,23,473,28],[473,29,473,32],[470,21,470,22],[470,15,470,20],[470,23,470,28],[470,29,470,32],[471,21,471,22],[471,15,471,20],[471,23,471,28],[471,29,471,32],[468,21,468,22],[468,15,468,20],[468,23,468,28],[468,29,468,32],[469,21,469,22],[469,15,469,20],[469,23,469,28],[469,29,469,32],[466,21,466,22],[466,15,466,20],[466,23,466,28],[466,29,466,32],[467,21,467,22],[467,15,467,20],[467,23,467,28],[467,29,467,32],[464,23,464,24],[464,17,464,22],[464,25,464,30],[464,31,464,34],[465,22,465,23],[465,16,465,21],[465,24,465,29],[465,30,465,33],[462,23,462,24],[462,17,462,22],[462,25,462,30],[462,31,462,34],[463,23,463,24],[463,17,463,22],[463,25,463,30],[463,31,463,34],[460,25,460,26],[460,19,460,24],[460,27,460,32],[460,33,460,36],[461,23,461,24],[461,17,461,22],[461,25,461,30],[461,31,461,34],[458,24,458,25],[458,18,458,23],[458,26,458,31],[458,32,458,35],[459,24,459,25],[459,18,459,23],[459,26,459,31],[459,32,459,35],[456,24,456,25],[456,18,456,23],[456,26,456,31],[456,32,456,35],[457,23,457,24],[457,17,457,22],[457,25,457,30],[457,31,457,34],[454,23,454,24],[454,17,454,22],[454,25,454,30],[454,31,454,34],[455,24,455,25],[455,18,455,23],[455,26,455,31],[455,32,455,35],[452,23,452,24],[452,17,452,22],[452,25,452,30],[452,31,452,34],[453,23,453,24],[453,17,453,22],[453,25,453,30],[453,31,453,34],[450,23,450,24],[450,17,450,22],[450,25,450,30],[450,31,450,34],[451,23,451,24],[451,17,451,22],[451,25,451,30],[451,31,451,34],[448,23,448,24],[448,17,448,22],[448,25,448,30],[448,31,448,34],[449,23,449,24],[449,17,449,22],[449,25,449,30],[449,31,449,34],[446,25,446,26],[446,19,446,24],[446,27,446,32],[446,33,446,36],[447,25,447,26],[447,19,447,24],[447,27,447,32],[447,33,447,36],[444,23,444,24],[444,17,444,22],[444,25,444,30],[444,31,444,34],[445,24,445,25],[445,18,445,23],[445,26,445,31],[445,32,445,35],[442,23,442,24],[442,17,442,22],[442,25,442,30],[442,31,442,34],[443,24,443,25],[443,18,443,23],[443,26,443,31],[443,32,443,35],[440,22,440,23],[440,16,440,21],[440,24,440,29],[440,30,440,33],[441,22,441,23],[441,16,441,21],[441,24,441,29],[441,30,441,33],[438,24,438,25],[438,18,438,23],[438,26,438,31],[438,32,438,35],[439,22,439,23],[439,16,439,21],[439,24,439,29],[439,30,439,33],[436,23,436,24],[436,17,436,22],[436,25,436,30],[436,31,436,34],[437,23,437,24],[437,17,437,22],[437,25,437,30],[437,31,437,34],[434,25,434,26],[434,19,434,24],[434,27,434,32],[434,33,434,36],[435,25,435,26],[435,19,435,24],[435,27,435,32],[435,33,435,36],[432,24,432,25],[432,18,432,23],[432,26,432,31],[432,32,432,35],[433,24,433,25],[433,18,433,23],[433,26,433,31],[433,32,433,35],[430,22,430,23],[430,16,430,21],[430,24,430,29],[430,30,430,33],[431,23,431,24],[431,17,431,22],[431,25,431,30],[431,31,431,34],[428,22,428,23],[428,16,428,21],[428,24,428,29],[428,30,428,33],[429,22,429,23],[429,16,429,21],[429,24,429,29],[429,30,429,33],[426,23,426,24],[426,17,426,22],[426,25,426,30],[426,31,426,34],[427,23,427,24],[427,17,427,22],[427,25,427,30],[427,31,427,34],[424,23,424,24],[424,17,424,22],[424,25,424,30],[424,31,424,34],[425,23,425,24],[425,17,425,22],[425,25,425,30],[425,31,425,34],[422,21,422,22],[422,15,422,20],[422,23,422,28],[422,29,422,32],[423,22,423,23],[423,16,423,21],[423,24,423,29],[423,30,423,33],[420,24,420,25],[420,18,420,23],[420,26,420,31],[420,32,420,35],[421,24,421,25],[421,18,421,23],[421,26,421,31],[421,32,421,35],[418,24,418,25],[418,18,418,23],[418,26,418,31],[418,32,418,35],[419,24,419,25],[419,18,419,23],[419,26,419,31],[419,32,419,35],[416,24,416,25],[416,18,416,23],[416,26,416,31],[416,32,416,35],[417,24,417,25],[417,18,417,23],[417,26,417,31],[417,32,417,35],[414,24,414,25],[414,18,414,23],[414,26,414,31],[414,32,414,35],[415,24,415,25],[415,18,415,23],[415,26,415,31],[415,32,415,35],[412,23,412,24],[412,17,412,22],[412,25,412,30],[412,31,412,34],[413,24,413,25],[413,18,413,23],[413,26,413,31],[413,32,413,35],[410,24,410,25],[410,18,410,23],[410,26,410,31],[410,32,410,35],[411,24,411,25],[411,18,411,23],[411,26,411,31],[411,32,411,35],[408,24,408,25],[408,18,408,23],[408,26,408,31],[408,32,408,35],[409,23,409,24],[409,17,409,22],[409,25,409,30],[409,31,409,34],[406,24,406,25],[406,18,406,23],[406,26,406,31],[406,32,406,35],[407,24,407,25],[407,18,407,23],[407,26,407,31],[407,32,407,35],[404,22,404,23],[404,16,404,21],[404,24,404,29],[404,30,404,33],[405,23,405,24],[405,17,405,22],[405,25,405,30],[405,31,405,34],[402,22,402,23],[402,16,402,21],[402,24,402,29],[402,30,402,33],[403,22,403,23],[403,16,403,21],[403,24,403,29],[403,30,403,33],[400,22,400,23],[400,16,400,21],[400,24,400,29],[400,30,400,33],[401,21,401,22],[401,15,401,20],[401,23,401,28],[401,29,401,32],[398,22,398,23],[398,16,398,21],[398,24,398,29],[398,30,398,33],[399,22,399,23],[399,16,399,21],[399,24,399,29],[399,30,399,33],[396,21,396,22],[396,15,396,20],[396,23,396,28],[396,29,396,32],[397,22,397,23],[397,16,397,21],[397,24,397,29],[397,30,397,33],[394,21,394,22],[394,15,394,20],[394,23,394,28],[394,29,394,32],[395,21,395,22],[395,15,395,20],[395,23,395,28],[395,29,395,32],[392,22,392,23],[392,16,392,21],[392,24,392,29],[392,30,392,33],[393,21,393,22],[393,15,393,20],[393,23,393,28],[393,29,393,32],[390,22,390,23],[390,16,390,21],[390,24,390,29],[390,30,390,33],[391,22,391,23],[391,16,391,21],[391,24,391,29],[391,30,391,33],[388,24,388,25],[388,18,388,23],[388,26,388,31],[388,32,388,35],[389,22,389,23],[389,16,389,21],[389,24,389,29],[389,30,389,33],[386,25,386,26],[386,19,386,24],[386,27,386,32],[386,33,386,36],[387,23,387,24],[387,17,387,22],[387,25,387,30],[387,31,387,34],[384,25,384,26],[384,19,384,24],[384,27,384,32],[384,33,384,36],[385,25,385,26],[385,19,385,24],[385,27,385,32],[385,33,385,36],[382,24,382,25],[382,18,382,23],[382,26,382,31],[382,32,382,35],[383,24,383,25],[383,18,383,23],[383,26,383,31],[383,32,383,35],[380,25,380,26],[380,19,380,24],[380,27,380,32],[380,33,380,36],[381,23,381,24],[381,17,381,22],[381,25,381,30],[381,31,381,34],[378,23,378,24],[378,17,378,22],[378,25,378,30],[378,31,378,34],[379,24,379,25],[379,18,379,23],[379,26,379,31],[379,32,379,35],[376,23,376,24],[376,17,376,22],[376,25,376,30],[376,31,376,34],[377,23,377,24],[377,17,377,22],[377,25,377,30],[377,31,377,34],[374,24,374,25],[374,18,374,23],[374,26,374,31],[374,32,374,35],[375,24,375,25],[375,18,375,23],[375,26,375,31],[375,32,375,35],[372,23,372,24],[372,17,372,22],[372,25,372,30],[372,31,372,34],[373,24,373,25],[373,18,373,23],[373,26,373,31],[373,32,373,35],[370,23,370,24],[370,17,370,22],[370,25,370,30],[370,31,370,34],[371,24,371,25],[371,18,371,23],[371,26,371,31],[371,32,371,35],[368,23,368,24],[368,17,368,22],[368,25,368,30],[368,31,368,34],[369,23,369,24],[369,17,369,22],[369,25,369,30],[369,31,369,34],[366,24,366,25],[366,18,366,23],[366,26,366,31],[366,32,366,35],[367,23,367,24],[367,17,367,22],[367,25,367,30],[367,31,367,34]],"merged_total":2464,"flags":["merged_cut"]}
[null,null,"FunctionalObject",null,null,null,null,null,null,null,null,null,null,null,"SUPPORT",null,null,null,null,null,"rdl:RDS6728598",null,"A <SUPPORT> is a <FunctionalObject> that has a capability of <SUPPORTING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"ADAPTER SEAT",null,null,null,null,null,"rdl:RDS393982491",null,"An <ADAPTER SEAT> is an <ARTEFACT> and a <SUPPORT> for the bottom part of the column in which the cryogenic pump is housed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"ANCHOR CHAIR",null,null,null,null,null,"rdl:RDS6911960",null,"An <ANCHOR CHAIR> is an <ARTEFACT> and a <SUPPORT> intended to fix a skirt to a foundation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"ANGLE SUPPORT",null,null,null,null,null,"rdl:RDS43164553132",null,"An <ANGLE SUPPORT> is an <ARTEFACT> and a <SUPPORT> consisting of a web and at least one flange",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RING","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"BASE RING",null,null,null,null,null,"rdl:RDS6760380",null,"A <BASE RING> is a <RING> and a <SUPPORT> that is a circular base used to support something",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BASE RING",null,null,null,null,null,null,null,null,null,null,null,null,null,"ANCHOR BOLT RING",null,null,null,null,null,"rdl:RDS7035110",null,"An <ANCHOR BOLT RING> is a <BASE RING> used in fixing a <SKIRT> to a foundation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"BEAM",null,null,null,null,null,"rdl:RDS5754776",null,"A <BEAM> is an <ARTEFACT> and a <SUPPORT> that is a large and straight piece of normally timber or iron forming one of the main structural member of a building or supporting structure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BEAM",null,null,null,null,null,null,null,null,null,null,null,null,null,"BOOM",null,null,null,null,null,"rdl:RDS13705222",null,"A <BOOM> is a <BEAM> extending out from a fixed foundation or structure for lifting or hoisting, a movable arm with a pulley and cable at the outer end for exerting tension on an object.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BEAM",null,null,null,null,null,null,null,null,null,null,null,null,null,"GRID SUPPORT BEAM",null,null,null,null,null,"rdl:RDS43167560154",null,"A <GRID SUPPORT BEAM> is a <BEAM> intended to support a grid.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BEAM",null,null,null,null,null,null,null,null,null,null,null,null,null,"LIFTING BEAM",null,null,null,null,null,"rdl:RDS5778110",null,"A <LIFTING BEAM> is a <BEAM> that is structurally able to handle the load throughout the beam spread.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BEAM",null,null,null,null,null,null,null,null,null,null,null,null,null,"SPREADER BEAM",null,null,null,null,null,"rdl:RDS1325712361",null,"An <SPREADER BEAM> is a <BEAM> for spacing the chains or cables hanging from the boom of a crane.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BEAM",null,null,null,null,null,null,null,null,null,null,null,null,null,"TRAY SUPPORT BEAM",null,null,null,null,null,"rdl:RDS13034295",null,"A <TRAY SUPPORT BEAM> is a <BEAM> intended to limit the deflection of a tray.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUPPORT",null,null,null,null,null,null,null,null,null,null,null,null,"BEARING",null,null,null,null,null,"rdl:RDS286874",null,"A <BEARING> is a <SUPPORT> intended to support and locate a moving or static element",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"ANTI FRICTION BEARING",null,null,null,null,null,"rdl:RDS394025741",null,"An <ANTI FRICTION BEARING> is an<ARTEFACT> and a <BEARING> that uses rolling bearing elements",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"BEARING DRIVEN END",null,null,null,null,null,"rdl:RDS395043291",null,"A <BEARING DRIVEN END> is an<ARTEFACT> and a <BEARING> that is located at the driven end of an equipment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"BEARING NON-DRIVEN END",null,null,null,null,null,"rdl:RDS395061051",null,"A <BEARING NON-DRIVEN END> is an<ARTEFACT> and a <BEARING> that is located at the non driven end of an equipment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"CAMSHAFT BEARING",null,null,null,null,null,"rdl:RDS13662536",null,"A <CAMSHAFT BEARING> is an<ARTEFACT> and a <BEARING> that is supporting the camshaft",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"CRANK JOURNAL BEARING",null,null,null,null,null,"rdl:RDS13662102",null,"A <CRANK JOURNAL BEARING> is an<ARTEFACT> and a <BEARING> that is the main centric bearing supporting the crank journal of a crankshaft",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"CRANKPIN BEARING",null,null,null,null,null,"rdl:RDS16768674",null,"A <CRANKPIN BEARING> is an<ARTEFACT> and a <BEARING> that is the connection rod bearing located at the crankshaft side",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"CRANKSHAFT MAIN BEARING",null,null,null,null,null,"rdl:RDS16768404",null,"A <CRANKSHAFT MAIN BEARING> is an<ARTEFACT> and a <BEARING> that is used inside a crankcase to support the crankshaft",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"CROSSHEAD BEARING",null,null,null,null,null,"rdl:RDS13660531",null,"A <CROSSHEAD BEARING> is an<ARTEFACT> and a <BEARING> that constitute a part of the connection between the crosshead connecting rod and the crosshead pin in a crosshead engine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"DRIVE END BEARING",null,null,null,null,null,"rdl:RDS7510720",null,"A <DRIVE END BEARING> is an <ARTEFACT> and a <BEARING> for a drive end of a driver, i.e. for support of the end of the shaft where torque is transferred",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DRIVE END BEARING","RADIAL/THRUST BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,"DRIVE END RADIAL/THRUST BEARING",null,null,null,null,null,"rdl:RDS6649991",null,"A <DRIVE END RADIAL/THRUST BEARING> is a <DRIVE END BEARING> and a <RADIAL/THRUST BEARING> that is located at a drive end.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"DRIVEN END BEARING",null,null,null,null,null,"rdl:RDS13649830",null,"A <DRIVEN END BEARING> is an<ARTEFACT> and a <BEARING> that can be installed at driven end",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"INBOARD BEARING",null,null,null,null,null,"rdl:RDS407092411",null,"An <INBOARD BEARING> is an<ARTEFACT> and a <BEARING> that is located closest to the center of the equipment. Typically the process side in case of pumps and compressors",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"INTERMEDIATE BEARING",null,null,null,null,null,"rdl:RDS407886471",null,"An <INTERMEDIATE BEARING> is an<ARTEFACT> and a <BEARING> that is located between the inboard and outboard bearing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"LUBRICATED BEARING",null,null,null,null,null,"rdl:RDS889334",null,"A <LUBRICATED BEARING> is an<ARTEFACT> and a <BEARING> where the presence of a lubricant is required",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LUBRICATED BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GREASE LUBRICATED BEARING",null,null,null,null,null,"rdl:RDS6690177",null,"A <GREASE LUBRICATED BEARING> is a <LUBRICATED BEARING> that is provided with grease.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GREASE LUBRICATED BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIFETIME PRELUBRICATED BEARING",null,null,null,null,null,"rdl:RDS6690239",null,"A <LIFETIME PRELUBRICATED BEARING> is a <GREASE LUBRICATED BEARING> that contains shields or seals at both sides by which the grease doesn&#39;t need to be refilled at all during the lifetime of the bearing.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LUBRICATED BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MUD LUBRICATED BEARING",null,null,null,null,null,"rdl:RDS16809440",null,"A <MUD LUBRICATED BEARING> is a <LUBRICATED BEARING> used in drill bits which is lubricated using drilling mud.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LUBRICATED BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OIL LUBRICATED BEARING",null,null,null,null,null,"rdl:RDS6690301",null,"An <OIL LUBRICATED BEARING> is a <LUBRICATED BEARING> intended to be lubricated with oil.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"MAGNETIC BEARING",null,null,null,null,null,"rdl:RDS434834",null,"A <MAGNETIC BEARING> is an <ARTEFACT> and a <BEARING> that is an electromagnetic device which maintains the relative position of a rotating assembly (rotor) with respect to the stationary part",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"NON LUBRICATED BEARING",null,null,null,null,null,"rdl:RDS889379",null,"A <NON LUBRICATED BEARING> is an <ARTEFACT> and a <BEARING> where no lubrication is in place",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"NON-DRIVE END BEARING",null,null,null,null,null,"rdl:RDS7510782",null,"A <NON-DRIVE END BEARING> is an <ARTEFACT> and a <BEARING> for a non-drive end of a driver, i.e. for support of the end of the shaft where torque is not transferred",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"NON-DRIVE END BEARING","RADIAL/THRUST BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-DRIVE END RADIAL/THRUST BEARING",null,null,null,null,null,"rdl:RDS6650036",null,"A <NON-DRIVE END RADIAL/THRUST BEARING> is a <NON-DRIVE END BEARING> and a <RADIAL/THRUST BEARING> that is located at a non-drive end.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"NON-DRIVEN END BEARING",null,null,null,null,null,"rdl:RDS13649605",null,"A <NON-DRIVEN END BEARING> is an<ARTEFACT> and a <BEARING> that can be installed at non-driven end",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"OUTBOARD BEARING",null,null,null,null,null,"rdl:RDS412223971",null,"An <OUTBOARD BEARING> is an<ARTEFACT> and a <BEARING> that is located closest to the shaft-end",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"PLAIN BEARING",null,null,null,null,null,"rdl:RDS14199376",null,"A <PLAIN BEARING> is an<ARTEFACT> and a <BEARING> that is plain",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLAIN BEARING","RADIAL BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL PLAIN BEARING",null,null,null,null,null,"rdl:RDS14199691",null,"A <RADIAL PLAIN BEARING> is a <PLAIN BEARING> and a <RADIAL BEARING>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLAIN BEARING","RADIAL/THRUST BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL/THRUST PLAIN BEARING",null,null,null,null,null,"rdl:RDS14199556",null,"A <RADIAL/THRUST PLAIN BEARING> is a <PLAIN BEARING> and a <RADIAL/THRUST BEARING>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLAIN BEARING","THRUST BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,"THRUST PLAIN BEARING",null,null,null,null,null,"rdl:RDS14199331",null,"A <THRUST PLAIN BEARING> is a <PLAIN BEARING> and a <THRUST BEARING>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL BEARING",null,null,null,null,null,"rdl:RDS6810280",null,"A <RADIAL BEARING> is an<ARTEFACT> and a <BEARING> intended to support a shaft or rotor in radial direction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RADIAL BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PILLOW BLOCK BEARING",null,null,null,null,null,"rdl:RDS13068050",null,"A <PILLOW BLOCK BEARING> is a <RADIAL BEARING> intended for guidance.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL BEARING","RADIAL BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL BALL BEARING",null,null,null,null,null,"rdl:RDS14199646",null,"A <RADIAL BALL BEARING> is a <RADIAL BEARING> that is also a ball bearing.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RADIAL BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL BEARING DRIVEN END",null,null,null,null,null,"rdl:RDS414145561",null,"A <RADIAL BEARING DRIVEN END> is a <RADIAL BEARING> that is located at the driven end of a shaft.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RADIAL BEARING","ROLLER BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL ROLLER BEARING",null,null,null,null,null,"rdl:RDS14199736",null,"A <RADIAL ROLLER BEARING> is a <RADIAL BEARING> and a <ROLLER BEARING> that is capable of providing both axial and radial support simultanously.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RADIAL BEARING","THRUST BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL/THRUST BEARING",null,null,null,null,null,"rdl:RDS14199511",null,"A <RADIAL/THRUST BEARING> is a <RADIAL BEARING> and a <THRUST BEARING> that is capable of providing both axial and radial support simultanously.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL BEARING","RADIAL/THRUST BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL/THRUST BALL BEARING",null,null,null,null,null,"rdl:RDS14199466",null,"A <RADIAL/THRUST BALL BEARING> is a <BALL BEARING> and a <RADIAL/THRUST BEARING>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RADIAL/THRUST BALL BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Y-BEARING UNIT",null,null,null,null,null,"rdl:RDS889244",null,"A <Y-BEARING UNIT> is a <RADIAL/THRUST BALL BEARING> that is a simple economic ball bearing unit consisting of a deep groove ball bearing and a bearing housing made of cast iron or pressed steel having a sphered bore enabling the unit to allow moderate errors of alignment.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RADIAL/THRUST BEARING","ROLLER BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL/THRUST ROLLER BEARING",null,null,null,null,null,"rdl:RDS14199601",null,"A <RADIAL/THRUST ROLLER BEARING> is a <ROLLER BEARING> and a <RADIAL/THRUST BEARING>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RADIAL BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STEADY BEARING",null,null,null,null,null,"rdl:RDS424682321",null,"A <STEADY BEARING> is a <RADIAL BEARING> that is intended to be used for relatively long shafts for mixers to reduce the drive bearing reactions and gearing deflections.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"ROLLING ELEMENT BEARING",null,null,null,null,null,"rdl:RDS445499",null,"A <ROLLING ELEMENT BEARING> is an<ARTEFACT> and a <BEARING> that utilizes rolling balls, cylinders and other rolling elements between tracks",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLING ELEMENT BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BALL BEARING",null,null,null,null,null,"rdl:RDS445544",null,"A <BALL BEARING> is a <ROLLING ELEMENT BEARING> in which the parts are separated by a ring of small freely rotating metal balls which reduce friction.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANGULAR CONTACT BALL BEARING",null,null,null,null,null,"rdl:RDS889199",null,"An <ANGULAR CONTACT BALL BEARING> is a <BALL BEARING> with raceways in the inner and outer rings which are displaced with respect to each other in the direction of the bearing axis.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANGULAR CONTACT BALL BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE ROW ANGULAR CONTACT BEARING",null,null,null,null,null,"rdl:RDS6690658",null,"A <DOUBLE ROW ANGULAR CONTACT BEARING> is an <ANGULAR CONTACT BALL BEARING> provided with two rows bearing balls and destined to accommodate for thrust loads in both directions.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ANGULAR CONTACT BALL BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE ROW ANGULAR CONTACT BEARING",null,null,null,null,null,"rdl:RDS6690596",null,"A <SINGLE ROW ANGULAR CONTACT BEARING> is an <ANGULAR CONTACT BALL BEARING> provided with a single row bearing balls and destined to accommodate for thrust loads in one direction.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DEEP GROOVE BALL BEARING",null,null,null,null,null,"rdl:RDS889109",null,"A <DEEP GROOVE BALL BEARING> is a <BALL BEARING> that uses balls running in one or two deep uninterrupted raceways in the inner and outer ring.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SELF-ALIGNING BALL BEARING",null,null,null,null,null,"rdl:RDS889154",null,"A <SELF-ALIGNING BALL BEARING> is a <BALL BEARING> that has two rows of balls with two separate raceways in the inner ring and a common sphered raceway in the outer ring, permitting angular misalignment of the shaft relative to the housing.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL BEARING","THRUST BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THRUST BALL BEARING",null,null,null,null,null,"rdl:RDS885014",null,"A <THRUST BALL BEARING> is a <BALL BEARING> and a <THRUST BEARING> that contains a ball and cage thrust assembly between a shaft washer and a housing washer with raceway grooves. This type of bearings is suitable for axial loads in one direction and may not be subject to any radial load.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLING ELEMENT BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE ROW BEARING",null,null,null,null,null,"rdl:RDS6690425",null,"A <DOUBLE ROW BEARING> is a <ROLLING ELEMENT BEARING> that contains two rows of rolling elements.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLING ELEMENT BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROLLER BEARING",null,null,null,null,null,"rdl:RDS445589",null,"A <ROLLER BEARING> is a <ROLLING ELEMENT BEARING> utilizing cylindrical, conical or spherical rollers.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLER BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CYLINDRICAL ROLLER BEARING",null,null,null,null,null,"rdl:RDS888884",null,"A <CYLINDRICAL ROLLER BEARING> is a <ROLLER BEARING> that contains one or two rows of rollers, alternatively one row with crossed rollers between the outer and inner ring.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CYLINDRICAL ROLLER BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CROSSED CYLINDRICAL ROLLER BEARING",null,null,null,null,null,"rdl:RDS1009619",null,"A <CROSSED CYLINDRICAL ROLLER BEARING> is a <CYLINDRICAL ROLLER BEARING> that has raceways in both the inner and outer ring which are inclined at an angle of 45 degrees to the bearing axis and where cylindrical rollers are arranged alternately at 90 degrees to each other. The rollers have a slightly larger diameter than their length.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLER BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CYLINDRICAL ROLLER THRUST BEARING",null,null,null,null,null,"rdl:RDS888974",null,"A <CYLINDRICAL ROLLER THRUST BEARING> is a <ROLLER BEARING> that contains a cylindrical roller and cage thrust assembly located between a shaft washer and a housing washer to accommodate for axial loads in one direction.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLER BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NEEDLE ROLLER BEARING",null,null,null,null,null,"rdl:RDS445724",null,"A <NEEDLE ROLLER BEARING> is a <ROLLER BEARING> that contains cylindrical rollers which have a small diameter and are long relative to their diameter.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLER BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NEEDLE ROLLER THRUST BEARING",null,null,null,null,null,"rdl:RDS889064",null,"A <NEEDLE ROLLER THRUST BEARING> is a <ROLLER BEARING> that consists of a needle roller and thrust cage located between a shaft washer and a housing washer to accommodate axial loads in one direction.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLER BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPHERICAL ROLLER BEARING",null,null,null,null,null,"rdl:RDS888929",null,"An <SPHERICAL ROLLER BEARING> is a <ROLLER BEARING> provided with two rows of rollers with a common sphered raceway in the outer ring. The two inner ring raceways are inclined at an angle to the bearing axis. This bearing is of the self-aligning type and can also accommodate for limited axial loads in both directions.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLER BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPHERICAL ROLLER THRUST BEARING",null,null,null,null,null,"rdl:RDS889019",null,"An <SPHERICAL ROLLER THRUST BEARING> is a <ROLLER BEARING> utilizing spherical rollers between an outer and inner ring where the raceways are positioned at an angle to the bearing axis. These types of bearings can handle both axial and radial loads as well as misalignment to the shaft axis.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLER BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TAPER ROLLER BEARING",null,null,null,null,null,"rdl:RDS445634",null,"A <TAPER ROLLER BEARING> is a <ROLLER BEARING> that has tapered inner and outer ring raceways between which tapered rollers are arranged to accommodate for both radial and axial loads in both directions.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLER BEARING","THRUST BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THRUST ROLLER BEARING",null,null,null,null,null,"rdl:RDS14199421",null,"A <THRUST ROLLER BEARING> is a <ROLLER BEARING> and a <THRUST BEARING>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THRUST ROLLER BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CENTRIFUGAL COMPRESSOR THRUST BEARING",null,null,null,null,null,"rdl:RDS14310998",null,"A <CENTRIFUGAL COMPRESSOR THRUST BEARING> is a <THRUST ROLLER BEARING> that is designed to take up axial load on a centrifugal compressor.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLING ELEMENT BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE ROW BEARING",null,null,null,null,null,"rdl:RDS6690363",null,"A <SINGLE ROW BEARING> is a <ROLLING ELEMENT BEARING> provided with one row of rolling elements.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLING ELEMENT BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLEWING BEARING",null,null,null,null,null,"rdl:RDS486224",null,"An <SLEWING BEARING> is a <ROLLING ELEMENT BEARING> that contains one or more rows of rolling elements.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROLLING ELEMENT BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRACK RUNNER BEARING",null,null,null,null,null,"rdl:RDS889289",null,"A <TRACK RUNNER BEARING> is a <ROLLING ELEMENT BEARING> that contains a deep groove ball bearing or a roller bearing with a thick-walled outer ring.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"SLIDING TYPE BEARING",null,null,null,null,null,"rdl:RDS445679",null,"A <SLIDING TYPE BEARING> is an<ARTEFACT> and a <BEARING> that contains bearing bushings, pads or shoes to support and locate revolving, reciprocating and sliding elements",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SLIDING TYPE BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLEEVE BEARING",null,null,null,null,null,"rdl:RDS6690517",null,"An <SLEEVE BEARING> is a <SLIDING TYPE BEARING> that is a bushing type bearing intended to carry primarily radial load and possibly axial load in addition.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SLEEVE BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONNECTING ROD PIN BUSHING",null,null,null,null,null,"rdl:RDS16769169",null,"A <CONNECTING ROD PIN BUSHING> is an <SLEEVE BEARING> which is located inside the connecting rod at the crosshead side and moves over the crosshead pin.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SLIDING TYPE BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPHERICAL PLAIN BEARING",null,null,null,null,null,"rdl:RDS889424",null,"An <SPHERICAL PLAIN BEARING> is a <SLIDING TYPE BEARING> consisting of a cylindrical outer ring with a spherical supported inner ring. The bearing is suitable for alignment movements or oscillating, tilting and slewing movements.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SLIDING TYPE BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TILTING PAD BEARING",null,null,null,null,null,"rdl:RDS417734",null,"A <TILTING PAD BEARING> is a <SLIDING TYPE BEARING> that contains tilted bearing pads to allow oil wedges to form between the pads and the rotor.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TILTING PAD BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TILTING PAD COMBINED RADIAL/THRUST BEARING",null,null,null,null,null,"rdl:RDS1143314",null,"A <TILTING PAD COMBINED RADIAL/THRUST BEARING> is a <TILTING PAD BEARING> intended to provide both radial and axial support to a rotating component.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TILTING PAD BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TILTING PAD RADIAL BEARING",null,null,null,null,null,"rdl:RDS1143269",null,"A <TILTING PAD RADIAL BEARING> is a <TILTING PAD BEARING> intended to provide radial support to a rotating component.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THRUST BEARING","TILTING PAD BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TILTING PAD THRUST BEARING",null,null,null,null,null,"rdl:RDS1143224",null,"A <TILTING PAD THRUST BEARING> is a <TILTING PAD BEARING> and a <THRUST BEARING> where the bearing pads tilt to allow oil wedges to form between the pad and thrust disc.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BEARING",null,null,null,null,null,null,null,null,null,null,null,null,"THRUST BEARING",null,null,null,null,null,"rdl:RDS6810235",null,"A <THRUST BEARING> is an<ARTEFACT> and a <BEARING> used to accommodate for any residual axial load within any rotating equipment design under all possible operating conditions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THRUST BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CRANKSHAFT AXIAL BEARING",null,null,null,null,null,"rdl:RDS16768314",null,"A <CRANKSHAFT AXIAL BEARING> is a <THRUST BEARING> that is the crankshaft location bearing at the driven side carrying both axial and radial loads.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THRUST BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INTERNAL THRUST BEARING",null,null,null,null,null,"rdl:RDS13310740",null,"An <INTERNAL THRUST BEARING> is a <THRUST BEARING> built into an engine to take the propeller thrust forces.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THRUST BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THRUST BEARING DRIVEN END",null,null,null,null,null,"rdl:RDS426478811",null,"A <THRUST BEARING DRIVEN END> is a <THRUST BEARING> that is located at the driven end of a shaft.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THRUST BEARING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THRUST BEARING NON-DRIVEN END",null,null,null,null,null,"rdl:RDS426483651",null,"A <THRUST BEARING NON-DRIVEN END> is a <THRUST BEARING> that is located at the non-driven end of a shaft.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"BEARING ASSEMBLY",null,null,null,null,null,"rdl:RDS12956450",null,"A <BEARING ASSEMBLY> is an <ARTEFACT> and a <SUPPORT> that consists of one or more bearings and associated components",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BEARING ASSEMBLY",null,null,null,null,null,null,null,null,null,null,null,null,null,"DEEP GROOVE BALL BEARING ASSEMBLY",null,null,null,null,null,"rdl:RDS12956354",null,"A <DEEP GROOVE BALL BEARING ASSEMBLY> is a <BEARING ASSEMBLY> consisting of two or more deep groove ball bearings.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BEARING ASSEMBLY",null,null,null,null,null,null,null,null,null,null,null,null,null,"HANGER BEARING",null,null,null,null,null,"rdl:RDS406152751",null,"A <HANGER BEARING> is a <BEARING ASSEMBLY> that consists of a bearing mounted in a hanger.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"BEARING CARTRIDGE",null,null,null,null,null,"rdl:RDS16771059",null,"A <BEARING CARTRIDGE> is an <ARTEFACT> and a <SUPPORT> that is a preassembly of the bearing bracket, bearings, and associated parts for sliding onto a shaft and bolted to a static pump part",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"BRACKET",null,null,null,null,null,"rdl:RDS329219",null,"A <BRACKET> is an <ARTEFACT> and a <SUPPORT> that is an overhanging member that projects from a structure (as a wall) and is usually designed to support a vertical load or to strengthen an angle",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,"BEARING BRACKET",null,null,null,null,null,"rdl:RDS6234259",null,"A <BEARING BRACKET> is a <BRACKET> intended to support a bearing assembly.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BEARING BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL BEARING BRACKET",null,null,null,null,null,"rdl:RDS414143841",null,"A <RADIAL BEARING BRACKET> is a <BEARING BRACKET> that is a support for a radial bearing assembly.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BEARING BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THRUST BEARING BRACKET",null,null,null,null,null,"rdl:RDS426477051",null,"A <THRUST BEARING BRACKET> is a <BEARING BRACKET> that is a support for a thrust bearing assembly.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,"CANTILEVER",null,null,null,null,null,"rdl:RDS290519",null,"A <CANTILEVER> is a <BRACKET> whose length is many times its breadth and more than twice its depth, which projects from the face of e.g. a wall.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,"GEAR SHIFTER UNIT BRACKET",null,null,null,null,null,"rdl:RDS16307015",null,"A <GEAR SHIFTER UNIT BRACKET> is a <BRACKET> that holds the gear shifter unit together and clamp it to the handle bar.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT MOUNTING BRACKET",null,null,null,null,null,"rdl:RDS743624",null,"An <INSTRUMENT MOUNTING BRACKET> is a <BRACKET> that is intended for supporting an instrument.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT MOUNTING BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PANEL MOUNTING BRACKET",null,null,null,null,null,"rdl:RDS743714",null,"A <PANEL MOUNTING BRACKET> is an <INSTRUMENT MOUNTING BRACKET> that is a support structure for mounting an instrument on a panel or wall.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT MOUNTING BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PIPE MOUNTING BRACKET",null,null,null,null,null,"rdl:RDS743669",null,"A <PIPE MOUNTING BRACKET> is an <INSTRUMENT MOUNTING BRACKET> that is a support structure for mounting an instrument on a pipe.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSULATION SUPPORT BRACKET",null,null,null,null,null,"rdl:RDS444194",null,"An <INSULATION SUPPORT BRACKET> is a <BRACKET> intended to support insulation when mounted on e.g. tanks, vessels and walls.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,"LADDER BRACKET",null,null,null,null,null,"rdl:RDS444239",null,"A <LADDER BRACKET> is a <BRACKET> intended for laddersupport.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BRACKET","CLIP",null,null,null,null,null,null,null,null,null,null,null,null,"LADDER SUPPORT CLIP",null,null,null,null,null,"rdl:RDS437624",null,"A <LADDER SUPPORT CLIP> is a <BRACKET> and a <CLIP> intended to connect a ladder or a ladder support",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,"LANTERN BRACKET",null,null,null,null,null,"rdl:RDS408880101",null,"A <LANTERN BRACKET> is a <BRACKET> that is intended to mount pump and motor together.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,"LUMINAIRE BRACKET",null,null,null,null,null,"rdl:RDS484559",null,"A <LUMINAIRE BRACKET> is a <BRACKET> intended to hold luminaires.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,"NON TUBULAR HEAT EXCHANGER BRACKET",null,null,null,null,null,"rdl:RDS14118685",null,"A <NON TUBULAR HEAT EXCHANGER BRACKET> is a <BRACKET> on a non tubular heat exchanger.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BRACKET",null,null,null,null,null,null,null,null,null,null,null,null,null,"SUPPORT BRACKET",null,null,null,null,null,"rdl:RDS43168639266",null,"A <SUPPORT BRACKET> is a <BRACKET> intended to facilitate the support and fixation of an item to a foundation or structure.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"BRIDGE LANDING",null,null,null,null,null,"rdl:RDS290564",null,"A <BRIDGE LANDING> is an <ARTEFACT> and a <SUPPORT> which is intended to support an end of a bridge",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"BRUSH HOLDER ROCKER YOKE",null,null,null,null,null,"rdl:RDS7248515",null,"A <BRUSH HOLDER ROCKER YOKE> is an <ARTEFACT> and a <SUPPORT> that is a structure on which the brush-holder rocker is mounted when the rocker is not supported by the frame or pedestal of the machine itself",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"BRUSH HOLDER SUPPORTING STRUCTURE",null,null,null,null,null,"rdl:RDS7248380",null,"A <BRUSH HOLDER SUPPORTING STRUCTURE> is an <ARTEFACT> and a <SUPPORT> that is a structure on which the brush-holders are mounted and are fixed relative to each other",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BRUSH HOLDER SUPPORTING STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BRUSH HOLDER ROCKER",null,null,null,null,null,"rdl:RDS7248425",null,"A <BRUSH HOLDER ROCKER> is a <BRUSH HOLDER SUPPORTING STRUCTURE> that is arranged in such a manner that the whole structure may be moved circumferentially.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"CABLE BRACKET",null,null,null,null,null,"rdl:RDS6570425",null,"A <CABLE BRACKET> is an <ARTEFACT> and a <SUPPORT> that is horizontally fixed at one end only, spaced at intervals, and on which cables rest",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"CABLE GLAND",null,null,null,null,null,"rdl:RDS429029",null,"A <CABLE GLAND> is an <ARTEFACT> and a <SUPPORT>> that is a device designed to attach and secure the end of a cable to the equipment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER SECTION",null,null,null,null,null,"rdl:RDS6232222",null,"A <CABLE LADDER SECTION> is a <ARTEFACT> and a <SUPPORT> that is a part of a <CABLE LADDER SYSTEM>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND",null,null,null,null,null,"rdl:RDS484604",null,"A <CABLE LADDER BEND> is a <CABLE LADDER SECTION> that is a bend",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER FIXED BEND",null,null,null,null,null,"rdl:RDS879704",null,"A <CABLE LADDER FIXED BEND> is a <CABLE LADDER BEND> that is fixed.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER FIXED BEND",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 30 DEG",null,null,null,null,null,"rdl:RDS484064",null,"A <CABLE LADDER BEND 30 DEG> is a <CABLE LADDER FIXED BEND> where the angle between the vectors normal to the end planes is 30 degrees.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 30 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 30 DEG 150 MM",null,null,null,null,null,"rdl:RDS907739",null,"A <CABLE LADDER BEND 30 DEG 150 MM> is a <CABLE LADDER BEND 30 DEG> where the angle between the vectors normal to the end planes is 30 degrees and with a width of 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 30 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 30 DEG 300 MM",null,null,null,null,null,"rdl:RDS907784",null,"A <CABLE LADDER BEND 30 DEG 300 MM> is a <CABLE LADDER BEND 30 DEG> where the angle between the vectors normal to the end planes is 30 degrees and with a width of 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 30 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 30 DEG 450 MM",null,null,null,null,null,"rdl:RDS907829",null,"A <CABLE LADDER BEND 30 DEG 450 MM> is a <CABLE LADDER BEND 30 DEG> where the angle between the vectors normal to the end planes is 30 degrees and with a width of 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 30 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 30 DEG 600 MM",null,null,null,null,null,"rdl:RDS907874",null,"A <CABLE LADDER BEND 30 DEG 600 MM> is a <CABLE LADDER BEND 30 DEG> where the angle between the vectors normal to the end planes is 30 degrees and with a width of 600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 30 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 30 DEG 750 MM",null,null,null,null,null,"rdl:RDS907919",null,"A <CABLE LADDER BEND 30 DEG 750 MM> is a <CABLE LADDER BEND 30 DEG> where the angle between the vectors normal to the end planes is 30 degrees and with a width of 750 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 30 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 30 DEG 900 MM",null,null,null,null,null,"rdl:RDS907964",null,"A <CABLE LADDER BEND 30 DEG 900 MM> is a <CABLE LADDER BEND 30 DEG> where the angle between the vectors normal to the end planes is 30 degrees and with a width of 900 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER FIXED BEND",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 45 DEG",null,null,null,null,null,"rdl:RDS484019",null,"A <CABLE LADDER BEND 45 DEG> is a <CABLE LADDER FIXED BEND> where the angle between the vectors normal to the end planes is 45 degrees.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 45 DEG 150 MM",null,null,null,null,null,"rdl:RDS908009",null,"A <CABLE LADDER BEND 45 DEG 150 MM> is a <CABLE LADDER BEND 45 DEG> where the angle between the vectors normal to the end planes is 45 degrees and with a width of 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 45 DEG 300 MM",null,null,null,null,null,"rdl:RDS908054",null,"A <CABLE LADDER BEND 45 DEG 300 MM> is a <CABLE LADDER BEND 45 DEG> where the angle between the vectors normal to the end planes is 45 degrees and with a width of 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 45 DEG 450 MM",null,null,null,null,null,"rdl:RDS908099",null,"A <CABLE LADDER BEND 45 DEG 450 MM> is a <CABLE LADDER BEND 45 DEG> where the angle between the vectors normal to the end planes is 45 degrees and with a width of 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 45 DEG 600 MM",null,null,null,null,null,"rdl:RDS908144",null,"A <CABLE LADDER BEND 45 DEG 600 MM> is a <CABLE LADDER BEND 45 DEG> where the angle between the vectors normal to the end planes is 45 degrees and with a width of 600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 45 DEG 750 MM",null,null,null,null,null,"rdl:RDS908189",null,"A <CABLE LADDER BEND 45 DEG 750 MM> is a <CABLE LADDER BEND 45 DEG> where the angle between the vectors normal to the end planes is 45 degrees and with a width of 750 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 45 DEG 900 MM",null,null,null,null,null,"rdl:RDS908234",null,"A <CABLE LADDER BEND 45 DEG 900 MM> is a <CABLE LADDER BEND 45 DEG> where the angle between the vectors normal to the end planes is 45 degrees and with a width of 900 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER FIXED BEND",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 60 DEG",null,null,null,null,null,"rdl:RDS484109",null,"A <CABLE LADDER BEND 60 DEG> is a <CABLE LADDER FIXED BEND> where the angle between the vectors normal to the end planes is 60 degrees.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 60 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 60 DEG 150 MM",null,null,null,null,null,"rdl:RDS908279",null,"A <CABLE LADDER BEND 60 DEG 150 MM> is a <CABLE LADDER BEND 60 DEG> where the angle between the vectors normal to the end planes is 60 degrees and with a width of 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 60 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 60 DEG 300 MM",null,null,null,null,null,"rdl:RDS908324",null,"A <CABLE LADDER BEND 60 DEG 300 MM> is a <CABLE LADDER BEND 60 DEG> where the angle between the vectors normal to the end planes is 60 degrees and with a width of 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 60 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 60 DEG 450 MM",null,null,null,null,null,"rdl:RDS908369",null,"A <CABLE LADDER BEND 60 DEG 450 MM> is a <CABLE LADDER BEND 60 DEG> where the angle between the vectors normal to the end planes is 60 degrees and with a width of 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 60 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 60 DEG 600 MM",null,null,null,null,null,"rdl:RDS908414",null,"A <CABLE LADDER BEND 60 DEG 600 MM> is a <CABLE LADDER BEND 60 DEG> where the angle between the vectors normal to the end planes is 60 degrees and with a width of 600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 60 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 60 DEG 750 MM",null,null,null,null,null,"rdl:RDS908459",null,"A <CABLE LADDER BEND 60 DEG 750 MM> is a <CABLE LADDER BEND 60 DEG> where the angle between the vectors normal to the end planes is 60 degrees and with a width of 750 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 60 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 60 DEG 900 MM",null,null,null,null,null,"rdl:RDS908504",null,"A <CABLE LADDER BEND 60 DEG 900 MM> is a <CABLE LADDER BEND 60 DEG> where the angle between the vectors normal to the end planes is 60 degrees and with a width of 900 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER FIXED BEND",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 90 DEG",null,null,null,null,null,"rdl:RDS483974",null,"A <CABLE LADDER BEND 90 DEG> is a <CABLE LADDER FIXED BEND> where the angle between the vectors normal to the end planes is 90 degrees.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 90 DEG 150 MM",null,null,null,null,null,"rdl:RDS908549",null,"A <CABLE LADDER BEND 90 DEG 150 MM> is a <CABLE LADDER BEND 90 DEG> where the angle between the vectors normal to the end planes is 90 degrees and with a width of 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 90 DEG 300 MM",null,null,null,null,null,"rdl:RDS908594",null,"A <CABLE LADDER BEND 90 DEG 300 MM> is a <CABLE LADDER BEND 90 DEG> where the angle between the vectors normal to the end planes is 90 degrees and with a width of 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 90 DEG 450 MM",null,null,null,null,null,"rdl:RDS908639",null,"A <CABLE LADDER BEND 90 DEG 450 MM> is a <CABLE LADDER BEND 90 DEG> where the angle between the vectors normal to the end planes is 90 degrees and with a width of 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 90 DEG 600 MM",null,null,null,null,null,"rdl:RDS908684",null,"A <CABLE LADDER BEND 90 DEG 600 MM> is a <CABLE LADDER BEND 90 DEG> where the angle between the vectors normal to the end planes is 90 degrees and with a width of 600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 90 DEG 750 MM",null,null,null,null,null,"rdl:RDS908729",null,"A <CABLE LADDER BEND 90 DEG 750 MM> is a <CABLE LADDER BEND 90 DEG> where the angle between the vectors normal to the end planes is 90 degrees and with a width of 750 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER BEND 90 DEG 900 MM",null,null,null,null,null,"rdl:RDS908774",null,"A <CABLE LADDER BEND 90 DEG 900 MM> is a <CABLE LADDER BEND 90 DEG> where the angle between the vectors normal to the end planes is 90 degrees and with a width of 900 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER BEND",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER FLEXI-BEND",null,null,null,null,null,"rdl:RDS879749",null,"A <CABLE LADDER FLEXI-BEND> is a <CABLE LADDER BEND> that is adjustable.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER CROSS",null,null,null,null,null,"rdl:RDS484334",null,"A <CABLE LADDER CROSS> is a <CABLE LADDER SECTION> that is a cross",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER CROSS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER CROSS 150 MM",null,null,null,null,null,"rdl:RDS908819",null,"A <CABLE LADDER CROSS 150 MM> is a <CABLE LADDER CROSS> that is a cross-piece for cable ladders with the width 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER CROSS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER CROSS 300 MM",null,null,null,null,null,"rdl:RDS908864",null,"A <CABLE LADDER CROSS 300 MM> is a <CABLE LADDER CROSS> that is a cross-piece for cable ladders with the width 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER CROSS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER CROSS 450 MM",null,null,null,null,null,"rdl:RDS908909",null,"A <CABLE LADDER CROSS 450 MM> is a <CABLE LADDER CROSS> that is a cross-piece for cable ladders with the width 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER CROSS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER CROSS 600 MM",null,null,null,null,null,"rdl:RDS908954",null,"A <CABLE LADDER CROSS 600 MM> is a <CABLE LADDER CROSS> that is a cross-piece for cable ladders with the width 600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER CROSS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER CROSS 750 MM",null,null,null,null,null,"rdl:RDS908999",null,"A <CABLE LADDER CROSS 750 MM> is a <CABLE LADDER CROSS> that is a cross-piece for cable ladders with the width 750 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER CROSS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER CROSS 900 MM",null,null,null,null,null,"rdl:RDS909044",null,"A <CABLE LADDER CROSS 900 MM> is a <CABLE LADDER CROSS> that is a cross-piece for cable ladders with the width 900 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER DIVIDER",null,null,null,null,null,"rdl:RDS484424",null,"A <CABLE LADDER DIVIDER> is a <CABLE LADDER SECTION> intended to divide between different cable systems and duties",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER SECTION","JOINT",null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER JOINT",null,null,null,null,null,"rdl:RDS483884",null,"A <CABLE LADDER JOINT> is a <CABLE LADDER SECTION> and a <JOINT> intended to join other cable ladder sections",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER JOINT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER FIXED JOINT",null,null,null,null,null,"rdl:RDS866024",null,"A <CABLE LADDER FIXED JOINT> is a <CABLE LADDER JOINT> that is a fixed device for splicing cable ladder parts.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER JOINT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER FLEXIBLE JOINT",null,null,null,null,null,"rdl:RDS483929",null,"A <CABLE LADDER FLEXIBLE JOINT> is a <CABLE LADDER JOINT> that is flexible.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER SECTION","REDUCER",null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER",null,null,null,null,null,"rdl:RDS484379",null,"A <CABLE LADDER REDUCER> is a <CABLE LADDER SECTION> and a <REDUCER> intended to join cable ladders having different width",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,"rdl:RDS900449",null,"A <CABLE LADDER REDUCER LEFT> is a <CABLE LADDER REDUCER> that is reduced on the left hand side.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 300 MM-150 MM",null,null,null,null,null,"rdl:RDS901124",null,"A <CABLE LADDER REDUCER LEFT 300 MM-150 MM> is a <CABLE LADDER REDUCER LEFT> that is reduced on the left hand side from 300 mm to 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 450 MM-150 MM",null,null,null,null,null,"rdl:RDS901079",null,"A <CABLE LADDER REDUCER LEFT 450 MM-150 MM> is a <CABLE LADDER REDUCER LEFT> that is reduced on the left hand side from 450 mm to 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 450 MM-300 MM",null,null,null,null,null,"rdl:RDS901034",null,"A <CABLE LADDER REDUCER LEFT 450 MM-300 MM> is a <CABLE LADDER REDUCER LEFT> that is reduced on the left hand side from 450 mm to 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 600 MM-150 MM",null,null,null,null,null,"rdl:RDS900989",null,"A <CABLE LADDER REDUCER LEFT 600 MM-150 MM> is a <CABLE LADDER REDUCER LEFT> that is reduced on the left hand side from 600 mm to 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 600 MM-300 MM",null,null,null,null,null,"rdl:RDS900944",null,"A <CABLE LADDER REDUCER LEFT 600 MM-300 MM> is a <CABLE LADDER REDUCER LEFT> that is reduced on the left hand side from 600 mm to 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 600 MM-450 MM",null,null,null,null,null,"rdl:RDS900899",null,"A <CABLE LADDER REDUCER LEFT 600 MM-450 MM> is a <CABLE LADDER REDUCER LEFT> that is reduced on the left hand side from 600 mm to 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 750 MM-300 MM",null,null,null,null,null,"rdl:RDS900854",null,"A <CABLE LADDER REDUCER LEFT 750 MM-300 MM> is a <CABLE LADDER REDUCER LEFT> that is reduced on the left hand side from 750 mm to 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 750 MM-450 MM",null,null,null,null,null,"rdl:RDS900809",null,"A <CABLE LADDER REDUCER LEFT 750 MM-450 MM> is a <CABLE LADDER REDUCER LEFT> that is reduced on the left hand side from 750 mm to 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 750 MM-600 MM",null,null,null,null,null,"rdl:RDS900764",null,"A <CABLE LADDER REDUCER LEFT 750 MM-600 MM> is a <CABLE LADDER REDUCER LEFT> that is reduced on the left hand side from 750 mm to 600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 900 MM-150 MM",null,null,null,null,null,"rdl:RDS900719",null,"A <CABLE LADDER REDUCER LEFT 900 MM-150 MM> is a <CABLE LADDER REDUCER LEFT> that is reduced on the left hand side from 900 mm to 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 900 MM-300 MM",null,null,null,null,null,"rdl:RDS900674",null,"A <CABLE LADDER REDUCER LEFT 900 MM-300 MM> is a <CABLE LADDER REDUCER LEFT> that is reduced on the left hand side from 900 mm to 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 900 MM-450 MM",null,null,null,null,null,"rdl:RDS900629",null,"A <CABLE LADDER REDUCER LEFT 900 MM-450 MM> is a <CABLE LADDER REDUCER LEFT> that is reduced on the left hand side from 900 mm to 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 900 MM-600 MM",null,null,null,null,null,"rdl:RDS900584",null,"A <CABLE LADDER REDUCER LEFT 900 MM-600 MM> is a cable ladder reduser which is reduced on the left hand side from 900> mm to 600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER LEFT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER LEFT 900 MM-750 MM",null,null,null,null,null,"rdl:RDS900539",null,"A <CABLE LADDER REDUCER LEFT 900 MM-750 MM> is a <CABLE LADDER REDUCER LEFT> that is reduced on the left hand side from 900 mm to 750 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,"rdl:RDS900494",null,"A <CABLE LADDER REDUCER RIGHT> is a <CABLE LADDER REDUCER> that is reduced on the right hand side",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 300 MM-150 MM",null,null,null,null,null,"rdl:RDS901169",null,"A <CABLE LADDER REDUCER RIGHT 300 MM-150 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 300 mm to 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 450 MM-150 MM",null,null,null,null,null,"rdl:RDS901214",null,"A <CABLE LADDER REDUCER RIGHT 450 MM-150 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 450 mm to 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 450 MM-300 MM",null,null,null,null,null,"rdl:RDS901304",null,"A <CABLE LADDER REDUCER RIGHT 450 MM-300 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 450 mm to 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 600 MM-150 MM",null,null,null,null,null,"rdl:RDS901439",null,"A <CABLE LADDER REDUCER RIGHT 600 MM-150 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 600 mm to 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 600 MM-300 MM",null,null,null,null,null,"rdl:RDS901394",null,"A <CABLE LADDER REDUCER RIGHT 600 MM-300 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 600 mm to 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 600 MM-450 MM",null,null,null,null,null,"rdl:RDS901349",null,"A <CABLE LADDER REDUCER RIGHT 600 MM-450 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 600 mm to 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 750 MM-300 MM",null,null,null,null,null,"rdl:RDS901574",null,"A <CABLE LADDER REDUCER RIGHT 750 MM-300 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 750 mm to 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 750 MM-450 MM",null,null,null,null,null,"rdl:RDS901529",null,"A <CABLE LADDER REDUCER RIGHT 750 MM-450 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 750 mm to 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 750 MM-600 MM",null,null,null,null,null,"rdl:RDS901484",null,"A <CABLE LADDER REDUCER RIGHT 750 MM-600 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 750 mm to 600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 900 MM-150 MM",null,null,null,null,null,"rdl:RDS901799",null,"A <CABLE LADDER REDUCER RIGHT 900 MM-150 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 900 mm to 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 900 MM-300 MM",null,null,null,null,null,"rdl:RDS901754",null,"A <CABLE LADDER REDUCER RIGHT 900 MM-300 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 900 mm to 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 900 MM-450 MM",null,null,null,null,null,"rdl:RDS901709",null,"A <CABLE LADDER REDUCER RIGHT 900 MM-450 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 900 mm to 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 900 MM-600 MM",null,null,null,null,null,"rdl:RDS901664",null,"A <CABLE LADDER REDUCER RIGHT 900 MM-600 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 900 mm to 600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER REDUCER RIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER REDUCER RIGHT 900 MM-750 MM",null,null,null,null,null,"rdl:RDS901619",null,"A <CABLE LADDER REDUCER RIGHT 900 MM-750 MM> is a <CABLE LADDER REDUCER RIGHT> that is reduced on the right hand side from 900 mm to 750 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER SECTION","ELBOW",null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER RISER",null,null,null,null,null,"rdl:RDS484154",null,"A <CABLE LADDER RISER> is a <CABLE LADDER SECTION> and an <ELBOW> that changes the direction of cables between horizontal and vertical",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER RISER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER INSIDE RISER",null,null,null,null,null,"rdl:RDS484199",null,"A <CABLE LADDER INSIDE RISER> is a <CABLE LADDER RISER> that changes the elevation of cables running inside the bend.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER RISER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER OUTSIDE RISER",null,null,null,null,null,"rdl:RDS484244",null,"A <CABLE LADDER OUTSIDE RISER> is a <CABLE LADDER RISER> that changes the elevation of cables running outside the bend.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER STRAIGHT",null,null,null,null,null,"rdl:RDS865394",null,"A <CABLE LADDER STRAIGHT> is a <CABLE LADDER SECTION> that is a straight length",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER STRAIGHT 150 MM",null,null,null,null,null,"rdl:RDS907469",null,"A <CABLE LADDER STRAIGHT 150 MM> is a <CABLE LADDER STRAIGHT> with the width 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER STRAIGHT 300 MM",null,null,null,null,null,"rdl:RDS907514",null,"A <CABLE LADDER STRAIGHT 300 MM> is a <CABLE LADDER STRAIGHT> with the width 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER STRAIGHT 450 MM",null,null,null,null,null,"rdl:RDS907559",null,"A <CABLE LADDER STRAIGHT 450 MM> is a <CABLE LADDER STRAIGHT> with the width 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER STRAIGHT 600 MM",null,null,null,null,null,"rdl:RDS907604",null,"A <CABLE LADDER STRAIGHT 600 MM> is a <CABLE LADDER STRAIGHT> with the width 600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER STRAIGHT 750 MM",null,null,null,null,null,"rdl:RDS907649",null,"A <CABLE LADDER STRAIGHT 750 MM> is a <CABLE LADDER STRAIGHT> with the width 750 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER STRAIGHT 900 MM",null,null,null,null,null,"rdl:RDS907694",null,"A <CABLE LADDER STRAIGHT 900 MM> is a <CABLE LADDER STRAIGHT> with the width 900 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE",null,null,null,null,null,"rdl:RDS484289",null,"A <CABLE LADDER TEE> is a <CABLE LADDER SECTION> that is joint between 3 other cable ladder sections",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 150/150 MM",null,null,null,null,null,"rdl:RDS905939",null,"A <CABLE LADDER TEE 150/150 MM> is a <CABLE LADDER TEE> with the size 150/150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 150/300 MM",null,null,null,null,null,"rdl:RDS905984",null,"A <CABLE LADDER TEE 150/300 MM> is a <CABLE LADDER TEE> with the size 150/300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 150/450 MM",null,null,null,null,null,"rdl:RDS906029",null,"A <CABLE LADDER TEE 150/450 MM> is a <CABLE LADDER TEE> with the size 150/450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 150/600 MM",null,null,null,null,null,"rdl:RDS906074",null,"A <CABLE LADDER TEE 150/600 MM> is a <CABLE LADDER TEE> with the size 150/600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 300/150 MM",null,null,null,null,null,"rdl:RDS906119",null,"A <CABLE LADDER TEE 300/150 MM> is a <CABLE LADDER TEE> with the size 300/150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 300/300 MM",null,null,null,null,null,"rdl:RDS906164",null,"A <CABLE LADDER TEE 300/300 MM> is a <CABLE LADDER TEE> with the size 300/300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 300/450 MM",null,null,null,null,null,"rdl:RDS906209",null,"A <CABLE LADDER TEE 300/450 MM> is a <CABLE LADDER TEE> with the size 300/450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 300/600 MM",null,null,null,null,null,"rdl:RDS906254",null,"A <CABLE LADDER TEE 300/600 MM> is a <CABLE LADDER TEE> with the size 300/600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 300/750 MM",null,null,null,null,null,"rdl:RDS906299",null,"A <CABLE LADDER TEE 300/750 MM> is a <CABLE LADDER TEE> with the size 300/750 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 300/900 MM",null,null,null,null,null,"rdl:RDS906344",null,"A <CABLE LADDER TEE 300/900 MM> is a <CABLE LADDER TEE> with the size 300/900 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 450/150 MM",null,null,null,null,null,"rdl:RDS906389",null,"A <CABLE LADDER TEE 450/150 MM> is a <CABLE LADDER TEE> with the size 450/150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 450/300 MM",null,null,null,null,null,"rdl:RDS906434",null,"A <CABLE LADDER TEE 450/300 MM> is a <CABLE LADDER TEE> with the size 450/300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 450/450 MM",null,null,null,null,null,"rdl:RDS906479",null,"A <CABLE LADDER TEE 450/450 MM> is a <CABLE LADDER TEE> with the size 45>/450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 450/600 MM",null,null,null,null,null,"rdl:RDS906524",null,"A <CABLE LADDER TEE 450/600 MM> is a <CABLE LADDER TEE> with the size 450/600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 450/750 MM",null,null,null,null,null,"rdl:RDS906569",null,"A <CABLE LADDER TEE 450/750 MM> is a <CABLE LADDER TEE> with the size 450/750 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 450/900 MM",null,null,null,null,null,"rdl:RDS906614",null,"A <CABLE LADDER TEE 450/900 MM> is a <CABLE LADDER TEE> with the size 450/900 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 600/150 MM",null,null,null,null,null,"rdl:RDS906659",null,"A <CABLE LADDER TEE 600/150 MM> is a <CABLE LADDER TEE> with the size 600/150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 600/300 MM",null,null,null,null,null,"rdl:RDS906704",null,"A <CABLE LADDER TEE 600/300 MM> is a <CABLE LADDER TEE> with the size 600/300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 600/450 MM",null,null,null,null,null,"rdl:RDS906749",null,"A <CABLE LADDER TEE 600/450 MM> is a <CABLE LADDER TEE> with the size 600/450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 600/600 MM",null,null,null,null,null,"rdl:RDS906794",null,"A <CABLE LADDER TEE 600/600 MM> is a <CABLE LADDER TEE> with the size 600/600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 600/750 MM",null,null,null,null,null,"rdl:RDS906839",null,"A <CABLE LADDER TEE 600/750 MM> is a <CABLE LADDER TEE> with the size 600/750 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 600/900 MM",null,null,null,null,null,"rdl:RDS906884",null,"A <CABLE LADDER TEE 600/900 MM> is a <CABLE LADDER TEE> with the size 600/900 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 750/150 MM",null,null,null,null,null,"rdl:RDS906929",null,"A <CABLE LADDER TEE 750/150 MM> is a <CABLE LADDER TEE> with the size 750/150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 750/300 MM",null,null,null,null,null,"rdl:RDS906974",null,"A <CABLE LADDER TEE 750/300 MM> is a <CABLE LADDER TEE> with the size 750/300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 750/450 MM",null,null,null,null,null,"rdl:RDS907019",null,"A <CABLE LADDER TEE 750/450 MM> is a <CABLE LADDER TEE> with the size 750/450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 750/600 MM",null,null,null,null,null,"rdl:RDS907064",null,"A <CABLE LADDER TEE 750/600 MM> is a <CABLE LADDER TEE> with the size 750/600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 750/750 MM",null,null,null,null,null,"rdl:RDS907109",null,"A <CABLE LADDER TEE 750/750 MM> is a <CABLE LADDER TEE> with the size 750/750 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 750/900 MM",null,null,null,null,null,"rdl:RDS907154",null,"A <CABLE LADDER TEE 750/900 MM> is a <CABLE LADDER TEE> with the size 750/900 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 900/150 MM",null,null,null,null,null,"rdl:RDS907199",null,"A <CABLE LADDER TEE 900/150 MM> is a <CABLE LADDER TEE> with the size 900/150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 900/300 MM",null,null,null,null,null,"rdl:RDS907244",null,"A <CABLE LADDER TEE 900/300 MM> is a <CABLE LADDER TEE> with the size 900/300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 900/450 MM",null,null,null,null,null,"rdl:RDS907289",null,"A <CABLE LADDER TEE 900/450 MM> is a <CABLE LADDER TEE> with the size 900/450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 900/600 MM",null,null,null,null,null,"rdl:RDS907334",null,"A <CABLE LADDER TEE 900/600 MM> is a <CABLE LADDER TEE> with the size 900/600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 900/750 MM",null,null,null,null,null,"rdl:RDS907379",null,"A <CABLE LADDER TEE 900/750 MM> is a <CABLE LADDER TEE> with the size 900/750 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE LADDER TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE LADDER TEE 900/900 MM",null,null,null,null,null,"rdl:RDS907424",null,"A <CABLE LADDER TEE 900/900 MM> is a <CABLE LADDER TEE> with the size 900/900 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"CABLE RACK",null,null,null,null,null,"rdl:RDS959714",null,"A <CABLE RACK> is an <ARTEFACT> and a <SUPPORT> intended to receive cables that are usually arranged to run side by side",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY SECTION",null,null,null,null,null,"rdl:RDS6232284",null,"A <CABLE TRAY SECTION> is an <ARTEFACT> and a <SUPPORT> that is a part of a <CABLE TRAY SYSTEM>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND",null,null,null,null,null,"rdl:RDS878939",null,"A <CABLE TRAY BEND> is a <CABLE TRAY SECTION> that turns the direction of the cable tray run through an angle in the plane of the cable tray",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY FIXED BEND",null,null,null,null,null,"rdl:RDS879614",null,"A <CABLE TRAY FIXED BEND> is a <CABLE TRAY BEND> which is fixed.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY FIXED BEND",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 45 DEG",null,null,null,null,null,"rdl:RDS901889",null,"A <CABLE TRAY BEND 45 DEG> is a <CABLE TRAY FIXED BEND> where the angle between the vectors normal to the end planes is 45 degrees.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 45 DEG 100 MM",null,null,null,null,null,"rdl:RDS909404",null,"A <CABLE TRAY BEND 45 DEG 100 MM> is a <CABLE TRAY BEND 45 DEG> with a width of 100 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 45 DEG 150 MM",null,null,null,null,null,"rdl:RDS909359",null,"A <CABLE TRAY BEND 45 DEG 150 MM> is a <CABLE TRAY BEND 45 DEG> with a width of 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 45 DEG 200 MM",null,null,null,null,null,"rdl:RDS909494",null,"A <CABLE TRAY BEND 45 DEG 200 MM> is a <CABLE TRAY BEND 45 DEG> with a width of 200 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 45 DEG 300 MM",null,null,null,null,null,"rdl:RDS909539",null,"A <CABLE TRAY BEND 45 DEG 300 MM> is a <CABLE TRAY BEND 45 DEG> with a width of 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 45 DEG 400 MM",null,null,null,null,null,"rdl:RDS909584",null,"A <CABLE TRAY BEND 45 DEG 400 MM> is a <CABLE TRAY BEND 45 DEG> with a width of 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 45 DEG 50 MM",null,null,null,null,null,"rdl:RDS909449",null,"A <CABLE TRAY BEND 45 DEG 50 MM> is a <CABLE TRAY BEND 45 DEG> with a width of 50 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 45 DEG 500 MM",null,null,null,null,null,"rdl:RDS909629",null,"A <CABLE TRAY BEND 45 DEG 500 MM> is a <CABLE TRAY BEND 45 DEG> with a width of 500 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 45 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 45 DEG 600 MM",null,null,null,null,null,"rdl:RDS909674",null,"A <CABLE TRAY BEND 45 DEG 600 MM> is a <CABLE TRAY BEND 45 DEG> with a width of 600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY FIXED BEND",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 90 DEG",null,null,null,null,null,"rdl:RDS901844",null,"A <CABLE TRAY BEND 90 DEG> is a <CABLE TRAY FIXED BEND> where the angle between the vectors normal to the end planes is 90 degrees.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 90 DEG 100 MM",null,null,null,null,null,"rdl:RDS909764",null,"A <CABLE TRAY BEND 90 DEG 100 MM> is a <CABLE TRAY BEND 90 DEG> with a width of 100 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 90 DEG 150 MM",null,null,null,null,null,"rdl:RDS909809",null,"A <CABLE TRAY BEND 90 DEG 150 MM> is a <CABLE TRAY BEND 90 DEG> with a width of 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 90 DEG 200 MM",null,null,null,null,null,"rdl:RDS909854",null,"A <CABLE TRAY BEND 90 DEG 200 MM> is a <CABLE TRAY BEND 90 DEG> with a width of 200 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 90 DEG 300 MM",null,null,null,null,null,"rdl:RDS909899",null,"A <CABLE TRAY BEND 90 DEG 300 MM> is a <CABLE TRAY BEND 90 DEG> with a width of 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 90 DEG 400 MM",null,null,null,null,null,"rdl:RDS909944",null,"A <CABLE TRAY BEND 90 DEG 400 MM> is a <CABLE TRAY BEND 90 DEG> with a width of 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 90 DEG 50 MM",null,null,null,null,null,"rdl:RDS909719",null,"A <CABLE TRAY BEND 90 DEG 50 MM> is a <CABLE TRAY BEND 90 DEG> with a width of 50 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 90 DEG 500 MM",null,null,null,null,null,"rdl:RDS909989",null,"A <CABLE TRAY BEND 90 DEG 500 MM> is a <CABLE TRAY BEND 90 DEG> with a width of 500 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND 90 DEG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY BEND 90 DEG 600 MM",null,null,null,null,null,"rdl:RDS910034",null,"A <CABLE TRAY BEND 90 DEG 600 MM> is a <CABLE TRAY BEND 90 DEG> with a width of 600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY BEND",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY FLEXI-BEND",null,null,null,null,null,"rdl:RDS879389",null,"A <CABLE TRAY FLEXI-BEND> is a <CABLE TRAY BEND> which is adjustable.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY CROSS",null,null,null,null,null,"rdl:RDS878984",null,"A <CABLE TRAY CROSS> i a <CABLE TRAY SECTION> that provides a cross between two cable tray runs",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY SECTION","JOINT",null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY JOINT",null,null,null,null,null,"rdl:RDS484964",null,"A <CABLE TRAY JOINT> is a <CABLE TRAY SECTION> and a <JOINT> intended to join other cable tray sections",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY JOINT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY FIXED JOINT",null,null,null,null,null,"rdl:RDS879074",null,"A <CABLE TRAY FIXED JOINT> is a <CABLE TRAY JOINT> that is fixed.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY JOINT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY FLEXIBLE JOINT",null,null,null,null,null,"rdl:RDS879029",null,"A <CABLE TRAY FLEXIBLE JOINT> is a <CABLE TRAY JOINT> that is adjustable.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY SECTION","REDUCER",null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY REDUCER",null,null,null,null,null,"rdl:RDS485009",null,"A <CABLE TRAY REDUCER> is a <CABLE TRAY SECTION> and a <REDUCER> intended to join cable trays with different widths",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY SECTION","ELBOW",null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY RISER",null,null,null,null,null,"rdl:RDS485099",null,"A <CABLE TRAY RISER> is a <CABLE TRAY SECTION> and an <ELBOW> that changes the direction of a cable tray between horizontal and vertical",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY RISER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY INSIDE RISER",null,null,null,null,null,"rdl:RDS484874",null,"A <CABLE TRAY INSIDE RISER> is a <CABLE TRAY RISER> intended to change the elevation of cables running inside the bend.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY RISER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY OUTSIDE RISER",null,null,null,null,null,"rdl:RDS484919",null,"A <CABLE TRAY OUTSIDE RISER> is a <CABLE TRAY RISER> intended to change the elevation of cables running outside the bend.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY STRAIGHT",null,null,null,null,null,"rdl:RDS866069",null,"A <CABLE TRAY STRAIGHT> is a <CABLE TRAY SECTION> that is straight",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY STRAIGHT 100 MM",null,null,null,null,null,"rdl:RDS910124",null,"A <CABLE TRAY STRAIGHT 100 MM> is a <CABLE TRAY STRAIGHT> with a width of 100 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY STRAIGHT 150 MM",null,null,null,null,null,"rdl:RDS910169",null,"A <CABLE TRAY STRAIGHT 150 MM> is a <CABLE TRAY STRAIGHT> with a width of 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY STRAIGHT 200 MM",null,null,null,null,null,"rdl:RDS910214",null,"A <CABLE TRAY STRAIGHT 200 MM> is a <CABLE TRAY STRAIGHT> with a width of 200 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY STRAIGHT 300 MM",null,null,null,null,null,"rdl:RDS910259",null,"A <CABLE TRAY STRAIGHT 300 MM> is a <CABLE TRAY STRAIGHT> with a width of 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY STRAIGHT 400 MM",null,null,null,null,null,"rdl:RDS910304",null,"A <CABLE TRAY STRAIGHT 400 MM> is a <CABLE TRAY STRAIGHT> with a width of 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY STRAIGHT 50 MM",null,null,null,null,null,"rdl:RDS910079",null,"A <CABLE TRAY STRAIGHT 50 MM> is a <CABLE TRAY STRAIGHT> with a width of 50 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY STRAIGHT 500 MM",null,null,null,null,null,"rdl:RDS910349",null,"A <CABLE TRAY STRAIGHT 500 MM> is a <CABLE TRAY STRAIGHT> with a width of 500 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY STRAIGHT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY STRAIGHT 600 MM",null,null,null,null,null,"rdl:RDS910394",null,"A <CABLE TRAY STRAIGHT 600 MM> is a <CABLE TRAY STRAIGHT> with a width of 600 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY TEE",null,null,null,null,null,"rdl:RDS879119",null,"A <CABLE TRAY TEE> is a <CABLE TRAY SECTION> that is a tee for joining one cable tray run to the side of another run",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY TEE 100 MM",null,null,null,null,null,"rdl:RDS910484",null,"A <CABLE TRAY TEE 100 MM> is a <CABLE TRAY TEE> with a width of 100 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY TEE 150 MM",null,null,null,null,null,"rdl:RDS910529",null,"A <CABLE TRAY TEE 150 MM> is a <CABLE TRAY TEE> with a width of 150 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY TEE 200 MM",null,null,null,null,null,"rdl:RDS910574",null,"A <CABLE TRAY TEE 200 MM> is a <CABLE TRAY TEE> with a width of 200 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY TEE 300 MM",null,null,null,null,null,"rdl:RDS910619",null,"A <CABLE TRAY TEE 300 MM> is a <CABLE TRAY TEE> with a width of 300 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY TEE 400 MM",null,null,null,null,null,"rdl:RDS910664",null,"A <CABLE TRAY TEE 400 MM> is a <CABLE TRAY TEE> with a width of 450 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY TEE 50 MM",null,null,null,null,null,"rdl:RDS910439",null,"A <CABLE TRAY TEE 50 MM> is a <CABLE TRAY TEE> with a width of 50 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY TEE 500 MM",null,null,null,null,null,"rdl:RDS910709",null,"A <CABLE TRAY TEE 500 MM> is a <CABLE TRAY TEE> with a width of 500 mm.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRAY TEE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRAY TEE 600 MM",null,null,null,null,null,"rdl:RDS910754",null,"A <CABLE TRAY TEE 600 MM> is a <CABLE TRAY TEE> with a width of 600 mm",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"CABLE TRUNK SECTION",null,null,null,null,null,"rdl:RDS672984631",null,"A <CABLE TRUNK SECTION> is a <ARTEFACT> and a <SUPPORT> that is a part of a <CABLE TRUNK SYSTEM>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRUNK SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRUNK BEND",null,null,null,null,null,"rdl:RDS6570320",null,"A <CABLE TRUNK BEND> i a <CABLE TRUNK SECTION> where the angle between the vectors normal to the end planes differs from 180 degrees",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRUNK SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRUNK CROSS",null,null,null,null,null,"rdl:RDS6569495",null,"A <CABLE TRUNK CROSS> is a <CABLE TRUNK SECTION> formed as a cross",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRUNK SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRUNK JOINT",null,null,null,null,null,"rdl:RDS6569570",null,"A <CABLE TRUNK JOINT> is a <CABLE TRUNK SECTION> intended for splicing cable trunk sections",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRUNK SECTION","REDUCER",null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRUNK REDUCER",null,null,null,null,null,"rdl:RDS6569690",null,"A <CABLE TRUNK REDUCER> is a <CABLE TRUNK SECTION> and a <REDUCER> intended to join cable trunk sections of different widths",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRUNK SECTION","ELBOW",null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRUNK RISER",null,null,null,null,null,"rdl:RDS6569765",null,"A <CABLE TRUNK RISER> is a <CABLE TRUNK SECTION> and an <ELBOW> and that changes the direction of a cable trunk section between horizontal and vertical",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRUNK RISER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRUNKING RISER INSIDE",null,null,null,null,null,"rdl:RDS6569270",null,"A <CABLE TRUNKING RISER INSIDE> is a <CABLE TRUNKING RISER> that changes the elevation of cables running inside the bend.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRUNK RISER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRUNKING RISER OUTSIDE",null,null,null,null,null,"rdl:RDS6569345",null,"A <CABLE TRUNKING RISER OUTSIDE> is a <CABLE TRUNKING RISER> that changes the elevation of cables running outside the bend.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRUNK SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRUNK STRAIGHT",null,null,null,null,null,"rdl:RDS6569840",null,"A <CABLE TRUNK STRAIGHT> a <CABLE TRUNK SECTION> that is a straight length",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CABLE TRUNK SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,"CABLE TRUNK TEE",null,null,null,null,null,"rdl:RDS6569390",null,"A <CABLE TRUNK TEE> a <CABLE TRUNK SECTION> intended to connect two cable trunk sections perpendicular to one another",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"CAISSON SUPPORT",null,null,null,null,null,"rdl:RDS286514",null,"A <CAISSON SUPPORT> is an <ARTEFACT> and a <SUPPORT> for a caisson, i.e. connecting it to the structure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BAR OBJECT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"CARRYING BAR",null,null,null,null,null,"rdl:RDS5859400",null,"A <CARRYING BAR> is a <BAR OBJECT> and a <SUPPORT> that is intended to carry or support something.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"CHRISTMAS TREE TEST STUMP",null,null,null,null,null,"rdl:RDS16708009",null,"A <CHRISTMAS TREE TEST STUMP> is an <ARTEFACT> and a <SUPPORT> for a subsea christmas tree during testing and transport",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","CONNECTOR","SUPPORT",null,null,null,null,null,null,null,null,null,null,"CIRCUIT BOARD",null,null,null,null,null,"rdl:RDS1318162621",null,"A <CIRCUIT BOARD> is an <ARTEFACT> and a <SUPPORT> and a <CONNECTOR> that mechanically supports and electrically connects electronic components using conductive tracks, pads and other features etched from copper sheets laminated onto a non-conductive substrate",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,"BREADBOARD",null,null,null,null,null,"rdl:RDS1318181601",null,"A <BREADBOARD> is a <CIRCUIT BOARD> that is a construction base for a one-of-a-kind electronic circuit, a prototype.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC CIRCUIT BOARD",null,null,null,null,null,"rdl:RDS5767545",null,"An <ELECTRONIC CIRCUIT BOARD> is a <CIRCUIT BOARD> that comprises a printed circuit board with electronic components intended for receive, process/transform and transmit electrical signals.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AMPLIFIER CIRCUIT BOARD",null,null,null,null,null,"rdl:RDS5767720",null,"An <AMPLIFIER CIRCUIT BOARD> is an <ELECTRONIC CIRCUIT BOARD> for mounting an <AMPLIFIER>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONTROL CIRCUIT BOARD",null,null,null,null,null,"rdl:RDS5783999",null,"A <CONTROL CIRCUIT BOARD> is an <ELECTRONIC CIRCUIT BOARD> that is a transmitter mounted on a <CIRCUIT BOARD> intended to receive and encode one or more signals and produce signals to control handling units",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALARM SIGNAL PROCESSING CIRCUIT BOARD",null,null,null,null,null,"rdl:RDS5767658",null,"An <ALARM SIGNAL PROCESSING CIRCUIT BOARD> is a <CONTROL CIRCUIT BOARD> that is intended to receive and encode one or more signals and produce an output sinal to an alarm unit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INTERFACE CARD",null,null,null,null,null,"rdl:RDS5784405",null,"An <INTERFACE CARD> is an <ELECTRONIC CIRCUIT BOARD> (network card) that is intended for communication between systems, to part of a system or to a computer network.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTERFACE CARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPU SOCKET",null,null,null,null,null,"rdl:RDS5774485",null,"A <CPU SOCKET> is an <INTERFACE CARD> that is a socket or slot that interfaces between a computer&#39;s motherboard and the cpu itself.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTERFACE CARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INPUT-OUTPUT CIRCUIT BOARD",null,null,null,null,null,"rdl:RDS472634",null,"An <INPUT-OUTPUT CIRCUIT BOARD> is an <INTERFACE CARD> with electronic components that is intended to receive/transmit and encode/decode one or more analogue or binary electrical signals to/from a computer interpretable format.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INPUT-OUTPUT CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INPUT CIRCUIT BOARD",null,null,null,null,null,"rdl:RDS5757605",null,"An <INPUT CIRCUIT BOARD> is an <INPUT-OUTPUT CIRCUIT BOARD> containing electronic components intended to receive and encode one or more signals to a computer interpretable format.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INPUT CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANALOGUE SIGNAL INPUT CIRCUIT BOARD",null,null,null,null,null,"rdl:RDS460214",null,"An <ANALOGUE SIGNAL INPUT CIRCUIT BOARD> is an <INPUT CIRCUIT BOARD> intended to receive and encode one or more analogue signals into a computer interpretable format.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INPUT CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIGITAL INPUT CIRCUIT BOARD",null,null,null,null,null,"rdl:RDS460304",null,"A <DIGITAL INPUT CIRCUIT BOARD> is an <INPUT CIRCUIT BOARD> that is intended to receive and encode one or more electrical binary signal(s) to a computer interpretable format.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INPUT-OUTPUT CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OUTPUT CIRCUIT BOARD",null,null,null,null,null,"rdl:RDS5757650",null,"An <OUTPUT CIRCUIT BOARD> is an <INPUT-OUTPUT CIRCUIT BOARD> that is intended to decode and transmit one or more electrical signals from a computer interpretable format to an output signal.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"OUTPUT CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANALOGUE SIGNAL OUTPUT CIRCUIT BOARD",null,null,null,null,null,"rdl:RDS460259",null,"An <ANALOGUE SIGNAL OUTPUT CIRCUIT BOARD> is an <OUTPUT CIRCUIT BOARD> intended to decode and transmit one or more analogue signals from a computer interpretable format into an analogue output signal.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"OUTPUT CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIGITAL OUTPUT CIRCUIT BOARD",null,null,null,null,null,"rdl:RDS460349",null,"A <DIGITAL OUTPUT CIRCUIT BOARD> is an <OUTPUT CIRCUIT BOARD> that is intended to decode and transmit one or more binary signals from a computer interpretable format to a digital output signal.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTERFACE CARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NETWORK CARD",null,null,null,null,null,"rdl:RDS1318193371",null,"A <NETWORK CARD> is an <INTERFACE CARD> that is a network card <THAT> installs into a computer and enables that computer to physically connect to a local area network.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INTERFACE CARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RECEIVER CARD",null,null,null,null,null,"rdl:RDS5784264",null,"A <RECEIVER CARD> is an <INTERFACE CARD> that is an internal power supply that is arranged on an <ELECTRONIC CIRCUIT BOARD>.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOTHERBOARD",null,null,null,null,null,"rdl:RDS5774282",null,"A <MOTHERBOARD> is an <ELECTRONIC CIRCUIT BOARD> that is the main printed circuit board of e.g. a computer that contains the microprocessor, main memory, bus lines and edge connectors to accommodate other boards in the system.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT BOARD","INTERNAL ELECTRIC POWER SUPPLY UNIT",null,null,null,null,null,null,null,null,null,null,null,null,null,"POWER SUPPLY CARD",null,null,null,null,null,"rdl:RDS5784219",null,"A <POWER SUPPLY CARD> is an <ELECTRONIC CIRCUIT BOARD> and an <INTERNAL ELECTRIC POWER SUPPLY UNIT> that is a power supply arranged on an electronic circuit board",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RELAY CARD",null,null,null,null,null,"rdl:RDS5784309",null,"A <RELAY CARD> is an <ELECTRONIC CIRCUIT BOARD> with relays installed on it.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRONIC CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEQUENCE OF EVENTS CARD",null,null,null,null,null,"rdl:RDS1318344241",null,"A <SEQUENCE OF EVENTS CARD> is an <ELECTRONIC CIRCUIT BOARD> that captures events from devices in the field.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,"PRINTED CIRCUIT BOARD",null,null,null,null,null,"rdl:RDS6233550",null,"A <PRINTED CIRCUIT BOARD> is a <CIRCUIT BOARD> consisting of electrical conductors printed on an insulating board and intended to carry electronic devices.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,"STRIPBOARD",null,null,null,null,null,"rdl:RDS1318184171",null,"A <STRIPBOARD> is a <CIRCUIT BOARD> characterized by a 0.1 inch (2.54 mm) regular (rectangular) grid of holes, with wide parallel strips of copper cladding running in one direction all the way across one side of the board.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"COLUMN",null,null,null,null,null,"rdl:RDS288179",null,"A <COLUMN> is an <ARTEFACT> and a <SUPPORT> which is a cylindrical or slightly tapering body of conciderably greater length than diameter, erected vertically as a support",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COLUMN",null,null,null,null,null,null,null,null,null,null,null,null,null,"WOOD COLUMN",null,null,null,null,null,"rdl:RDS500011161",null,"A <WOOD COLUMN> is a <COLUMN> made of wood.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"COLUMN PIPE",null,null,null,null,null,"rdl:RDS879569",null,"A <COLUMN PIPE> is an <ARTEFACT> and a <SUPPORT> that is a vertical pipe by which the pumping elements on a submerged vertical suspended centrifugal pump is mounted",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COLUMN PIPE",null,null,null,null,null,null,null,null,null,null,null,null,null,"COLUMN PIPE - FLANGED",null,null,null,null,null,"rdl:RDS879659",null,"A <COLUMN PIPE - FLANGED> is a <COLUMN PIPE> that is joined using flanges.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COLUMN PIPE",null,null,null,null,null,null,null,null,null,null,null,null,null,"COLUMN PIPE - THREADED",null,null,null,null,null,"rdl:RDS879794",null,"A <COLUMN PIPE - THREADED> is a <COLUMN PIPE> that is joined using threaded couplings.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"CONDUCTOR SUPPORT",null,null,null,null,null,"rdl:RDS286334",null,"A <CONDUCTOR SUPPORT> is an <ARTEFACT> and a <SUPPORT> for a conductor, i.e. connecting it to the J-tube support structure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"CROSSTIE",null,null,null,null,null,"rdl:RDS292184",null,"A <CROSSTIE> is an <ARTEFACT> and a <SUPPORT> tie placed transversely. In ships a horizontal support in a bulkhead frame",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"DRIVER STOOL",null,null,null,null,null,"rdl:RDS402808311",null,"A <DRIVER STOOL> is an <ARTEFACT> and a <SUPPORT> intended to support a motor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL CONTACT BRUSH HOLDER",null,null,null,null,null,"rdl:RDS1004759",null,"An <ELECTRICAL CONTACT BRUSH HOLDER> is an <ARTEFACT> and a <SUPPORT> that is a structure which maintains one or more brushes in a definite position relative to a commutator or slip-ring and usually applies an approximately constant thrust on the brush or brushes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"FOOT SUPPORT",null,null,null,null,null,"rdl:RDS403701211",null,"A <FOOT SUPPORT> is an <ARTEFACT> and a <SUPPORT> that is intended to fix equipment or equipment parts to the base plate/pedestals etc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FOOT SUPPORT",null,null,null,null,null,null,null,null,null,null,null,null,null,"PUMP FOOT",null,null,null,null,null,"rdl:RDS414075091",null,"A <PUMP FOOT> is a <FOOT SUPPORT> that is the particular part of the pump assembly on which the pump is mounted.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"FRAME",null,null,null,null,null,"rdl:RDS8351535",null,"A <FRAME> is an <ARTEFACT> and a <SUPPORT> that is an open structure of beams or bars",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,"A-FRAME",null,null,null,null,null,"rdl:RDS8179980",null,"An <A-FRAME> is a <FRAME> that is a two-legged frame in the form of the letter A for hoisting or excering a vertical pull with block and tackle or winch line attached to the apex of the A-frame",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,"BASE FRAME",null,null,null,null,null,"rdl:RDS13290577",null,"A <BASE FRAME> is a <FRAME>, usually welded, that is acting as the foundation and/or support of a machine or equipment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BASE FRAME","SKID",null,null,null,null,null,null,null,null,null,null,null,null,null,"SKID FRAME",null,null,null,null,null,"rdl:RDS1318965931",null,"A <SKID FRAME> is a <BASE FRAME> and a <SKID> that is the main support in a <SKID ASSEMBLY>.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRAME","MOUNTING PLATE",null,null,null,null,null,null,null,null,null,null,null,null,"CLOSED BEAM SUPPORT FRAME",null,null,null,null,null,"rdl:RDS5677782",null,"A <CLOSED BEAM SUPPORT FRAME> is a <FRAME> and an <MOUNTING PLATE> made from closed steel profiles (hollow steel profiles)",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,"DOOR FRAME",null,null,null,null,null,"rdl:RDS8354730",null,"A <DOOR FRAME> is a <FRAME> built into a wall consisting of two upright members (door jambs) and a door frame head (lintel) over the doorway, and optionally a door sill",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACOUSTIC RATED DOOR FRAME",null,null,null,null,null,"rdl:RDS8355765",null,"An <ACOUSTIC RATED DOOR FRAME> is a <DOOR FRAME> that is capable of dampening sound as defined for the rated conditions under which the type of door has been approved.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE DOORS FRAME",null,null,null,null,null,"rdl:RDS8352930",null,"A <DOUBLE DOORS FRAME> is a <DOOR FRAME> intended to support two door panels mounted in the same door frame, and where both door panels are hinged on the same side of the door frame and are opening in oposite directions.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DUTCH DOOR FRAME",null,null,null,null,null,"rdl:RDS8352795",null,"A <DUTCH DOOR FRAME> is a <DOOR FRAME> that is intended to suport two door panels divided horizontally so that the lower or upper part can be shut separately.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIRE RATED DOOR FRAME",null,null,null,null,null,"rdl:RDS8352030",null,"A <FIRE RATED DOOR FRAME> is a <DOOR FRAME> that is capable of withstanding fire as defined for the rated conditions under which the type of door has been approved.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FOLDING DOOR FRAME",null,null,null,null,null,"rdl:RDS8351805",null,"A <FOLDING DOOR FRAME> is a <DOOR FRAME> intended to support folding door panels.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GLAZED DOOR FRAME",null,null,null,null,null,"rdl:RDS8351085",null,"A <GLAZED DOOR FRAME> is a <DOOR FRAME> intended for a glazed door set.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INNER DOOR FRAME",null,null,null,null,null,"rdl:RDS8350635",null,"An <INNER DOOR FRAME> is a <DOOR FRAME> designed to separate two indoor environments and that is capable of providing specified separation, strength and stability.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INWARD OPENING DOOR FRAME",null,null,null,null,null,"rdl:RDS8350050",null,"An <INWARD OPENING DOOR FRAME> is a <DOOR FRAME> intended to support a door panel which swing inwards into the building or room or towards a defined location when opened.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OUTER DOOR FRAME",null,null,null,null,null,"rdl:RDS8349915",null,"An <OUTER DOOR FRAME> is a <DOOR FRAME> designed to separate an outdoor environment from an indoor environment and that is capable of withstanding the difference in environment between the two sides without malfunction.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OUTWARD OPENING DOOR FRAME",null,null,null,null,null,"rdl:RDS8349465",null,"An <OUTWARD OPENING DOOR FRAME> is a <DOOR FRAME> intended to support a door panel which swing outwards out of the building or room or away from a defined location when opened.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PENDULUM DOOR FRAME",null,null,null,null,null,"rdl:RDS8349330",null,"A <PENDULUM DOOR FRAME> is a <DOOR FRAME> that is capable of supporting a door panel opening both ways.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PIVOT HINGED DOOR FRAME",null,null,null,null,null,"rdl:RDS8349150",null,"A <PIVOT HINGED DOOR FRAME> is a <DOOR FRAME> intended to support a door panel hinged at the upper and lower edges.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"REVOLVING DOOR FRAME",null,null,null,null,null,"rdl:RDS8348970",null,"A <REVOLVING DOOR FRAME> is a <DOOR FRAME> that is intended for a revolving door set.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SECURITY RATED DOOR FRAME",null,null,null,null,null,"rdl:RDS8348880",null,"An <SECURITY RATED DOOR FRAME> is a <DOOR FRAME> that is capable of providing protection against forced entry as defined for the rated conditions under which the type of door has been approved.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE-SASHED DOOR FRAME",null,null,null,null,null,"rdl:RDS8348565",null,"A <SINGLE-SASHED DOOR FRAME> is a <DOOR FRAME> intended to support one door panel.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLIDING DOOR FRAME",null,null,null,null,null,"rdl:RDS8347665",null,"A <SLIDING DOOR FRAME> is a <DOOR FRAME> intended to accomdate a sliding door panel so that the panel can be pushed sideways for opening.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STRONGROOM DOOR FRAME",null,null,null,null,null,"rdl:RDS8347215",null,"A <STRONGROOM DOOR FRAME> is a <DOOR FRAME> made to be installed in a strongroom.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DOOR FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TWO-SASHED DOOR FRAME",null,null,null,null,null,"rdl:RDS8346945",null,"A <TWO-SASHED DOOR FRAME> is a <DOOR FRAME> intended to support two door panels.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,"GANTRY",null,null,null,null,null,"rdl:RDS11526154",null,"A <GANTRY> is a <FRAME> that is a permanent or temporary erection raised on side supports so as to span over or around something",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,"GRATING PLATE",null,null,null,null,null,"rdl:RDS644309",null,"A <GRATING PLATE> is a <FRAME> of bars either parallel or crossing one another",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GRATING PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXPANDED METAL PLATE",null,null,null,null,null,"rdl:RDS644399",null,"An <EXPANDED METAL PLATE> is a <GRATING PLATE> having metal masks.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,"HVAC GRILLE",null,null,null,null,null,"rdl:RDS477314",null,"An <HVAC GRILLE> is a <FRAME> of metal bars or wire for delivering supply air to a room or for collecting extract air from a room",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIFFUSER","HVAC GRILLE",null,null,null,null,null,null,null,null,null,null,null,null,null,"EXTRACT GRILLE DIFFUSER",null,null,null,null,null,"rdl:RDS300419",null,"An <EXTRACT GRILLE DIFFUSER> is an <HVAC GRILLE> and a <DIFFUSER> that extracts air vertically without any deflection",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EXTRACT GRILLE DIFFUSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXTRACT GRILLE DIFFUSER WITH BALANCING DAMPER",null,null,null,null,null,"rdl:RDS300464",null,"An <EXTRACT GRILLE DIFFUSER WITH BALANCING DAMPER> is an <EXTRACT GRILLE DIFFUSER> with a balancing damper",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIFFUSER","HVAC GRILLE",null,null,null,null,null,null,null,null,null,null,null,null,null,"SUPPLY GRILLE DIFFUSER",null,null,null,null,null,"rdl:RDS312344",null,"An <SUPPLY GRILLE DIFFUSER> is an <HVAC GRILLE> and a <DIFFUSER> that supplies air vertically without any deflection",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUPPLY GRILLE DIFFUSER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUPPLY GRILLE DIFFUSER WITH BALANCING DAMPER",null,null,null,null,null,"rdl:RDS312389",null,"A <SUPPLY GRILLE/DIFFUSER WITH BALANCING DAMPER> is a <SUPPLY GRILLE DIFFUSER> with a balancing damper",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRAME","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,null,"STRUCTURAL FRAMEWORK",null,null,null,null,null,"rdl:RDS815080531",null,"A <STRUCTURAL FRAMEWORK> is a <FRAME> and a <SUPPORT> that is a complex of columns, and beams, girders, spandrels, and trusses connected to one another and to columns anchored in a foundation, as well as other components or members necessary for the stability of a structure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRUCTURAL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CRADLE",null,null,null,null,null,"rdl:RDS13621099",null,"A <CRADLE> is a <STRUCTURAL FRAMEWORK> or grating placed round anything to protect it.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CRADLE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SHIPPING CRADLE",null,null,null,null,null,"rdl:RDS13621054",null,"A <SHIPPING CRADLE> is a <CRADLE> intended for shipping goods.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRUCTURAL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CYLINDER COLUMN",null,null,null,null,null,"rdl:RDS13311190",null,"A <CYLINDER COLUMN> is a <STRUCTURAL FRAMEWORK> that supports the cylinder jacket and cylinder liner in large 2-stroke low speed diesel engines.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CAST ARTEFACT","CYLINDER COLUMN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CAST CYLINDER COLUMN",null,null,null,null,null,"rdl:RDS13700240",null,"A <CAST CYLINDER COLUMN> is a <CYLINDER COLUMN> (cylinder block) and a <CAST ARTEFACT> that is entirely made of cast iron",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CYLINDER COLUMN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEMICAST CYLINDER COLUMN",null,null,null,null,null,"rdl:RDS13700302",null,"A <SEMICAST CYLINDER COLUMN> is a <CYLINDER COLUMN> (cylinder block) that is partly made of cast iron and partly of welded steel.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CYLINDER COLUMN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WELDED CYLINDER COLUMN",null,null,null,null,null,"rdl:RDS13700364",null,"A <WELDED CYLINDER COLUMN> is a <CYLINDER COLUMN> (cylinder block) that is entirely made of welded steel.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRUCTURAL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CYLINDER JACKET AND FRAME BOX",null,null,null,null,null,"rdl:RDS13700696",null,"A <CYLINDER JACKET AND FRAME BOX> is a <STRUCTURAL FRAMEWORK> that is the assembly of a a cylinder jacket and an <A FRAME> box in a 2-stroke low speed diesel engine.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRUCTURAL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FRAME BOX",null,null,null,null,null,"rdl:RDS13700426",null,"A <FRAME BOX> is a <STRUCTURAL FRAMEWORK> that is the part of a piston engine block (motor frame) on large 2-stroke diesel engines standing between the cylinder column and the piston engine bed plate.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRUCTURAL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FRAME BOX AND COLUMN",null,null,null,null,null,"rdl:RDS13700534",null,"A <FRAME BOX AND COLUMN> is a <STRUCTURAL FRAMEWORK> that is an assembly of <A FRAME> box and a cylinder column in a 2-stroke low speed diesel engine.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRUCTURAL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT RACK",null,null,null,null,null,"rdl:RDS1030004",null,"An <INSTRUMENT RACK> is a <STRUCTURAL FRAMEWORK> that may be a standardized system for mounting instrument modules and/or other electronic modules.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT RACK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TELECOMMUNICATION RACK",null,null,null,null,null,"rdl:RDS1322264311",null,"A <TELECOMMUNICATION RACK> is an <INSTRUMENT RACK> intended for telecommuniucation equipment.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRUCTURAL FRAMEWORK","STRUCTURE(mechanical)",null,null,null,null,null,null,null,null,null,null,null,null,null,"MODULE STRUCTURE",null,null,null,null,null,"rdl:RDS284669",null,"A <MODULE STRUCTURE> is a <STRUCTURAL FRAMEWORK> and a <STRUCTURE(mechanical)> used to support the equipment in a module.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MODULE STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DRILLING MODULE STRUCTURE",null,null,null,null,null,"rdl:RDS288989",null,"A <DRILLING MODULE STRUCTURE> is a <MODULE STRUCTURE> for a drilling module.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MODULE STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIVING QUARTER STRUCTURE",null,null,null,null,null,"rdl:RDS289169",null,"A <LIVING QUARTER STRUCTURE> is a <MODULE STRUCTURE> that is a structural facility of the living quarter.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MODULE STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRODUCTION MODULE STRUCTURE",null,null,null,null,null,"rdl:RDS289124",null,"A <PRODUCTION MODULE STRUCTURE> is a <MODULE STRUCTURE> that is a structural facility of the production module.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRUCTURAL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OPEN BEAM SUPPORT FRAME",null,null,null,null,null,"rdl:RDS5677720",null,"An <OPEN BEAM SUPPORT FRAME> is a <STRUCTURAL FRAMEWORK> that is a foundation or support frame for a machine or an equipment item, made of open steel profiles.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","STRUCTURAL FRAMEWORK","TRANSPORTABLE CONTAINER",null,null,null,null,null,null,null,null,null,null,null,null,"SHIPPING RACK",null,null,null,null,null,"rdl:RDS1067820891",null,"A <SHIPPING RACK> is an <ARTEFACT> and a <STRUCTURAL FRAMEWORK> and a <TRANSPORTABLE CONTAINER> that is a framework intended for retainment of goods under transportation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRUCTURAL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRUSS",null,null,null,null,null,"rdl:RDS815165801",null,"A <TRUSS> is a <STRUCTURAL FRAMEWORK> that is a constructed as to form a firm support for a superincumbent weight, as that of a roof or bridge.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRUSS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ROOF TRUSS",null,null,null,null,null,"rdl:RDS1187774",null,"A <ROOF TRUSS> is a <TRUSS> to support a <ROOF>.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ROOF TRUSS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WOOD ROOF TRUSS",null,null,null,null,null,"rdl:RDS815174951",null,"A <WOOD ROOF TRUSS> is a <ROOF TRUSS> that is also a wood framework.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRUCTURAL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WALL FRAMEWORK",null,null,null,null,null,"rdl:RDS328319",null,"A <WALL FRAMEWORK> is a <STRUCTURAL FRAMEWORK> that is a rigid supportive and/or protective openwork or structural frame of an object.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WALL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STEEL WALL FRAMEWORK",null,null,null,null,null,"rdl:RDS487707631",null,"A <STEEL WALL FRAMEWORK> is a <WALL FRAMEWORK> assembled mainly from steel objects.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WALL FRAMEWORK","WOOD FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WOOD WALL FRAMEWORK",null,null,null,null,null,"rdl:RDS7905020",null,"A <WOOD WALL FRAMEWORK> is a <WALL FRAMEWORK> where the main structural members are wooden objects.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WOOD WALL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DISPLACED DOUBLE LEAF TIMBER FRAMEWORK",null,null,null,null,null,"rdl:RDS7905206",null,"A <DISPLACED DOUBLE LEAF TIMBER FRAMEWORK> is a <WOOD WALL FRAMEWORK> that is displaced.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WOOD WALL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE TIMBER FRAMEWORK",null,null,null,null,null,"rdl:RDS7905144",null,"A <DOUBLE TIMBER FRAMEWORK> is a <WOOD WALL FRAMEWORK> that is double.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WOOD WALL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE TIMBER FRAMEWORK",null,null,null,null,null,"rdl:RDS7905082",null,"A <SINGLE TIMBER FRAMEWORK> is a <WOOD WALL FRAMEWORK> that is single.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRUCTURAL FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WOOD FRAMEWORK",null,null,null,null,null,"rdl:RDS815110491",null,"A <WOOD FRAMEWORK> is a <STRUCTURAL FRAMEWORK> in which the main structural components are wooden objects.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WOOD FRAMEWORK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WOOD ROOF FRAMEWORK",null,null,null,null,null,"rdl:RDS815113521",null,"A <WOOD ROOF FRAMEWORK> is a <WOOD FRAMEWORK> that is a roof framework.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA CHRISTMAS TREE GUIDE FRAME",null,null,null,null,null,"rdl:RDS16679579",null,"A <SUBSEA CHRISTMAS TREE GUIDE FRAME> is a <FRAME> that is a structural framwork to provide guidance with the PGB interface, and used for installation of the subsea tree on the subsea wellhead. Also provides support for tree flowlines and connection equipment, control pods, anodes, and counterbalance weigths",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA FLOWLINE CONNECTOR SUPPORT FRAME",null,null,null,null,null,"rdl:RDS16680316",null,"A <SUBSEA FLOWLINE CONNECTOR SUPPORT FRAME> is a <FRAME> that receives and supports the flowline connector and transfers flowline loads back into the wellhead or seabed anchored structure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA MANIFOLD SUPPORT FRAME",null,null,null,null,null,"rdl:RDS16705128",null,"A <SUBSEA MANIFOLD SUPPORT FRAME> is a <FRAME> that is a structural framework to provide strength and protection for a subsea manifold",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FRAME",null,null,null,null,null,null,null,null,null,null,null,null,null,"WINDOW FRAME",null,null,null,null,null,"rdl:RDS8345725",null,"A <WINDOW FRAME> is a <FRAME> into which a window fits to shut the opening",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"FRAMEWORK STUD",null,null,null,null,null,"rdl:RDS329129",null,"A <FRAMEWORK STUD> is an <ARTEFACT> and a <SUPPORT> that consists of a series of slender vertical structural members placed as supporting elements",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"GROMMET",null,null,null,null,null,"rdl:RDS1005254",null,"A <GROMMET> is an <ARTEFACT> and a <SUPPORT> intended to support and protect the wires or cable at the point of entry",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"GUIDE BLADE CARRIER",null,null,null,null,null,"rdl:RDS406125111",null,"A <GUIDE BLADE CARRIER> is an <ARTEFACT> and a <SUPPORT> that is the stationary part inside the casing containing the stator blades",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"HANDLE",null,null,null,null,null,"rdl:RDS7294360",null,"A <HANDLE> is an <ARTEFACT> and a <SUPPORT> that is intended to be gripped by a human hand",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HANDLE",null,null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRAL HANDLE",null,null,null,null,null,"rdl:RDS14598460",null,"An <INTEGRAL HANDLE> is a <HANDLE> that forms an integral part of an object",null,null,null,null,null,"dm:ClassOfFeature"]
[null,null,"HANDLE",null,null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRAL ORIFICE PADDLE",null,null,null,null,null,"rdl:RDS6773811",null,"An <INTEGRAL ORIFICE PADDLE> is a <HANDLE> that is forming an integral of an orifice plate with paddle",null,null,null,null,null,"dm:ClassOfFeature"]
[null,null,"HANDLE","INSTRUMENTATION COMPONENT",null,null,null,null,null,null,null,null,null,null,null,null,"ORIFICE HANDLE",null,null,null,null,null,"rdl:RDS7042940",null,"An <ORIFICE HANDLE> is an <INSTRUMENTATION COMPONENT> and a <HANDLE> that is a rectangular plate forming part of an assembled <PADDLE ORIFICE PLATE>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HANDLE",null,null,null,null,null,null,null,null,null,null,null,null,null,"RUPTURE DISC HANDLE",null,null,null,null,null,"rdl:RDS8372990",null,"An <RUPTURE DISC HANDLE> is a <HANDLE> that is a rectangular plate forming part of an rupture disc.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"HANGER",null,null,null,null,null,"rdl:RDS408819271",null,"A <HANGER> is an <ARTEFACT> and a <SUPPORT> that suspends something",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,"BEARING HANGER",null,null,null,null,null,"rdl:RDS395049751",null,"A <BEARING HANGER> is a <HANGER> for a bearing that on its turn is intended to support a shaft. So the hanger is intended to carry the full load on the bearing.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,"PIPE HANGER",null,null,null,null,null,"rdl:RDS5786299",null,"A <PIPE HANGER> is a <HANGER> that is designed to support piping components from above.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,"WELL STRING HANGER",null,null,null,null,null,"rdl:RDS5859620",null,"A <WELL STRING HANGER> is a <HANGER> that is designed to fit on a well component and suspend a pipe string in a well.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WELL STRING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CASING HANGER",null,null,null,null,null,"rdl:RDS5796704",null,"A <CASING HANGER> is a <WELL STRING HANGER> that is designed to suspend a well casing string down the well.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CASING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE SLIPS CASING HANGER",null,null,null,null,null,"rdl:RDS7166932",null,"A <DOUBLE SLIPS CASING HANGER> is a <CASING HANGER> that has two sets of slips; one above the other.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CASING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HINGED CASING HANGER",null,null,null,null,null,"rdl:RDS7166887",null,"A <HINGED CASING HANGER> is a <CASING HANGER> that is equipped with a hinge so that it can be opened to fit around a casing.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CASING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPLIT CASING HANGER",null,null,null,null,null,"rdl:RDS7167011",null,"An <SPLIT CASING HANGER> is a <CASING HANGER> that is made in two halves so that it can be fit around a casing.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WELL STRING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LINER HANGER",null,null,null,null,null,"rdl:RDS5802248",null,"A <LINER HANGER> is a <WELL STRING HANGER> that is designed to hang liners in casings.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LINER HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC LINER HANGER",null,null,null,null,null,"rdl:RDS5802338",null,"A <HYDRAULIC LINER HANGER> is a <LINER HANGER> which set liners in casing by pressurizing the work string to set the slips. Work string manipulation need not be considered for setting operations.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LINER HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MECHANICAL LINER HANGER",null,null,null,null,null,"rdl:RDS5802293",null,"A <MECHANICAL LINER HANGER> is a <LINER HANGER> which set liners in casing by rotating and / or raising and lowering the work string to set the slips of the hanger.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"WELL STRING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TUBING HANGER",null,null,null,null,null,"rdl:RDS5796811",null,"A <TUBING HANGER> is a <WELL STRING HANGER> that is installed on top of the tubing string and supports the string when landed in the tubing hanger or tubing head.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUBING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONCENTRIC TUBING HANGER",null,null,null,null,null,"rdl:RDS16679993",null,"A <CONCENTRIC TUBING HANGER> is a <TUBING HANGER> that has the axis of the production tubing concentric with the wellhead axis.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUBING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DUAL TUBING HANGER",null,null,null,null,null,"rdl:RDS7161663",null,"A <DUAL TUBING HANGER> is a <TUBING HANGER> that holds two tubing strings.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUBING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECCENTRIC TUBING HANGER",null,null,null,null,null,"rdl:RDS16680055",null,"An <ECCENTRIC TUBING HANGER> is a <TUBING HANGER> that has the axis of the production tubing parallel with the wellhead axis.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUBING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EXTENDED SEAL NECK TUBING HANGER",null,null,null,null,null,"rdl:RDS7161798",null,"An <EXTENDED SEAL NECK TUBING HANGER> is a <TUBING HANGER> that has an extended neck for additional sealing.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUBING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HORIZONTAL TUBING HANGER",null,null,null,null,null,"rdl:RDS17873705",null,"A <HORIZONTAL TUBING HANGER> is a <TUBING HANGER> that is having the production bore branching off at right angles from the main bore.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUBING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE TUBING HANGER",null,null,null,null,null,"rdl:RDS7161618",null,"A <SINGLE TUBING HANGER> is a <TUBING HANGER> that holds a single tubing string.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUBING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SLIP TYPE TUBING HANGER",null,null,null,null,null,"rdl:RDS7161753",null,"A <SLIP TYPE TUBING HANGER> is a <TUBING HANGER> that has slips that holds the tubing string.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUBING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPLIT TUBING HANGER",null,null,null,null,null,"rdl:RDS7168660",null,"An <SPLIT TUBING HANGER> is a <TUBING HANGER> that is made in two parts which will be clamped around the tubing string.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUBING HANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THREADED TUBING HANGER",null,null,null,null,null,"rdl:RDS7161708",null,"A <THREADED TUBING HANGER> is a <TUBING HANGER> that has internal threads which connects to the tubing string.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ENCLOSURE","SUPPORT",null,null,null,null,null,null,null,null,null,null,"HOUSING",null,null,null,null,null,"rdl:RDS11008205",null,"A <HOUSING> is an <ARTEFACT> and an <ENCLOSURE> and a <SUPPORT> that, next to separation, also provides support",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,"BEARING HOUSING",null,null,null,null,null,"rdl:RDS433484",null,"A <BEARING HOUSING> is a <HOUSING> intended to support a bearing.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BEARING HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BEARING HEAD",null,null,null,null,null,"rdl:RDS16771284",null,"A <BEARING HEAD> is a <BEARING HOUSING> that contains bearing assemblies for male- and female rotor shafts. Typically used in screw pumps and screw compressors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BEARING HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CENTRIFUGAL COMPRESSOR BEARING HOUSING",null,null,null,null,null,"rdl:RDS14215852",null,"A <CENTRIFUGAL COMPRESSOR BEARING HOUSING> is a <BEARING HOUSING> for a centrifugal compressor.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BEARING HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIAL BEARING HOUSING",null,null,null,null,null,"rdl:RDS414146831",null,"A <RADIAL BEARING HOUSING> is a <BEARING HOUSING> intended to house a radial bearing.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BEARING HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THRUST BEARING HOUSING",null,null,null,null,null,"rdl:RDS426482161",null,"A <THRUST BEARING HOUSING> is a <BEARING HOUSING> intended to house a thrust bearing.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,"EXHAUST VALVE HOUSING",null,null,null,null,null,"rdl:RDS13701600",null,"An <EXHAUST VALVE HOUSING> is a <HOUSING> of an exhaust valve constituting the support as well as the valve seat for the valve blade.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,"GEAR CASING",null,null,null,null,null,"rdl:RDS13291748",null,"A <GEAR CASING> is a <HOUSING> that contains the internal components of a gear.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT HOUSING",null,null,null,null,null,"rdl:RDS431099",null,"An <INSTRUMENT HOUSING> is a <HOUSING> that is the static part of an instrument.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDICATOR HOUSING",null,null,null,null,null,"rdl:RDS4233424",null,"An <INDICATOR HOUSING> is an <INSTRUMENT HOUSING> that is the static part of an indicator.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDICATOR HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE MEASURING GAUGE CASE",null,null,null,null,null,"rdl:RDS1467380111",null,"A <PRESSURE MEASURING GAUGE CASE> is an <INDICATOR HOUSING> of a <PRESSURE MEASURING GAUGE>.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INDICATOR HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE INDICATOR HOUSING",null,null,null,null,null,"rdl:RDS7349321",null,"A <TEMPERATURE INDICATOR HOUSING> is an <INDICATOR HOUSING> that is the static part of a temperature indicator.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE INDICATOR HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANALOGUE TEMPERATURE INDICATOR HOUSING",null,null,null,null,null,"rdl:RDS7351111",null,"An <ANALOGUE TEMPERATURE INDICATOR HOUSING> is a <TEMPERATURE INDICATOR HOUSING> that is intended for an analogue indicator.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TEMPERATURE INDICATOR HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIGITAL TEMPERATURE INDICATOR HOUSING",null,null,null,null,null,"rdl:RDS7351156",null,"A <DIGITAL TEMPERATURE INDICATOR HOUSING> is a <TEMPERATURE INDICATOR HOUSING> that is the static part of an analogue temperature indicator.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROBE HOUSING",null,null,null,null,null,"rdl:RDS5785920",null,"A <PROBE HOUSING> is an <INSTRUMENT HOUSING> that is intended for support and protecting a probe (detecting element).",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRANSMITTER HOUSING",null,null,null,null,null,"rdl:RDS735074",null,"A <TRANSMITTER HOUSING> is an <INSTRUMENT HOUSING> of a transmitter.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSMITTER HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EPOXY-POLYESTER-COVERED ALUMINIUM TRANSMITTER HOUSING",null,null,null,null,null,"rdl:RDS5558203",null,"An <EPOXY-POLYESTER-COVERED ALUMINIUM TRANSMITTER HOUSING> is a <TRANSMITTER HOUSING> that is made of aluminium and covered by Epoxy-polyester.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,"MECHANICAL DRIVE HOUSING",null,null,null,null,null,"rdl:RDS997539911",null,"A <MECHANICAL DRIVE HOUSING> is a <HOUSING> fabricated from a single, internally cored casting, or composed of two or more separate castings, and designed to position and protect bearings, shafts, gears, and/or other components required for a mechanical drive.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE ACTUATOR HOUSING",null,null,null,null,null,"rdl:RDS7504673",null,"A <VALVE ACTUATOR HOUSING> is a <HOUSING> that is intended to enclose a <VALVE ACTUATOR>.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HOUSING","VALVE COMPONENT",null,null,null,null,null,null,null,null,null,null,null,null,"VALVE BONNET",null,null,null,null,null,"rdl:RDS431189",null,"A <VALVE BONNET> is a <VALVE COMPONENT> and a <HOUSING> that is a fluid or pressure containing part of a valve body, intended to support the stem and its sealing arrangement, and which may accommodate the valve closure member when in the open position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BALL VALVE BONNET",null,null,null,null,null,"rdl:RDS6328643",null,"A <BALL VALVE BONNET> is a <VALVE BONNET> that is intended for a ball valve.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BALL VALVE BONNET","BOLTED VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BOLTED BALL VALVE BONNET",null,null,null,null,null,"rdl:RDS676394",null,"A <BOLTED BALL VALVE BONNET> is a <BALL VALVE BONNET> that is bolted to the valve body.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BOLTED VALVE BONNET",null,null,null,null,null,"rdl:RDS610334",null,"A <BOLTED VALVE BONNET> is a <VALVE BONNET> that is bolted to the valve body.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BOLTED VALVE BONNET","GATE VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BOLTED GATE VALVE BONNET",null,null,null,null,null,"rdl:RDS722789",null,"A <BOLTED GATE VALVE BONNET> is a <BOLTED VALVE BONNET> that is a gate valve bonnet.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BOLTED GATE VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GATE VALVE BOLTED BONNET WITH INTEGRAL YOKE",null,null,null,null,null,"rdl:RDS866609",null,"A <GATE VALVE BOLTED BONNET WITH INTEGRAL YOKE> is a <BOLTED GATE VALVE BONNET> that is equipped with an integral yoke.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BOLTED GATE VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GATE VALVE BOLTED BONNET WITH SEPARATE YOKE",null,null,null,null,null,"rdl:RDS866654",null,"A <GATE VALVE BOLTED BONNET WITH SEPARATE YOKE> is a <BOLTED GATE VALVE BONNET> that has a separate yoke.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIAPHRAGM VALVE BONNET",null,null,null,null,null,"rdl:RDS6329069",null,"A <DIAPHRAGM VALVE BONNET> is a <VALVE BONNET> that is intended for a diaphragm valve.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GATE VALVE BONNET",null,null,null,null,null,"rdl:RDS6328502",null,"A <GATE VALVE BONNET> is a <VALVE BONNET> that is intended for a gate valve.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GLOBE VALVE BONNET",null,null,null,null,null,"rdl:RDS6330228",null,"A <GLOBE VALVE BONNET> is a <VALVE BONNET> that is intended for a globe valve.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JACKETED VALVE BONNET",null,null,null,null,null,"rdl:RDS6330501",null,"A <JACKETED VALVE BONNET> is a <VALVE BONNET> that is for a jacketed valve.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON VENTED VALVE BONNET",null,null,null,null,null,"rdl:RDS7464745",null,"A <NON VENTED VALVE BONNET> is a <VALVE BONNET> that is solid.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PLUG VALVE BONNET",null,null,null,null,null,"rdl:RDS6330597",null,"A <PLUG VALVE BONNET> is a <VALVE BONNET> that is for a plug valve.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RELIEF VALVE BONNET",null,null,null,null,null,"rdl:RDS6329260",null,"A <RELIEF VALVE BONNET> is a <VALVE BONNET> that is intended for a relief valve.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RELIEF VALVE BONNET WITH CAP",null,null,null,null,null,"rdl:RDS7465337",null,"A <RELIEF VALVE BONNET WITH CAP> is a <RELIEF VALVE BONNET> that has a cap.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RELIEF VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RELIEF VALVE BONNET WITH LEVER",null,null,null,null,null,"rdl:RDS7465399",null,"A <RELIEF VALVE BONNET WITH LEVER> is a <RELIEF VALVE BONNET> that has a lever.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SCREWED VALVE BONNET",null,null,null,null,null,"rdl:RDS646559",null,"A <SCREWED VALVE BONNET> is a <VALVE BONNET> that is screwed to the valve body.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SCREWED VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE BONNET INSIDE SCREW",null,null,null,null,null,"rdl:RDS11480067",null,"A <VALVE BONNET INSIDE SCREW> is a <SCREWED VALVE BONNET> that is screwed to the valve body with inside located screws.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SCREWED VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE BONNET OUTSIDE SCREW",null,null,null,null,null,"rdl:RDS11479988",null,"A <VALVE BONNET OUTSIDE SCREW> is a <SCREWED VALVE BONNET> that is screwed to the valve body with outside located screws.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET OUTSIDE SCREW","YOKE-TYPE VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE BONNET OUTSIDE SCREW AND YOKE",null,null,null,null,null,"rdl:RDS11480146",null,"A <VALVE BONNET OUTSIDE SCREW AND YOKE> is a <VALVE BONNET OUTSIDE SCREW> and a <YOKE-TYPE VALVE BONNET> in the form of a yoke that is screwed to the valve body with outside located screws.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE MANIFOLD BONNET",null,null,null,null,null,"rdl:RDS1471136721",null,"A <VALVE MANIFOLD BONNET> is a <VALVE BONNET> that is mounted on to a manifold chamber and that supports a <VALVE STEM> and a <VALVE HANDLE> and that allows the opening or closing of a port of the manifold chamber.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VENTED VALVE BONNET",null,null,null,null,null,"rdl:RDS7464700",null,"A <VENTED VALVE BONNET> is a <VALVE BONNET> that has a hole for venting excess pressure.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WELDED VALVE BONNET",null,null,null,null,null,"rdl:RDS6328581",null,"A <WELDED VALVE BONNET> is a <VALVE BONNET> that is welded to the valve body.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE BONNET",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"YOKE-TYPE VALVE BONNET",null,null,null,null,null,"rdl:RDS7464790",null,"A <YOKE-TYPE VALVE BONNET> is a <VALVE BONNET> that is in the form of a yoke.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HOUSING",null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE SEAT HOUSING",null,null,null,null,null,"rdl:RDS14598988",null,"A <VALVE SEAT HOUSING> is a <HOUSING> that is a pocket in the valve body where the valve seat is withdrawn to when the valve is in open position (for not to obstruct the flow). This pocket is where the seat holder is located on valves with floating seats.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"IMPELLER SUPPORT - BETWEEN BEARINGS",null,null,null,null,null,"rdl:RDS2229060",null,"An <IMPELLER SUPPORT - BETWEEN BEARINGS> is an <ARTEFACT> and a <SUPPORT> that supports the <IMPELLER> with a <BEARING> at both sides",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"IMPELLER SUPPORT - OVERHUNG",null,null,null,null,null,"rdl:RDS2229059",null,"An <IMPELLER SUPPORT - OVERHUNG> is an <ARTEFACT> and a <SUPPORT> that supports the <IMPELLER> with a <BEARING> at shaft side only",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"INTERMEDIATE BEARING SPIDER",null,null,null,null,null,"rdl:RDS407887171",null,"An <INTERMEDIATE BEARING SPIDER> is an <ARTEFACT> and a <SUPPORT> that is intended to serve as support structure for an intermediate bearing",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"J-TUBE SUPPORT",null,null,null,null,null,"rdl:RDS286424",null,"A <J-TUBE SUPPORT> is an <ARTEFACT> and a <SUPPORT> for a <J-TUBE>, connecting it to the <J-TUBE SUPPORT FRAME> structure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"J-TUBE SUPPORT FRAME",null,null,null,null,null,"rdl:RDS286469",null,"A <J-TUBE SUPPORT FRAME> is an <ARTEFACT> and a <SUPPORT> for a <J-TUBE> connecting it to the main structure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"JOIST",null,null,null,null,null,"rdl:RDS500777681",null,"A <JOIST> is an <ARTEFACT> and a <SUPPORT> that consists of a series of parallel horizontal beams used to support floor and ceiling loads, and supported in turn by larger beams, girders, or bearing walls",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"JOIST","WOODEN OBJECT",null,null,null,null,null,null,null,null,null,null,null,null,"WOOD JOIST",null,null,null,null,null,"rdl:RDS500779851",null,"A <WOOD JOIST> is a <JOIST> and a <WOODEN OBJECT>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"LADDER SUPPORT",null,null,null,null,null,"rdl:RDS4316790417",null,"A <LADDER SUPPORT> is an <ARTEFACT> and a <SUPPORT> intended to support a ladder",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"LIFTING ATTACHMENT",null,null,null,null,null,"rdl:RDS290609",null,"A <LIFTING ATTACHMENT> is an <ARTEFACT> and a <SUPPORT> on structures, equipment etc. to attach equipment for lifting or repositioning",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","LIFTING ATTACHMENT",null,null,null,null,null,null,null,null,null,null,null,null,"CRANE PENNANT WIRE",null,null,null,null,null,"rdl:RDS1324994481",null,"A <CRANE PENNANT WIRE> is an <ARTEFACT> and a <LIFTING ATTACHMENT> that is a wire rope having at its lower end a block or a thimble spliced to an eye for receiving the hooks of the fore and main tackles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LIFTING ATTACHMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,"PADEYE",null,null,null,null,null,"rdl:RDS286154",null,"A <PADEYE> is a <LIFTING ATTACHMENT> used to fasten lifting or movement equipment to the structure. A padeye have hole for a shackle.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"LIFTING ATTACHMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,"TRUNNION",null,null,null,null,null,"rdl:RDS445004",null,"A <TRUNNION> is a <LIFTING ATTACHMENT> that consists of a cylindrical body and generally a plate, welded to an item. Typically used for lifting.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRUNNION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIFTING TRUNNION",null,null,null,null,null,"rdl:RDS431679050",null,"A <LIFTING TRUNNION> is a <TRUNNION> n intended to facilitate the lifting of an item.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"MOTOR SLIDE RAIL",null,null,null,null,null,"rdl:RDS816704",null,"A <MOTOR SLIDE RAIL> is an <ARTEFACT> and a <SUPPORT> on which an electric motor is mounted and serves as a tensioning device when a v-belt drive is involved",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLATE","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"MOUNTING PLATE",null,null,null,null,null,"rdl:RDS435059",null,"An <MOUNTING PLATE> is a <PLATE> and a <SUPPORT> that is intended to support a machine or equipment item",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MOUNTING PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BASE PLATE",null,null,null,null,null,"rdl:RDS417644",null,"A <BASE PLATE> is an <MOUNTING PLATE> that is for an equipment item and that is assembled with that equipment item.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BASE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CENTRIFUGAL COMPRESSOR BASE PLATE",null,null,null,null,null,"rdl:RDS14216752",null,"A <CENTRIFUGAL COMPRESSOR BASE PLATE> is a <BASE PLATE> for a centrifugal compressor.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BASE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HEAVY DUTY BASE PLATE",null,null,null,null,null,"rdl:RDS5644494",null,"A <HEAVY DUTY BASE PLATE> is a <BASE PLATE> that is strengthened and a metal member on which a machine and its driver can be mounted.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"BASE PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOTOR STOOL",null,null,null,null,null,"rdl:RDS435014",null,"A <MOTOR STOOL> is a <BASE PLATE> that is a support structure for mounting of a electric motor, customary used on vertical centrifugal pumps.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MOUNTING PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,"GROUTED MOUNTING PLATE",null,null,null,null,null,"rdl:RDS5677906",null,"A <GROUTED MOUNTING PLATE> is an <MOUNTING PLATE> that is a foundation or support frame for a machine or an equipment item, which is designed for beeing grouted/ filled with grouting.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MOUNTING PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,"SOLE PLATE",null,null,null,null,null,"rdl:RDS329354",null,"A <SOLE PLATE> is an <MOUNTING PLATE> located under the feet of a piece of equipment and embedded in a foundation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MOUNTING PLATE",null,null,null,null,null,null,null,null,null,null,null,null,null,"UNGROUTED MOUNTING PLATE",null,null,null,null,null,"rdl:RDS5677844",null,"A <UNGROUTED MOUNTING PLATE> is an <MOUNTING PLATE> that is a foundation or support frame for a machine or an equipment item, which is not designed for beeing grouted /filled with grouting.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"MOUNTING RAIL",null,null,null,null,null,"rdl:RDS5858840",null,"An <MOUNTING RAIL> is an <ARTEFACT> and a <SUPPORT> upon which other artefacts can be mounted",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"MUDMAT",null,null,null,null,null,"rdl:RDS287324",null,"A <MUDMAT> is an <ARTEFACT> and a <SUPPORT> intended to prevent excessive jacket penetration into the soil",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"NON-TUBULAR HEAT EXCHANGER SUPPORT",null,null,null,null,null,"rdl:RDS14066865",null,"A <NON-TUBULAR HEAT EXCHANGER SUPPORT> is an <ARTEFACT> and a <SUPPORT> that is the support frame on a non-tubular heat exchanger",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"PACKING SUPPORT",null,null,null,null,null,"rdl:RDS43168246105",null,"A <PACKING SUPPORT> is an <ARTEFACT> and a <SUPPORT> intended to support packing material",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"PANEL",null,null,null,null,null,"rdl:RDS2229062",null,"A <PANEL> is an <SUPPORT> that is a usually vertical mount for <DISPLAYING> something",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT PANEL",null,null,null,null,null,"rdl:RDS7199468",null,"An <INSTRUMENT PANEL> is a <PANEL> that contains instruments, controlling and/or signalling devices arranged in a suitable manner",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALARM PANEL",null,null,null,null,null,"rdl:RDS7057363",null,"An <ALARM PANEL> is an <INSTRUMENT PANEL> containing full set of alarms required for a system or part of it.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONTROL PANEL",null,null,null,null,null,"rdl:RDS874124",null,"A <CONTROL PANEL> is an <INSTRUMENT PANEL> containing a set of indicating devices and control units required for operation of a system or part of it.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CENTRIFUGAL COMPRESSOR LUBE OIL CONSOLE",null,null,null,null,null,"rdl:RDS14215897",null,"A <CENTRIFUGAL COMPRESSOR LUBE OIL CONSOLE> is a <CONTROL PANEL> for the centrifugal compressor lube oil system.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CENTRIFUGAL COMPRESSOR SEAL OIL CONSOLE",null,null,null,null,null,"rdl:RDS14215942",null,"A <CENTRIFUGAL COMPRESSOR SEAL OIL CONSOLE> is a <CONTROL PANEL> for the centrifugal compressor seal oil system.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL CONTROL PANEL",null,null,null,null,null,"rdl:RDS1295560811",null,"An <ELECTRICAL CONTROL PANEL> is a <CONTROL PANEL> intended for electrical aparatuses.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL CONTROL PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HEAT TRACING CONTROL PANEL",null,null,null,null,null,"rdl:RDS1295566301",null,"A <HEAT TRACING CONTROL PANEL> is an <ELECTRICAL CONTROL PANEL> designed to control one or more <HEAT TRACING CIRCUIT>s.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"KEYBOARD",null,null,null,null,null,"rdl:RDS5778172",null,"A <KEYBOARD> is a <CONTROL PANEL> with an array of systematically arranged (piano like) keys by which a machine is operated or by which an instrument can be played on.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OPERATOR INTERFACE PANEL",null,null,null,null,null,"rdl:RDS5777320",null,"An <OPERATOR INTERFACE PANEL> is a <CONTROL PANEL> that is intended for connection/communication between systems or parts of a system.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THYRISTOR CONTROL PANEL",null,null,null,null,null,"rdl:RDS1295511221",null,"A <THYRISTOR CONTROL PANEL> is a <CONTROL PANEL> that contains devices required for the operation of thyristors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIRE AND GAS PANEL",null,null,null,null,null,"rdl:RDS300959",null,"A <FIRE AND GAS PANEL> is an <INSTRUMENT PANEL> for monitoring and controlling fire and gas dequipment.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIRE DAMPER PANEL",null,null,null,null,null,"rdl:RDS301004",null,"A <FIRE DAMPER PANEL> is an <INSTRUMENT PANEL> for controlling and monitoring fire dampers.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LOCAL INSTRUMENT PANEL",null,null,null,null,null,"rdl:RDS1295474221",null,"A <LOCAL INSTRUMENT PANEL> is an <INSTRUMENT PANEL> that is mounted on, or close to, a process instrument, as opposed to one that is located at a central location.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA ROV PANEL",null,null,null,null,null,"rdl:RDS16706621",null,"A <SUBSEA ROV PANEL> is an <INSTRUMENT PANEL> attached to a subsea structure, e.g. a christmas tree, centralizing the interfaces between an ROV and the valves on the unit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SYSTEM PANEL",null,null,null,null,null,"rdl:RDS1318770571",null,"A <SYSTEM PANEL> is an <INSTRUMENT PANEL> dedicated to a particular <SYSTEM>.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PANEL",null,null,null,null,null,null,null,null,null,null,null,null,null,"TELECOMMUNICATIONS PANEL",null,null,null,null,null,"rdl:RDS1295603491",null,"A <TELECOMMUNICATIONS PANEL> is a <PANEL> specifically intended for telecommunications devices",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"PEDESTAL",null,null,null,null,null,"rdl:RDS412306721",null,"A <PEDESTAL> is an <ARTEFACT> and a <SUPPORT> that is the base or foot of a column or other upright structure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"PILE",null,null,null,null,null,"rdl:RDS287414",null,"A <PILE> is an <ARTEFACT> and a <SUPPORT> that is a slender structural member substantialy under ground to transmit forces from the structure into the loadbearing strata below the surface of the ground",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PILE",null,null,null,null,null,null,null,null,null,null,null,null,null,"ANCHOR PILE",null,null,null,null,null,"rdl:RDS1292423521",null,"An <ANCHOR PILE> is a <PILE> used for the attachment of lines for anchorage purposes.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"PILE CLUSTER",null,null,null,null,null,"rdl:RDS286109",null,"A <PILE CLUSTER> is an <ARTEFACT> and a <SUPPORT> that is a cluster of piles",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"PIPE SUPPORT",null,null,null,null,null,"rdl:RDS286559",null,"A <PIPE SUPPORT> is an <ARTEFACT> and a <SUPPORT> intended to support one or more pipes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPE SUPPORT",null,null,null,null,null,null,null,null,null,null,null,null,null,"ADJUSTABLE PIPE SUPPORT",null,null,null,null,null,"rdl:RDS1300656381",null,"An <ADJUSTABLE PIPE SUPPORT> is a <PIPE SUPPORT> that can be adjusted.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","GUIDE","PIPE SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"PIPE GUIDE",null,null,null,null,null,"rdl:RDS4316824823",null,"A <PIPE GUIDE> is an <ARTEFACT> and a <PIPE SUPPORT> and a <GUIDE> intended to prevent movement of a pipe in one or more directions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"PIPELINE SPAN SUPPORT",null,null,null,null,null,"rdl:RDS8775568",null,"A <PIPELINE SPAN SUPPORT> is an <ARTEFACT> and a <SUPPORT> that can support a pipeline at the start and end of pipeline freespan section or a pipeline intermittent spanning section",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPELINE COVERAGE","PIPELINE SPAN SUPPORT",null,null,null,null,null,null,null,null,null,null,null,null,"GROUT BAG",null,null,null,null,null,"rdl:RDS8656521",null,"A <GROUT BAG> is a <PIPELINE SPAN SUPPORT> and a <PIPELINE COVERAGE> that is a bag filled with grout.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"PIPELINE SUPPORT MATERIAL",null,null,null,null,null,"rdl:RDS13116240",null,"A <PIPELINE SUPPORT MATERIAL> is an <ARTEFACT> and a <SUPPORT> that is used for pipeline support",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPELINE SUPPORT MATERIAL",null,null,null,null,null,null,null,null,null,null,null,null,null,"NATURAL PIPELINE SUPPORT MATERIAL",null,null,null,null,null,"rdl:RDS13116718",null,"A <NATURAL PIPELINE SUPPORT MATERIAL> is a <PIPELINE SUPPORT MATERIAL> that is naturally occuring",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"PLATFORM",null,null,null,null,null,"rdl:RDS7906377",null,"A <PLATFORM> is an <ARTEFACT> and a <SUPPORT> which is a usually raised horizontal flat surface; especially a raised flooring",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLATFORM",null,null,null,null,null,null,null,null,null,null,null,null,null,"INNER BOTTOM",null,null,null,null,null,"rdl:RDS290834",null,"A <INNER BOTTOM> is a <PLATFORM> plating forming the top of the double bottom",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLATFORM",null,null,null,null,null,null,null,null,null,null,null,null,null,"SERVICE PLATFORM",null,null,null,null,null,"rdl:RDS285029",null,"A <SERVICE PLATFORM> is a <PLATFORM> giving service access to an equipment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLATFORM",null,null,null,null,null,null,null,null,null,null,null,null,null,"UPENDING PLATFORM",null,null,null,null,null,"rdl:RDS289709",null,"A <UPENDING PLATFORM> is a <PLATFORM> installed to position and operate the upending balsting system on a floating structure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"PLATFORM SUPPORT",null,null,null,null,null,"rdl:RDS43168248148",null,"A <PLATFORM SUPPORT> is an <ARTEFACT> and a <SUPPORT> intended to support a platform",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","FLOAT","SUPPORT",null,null,null,null,null,null,null,null,null,null,"PONTOON",null,null,null,null,null,"rdl:RDS11526649",null,"A <PONTOON> is an <ARTEFACT> and a <SUPPORT> and a <FLOAT> that is a large flat-bottomed barge, boat, hollow metal cylinder or lighter that can be equipped with cranes and tackle for careening ships and salvage work, or can be used to support a temporary bridge or floating landing stage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"PUMP COLUMN",null,null,null,null,null,"rdl:RDS14287100",null,"A <PUMP COLUMN> is an <ARTEFACT> and a <SUPPORT> that is the a vertical circular pipe constituting of the suspension and discharge pipe for a vertical centrifugal pump. The pump column can also accommodate the guide bushings for line shaft pumps",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","ENCLOSURE","SUPPORT",null,null,null,null,null,null,null,null,null,null,"PUSH-PULL CABLE CASING",null,null,null,null,null,"rdl:RDS1287764381",null,"A <PUSH-PULL CABLE CASING> is an <ARTEFACT> and an <ENCLOSURE> and a <SUPPORT> that surrounds a <WIRE> or <CABLE>, and that allows those to move freely in that axial direction",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"RAFTER",null,null,null,null,null,"rdl:RDS500771941",null,"A <RAFTER> is an <ARTEFACT> and a <SUPPORT> that consists of a series of structural members designed to support roof loads",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"REACTOR BED SUPPORT",null,null,null,null,null,"rdl:RDS43168514122",null,"A <REACTOR BED SUPPORT> is an <ARTEFACT> and a <SUPPORT> for a reactor bed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"RISER SUPPORT",null,null,null,null,null,"rdl:RDS286379",null,"A <RISER SUPPORT> is an <ARTEFACT> and a <SUPPORT> connecting a riser to a structure",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SADDLE BLOCK",null,null,null,null,null,"rdl:RDS13175355",null,"A <SADDLE BLOCK> is an <ARTEFACT> and a <SUPPORT> that is u-shaped as a saddle and used for holding down and/or stabilising an equipment or item",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SADDLE BLOCK",null,null,null,null,null,null,null,null,null,null,null,null,null,"PIGGY BACK SADDLE BLOCK",null,null,null,null,null,"rdl:RDS13173870",null,"A <PIGGY BACK SADDLE BLOCK> is a <SADDLE BLOCK> used to piggyback a pipeline, cable or umbilical onto another pipeline",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SADDLE BLOCK",null,null,null,null,null,null,null,null,null,null,null,null,null,"STABILISATION SADDLE BLOCK",null,null,null,null,null,"rdl:RDS13173015",null,"A <STABILISATION SADDLE BLOCK> is a <SADDLE BLOCK> which is an inverted <U->shaped concrete block used to stabilise a pipeline.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SADDLE SUPPORT",null,null,null,null,null,"rdl:RDS418904",null,"A <SADDLE SUPPORT> is an <ARTEFACT> and a <SUPPORT> that is an assembly of plates and profiles with a saddleshaped plate at the top intended to support an horizontal vessel or tank",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLATE","SADDLE SUPPORT",null,null,null,null,null,null,null,null,null,null,null,null,"HORIZONTAL CYLINDRICAL ATMOSPHERIC TANK SADDLE PLATE",null,null,null,null,null,"rdl:RDS14321424",null,"A <HORIZONTAL CYLINDRICAL ATMOSPHERIC TANK SADDLE PLATE> is a <SADDLE SUPPORT> and a <PLATE> used for a horizontal cylindrical tank",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SEATING",null,null,null,null,null,"rdl:RDS14639125",null,"A <SEATING> is an <ARTEFACT> and a <SUPPORT> that is serving as the base of something else",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SKEG",null,null,null,null,null,"rdl:RDS293444",null,"A <SKEG> is an <ARTEFACT> and a <SUPPORT> that is a deep, vertical finlike projection on bottom of a vessel near the stern, installed to support the lower edge of the rudder. to support the propeller shaft for single screw skips, and for the support of vessel in dray dock. Also used on barges to minimize erratic steering in seaway",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SKID",null,null,null,null,null,"rdl:RDS283589",null,"A <SKID> is an <ARTEFACT> and a <SUPPORT> intended to support items when being manufactured, transported, handled or installed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLATE","SKID",null,null,null,null,null,null,null,null,null,null,null,null,"SKID PLATE",null,null,null,null,null,"rdl:RDS890639",null,"A <SKID PLATE> is a <PLATE> and a <SKID> intended to support, lift and transport a smaller or larger group of equipment items",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SLIDE RAIL",null,null,null,null,null,"rdl:RDS418745191",null,"A <SLIDE RAIL> is an <ARTEFACT> and a <SUPPORT> intended for mounting an electric motor and that enables adjustment",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SLIDING SUPPORT",null,null,null,null,null,"rdl:RDS431686359",null,"A <SLIDING SUPPORT> is an <ARTEFACT> and a <SUPPORT> that allows the supported object(s) to slide",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"STRETCHER",null,null,null,null,null,"rdl:RDS12137448",null,"A <STRETCHER> is an <ARTEFACT> and a <SUPPORT> that is a framework of poles, canvas, etc. for carrying a sick, injured or wounded person",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRETCHER",null,null,null,null,null,null,null,null,null,null,null,null,null,"BASKET TYPE STRETCHER",null,null,null,null,null,"rdl:RDS7064904",null,"A <BASKET TYPE STRETCHER> is a <STRETCHER> having a basket like shape.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PLATE","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"STRIP",null,null,null,null,null,"rdl:RDS5998102",null,"A <STRIP> is a <PLATE> and a <SUPPORT> that is a long and narrow sheet or plate of solid material",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRIP",null,null,null,null,null,null,null,null,null,null,null,null,null,"BACKING STRIP",null,null,null,null,null,"rdl:RDS431648901",null,"A <BACKING STRIP> is a <STRIP> that is placed under a weld seam intended to prevent oxidation during welding.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRIP",null,null,null,null,null,null,null,null,null,null,null,null,null,"NONFERROUS METAL ALLOY STRIP",null,null,null,null,null,"rdl:RDS5998012",null,"A <NONFERROUS METAL ALLOY STRIP> is a <STRIP> that is made from a nonferrous metal alloy.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRIP",null,null,null,null,null,null,null,null,null,null,null,null,null,"SEALING STRIP",null,null,null,null,null,"rdl:RDS418637191",null,"A <SEALING STRIP> is a <STRIP> intended to minimize leakage and typically applied in steam turbines preventing steam leakage to pass a steam turbine blade tip into the following nozzle and mounted between blade shrouds and casing diaphragms.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STEEL","STRIP",null,null,null,null,null,null,null,null,null,null,null,null,"STEEL STRIP",null,null,null,null,null,"rdl:RDS5997877",null,"A <STEEL STRIP> is a <STRIP> that is made from <STEEL>.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AUSTENITIC STAINLESS STEEL","STEEL STRIP",null,null,null,null,null,null,null,null,null,null,null,null,null,"AUSTENITIC STAINLESS STEEL STRIP",null,null,null,null,null,"rdl:RDS5997967",null,"An <AUSTENITIC STAINLESS STEEL STRIP> is a <STEEL STRIP> that is made from <AUSTENITIC STAINLESS STEEL>.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SUBSEA CHOKE MODULE",null,null,null,null,null,"rdl:RDS16762494",null,"A <SUBSEA CHOKE MODULE> is an <ARTEFACT> and a <SUPPORT> that is a retrievable/fixed module for installation of a subsea choke valve",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SUBSEA FLOW CONTROL MODULE",null,null,null,null,null,"rdl:RDS16696102",null,"A <SUBSEA FLOW CONTROL MODULE> is an <ARTEFACT> and a <SUPPORT> that is installed between a christmas tree and a manifold",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","STRUCTURE(mechanical)","SUPPORT",null,null,null,null,null,null,null,null,null,null,"SUBSTRUCTURE",null,null,null,null,null,"rdl:RDS284489",null,"A <SUBSTRUCTURE> is an <ARTEFACT> and a <SUPPORT> and a <STRUCTURE(mechanical)> that supports a <FACILITY>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSTRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,"FIXED STRUCTURE",null,null,null,null,null,"rdl:RDS282239",null,"A <FIXED STRUCTURE> is a <SUBSTRUCTURE> that is fixed to the earth by e.g. piles, its gravity. The structure is intended for supporting a facility.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FIXED STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GRAVITY BASED STRUCTURE",null,null,null,null,null,"rdl:RDS282284",null,"A <GRAVITY BASED STRUCTURE> is a <FIXED STRUCTURE> that is a facility that is a solid structure located at the sea bottom, and fixed at the location to the sea bottom by its own weight (gravity).",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FIXED STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JACKET STRUCTURE",null,null,null,null,null,"rdl:RDS282554",null,"A <JACKET STRUCTURE> is a <FIXED STRUCTURE> that is a functional unit that is consisting of a bottom founded framework structure with three or more legs.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FIXED STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JACKUP STRUCTURE",null,null,null,null,null,"rdl:RDS282599",null,"A <JACKUP STRUCTURE> is a <FIXED STRUCTURE> that is a facility consisting of a mobile drilling rig with three or more legs which can be jacked up until the topside part is a safe height above the sea level.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FIXED STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA FIXED STRUCTURE",null,null,null,null,null,"rdl:RDS282329",null,"A <SUBSEA FIXED STRUCTURE> is a <FIXED STRUCTURE> located at the sea bottom and intended for supporting a subsea facility. All structure and equipment are below sealevel.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","PIPING NETWORK TERMINATOR","SUBSEA FIXED STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,"PIPELINE END TERMINAL",null,null,null,null,null,"rdl:RDS16557108",null,"A <PIPELINE END TERMINAL> is an <ARTEFACT> and a <PIPING NETWORK TERMINATOR> and a <SUBSEA FIXED STRUCTURE> in a subsea flowline",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PIPELINE END TERMINAL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RISER BASE",null,null,null,null,null,"rdl:RDS285164",null,"A <RISER BASE> is a <PIPELINE END TERMINAL> that forms the termination of a subsea flowline where it is connected to a riser.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RISER BASE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS LIFT RISER BASE",null,null,null,null,null,"rdl:RDS16557018",null,"A <GAS LIFT RISER BASE> is a <RISER BASE> with equipment for facilititating gas lift.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA FIXED STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA GUIDE BASE",null,null,null,null,null,"rdl:RDS16551297",null,"A <SUBSEA GUIDE BASE> is a <SUBSEA FIXED STRUCTURE> supporting a wellhead.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA GUIDE BASE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PERMANENT GUIDE BASE",null,null,null,null,null,"rdl:RDS12182209",null,"A <PERMANENT GUIDE BASE> is a <SUBSEA GUIDE BASE> that is set in a permanent alignment to the wellhead system and provides entry guidance for running equipment on or into the wellhead.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA GUIDE BASE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPORARY GUIDE BASE",null,null,null,null,null,"rdl:RDS12182085",null,"A <TEMPORARY GUIDE BASE> is a <SUBSEA GUIDE BASE> intended to be placed on the seabed to provide a guide template for drilling the conductor (30-inch) hole and provide a support base for the permanent guide base.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA FIXED STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA MANIFOLD CENTRE",null,null,null,null,null,"rdl:RDS18140720",null,"A <SUBSEA MANIFOLD CENTRE> is a <SUBSEA FIXED STRUCTURE> supporting a manifold and tie-in equipment.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA FIXED STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA PROTECTION STRUCTURE",null,null,null,null,null,"rdl:RDS289439",null,"A <SUBSEA PROTECTION STRUCTURE> is a <SUBSEA FIXED STRUCTURE> that protects sensitive subsea located equipment from dropped objects and from trawl activities.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSEA FIXED STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SUBSEA TEMPLATE",null,null,null,null,null,"rdl:RDS16551212",null,"A <SUBSEA TEMPLATE> is a <SUBSEA FIXED STRUCTURE> with slots for several wells.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSTRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOATING STRUCTURE",null,null,null,null,null,"rdl:RDS282194",null,"A <FLOATING STRUCTURE> is a <SUBSTRUCTURE> that is a facility that describes an installation located on the surface of the sea, and is moveable. Supposed to be fixed to the sea bottom by anchor chains or tension legs.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOATING STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOATING STORAGE UNIT",null,null,null,null,null,"rdl:RDS291329",null,"A <FLOATING STORAGE UNIT> is a <FLOATING STRUCTURE> that is a facility used for storage which describe an installation located on the surface of the sea, and is moveable. Supposed to be fixed to the sea bottom by anchor chains or tension legs.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOATING STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRODUCTION SHIP STRUCTURE",null,null,null,null,null,"rdl:RDS282509",null,"A <PRODUCTION SHIP STRUCTURE> is a <FLOATING STRUCTURE> that is a facility that is a purpose-built vessel (ship/barge), intended to carry topside installations.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOATING STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEMI SUBMERSIBLE STRUCTURE",null,null,null,null,null,"rdl:RDS282464",null,"A <SEMI SUBMERSIBLE STRUCTURE> is a <FLOATING STRUCTURE> that is a facility that is a seabed-anchored or dynamically positioned buoyant/compliant substructure which provides support for topside structure and equipment.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"FLOATING STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TENSION LEG PLATFORM STRUCTURE",null,null,null,null,null,"rdl:RDS282419",null,"A <TENSION LEG PLATFORM STRUCTURE> is a <FLOATING STRUCTURE> that is a facility that is a seabed-anchored buoyant/compliant substructure which provides support for topside installations.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUBSTRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,"MOVABLE STRUCTURE",null,null,null,null,null,"rdl:RDS16228077",null,"A <MOVABLE STRUCTURE> is a <SUBSTRUCTURE> that can be moved to other locations for temporarily supporting facilities.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SUPPORT ASSEMBLY",null,null,null,null,null,"rdl:RDS13703020",null,"A <SUPPORT ASSEMBLY> is an <ARTEFACT> and a <SUPPORT> that is a structural arrangement for holding an object in place",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUPPORT ASSEMBLY",null,null,null,null,null,null,null,null,null,null,null,null,null,"COMBUSTION ENGINE FOUNDATION ARRANGEMENT",null,null,null,null,null,"rdl:RDS13703082",null,"A <COMBUSTION ENGINE FOUNDATION ARRANGEMENT> is a <SUPPORT ARRANGEMENT> that is designed to support combustion engines.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COMBUSTION ENGINE FOUNDATION ARRANGEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESILIANT ENGINE SUPPORT ARRANGEMENT",null,null,null,null,null,"rdl:RDS13659420",null,"A <RESILIANT ENGINE SUPPORT ARRANGEMENT> is a <COMBUSTION ENGINE FOUNDATION ARRANGEMENT> that has the function to give flexible or resilient support to a reciprocating piston engine.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RESILIANT ENGINE SUPPORT ARRANGEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE SUPPORTED COMMON FRAME",null,null,null,null,null,"rdl:RDS13703336",null,"A <FLEXIBLE SUPPORTED COMMON FRAME> is a <RESILIANT ENGINE SUPPORT ARRANGEMENT> that gives resiliant support to a reciprocating piston engine and the driven equipment fixed mounted on a common frame.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RESILIANT ENGINE SUPPORT ARRANGEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLEXIBLE SUPPORTED ENGINE",null,null,null,null,null,"rdl:RDS13703274",null,"A <FLEXIBLE SUPPORTED ENGINE> is a <RESILIANT ENGINE SUPPORT ARRANGEMENT> that gives support to a reciprocating piston engine.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COMBUSTION ENGINE FOUNDATION ARRANGEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIGID ENGINE SUPPORT ARRANGEMENT",null,null,null,null,null,"rdl:RDS13659482",null,"A <RIGID ENGINE SUPPORT ARRANGEMENT> is a <COMBUSTION ENGINE FOUNDATION ARRANGEMENT> that has the function to give rigid support to an reciprocating combustion engine.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RIGID ENGINE SUPPORT ARRANGEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIGID SUPPORT ON ADJUSTABLE STEEL CHOCKS",null,null,null,null,null,"rdl:RDS13659606",null,"A <RIGID SUPPORT ON ADJUSTABLE STEEL CHOCKS> is a <RIGID ENGINE SUPPORT ARRANGEMENT> that gives support to an engine through steel chocks with adjustable height.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RIGID ENGINE SUPPORT ARRANGEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIGID SUPPORT ON EPOXY RESIN CHOCKS",null,null,null,null,null,"rdl:RDS13659544",null,"A <RIGID SUPPORT ON EPOXY RESIN CHOCKS> is a <RIGID ENGINE SUPPORT ARRANGEMENT> that gives rigid support to a reciprocating piston engine through chocks filleed with epoxy.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RIGID ENGINE SUPPORT ARRANGEMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIGID SUPPORTED COMMON FRAME",null,null,null,null,null,"rdl:RDS13703212",null,"A <RIGID SUPPORTED COMMON FRAME> is a <RIGID ENGINE SUPPORT ARRANGEMENT> that gives rigid support to a reciprocating piston engine and the driven equipment that is fixed mounted on a common frame.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SUPPORT LEG",null,null,null,null,null,"rdl:RDS280889",null,"A <SUPPORT LEG> is an <ARTEFACT> and a <SUPPORT> that is more or less resembling a leg, or performing its function as a support for a body",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUPPORT LEG",null,null,null,null,null,null,null,null,null,null,null,null,null,"VERTICAL CYLINDRICAL ATMOSPHERIC TANK LEG",null,null,null,null,null,"rdl:RDS14320029",null,"A <VERTICAL CYLINDRICAL ATMOSPHERIC TANK LEG> is a <SUPPORT LEG> of a vertical cylindrical atmospheric tank.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"RING","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SUPPORT RING",null,null,null,null,null,"rdl:RDS431686404",null,"A <SUPPORT RING> is a <RING> and a <SUPPORT> intended to carry an item",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUPPORT RING",null,null,null,null,null,null,null,null,null,null,null,null,null,"INSULATION SUPPORT RING",null,null,null,null,null,"rdl:RDS437489",null,"An <INSULATION SUPPORT RING> is a <SUPPORT RING> designed to support insulation material that has an annular shape.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUPPORT RING",null,null,null,null,null,null,null,null,null,null,null,null,null,"VALVE SEAT RING",null,null,null,null,null,"rdl:RDS646874",null,"A <VALVE SEAT RING> is a <SUPPORT RING> that is intended to support the valve closure member. One face of the ring forms the valve seat which may contain a seat insert. The reverse face is fastened to the body of the valve by a threaded portion or by swaging in small bore valves.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SUPPORT TRAY",null,null,null,null,null,"rdl:RDS13034700",null,"A <SUPPORT TRAY> is a <TRAY> and a <SUPPORT> intended to bear other internals",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUPPORT TRAY",null,null,null,null,null,null,null,null,null,null,null,null,null,"DEMISTER SUPPORT TRAY",null,null,null,null,null,"rdl:RDS13035285",null,"A <DEMISTER SUPPORT TRAY> is a <SUPPORT TRAY> intended to support a demister.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUPPORT TRAY",null,null,null,null,null,null,null,null,null,null,null,null,null,"GRID TRAY",null,null,null,null,null,"rdl:RDS13035195",null,"A <GRID TRAY> is a <TRAY> intended to support packing and that has the shape of a grid.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STRUCTURE(mechanical)","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"SUPPORTING STRUCTURE",null,null,null,null,null,"rdl:RDS13310380",null,"A <SUPPORTING STRUCTURE> is a <SUPPORT> and a <STRUCTURE(mechanical)> supporting an object",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUPPORTING STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,"DERRICK",null,null,null,null,null,"rdl:RDS289034",null,"A <DERRICK> is a <SUPPORTING STRUCTURE> that is a kind of crane with a movable pivoted arm for moving heavy weights, for example built over a wellsite to provide support for drilling equipment and a tall mast for raising and lowering drillpipe and casing.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SUPPORTING STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,"FLARE STACK STRUCTURE",null,null,null,null,null,"rdl:RDS1324077151",null,"A <FLARE STACK STRUCTURE> is a <SUPPORTING STRUCTURE> that is an elevated vertical conveyance that is part of installations such as oil and gas wells, oil rigs, refineries, chemical, petrochemical and natural gas plants, and other facilities. On oil- production rigs and in refineries and petrochemical plants, the flare stacks primarily serve to protect vessels or pipes from over-pressuring during unexpected plant upsets.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"TERMINAL RAIL",null,null,null,null,null,"rdl:RDS881594",null,"A <TERMINAL RAIL> is an <ARTEFACT> and a <SUPPORT> to which terminals can be attached to form a terminal row",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"THRUST BEARING PAD",null,null,null,null,null,"rdl:RDS14205349",null,"A <THRUST BEARING PAD> is an <ARTEFACT> and a <SUPPORT> that is a thrust bearing component that consists of segments of a bearing sleeve mounted in a housing being able to transfer load from the shaft",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","STRUCTURE(mechanical)","SUPPORT",null,null,null,null,null,null,null,null,null,null,"TOPSIDE SUPPORT STRUCTURE",null,null,null,null,null,"rdl:RDS284534",null,"A <TOPSIDE SUPPORT STRUCTURE> is an <ARTEFACT> and a <SUPPORT> and a <STRUCTURE(mechanical)> for a platform topside",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TOPSIDE SUPPORT STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,"TOPSIDE DECK STRUCTURE",null,null,null,null,null,"rdl:RDS284624",null,"A <TOPSIDE DECK STRUCTURE> is a <TOPSIDE SUPPORT STRUCTURE> that is a facility to support topside modules and equipment.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TOPSIDE DECK STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONCRETE BEAM DECK STRUCTURE",null,null,null,null,null,"rdl:RDS285299",null,"A <CONCRETE BEAM DECK STRUCTURE> is a <TOPSIDE DECK STRUCTURE> that is a supporting facility consisting of single girders constructed in concrete.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TOPSIDE DECK STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LOAD TRANSFER FRAME",null,null,null,null,null,"rdl:RDS285344",null,"A <LOAD TRANSFER FRAME> is a <TOPSIDE DECK STRUCTURE> that is a facility installed on top of jacket, <GBS>, compliant tower etc. to transfere loads from the deck structure tu the substructure. Built as a steel space frame from standard or prefabricated profiles.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TOPSIDE DECK STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OPEN TRUSS DECK STRUCTURE",null,null,null,null,null,"rdl:RDS285209",null,"An <OPEN TRUSS DECK STRUCTURE> is a <TOPSIDE DECK STRUCTURE> that is a Model Suport Frame facility to support topside equipment constructed by prefabricated boxes and nodes, welded profiles and/or standard profiles.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TOPSIDE DECK STRUCTURE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PLATED GIRDER DECK STRUCTURE",null,null,null,null,null,"rdl:RDS285254",null,"A <PLATED GIRDER DECK STRUCTURE> is a <TOPSIDE DECK STRUCTURE> that is a plated girder Module Support Frame that consists of single plate-constructed girders or a frame constructed by prefabricated plate girders and plated deck constructions for installation of pre-assembled packages/pancakes.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","STRUCTURAL MEMBER","SUPPORT",null,null,null,null,null,null,null,null,null,null,"TRANSVERSE",null,null,null,null,null,"rdl:RDS290924",null,"A <TRANSVERSE> is an <ARTEFACT> and a <SUPPORT> and a <STRUCTURAL MEMBER> that is a deep member supporting longitudinal frames of bottom or side shell or longitudinal deck beams. A transverse is directed at right angles to the fore-and-aft centerline",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSVERSE",null,null,null,null,null,null,null,null,null,null,null,null,null,"BOTTOM TRANSVERSE",null,null,null,null,null,"rdl:RDS291014",null,"A <BOTTOM TRANSVERSE> is a <TRANSVERSE> supporting longitudinal frames of bottom shell beams.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSVERSE",null,null,null,null,null,null,null,null,null,null,null,null,null,"DECK TRANSVERSE",null,null,null,null,null,"rdl:RDS290969",null,"A <DECK TRANSVERSE> is a <TRANSVERSE> supporting longitudinal deck beams.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","BAFFLE","SUPPORT",null,null,null,null,null,null,null,null,null,null,"TRANSVERSE BAFFLE",null,null,null,null,null,"rdl:RDS443789",null,"A <TRANSVERSE BAFFLE> is an <ARTEFACT> and a <BAFFLE> and a <SUPPORT> that is mounted orthogonal to the tubes in a shell and tube heat exchanger to support the tubes and force the shell-side flow across the tubes for better performance",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSVERSE BAFFLE",null,null,null,null,null,null,null,null,null,null,null,null,null,"DISK AND DOUGHNUT BAFFLE",null,null,null,null,null,"rdl:RDS440414",null,"A <DISK AND DOUGHNUT BAFFLE> is a <TRANSVERSE BAFFLE> that is several disk baffles and doughnut baffles placed in series.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TRANSVERSE BAFFLE",null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE SEGMENTAL BAFFLE",null,null,null,null,null,"rdl:RDS440504",null,"A <DOUBLE SEGMENTAL BAFFLE> is a <TRANSVERSE BAFFLE> that consists of two segmental parts in one plane.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"TRENCH BED",null,null,null,null,null,"rdl:RDS13288559",null,"A <TRENCH BED> is an <ARTEFACT> and a <SUPPORT> for a pipeline which is a continous layer of compound at the bottom of the excavated trench",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIVIDER(separator)","PLATE","SUPPORT",null,null,null,null,null,null,null,null,null,null,"TUBE SHEET",null,null,null,null,null,"rdl:RDS415304",null,"A <TUBE SHEET> is a <PLATE> and a <SUPPORT> and a <DIVIDER> that is intended to support tubes and to isolate the shell side from the tube side of a shell and tube heat exchanger",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUBE SHEET",null,null,null,null,null,null,null,null,null,null,null,null,null,"CLADDED TUBE SHEET",null,null,null,null,null,"rdl:RDS11018645",null,"A <CLADDED TUBE SHEET> is a <TUBE SHEET> that is protected by one or more layers of other material.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUBE SHEET",null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE TUBE SHEET",null,null,null,null,null,"rdl:RDS11018015",null,"A <DOUBLE TUBE SHEET> is a <TUBE SHEET> that is an assembly of a pair of tube sheets with a gap between them, where one sheet seal the tube side fluid and the other seals the shell side fluid.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUBE SHEET",null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOATING TUBE SHEET",null,null,null,null,null,"rdl:RDS442754",null,"A <FLOATING TUBE SHEET> is a <TUBE SHEET> that can move inside a shell in order to allow thermal expansion.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TUBE SHEET",null,null,null,null,null,null,null,null,null,null,null,null,null,"STATIONARY TUBE SHEET",null,null,null,null,null,"rdl:RDS416114",null,"A <STATIONARY TUBE SHEET> is a <TUBE SHEET> that is held in a fixed position with respect to the vessel shell.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SUPPORT",null,null,null,null,null,null,null,null,null,null,null,"VALVE YOKE",null,null,null,null,null,"rdl:RDS415979",null,"A <VALVE YOKE> is an <ARTEFACT> and a <SUPPORT> for the valve operating mechanism on the bonnet assembly",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE YOKE",null,null,null,null,null,null,null,null,null,null,null,null,null,"ACTUATOR YOKE",null,null,null,null,null,"rdl:RDS7773326",null,"An <ACTUATOR YOKE> is a <VALVE YOKE> that supports the valve actuator on the bonnet assembly.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"VALVE YOKE",null,null,null,null,null,null,null,null,null,null,null,null,null,"GATE VALVE YOKE",null,null,null,null,null,"rdl:RDS866789",null,"A <GATE VALVE YOKE> is a <VALVE YOKE> by which the valve operator (actuator or hand wheel) is supported rigidly to the bonnet assembly of a gate valve.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]