{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["RDL browser","Settings","about","Results1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"RDL browser","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[[0,0,0,4]]}
["RDL2 browser to spreadsheet tool version 75",null,null,null,null,null,"Endpoint: http://data.15926.org/rdl/"]
["Contact: onno.paap@gmail.com",null,null,null,null,"Action","FIXED TRIP MECHANICAL SWITCHING DEVICE","http://data.15926.org/rdl/RDS935729"]
[null,null,null,null,null,"Action","POLE OF A SWITCHING DEVICE","http://data.15926.org/rdl/RDS954314"]
["Search:","SWITCHING DEVICE",null,null,null,"Action","RELEASER OF A MECHANICAL SWITCHING DEVICE","http://data.15926.org/rdl/RDS954899"]
[null,null,null,null,null,"Action","SEMICONDUCTOR SWITCHING DEVICE","http://data.15926.org/rdl/RDS934424"]
[null,null,null,null,null,"Action","SWITCHING DEVICE","http://data.15926.org/rdl/RDS934334"]
[null,null,null,null,null,"Action","TRIP-FREE MECHANICAL SWITCHING DEVICE","http://data.15926.org/rdl/RDS935774"]
[]
[]
[]
[]
[]
[null,"Note: first set coloring on in Settings"]
[null,"Coloring (containing this string will give this color)"]
[null,"ClassOfFunctionalObject"]
[null,"ClassOfInanimatePhysicalObject "]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Namespace replacer (definition containing this string replaces the namespace)"]
[null,"API","API:"]
[null,"ASME","ASME:"]
[null,"ASTM","ASTM:"]
[null,"DIN","DIN:"]
[null,"EN","EN:"]
[null,"ISO","ISO:"]
[null,"NORSOK","NOR:"]
[null,"NPD","NOR:"]
[null,"NS","NOR:"]
[null,"ROSEMOUNT","ROS:"]
[null,"SAE","SAE:"]
[null,"SIEMENS","SIE:"]
[null,"SKOTSELV","SKOT:"]
[null,"TWR","TWR:"]

{"sheet":"Settings","index":1,"n_rows":87,"n_cols":8,"rows_kept":87,"cut":false,"hidden":true,"merged":[]}
["Setting name","Select name","OnKey","Value","Status","RDLType"]
["Endpoint","RDL2 (15926.org)",null,"http://data.15926.org/rdl/","Current",null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA RDL",null,"http://data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA Staging",null,"http://staging.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA SVRDL",null,"http://svrdl.community.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P4",null,"http://posccaesar.org/p4/sparql",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","PCA P12",null,"http://sti.data.posccaesar.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","Localhost",null,"http://localhost:8890/sparql/",null,null,null,"Note: end address always with a slash (/)"]
[]
["gBaseNamespace",null,"http://data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://staging.data.posccaesar.org/rdl/","http://data.posccaesar.org/rdl/",null,"RDS2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://svrdl.community.data.posccaesar.org/rdl/","http://svrdl.community.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://posccaesar.org/p4/sparql","http://posccaesar.org/rdl/",null,"RDS"]
["gBaseNamespace",null,"http://sti.data.posccaesar.org/rdl/","http://sti.data.posccaesar.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://localhost:8890/sparql/","http://data.15926.org/rdl/",null,"RDL2"]
["gKeepSettings",null,null,"T"]
["gShowDeprecated",null,null,"F"]
["gColoring",null,null,"T"]
["gNamespaceReplacing",null,null,"F"]
["gHyperlinkReplacing",null,null,"F"]
[]
["Endpoint","aisi",null,"http://data.15926.org/aisi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ansi",null,"http://data.15926.org/ansi/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","api",null,"http://data.15926.org/api/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","all",null,"http://data.15926.org/all/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","asme",null,"http://data.15926.org/asme/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","astm",null,"http://data.15926.org/astm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","atex",null,"http://data.15926.org/atex/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","bs",null,"http://data.15926.org/bs/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","din",null,"http://data.15926.org/din/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dm",null,"http://data.15926.org/dm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","dnv",null,"http://data.15926.org/dnv/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","edm",null,"http://data.15926.org/edm/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","en",null,"http://data.15926.org/en/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","eu",null,"http://data.15926.org/eu/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iec",null,"http://data.15926.org/iec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","ieee",null,"http://data.15926.org/ieee/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","iso",null,"http://data.15926.org/iso/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","lci",null,"http://data.15926.org/lci/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","mss",null,"http://data.15926.org/mss/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nace",null,"http://data.15926.org/nace/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nec",null,"http://data.15926.org/nec/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nema",null,"http://data.15926.org/nema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nfpa",null,"http://data.15926.org/nfpa/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","nor",null,"http://data.15926.org/nor/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","rdl",null,"http://data.15926.org/rdl/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sae",null,"http://data.15926.org/sae/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","sie",null,"http://data.15926.org/sie/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","tema",null,"http://data.15926.org/tema/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","twr",null,"http://data.15926.org/twr/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","uns",null,"http://data.15926.org/uns/",null,null,null,"Note: end address always with a slash (/)"]
["Endpoint","wits",null,"http://data.15926.org/wits/",null,null,null,"Note: end address always with a slash (/)"]
[]
[]
["gBaseNamespace",null,"http://data.15926.org/aisi/","http://data.15926.org/aisi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ansi/","http://data.15926.org/ansi/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/api/","http://data.15926.org/api/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/asme/","http://data.15926.org/asme/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/all/","http://data.15926.org/all/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/astm/","http://data.15926.org/astm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/atex/","http://data.15926.org/atex/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/bs/","http://data.15926.org/bs/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/din/","http://data.15926.org/din/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dm/","http://data.15926.org/dm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/dnv/","http://data.15926.org/dnv/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/edm/","http://data.15926.org/edm/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/en/","http://data.15926.org/en/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/eu/","http://data.15926.org/eu/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iec/","http://data.15926.org/iec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/ieee/","http://data.15926.org/ieee/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/iso/","http://data.15926.org/iso/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/lci/","http://data.15926.org/lci/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/mss/","http://data.15926.org/mss/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nace/","http://data.15926.org/nace/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nec/","http://data.15926.org/nec/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nema/","http://data.15926.org/nema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nfpa/","http://data.15926.org/nfpa/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/nor/","http://data.15926.org/nor/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/rdl/","http://data.15926.org/rdl/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sae/","http://data.15926.org/sae/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/sie/","http://data.15926.org/sie/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/tema/","http://data.15926.org/tema/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/twr/","http://data.15926.org/twr/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/uns/","http://data.15926.org/uns/",null,"RDL2"]
["gBaseNamespace",null,"http://data.15926.org/wits/","http://data.15926.org/wits/",null,"RDL2"]
["                                          "]

{"sheet":"about","index":2,"n_rows":176,"n_cols":3,"rows_kept":176,"cut":false,"hidden":false,"merged":[]}
["Version 75 changes","2018-10-05","Onno Paap"]
["missing superclasses - and orphans- filter no deprecated classes"]
[]
["Version 74 changes","2018-09-30","Onno Paap"]
["Repaired bug missing label"]
[]
["Version 73 changes","2018-05-16","Onno Paap"]
["Repaired bug Deprecated Superclass"]
[]
[]
[]
["Version 71 changes","2016-07-17","Onno Paap"]
["Aded report button for comparison of RDL2 with a subfolder called views filled with spreadsheets."]
[]
[]
["Version 69 changes","2016-06-16","Onno Paap"]
["Added button: \"errors in definitions\" that lists all classes that have more or less \"<\" brackets than the number of super class relationships + 1. Where the part after the word \"that \"  is ignored in the count of \"<\" brackets."]
[]
["Version 68 changes","2016-06-13","Onno Paap"]
["Updated endpoint of RDL2 sparql "]
[]
["Version 67 changes","2016-05-22","Onno Paap"]
["Added button list subclasses from superclass "]
[]
["Version 65 changes","2016-04-25","Onno Paap"]
["Added checkbox at action dialog \"supress double child occurances\" so that this built-in feature can be switched off"]
[]
["Version 64 changes","2016-04-20","Onno Paap"]
["Made search case-insensitive and added endpoint \"all\""]
[]
["Version 63 changes","2016-09-28","Onno Paap"]
["Made entity list working on P4 endpoint (they changed the database version which was not accepting som sparql setting)"]
["Version 62 changes","2016-09-28","Onno Paap"]
["Applied show deprecated to searched result list"]
[]
["Version 61 changes","2016-08-29","Onno Paap"]
["Added query from pcardl for ClassOfIndirectProperty"]
[]
["Version 60 changes","2016-08-19","Onno Paap"]
["Repaired failing entity reports"]
[]
["Version 59 changes","2016-08-19","Onno Paap"]
["Missing superclasses now queries whole federation of RDL2"]
[]
["Version 58 changes","2016-08-16","Onno Paap"]
["Repaired missing output for entities and doubles in RDL2 endpoints other than rdl"]
[]
["Version 57 changes","2016-08-13","Onno Paap"]
["Doubles report now skips classes that are deprecated"]
[]
["Version 56 changes","2016-07-22","Onno Paap"]
["Made rowheight suitable for longer definitions to example DESIGN BASIS"]
[]
["Version 55 changes","2016-07-19","Onno Paap"]
["Made rowheight suitable for longer definitions"]
[]
["Version 54 changes","2016-07-03","Onno Paap"]
["Entity Type field changed to 6 merged cells."]
[]
["Version 53 changes","2016-06-23","Onno Paap"]
["added lci namespace"]
[]
["Version 52 changes","2016-06-23","Onno Paap"]
["Added deprecated count to list entities"]
[]
["Version 51 changes","2016-06-19","Onno Paap"]
["Updated namespaces of staging RDL"]
[]
["Version 50 changes","2016-06-19","Onno Paap"]
["taxonomy view repaired missing entity type"]
[]
["Version 49 changes","2016-06-14","Onno Paap"]
["Room for 12 superclasses"]
[]
["Version 48 changes","2016-06-14","Onno Paap"]
["Repaired NOR:/RDS  bug"]
[]
["Version 47 changes","2016-06-14","Onno Paap"]
["Repaired endpoint bug"]
[]
["Version 46 changes","2016-06-13","Onno Paap"]
["Updated endpoints"]
[]
["Version 45 changes","2016-06-06","Onno Paap"]
["Completed Missing Superclasses report"]
[]
["Version 44 changes","2016-05-20","Onno Paap"]
["Added Clear Cache button (use on any database changes)"]
[]
["Version 43 changes","2016-05-19","Onno Paap"]
["Changed non-existing super classes to show as \"no label\""]
[]
["Version 42 changes","2016-05-02","Onno Paap"]
["bug fix"]
[]
["Version 41 changes","2016-05-02","Onno Paap"]
["Added setting to show/not show deprecated items. If shown, they are stricken through"]
[]
["Version 40 changes","2016-03-31","Onno Paap"]
["Added  in doubles: two classes having the same label."]
[]
["Version 39 changes","2016-03-21","Onno Paap"]
["Made the query more robust, after the server hass been returning a 404 occasionally"]
[]
["Version 38 changes","2016-03-03","Onno Paap"]
["Repaired bug entity type query on PCA endpoint"]
[]
["Version 37 changes","2016-01-29","Onno Paap"]
["Showing deprecated class in taxonomy with label in strikethrough."]
[]
["Version 36 changes","2016-01-13","Onno Paap"]
["Added the 17 endpoints of http://data.15926.org/rdl"]
[]
["Version 35 changes","2016-01-13","Onno Paap"]
["In taxonomy view, disregard all rdf:type that is not data model.  So only show rdf:type that is dm:"]
[]
["Version 34 changes","2016-01-13","Onno Paap"]
["Solved taxonomy levels regression bug"]
[]
["Version 33 changes","2016-01-11","Onno Paap"]
["Enhanced the doubled query. First 4 columns are about the triple, the rest is info."]
[]
["Repaired bug in entity type query."]
[]
["Version 30 changes","2016-01-03","Onno Paap"]
["Repaired entity type query for old PCA RDL. \nRepaired bug in entity type query where a class that has a superclass of the wanted type as well as  of another type became  the start point of a new taxonomy as well as part in the main taxonomy. (read that again)"]
[]
["Version 29 changes","2016-01-02","Onno Paap"]
["Filtered entity filtered taxonomy to only show the filtered entity not subClassOf of another entity"]
[]
["Version 27 changes","2016-01-01","Onno Paap"]
["few bugs repaired.  Changed entity search into presenting taxonomies. "]
[]
["Version 26 changes","2015-12-26","Onno Paap"]
["few bugs repaired. "]
[]
["Version 25 changes","2015-12-26","Onno Paap"]
["Added Part 12 and localhost endpoints"]
["Added button for selecting double labels and definitions. "]
["Version 24 changes","2015-12-14","Onno Paap"]
["Added button to list all distinct entity data types and their counts, and click to show."]
["Added a button to show all orphans that have a rdfs:label"]
["Version 23 changes"]
["Added endpoint posccaesar.org/p4/sparql"]
["Version 22 changes"]
["Added endpoint staging.data.posccaesar.org/rdl"]
[]
["Version 21 changes"]
["Repaired bug where namespace replace was based upon definition instead of class label"]
[]
["Version 20 changes"]
["Repaired bug where definition did not show up if hyperlink replace was on."]
[]
["Version 19 changes (skip version 16-18)"]
["Settings expanded with persist settings, namespace replacer and hyperlink replacer"]
["Added namespace replacer which will replace the RDL: namespace of the ID with the namespace given in the list on the front page."]
["Added hyperlink replacer which will find terms between single quotes and look them up in the RDL, then add a hyperlink in the text if found. Anchor tag <a></a> used not &hyperlink() so looks ugly."]
[]
["Version 15 changes"]
["Changed browser page Action buttons to hyperlinks because buttons are not equally spaced between Excel versions (Office 2007 versus Office 365)"]
["First row is empty. Move all up."]
["Make stop button for during query taxonomy query execution"]
[]
[]
["Version 14 changes"]
["Aligned buttons on browser page"]
["Made color notification work. Note: switch it on first in settings. Default is off"]
["Top align subclasses in taxonomy"]
["Subclasses made to hyperlink in taxonomy"]
["Subclasses made to increase column width in taxonomy"]
["Made browser search go when hitting enter in search field"]
[]
[]
[]
["todo"]
["Make setting for outputting to other result pages"]

{"sheet":"Results1","index":3,"n_rows":175,"n_cols":35,"rows_kept":175,"cut":false,"hidden":false,"merged":[[174,21,174,22],[174,15,174,20],[174,23,174,28],[174,29,174,32],[172,22,172,23],[172,16,172,21],[172,24,172,29],[172,30,172,33],[173,22,173,23],[173,16,173,21],[173,24,173,29],[173,30,173,33],[170,22,170,23],[170,16,170,21],[170,24,170,29],[170,30,170,33],[171,22,171,23],[171,16,171,21],[171,24,171,29],[171,30,171,33],[168,21,168,22],[168,15,168,20],[168,23,168,28],[168,29,168,32],[169,22,169,23],[169,16,169,21],[169,24,169,29],[169,30,169,33],[166,22,166,23],[166,16,166,21],[166,24,166,29],[166,30,166,33],[167,21,167,22],[167,15,167,20],[167,23,167,28],[167,29,167,32],[164,22,164,23],[164,16,164,21],[164,24,164,29],[164,30,164,33],[165,22,165,23],[165,16,165,21],[165,24,165,29],[165,30,165,33],[162,22,162,23],[162,16,162,21],[162,24,162,29],[162,30,162,33],[163,22,163,23],[163,16,163,21],[163,24,163,29],[163,30,163,33],[160,21,160,22],[160,15,160,20],[160,23,160,28],[160,29,160,32],[161,21,161,22],[161,15,161,20],[161,23,161,28],[161,29,161,32],[158,22,158,23],[158,16,158,21],[158,24,158,29],[158,30,158,33],[159,21,159,22],[159,15,159,20],[159,23,159,28],[159,29,159,32],[156,21,156,22],[156,15,156,20],[156,23,156,28],[156,29,156,32],[157,22,157,23],[157,16,157,21],[157,24,157,29],[157,30,157,33],[154,22,154,23],[154,16,154,21],[154,24,154,29],[154,30,154,33],[155,21,155,22],[155,15,155,20],[155,23,155,28],[155,29,155,32],[152,22,152,23],[152,16,152,21],[152,24,152,29],[152,30,152,33],[153,22,153,23],[153,16,153,21],[153,24,153,29],[153,30,153,33],[150,24,150,25],[150,18,150,23],[150,26,150,31],[150,32,150,35],[151,24,151,25],[151,18,151,23],[151,26,151,31],[151,32,151,35],[148,23,148,24],[148,17,148,22],[148,25,148,30],[148,31,148,34],[149,23,149,24],[149,17,149,22],[149,25,149,30],[149,31,149,34],[146,23,146,24],[146,17,146,22],[146,25,146,30],[146,31,146,34],[147,23,147,24],[147,17,147,22],[147,25,147,30],[147,31,147,34],[144,23,144,24],[144,17,144,22],[144,25,144,30],[144,31,144,34],[145,23,145,24],[145,17,145,22],[145,25,145,30],[145,31,145,34],[142,26,142,27],[142,20,142,25],[142,28,142,33],[142,34,142,37],[143,25,143,26],[143,19,143,24],[143,27,143,32],[143,33,143,36],[140,24,140,25],[140,18,140,23],[140,26,140,31],[140,32,140,35],[141,25,141,26],[141,19,141,24],[141,27,141,32],[141,33,141,36],[138,25,138,26],[138,19,138,24],[138,27,138,32],[138,33,138,36],[139,24,139,25],[139,18,139,23],[139,26,139,31],[139,32,139,35],[136,23,136,24],[136,17,136,22],[136,25,136,30],[136,31,136,34],[137,24,137,25],[137,18,137,23],[137,26,137,31],[137,32,137,35],[134,24,134,25],[134,18,134,23],[134,26,134,31],[134,32,134,35],[135,23,135,24],[135,17,135,22],[135,25,135,30],[135,31,135,34],[132,23,132,24],[132,17,132,22],[132,25,132,30],[132,31,132,34],[133,24,133,25],[133,18,133,23],[133,26,133,31],[133,32,133,35],[130,25,130,26],[130,19,130,24],[130,27,130,32],[130,33,130,36],[131,23,131,24],[131,17,131,22],[131,25,131,30],[131,31,131,34],[128,24,128,25],[128,18,128,23],[128,26,128,31],[128,32,128,35],[129,25,129,26],[129,19,129,24],[129,27,129,32],[129,33,129,36],[126,24,126,25],[126,18,126,23],[126,26,126,31],[126,32,126,35],[127,24,127,25],[127,18,127,23],[127,26,127,31],[127,32,127,35],[124,23,124,24],[124,17,124,22],[124,25,124,30],[124,31,124,34],[125,23,125,24],[125,17,125,22],[125,25,125,30],[125,31,125,34],[122,22,122,23],[122,16,122,21],[122,24,122,29],[122,30,122,33],[123,23,123,24],[123,17,123,22],[123,25,123,30],[123,31,123,34],[120,22,120,23],[120,16,120,21],[120,24,120,29],[120,30,120,33],[121,22,121,23],[121,16,121,21],[121,24,121,29],[121,30,121,33],[118,22,118,23],[118,16,118,21],[118,24,118,29],[118,30,118,33],[119,21,119,22],[119,15,119,20],[119,23,119,28],[119,29,119,32],[116,24,116,25],[116,18,116,23],[116,26,116,31],[116,32,116,35],[117,22,117,23],[117,16,117,21],[117,24,117,29],[117,30,117,33],[114,25,114,26],[114,19,114,24],[114,27,114,32],[114,33,114,36],[115,24,115,25],[115,18,115,23],[115,26,115,31],[115,32,115,35],[112,24,112,25],[112,18,112,23],[112,26,112,31],[112,32,112,35],[113,25,113,26],[113,19,113,24],[113,27,113,32],[113,33,113,36],[110,22,110,23],[110,16,110,21],[110,24,110,29],[110,30,110,33],[111,23,111,24],[111,17,111,22],[111,25,111,30],[111,31,111,34],[108,22,108,23],[108,16,108,21],[108,24,108,29],[108,30,108,33],[109,22,109,23],[109,16,109,21],[109,24,109,29],[109,30,109,33],[106,23,106,24],[106,17,106,22],[106,25,106,30],[106,31,106,34],[107,23,107,24],[107,17,107,22],[107,25,107,30],[107,31,107,34],[104,22,104,23],[104,16,104,21],[104,24,104,29],[104,30,104,33],[105,23,105,24],[105,17,105,22],[105,25,105,30],[105,31,105,34],[102,22,102,23],[102,16,102,21],[102,24,102,29],[102,30,102,33],[103,22,103,23],[103,16,103,21],[103,24,103,29],[103,30,103,33],[100,21,100,22],[100,15,100,20],[100,23,100,28],[100,29,100,32],[101,22,101,23],[101,16,101,21],[101,24,101,29],[101,30,101,33],[98,22,98,23],[98,16,98,21],[98,24,98,29],[98,30,98,33],[99,21,99,22],[99,15,99,20],[99,23,99,28],[99,29,99,32],[96,23,96,24],[96,17,96,22],[96,25,96,30],[96,31,96,34],[97,23,97,24],[97,17,97,22],[97,25,97,30],[97,31,97,34],[94,22,94,23],[94,16,94,21],[94,24,94,29],[94,30,94,33],[95,22,95,23],[95,16,95,21],[95,24,95,29],[95,30,95,33],[92,23,92,24],[92,17,92,22],[92,25,92,30],[92,31,92,34],[93,22,93,23],[93,16,93,21],[93,24,93,29],[93,30,93,33],[90,23,90,24],[90,17,90,22],[90,25,90,30],[90,31,90,34],[91,23,91,24],[91,17,91,22],[91,25,91,30],[91,31,91,34],[88,23,88,24],[88,17,88,22],[88,25,88,30],[88,31,88,34],[89,23,89,24],[89,17,89,22],[89,25,89,30],[89,31,89,34],[86,23,86,24],[86,17,86,22],[86,25,86,30],[86,31,86,34],[87,23,87,24],[87,17,87,22],[87,25,87,30],[87,31,87,34],[84,23,84,24],[84,17,84,22],[84,25,84,30],[84,31,84,34],[85,23,85,24],[85,17,85,22],[85,25,85,30],[85,31,85,34],[82,22,82,23],[82,16,82,21],[82,24,82,29],[82,30,82,33],[83,23,83,24],[83,17,83,22],[83,25,83,30],[83,31,83,34],[80,22,80,23],[80,16,80,21],[80,24,80,29],[80,30,80,33],[81,22,81,23],[81,16,81,21],[81,24,81,29],[81,30,81,33],[78,21,78,22],[78,15,78,20],[78,23,78,28],[78,29,78,32],[79,22,79,23],[79,16,79,21],[79,24,79,29],[79,30,79,33],[76,21,76,22],[76,15,76,20],[76,23,76,28],[76,29,76,32],[77,21,77,22],[77,15,77,20],[77,23,77,28],[77,29,77,32],[74,21,74,22],[74,15,74,20],[74,23,74,28],[74,29,74,32],[75,21,75,22],[75,15,75,20],[75,23,75,28],[75,29,75,32],[72,22,72,23],[72,16,72,21],[72,24,72,29],[72,30,72,33],[73,22,73,23],[73,16,73,21],[73,24,73,29],[73,30,73,33],[70,22,70,23],[70,16,70,21],[70,24,70,29],[70,30,70,33],[71,22,71,23],[71,16,71,21],[71,24,71,29],[71,30,71,33],[68,22,68,23],[68,16,68,21],[68,24,68,29],[68,30,68,33],[69,22,69,23],[69,16,69,21],[69,24,69,29],[69,30,69,33],[66,21,66,22],[66,15,66,20],[66,23,66,28],[66,29,66,32],[67,21,67,22],[67,15,67,20],[67,23,67,28],[67,29,67,32],[64,22,64,23],[64,16,64,21],[64,24,64,29],[64,30,64,33],[65,21,65,22],[65,15,65,20],[65,23,65,28],[65,29,65,32],[62,23,62,24],[62,17,62,22],[62,25,62,30],[62,31,62,34],[63,22,63,23],[63,16,63,21],[63,24,63,29],[63,30,63,33],[60,22,60,23],[60,16,60,21],[60,24,60,29],[60,30,60,33],[61,22,61,23],[61,16,61,21],[61,24,61,29],[61,30,61,33],[58,22,58,23],[58,16,58,21],[58,24,58,29],[58,30,58,33],[59,22,59,23],[59,16,59,21],[59,24,59,29],[59,30,59,33],[56,21,56,22],[56,15,56,20],[56,23,56,28],[56,29,56,32],[57,22,57,23],[57,16,57,21],[57,24,57,29],[57,30,57,33],[54,23,54,24],[54,17,54,22],[54,25,54,30],[54,31,54,34],[55,23,55,24],[55,17,55,22],[55,25,55,30],[55,31,55,34],[52,22,52,23],[52,16,52,21],[52,24,52,29],[52,30,52,33],[53,22,53,23],[53,16,53,21],[53,24,53,29],[53,30,53,33],[50,23,50,24],[50,17,50,22],[50,25,50,30],[50,31,50,34],[51,22,51,23],[51,16,51,21],[51,24,51,29],[51,30,51,33],[48,23,48,24],[48,17,48,22],[48,25,48,30],[48,31,48,34],[49,23,49,24],[49,17,49,22],[49,25,49,30],[49,31,49,34],[46,23,46,24],[46,17,46,22],[46,25,46,30],[46,31,46,34],[47,23,47,24],[47,17,47,22],[47,25,47,30],[47,31,47,34],[44,23,44,24],[44,17,44,22],[44,25,44,30],[44,31,44,34],[45,23,45,24],[45,17,45,22],[45,25,45,30],[45,31,45,34],[42,24,42,25],[42,18,42,23],[42,26,42,31],[42,32,42,35],[43,22,43,23],[43,16,43,21],[43,24,43,29],[43,30,43,33],[40,24,40,25],[40,18,40,23],[40,26,40,31],[40,32,40,35],[41,24,41,25],[41,18,41,23],[41,26,41,31],[41,32,41,35],[38,24,38,25],[38,18,38,23],[38,26,38,31],[38,32,38,35],[39,24,39,25],[39,18,39,23],[39,26,39,31],[39,32,39,35],[36,23,36,24],[36,17,36,22],[36,25,36,30],[36,31,36,34],[37,24,37,25],[37,18,37,23],[37,26,37,31],[37,32,37,35],[34,23,34,24],[34,17,34,22],[34,25,34,30],[34,31,34,34],[35,22,35,23],[35,16,35,21],[35,24,35,29],[35,30,35,33],[32,21,32,22],[32,15,32,20],[32,23,32,28],[32,29,32,32],[33,22,33,23],[33,16,33,21],[33,24,33,29],[33,30,33,33],[30,22,30,23],[30,16,30,21],[30,24,30,29],[30,30,30,33],[31,22,31,23],[31,16,31,21],[31,24,31,29],[31,30,31,33],[28,23,28,24],[28,17,28,22],[28,25,28,30],[28,31,28,34],[29,23,29,24],[29,17,29,22],[29,25,29,30],[29,31,29,34],[26,22,26,23],[26,16,26,21],[26,24,26,29],[26,30,26,33],[27,22,27,23],[27,16,27,21],[27,24,27,29],[27,30,27,33],[24,22,24,23],[24,16,24,21],[24,24,24,29],[24,30,24,33],[25,21,25,22],[25,15,25,20],[25,23,25,28],[25,29,25,32],[22,22,22,23],[22,16,22,21],[22,24,22,29],[22,30,22,33],[23,22,23,23],[23,16,23,21],[23,24,23,29],[23,30,23,33],[20,22,20,23],[20,16,20,21],[20,24,20,29],[20,30,20,33],[21,22,21,23],[21,16,21,21],[21,24,21,29],[21,30,21,33],[18,22,18,23],[18,16,18,21],[18,24,18,29],[18,30,18,33],[19,23,19,24],[19,17,19,22],[19,25,19,30],[19,31,19,34],[16,22,16,23],[16,16,16,21],[16,24,16,29],[16,30,16,33],[17,22,17,23],[17,16,17,21],[17,24,17,29],[17,30,17,33],[14,23,14,24],[14,17,14,22],[14,25,14,30],[14,31,14,34],[15,22,15,23],[15,16,15,21],[15,24,15,29],[15,30,15,33],[12,24,12,25],[12,18,12,23],[12,26,12,31],[12,32,12,35],[13,23,13,24],[13,17,13,22],[13,25,13,30],[13,31,13,34],[10,22,10,23],[10,16,10,21],[10,24,10,29],[10,30,10,33],[11,23,11,24],[11,17,11,22],[11,25,11,30],[11,31,11,34],[8,24,8,25],[8,18,8,23],[8,26,8,31],[8,32,8,35],[9,21,9,22],[9,15,9,20],[9,23,9,28],[9,29,9,32],[6,23,6,24],[6,17,6,22],[6,25,6,30],[6,31,6,34],[7,23,7,24],[7,17,7,22],[7,25,7,30],[7,31,7,34],[4,23,4,24],[4,17,4,22],[4,25,4,30],[4,31,4,34],[5,23,5,24],[5,17,5,22],[5,25,5,30],[5,31,5,34],[2,22,2,23],[2,16,2,21],[2,24,2,29],[2,30,2,33],[3,22,3,23],[3,16,3,21],[3,24,3,29],[3,30,3,33],[0,20,0,21],[0,14,0,19],[0,22,0,27],[0,28,0,31],[1,21,1,22],[1,15,1,20],[1,23,1,28],[1,29,1,32]]}
[null,null,"FunctionalObject",null,null,null,null,null,null,null,null,null,null,null,"SWITCHING DEVICE",null,null,null,null,null,"rdl:RDS934334",null,"A <SWITCHING DEVICE> is a <FunctionalObject> that has the capability of <SWITCHING>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"AUTOMATIC SWITCHING EQUIPMENT",null,null,null,null,null,"rdl:RDS1026134",null,"An <AUTOMATIC SWITCHING EQUIPMENT> is an <ARTEFACT> and a <SWITCHING DEVICE> that is automatic and designed to initiate the operation of circuit breakers and/or disconnectors in a substation according to a specific programme",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AUTOMATIC SWITCHING EQUIPMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,"AUTOMATIC LOAD RESTORATION EQUIPMENT",null,null,null,null,null,"rdl:RDS1026494",null,"An <AUTOMATIC LOAD RESTORATION EQUIPMENT> is an <AUTOMATIC SWITCHING EQUIPMENT> intended to initiate reclosing of circuit-breakers automatically after tripping due to a load shedding operation",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AUTOMATIC SWITCHING EQUIPMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,"AUTOMATIC RECLOSING EQUIPMENT",null,null,null,null,null,"rdl:RDS1026179",null,"An <AUTOMATIC RECLOSING EQUIPMENT> is an <AUTOMATIC SWITCHING EQUIPMENT> which is designed to initiate the reclosing of circuit-breaker(s) after operation of the protection on the associated circuit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AUTOMATIC RECLOSING EQUIPMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AUTOMATIC RESTORATION EQUIPMENT",null,null,null,null,null,"rdl:RDS1026449",null,"An <AUTOMATIC RESTORATION EQUIPMENT> is an <AUTOMATIC RECLOSING EQUIPMENT> intended to initiate the scheduled, sequential and delayed automatic reconnection of circuit-breakers or other specific switching devices.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AUTOMATIC RECLOSING EQUIPMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MULTIPLE-SHOT RECLOSING EQUIPMENT",null,null,null,null,null,"rdl:RDS1026359",null,"A <MULTIPLE-SHOT RECLOSING EQUIPMENT> is an <AUTOMATIC RECLOSING EQUIPMENT> repeated two or three times (usually not more) if unsuccessful.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AUTOMATIC RECLOSING EQUIPMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SINGLE-POLE RECLOSING EQUIPMENT",null,null,null,null,null,"rdl:RDS1026224",null,"A <SINGLE-POLE RECLOSING EQUIPMENT> is an <AUTOMATIC RECLOSING EQUIPMENT> intended to reclose one pole of a circuit-breaker following a single-phase power system fault.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AUTOMATIC RECLOSING EQUIPMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE-POLE RECLOSING EQUIPMENT",null,null,null,null,null,"rdl:RDS1026269",null,"A <THREE-POLE RECLOSING EQUIPMENT> is an <AUTOMATIC RECLOSING EQUIPMENT> intended to reclose three poles of a circuit-breaker following power system fault.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THREE-POLE RECLOSING EQUIPMENT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THREE-POLE RECLOSING EQUIPMENT WITH SYNCHROCHECK",null,null,null,null,null,"rdl:RDS1026404",null,"A <THREE-POLE RECLOSING EQUIPMENT WITH SYNCHROCHECK> is a <THREE-POLE RECLOSING EQUIPMENT> with a check on voltage, frequency difference, and phase angle before closing the circuit-breaker.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS463994",null,"A <CIRCUIT BREAKER> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE> that at regular intervals interrupts an electric current",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876239",null,"An <AIR CIRCUIT BREAKER> is a <CIRCUIT BREAKER> in which the contacts open and close in air at atmospheric pressure.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AIR CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTH LEAKAGE CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876509",null,"An <EARTH LEAKAGE CIRCUIT BREAKER> is an <AIR CIRCUIT BREAKER> intended to break the supply in the event of an earth fault being detected.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EARTH LEAKAGE CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RESIDUAL CURRENT CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876644",null,"A <RESIDUAL CURRENT CIRCUIT BREAKER> is an <EARTH LEAKAGE CIRCUIT BREAKER> in which the earth fault is detected by an imbalance in the current in the phase and neutral conductors.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AIR CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MINIATURE CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876554",null,"A <MINIATURE CIRCUIT BREAKER> is an <AIR CIRCUIT BREAKER> intended for low power low voltage installations.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"AIR CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOULDED-CASE CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876599",null,"An <MOULDED-CASE CIRCUIT BREAKER> is an <AIR CIRCUIT BREAKER> having a supporting housing of moulded insulating material forming an integral part of the <CIRCUIT BREAKER>.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,"CIRCUIT BREAKER WITH LOCK-OUT PREVENTING CLOSING",null,null,null,null,null,"rdl:RDS913814",null,"A <CIRCUIT BREAKER WITH LOCK-OUT PREVENTING CLOSING> is a <CIRCUIT BREAKER> in which none of the moving contacts can make current if the closing command is initiated while the conditions which should cause the opening operation remain established.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,"CURRENT-LIMITING CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS913724",null,"A <CURRENT-LIMITING CIRCUIT BREAKER> is a <CIRCUIT BREAKER> with a break-time short enough to prevent the short circuit current reaching its otherwise attainable peak value.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,"DEAD TANK CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS913679",null,"A <DEAD TANK CIRCUIT BREAKER> is a <CIRCUIT BREAKER> with interrupters in an earthed metal tank.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,"GAS-BLAST CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS913544",null,"A <GAS-BLAST CIRCUIT BREAKER> is a <CIRCUIT BREAKER> in which the arc develops in a blast of gas.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"GAS-BLAST CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR-BLAST CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876284",null,"An <AIR-BLAST CIRCUIT BREAKER> is a <GAS-BLAST CIRCUIT BREAKER> in which the gas used is air.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,"INTEGRALLY FUSED CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS913769",null,"An <INTEGRALLY FUSED CIRCUIT BREAKER> is a <CIRCUIT BREAKER> that is a combination, in a single device, of A <CIRCUIT BREAKER> and fuses, one fuse being placed in series with each pole of the circuit breaker intended to be connected to a phase conductor.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,"LIVE TANK CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS913634",null,"A <LIVE TANK CIRCUIT BREAKER> is a <CIRCUIT BREAKER> with interrupters in a tank insulated from earth.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,"OIL CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876329",null,"An <OIL CIRCUIT BREAKER> is a <CIRCUIT BREAKER> in which the contacts open and close in oil.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,"SF6 CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876419",null,"An <SF6 CIRCUIT BREAKER> is a <CIRCUIT BREAKER> in which the contacts open and close in sulphur hexafluoride.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CIRCUIT BREAKER",null,null,null,null,null,null,null,null,null,null,null,null,null,"VACUUM CIRCUIT BREAKER",null,null,null,null,null,"rdl:RDS876464",null,"A <VACUUM CIRCUIT BREAKER> is a <CIRCUIT BREAKER> in which the contacts open and close within a highly evacuated envelope.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"CONTACTOR",null,null,null,null,null,"rdl:RDS464039",null,"A <CONTACTOR> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE> having only one position of rest, operated otherwise than by hand, capable of making, carrying and breaking currents under normal circuit conditions including operating overload conditions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTACTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR CONTACTOR",null,null,null,null,null,"rdl:RDS876734",null,"An <AIR CONTACTOR> is a <CONTACTOR> that has its contacts in air.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","CONTACTOR","RELAY",null,null,null,null,null,null,null,null,null,null,null,"CONTACTOR RELAY",null,null,null,null,null,"rdl:RDS935189",null,"A <CONTACTOR RELAY> is an <ARTEFACT> and a <RELAY> and a <CONTACTOR>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTACTOR RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTANTANEOUS CONTACTOR RELAY",null,null,null,null,null,"rdl:RDS935234",null,"An <INSTANTANEOUS CONTACTOR RELAY> is a <CONTACTOR RELAY> operating without any intentional time delay.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTACTOR RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TIME-DELAY CONTACTOR RELAY",null,null,null,null,null,"rdl:RDS935279",null,"A <TIME-DELAY CONTACTOR RELAY> is a <CONTACTOR RELAY> with specified time-delay characteristics.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTACTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"LATCHED CONTACTOR",null,null,null,null,null,"rdl:RDS935144",null,"A <LATCHED CONTACTOR> is a <CONTACTOR>, the moving elements of which are prevented by means of a latching arrangement from returning to the position of rest when the operating means are de-energized.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTACTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"VACUUM CONTACTOR",null,null,null,null,null,"rdl:RDS876779",null,"A <VACUUM CONTACTOR> is a <CONTACTOR> that make/break electrical contacts inside a sealed vacuum interrupter called a vacuum bottle.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"CONTROL SWITCH",null,null,null,null,null,"rdl:RDS935459",null,"A <CONTROL SWITCH> is an <ARTEFACT> and a <SWITCHING DEVICE> that serves the purpose of controlling the operation of switchgear or controlgear, including signalling, electrical interlocking, etc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"DISCREPANCY SWITCH",null,null,null,null,null,"rdl:RDS1006019",null,"A <DISCREPANCY SWITCH> is a <CONTROL SWITCH> that is a switched indicator, with an acknowledgement facility, which shows any discrepancy between the actual and indicated state of the equipment being monitored.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCREPANCY SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONTROL DISCREPANCY SWITCH",null,null,null,null,null,"rdl:RDS1006064",null,"A <CONTROL DISCREPANCY SWITCH> is a <DISCREPANCY SWITCH> incorporating a control function.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"HYDRAULIC SWITCH",null,null,null,null,null,"rdl:RDS6452046",null,"A <HYDRAULIC SWITCH> is a <CONTROL SWITCH> intended to switch one or more hydraulic signals",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HYDRAULIC SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT MANIFOLD",null,null,null,null,null,"rdl:RDS2223280",null,"An <INSTRUMENT MANIFOLD> is a <HYDRAULIC SWITCH> that combines one or more block/isolate valves and one or more bleed/vent valves into one component for the interface between a process fluid and an instrument",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT MANIFOLD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW MANIFOLD",null,null,null,null,null,"rdl:RDS2222917",null,"A <FLOW MANIFOLD> is an <INSTRUMENT MANIFOLD> that is is suitable for all types of differential pressure instruments, , enabling isolation, calibration and venting in a single unit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT MANIFOLD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT MANIFOLD - 2-VALVE",null,null,null,null,null,"rdl:RDS2223282",null,"An <INSTRUMENT MANIFOLD - 2-VALVE> is an <INSTRUMENT MANIFOLD> with 2 valves",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT MANIFOLD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT MANIFOLD - 3-VALVE",null,null,null,null,null,"rdl:RDS2223283",null,"An <INSTRUMENT MANIFOLD - 3-VALVE> is an <INSTRUMENT MANIFOLD> with 3 valves",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT MANIFOLD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT MANIFOLD - 5-VALVE",null,null,null,null,null,"rdl:RDS2223285",null,"An <INSTRUMENT MANIFOLD - 5-VALVE> is an <INSTRUMENT MANIFOLD> with 5 valves",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT MANIFOLD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT MANIFOLD - DIRECT MOUNT",null,null,null,null,null,"rdl:RDS2223286",null,"An <INSTRUMENT MANIFOLD - DIRECT MOUNT> is an <INSTRUMENT MANIFOLD> that is directly mounted on the instrument involved",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENT MANIFOLD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INSTRUMENT MANIFOLD - REMOTE MOUNT",null,null,null,null,null,"rdl:RDS2223287",null,"An <INSTRUMENT MANIFOLD - REMOTE MOUNT> is an <INSTRUMENT MANIFOLD> that is remotely mounted from the instrument involved",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"PILOT SWITCH",null,null,null,null,null,"rdl:RDS935549",null,"A <PILOT SWITCH> is a <CONTROL SWITCH> actuated in response to specified conditions of an actuating quantity.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PILOT SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AUTOMATIC RESET SWITCH",null,null,null,null,null,"rdl:RDS7457204",null,"An <AUTOMATIC RESET SWITCH> is a <PILOT SWITCH> of which the resetting is automatic.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PILOT SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL PRESSURE SWITCH",null,null,null,null,null,"rdl:RDS850949",null,"A <DIFFERENTIAL PRESSURE SWITCH> is a <PILOT SWITCH> intended to switch or give an on/off signal when the measured differential pressure has reached a preset value.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PILOT SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIFFERENTIAL TEMPERATURE SWITCH",null,null,null,null,null,"rdl:RDS879434",null,"A <DIFFERENTIAL TEMPERATURE SWITCH> is a <PILOT SWITCH> that is intended to measure and indicate and/or produce a signal which represents the measured differential temperature.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PILOT SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MANUAL RESET SWITCH",null,null,null,null,null,"rdl:RDS7457266",null,"A <MANUAL RESET SWITCH> is a <PILOT SWITCH> of which the resetting is manually operated.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PILOT SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MICRO SWITCH",null,null,null,null,null,"rdl:RDS5779175",null,"A <MICRO SWITCH> is a <PILOT SWITCH> operated by very small movements of a lever, the circuit being made or broken or closed by spring-loaded contacts.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PILOT SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RADIOACTIVE SWITCH",null,null,null,null,null,"rdl:RDS7022455",null,"A <RADIOACTIVE SWITCH> is a <PILOT SWITCH> that uses absorption of gamma radiation from a radioactive isotope to monitor e.g. an area.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PILOT SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TRIP AMPLIFIER",null,null,null,null,null,"rdl:RDS6452934",null,"A <TRIP AMPLIFIER> is a <PILOT SWITCH> intended to create a switch action at a preset value.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SWITCH","PNEUMATIC APPARATUS",null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC SWITCH",null,null,null,null,null,"rdl:RDS5779085",null,"A <PNEUMATIC SWITCH> is a <CONTROL SWITCH> and a <PNEUMATIC APPARATUS>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"SENSITIVE SWITCH",null,null,null,null,null,"rdl:RDS964484",null,"A <SENSITIVE SWITCH> is a <CONTROL SWITCH> having a snap-action, micro-gap, mechanism which is operated directly by a defined force through a defined travel.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMAL TIME DELAY SWITCH",null,null,null,null,null,"rdl:RDS964529",null,"A <THERMAL TIME DELAY SWITCH> is a <CONTROL SWITCH> whose contacts control a load circuit and are delayed from operating for a predetermined time interval.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMAL TIME DELAY SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE COMPENSATED THERMAL TIME DELAY SWITCH",null,null,null,null,null,"rdl:RDS964574",null,"A <TEMPERATURE COMPENSATED THERMAL TIME DELAY SWITCH> is a <THERMAL TIME DELAY SWITCH> in which the time delay is substantially independent of changes in ambient temperature.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMAL TIME DELAY SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VARIABLE THERMAL TIME DELAY SWITCH",null,null,null,null,null,"rdl:RDS964619",null,"A <VARIABLE THERMAL TIME DELAY SWITCH> is a <THERMAL TIME DELAY SWITCH> in which the time delay is variable within predetermined intervals.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"DISCONNECTOR",null,null,null,null,null,"rdl:RDS934559",null,"A <DISCONNECTOR> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE> that provides, in the open position, an isolating distance in accordance with specified requirements",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"CENTRE-BREAK DISCONNECTOR",null,null,null,null,null,"rdl:RDS934694",null,"A <CENTRE-BREAK DISCONNECTOR> is a <DISCONNECTOR> in which both contacts of each pole are movable and engage at a point substantially midway between their supports.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"DISCONNECTOR FUSE",null,null,null,null,null,"rdl:RDS934919",null,"A <DISCONNECTOR FUSE> is a <DISCONNECTOR> in which one or more poles have a fuse in series in a composite unit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"DIVIDED SUPPORT DISCONNECTOR",null,null,null,null,null,"rdl:RDS934604",null,"A <DIVIDED SUPPORT DISCONNECTOR> is a <DISCONNECTOR> in which the fixed and moving contacts of each pole are not supported by a common base or frame.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"DOUBLE-BREAK DISCONNECTOR",null,null,null,null,null,"rdl:RDS934739",null,"A <DOUBLE-BREAK DISCONNECTOR> is a <DISCONNECTOR> that opens a circuit at two points.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"EARTHING SWITCH",null,null,null,null,null,"rdl:RDS876869",null,"An <EARTHING SWITCH> is a <DISCONNECTOR> for earthing parts of a circuit, capable of withstanding for a specified time currents under abnormal conditions such as those of short circuit, but not required to carry current under normal conditions of the circuit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"EARTHING SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIVIDED SUPPORT EARTHING SWITCH",null,null,null,null,null,"rdl:RDS934649",null,"A <DIVIDED SUPPORT EARTHING SWITCH> is an <EARTHING SWITCH> in which the fixed and moving contacts of each pole are not supported by a common base or frame.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"FUSE-DISCONNECTOR",null,null,null,null,null,"rdl:RDS935054",null,"A <FUSE-DISCONNECTOR> is a <DISCONNECTOR> in which a fuse-link or a fuse-carrier with fuse-link forms the moving contact.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"MAGNETIC DOOR CLOSER RELEASE",null,null,null,null,null,"rdl:RDS1299240441",null,"A <MAGNETIC DOOR CLOSER RELEASE> is a <DISCONNECTOR> that switches off the current to a magnetic door shutter so that the door closes",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"EARTH FAULT SWITCH",null,null,null,null,null,"rdl:RDS5779023",null,"An <EARTH FAULT SWITCH> is an <ARTEFACT> and a <SWITCHING DEVICE> which operates after an accidental connection between a live part of an electrical system and earth",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL BREAKER",null,null,null,null,null,"rdl:RDS5762815",null,"An <ELECTRICAL BREAKER> is an <ARTEFACT> and a <SWITCHING DEVICE> that is an automatically operated electrical switch designed to protect an electrical circuit from damage caused by excess current, typically resulting from an overload or short circuit. Its basic function is to interrupt current flow after a fault is detected",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL SWITCH",null,null,null,null,null,"rdl:RDS316394",null,"An <ELECTRICAL SWITCH> is an <ARTEFACT> and a <SWITCHING DEVICE> that turns electrical current on and/or off",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"DPCO SWITCH",null,null,null,null,null,"rdl:RDS1472121461",null,"A <DPCO SWITCH> is an <ELECTRICAL SWITCH> that is a Double Pole ChangeOver or Double Pole, Centre Off switch, i.e. a changeover switch equivalent to DPDT switches.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"DPDT SWITCH",null,null,null,null,null,"rdl:RDS1472119881",null,"A <DPDT SWITCH> is an <ELECTRICAL SWITCH> that is a Double Pole, Double Throw switch, i.e. a simple changeover switch equivalent to two SPDT switches controlled by a single mechanism: A is connected to B and D to E, or A is connected to C and D to F.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"DPST SWITCH",null,null,null,null,null,"rdl:RDS1472118481",null,"A <DPST SWITCH> is an <ELECTRICAL SWITCH> that is a Double Pole, Single Throw switch, i.e. a simple changeover switch equivalent to two SPST switches controlled by a single mechanism.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"SPCO SWITCH",null,null,null,null,null,"rdl:RDS1472116611",null,"An <SPCO SWITCH> is an <ELECTRICAL SWITCH> that is a Single Pole ChangeOver switch, i.e. a simple changeover switch.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"SPDT SWITCH",null,null,null,null,null,"rdl:RDS1472069631",null,"An <SPDT SWITCH> is an <ELECTRICAL SWITCH> that is a Single Pole, Double Throw switch, i.e. a simple changeover switch: C (COM, Common) is connected to L1 or to L2.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"SPST SWITCH",null,null,null,null,null,"rdl:RDS1472066441",null,"An <SPST SWITCH> is an <ELECTRICAL SWITCH> that is a single pole, single throw switch, i.e. the two terminals are either connected together or disconnected from each other.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"FIXED TRIP MECHANICAL SWITCHING DEVICE",null,null,null,null,null,"rdl:RDS935729",null,"A <FIXED TRIP MECHANICAL SWITCHING DEVICE> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE> that cannot be released except when it is in the closed position",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"FUSE-COMBINATION UNIT",null,null,null,null,null,"rdl:RDS934514",null,"A <FUSE-COMBINATION UNIT> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE> and one or more fuses in a composite unit, assembled by the manufacturer or in accordance with his instructions",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"FUSE-SWITCH",null,null,null,null,null,"rdl:RDS935009",null,"A <FUSE-SWITCH> is an <ARTEFACT> and a <SWITCHING DEVICE> in which a fuse-link or a fuse-carrier with fuse-link forms the moving contact",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"GAS EVOLVING SWITCH",null,null,null,null,null,"rdl:RDS934829",null,"A <GAS EVOLVING SWITCH> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE> in which the gas is evolved and moved by the thermal action of the arc",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"HUMAN-OPERATED SWITCH",null,null,null,null,null,"rdl:RDS880919",null,"A <HUMAN-OPERATED SWITCH> is an <ARTEFACT> and a <SWITCHING DEVICE> that is operated by a person",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HUMAN-OPERATED SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"CHANGE-OVER SWITCH",null,null,null,null,null,"rdl:RDS966599",null,"A <CHANGE-OVER SWITCH> is a <HUMAN-OPERATED SWITCH> for changing the connections from one set of its terminals to another.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HUMAN-OPERATED SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"FOOT SWITCH",null,null,null,null,null,"rdl:RDS935639",null,"A <FOOT SWITCH> is a <HUMAN-OPERATED SWITCH> having an actuator intended to be operated by foot.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HUMAN-OPERATED SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"KEY SWITCH",null,null,null,null,null,"rdl:RDS5779130",null,"A <KEY SWITCH> is a <HUMAN-OPERATED SWITCH> that may only be actuated by key.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HUMAN-OPERATED SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"PUSH BUTTON",null,null,null,null,null,"rdl:RDS473894",null,"A <PUSH BUTTON> is a <HUMAN-OPERATED SWITCH> having an actuator intended to be operated by force exerted by a part of the human body, usually the finger or palm of the hand, and having stored energy (spring) return.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUSH BUTTON",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EMERGENCY SHUT DOWN BUTTON",null,null,null,null,null,"rdl:RDS7057791",null,"An <EMERGENCY SHUT DOWN BUTTON> is a <PUSH BUTTON> which when manually activated starts a shut down system.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUSH BUTTON",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIRE WATER DELUGE RELEASE BUTTON",null,null,null,null,null,"rdl:RDS7057836",null,"A <FIRE WATER DELUGE RELEASE BUTTON> is a <PUSH BUTTON> which is intended to start the deluge fire water system.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUSH BUTTON",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ILLUMINATED BUTTON",null,null,null,null,null,"rdl:RDS965159",null,"An <ILLUMINATED BUTTON> is a <PUSH BUTTON> that is associated with a lamp or lamps that can give a visual indication by illumination.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUSH BUTTON",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INERGEN RELEASE BUTTON",null,null,null,null,null,"rdl:RDS305054",null,"An <INERGEN RELEASE BUTTON> is a <PUSH BUTTON> for <ACTUATING> an inergen system.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUSH BUTTON",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LOCKING PUSH-BUTTON",null,null,null,null,null,"rdl:RDS877094",null,"A <LOCKING PUSH-BUTTON> is a <PUSH BUTTON> that stays depressed until released with a key.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUSH BUTTON",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MOMENTARY PUSH BUTTON",null,null,null,null,null,"rdl:RDS877139",null,"A <MOMENTARY PUSH BUTTON> is a <PUSH BUTTON> that provides contact only when pressed.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUSH BUTTON",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PUSH-PUSH PUSH BUTTON",null,null,null,null,null,"rdl:RDS6768180",null,"A <PUSH-PUSH PUSH BUTTON> is a <PUSH BUTTON> that is activated, and later released, by <PUSHING>.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUSH BUTTON",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPRING RETURN PUSH BUTTON",null,null,null,null,null,"rdl:RDS1466086171",null,"An <SPRING RETURN PUSH BUTTON> is a <PUSH BUTTON> where a <SPRING> will return the <PUSH BUTTON> to a de-activated state.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUSH BUTTON",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STAY-PUT PUSH BUTTON",null,null,null,null,null,"rdl:RDS877184",null,"A <STAY-PUT PUSH BUTTON> is a <PUSH BUTTON> that stays in the activated state until manually released.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PUSH BUTTON",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WATER MIST RELEASE BUTTON",null,null,null,null,null,"rdl:RDS315089",null,"A <WATER MIST RELEASE BUTTON> is a <PUSH BUTTON> for <ACTUATING> a water mist system.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HUMAN-OPERATED SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTARY CONTROL SWITCH",null,null,null,null,null,"rdl:RDS935504",null,"A <ROTARY CONTROL SWITCH> is a <HUMAN-OPERATED SWITCH> having an actuator intended to be operated by rotation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HUMAN-OPERATED SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"SELECTOR SWITCH",null,null,null,null,null,"rdl:RDS891494",null,"A <SELECTOR SWITCH> is a <HUMAN-OPERATED SWITCH> that has more then two possible positoning states.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HUMAN-OPERATED SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"TAP CHANGER",null,null,null,null,null,"rdl:RDS877634",null,"A <TAP CHANGER> is a <HUMAN-OPERATED SWITCH> that changes the connection to a transformer from one tap to another so as to vary the turns ratio and hence control the output voltage under a varying load.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TAP CHANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OFF LOAD TAP CHANGER",null,null,null,null,null,"rdl:RDS877679",null,"An <OFF LOAD TAP CHANGER> is a <TAP CHANGER> for changing the tapping connections of a winding, suitable for operation while the transformer is off load.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TAP CHANGER",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ON LOAD TAP CHANGER",null,null,null,null,null,"rdl:RDS877724",null,"An <ON LOAD TAP CHANGER> is a <TAP CHANGER> for changing the tapping connections of a winding, suitable for operation while the transformer is energized or on load.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"HUMAN-OPERATED SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"TOGGLE SWITCH",null,null,null,null,null,"rdl:RDS964844",null,"A <TOGGLE SWITCH> is a <HUMAN-OPERATED SWITCH> operated by means of a projecting lever that is moved with a snap action, usually up and down.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"MULTI-CELL SWITCH",null,null,null,null,null,"rdl:RDS964439",null,"A <MULTI-CELL SWITCH> is an <ARTEFACT> and a <SWITCHING DEVICE> that is a frame assembly containing two or more basic cells, each of which may have any mechanical systems",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MEASURING FUNCTION","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"PROCESS SWITCH",null,null,null,null,null,"rdl:RDS7210156",null,"A <PROCESS SWITCH> is an <MEASURING FUNCTION> and a <SWITCHING DEVICE> that operates when the output of a <MEASURING ELEMENT> reaches a preset criterium",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"DUST SWITCH",null,null,null,null,null,"rdl:RDS2220007",null,"A <DUST SWITCH> is a <PROCESS SWITCH> using a <DUST MEASURING ELEMENT> that switches when the dust concentration in a gas flow has reached a preset value",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"FLOW SWITCH",null,null,null,null,null,"rdl:RDS302894",null,"A <FLOW SWITCH> is a <PROCESS SWITCH> using a <FLOW MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"LEVEL SWITCH",null,null,null,null,null,"rdl:RDS316754",null,"A <LEVEL SWITCH> is a <PROCESS SWITCH> using a <LEVEL MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"POSITION SWITCH",null,null,null,null,null,"rdl:RDS935594",null,"A <POSITION SWITCH> isa <PROCESS SWITCH> using a <POSITION MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","POSITION SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"LIMIT SWITCH",null,null,null,null,null,"rdl:RDS418814",null,"A <LIMIT SWITCH> is an <INSTRUMENTATION ITEM> and a <POSITION SWITCH> that is a switch preventing the travel of an object in a mechanism past some predetermined point, mechanically operated by the motion of the object itself",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","POSITION SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"PROXIMITY SWITCH",null,null,null,null,null,"rdl:RDS851084",null,"A <PROXIMITY SWITCH> is a <POSITION SWITCH> and a <PROXIMITY MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","POSITION SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"TRAVEL STOP",null,null,null,null,null,"rdl:RDS7773461",null,"A <TRAVEL STOP> is a <POSITION SWITCH> that terminates a rotation when a predefined position has been reached",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"PRESSURE SWITCH",null,null,null,null,null,"rdl:RDS309419",null,"A <PRESSURE SWITCH> isa <PROCESS SWITCH> using a <PRESSURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"ROTATIONAL SPEED SWITCH",null,null,null,null,null,"rdl:RDS317159",null,"A <ROTATIONAL SPEED SWITCH> isa <PROCESS SWITCH> using a <ROTATIONAL SPEED MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"TEMPERATURE SWITCH",null,null,null,null,null,"rdl:RDS2229401",null,"A <TEMPERATURE SWITCH> isa <PROCESS SWITCH> using a <TEMPERATURE MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"INSTRUMENTATION ITEM","TEMPERATURE SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMOSTAT",null,null,null,null,null,"rdl:RDS964664",null,"A <THERMOSTAT> is an <INSTRUMENTATION ITEM> and a <TEMPERATURE SWITCH> whose function is controlled by variations of temperature and whose contacts make or break automatically a load circuit when the temperature of the ambient space in which its sensing element placed or the temperature of the surface on which it is fixed reaches a predetermined value",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMOSTAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ADJUSTABLE THERMOSTAT",null,null,null,null,null,"rdl:RDS964709",null,"An <ADJUSTABLE THERMOSTAT> is a <THERMOSTAT> whose operating temperature may be varied by the user by adjusting the actuating mechanism, the position of which can be readily identified",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ADJUSTABLE THERMOSTAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MECHANICALLY ADJUSTABLE THERMOSTAT",null,null,null,null,null,"rdl:RDS1462231991",null,"A <MECHANICALLY ADJUSTABLE THERMOSTAT> is an <ADJUSTABLE THERMOSTAT> where the settings must be changed via mechanical means",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ADJUSTABLE THERMOSTAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROGRAMMABLE ADJUSTABLE THERMOSTAT",null,null,null,null,null,"rdl:RDS1462230971",null,"A <PROGRAMMABLE ADJUSTABLE THERMOSTAT> is an <ADJUSTABLE THERMOSTAT> that is programmable; i.e. the settings can be changed in software",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMOSTAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AMBIENT THERMOSTAT",null,null,null,null,null,"rdl:RDS964754",null,"An <AMBIENT THERMOSTAT> is a <THERMOSTAT> that responds to changes in the temperature of the space into which its sensing element penetrates or is housed",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"THERMOSTAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-ADJUSTABLE THERMOSTAT",null,null,null,null,null,"rdl:RDS964799",null,"A <NON-ADJUSTABLE THERMOSTAT> is a <THERMOSTAT> whose operating temperature is determined by a permanent setting carried out by the manufacturer",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"VIBRATION SWITCH",null,null,null,null,null,"rdl:RDS317204",null,"A <VIBRATION SWITCH> isa <PROCESS SWITCH> using a <VIBRATION MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"PROCESS SWITCH",null,null,null,null,null,null,null,null,null,null,null,null,null,"WEIGHT SWITCH",null,null,null,null,null,"rdl:RDS317249",null,"A <WEIGHT SWITCH> isa <PROCESS SWITCH> using a <WEIGHT MEASURING ELEMENT>",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,"RELAY",null,null,null,null,null,"rdl:RDS876194",null,"A <RELAY> is a <SWITCHING DEVICE> that usually is incorporating an electromagnet, whereby a current or signal in one circuit can open or close another circuit",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ARTEFACT","RELAY",null,null,null,null,null,null,null,null,null,null,null,null,"AUXILIARY RELAY",null,null,null,null,null,"rdl:RDS877229",null,"An <AUXILIARY RELAY> is an <ARTEFACT> and a <RELAY> that is mounted on the main actuating mechanism of another switch (typically a circuit breaker or a contactor) that operates in tandem with the main switch",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","RELAY",null,null,null,null,null,null,null,null,null,null,null,null,"EARTH FAULT RELAY",null,null,null,null,null,"rdl:RDS5779254",null,"An <EARTH FAULT RELAY> is an <ARTEFACT> and a <RELAY> that operates when a failure of insulation to earth is detected in the equipment or circuits protected",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","RELAY",null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRICAL RELAY",null,null,null,null,null,"rdl:RDS956339",null,"An <ELECTRICAL RELAY> is an <ARTEFACT> and a <RELAY> designed to produce sudden, predetermined changes in one or more electrical output circuits when certain conditions are fulfilled in the electrical input circuits controlling the device",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ALL-OR-NOTHING RELAY",null,null,null,null,null,"rdl:RDS956429",null,"An <ALL-OR-NOTHING RELAY> is an <ELECTRICAL RELAY> that is intended to be energized by a quantity whose value is either within its operative range or effectively zero.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BISTABLE RELAY",null,null,null,null,null,"rdl:RDS6233325",null,"A <BISTABLE RELAY> is an <ELECTRICAL RELAY> that, having responded to an energizing quantity and having changed its condition, remains in that condition after the quantity has been removed.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CONTROL RELAY",null,null,null,null,null,"rdl:RDS877274",null,"A <CONTROL RELAY> is an <ELECTRICAL RELAY> that is operating by permitting the next step in a control circuit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHANGE OVER CONTACT RELAY",null,null,null,null,null,"rdl:RDS877364",null,"A <CHANGE OVER CONTACT RELAY> is a <CONTROL RELAY> that has change-over contacts.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PLUG-IN RELAY",null,null,null,null,null,"rdl:RDS877454",null,"A <PLUG-IN RELAY> is a <CONTROL RELAY> that has plug-in terminals so that all connections can be made simultaneously by pushing the unit into a socket.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"CONTROL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TIMER RELAY",null,null,null,null,null,"rdl:RDS877499",null,"A <TIMER RELAY> is a <CONTROL RELAY> that will not close its front contacts or open its back contacts, or both, until expiration of a definite time interval after the relay has been energized.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TIMER RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DELAY ON DE-ENERGISE RELAY",null,null,null,null,null,"rdl:RDS6233100",null,"A <DELAY ON DE-ENERGISE RELAY> is a <TIMER RELAY> that delays switching the contacts when the coil is de-energised.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"TIMER RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DELAY ON ENERGISE RELAY",null,null,null,null,null,"rdl:RDS877589",null,"A <DELAY ON ENERGISE RELAY> is a <TIMER RELAY> that delays switching the contacts when the coil is energised.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COUNTER RELAY",null,null,null,null,null,"rdl:RDS5782760",null,"A <COUNTER RELAY> is an <ELECTRICAL RELAY> that is controlled by a counter.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DIRECT CURRENT RELAY",null,null,null,null,null,"rdl:RDS957059",null,"A <DIRECT CURRENT RELAY> is an <ELECTRICAL RELAY> designed for operation from a direct current source.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECT CURRENT RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-POLARIZED RELAY",null,null,null,null,null,"rdl:RDS957014",null,"A <NON-POLARIZED RELAY> is a <DIRECT CURRENT RELAY>, the change of condition of which does not depend upon the polarity of its input energizing quantity(ies).",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DIRECT CURRENT RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"POLARIZED RELAY",null,null,null,null,null,"rdl:RDS956969",null,"A <POLARIZED RELAY> is a <DIRECT CURRENT RELAY>, the change of condition of which depends upon the polarity of its input energizing quantity(ies).",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTROMECHANICAL RELAY",null,null,null,null,null,"rdl:RDS956699",null,"An <ELECTROMECHANICAL RELAY> is an <ELECTRICAL RELAY> in which the designed response is developed by the relative movement of mechanical elements under the action of a current in the input circuit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MEASURING RELAY",null,null,null,null,null,"rdl:RDS956474",null,"A <MEASURING RELAY> is an <ELECTRICAL RELAY> intended to operate when its characteristic quantity, under specified accuracy, attains its operate value.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MEASURING RELAY","SPECIFIED-TIME RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DEPENDENT-TIME MEASURING RELAY",null,null,null,null,null,"rdl:RDS956609",null,"A <DEPENDENT-TIME MEASURING RELAY> is a <MEASURING RELAY> and a <SPECIFIED-TIME RELAY> for which times depend, in a specified manner, on the value of the characteristic quantity.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"DEPENDENT-TIME MEASURING RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"THERMAL ELECTRICAL RELAY",null,null,null,null,null,"rdl:RDS957239",null,"A <THERMAL ELECTRICAL RELAY> is a <DEPENDENT-TIME MEASURING RELAY> that is intended to protect an equipment from electrical thermal damage by the measurement of the current flowing in the protected equipment and by a characteristic curve stimulating its thermal behaviour.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MEASURING RELAY","SPECIFIED-TIME RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"INDEPENDENT-TIME MEASURING RELAY",null,null,null,null,null,"rdl:RDS956654",null,"An <INDEPENDENT-TIME MEASURING RELAY> is a <MEASURING RELAY> and a <SPECIFIED-TIME RELAY> that is also a measuring relay the specified time of which can be considered as being independent, within specified limits, of the value of the characteristic quantity.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"MEASURING RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROTECTION RELAY",null,null,null,null,null,"rdl:RDS875204",null,"A <PROTECTION RELAY> is a <MEASURING RELAY> that, either solely or in combination with other relays, is a constituent of a protection equipment.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PROTECTION RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-PROGRAMMABLE PROTECTION RELAY",null,null,null,null,null,"rdl:RDS875519",null,"A <NON-PROGRAMMABLE PROTECTION RELAY> is a <PROTECTION RELAY> that is not programmable and is designed to inherently perform a certain protection function.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"NON-PROGRAMMABLE PROTECTION RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BUCHHOLZ RELAY",null,null,null,null,null,"rdl:RDS877319",null,"A <BUCHHOLZ RELAY> is a <NON-PROGRAMMABLE PROTECTION RELAY> that detects gassing of transformer coolant.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"PROTECTION RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PROGRAMMABLE PROTECTION RELAY",null,null,null,null,null,"rdl:RDS875474",null,"A <PROGRAMMABLE PROTECTION RELAY> is a <PROTECTION RELAY> that may be electronically programmed to perform any number of protection algorithms.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MONOSTABLE RELAY",null,null,null,null,null,"rdl:RDS956879",null,"A <MONOSTABLE RELAY> is an <ELECTRICAL RELAY> that, having responded to an input energizing quantity (or characteristic quantity) and having changed its condition, returns to its previous condition when the quantity is removed.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NON-SPECIFIED-TIME RELAY",null,null,null,null,null,"rdl:RDS956564",null,"A <NON-SPECIFIED-TIME RELAY> is an <ELECTRICAL RELAY> for which the times are not subject to any accuracy specification.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PRIMARY RELAY",null,null,null,null,null,"rdl:RDS957104",null,"A <PRIMARY RELAY> is an <ELECTRICAL RELAY> that is directly energized by the current or voltage in a main circuit, without an intermediate instrument transformer or shunt or transducer.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SECONDARY RELAY",null,null,null,null,null,"rdl:RDS957149",null,"A <SECONDARY RELAY> is an <ELECTRICAL RELAY> that is energized by the current or voltage derived from an instrument transformer or a transducer.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SPECIFIED-TIME RELAY",null,null,null,null,null,"rdl:RDS956519",null,"A <SPECIFIED-TIME RELAY> is an <ELECTRICAL RELAY> such that one or more of the times which characterize it (e.g. operate time) are subject to specified requirements, in particular concerning accuracy.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ELECTRICAL RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STATIC RELAY",null,null,null,null,null,"rdl:RDS956744",null,"A <STATIC RELAY> is an <ELECTRICAL RELAY> in which the designed response is developed by electronic, magnetic, optical or other components without mechanical motion.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STATIC RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STATIC RELAY WITH OUTPUT CONTACT",null,null,null,null,null,"rdl:RDS956789",null,"A <STATIC RELAY WITH OUTPUT CONTACT> is a <STATIC RELAY> having a contact in one or more of its output circuits.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"STATIC RELAY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"STATIC RELAY WITHOUT OUTPUT CONTACT",null,null,null,null,null,"rdl:RDS956834",null,"A <STATIC RELAY WITHOUT OUTPUT CONTACT> is a <STATIC RELAY> having no contact in its output circuits.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","RELAY",null,null,null,null,null,null,null,null,null,null,null,null,"PNEUMATIC RELAY",null,null,null,null,null,"rdl:RDS5780264",null,"A <PNEUMATIC RELAY> is an <ARTEFACT> and a <RELAY> that is pneumatically operated and which changes status or breaks another pneumatic circuit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","RELAY",null,null,null,null,null,null,null,null,null,null,null,null,"START RELAY",null,null,null,null,null,"rdl:RDS5779320",null,"A <START RELAY> is an <ARTEFACT> and a <RELAY> that is used in a control circuit with a contactor for starting an electrical machine",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","RELAY",null,null,null,null,null,null,null,null,null,null,null,null,"VOLTAGE RELAY",null,null,null,null,null,"rdl:RDS5778747",null,"A <VOLTAGE RELAY> is an <ARTEFACT> and a <RELAY> that is designed for voltage",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"REVERSING SWITCH",null,null,null,null,null,"rdl:RDS966644",null,"A <REVERSING SWITCH> is an <ARTEFACT> and a <SWITCHING DEVICE> for changing the direction of a current in part of an electric circuit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"SEMICONDUCTOR SWITCHING DEVICE",null,null,null,null,null,"rdl:RDS934424",null,"A <SEMICONDUCTOR SWITCHING DEVICE> is an <ARTEFACT> and a <SWITCHING DEVICE> designed to make the current in an electric circuit by means of the controlled conductivity of a semiconductor",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC AC POWER SWITCH",null,null,null,null,null,"rdl:RDS953054",null,"An <ELECTRONIC AC POWER SWITCH> is a <SEMICONDUCTOR SWITCHING DEVICE> capable of switching alternating current.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SEMICONDUCTOR SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,null,null,"ELECTRONIC DC POWER SWITCH",null,null,null,null,null,"rdl:RDS953099",null,"An <ELECTRONIC DC POWER SWITCH> is a <SEMICONDUCTOR SWITCHING DEVICE> capable of switching direct current.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"INSTRUMENTATION ITEM","STANDARD SIGNAL RECEIVER","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,"SIGNAL SWITCH",null,null,null,null,null,"rdl:RDS222463",null,"A <SIGNAL SWITCH> is a <INSTRUMENTATION ITEM> and a <STANDARD SIGNAL RECEIVER> and a <SWITCHING DEVICE> that operates when an input standard signal reaches a preset criterium",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"SWITCH ASSEMBLY",null,null,null,null,null,"rdl:RDS13610345",null,"A <SWITCH ASSEMBLY> is an <ARTEFACT> and a <SWITCHING DEVICE> that is an assembly of a <SWITCH> and supporting components",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"SWITCH-DISCONNECTOR",null,null,null,null,null,"rdl:RDS934784",null,"A <SWITCH-DISCONNECTOR> is an <ARTEFACT> and a <SWITCHING DEVICE> that, in the open position, satisfies the isolating requirements specified for a disconnector",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH-DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"AIR SWITCH",null,null,null,null,null,"rdl:RDS6568505",null,"An <AIR SWITCH> is a <SWITCH-DISCONNECTOR> in which the contacts are in air.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH-DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"FUSE-SWITCH-DISCONNECTOR",null,null,null,null,null,"rdl:RDS935099",null,"A <FUSE-SWITCH-DISCONNECTOR> is a <SWITCH-DISCONNECTOR> in which a fuse-link or a fuse-carrier with fuse-link forms the moving contact.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH-DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"SF6 SWITCH",null,null,null,null,null,"rdl:RDS877004",null,"An <SF6 SWITCH> is a <SWITCH-DISCONNECTOR> in which the contacts are in a SF6 gas chamber.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH-DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"SWITCH-DISCONNECTOR-FUSE",null,null,null,null,null,"rdl:RDS934964",null,"A <SWITCH-DISCONNECTOR-FUSE> is a <SWITCH-DISCONNECTOR> in which one or more poles have a fuse in series in a composite unit.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCH-DISCONNECTOR",null,null,null,null,null,null,null,null,null,null,null,null,null,"VACUUM SWITCH",null,null,null,null,null,"rdl:RDS877049",null,"A <VACUUM SWITCH> is a <SWITCH-DISCONNECTOR> in which the contacts are in a vacuum chamber.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","FUSE","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,"SWITCH-FUSE",null,null,null,null,null,"rdl:RDS934874",null,"A <SWITCH-FUSE> is an <ARTEFACT> and a <SWITCHING DEVICE> and a <FUSE> in which one or more poles have a fuse in series in a composite unit",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"ARTEFACT","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"SWITCHBOARD",null,null,null,null,null,"rdl:RDS464129",null,"A <SWITCHBOARD> is an <ARTEFACT> and a <SWITCHING DEVICE>that is one or more panels accommodating control switches, indicators, and other apparatus for operating electric circuits",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCHBOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,"AUXILIARY SWITCHBOARD",null,null,null,null,null,"rdl:RDS1006154",null,"An <AUXILIARY SWITCHBOARD> is a <SWITCHBOARD> (or a cubicle) on which are fixed the devices necessary to control, to protect and to distribute auxiliary a.c. and d.c. supplies within a substation.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCHBOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,"EMERGENCY SWITCHBOARD",null,null,null,null,null,"rdl:RDS5771680",null,"An <EMERGENCY SWITCHBOARD> is a <SWITCHBOARD> that has the function to be used in emergency.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCHBOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,"MAIN SWITCHBOARD",null,null,null,null,null,"rdl:RDS5771725",null,"An <MAIN SWITCHBOARD> is a <SWITCHBOARD> intended to be used as a main switchboard.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"SWITCHBOARD",null,null,null,null,null,null,null,null,null,null,null,null,null,"SUB SWITCHBOARD",null,null,null,null,null,"rdl:RDS5771770",null,"A <SUB SWITCHBOARD> is a <SWITCHBOARD> intended to be used as a sub switchboard.",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]
[null,null,"COMMUNICATIONS DEVICE","SWITCHBOARD",null,null,null,null,null,null,null,null,null,null,null,null,"TELEPHONE SWITCHBOARD",null,null,null,null,null,"rdl:RDS5762605",null,"A <TELEPHONE SWITCHBOARD> is a <SWITCHBOARD> and a <COMMUNICATIONS DEVICE> intended to connect and direct traffic between internal and externat telephone lines",null,null,null,null,null,"dm:ClassOfFunctionalObject"]
[null,null,"ELECTRICAL APPARATUS","SWITCHING DEVICE",null,null,null,null,null,null,null,null,null,null,null,"TRIP-FREE MECHANICAL SWITCHING DEVICE",null,null,null,null,null,"rdl:RDS935774",null,"A <TRIP-FREE MECHANICAL SWITCHING DEVICE> is an <ELECTRICAL APPARATUS> and a <SWITCHING DEVICE>, the moving contacts of which return to and remain in the open position when the opening operation is initiated after the initiation of the closing operation, even if the closing command is maintained",null,null,null,null,null,"dm:ClassOfInanimatePhysicalObject"]